[IBIS Ver]     5.0
[File Name]    EEsof_Tx_Pass_Through.ibs
[File Rev]     1.0
[Component]    EEsof_Tx_Pass_Through
[Manufacturer] Keysight Technologies, Inc.

[Package]

R_pkg  0.0    NA      NA
L_pkg  0.0    NA      NA
C_pkg  0.0    NA      NA

[Pin]    signal_name              model_name        R_pin L_pin  C_pin
1p       EEsof_Tx_Pass_Through_p          EEsof_Tx_Pass_Through
1n       EEsof_Tx_Pass_Through_n          EEsof_Tx_Pass_Through

[Diff_Pin] inv_pin vdiff tdelay_typ tdelay_min tdelay_max
1p       1n           NA    NA    NA    NA

[Model] EEsof_Tx_Pass_Through
Model_type Output

C_comp 0p 0p 0p
Cref = 0
Vref = 0.5
Rref = 50
Vmeas = 0.5

[Temperature_Range] 25 125 0
[Voltage Range] 1.0 1.0 1.0

[Algorithmic Model]
Executable Windows_cl17.00.60315.1_64 EEsof_Tx_Pass_Through_x64.dll EEsof_Tx_Pass_Through.ami

Executable Linux_gcc4.6.2_64 EEsof_Tx_Pass_Through_x64.so EEsof_Tx_Pass_Through.ami

[End Algorithmic Model]

[Pulldown]
-5.058466                 -0.1             -0.1            -0.1
 0.0               0.0                0.0               0.0
 5.058466                      0.1              0.1             0.1

[Pullup]
-5.058466                  0.1              0.1             0.1
 0.0               0.0                0.0               0.0
5.058466                   -0.1             -0.1            -0.1


[Ramp]
dV/dt_r 0.3/1.5p 0.3/1.5p 0.3/1.5p
dV/dt_f 0.3/1.5p 0.3/1.5p 0.3/1.5p

[END]
