After afe4404evm upgrade firmware from 1.3 to 1.5, GUI shows unable to connect图形用户界面

描述已自动生成图形用户界面, 文本, 应用程序, 电子邮件

描述已自动生成

After the firmware upgrade, the display is as follows:

图形用户界面, 文本, 应用程序, 电子邮件

描述已自动生成

Then it fails to connect, the AFE44xx EVM (COM3) is no longer shown in the device manager, but HID-compliant device and USB input device

图形用户界面, 文本, 应用程序

描述已自动生成

Pressing SW2 doesn't work, doesn't fix the problem

When it can be connected normally, after the 4404 is connected to the computer, the sensor’s LEDs flash, the LED1 on the 4404 development board is always on, and the LED2 and LED3 can be seen flashing when connected.

文本

中度可信度描述已自动生成

However, after the firmware upgrade, the sensor’s LEDs don’t flash, the LED1 on the 4404 development board is always on, and the LED2 and LED3 do not flash when connected.

电子仪器

中度可信度描述已自动生成