


I don't know where to see the following picture and where to set the NCO.




I run the line for the channel.


Then I open the capture window by double clicking on the ‘CGui\_Cgui\_custom\_GUI’ in the Custom GUI List.








After I click ‘Start’,the signal is shown below, however there are differences from the example.











Here is the GUI, where should I make changes to achieve the signals I need?

