root@j7-evm:/opt/vision_apps# ./run_app_single_cam.sh                                                                                                                                            
APP: Init ... !!!                                                                                                                                                                                
MEM: Init ... !!!                                                                                                                                                                                
MEM: Initialized DMA HEAP (fd=4) !!!                                                                                                                                                             
MEM: Init ... Done !!!                                                                                                                                                                           
IPC: Init ... !!!                                                                                                                                                                                
IPC: Init ... Done !!!                                                                                                                                                                           
REMOTE_SERVICE: Init ... !!!                                                                                                                                                                     
REMOTE_SERVICE: Init ... Done !!!                                                                                                                                                                
APP: Init ... Done !!!                                                                                                                                                                           
    64.352438 s:  VX_ZONE_INIT:Enabled                                                                                                                                                           
    64.352460 s:  VX_ZONE_ERROR:Enabled                                                                                                                                                          
    64.352465 s:  VX_ZONE_WARNING:Enabled                                                                                                                                                        
    64.353094 s:  VX_ZONE_INIT:[tivxInit:71] Initialization Done !!!                                                                                                                             
    64.353253 s:  VX_ZONE_INIT:[tivxHostInit:48] Initialization Done for HOST !!!                                                                                                                
Invalid token [                                                                                                                                                                                  
]                                                                                                                                                                                                
sensor_selection = [0]                                                                                                                                                                           
Invalid token [                                                                                                                                                                                  
]                                                                                                                                                                                                
ldc_enable = [0]                                                                                                                                                                                 
Invalid token [                                                                                                                                                                                  
]                                                                                                                                                                                                
num_frames_to_run = [1000000000]                                                                                                                                                                 
Invalid token [                                                                                                                                                                                  
]                                                                                                                                                                                                
is_interactive = [1]                                                                                                                                                                             
IttCtrl_registerHandler: command echo registered at location 0                                                                                                                                   
IttCtrl_registerHandler: command iss_read_2a_params registered at location 1                                                                                                                     
IttCtrl_registerHandler: command iss_write_2a_params registered at location 2                                                                                                                    
IttCtrl_registerHandler: command iss_raw_save registered at location 3                                                                                                                           
IttCtrl_registerHandler: command iss_yuv_save registered at location 4                                                                                                                           
IttCtrl_registerHandler: command iss_read_sensor_reg registered at location 5                                                                                                                    
IttCtrl_registerHandler: command iss_write_sensor_reg registered at location 6                                                                                                                   
IttCtrl_registerHandler: command dev_ctrl registered at location 7                                                                                                                               
IttCtrl_registerHandler: command iss_send_dcc_file registered at location 8                                                                                                                      
tivxImagingLoadKernels done                                                                                                                                                                      
    64.355627 s: ISS: Enumerating sensors ... !!!                                                                                                                                                
 NETWORK: Opened at IP Addr = 192.168.1.143, socket port=5000!!!                                                                                                                                 
    64.356042 s: ISS: Enumerating sensors ... found 0 : IMX390-UB953_D3                                                                                                                          
    64.356049 s: ISS: Enumerating sensors ... found 1 : AR0233-UB953_MARS                                                                                                                        
    64.356053 s: ISS: Enumerating sensors ... found 2 : AR0820-UB953_LI                                                                                                                          
    64.356058 s: ISS: Enumerating sensors ... found 3 : UB9xxx_RAW12_TESTPATTERN                                                                                                                 
    64.356062 s: ISS: Enumerating sensors ... found 4 : UB96x_UYVY_TESTPATTERN                                                                                                                   
    64.356066 s: ISS: Enumerating sensors ... found 5 : GW_AR0233_UYVY                                                                                                                           
6 sensor(s) found                                                                                                                                                                                
Supported sensor list:                                                                                                                                                                           
a : IMX390-UB953_D3                                                                                                                                                                              
b : AR0233-UB953_MARS                                                                                                                                                                            
c : AR0820-UB953_LI                                                                                                                                                                              
d : UB9xxx_RAW12_TESTPATTERN                                                                                                                                                                     
e : UB96x_UYVY_TESTPATTERN                                                                                                                                                                       
f : GW_AR0233_UYVY                                                                                                                                                                               
Select a sensor                                                                                                                                                                                  
[MCU2_0]     64.355751 s: ImageSensor_RemoteServiceHandler: IM_SENSOR_CMD_CREATE                                                                                                                 
[MCU2_0]     64.355823 s: Sensor at index 0 = IMX390-UB953_D3                                                                                                                                    
[MCU2_0]     64.355855 s: Sensor at index 1 = AR0233-UB953_MARS                                                                                                                                  
[MCU2_0]     64.355882 s: Sensor at index 2 = AR0820-UB953_LI                                                                                                                                    
[MCU2_0]     64.355907 s: Sensor at index 3 = UB9xxx_RAW12_TESTPATTERN                                                                                                                           
[MCU2_0]     64.355933 s: Sensor at index 4 = UB96x_UYVY_TESTPATTERN                                                                                                                             
[MCU2_0]     64.355958 s: Sensor at index 5 = GW_AR0233_UYVY                                                                                                                                     
a                                                                                                                                                                                                
                                                                                                                                                                                                 
LDC Selection Yes(1)/No(0)                                                                                                                                                                       
LDC Selection Yes(1)/No(0)                                                                                                                                                                       
0                                                                                                                                                                                                
Sensor selected : IMX390-UB953_D3                                                                                                                                                                
app_init done                                                                                                                                                                                    
app_create_graph with RGB output                                                                                                                                                                 
Querying IMX390-UB953_D3                                                                                                                                                                         
    82.857814 s: ISS: Querying sensor [IMX390-UB953_D3] ... !!!                                                                                                                                  
    82.858080 s: ISS: Querying sensor [IMX390-UB953_D3] ... Done !!!                                                                                                                             
WDR mode is supported                                                                                                                                                                            
Expsoure control is supported                                                                                                                                                                    
Gain control is supported                                                                                                                                                                        
CMS Usecase is supported                                                                                                                                                                         
obj->aewb_cfg.ae_mode = 0                                                                                                                                                                        
obj->aewb_cfg.awb_mode = 0                                                                                                                                                                       
Sensor DCC is enabled                                                                                                                                                                            
Sensor width = 1936                                                                                                                                                                              
Sensor height = 1096                                                                                                                                                                             
Sensor DCC ID = 390                                                                                                                                                                              
Sensor Supported Features = 0x378                                                                                                                                                                
Sensor Enabled Features = 0x358                                                                                                                                                                  
    82.858117 s: ISS: Initializing sensor [IMX390-UB953_D3], doing IM_SENSOR_CMD_PWRON ... !!!                                                                                                   
[MCU2_0]     82.857925 s: ImageSensor_RemoteServiceHandler: IM_SENSOR_CMD_QUERY                                                                                                                  
[MCU2_0]     82.857993 s: Received Query for IMX390-UB953_D3                                                                                                                                     
[MCU2_0]     82.858189 s: ImageSensor_RemoteServiceHandler: IM_SENSOR_CMD_PWRON                                                                                                                  
[MCU2_0]     82.858269 s: IM_SENSOR_CMD_PWRON : channel_mask = 0x1                                                                                                                               
[MCU2_0]     82.858396 s: IMX390_PowerOn : chMask = 0x1                                                                                                                                          
[MCU2_0]     82.858444 s: ub960_cfgScript : ub960I2cAddr = 0x3d                                                                                                                                  
[MCU2_0]     82.858469 s: UB960 config start                                                                                                                                                     
    83.058075 s: ISS: Initializing sensor [IMX390-UB953_D3], doing IM_SENSOR_CMD_CONFIG ... !!!                                                                                                  
[MCU2_0]     83.057939 s:  End of UB960 config                                                                                                                                                   
[MCU2_0]     83.058182 s: ImageSensor_RemoteServiceHandler: IM_SENSOR_CMD_CONFIG                                                                                                                 
[MCU2_0]     83.058236 s: Application requested features = 0x358                                                                                                                                 
[MCU2_0]                                                                                                                                                                                         
[MCU2_0]     83.058305 s: ub960_cfgScript : ub960I2cAddr = 0x3d                                                                                                                                  
[MCU2_0]     83.058338 s: UB960 config start                                                                                                                                                     
[MCU2_0]     83.313775 s:  End of UB960 config                                                                                                                                                   
[MCU2_0]     83.313870 s: ub960_cfgScript : ub960I2cAddr = 0x36                                                                                                                                  
[MCU2_0]     83.313905 s: UB960 config start                                                                                                                                                     
[MCU2_0]     83.569772 s:  End of UB960 config                                                                                                                                                   
[MCU2_0]     83.569828 s: Configuring camera # 0                                                                                                                                                 
[MCU2_0]     83.569859 s: ub953 config start : slaveAddr = 0x74                                                                                                                                  
[MCU2_0]     83.759776 s:  End of UB953 config                                                                                                                                                   
[MCU2_0]     83.759871 s:  Configuring IMX390 imager 0x40.. Please wait till it finishes                                                                                                         
    85.811909 s: ISS: Initializing sensor [IMX390-UB953_D3] ... Done !!!                                                                                                                         
Creating graph                                                                                                                                                                                   
Initializing params for capture node                                                                                                                                                             
Initializing params for capture node                                                                                                                                                             
local_capture_config.numDataLanes = 4                                                                                                                                                            
local_capture_config.dataLanesMap[0] = 1                                                                                                                                                         
local_capture_config.dataLanesMap[1] = 2                                                                                                                                                         
local_capture_config.dataLanesMap[2] = 3                                                                                                                                                         
local_capture_config.dataLanesMap[3] = 4                                                                                                                                                         
capture_config = 0x0x6e6380                                                                                                                                                                      
Creating capture node                                                                                                                                                                            
obj->capture_node = 0x0x6a0c80                                                                                                                                                                   
Test data path is NULL. Defaulting to current folder                                                                                                                                             
reading test RAW image .//img_test.raw                                                                                                                                                           
read_test_image_raw : Unable to open file .//img_test.raw                                                                                                                                        
VISS Set Reference done                                                                                                                                                                          
[MCU2_0]     85.811715 s:  IMX390 config done                                                                                                                                                    
[MCU2_0]     85.811776 s: IM_SENSOR_CMD_CONFIG returning status = 0                                                                                                                              
AEWB Set Reference done                                                                                                                                                                          
vxVISS_RGB!                                                                                                                                                                                      
 VX_TYPE_IMAGE: image_109, 1936 x 1096, 1 plane(s), 6383104 B, VX_DF_IMAGE_RGB VX_COLOR_SPACE_BT709 VX_CHANNEL_RANGE_FULL VX_MEMORY_TYPE_NONE, 1 refs                                            
 VX_TYPE_GRAPH: graph_85, 4 nodes, VX_GRAPH_STATE_UNVERIFIED, avg perf  0.000000s, 0 parameters, 1 refs                                                                                          
 VX_TYPE_NODE: VISS_RGB_Conversion, 5 params, avg perf  0.000000s, VX_SUCCESS, 1 refs                                                                                                            
vxVISS_RGB DONE!                                                                                                                                                                                 
Scaler is set to enabled                                                                                                                                                                         
Disabling scaler for RGB                                                                                                                                                                         
VISS_RGB is enabled                                                                                                                                                                              
Display Set Target done                                                                                                                                                                          
vxSetGraphScheduleConfig done                                                                                                                                                                    
Scaler is disabled                                                                                                                                                                               
app_create_graph exiting                                                                                                                                                                         
app_create_graph done                                                                                                                                                                            

 ==========================                                                                                                                                                                      
 Demo : Single Camera w/ 2A                                                                                                                                                                      
 ==========================                                                                                                                                                                      
                                                                                                                                                                                                 
 p: Print performance statistics                                                                                                                                                                 
                                                                                                                                                                                                 
 s: Save Sensor RAW, VISS Output and H3A output images to File System                                                                                                                            
                                                                                                                                                                                                 
 e: Export performance statistics                                                                                                                                                                
                                                                                                                                                                                                 
 u: Update DCC from File System                                                                                                                                                                  

 x: Exit                                                                                                                                                                                         
                                                                                                                                                                                                 
 Enter Choice:                                                                                                                                                                                   
Unsupported command                                                                                                                                                                              

                                                                                                                                                                                                 
 ==========================                                                                                                                                                                      
 Demo : Single Camera w/ 2A                                                                                                                                                                      
 ==========================                                                                                                                                                                      
                                                                                                                                                                                                 
 p: Print performance statistics                                                                                                                                                                 
                                                                                                                                                                                                 
 s: Save Sensor RAW, VISS Output and H3A output images to File System                                                                                                                            
                                                                                                                                                                                                 
 e: Export performance statistics                                                                                                                                                                
                                                                                                                                                                                                 
 u: Update DCC from File System                                                                                                                                                                  

 x: Exit                                                                                                                                                                                         
                                                                                                                                                                                                 
 Enter Choice:     85.905735 s: ISS: Starting sensor [IMX390-UB953_D3] ... !!!                                                                                                                   
[MCU2_0]     85.905861 s: ImageSensor_RemoteServiceHandler: IM_SENSOR_CMD_STREAM_ON                                                                                                              
[MCU2_0]     85.905937 s: IM_SENSOR_CMD_STREAM_ON:  channel_mask = 0x1                                                                                                                           
[MCU2_0]     85.906007 s: ub960_cfgScript : ub960I2cAddr = 0x3d                                                                                                                                  
[MCU2_0]     85.906037 s: UB960 config start                                                                                                                                                     
[MCU2_0]     86.161780 s:  End of UB960 config                                                                                                                                                   
[MCU2_0]     86.161873 s: ub960_cfgScript : ub960I2cAddr = 0x36                                                                                                                                  
[MCU2_0]     86.161906 s: UB960 config start                                                                                                                                                     
[MCU2_0]     86.417774 s:  End of UB960 config                                                                                                                                                   
[MCU2_0]     86.417831 s: Starting camera # 0                                                                                                                                                    
[MCU2_0]     86.417880 s: Entering IssSensor_Start                                                                                                                                               
[MCU2_0]     86.427724 s: enableUB960Streaming ub960InstanceId = 0                                                                                                                               
[MCU2_0]     86.427926 s: ub960_cfgScript : ub960I2cAddr = 0x3d                                                                                                                                  
[MCU2_0]     86.427959 s: UB960 config start                                                                                                                                                     
    86.459898 s: ISS: Starting sensor [IMX390-UB953_D3] ... !!!                                                                                                                                  
[MCU2_0]     86.459773 s:  End of UB960 config                                                                                                                                                   
p                                                                                                                                                                                                

Summary of CPU load,                                                                                                                                                                             
====================                                                                                                                                                                             
                                                                                                                                                                                                 
CPU: mpu1_0: TOTAL LOAD =   0.27 % ( HWI =   0. 2 %, SWI =   0. 1 % )                                                                                                                            
CPU: mcu2_0: TOTAL LOAD =   2.63 % ( HWI =   0.84 %, SWI =   0.14 % )                                                                                                                            
CPU: mcu2_1: TOTAL LOAD =   0. 9 % ( HWI =   0. 6 %, SWI =   0. 2 % )                                                                                                                            
CPU:  c6x_1: TOTAL LOAD =   0. 5 % ( HWI =   0. 2 %, SWI =   0. 1 % )                                                                                                                            
CPU:  c6x_2: TOTAL LOAD =   0. 5 % ( HWI =   0. 2 %, SWI =   0. 1 % )                                                                                                                            
CPU:  c7x_1: TOTAL LOAD =   0. 7 % ( HWI =   0. 3 %, SWI =   0. 2 % )                                                                                                                            

HWA performance statistics,                                                                                                                                                                      
===========================                                                                                                                                                                      

                                                                                                                                                                                                 
DDR performance statistics,                                                                                                                                                                      
===========================                                                                                                                                                                      
                                                                                                                                                                                                 
DDR: READ  BW: AVG =     56 MB/s, PEAK =    890 MB/s                                                                                                                                             
DDR: WRITE BW: AVG =     88 MB/s, PEAK =    738 MB/s                                                                                                                                             
DDR: TOTAL BW: AVG =    144 MB/s, PEAK =   1628 MB/s                                                                                                                                             

Detailed CPU performance/memory statistics,                                                                                                                                                      
===========================================                                                                                                                                                      
                                                                                                                                                                                                 
CPU: mcu2_0: TASK:           IPC_RX:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:       REMOTE_SRV:   0. 2 %                                                                                                                                                    
CPU: mcu2_0: TASK:         TIVX_CPU:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:          TIVX_NF:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:        TIVX_LDC1:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:        TIVX_MSC1:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:        TIVX_MSC2:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:       TIVX_VISS1:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:       TIVX_CAPT1:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:       TIVX_CAPT2:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:       TIVX_DISP1:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:       TIVX_DISP2:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:       TIVX_CSITX:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:       TIVX_CAPT3:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:       TIVX_CAPT4:   0. 0 %                                                                                                                                                    
CPU: mcu2_0: TASK:       TIVX_CAPT5:   0. 0 %                                                                                                                                                    
                                                                                                                                                                                                 
CPU: mcu2_0: HEAP:   DDR_SHARED_MEM: size =    8388608 B, free =    8023808 B ( 95 % unused)                                                                                                     
CPU: mcu2_0: HEAP:           L3_MEM: size =     131072 B, free =     131072 B (100 % unused)                                                                                                     
CPU: mcu2_0: HEAP:  DDR_NON_CACHE_M: size =      65536 B, free =      65536 B (100 % unused)                                                                                                     
                                                                                                                                                                                                 
CPU: mcu2_1: TASK:           IPC_RX:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:       REMOTE_SRV:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:         TIVX_SDE:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:         TIVX_DOF:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:       TIVX_VDEC1:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:       TIVX_VDEC2:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:       TIVX_VENC1:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:       TIVX_VENC2:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:      IPC_TEST_RX:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU: mcu2_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
                                                                                                                                                                                                 
CPU: mcu2_1: HEAP:   DDR_SHARED_MEM: size =   16777216 B, free =   16774912 B ( 99 % unused)                                                                                                     
CPU: mcu2_1: HEAP:           L3_MEM: size =     131072 B, free =     131072 B (100 % unused)                                                                                                     
CPU: mcu2_1: HEAP:  DDR_NON_CACHE_M: size =   67043328 B, free =   47144960 B (  6 % unused)                                                                                                     
                                                                                                                                                                                                 
CPU:  c6x_1: TASK:           IPC_RX:   0. 0 %                                                                                                                                                    
CPU:  c6x_1: TASK:       REMOTE_SRV:   0. 0 %                                                                                                                                                    
CPU:  c6x_1: TASK:         TIVX_CPU:   0. 0 %                                                                                                                                                    
CPU:  c6x_1: TASK:      IPC_TEST_RX:   0. 0 %                                                                                                                                                    
CPU:  c6x_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c6x_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c6x_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c6x_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c6x_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
                                                                                                                                                                                                 
CPU:  c6x_1: HEAP:   DDR_SHARED_MEM: size =   16777216 B, free =   16774912 B ( 99 % unused)                                                                                                     
CPU:  c6x_1: HEAP:           L2_MEM: size =     229376 B, free =     229376 B (100 % unused)                                                                                                     
CPU:  c6x_1: HEAP:  DDR_SCRATCH_MEM: size =   50331648 B, free =   50331648 B ( 14 % unused)                                                                                                     
                                                                                                                                                                                                 
CPU:  c6x_2: TASK:           IPC_RX:   0. 0 %                                                                                                                                                    
CPU:  c6x_2: TASK:       REMOTE_SRV:   0. 0 %                                                                                                                                                    
CPU:  c6x_2: TASK:         TIVX_CPU:   0. 0 %                                                                                                                                                    
CPU:  c6x_2: TASK:      IPC_TEST_RX:   0. 0 %                                                                                                                                                    
CPU:  c6x_2: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c6x_2: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c6x_2: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c6x_2: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c6x_2: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
                                                                                                                                                                                                 
CPU:  c6x_2: HEAP:   DDR_SHARED_MEM: size =   16777216 B, free =   16774912 B ( 99 % unused)                                                                                                     
CPU:  c6x_2: HEAP:           L2_MEM: size =     229376 B, free =     229376 B (100 % unused)                                                                                                     
CPU:  c6x_2: HEAP:  DDR_SCRATCH_MEM: size =   50331648 B, free =   50331648 B ( 14 % unused)                                                                                                     
                                                                                                                                                                                                 
CPU:  c7x_1: TASK:           IPC_RX:   0. 0 %                                                                                                                                                    
CPU:  c7x_1: TASK:       REMOTE_SRV:   0. 0 %                                                                                                                                                    
CPU:  c7x_1: TASK:         TIVX_CPU:   0. 0 %                                                                                                                                                    
CPU:  c7x_1: TASK:      IPC_TEST_RX:   0. 0 %                                                                                                                                                    
CPU:  c7x_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c7x_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c7x_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c7x_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
CPU:  c7x_1: TASK:      IPC_TEST_TX:   0. 0 %                                                                                                                                                    
                                                                                                                                                                                                 
CPU:  c7x_1: HEAP:   DDR_SHARED_MEM: size =  268435456 B, free =  268435456 B (  4 % unused)                                                                                                     
CPU:  c7x_1: HEAP:           L3_MEM: size =    8159232 B, free =    8159232 B (100 % unused)                                                                                                     
CPU:  c7x_1: HEAP:           L2_MEM: size =     491520 B, free =     491520 B (100 % unused)                                                                                                     
CPU:  c7x_1: HEAP:           L1_MEM: size =      16384 B, free =      16384 B (100 % unused)                                                                                                     
CPU:  c7x_1: HEAP:  DDR_SCRATCH_MEM: size =  234881024 B, free =  234881024 B (  8 % unused)                                                                                                     

GRAPH:         graph_85 (#nodes =   5, #executions =      0)                                                                                                                                     
 NODE:   CAPTURE1:                  node_96: avg =      0 usecs, min/max = 18446744073709551 /      0 usecs, #executions =          0                                                            
 NODE: VPAC_VISS1:          VISS_Processing: avg =      0 usecs, min/max = 18446744073709551 /      0 usecs, #executions =          0                                                            
 NODE:     IPU1-0:               2A_AlgNode: avg =      0 usecs, min/max = 18446744073709551 /      0 usecs, #executions =          0                                                            
 NODE:      DSP-1:      VISS_RGB_Conversion: avg =      0 usecs, min/max = 18446744073709551 /      0 usecs, #executions =          0                                                            
 NODE:   DISPLAY1:                 node_112: avg =      0 usecs, min/max = 18446744073709551 /      0 usecs, #executions =          0                                                            
                                                                                                                                                                                                 
 PERF:            TOTAL: avg =      0 usecs, min/max = 4294967295 /      0 usecs, #executions =          0                                                                                       
                                                                                                                                                                                                 
 PERF:            TOTAL:    0. 0 FPS                                                                                                                                                             

                                                                                                                                                                                                 
 ==========================                                                                                                                                                                      
 Demo : Single Camera w/ 2A                                                                                                                                                                      
 ==========================                                                                                                                                                                      
                                                                                                                                                                                                 
 p: Print performance statistics                                                                                                                                                                 
                                                                                                                                                                                                 
 s: Save Sensor RAW, VISS Output and H3A output images to File System                                                                                                                            
                                                                                                                                                                                                 
 e: Export performance statistics                                                                                                                                                                
                                                                                                                                                                                                 
 u: Update DCC from File System                                                                                                                                                                  

 x: Exit                                                                                                                                                                                         
                                                                                                                                                                                                 
 Enter Choice:                                                                                                                                                                                   
Unsupported command                                                                                                                                                                              

                                                                                                                                                                                                 
 ==========================                                                                                                                                                                      
 Demo : Single Camera w/ 2A                                                                                                                                                                      
 ==========================                                                                                                                                                                      
                                                                                                                                                                                                 
 p: Print performance statistics                                                                                                                                                                 
                                                                                                                                                                                                 
 s: Save Sensor RAW, VISS Output and H3A output images to File System                                                                                                                            
                                                                                                                                                                                                 
 e: Export performance statistics                                                                                                                                                                
                                                                                                                                                                                                 
 u: Update DCC from File System                                                                                                                                                                  

 x: Exit                                                                                                                                                                                         
                                                                                                                                                                                                 
 Enter Choice: x                                                                                                                                                                                 
                                                                                                                                                                                                 
^C                                                                                                                                                                                               
Clean up and exit while handling signal 2                                                                                                                                                        
Application did not close some rpmsg_char devices