################################################################################
# Configuration file for TDA4x LDC C Model                                     #
################################################################################
   42     # PRIVATE_MEMSIZE       pixmem_size          Fixed to 42
   30     # PRIVATE_MEMSIZE       pixmem_sizeC         Fixed to 30
   10     # PRIVATE_MEMSIZE       meshmem_size         Fixed to 10
    1     # LDC_CTRL              LDC_EN               LDC Enable, 0: Disable,  1: Enable
    1     # LDC_CTRL              LDMAPEN              LD Mapping enable, 0: disable, 1: enable
    2     # LDC_CTRL              DATAMODE             Input data mode, 0: UYVY,  1: Y only, 2: YUV420SP, 3: UV only
    0     # LDC_CTRL              OP_DATAMODE          Output data mode, 0: keep UYVY; 1: convert to 420
    0     # LDC_CTRL              IP_DFMT              Input pixel format, 0: 8b,  1: 12b packed, 2: 12b unpacked
    1     # LDC_CTRL              PWARPEN              0: Disable perspective warp. 1: Enable perspective warp
    1     # LDC_CFG               YINT_TYP             Interpolation type for Y data.  0: Bicubic,  1: Bilinear
    0     # LDC_CFG               REGMODE_EN           Region mode, 0: disable, 1: enable
    4     # LDC_MESHTABLE_CFG     M                    Mesh table subsampling factor (0-7)
 1280     # LDC_MESH_FRSZ         W                    Mesh frame width (0-8192)
  720     # LDC_MESH_FRSZ         H                    Mesh frame height (0-8192)
 1280     # LDC_COMPUTE_FRSZ      W                    Compute width (0-8192)
  720     # LDC_COMPUTE_FRSZ      H                    Compute height (0-8192)
    0     # LDC_INITXY            INITX                Output starting horizontal coordinate (0-8191)
    0     # LDC_INITXY            INITY                Output starting vertical coordinate (0-8191)
 1280     # LDC_INPUT_FRSZ        W                    Input frame width (0-8192)
  720     # LDC_INPUT_FRSZ        H                    Input frame height (0-8192)
   32     # LDC_BLOCK_SIZE        OBW                  Output block width (0-255)
   32     # LDC_BLOCK_SIZE        OBH                  Output block height (0-255)
    1     # LDC_BLOCK_SIZE        PIXPAD               Pixel pad (0-15)
 4096     # LDC_AB                A                    Affine Transform warp, A S16Q12
    0     # LDC_AB                B                    Affine Transform warp, B S16Q12
    0     # LDC_CD                C                    Affine Transform warp, C S16Q3
    0     # LDC_CD                D                    Affine Transform warp, D S16Q12
 4096     # LDC_EF                E                    Affine Transform warp, E S16Q12
    0     # LDC_EF                F                    Affine Transform warp, F S16Q3  
    0     # LDC_GH                G                    Affine Transform warp, G S16Q23
    0     # LDC_GH                H                    Affine Transform warp, H S16Q23
    0     # LDC_SF_W1             W1                   Width 1 (0-8191)
    0     # LDC_SF_W2             W1                   Width 2 (0-8191)
    0     # LDC_SF_W3             W1                   Width 3 (0-8191)
    0     # LDC_SF_H1             H1                   Height 1 (0-8191)
    0     # LDC_SF_H2             H2                   Height 2 (0-8191)
    0     # LDC_SF_H3             H3                   Height 3 (0-8191)
    0     # LDC_SF_EN0            EN                   Enable
    0     # LDC_BLOCK_SIZE0       OBW                  Output block width (0-255)
    0     # LDC_BLOCK_SIZE0       OBH                  Output block height (0-255)
    0     # LDC_BLOCK_SIZE0       PIXPAD               Pixel pad (0-15)
    0     # LDC_SF_EN1            EN                   Enable
    0     # LDC_BLOCK_SIZE1       OBW                  Output block width (0-255)
    0     # LDC_BLOCK_SIZE1       OBH                  Output block height (0-255)
    0     # LDC_BLOCK_SIZE1       PIXPAD               Pixel pad (0-15)
    0     # LDC_SF_EN2            EN                   Enable
    0     # LDC_BLOCK_SIZE2       OBW                  Output block width (0-255)
    0     # LDC_BLOCK_SIZE2       OBH                  Output block height (0-255)
    0     # LDC_BLOCK_SIZE2       PIXPAD               Pixel pad (0-15)
    0     # LDC_SF_EN3            EN                   Enable
    0     # LDC_BLOCK_SIZE3       OBW                  Output block width (0-255)
    0     # LDC_BLOCK_SIZE3       OBH                  Output block height (0-255)
    0     # LDC_BLOCK_SIZE3       PIXPAD               Pixel pad (0-15)
    0     # LDC_SF_EN4            EN                   Enable
    0     # LDC_BLOCK_SIZE4       OBW                  Output block width (0-255)
    0     # LDC_BLOCK_SIZE4       OBH                  Output block height (0-255)
    0     # LDC_BLOCK_SIZE4       PIXPAD               Pixel pad (0-15)
    0     # LDC_SF_EN5            EN                   Enable
    0     # LDC_BLOCK_SIZE5       OBW                  Output block width (0-255)
    0     # LDC_BLOCK_SIZE5       OBH                  Output block height (0-255)
    0     # LDC_BLOCK_SIZE5       PIXPAD               Pixel pad (0-15)
    0     # LDC_SF_EN6            EN                   Enable
    0     # LDC_BLOCK_SIZE6       OBW                  Output block width (0-255)
    0     # LDC_BLOCK_SIZE6       OBH                  Output block height (0-255)
    0     # LDC_BLOCK_SIZE6       PIXPAD               Pixel pad (0-15)
    0     # LDC_SF_EN7            EN                   Enable
    0     # LDC_BLOCK_SIZE7       OBW                  Output block width (0-255)
    0     # LDC_BLOCK_SIZE7       OBH                  Output block height (0-255)
    0     # LDC_BLOCK_SIZE7       PIXPAD               Pixel pad (0-15)
    0     # LDC_SF_EN8            EN                   Enable
    0     # LDC_BLOCK_SIZE8       OBW                  Output block width (0-255)
    0     # LDC_BLOCK_SIZE8       OBH                  Output block height (0-255)
    0     # LDC_BLOCK_SIZE8       PIXPAD               Pixel pad (0-15)
    0     # LDC_DUALOUT_CFG       YLUT_EN              Luma LUT enable (0-1)
    8     # LDC_DUALOUT_CFG       YIN_BITDPTH          Luma input bit depth (8-12)
    8     # LDC_DUALOUT_CFG       YOUT_BITDPTH         Luma output bit depth (8-12)
    0     # LDC_DUALOUT_CFG       CLUT_EN              Chroma LUT enable (0-1)
    8     # LDC_DUALOUT_CFG       CIN_BITDPTH          Chroma input bit depth (8-12)
    8     # LDC_DUALOUT_CFG       COUT_BITDPTH         Chroma output bit depth (8-12)
