


# TSMASTER HARDWARE CONFIG





# TX TEST RESULT

We have DUT to output classic CAN msg with data[0x1, 0x2, 0x3, 0x4, 0x5, 0x6, 0x7, 0x8] and TSMaster can interpret the classic CAN frame normally.



RX TEST PROCEDURE

* Load ASC file as attached XCP\_Trigger\_svnv27639\_V2.ASC.
* Play the msg but no data can be captured from ***canBus0RxQueue*** or ***canBus1RxQueue***

