Easy measurement points:

-0-
The J7 EVM EVM has INA226 (or INA231) ADCs which can be controlled via I2C. This allow high side measurements.
	TP10112, TP10113: VDD_DDR_1v1		.002 ohms
	TP10114, TP10115: VDD_CPU_AVS		.002 ohms
	TP10116, TP10117: VDD_CORE_0V8		.002 ohms
	TP2205, TP2206:   VDD_MCU_0V8		.01 ohms
	TP2207, TP2208:   VDA_MCU_1V8		.01 ohms
	TP2209, TP2210:   VDD_MCUIO_1V8		.01 ohms
	TP2211, TP2212    VDD_MCUIO_3V3		.01 ohms
	TP2217, TP2218    VDA_DLL_0V8		.01 ohms
	TP2213, TP2214    VDD_RAM_0V85		.01 ohms
	TP2221, TP2222    VDA_PLL_1V8		.01 ohms
	TP2227, TP2228    VDA_PHY_1V8		.01 ohms
	TP2233, TP2234    VDD_IO_1V8		.01 ohms
	TP2237, TP2238    VDD_IO_3V3		.01 ohms
	TP10107, TP10106  VDD_GPIORET_WK_0V8	.01 ohms
	TP2229, TP2230    VDD_GPIORET_IO_3V3	.01 ohms
	TP2235, TP2236    VDD_SD_DV		.01 ohms
	TP2237, TP2238    VDD_IO_3V3		.01 ohms
	TP2239, TP2240    VDA_USB_3V3		.01 ohms
	TP2243, TP2244    VDD1_DDR_1V8		.01 ohms
	TP2245, TP2246    VDD_MCUIO_1V8		.01 ohms
	TP2247, TP2248    VDD_MCUIO_3V3		.01 ohms
	TP2249, TP2250    VDD_IO_1V8		.01 ohms
	TP2251, TP2252    VDD_IO_3V3		.01 ohms
	R2287             VDD_GPIORET.01 ohms	.01 ohms

The sense resistors also have a jumper across them which can be used with the pi_analog probe.

-1-
Several VDDs also has a pair of through hole test points which can be used for high accuracy Kelvin sensing. 
	VDD_CORE_0V8	TP72,TP73
	VDD_CPU_AVS	TP70,TP71
	VDD_DDR_1V1	TP76,TP77
	VDD_MCU_0V85	TP74,TP75	
	VDDAR_CORE_0V85	TP78,TP79
	VDDAR_CPU_0V85	TP64,TP65	


