Scripts at this directory level
	burn_flash - provides controller-based flashing for EVM flashes.  Usually launched from bare metal
	
Other scripts at this directory level are typically used to attach to a running CPU which has already been powered and clocked.

Examples which first power and clock the CPU then load bare metal or PDK tests can be found at:
 	../x_gel_to_cmm/pdk_rtos_test/pdk_launch_freertos_r5.cmm
	../x_gel_to_cmm/_J784S4_ddr_test.cmm

