Scripts at this directory level are typically used to attach to a running CPU which has already been powered and clocked.
	Typical use is with HLOS like Linux, QNX, possibly combined with an RTOS running under a hypervisor

Scripts under onchip stream processor and system trace data into an onchip memory.  The memory typically holds some 10's of mS of information.

Scripts under the offchip stream processor and system trace date to an offchip receiver.  This memory typically holds some minutes of information.
	* Note, an LA-3505 can also stream directly to a hard drive via PowerTRACE-II/III when USB3 is connected.

Examples which first power and clock the CPU then load bare metal or PDK tests can be found at:
 	../x_gel_to_cmm/pdk_rtos_test/<>.cmm
	../x_gel_to_cmm/_J784S4_ddr_test.cmm

