generate a single common gel J7AHP_PLL_MMR_PARAMS_PLL.gel by merging files. The order is the gel load order.

 + J7AHP_PLL_MMR.gel
 + J7AHP_PLL.gel
 + J7AHP_PLL_PARAMS.gel
 + Global Helpers
 =
-----------------------------------------
J7AHP_PLL_MMR_PARAMS_PLL.gel

run the converter:
	./gel_converter J7AHP_PLL_MMR_PARAMS_PLL.gel J7AHP_PLL_MMR_PARAMS_PLL.cmm

Fix up global call outs:
	// GOSUB Turn_On_LPSC_WKUPMCU2MAIN
        DO "&path_J7AHP_PSC_cmm" Turn_On_LPSC_WKUPMCU2MAIN

If using J742S2 comment add run time check to remove setup of unused EMIF PLLs

  IF ((data.long(eaxi:0x43000018)&7)==5)  //CTRL_MMR_CFG0_JTAG_USER_IDAHP[2:0] -> 31x31 has 4 EMIFs, AHP27x27 has 2 EMIFS
  (
        PRINT "Programming Main PLL 27 (DDR2 PLL)"
	PRINT ""
	GOSUB Setup &__CSL_PLL0_CFG_BASE Var.VALUE(\address_offset) &__DDR2_PLL_INDEX &__OFC1
	PRINT "Main PLL 27 (DDR2 PLL) Set."
	PRINT ""
	PRINT "Programming Main PLL 28 (DDR3 PLL)"
	PRINT ""
	GOSUB Setup &__CSL_PLL0_CFG_BASE Var.VALUE(\address_offset) &__DDR3_PLL_INDEX &__OFC1
	PRINT "Main PLL 28 (DDR3 PLL) Set."
	PRINT ""
  )


