; set up ADC
pod ip                             ; display ADC settings
pod.adc.ip.v0 on                   ; voltage channel 0 is enable
pod.adc.ip.i0 on 1/1 always 0.010  ; differential current with a .010 ohm shunt
pod.adc.ip.p0 on                   ; enable power channel (math v0*i0)

; load up saved data
IProbe.LOAD d:\iprobe.ad

; list and draw it
IProbe.List
Iprobe.Draw

