Hi,
[bookmark: _GoBack]I am using TMS320C5515 EVM and trying to use the CSL_USB_CDCExample_Out. While running the code, the device C5515 (COM5) appeared in the device manager:
[image: ]
 but it wasn't identified by PUTTY or any other terminal except Tera Term. I got an error message:
[image: ]
I configured the baud rate, data bits and the rest properties as required. I downloaded the driver according the instructions and got:
[image: ]
In addition, before installing the .inf file I made sure that Windows signed driver requirement is turned off. (by setting the drop box to "ignore" at User Config/Admin Templ./System/Driver installation).
Would you please assist us to connect Putty to the COM PORT?
I would appreciate any help. Thanks in advance!!
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