**AM64 GP RevC MMC1 Rework**

* Install 10K resistor on R479, R480, R483, R484 and R485 in bottom side

