These scripts allow for capturing bus and core information which is exported into the trace network via the CPTRACER engine.

A typical usage would be:
 - to select an aggregator(s) and select probe(s) of interest.  
 - data will stream into an offchip receiver 'analyzer'
 - setup a trigger condition (often collect on go, and stop on break)
 - capture the data and display a report

Generic throughput, latency, and transaction reports exist.  CPtracers associated with the C7x stream DSP specific memory events
