generate a single common gel AM64_PLL_merge.gel by merging files. The order is the gel load order.

AM62_PLL_MMR.gel
+
AM62_PLL_PARAMS_OFC1.gel
+
AM62_PLL_OFC1.gel
+
AM62_PLL_non_UC_configurations.gel
+
AM62_PLL_bypass.gel
+
AM62_PLL.gel
-----------------------------------------
AM62_PLL_bp_mmr_uc_ofc1.gel


Next: Pull up globals from middle to top.

//Global definitions
#define DEBUG 	  0 //turn on this for debugging messages
#define GEL_TRACE 0 //turn this on for gel_trace debug messages

#define MAIN_PSC_BASE 		(0x00400000)
#define M3_MCU_OFFSET 		(0x80000000)
#define M3_MAIN_OFFSET 		(0x80000000)

//PLL Locations
#define CSL_PLL0_CFG_BASE 										(0x680000ul)
#define CSL_MCU_PLL0_CFG_BASE  									(0x4040000ul)

//PLL Controller Locations
#define CSL_PLLCTRL0_BASE   									(0x410000ul)
#define CSL_MCU_PLLCTRL0_BASE  								    (0x4020000ul)

#define KICK0_UNLOCK 	0x68EF3490
#define KICK1_UNLOCK 	0xD172BC5A
#define KICK_LOCK		0x00000000

#define MAIN_DOMAIN	0
#define MCU_DOMAIN	1

#define CENTER_SPREAD	0
#define DOWN_SPREAD		1

#define FRAC_PLL 		0
#define FRAC_F_PLL		1
#define DESKEW_PLL 		2

//Needed for Address Offset if running from the SMS.
unsigned int address_offset = 0;



