/*
 * Copyright (C) 2014 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 * Based on "omap4.dtsi"
 */

#include "dra7.dtsi"

/ {
	compatible = "ti,dra722", "ti,dra72", "ti,dra7";

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <0>;

			/* cooling options */
			cooling-min-level = <0>;
			cooling-max-level = <2>;
			#cooling-cells = <2>; /* min followed by max */
		};
	};

	aliases {
		rproc0 = &ipu1;
		rproc1 = &ipu2;
		rproc2 = &dsp1;
	};

	pmu {
		compatible = "arm,cortex-a15-pmu";
		interrupt-parent = <&wakeupgen>;
		interrupts = <GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>;
	};

	ocp {
		cal: cal@4845b000 {
			compatible = "ti,dra72-cal";
			ti,hwmods = "cal";
			reg = <0x4845B000 0x400>,
			      <0x4845B800 0x40>,
			      <0x4845B900 0x40>,
			      <0x4A002e94 0x4>;
			reg-names = "cal_top",
				    "cal_rx_core0",
				    "cal_rx_core1",
				    "camerrx_control";
			interrupts = <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				csi2_0: port@0 {
					reg = <0>;
				};
				csi2_1: port@1 {
					reg = <1>;
				};
			};
		};
	};
};

&scm {
	dra72_vip_mux: pinmux@4a002e8c {
		compatible = "pinctrl-single";
		reg = <0xe8c 0x4>;
		#address-cells = <1>;
		#size-cells = <0>;
		pinctrl-single,register-width = <32>;
		pinctrl-single,function-mask = <0x7f>;
	};
};

&dss {
	reg = <0x58000000 0x80>,
	      <0x58004054 0x4>,
	      <0x58004300 0x20>;
	reg-names = "dss", "pll1_clkctrl", "pll1";

	clocks = <&dss_dss_clk>,
		 <&dss_video1_clk>;
	clock-names = "fck", "video1_clk";
};

&mailbox3 {
	mbox_pru1_0: mbox_pru1_0 {
		ti,mbox-tx = <0 0 0>;
		ti,mbox-rx = <1 0 0>;
		status = "disabled";
	};
	mbox_pru1_1: mbox_pru1_1 {
		ti,mbox-tx = <2 0 0>;
		ti,mbox-rx = <3 0 0>;
		status = "disabled";
	};
};

&mailbox4 {
	mbox_pru2_0: mbox_pru2_0 {
		ti,mbox-tx = <0 0 0>;
		ti,mbox-rx = <1 0 0>;
		status = "disabled";
	};
	mbox_pru2_1: mbox_pru2_1 {
		ti,mbox-tx = <2 0 0>;
		ti,mbox-rx = <3 0 0>;
		status = "disabled";
	};
};

&mailbox5 {
	mbox_ipu1_ipc3x: mbox_ipu1_ipc3x {
		ti,mbox-tx = <6 2 2>;
		ti,mbox-rx = <4 2 2>;
		status = "disabled";
	};
	mbox_dsp1_ipc3x: mbox_dsp1_ipc3x {
		ti,mbox-tx = <5 2 2>;
		ti,mbox-rx = <1 2 2>;
		status = "disabled";
	};
};

&mailbox6 {
	mbox_ipu2_ipc3x: mbox_ipu2_ipc3x {
		ti,mbox-tx = <6 2 2>;
		ti,mbox-rx = <4 2 2>;
		status = "disabled";
	};
};
