[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 4.19.94-gbe5389fd85 (nfk@ubuntu) (gcc version 8.3.0 (GNU Toolchain for the A-profile Architecture 8.3-2019.03 (arm-rel-8.36))) #1 PREEMPT Wed Dec 23 18:10:27 CST 2020
[    0.000000] CPU: ARMv7 Processor [413fc082] revision 2 (ARMv7), cr=10c5387d
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] OF: fdt: Machine model: TI AM335x EVM-SK
[    0.000000] Memory policy: Data cache writeback
[    0.000000] efi: Getting EFI parameters from FDT:
[    0.000000] efi: UEFI not found.
[    0.000000] cma: Reserved 48 MiB at 0x9d000000
[    0.000000] On node 0 totalpages: 131072
[    0.000000]   Normal zone: 1152 pages used for memmap
[    0.000000]   Normal zone: 0 pages reserved
[    0.000000]   Normal zone: 131072 pages, LIFO batch:31
[    0.000000] CPU: All CPU(s) started in SVC mode.
[    0.000000] AM335X ES2.1 (sgx neon)
[    0.000000] random: get_random_bytes called from start_kernel+0xa4/0x434 with crng_init=0
[    0.000000] pcpu-alloc: s0 r0 d32768 u32768 alloc=1*32768
[    0.000000] pcpu-alloc: [0] 0 
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 129920
[    0.000000] Kernel command line: console=ttyO0,115200n8 root=PARTUUID=b511c40f-02 rw rootfstype=ext4 rootwait
[    0.000000] Dentry cache hash table entries: 65536 (order: 6, 262144 bytes)
[    0.000000] Inode-cache hash table entries: 32768 (order: 5, 131072 bytes)
[    0.000000] Memory: 455932K/524288K available (9216K kernel code, 307K rwdata, 2728K rodata, 1024K init, 252K bss, 19204K reserved, 49152K cma-reserved, 0K highmem)
[    0.000000] Virtual kernel memory layout:
                   vector  : 0xffff0000 - 0xffff1000   (   4 kB)
                   fixmap  : 0xffc00000 - 0xfff00000   (3072 kB)
                   vmalloc : 0xe0800000 - 0xff800000   ( 496 MB)
                   lowmem  : 0xc0000000 - 0xe0000000   ( 512 MB)
                   pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
                   modules : 0xbf000000 - 0xbfe00000   (  14 MB)
                     .text : 0x(ptrval) - 0x(ptrval)   (10208 kB)
                     .init : 0x(ptrval) - 0x(ptrval)   (1024 kB)
                     .data : 0x(ptrval) - 0x(ptrval)   ( 308 kB)
                      .bss : 0x(ptrval) - 0x(ptrval)   ( 253 kB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] rcu: Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] IRQ: Found an INTC at 0x(ptrval) (revision 5.0) with 128 interrupts
[    0.000000] OMAP clockevent source: timer2 at 24000000 Hz
[    0.000019] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 89478484971ns
[    0.000048] clocksource: timer1: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.000063] OMAP clocksource: timer1 at 24000000 Hz
[    0.000308] timer_probe: no matching timers found
[    0.000542] Console: colour dummy device 80x30
[    0.000576] WARNING: Your 'console=ttyO0' has been replaced by 'ttyS0'
[    0.000585] This ensures that you still see kernel messages. Please
[    0.000594] update your kernel commandline.
[    0.000658] Calibrating delay loop... 597.60 BogoMIPS (lpj=2988032)
[    0.118767] pid_max: default: 32768 minimum: 301
[    0.119037] Mount-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.119058] Mountpoint-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.120089] CPU: Testing write buffer coherency: ok
[    0.120169] CPU0: Spectre v2: using BPIALL workaround
[    0.121286] Setting up static identity map for 0x80100000 - 0x80100060
[    0.121488] rcu: Hierarchical SRCU implementation.
[    0.121948] EFI services will not be available.
[    0.123881] devtmpfs: initialized
[    0.136020] VFP support v0.3: implementor 41 architecture 3 part 30 variant c rev 3
[    0.136521] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.136552] futex hash table entries: 256 (order: -1, 3072 bytes)
[    0.141202] pinctrl core: initialized pinctrl subsystem
[    0.142164] DMI not present or invalid.
[    0.142713] NET: Registered protocol family 16
[    0.145867] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.176107] l4_wkup_cm:clk:0010:0: failed to disable
[    0.231250] cpuidle: using governor ladder
[    0.231303] cpuidle: using governor menu
[    0.238074] gpio gpiochip0: (gpio-0-31): added GPIO chardev (254:0)
[    0.238207] gpiochip_setup_dev: registered GPIOs 0 to 31 on device: gpiochip0 (gpio-0-31)
[    0.238262] OMAP GPIO hardware version 0.1
[    0.239447] gpio gpiochip1: (gpio-32-63): added GPIO chardev (254:1)
[    0.239568] gpiochip_setup_dev: registered GPIOs 32 to 63 on device: gpiochip1 (gpio-32-63)
[    0.240553] gpio gpiochip2: (gpio-64-95): added GPIO chardev (254:2)
[    0.240657] gpiochip_setup_dev: registered GPIOs 64 to 95 on device: gpiochip2 (gpio-64-95)
[    0.241595] gpio gpiochip3: (gpio-96-127): added GPIO chardev (254:3)
[    0.241699] gpiochip_setup_dev: registered GPIOs 96 to 127 on device: gpiochip3 (gpio-96-127)
[    0.251149] No ATAGs?
[    0.251165] hw-breakpoint: debug architecture 0x4 unsupported.
[    0.271203] edma 49000000.edma: TI EDMA DMA engine driver
[    0.271988] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/fixedregulator@0[0]'
[    0.275393] SCSI subsystem initialized
[    0.275997] media: Linux media interface: v0.10
[    0.276065] videodev: Linux video capture interface: v2.00
[    0.276203] pps_core: LinuxPPS API ver. 1 registered
[    0.276216] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.276248] PTP clock support registered
[    0.276298] EDAC MC: Ver: 3.0.0
[    0.277661] omap-mailbox 480c8000.mailbox: omap mailbox rev 0x400
[    0.278426] Advanced Linux Sound Architecture Driver Initialized.
[    0.280242] clocksource: Switched to clocksource timer1
[    0.291994] NET: Registered protocol family 2
[    0.293070] tcp_listen_portaddr_hash hash table entries: 512 (order: 0, 4096 bytes)
[    0.293115] TCP established hash table entries: 4096 (order: 2, 16384 bytes)
[    0.293180] TCP bind hash table entries: 4096 (order: 2, 16384 bytes)
[    0.293242] TCP: Hash tables configured (established 4096 bind 4096)
[    0.293372] UDP hash table entries: 256 (order: 0, 4096 bytes)
[    0.293403] UDP-Lite hash table entries: 256 (order: 0, 4096 bytes)
[    0.293610] NET: Registered protocol family 1
[    0.294356] RPC: Registered named UNIX socket transport module.
[    0.294373] RPC: Registered udp transport module.
[    0.294383] RPC: Registered tcp transport module.
[    0.294392] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.294411] PCI: CLS 0 bytes, default 64
[    0.295558] hw perfevents: enabled with armv7_cortex_a8 PMU driver, 5 counters available
[    0.297236] Initialise system trusted keyrings
[    0.297629] workingset: timestamp_bits=14 max_order=17 bucket_order=3
[    0.304563] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.305542] NFS: Registering the id_resolver key type
[    0.305594] Key type id_resolver registered
[    0.305606] Key type id_legacy registered
[    0.305667] ntfs: driver 2.1.32 [Flags: R/O].
[    0.308771] Key type asymmetric registered
[    0.308796] Asymmetric key parser 'x509' registered
[    0.308887] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.308905] io scheduler noop registered
[    0.308917] io scheduler deadline registered
[    0.309247] io scheduler cfq registered (default)
[    0.309264] io scheduler mq-deadline registered
[    0.309276] io scheduler kyber registered
[    0.311960] pinctrl-single 44e10800.pinmux: 142 pins, size 568
[    0.316442] pwm-backlight backlight: GPIO lookup for consumer enable
[    0.316459] pwm-backlight backlight: using device tree for GPIO lookup
[    0.316494] of_get_named_gpiod_flags: can't parse 'enable-gpios' property of node '/backlight[0]'
[    0.316515] of_get_named_gpiod_flags: can't parse 'enable-gpio' property of node '/backlight[0]'
[    0.316529] pwm-backlight backlight: using lookup tables for GPIO lookup
[    0.316540] pwm-backlight backlight: No GPIO consumer enable found
[    0.316570] pwm-backlight backlight: backlight supply power not found, using dummy regulator
[    0.316705] pwm-backlight backlight: Linked as a consumer to regulator.0
[    0.386000] Serial: 8250/16550 driver, 10 ports, IRQ sharing enabled
[    0.391458] 44e09000.serial: ttyS0 at MMIO 0x44e09000 (irq = 30, base_baud = 3000000) is a 8250
[    1.024500] console [ttyS0] enabled
[    1.030683] omap_rng 48310000.rng: Random Number Generator ver. 20
[    1.038767] tilcdc-panel panel: GPIO lookup for consumer enable
[    1.038781] tilcdc-panel panel: using device tree for GPIO lookup
[    1.038813] of_get_named_gpiod_flags: can't parse 'enable-gpios' property of node '/panel[0]'
[    1.038834] of_get_named_gpiod_flags: can't parse 'enable-gpio' property of node '/panel[0]'
[    1.038846] tilcdc-panel panel: using lookup tables for GPIO lookup
[    1.038857] tilcdc-panel panel: No GPIO consumer enable found
[    1.039200] OF: graph: no port node found in /ocp/lcdc@4830e000
[    1.045374] random: fast init done
[    1.049083] random: crng init done
[    1.053517] OF: graph: no port node found in /ocp/lcdc@4830e000
[    1.060065] OF: graph: no port node found in /ocp/lcdc@4830e000
[    1.066096] [drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
[    1.072763] [drm] No driver support for vblank timestamp query.
[    1.090956] Console: switching to colour frame buffer device 100x30
[    1.104739] tilcdc 4830e000.lcdc: fb0: DRM emulated frame buffer device
[    1.112135] [drm] Initialized tilcdc 1.0.0 20121205 for 4830e000.lcdc on minor 0
[    1.135221] brd: module loaded
[    1.147507] loop: module loaded
[    1.154956] mdio_bus fixed-0: GPIO lookup for consumer reset
[    1.154972] mdio_bus fixed-0: using lookup tables for GPIO lookup
[    1.154983] mdio_bus fixed-0: No GPIO consumer reset found
[    1.155015] libphy: Fixed MDIO Bus: probed
[    1.176889] mdio_bus 4a101000.mdio: GPIO lookup for consumer reset
[    1.176906] mdio_bus 4a101000.mdio: using device tree for GPIO lookup
[    1.176940] of_get_named_gpiod_flags: can't parse 'reset-gpios' property of node '/ocp/ethernet@4a100000/mdio@4a101000[0]'
[    1.176962] of_get_named_gpiod_flags: can't parse 'reset-gpio' property of node '/ocp/ethernet@4a100000/mdio@4a101000[0]'
[    1.176975] mdio_bus 4a101000.mdio: using lookup tables for GPIO lookup
[    1.176985] mdio_bus 4a101000.mdio: No GPIO consumer reset found
[    1.230341] davinci_mdio 4a101000.mdio: davinci mdio revision 1.6, bus freq 1000000
[    1.238053] davinci_mdio 4a101000.mdio: detected phy mask fffffffe
[    1.245624] libphy: 4a101000.mdio: probed
[    1.249678] davinci_mdio 4a101000.mdio: phy[0]: device 4a101000.mdio:00, driver Micrel KSZ9031 Gigabit PHY
[    1.260819] cpsw 4a100000.ethernet: No slave[1] phy_id, phy-handle, or fixed-link property
[    1.269142] cpsw 4a100000.ethernet: Detected MACID = 0c:b2:b7:a1:ed:65
[    1.275986] cpsw 4a100000.ethernet: initialized cpsw ale version 1.4
[    1.282460] cpsw 4a100000.ethernet: ALE Table size 1024
[    1.287757] cpsw 4a100000.ethernet: cpts: overflow check period 500 (jiffies)
[    1.296904] i2c /dev entries driver
[    1.303569] sdhci: Secure Digital Host Controller Interface driver
[    1.309795] sdhci: Copyright(c) Pierre Ossman
[    1.315069] omap_hsmmc 48060000.mmc: GPIO lookup for consumer cd
[    1.315082] omap_hsmmc 48060000.mmc: using device tree for GPIO lookup
[    1.315135] of_get_named_gpiod_flags: parsed 'cd-gpios' property of node '/ocp/mmc@48060000[0]' - status (0)
[    1.315231] gpio gpiochip0: Persistence not supported for GPIO 6
[    1.315253] omap_gpio 44e07000.gpio: Could not set line 6 debounce to 200000 microseconds (-22)
[    1.324066] omap_hsmmc 48060000.mmc: Got CD GPIO
[    1.328715] omap_hsmmc 48060000.mmc: GPIO lookup for consumer wp
[    1.328723] omap_hsmmc 48060000.mmc: using device tree for GPIO lookup
[    1.328749] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/ocp/mmc@48060000[0]'
[    1.328769] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/ocp/mmc@48060000[0]'
[    1.328782] omap_hsmmc 48060000.mmc: using lookup tables for GPIO lookup
[    1.328792] omap_hsmmc 48060000.mmc: No GPIO consumer wp found
[    1.329813] sdhci-pltfm: SDHCI platform and OF driver helper
[    1.336501] ledtrig-cpu: registered to indicate activity on CPUs
[    1.347991] NET: Registered protocol family 10
[    1.354410] Segment Routing with IPv6
[    1.358216] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.365258] NET: Registered protocol family 17
[    1.370081] Key type dns_resolver registered
[    1.374836] omap_voltage_late_init: Voltage driver support not added
[    1.382466] Loading compiled-in X.509 certificates
[    1.399841] omap-gpmc 50000000.gpmc: GPMC revision 6.0
[    1.405240] gpmc_mem_init: disabling cs 0 mapped at 0x0-0x1000000
[    1.411462] gpiochip_find_base: found new base at 510
[    1.411851] gpio gpiochip4: (omap-gpmc): added GPIO chardev (254:4)
[    1.411973] gpiochip_setup_dev: registered GPIOs 510 to 511 on device: gpiochip4 (omap-gpmc)
[    1.412541] ------------[ cut here ]------------
[    1.417217] WARNING: CPU: 0 PID: 16 at arch/arm/mach-omap2/omap_hwmod.c:1916 _enable+0x27c/0x284
[    1.426042] omap_hwmod: gpmc: enabled state can only be entered from initialized, idle, or disabled state
[    1.435650] Modules linked in:
[    1.438730] CPU: 0 PID: 16 Comm: kworker/0:1 Not tainted 4.19.94-gbe5389fd85 #1
[    1.446070] Hardware name: Generic AM33XX (Flattened Device Tree)
[    1.452212] Workqueue: events deferred_probe_work_func
[    1.457375] Backtrace: 
[    1.459846] [<c010cb64>] (dump_backtrace) from [<c010ced4>] (show_stack+0x18/0x1c)
[    1.467455]  r7:00000009 r6:00000000 r5:c0bc24a4 r4:dc119a64
[    1.473157] [<c010cebc>] (show_stack) from [<c091642c>] (dump_stack+0x24/0x28)
[    1.480428] [<c0916408>] (dump_stack) from [<c012ad48>] (__warn+0xe0/0xf8)
[    1.487342] [<c012ac68>] (__warn) from [<c012a988>] (warn_slowpath_fmt+0x50/0x6c)
[    1.494866]  r9:00000001 r8:dc611c00 r7:00000001 r6:00000001 r5:c0bc267c r4:c0e03048
[    1.502651] [<c012a93c>] (warn_slowpath_fmt) from [<c011c4cc>] (_enable+0x27c/0x284)
[    1.510428]  r3:c0bc3f64 r2:c0bc267c
[    1.514021]  r5:a0000013 r4:c0e0aaf8
[    1.517619] [<c011c250>] (_enable) from [<c011db48>] (omap_hwmod_enable+0x40/0x88)
[    1.525226]  r7:00000001 r6:00000001 r5:a0000013 r4:ffffe000
[    1.530920] [<c011db08>] (omap_hwmod_enable) from [<c011e74c>] (omap_device_enable+0x48/0x9c)
[    1.539483]  r5:dc66b6c0 r4:00000000
[    1.543082] [<c011e704>] (omap_device_enable) from [<c011ed5c>] (_omap_device_notifier_call+0x3f0/0x428)
[    1.552608]  r7:00000001 r6:00000001 r5:dc611c10 r4:c0e03048
[    1.558307] [<c011e96c>] (_omap_device_notifier_call) from [<c014a84c>] (notifier_call_chain+0x50/0x8c)
[    1.567749]  r10:00000000 r9:c0e830b0 r8:00000000 r7:00000001 r6:dc611c10 r5:c0e205c4
[    1.575613]  r4:ffffffff
[    1.578167] [<c014a7fc>] (notifier_call_chain) from [<c014b154>] (blocking_notifier_call_chain+0x58/0x70)
[    1.587782]  r9:c0e830b0 r8:dc611c10 r7:dc145610 r6:dc611c10 r5:dc0381ec r4:00000001
[    1.595568] [<c014b0fc>] (blocking_notifier_call_chain) from [<c05aeb9c>] (device_add+0x368/0x620)
[    1.604570]  r6:00000000 r5:c0e03048 r4:dc611c18
[    1.609225] [<c05ae834>] (device_add) from [<c07567f4>] (of_device_add+0x3c/0x44)
[    1.616748]  r10:dc611640 r9:00000000 r8:00000000 r7:dc145610 r6:00000000 r5:dcb5c4ac
[    1.624612]  r4:dc611c00
[    1.627166] [<c07567b8>] (of_device_add) from [<c0756dac>] (of_platform_device_create_pdata+0xa4/0xe0)
[    1.636523] [<c0756d08>] (of_platform_device_create_pdata) from [<c0756e00>] (of_platform_device_create+0x18/0x1c)
[    1.646921]  r7:c0e8523c r6:dc145610 r5:c0e03048 r4:dcb5c4ac
[    1.652624] [<c0756de8>] (of_platform_device_create) from [<c076e6e4>] (gpmc_probe_generic_child+0x30c/0x988)
[    1.662592] [<c076e3d8>] (gpmc_probe_generic_child) from [<c076f18c>] (gpmc_probe+0x42c/0x590)
[    1.671248]  r10:c0e42150 r9:00000000 r8:dc145610 r7:00000000 r6:dc145600 r5:c0c479ec
[    1.679112]  r4:dcb5c4ac
[    1.681669] [<c076ed60>] (gpmc_probe) from [<c05b5058>] (platform_drv_probe+0x50/0xa0)
[    1.689627]  r10:00000001 r9:c0e4216c r8:00000000 r7:00000000 r6:c0e4216c r5:00000000
[    1.697490]  r4:dc145610
[    1.700042] [<c05b5008>] (platform_drv_probe) from [<c05b3050>] (really_probe+0x204/0x2c0)
[    1.708347]  r7:00000000 r6:c0e830d8 r5:dc145610 r4:c0e830d4
[    1.714039] [<c05b2e4c>] (really_probe) from [<c05b32b0>] (driver_probe_device+0x68/0x180)
[    1.722346]  r10:c0e31a3c r9:00000000 r8:00000001 r7:c05b34c0 r6:dc145610 r5:c0e4216c
[    1.730211]  r4:dc145610 r3:00000000
[    1.733812] [<c05b3248>] (driver_probe_device) from [<c05b3564>] (__device_attach_driver+0xa4/0xc8)
[    1.742905]  r9:00000000 r8:00000001 r7:c05b34c0 r6:dc145610 r5:dc119e74 r4:c0e4216c
[    1.750691] [<c05b34c0>] (__device_attach_driver) from [<c05b106c>] (bus_for_each_drv+0x88/0xcc)
[    1.759519]  r7:c05b34c0 r6:dc119e74 r5:c0e03048 r4:00000000
[    1.765210] [<c05b0fe4>] (bus_for_each_drv) from [<c05b2dcc>] (__device_attach+0xd8/0x140)
[    1.773515]  r7:c0e31a1c r6:dc145644 r5:c0e03048 r4:dc145610
[    1.779206] [<c05b2cf4>] (__device_attach) from [<c05b35d4>] (device_initial_probe+0x14/0x18)
[    1.787775]  r8:c0e0dfcc r7:c0e31a1c r6:c0e31c30 r5:dc145610 r4:dc145610
[    1.794514] [<c05b35c0>] (device_initial_probe) from [<c05b2134>] (bus_probe_device+0x8c/0x94)
[    1.803172] [<c05b20a8>] (bus_probe_device) from [<c05b25f4>] (deferred_probe_work_func+0x68/0x94)
[    1.812176]  r7:c0e31a1c r6:c0e31a08 r5:c0e31a08 r4:dc145610
[    1.817874] [<c05b258c>] (deferred_probe_work_func) from [<c0142b08>] (process_one_work+0x210/0x430)
[    1.827051]  r7:00000000 r6:dcb3c100 r5:dc03d880 r4:c0e31a38
[    1.832743] [<c01428f8>] (process_one_work) from [<c0143020>] (worker_thread+0x2f8/0x674)
[    1.840965]  r10:c0e0dfcc r9:c0e0dfe0 r8:ffffe000 r7:c0e14a60 r6:dc03d894 r5:c0e0dfcc
[    1.848829]  r4:dc03d880
[    1.851380] [<c0142d28>] (worker_thread) from [<c0148e94>] (kthread+0x158/0x160)
[    1.858816]  r10:dc06fe78 r9:c0142d28 r8:dc03d880 r7:dc118000 r6:00000000 r5:dc0fab80
[    1.866680]  r4:dc0fabc0
[    1.869231] [<c0148d3c>] (kthread) from [<c01010e8>] (ret_from_fork+0x14/0x2c)
[    1.876486] Exception stack(0xdc119fb0 to 0xdc119ff8)
[    1.881565] 9fa0:                                     00000000 00000000 00000000 00000000
[    1.889786] 9fc0: 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000
[    1.898006] 9fe0: 00000000 00000000 00000000 00000000 00000013 00000000
[    1.904656]  r10:00000000 r9:00000000 r8:00000000 r7:00000000 r6:00000000 r5:c0148d3c
[    1.912520]  r4:dc0fab80
[    1.915063] ---[ end trace 32038a40bda8c906 ]---
[    1.920584] omap2-nand 8000000.nand: GPIO lookup for consumer rb
[    1.920598] omap2-nand 8000000.nand: using device tree for GPIO lookup
[    1.920631] of_get_named_gpiod_flags: can't parse 'rb-gpios' property of node '/ocp/gpmc@50000000/nand@0,0[0]'
[    1.920655] of_get_named_gpiod_flags: can't parse 'rb-gpio' property of node '/ocp/gpmc@50000000/nand@0,0[0]'
[    1.920669] omap2-nand 8000000.nand: using lookup tables for GPIO lookup
[    1.920680] omap2-nand 8000000.nand: No GPIO consumer rb found
[    1.920992] nand: device found, Manufacturer ID: 0x2c, Chip ID: 0xd3
[    1.927385] nand: Micron MT29F8G08ABACAWP
[    1.931474] nand: 1024 MiB, SLC, erase size: 256 KiB, page size: 4096, OOB size: 224
[    1.939302] nand: using OMAP_ECC_BCH8_CODE_HW ECC scheme
[    1.944805] 10 fixed-partitions partitions found on MTD device omap2-nand.0
[    1.951829] Creating 10 MTD partitions on "omap2-nand.0":
[    1.957264] 0x000000000000-0x000000040000 : "NAND.SPL"
[    1.963951] 0x000000040000-0x000000080000 : "NAND.SPL.backup1"
[    1.971094] 0x000000080000-0x0000000c0000 : "NAND.SPL.backup2"
[    1.978086] 0x0000000c0000-0x000000100000 : "NAND.SPL.backup3"
[    1.985192] 0x000000100000-0x000000140000 : "NAND.u-boot-spl-os"
[    1.992437] 0x000000140000-0x000000340000 : "NAND.u-boot"
[    1.999529] 0x000000340000-0x000000380000 : "NAND.u-boot-env"
[    2.006572] 0x000000380000-0x0000003c0000 : "NAND.u-boot-env.backup1"
[    2.014277] 0x0000003c0000-0x000000bc0000 : "NAND.kernel"
[    2.023226] 0x000000bc0000-0x000040000000 : "NAND.file-system"
[    2.360542] tps65910 0-002d: No interrupt support, no core IRQ
[    2.366676] tps65910-gpio tps65910-gpio: ti,en-gpio-sleep not specified
[    2.366708] gpiochip_find_base: found new base at 504
[    2.367031] gpio gpiochip5: (tps65910): added GPIO chardev (254:5)
[    2.367157] gpiochip_setup_dev: registered GPIOs 504 to 509 on device: gpiochip5 (tps65910)
[    2.368914] vrtc: supplied by vbat
[    2.376290] vio: supplied by vbat
[    2.381263] vdd1: supplied by vbat
[    2.386635] vdd2: supplied by vbat
[    2.393638] vdig1: supplied by vbat
[    2.398640] vdig2: supplied by vbat
[    2.403705] vpll: supplied by vbat
[    2.408620] vdac: supplied by vbat
[    2.413579] vaux1: supplied by vbat
[    2.418578] vaux2: supplied by vbat
[    2.423610] vaux33: supplied by vbat
[    2.428690] vmmc: supplied by vbat
[    2.433657] vbb: supplied by vbat
[    2.438394] omap_i2c 44e0b000.i2c: bus 0 rev0.11 at 400 kHz
[    2.444491] cpu cpu0: Linked as a consumer to regulator.4
[    2.450013] cpu cpu0: Dropping the link to regulator.4
[    2.455551] cpu cpu0: Linked as a consumer to regulator.4
[    2.462845] omap_hsmmc 48060000.mmc: GPIO lookup for consumer cd
[    2.462860] omap_hsmmc 48060000.mmc: using device tree for GPIO lookup
[    2.462916] of_get_named_gpiod_flags: parsed 'cd-gpios' property of node '/ocp/mmc@48060000[0]' - status (0)
[    2.463010] gpio gpiochip0: Persistence not supported for GPIO 6
[    2.463032] omap_gpio 44e07000.gpio: Could not set line 6 debounce to 200000 microseconds (-22)
[    2.471968] omap_hsmmc 48060000.mmc: Got CD GPIO
[    2.476649] omap_hsmmc 48060000.mmc: GPIO lookup for consumer wp
[    2.476658] omap_hsmmc 48060000.mmc: using device tree for GPIO lookup
[    2.476685] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/ocp/mmc@48060000[0]'
[    2.476705] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/ocp/mmc@48060000[0]'
[    2.476718] omap_hsmmc 48060000.mmc: using lookup tables for GPIO lookup
[    2.476728] omap_hsmmc 48060000.mmc: No GPIO consumer wp found
[    2.477309] omap_hsmmc 48060000.mmc: Linked as a consumer to regulator.14
[    2.512042] hctosys: unable to open rtc device (rtc0)
[    2.518430] ALSA device list:
[    2.521734]   No soundcards found.
[    2.526965] Waiting for root device PARTUUID=b511c40f-02...
[    2.562351] mmc0: host does not support reading read-only switch, assuming write-enable
[    2.572426] mmc0: new high speed SDXC card at address 0001
[    2.579295] mmcblk0: mmc0:0001 SD16G 58.4 GiB 
[    2.586029]  mmcblk0: p1 p2
[    2.639340] EXT4-fs (mmcblk0p2): warning: mounting fs with errors, running e2fsck is recommended
[    2.690052] EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Opts: (null)
[    2.698484] VFS: Mounted root (ext4 filesystem) on device 179:2.
[    2.714308] devtmpfs: mounted
[    2.719021] Freeing unused kernel memory: 1024K
[    2.724244] Run /sbin/init as init process
[    3.130162] systemd[1]: System time before build time, advancing clock.
[    3.187273] systemd[1]: systemd 239 running in system mode. (+PAM -AUDIT -SELINUX +IMA -APPARMOR +SMACK +SYSVINIT +UTMP -LIBCRYPTSETUP -GCRYPT -GNUTLS +ACL +XZ -LZ4 -SECCOMP +BLKID -ELFUTILS +KMOD -IDN2 -IDN -PCRE2 default-hierarchy=hybrid)
[    3.209659] systemd[1]: Detected architecture arm.
[    3.262911] systemd[1]: Set hostname to <am335x-evm>.
[    3.642023] systemd[1]: File /lib/systemd/system/systemd-journald.service:36 configures an IP firewall (IPAddressDeny=any), but the local system does not support BPF/cgroup based firewalling.
[    3.659374] systemd[1]: Proceeding WITHOUT firewalling in effect! (This warning is only shown for the first loaded unit using IP firewalling.)
[    3.758801] systemd[1]: /lib/systemd/system/gadget-init.service:15: Unknown lvalue 'ExecStopPre' in section 'Service'
[    4.208962] systemd[1]: Listening on Network Service Netlink Socket.
[    4.251987] systemd[1]: Listening on Journal Socket.
[    4.285447] systemd[1]: Started Dispatch Password Requests to Console Directory Watch.
[    4.331884] systemd[1]: Listening on udev Control Socket.
[    4.534168] EXT4-fs (mmcblk0p2): re-mounted. Opts: (null)
[    4.638250] cryptodev: loading out-of-tree module taints kernel.
[    4.673087] cryptodev: driver 1.9 loaded.
[    4.718482] usbcore: registered new interface driver usbfs
[    4.730669] usbcore: registered new interface driver hub
[    4.744271] usbcore: registered new device driver usb
[    4.785720] usbcore: registered new interface driver ftdi_sio
[    4.794098] usbserial: USB Serial support registered for FTDI USB Serial Device
[    6.203383] systemd-journald[78]: Received request to flush runtime journal from PID 1
[    8.630905] omap_wdt: OMAP Watchdog Timer Rev 0x01: initial timeout 60 sec
[    8.771247] omap_rtc 44e3e000.rtc: char device (253:0)
[    8.771280] omap_rtc 44e3e000.rtc: registered as rtc0
[    9.998459] omap-sham 53100000.sham: hw accel on OMAP rev 4.3
[   10.027651] omap-aes 53500000.aes: OMAP AES hw accel rev: 3.2
[   10.180992] omap-aes 53500000.aes: will run requests pump with realtime priority
[   12.043478] remoteproc remoteproc0: wkup_m3 is available
[   12.063357] net eth0: initializing cpsw version 1.12 (0)
[   12.205387] Micrel KSZ9031 Gigabit PHY 4a101000.mdio:00: attached PHY driver [Micrel KSZ9031 Gigabit PHY] (mii_bus:phy_addr=4a101000.mdio:00, irq=POLL)
[   12.438855] libphy: PHY  not found
[   12.492512] net eth0: phy "" not found on slave 1, err -19
[   12.695113] IPv6: ADDRCONF(NETDEV_UP): eth0: link is not ready
[   12.973124] remoteproc remoteproc0: powering up wkup_m3
[   12.980129] PM: Cannot get wkup_m3_ipc handle
[   13.123952] remoteproc remoteproc0: Booting fw image am335x-pm-firmware.elf, size 242888
[   13.341487] remoteproc remoteproc0: remote processor wkup_m3 is now up
[   13.341511] wkup_m3_ipc 44e11324.wkup_m3_ipc: CM3 Firmware Version = 0x192
[   13.640418] gpio gpiochip3: Persistence not supported for GPIO 21
[   14.042193] EXT4-fs error (device mmcblk0p2): ext4_mb_generate_buddy:747: group 432, block bitmap and bg descriptor inconsistent: 32254 vs 32255 free clusters
[   19.618748] TI-am335x-tsc TI-am335x-tsc.0.auto: ti,charge-delay not specified
[   19.684642] PM: bootloader does not support rtc-only!
[   19.718817] input: ti-tsc as /devices/platform/ocp/44e0d000.tscadc/TI-am335x-tsc.0.auto/input/input0
[   21.587188] am335x-phy-driver 47401300.usb-phy: GPIO lookup for consumer reset
[   21.587209] am335x-phy-driver 47401300.usb-phy: using device tree for GPIO lookup
[   21.587252] of_get_named_gpiod_flags: can't parse 'reset-gpios' property of node '/ocp/usb@47400000/usb-phy@47401300[0]'
[   21.587271] of_get_named_gpiod_flags: can't parse 'reset-gpio' property of node '/ocp/usb@47400000/usb-phy@47401300[0]'
[   21.587284] am335x-phy-driver 47401300.usb-phy: using lookup tables for GPIO lookup
[   21.587294] am335x-phy-driver 47401300.usb-phy: No GPIO consumer reset found
[   21.587304] am335x-phy-driver 47401300.usb-phy: GPIO lookup for consumer vbus-detect
[   21.587310] am335x-phy-driver 47401300.usb-phy: using device tree for GPIO lookup
[   21.587325] of_get_named_gpiod_flags: can't parse 'vbus-detect-gpios' property of node '/ocp/usb@47400000/usb-phy@47401300[0]'
[   21.587340] of_get_named_gpiod_flags: can't parse 'vbus-detect-gpio' property of node '/ocp/usb@47400000/usb-phy@47401300[0]'
[   21.587347] am335x-phy-driver 47401300.usb-phy: using lookup tables for GPIO lookup
[   21.587354] am335x-phy-driver 47401300.usb-phy: No GPIO consumer vbus-detect found
[   21.587495] am335x-phy-driver 47401300.usb-phy: 47401300.usb-phy supply vcc not found, using dummy regulator
[   21.685695] am335x-phy-driver 47401300.usb-phy: Linked as a consumer to regulator.0
[   21.775722] musb-hdrc musb-hdrc.0: MUSB HDRC host driver
[   21.855756] musb-hdrc musb-hdrc.0: new USB bus registered, assigned bus number 1
[   21.953463] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 4.19
[   22.007875] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[   22.083637] usb usb1: Product: MUSB HDRC host driver
[   22.150556] usb usb1: Manufacturer: Linux 4.19.94-gbe5389fd85 musb-hcd
[   22.157139] usb usb1: SerialNumber: musb-hdrc.0
[   22.251611] hub 1-0:1.0: USB hub found
[   22.279833] hub 1-0:1.0: 1 port detected
[   30.893623] udc-core: couldn't find an available UDC - added [g_multi] to list of pending drivers
[  128.658514] NET: Registered protocol family 15
[  128.942213] Initializing XFRM netlink socket