OMAPCONF (rev v1.72-11-g340f7dd built Fri Jul 8 19:17:16 EDT 2016)

HW Platform:
  Generic AM33XX (Flattened Device Tree)
  AM335X ES2.1 GP Device (UNKNOWN performance ZCE package (600MHz))
[ 1072.432018] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
[ 1073.441976] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
[ 1074.461973] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
  UNKNOWN POWER IC
[ 1075.481976] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
  UNKNOWN AUDIO IC

SW Build Details:
  Build:
    Version:  _____                    _____           _         _
  Kernel:
    Version: 4.4.12-g7bab2ee-dirty
    Author: root@tim-VM40B
    Toolchain: gcc version 5.3.1 20160113 (Linaro GCC 5.3-2016.02)
    Type: #8 PREEMPT
    Date: Tue Dec 20 01:44:36 EST 2016

|--------------------------------------------|
| DPLL Configuration         | DPLL_PER      |
|--------------------------------------------|
| Status                     | Locked        |
|                            |               |
| Mode                       | Lock          |
| Automatic Control          | Not Supported |
|  LPST = Low-Power STop     |               |
|  LPBP = Low-Power ByPass   |               |
|  FRBP = Fast-Relock ByPass |               |
|  MNBP = MN ByPass          |               |
|                            |               |
| Sigma-Delta Divider        | 4             |
| SELFREQDCO                 | 0             |
|                            |               |
| Ref. Frequency (MHz)       | 24.000        |
| M Multiplier Factor        | 960           |
| N Divider Factor           | 23            |
| Lock Frequency (MHz)       | 960           |
|                            |               |
| CLKOUT Output              |               |
|   Status                   | Enabled       |
|   Clock Divider            | 5             |
|   Clock Speed (MHz)        | 192           |
|                            |               |
| CLK_DCO_LDO Output         |               |
|   Status                   | Enabled       |
|   Clock Speed (MHz)        | 960           |
|                            |               |
|--------------------------------------------|

|---------------------------------------------------------------------------------------------|
| DPLL Configuration          | DPLL_CORE     | DPLL_MPU      | DPLL_DDR      | DPLL_DISP     |
|---------------------------------------------------------------------------------------------|
| Status                      | Locked        | Locked        | Locked        | Bypassed      |
|                             |               |               |               |               |
| Mode                        | Lock          | Lock          | Lock          | MNBP          |
| Automatic Control           | Not Supported | Not Supported | Not Supported | Not Supported |
|  LPBP = Low-Power ByPass    |               |               |               |               |
|  FRBP = Fast-Relock ByPass  |               |               |               |               |
|  MNBP = MN ByPass           |               |               |               |               |
| Low-Power Mode              | Disabled      | Disabled      | Disabled      | Disabled      |
|                             |               |               |               |               |
| Automatic Recalibration     | Disabled      | Disabled      | Disabled      | Disabled      |
| Clock Ramping during Relock | Disabled      | Disabled      | Disabled      | Disabled      |
| Ramping Rate (x REFCLK(s))  | 2             | 2             | 2             | 2             |
| Ramping Levels              | No Ramp       | No Ramp       | No Ramp       | No Ramp       |
|                             |               |               |               |               |
| Bypass Clock                | CLKINP        | CLKINP        | CLKINP        | CLKINP        |
| Bypass Clock Divider        |               |               |               |               |
| REGM4XEN Mode               | Disabled      | Disabled      | Disabled      | Disabled      |
|                             |               |               |               |               |
| Ref. Frequency (MHz)        | 24.000        | 24.000        | 24.000        | 24.000        |
| M Multiplier Factor         | 50            | 300           | 400           | 0             |
| N Divider Factor            | 23            | 23            | 23            | 0             |
| Lock Frequency (MHz)        | 50            | 300           | 400           | 0 (0)         |
|                             |               |               |               |               |
| M2 Output                   |               |               |               |               |
|   Status                    |               | Enabled       | Enabled       | Gated         |
|   Clock Divider             |               | 1             | 1             | 1             |
|   Clock Speed (MHz)         |               | 300           | 400           | 24 (24)       |
|                             |               |               |               |               |
| CLK_DCO_LDO Output          |               |               |               |               |
|   Status                    | Gated         |               |               |               |
|   Clock Speed (MHz)         | 100           |               |               |               |
|                             |               |               |               |               |
|                             |               |               |               |               |
| M4 Output                   |               |               |               |               |
|   Status                    | Enabled       |               |               |               |
|   Clock Divider             | 1             |               |               |               |
|   Clock Speed (MHz)         | 100           |               |               |               |
|                             |               |               |               |               |
| M5 Output                   |               |               |               |               |
|   Status                    | Gated         |               |               |               |
|   Clock Divider             | 1             |               |               |               |
|   Clock Speed (MHz)         | 100           |               |               |               |
|                             |               |               |               |               |
| M6 Output                   |               |               |               |               |
|   Status                    | Gated         |               |               |               |
|   Clock Divider             | 1             |               |               |               |
|   Clock Speed (MHz)         | 100           |               |               |               |
|---------------------------------------------------------------------------------------------|

root@am335x-evm:~#

root@am335x-evm:~# omapconf show opp
OMAPCONF (rev v1.72-11-g340f7dd built Fri Jul 8 19:17:16 EDT 2016)

HW Platform:
  Generic AM33XX (Flattened Device Tree)
  AM335X ES2.1 GP Device (UNKNOWN performance ZCE package (600MHz))
[ 1148.381987] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
[ 1149.401983] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
[ 1150.411978] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
  UNKNOWN POWER IC
[ 1151.432121] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
  UNKNOWN AUDIO IC

SW Build Details:
  Build:
    Version:  _____                    _____           _         _
  Kernel:
    Version: 4.4.12-g7bab2ee-dirty
    Author: root@tim-VM40B
    Toolchain: gcc version 5.3.1 20160113 (Linaro GCC 5.3-2016.02)
    Type: #8 PREEMPT
    Date: Tue Dec 20 01:44:36 EST 2016

/sys/devices/system/cpu/cpu0/cpufreq/scaling_governor not found, no CPUFREQ?

omapconf: temp_sensor_voltdm2sensor(): cpu not supported!!!
omapconf: temp_sensor_voltdm2sensor(): cpu not supported!!!
cpu_is_online(0): error opening /sys/devices/system/cpu/cpu0/online file!
|----------------------------------------------------------------------------|
|                      | Temperature | Voltage | Frequency | OPerating Point |
|----------------------------------------------------------------------------|
| VDD_CORE / VDD_CORE0 | NA          | NA      |           | OPP50           |
|   L3_SLOW            |             |         |  50   MHz |                 |
|   L3_FAST            |             |         |  100  MHz |                 |
|   EMIF4              |             |         |  200  MHz |                 |
|     DDR2/DDR3/mDDR   |             |         |  400  MHz |                 |
|   L4_PER             |             |         |  50   MHz |                 |
|   L4_FAST            |             |         |  100  MHz |                 |
|                      |             |         |           |                 |
| VDD_MPU / VDD_CORE1  | NA          | NA      |           | OPP50           |
|   MPU (CPU0 OFF)     |             |         |  300  MHz |                 |
|                      |             |         |           |                 |
|----------------------------------------------------------------------------|

Notes:
  (1) Module is disabled, rate may not be relevant.

/sys/devices/system/cpu/cpu0/cpufreq/scaling_governor not found, no CPUFREQ?

root@am335x-evm:~# omapconf export ctt
OMAPCONF (rev v1.72-11-g340f7dd built Fri Jul 8 19:17:16 EDT 2016)

HW Platform:
  Generic AM33XX (Flattened Device Tree)
  AM335X ES2.1 GP Device (UNKNOWN performance ZCE package (600MHz))
[ 1230.021974] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
[ 1231.041968] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
[ 1232.062121] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
  UNKNOWN POWER IC
[ 1233.081973] omap_i2c 44e0b000.i2c: timeout waiting for bus ready
Error: I2C Read failed
  UNKNOWN AUDIO IC

SW Build Details:
  Build:
    Version:  _____                    _____           _         _
  Kernel:
    Version: 4.4.12-g7bab2ee-dirty
    Author: root@tim-VM40B
    Toolchain: gcc version 5.3.1 20160113 (Linaro GCC 5.3-2016.02)
    Type: #8 PREEMPT
    Date: Tue Dec 20 01:44:36 EST 2016

The Clock Tree Tool can import register settings from a *.rd1 file.
The format of the *.rd1 file is:

DeviceName AM335x1.0
<register address> <register value>
<register address> <register value>
...

Copy the below output between the begin and end separators into a
file with the extension *.rd1 and this file can be read by the
Clock Tree Tool

|--------------------------- ctt dump begin ----------------------|
DeviceName AM335x1.0
0x44E00000 0x00004102
0x44E00004 0x0000000A
0x44E00008 0x00000102
0x44E0000C 0x00000016
0x44E00010 0x00070000
0x44E00014 0x00070000
0x44E00018 0x00070000
0x44E0001C 0x00000002
0x44E00020 0x00070000
0x44E00024 0x00000002
0x44E00028 0x00000002
0x44E0002C 0x00000002
0x44E00030 0x00000002
0x44E00034 0x00030000
0x44E00038 0x00030000
0x44E0003C 0x00030000
0x44E00040 0x00030000
0x44E00044 0x00030000
0x44E00048 0x00030000
0x44E0004C 0x00030000
0x44E00050 0x00030000
0x44E00054 0x00030000
0x44E00058 0x00030000
0x44E00060 0x00000002
0x44E00064 0x00000002
0x44E00068 0x00030000
0x44E0006C 0x00030000
0x44E00070 0x00030000
0x44E00074 0x00030000
0x44E00078 0x00030000
0x44E0007C 0x00030000
0x44E00080 0x00000002
0x44E00084 0x00030000
0x44E00088 0x00030000
0x44E0008C 0x00030000
0x44E00090 0x00000002
0x44E00094 0x00030000
0x44E00098 0x00030000
0x44E0009C 0x00030000
0x44E000A0 0x00030000
0x44E000A4 0x00030000
0x44E000A8 0x00030000
0x44E000AC 0x00030000
0x44E000B0 0x00000002
0x44E000B4 0x00030000
0x44E000B8 0x00030000
0x44E000BC 0x00000002
0x44E000C0 0x00030000
0x44E000C4 0x00030000
0x44E000C8 0x00030000
0x44E000CC 0x00030000
0x44E000D0 0x00000002
0x44E000D4 0x00000002
0x44E000D8 0x00000002
0x44E000DC 0x00000002
0x44E000E0 0x00000002
0x44E000E4 0x00070000
0x44E000E8 0x00070000
0x44E000EC 0x00030000
0x44E000F0 0x00030000
0x44E000F4 0x00030000
0x44E000F8 0x00030000
0x44E000FC 0x00000002
0x44E00100 0x00000002
0x44E00104 0x00030000
0x44E0010C 0x00030000
0x44E00110 0x00000002
0x44E0011C 0x0000000A
0x44E00120 0x00000002
0x44E00124 0x00070000
0x44E00128 0x00030000
0x44E0012C 0x00000012
0x44E00130 0x00040002
0x44E00134 0x00030000
0x44E00138 0x00030000
0x44E0013C 0x00030000
0x44E00140 0x00000001
0x44E00144 0x00000001
0x44E00148 0x00000001
0x44E0014C 0x00030000
0x44E00150 0x00000001
0x44E00400 0x00007E16
0x44E00404 0x00000002
0x44E00408 0x00030000
0x44E0040C 0x00000002
0x44E00410 0x00000002
0x44E00414 0x52500002
0x44E00418 0x0000001A
0x44E0041C 0x00000000
0x44E00420 0x00000001
0x44E00424 0x00000000
0x44E00428 0x00000000
0x44E0042C 0x00012C17
0x44E00430 0x00000000
0x44E00434 0x00000001
0x44E00438 0x00000000
0x44E0043C 0x00000000
0x44E00440 0x00019017
0x44E00444 0x00000000
0x44E00448 0x00000100
0x44E0044C 0x00000000
0x44E00450 0x00000000
0x44E00454 0x00000000
0x44E00458 0x00000000
0x44E0045C 0x00000001
0x44E00460 0x00000000
0x44E00464 0x00000000
0x44E00468 0x00003217
0x44E0046C 0x00000000
0x44E00470 0x00000001
0x44E00474 0x00000000
0x44E00478 0x00000000
0x44E0047C 0x00000300
0x44E00480 0x00000221
0x44E00484 0x00000021
0x44E00488 0x00000007
0x44E0048C 0x00000007
0x44E00490 0x00000007
0x44E00494 0x00000007
0x44E00498 0x00000004
0x44E0049C 0x0403C017
0x44E004A0 0x00000201
0x44E004A4 0x00000001
0x44E004A8 0x00000201
0x44E004AC 0x00000285
0x44E004B0 0x00040002
0x44E004B4 0x00000002
0x44E004B8 0x00000002
0x44E004BC 0x00000002
0x44E004C0 0x00030000
0x44E004C4 0x00000002
0x44E004C8 0x00030000
0x44E004CC 0x00000006
0x44E004D0 0x00000002
0x44E004D4 0x00030000
0x44E00504 0x00000001
0x44E00508 0x00000001
0x44E0050C 0x00000001
0x44E00510 0x00000001
0x44E00514 0x00000004
0x44E00518 0x00000001
0x44E0051C 0x00000001
0x44E00520 0x00000000
0x44E00528 0x00000000
0x44E0052C 0x00000000
0x44E00530 0x00000000
0x44E00534 0x00000000
0x44E00538 0x00000001
0x44E0053C 0x00000000
0x44E00600 0x00000006
0x44E00604 0x00000002
0x44E00700 0x00000080
0x44E00800 0x00000002
0x44E00804 0x00000302
0x44E00900 0x00000002
0x44E00904 0x00070000
0x44E00908 0x00070000
0x44E0090C 0x00000002
0x44E00910 0x00030000
0x44E00914 0x00030000
0x44E00A00 0x00000002
0x44E00A20 0x00030000
0x44E00B00 0x00000000
0x44E00B04 0x00000500
0x44E00B08 0x00000000
0x44E00B0C 0x00000100
0x44E00B10 0x00000000
0x44E00C00 0x00000003
0x44E00C04 0x00000000
0x44E00C08 0x01E60007
0x44E00C0C 0xEE0000EB
0x44E00D00 0x00000000
0x44E00D04 0x00000008
0x44E00D08 0x00000000
0x44E00D0C 0x00000020
0x44E00E00 0x01FF0007
0x44E00E04 0x000003F7
0x44E00E08 0x00000000
0x44E00F00 0x00000000
0x44E00F04 0x00001006
0x44E00F08 0x00000001
0x44E00F0C 0x78000017
0x44E00F10 0x00000003
0x44E00F14 0x00000000
0x44E00F18 0x00000003
0x44E00F1C 0x00000000
0x44E01000 0x00000004
0x44E01004 0x00000000
0x44E01100 0x00060047
0x44E01104 0x00000001
0x44E01110 0x00000037
0x44E01114 0x00000000
0x44E01200 0x00000003
0x44E01204 0x00000007
0x44E10040 0x004003F7
|---------------------------- ctt dump end -----------------------|

root@am335x-evm:~#