?
U-Boot SPL 2018.01-g313dcd69c2 (Dec 16 2018 - 10:41:59)
DRA752-GP ES2.0
Trying to boot from MMC1
no pinctrl state for default mode
no pinctrl state for default mode
Card did not respond to voltage select!
*** Warning - MMC init failed, using default environment



U-Boot 2018.01-00558-gca1e85ecb5-dirty (Sep 02 2019 - 17:04:47 +0800)

CPU  : DRA752-GP ES2.0
Model: TI AM5728 BeagleBoard-X15
Board: AM572x EVM REV A.3A
DRAM:  2 GiB
MMC:   OMAP SD/MMC: 0, OMAP SD/MMC: 1
Card did not respond to voltage select!
*** Warning - MMC init failed, using default environment

cm- name:AM572PM_ version:A.3A serial17184P551893 config: mac:C6FE35163A2
Card did not respond to voltage select!
invalid mmc device
SCSI:  SATA link 0 timeout.
AHCI 0001.0300 32 slots 1 ports 3 Gbps 0x1 impl SATA mode
flags: 64bit ncq stag pm led clo only pmp pio slum part ccc apst
scanning bus for devices...
Found 0 device(s).
Net:
Warning: ethernet@48484000 using MAC address from ROM
eth0: ethernet@48484000
Hit any key to stop autoboot:  0
switch to partitions #0, OK
mmc0 is current device
SD/MMC found on device 0
** Unable to read file boot.scr **
1490 bytes read in 2 ms (727.5 KiB/s)
Loaded env from uEnv.txt
Importing environment from mmc0 ...
Running uenvcmd ...
1 bytes read in 1 ms (1000 Bytes/s)
Already setup.
switch to partitions #0, OK
mmc0 is current device
SD/MMC found on device 0
4026880 bytes read in 239 ms (16.1 MiB/s)
147682 bytes read in 46 ms (3.1 MiB/s)
## Flattened Device Tree blob at 88000000
   Booting using the fdt blob at 0x88000000
   Loading Device Tree to 8ffd8000, end 8ffff0e1 ... OK

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 4.14.79-gbde58ab01e (oe-user@oe-host) (gcc version 7.2.1 20171011 (Linaro GCC 7.2-2017.11)) #1 SMP PREEMPT Thu Dec 20 04:51:24 UTC 2018
[    0.000000] CPU: ARMv7 Processor [412fc0f2] revision 2 (ARMv7), cr=30c5387d
[    0.000000] CPU: div instructions available: patching division code
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, PIPT instruction cache
[    0.000000] OF: fdt: Machine model: TI AM5728 EVM
[    0.000000] Memory policy: Data cache writealloc
[    0.000000] efi: Getting EFI parameters from FDT:
[    0.000000] efi: UEFI not found.
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000095800000, size 56 MiB
[    0.000000] OF: reserved mem: initialized node ipu2-memory@95800000, compatible id shared-dma-pool
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000099000000, size 64 MiB
[    0.000000] OF: reserved mem: initialized node dsp1-memory@99000000, compatible id shared-dma-pool
[    0.000000] Reserved memory: created CMA memory pool at 0x000000009d000000, size 32 MiB
[    0.000000] OF: reserved mem: initialized node ipu1-memory@9d000000, compatible id shared-dma-pool
[    0.000000] Reserved memory: created CMA memory pool at 0x000000009f000000, size 8 MiB
[    0.000000] OF: reserved mem: initialized node dsp2-memory@9f000000, compatible id shared-dma-pool
[    0.000000] cma: Reserved 24 MiB at 0x00000000fe400000
[    0.000000] OMAP4: Map 0x00000000ffd00000 to fe600000 for dram barrier
[    0.000000] DRA752 ES2.0
[    0.000000] percpu: Embedded 15 pages/cpu @eed29000 s31372 r8192 d21876 u61440
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 472640
[    0.000000] Kernel command line: console=ttyO2,115200n8 root=PARTUUID=07b1c964-02 rw rootfstype=ext4 rootwait
[    0.000000] PID hash table entries: 4096 (order: 2, 16384 bytes)
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes)
[    0.000000] Memory: 1675572K/1897472K available (8192K kernel code, 347K rwdata, 2628K rodata, 2048K init, 282K bss, 33484K reserved, 188416K cma-reserved, 1283072K highmem)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
[    0.000000]     fixmap  : 0xffc00000 - 0xfff00000   (3072 kB)
[    0.000000]     vmalloc : 0xf0800000 - 0xff800000   ( 240 MB)
[    0.000000]     lowmem  : 0xc0000000 - 0xf0000000   ( 768 MB)
[    0.000000]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
[    0.000000]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)
[    0.000000]       .text : 0xc0008000 - 0xc0a00000   (10208 kB)
[    0.000000]       .init : 0xc0e00000 - 0xc1000000   (2048 kB)
[    0.000000]       .data : 0xc1000000 - 0xc1056e98   ( 348 kB)
[    0.000000]        .bss : 0xc1058000 - 0xc109ebe0   ( 283 kB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=2, Nodes=1
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] GIC: Using split EOI/Deactivate mode
[    0.000000] OMAP clockevent source: timer1 at 32786 Hz
[    0.000000] arch_timer: cp15 timer(s) running at 6.14MHz (phys).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x16af5adb9, max_idle_ns: 440795202250 ns
[    0.000005] sched_clock: 56 bits at 6MHz, resolution 162ns, wraps every 4398046511023ns
[    0.000017] Switching to timer-based delay loop, resolution 162ns
[    0.000360] clocksource: 32k_counter: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 58327039986419 ns
[    0.000369] OMAP clocksource: 32k_counter at 32768 Hz
[    0.000880] Console: colour dummy device 80x30
[    0.000896] WARNING: Your 'console=ttyO2' has been replaced by 'ttyS2'
[    0.000904] This ensures that you still see kernel messages. Please
[    0.000911] update your kernel commandline.
[    0.000932] Calibrating delay loop (skipped), value calculated using timer frequency.. 12.29 BogoMIPS (lpj=61475)
[    0.000947] pid_max: default: 32768 minimum: 301
[    0.001064] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.001077] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.001602] CPU: Testing write buffer coherency: ok
[    0.001638] CPU0: Spectre v2: using ICIALLU workaround
[    0.001832] /cpus/cpu@0 missing clock-frequency property
[    0.001851] /cpus/cpu@1 missing clock-frequency property
[    0.001863] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000
[    0.039851] Setting up static identity map for 0x80200000 - 0x80200060
[    0.059861] Hierarchical SRCU implementation.
[    0.080048] EFI services will not be available.
[    0.099918] smp: Bringing up secondary CPUs ...
[    0.170286] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001
[    0.170291] CPU1: Spectre v2: using ICIALLU workaround
[    0.170392] smp: Brought up 1 node, 2 CPUs
[    0.170403] SMP: Total of 2 processors activated (24.59 BogoMIPS).
[    0.170411] CPU: All CPU(s) started in HYP mode.
[    0.170418] CPU: Virtualization extensions available.
[    0.170947] devtmpfs: initialized
[    0.191760] random: get_random_u32 called from bucket_table_alloc+0x108/0x230 with crng_init=0
[    0.192012] VFP support v0.3: implementor 41 architecture 4 part 30 variant f rev 0
[    0.192209] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.192226] futex hash table entries: 512 (order: 3, 32768 bytes)
[    0.195983] pinctrl core: initialized pinctrl subsystem
[    0.196432] DMI not present or invalid.
[    0.196691] NET: Registered protocol family 16
[    0.197730] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.198682] omap_hwmod: l3_main_2 using broken dt data from ocp
[    0.308141] omap_hwmod: dcan1: _wait_target_disable failed
[    0.406788] cpuidle: using governor ladder
[    0.406820] cpuidle: using governor menu
[    0.415529] OMAP GPIO hardware version 0.1
[    0.444249] No ATAGs?
[    0.444323] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.444337] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.444731] omap4_sram_init:Unable to allocate sram needed to handle errata I688
[    0.444742] omap4_sram_init:Unable to get sram pool needed to handle errata I688
[    0.445279] OMAP DMA hardware revision 0.0
[    0.455074] edma 43300000.edma: memcpy is disabled
[    0.458313] edma 43300000.edma: TI EDMA DMA engine driver
[    0.465134] omap-dma-engine 4a056000.dma-controller: OMAP DMA engine driver (LinkedList1/2/3 supported)
[    0.466472] evm_5v0: supplied by main_12v0
[    0.466897] com_3v6: supplied by evm_5v0
[    0.469940] omap-iommu 40d01000.mmu: 40d01000.mmu registered
[    0.470145] omap-iommu 40d02000.mmu: 40d02000.mmu registered
[    0.470383] omap-iommu 58882000.mmu: 58882000.mmu registered
[    0.470656] omap-iommu 55082000.mmu: 55082000.mmu registered
[    0.471018] omap-iommu 41501000.mmu: 41501000.mmu registered
[    0.471225] omap-iommu 41502000.mmu: 41502000.mmu registered
[    0.471485] iommu: Adding device 58820000.ipu to group 1
[    0.471573] iommu: Adding device 55020000.ipu to group 2
[    0.471736] iommu: Adding device 40800000.dsp to group 0
[    0.472009] iommu: Adding device 41000000.dsp to group 3
[    0.474281] palmas 0-0058: Irq flag is 0x00000008
[    0.502716] palmas 0-0058: Muxing GPIO 2b, PWM 0, LED 0
[    0.504214] SMPS12: supplied by regulator-dummy
[    0.505891] SMPS3: supplied by regulator-dummy
[    0.507538] SMPS45: supplied by regulator-dummy
[    0.509361] SMPS6: supplied by regulator-dummy
[    0.510769] SMPS7: supplied by regulator-dummy
[    0.512177] SMPS8: supplied by regulator-dummy
[    0.513444] SMPS9: supplied by regulator-dummy
[    0.514175] LDO1: supplied by regulator-dummy
[    0.521320] LDO2: supplied by regulator-dummy
[    0.521779] random: fast init done
[    0.531189] LDO3: supplied by regulator-dummy
[    0.541203] LDO4: supplied by regulator-dummy
[    0.551230] LDO5: supplied by regulator-dummy
[    0.551962] LDO6: supplied by regulator-dummy
[    0.552685] LDO7: supplied by regulator-dummy
[    0.553412] LDO8: supplied by regulator-dummy
[    0.554151] LDO9: supplied by regulator-dummy
[    0.561261] LDOLN: supplied by regulator-dummy
[    0.571278] LDOUSB: supplied by regulator-dummy
[    0.583959] omap_i2c 48070000.i2c: bus 0 rev0.12 at 400 kHz
[    0.584516] omap_i2c 48060000.i2c: bus 2 rev0.12 at 400 kHz
[    0.585037] omap_i2c 4807c000.i2c: bus 4 rev0.12 at 400 kHz
[    0.585238] media: Linux media interface: v0.10
[    0.585275] Linux video capture interface: v2.00
[    0.585354] pps_core: LinuxPPS API ver. 1 registered
[    0.585363] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.585381] PTP clock support registered
[    0.585407] EDAC MC: Ver: 3.0.0
[    0.590715] dmi: Firmware registration failed.
[    0.591118] omap-mailbox 48840000.mailbox: omap mailbox rev 0x400
[    0.591393] omap-mailbox 48842000.mailbox: omap mailbox rev 0x400
[    0.591736] Advanced Linux Sound Architecture Driver Initialized.
[    0.600789] clocksource: Switched to clocksource arch_sys_counter
[    0.608654] NET: Registered protocol family 2
[    0.609176] TCP established hash table entries: 8192 (order: 3, 32768 bytes)
[    0.609240] TCP bind hash table entries: 8192 (order: 4, 65536 bytes)
[    0.609366] TCP: Hash tables configured (established 8192 bind 8192)
[    0.609432] UDP hash table entries: 512 (order: 2, 16384 bytes)
[    0.609467] UDP-Lite hash table entries: 512 (order: 2, 16384 bytes)
[    0.609592] NET: Registered protocol family 1
[    0.609877] RPC: Registered named UNIX socket transport module.
[    0.609888] RPC: Registered udp transport module.
[    0.609896] RPC: Registered tcp transport module.
[    0.609904] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.610882] hw perfevents: no interrupt-affinity property for /pmu, guessing.
[    0.611058] hw perfevents: enabled with armv7_cortex_a15 PMU driver, 7 counters available
[    0.612080] workingset: timestamp_bits=14 max_order=19 bucket_order=5
[    0.616116] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.616601] NFS: Registering the id_resolver key type
[    0.616625] Key type id_resolver registered
[    0.616634] Key type id_legacy registered
[    0.616675] ntfs: driver 2.1.32 [Flags: R/O].
[    0.617976] bounce: pool size: 64 pages
[    0.618024] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.618034] io scheduler noop registered
[    0.618043] io scheduler deadline registered
[    0.618134] io scheduler cfq registered (default)
[    0.618144] io scheduler mq-deadline registered
[    0.618153] io scheduler kyber registered
[    0.622721] pinctrl-single 4a003400.pinmux: 282 pins at pa fc003400 size 1128
[    0.626073] dra7-pcie 51000000.pcie: Linked as a consumer to phy-4a094000.pciephy.1
[    0.626439] OF: PCI: host bridge /ocp/axi@0/pcie@51000000 ranges:
[    0.626474] OF: PCI:    IO 0x20003000..0x20012fff -> 0x00000000
[    0.626496] OF: PCI:   MEM 0x20013000..0x2fffffff -> 0x20013000
[    1.626774] dra7-pcie 51000000.pcie: phy link never came up
[    1.626907] dra7-pcie 51000000.pcie: PCI host bridge to bus 0000:00
[    1.626921] pci_bus 0000:00: root bus resource [bus 00-ff]
[    1.626932] pci_bus 0000:00: root bus resource [io  0x0000-0xffff]
[    1.626944] pci_bus 0000:00: root bus resource [mem 0x20013000-0x2fffffff]
[    1.627254] PCI: bus0: Fast back to back transfers disabled
[    1.627344] PCI: bus1: Fast back to back transfers enabled
[    1.627381] pci 0000:00:00.0: BAR 0: assigned [mem 0x20100000-0x201fffff 64bit]
[    1.627399] pci 0000:00:00.0: PCI bridge to [bus 01-ff]
[    1.627713] pcieport 0000:00:00.0: Signaling PME with IRQ 174
[    1.627836] pcieport 0000:00:00.0: AER enabled with IRQ 174
[    1.628732] pwm-backlight backlight: backlight supply power not found, using dummy regulator
[    1.631600] vdd_3v3: supplied by regen1
[    1.631862] aic_dvdd_fixed: supplied by vdd_3v3
[    1.631937] vtt_fixed: supplied by smps3
[    1.674408] Serial: 8250/16550 driver, 10 ports, IRQ sharing disabled
[    1.677085] 48020000.serial: ttyS2 at MMIO 0x48020000 (irq = 45, base_baud = 3000000) is a 8250
[    2.784256] console [ttyS2] enabled
[    2.788573] 48422000.serial: ttyS7 at MMIO 0x48422000 (irq = 46, base_baud = 3000000) is a 8250
[    2.799273] omap_rng 48090000.rng: Random Number Generator ver. 20
[    2.806396] DSS: OMAP DSS rev 6.1
[    2.811442] omapdss_dss 58000000.dss: bound 58001000.dispc (ops dispc_component_ops)
[    2.819853] omapdss_dss 58000000.dss: bound 58040000.encoder (ops hdmi5_component_ops)
[    2.830277] panel-dpi display: display supply vcc not found, using dummy regulator
[    2.848380] brd: module loaded
[    2.856857] loop: module loaded
[    2.863158] libphy: Fixed MDIO Bus: probed
[    2.920820] davinci_mdio 48485000.mdio: davinci mdio revision 1.6, bus freq 1000000
[    2.928515] libphy: 48485000.mdio: probed
[    2.936478] davinci_mdio: probe of 48485000.mdio failed with error -5
[    2.943488] cpsw 48484000.ethernet: Detected MACID = d8:a9:8b:41:ab:5a
[    2.950102] cpsw 48484000.ethernet: initialized cpsw ale version 1.4
[    2.956508] cpsw 48484000.ethernet: ALE Table size 1024
[    2.961786] cpsw 48484000.ethernet: device node lookup for pps timer failed
[    2.968812] cpsw 48484000.ethernet: cpts: overflow check period 500 (jiffies)
[    2.976717] cpsw 48484000.ethernet: cpsw: Detected MACID = d8:a9:8b:41:ab:5b
[    2.984979] i2c /dev entries driver
[    2.989433] IR NEC protocol handler initialized
[    2.994010] IR RC5(x/sz) protocol handler initialized
[    2.999084] IR RC6 protocol handler initialized
[    3.003652] IR JVC protocol handler initialized
[    3.008202] IR Sony protocol handler initialized
[    3.012858] IR SANYO protocol handler initialized
[    3.017582] IR Sharp protocol handler initialized
[    3.022324] IR MCE Keyboard/mouse protocol handler initialized
[    3.028182] IR XMP protocol handler initialized
[    3.035184] gpio-fan gpio_fan: GPIO fan initialized
[    3.040748] tmp102 0-0048: error reading config register
[    3.046240] tmp102: probe of 0-0048 failed with error -121
[    3.056065] sdhci: Secure Digital Host Controller Interface driver
[    3.062356] sdhci: Copyright(c) Pierre Ossman
[    3.067685] sdhci-pltfm: SDHCI platform and OF driver helper
[    3.074174] sdhci-omap 4809c000.mmc: Got CD GPIO
[    3.079559] sdhci-omap 4809c000.mmc: no pinctrl state for ddr_1_8v mode
[    3.086253] sdhci-omap 4809c000.mmc: no pinctrl state for hs200_1_8v mode
[    3.151018] mmc0: SDHCI controller on 4809c000.mmc [4809c000.mmc] using ADMA
[    3.220830] mmc1: SDHCI controller on 480b4000.mmc [480b4000.mmc] using ADMA
[    3.233729] sdhci-omap 480ad000.mmc: no pinctrl state for sdr104 mode
[    3.240309] sdhci-omap 480ad000.mmc: no pinctrl state for ddr50 mode
[    3.246829] sdhci-omap 480ad000.mmc: no pinctrl state for hs200_1_8v mode
[    3.289801] mmc0: host does not support reading read-only switch, assuming write-enable
[    3.301191] ti-iodelay 4844a000.padconf: Set reg 0x618 Delay(a: 1076 g: 330), Elements(C=2 F=7)0x29047
[    3.310544] ti-iodelay 4844a000.padconf: Set reg 0x620 Delay(a: 1271 g: 0), Elements(C=2 F=7)0x29047
[    3.310840] mmc2: SDHCI controller on 480ad000.mmc [480ad000.mmc] using PIO
[    3.319793] ledtrig-cpu: registered to indicate activity on CPUs
[    3.330300] NET: Registered protocol family 10
[    3.340912] ti-iodelay 4844a000.padconf: Set reg 0x624 Delay(a: 722 g: 0), Elements(C=1 F=6)0x29026
[    3.341142] Segment Routing with IPv6
[    3.341200] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    3.341659] NET: Registered protocol family 17
[    3.341865] Key type dns_resolver registered
[    3.341978] omap_voltage_late_init: Voltage driver support not added
[    3.341981] Power Management for TI OMAP4+ devices.
[    3.342207] Registering SWP/SWPB emulation handler
[    3.364808] dmm 4e000000.dmm: workaround for errata i878 in use
[    3.375852] dmm 4e000000.dmm: initialized all PAT entries
[    3.398534] ti-iodelay 4844a000.padconf: Set reg 0x628 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.407468] ti-iodelay 4844a000.padconf: Set reg 0x62c Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.416416] ti-iodelay 4844a000.padconf: Set reg 0x630 Delay(a: 751 g: 0), Elements(C=1 F=6)0x29026
[    3.425582] ti-iodelay 4844a000.padconf: Set reg 0x634 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.426515] [drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
[    3.426519] [drm] No driver support for vblank timestamp query.
[    3.434620] [drm] Enabling DMM ywrap scrolling
[    3.451998] ti-iodelay 4844a000.padconf: Set reg 0x638 Delay(a: 20 g: 0), Elements(C=0 F=0)0x29000
[    3.452008] ti-iodelay 4844a000.padconf: Set reg 0x63c Delay(a: 256 g: 0), Elements(C=0 F=6)0x29006
[    3.452016] ti-iodelay 4844a000.padconf: Set reg 0x640 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.452025] ti-iodelay 4844a000.padconf: Set reg 0x644 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.452034] ti-iodelay 4844a000.padconf: Set reg 0x648 Delay(a: 263 g: 0), Elements(C=0 F=7)0x29007
[    3.452043] ti-iodelay 4844a000.padconf: Set reg 0x64c Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.452051] ti-iodelay 4844a000.padconf: Set reg 0x650 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.452058] ti-iodelay 4844a000.padconf: Set reg 0x654 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.452066] ti-iodelay 4844a000.padconf: Set reg 0x658 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.452073] ti-iodelay 4844a000.padconf: Set reg 0x65c Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.452119] mmc0: new ultra high speed DDR50 SDHC card at address aaaa
[    3.452603] mmcblk0: mmc0:aaaa SL08G 7.40 GiB
[    3.453967]  mmcblk0: p1 p2
[    3.522102] Console: switching to colour frame buffer device 100x30
[    3.643716] omapdrm omapdrm.0: fb0: omapdrm frame buffer device
[    3.650471] [drm] Initialized omapdrm 1.0.0 20110917 for omapdrm.0 on minor 0
[    3.658825] input: gpio_keys as /devices/platform/gpio_keys/input/input0
[    3.666152] hctosys: unable to open rtc device (rtc0)
[    3.671958] aic_dvdd_fixed: disabling
[    3.676009] ldousb: disabling
[    3.679452] ALSA device list:
[    3.682444]   No soundcards found.
[    6.704183] EXT4-fs (mmcblk0p2): warning: mounting fs with errors, running e2fsck is recommended
[    6.715118] EXT4-fs (mmcblk0p2): recovery complete
[    6.721366] EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Opts: (null)
[    6.729532] VFS: Mounted root (ext4 filesystem) on device 179:2.
[    6.738292] devtmpfs: mounted
[    6.742213] Freeing unused kernel memory: 2048K
[    6.911298] systemd[1]: System time before build time, advancing clock.
[    6.941384] systemd[1]: systemd 234 running in system mode. (+PAM -AUDIT -SELINUX +IMA -APPARMOR +SMACK +SYSVINIT +UTMP -LIBCRYPTSETUP -GCRYPT -GNUTLS +ACL +XZ -LZ4 -SECCOMP +BLKID -ELFUTILS +KMOD -IDN2 -IDN default-hierarchy=hybrid)
[    6.962910] systemd[1]: Detected architecture arm.

Welcome to Arago 2018.10!

[    7.001556] systemd[1]: Set hostname to <am57xx-evm>.
[    7.266720] random: systemd: uninitialized urandom read (16 bytes read)
[    7.273549] systemd[1]: Listening on Network Service Netlink Socket.
[  OK  ] Listening on Network Service Netlink Socket.
[    7.310929] random: systemd: uninitialized urandom read (16 bytes read)
[    7.317608] systemd[1]: Reached target Remote File Systems.
[  OK  ] Reached target Remote File Systems.
[    7.351079] random: systemd: uninitialized urandom read (16 bytes read)
[    7.358205] systemd[1]: Started Forward Password Requests to Wall Directory Watch.
[  OK  ] Started Forward Password Requests to Wall Directory Watch.
[    7.401216] systemd[1]: Listening on udev Kernel Socket.
[  OK  ] Listening on udev Kernel Socket.
[    7.430990] systemd[1]: Listening on Syslog Socket.
[  OK  ] Listening on Syslog Socket.
[    7.460993] systemd[1]: Listening on Journal Socket.
[  OK  ] Listening on Journal Socket.
[    7.493189] systemd[1]: Created slice User and Session Slice.
[  OK  ] Created slice User and Session Slice.
[  OK  ] Reached target Swap.
[  OK  ] Listening on /dev/initctl Compatibility Named Pipe.
[  OK  ] Listening on udev Control Socket.
[  OK  ] Listening on Journal Socket (/dev/log).
[  OK  ] Created slice System Slice.
[  OK  ] Created slice system-getty.slice.
         Mounting Temporary Directory (/tmp)...
[  OK  ] Reached target Slices.
         Starting Load Kernel Modules...
         Starting Remount Root and Kernel File Systems...
[    7.797292] cmemk: loading out-of-tree module taints kernel.
[    7.805368] CMEMK module: reference Linux version 4.14.79
[    7.811600] allocated heap buffer 0x40500000 of size 0x100000
[    7.817426] cmemk initialized
         Mounting Kernel Debug File System...
[    7.827362] EXT4-fs (mmcblk0p2): re-mounted. Opts: (null)
[    7.845742] cryptodev: driver 1.9 loaded.
         Mounting POSIX Message Queue File System...
[    7.873090] usbcore: registered new interface driver usbfs
[    7.878643] usbcore: registered new interface driver hub
[    7.884183] usbcore: registered new device driver usb
         Starting Create list of required ste nodes for the current k[    7.893079] usbcore: registered new interface driver usbserial
ernel...
[    7.912828] usbcore: registered new interface driver ftdi_sio
[    7.918628] usbserial: USB Serial support registered for FTDI USB Serial Device
[  OK  ] Listening on Process Core Dump Socket.
         Starting Journal Service...
[  OK  ] Started Dispatch Password Requests to Console Directory Watch.
[  OK  ] Reached target Paths.
[  OK  ] Created slice system-serial\x2dgetty.slice.
[  OK  ] Mounted Kernel Debug File System.
[  OK  ] Mounted POSIX Message Queue File System.
[  OK  ] Mounted Temporary Directory (/tmp).
[  OK  ] Started Journal Service.
[  OK  ] Started Load Kernel Modules.
[  OK  ] Started Remount Root and Kernel File Systems.
[  OK  ] Started Create list of required staice nodes for the current kernel.
         Starting Rebuild Hardware Database...
         Starting Create System Users...
         Mounting Kernel Configuration File System...
         Starting Apply Kernel Variables...
         Starting Flush Journal to Persistent Storage...
[  OK  ] Mounted Kernel Configuration File System.
[  OK  ] Started Create System Users.
[  OK  ] Started Apply Kernel Variables.
[    8.527651] systemd-journald[91]: Received request to flush runtime journal from PID 1
         Starting Create Static Device Nodes in /dev...
[  OK  ] Started Flush Journal to Persistent Storage.
[  OK  ] Started Create Static Device Nodes in /dev.
[  OK  ] Reached target Local File Systems (Pre).
         Mounting /var/volatile...
         Mounting /media/ram...
         Starting udev Kernel Device Manager...
[  OK  ] Mounted /var/volatile.
[  OK  ] Mounted /media/ram.
         Starting Load/Save Random Seed...
[  OK  ] Reached target Local File Systems.
         Starting Rebuild Dynamic Linker Cache...
         Starting Rebuild Journal Catalog...
         Starting Create Volatile Files and Directories...
[  OK  ] Started udev Kernel Device Manager.
[  OK  ] Started Load/Save Random Seed.
[  OK  ] Started Rebuild Journal Catalog.
[    9.021100] EXT4-fs error (device mmcblk0p2): ext4_mb_generate_buddy:757: group 58, block bitmap and bg descriptor inconsistent: 4138 vs 4140 free clusters
[    9.035310] JBD2: Spotted dirty metadata buffer (dev = mmcblk0p2, blocknr = 0). There's a risk of filesystem corruption in case of system crash.
[  OK  ] Started Rebuild Dynamic Linker Cache.
[  OK  ] Started Create Volatile Files and Directories.
         Starting Update UTMP about System Boot/Shutdown...
[    9.138945] EXT4-fs error (device mmcblk0p2): ext4_mb_generate_buddy:757: group 4, block bitmap and bg descriptor inconsistent: 14491 vs 14492 free clusters
         Starting Network Time Synchronization...
[    9.162431] JBD2: Spotted dirty metadata buffer (dev = mmcblk0p2, blocknr = 0). There's a risk of filesystem corruption in case of system crash.
[  OK  ] Started Update UTMP about System Boot/Shutdown.
[  OK  ] Started Rebuild Hardware Database.
         Starting Update is Completed...
         Starting udev Coldplug all Devices...
[  OK  ] Started Update is Completed.
[  OK  ] Started udev Coldplug all Devices.
[  OK  ] Found device /dev/ttyS2.
[  OK  ] Started Network Time Synchronization.
[   11.046080] palmas-rtc 48070000.i2c:tps659038@58:tps659038_rtc: rtc core: registered 48070000.i2c:tps659038@58:tps659038_rtc as rtc1
[  OK  ] Reached target System Time Synchronized.
[  OK  ] Reached target System Initialization.
[   11.121100] rtc-ds1307: probe of 2-006f failed with error -121
[  OK  ] Listening on D-Bus System Message Bus Socket.
[  OK  ] Started Daily Cleanup of Temporary Directorie[   11.176661] omap-des 480a5000.des: OMAP DES hw accel rev: 2.2
s.
[   11.188942] omap-des 480a5000.des: will run requests pump with realtime priority
[  OK  ] Listening on RPCbind Server Activation Socket.
[   11.232036] pixcir_ts 4-005c: pixcir_set_power_mode: can't read reg 0x33 : -121
[   11.254329] pixcir_ts 4-005c: Failed to set IDLE mode
[   11.259554] pixcir_ts: probe of 4-005c failed with error -121
[  OK  ] Listening on dropbear.socket.
[   11.289003] omap-rproc 58820000.ipu: assigned reserved memory node ipu1-memory@9d000000
[   11.301739] remoteproc remoteproc0: 58820000.ipu is available
[  OK  ] Listening on Avahi mDNS/DNS-SD Stack Activation Socket.
[   11.316533] omap_rtc 48838000.rtc: registered as rtc2
[   11.330028] vpe 489d0000.vpe: loading firmware vpdma-1b8.bin
[   11.341992] omap-rproc 55020000.ipu: assigned reserved memory node ipu2-memory@95800000
[   11.350110] remoteproc remoteproc1: 55020000.ipu is available
[  OK  ] Reached target Sockets.
[   11.360478] omap-rproc 40800000.dsp: assigned reserved memory node dsp1-memory@99000000
[   11.374433] remoteproc remoteproc2: 40800000.dsp is available
[  OK  ] Reached target Basic System.
[   11.383933] vpe 489d0000.vpe: Device registered as /dev/video0
[   11.394500] omap-rproc 41000000.dsp: assigned reserved memory node dsp2-memory@9f000000
[   11.394586] remoteproc remoteproc3: 41000000.dsp is available
         Starting TI IPC Daemon...
[  OK  ] Reached target Containers.
[   11.496370] omap_wdt: OMAP Watchdog Timer Rev 0x01: initial timeout 60 sec
[   11.538362] SCSI subsystem initialized
[  OK  ] Started System Logging Service.
         Starting Print notice about GPLv3 packages...
[   11.684848] remoteproc remoteproc1: powering up 55020000.ipu
[   11.692830] remoteproc remoteproc1: Booting fw image dra7-ipu2-fw.xem4, size 3747220
[   11.700658] omap-iommu 55082000.mmu: 55082000.mmu: version 2.1
[   11.728850] remoteproc remoteproc0: powering up 58820000.ipu
[   11.735582] remoteproc remoteproc0: Booting fw image dra7-ipu1-fw.xem4, size 6680920
[   11.749280] omap-iommu 58882000.mmu: 58882000.mmu: version 2.1
[   11.805555] virtio_rpmsg_bus virtio0: rpmsg host is online
[   11.805590] virtio_rpmsg_bus virtio1: rpmsg host is online
[   11.805624] remoteproc remoteproc1: registered virtio1 (type 7)
[   11.805628] remoteproc remoteproc1: remote processor 55020000.ipu is now up
[   11.813710] virtio_rpmsg_bus virtio1: creating channel rpmsg-rpc addr 0x65
[   11.814591] virtio_rpmsg_bus virtio1: creating channel rpmsg-rpc addr 0x66
[   11.857266] remoteproc remoteproc0: registered virtio0 (type 7)
[   11.863537] remoteproc remoteproc0: remote processor 58820000.ipu is now up
[   11.871322] omap-aes 4b500000.aes: OMAP AES hw accel rev: 3.3
[   11.877375] omap-hdmi-audio omap-hdmi-audio.0.auto: snd-soc-dummy-dai <-> 58040000.encoder mapping ok
[   11.877492] omap-aes 4b500000.aes: will run requests pump with realtime priority
[   11.878142] omap-aes 4b700000.aes: OMAP AES hw accel rev: 3.3
[   11.878302] omap-aes 4b700000.aes: will run requests pump with realtime priority
[   11.891279] omap-sham 4b101000.sham: hw accel on OMAP rev 4.3
[   11.927555] virtio_rpmsg_bus virtio0: creating channel rpmsg-proto addr 0x3d
[   12.014219] [drm] Initialized pvr 1.14.3699939 20110701 for 56000000.gpu on minor 1
[   12.015305] ahci 4a140000.sata: SSS flag set, parallel bus scan disabled
[   12.015326] ahci 4a140000.sata: AHCI 0001.0300 32 slots 1 ports 3 Gbps 0x1 impl platform mode
[   12.015332] ahci 4a140000.sata: flags: 64bit ncq sntf stag pm led clo only pmp pio slum part ccc apst
[   12.037108] scsi host0: ahci
[   12.037328] ata1: SATA max UDMA/133 mmio [mem 0x4a140000-0x4a1410ff] port 0x100 irq 82
         Starting RPC Bind Service...
         Starting uim-sysfs.service...
[  OK  ] Started Kernel Logging Service.
[   12.176781] omap-hdmi-audio omap-hdmi-audio.0.auto: ASoC: no DMI vendor name!
[  OK  ] Started Hardware RNG Entropy Gatherer Daemon.
         Starting Avahi mDNS/DNS-SD Stack...
[  OK  ] Started Daily rotation of log files.
[  OK  ] Reached target Timers.
[  OK  ] Started Periodic Command Scheduler.
[  OK  ] Started D-Bus System Message Bus.
[   12.364511] ata1: SATA link down (SStatus 0 SControl 300)
[   12.459497] asoc-simple-card sound0: tlv320aic3x-hifi <-> 48468000.mcasp mapping ok
[   12.488896] asoc-simple-card sound0: ASoC: no DMI vendor name!
[   12.727977] remoteproc remoteproc2: powering up 40800000.dsp
[   12.733803] remoteproc remoteproc2: Booting fw image dra7-dsp1-fw.xe66, size 20392652
[   12.748555] omap_hwmod: mmu0_dsp1: _wait_target_disable failed
[   12.754441] omap-iommu 40d01000.mmu: 40d01000.mmu: version 3.0
[   12.760375] omap-iommu 40d02000.mmu: 40d02000.mmu: version 3.0
[   12.793933] random: crng init done
[   12.797356] random: 7 urandom warning(s) missed due to ratelimiting
[   12.807160] virtio_rpmsg_bus virtio2: rpmsg host is online
[   12.807214] remoteproc remoteproc2: registered virtio2 (type 7)
[   12.807218] remoteproc remoteproc2: remote processor 40800000.dsp is now up
[   12.809059] virtio_rpmsg_bus virtio2: creating channel rpmsg-proto addr 0x3d
[   12.999848] remoteproc remoteproc3: powering up 41000000.dsp
[   13.006631] remoteproc remoteproc3: Booting fw image dra7-dsp2-fw.xe66, size 20392652
[   13.031908] omap_hwmod: mmu0_dsp2: _wait_target_disable failed
[   13.037793] omap-iommu 41501000.mmu: 41501000.mmu: version 3.0
[   13.043719] omap-iommu 41502000.mmu: 41502000.mmu: version 3.0
[   13.133895] virtio_rpmsg_bus virtio3: rpmsg host is online
[   13.213662] remoteproc remoteproc3: registered virtio3 (type 7)
[   13.251208] FAT-fs (mmcblk0p1): Volume was not properly unmounted. Some data may be corrupt. Please run fsck.
[   13.320178] remoteproc remoteproc3: remote processor 41000000.dsp is now up
[   13.329984] virtio_rpmsg_bus virtio3: creating channel rpmsg-proto addr 0x3d
[  OK  ] Started Avahi mDNS/DNS-SD Stack.
         Starting Login Service...
         Starting Network Service...
[  OK  ] Started Job spooling tools.
         Starting TI MultiCore Tools Daemon...
[  OK  ] Started TI IPC Daemon.
[  OK  ] Started RPC Bind Service.
[  OK  ] Started TI MultiCore Tools Daemon.
[  OK  ] Started Network Service.
[   13.638624] net eth1: initializing cpsw version 1.15 (0)
[   13.658624] net eth1: phy "/ocp/ethernet@48484000/mdio@48485000/ethernet-phy@2" not found on slave 1
[  OK  ] Started uim-sysfs.service.
[   13.705010] IPv6: ADDRCONF(NETDEV_UP): eth1: link is not ready
[   13.725193] net eth0: initializing cpsw version 1.15 (0)
[   13.749558] net eth0: phy "/ocp/ethernet@48484000/mdio@48485000/ethernet-phy@1" not found on slave 0
[   13.774425] IPv6: ADDRCONF(NETDEV_UP): eth0: link is not ready
[   13.904522] Unable to handle kernel NULL pointer dereference at virtual address 0000080c
[   13.904526] pgd = ed245380
[   13.904529] [0000080c] *pgd=adada003, *pmd=00000000
[   13.904539] Internal error: Oops: 206 [#1] PREEMPT SMP ARM
[   13.904542] Modules linked in: snd_soc_simple_card snd_soc_simple_card_utils ahci_platform libahci_platform pvrsrvkm(O) omap_sham omap_aes_driver snd_soc_omap_hdmi_audio libahci libata pruss_soc_bus phy_omap_usb2 scsi_mod omap_wdt ti_vpe ti_sc ti_csc ti_vpdma dwc3_omap rtc_omap omap_remoteproc snd_soc_tlv320aic3x omap_des virtio_rpmsg_bus rpmsg_core remoteproc des_generic extcon_palmas crypto_engine omap_crypto rtc_ds1307 at24 pixcir_i2c_ts rtc_palmas sch_fq_codel uio_module_drv(O) uio ftdi_sio usbserial usbcore usb_common gdbserverproxy(O) cryptodev(O) cmemk(O)
[   13.904633] CPU: 1 PID: 433 Comm: systemd-udevd Tainted: G           O    4.14.79-gbde58ab01e #1
[   13.904636] Hardware name: Generic DRA74X (Flattened Device Tree)
[   13.904639] task: ee0a21c0 task.stack: ed270000
[   13.904649] PC is at _raw_spin_lock_irqsave+0x34/0x70
[   13.904655] LR is at __pm_relax.part.1+0x20/0x7c
[   13.904658] pc : [<c0949c28>]    lr : [<c06637d8>]    psr: 20070193
[   13.904661] sp : ed271e80  ip : ed271e90  fp : ed271e8c
[   13.904663] r10: 60070113  r9 : 00000000  r8 : 00000001
[   13.904666] r7 : ed271ec0  r6 : eda544b0  r5 : 0000080c  r4 : 00000800
[   13.904669] r3 : ed270000  r2 : 0000080c  r1 : 00000002  r0 : 20070193
[   13.904673] Flags: nzCv  IRQs off  FIQs on  Mode SVC_32  ISA ARM  Segment user
[   13.904676] Control: 30c5387d  Table: ad245380  DAC: 55555555
[   13.904679] Process systemd-udevd (pid: 433, stack limit = 0xed270210)
[   13.904682] Stack: (0xed271e80 to 0xed272000)
[   13.904686] 1e80: ed271eac ed271e90 c06637d8 c0949c00 00000000 c038054c 00000000 eda54480
[   13.904690] 1ea0: ed271ebc ed271eb0 c066384c c06637c4 ed271ef4 ed271ec0 c038126c c0663840
[   13.904694] 1ec0: ed271ec0 ed271ec0 edaac540 edaac540 00000004 bec82168 edaac540 eda54480
[   13.904698] 1ee0: 00000000 00000000 ed271fa4 ed271ef8 c0382310 c038113c 00000000 ed271f08
[   13.904702] 1f00: ed94af00 00000000 00000000 00000000 00000000 00000004 edaac540 ffffe000
[   13.904706] 1f20: 00000000 ed94af00 00000000 00000000 eda544b0 eda544b0 ed271f74 ed271f48
[   13.904710] 1f40: c033cc18 c033c978 ed271e90 0000000c 00000004 bec82168 00000000 00000000
[   13.904714] 1f60: 00000001 ee0a21c0 c0251e14 00000100 00000200 c033cb78 00000000 bec82168
[   13.904718] 1f80: bec82228 bec82228 000000fc c0207e44 ed270000 000000fc 00000000 ed271fa8
[   13.904722] 1fa0: c0207c40 c038210c bec82168 bec82228 00000004 bec82168 00000004 ffffffff
[   13.904726] 1fc0: bec82168 bec82228 bec82228 000000fc 00000000 00000003 00000004 0000000e
[   13.904729] 1fe0: 00000000 bec8206c 00515244 b6e265d8 600e0030 00000004 00000000 00000000
[   13.904731] Backtrace:
[   13.904739] [<c0949bf4>] (_raw_spin_lock_irqsave) from [<c06637d8>] (__pm_relax.part.1+0x20/0x7c)
[   13.904745] [<c06637b8>] (__pm_relax.part.1) from [<c066384c>] (__pm_relax+0x18/0x1c)
[   13.904748]  r5:eda54480 r4:00000000
[   13.904757] [<c0663834>] (__pm_relax) from [<c038126c>] (ep_scan_ready_list.constprop.0+0x13c/0x1e0)
[   13.904764] [<c0381130>] (ep_scan_ready_list.constprop.0) from [<c0382310>] (SyS_epoll_wait+0x210/0x460)
[   13.904769]  r10:00000000 r9:00000000 r8:eda54480 r7:edaac540 r6:bec82168 r5:00000004
[   13.904771]  r4:edaac540
[   13.904780] [<c0382100>] (SyS_epoll_wait) from [<c0207c40>] (ret_fast_syscall+0x0/0x4c)
[   13.904785]  r10:000000fc r9:ed270000 r8:c0207e44 r7:000000fc r6:bec82228 r5:bec82228
[   13.904787]  r4:bec82168
[   13.904792] Code: e5931004 e2811001 e5831004 f592f000 (e1923f9f)
[   13.904796] ---[ end trace 962b1cf5f5616f4f ]---
[   13.904808] note: systemd-udevd[433] exited with preempt_count 2
[   14.167396] pruss 4b200000.pruss: creating PRU cores and other child platform devices
[   14.175240] pruss 4b280000.pruss: creating PRU cores and other child platform devices
[  OK  ] Started Login Service.
[  OK  ] Reached target Sound Card.
[  OK  ] Listening on Load/Save RF Kill Switch Status /dev/rfkill Watch.
         Starting rc.pvr.service...
[   15.003410] BUG: Bad page state in process systemd  pfn:f3835
2m  OK  ] Reached target Network.
         Starting Lightni[   15.011640] page:efde0774 count:2048 mapcount:0 mapping:  (null) index:0x1
[   15.024115] flags: 0x80000000()
[   15.027270] raw: 80000000 00000000 00000001 ffffffff 00000800 00000100 00000200 00000000
[   15.035391] raw: 00000000
[   15.038017] page dumped because: nonzero _count
[   15.042560] Modules linked in: dwc3 udc_core pruss snd_soc_simple_card snd_soc_simple_card_utils ahci_platform libahci_platform pvrsrvkm(O) omap_sham omap_aes_driver snd_soc_omap_hdmi_audio libahci libata pruss_soc_bus phy_omap_usb2 scsi_mod omap_wdt ti_vpe ti_sc ti_csc ti_vpdma dwc3_omap rtc_omap omap_remoteproc snd_soc_tlv320aic3x omap_des virtio_rpmsg_bus rpmsg_core remoteproc des_generic extcon_palmas crypto_engine omap_crypto rtc_ds1307 at24 pixcir_i2c_ts rtc_palmas sch_fq_codel uio_module_drv(O) uio ftdi_sio usbserial usbcore usb_common gdbserverproxy(O) cryptodev(O) cmemk(O)
[   15.094426] CPU: 1 PID: 1 Comm: systemd Tainted: G      D    O    4.14.79-gbde58ab01e #1
[   15.102546] Hardware name: Generic DRA74X (Flattened Device Tree)
[   15.108661] Backtrace:
[   15.111124] [<c020b4dc>] (dump_backtrace) from [<c020b7c0>] (show_stack+0x18/0x1c)
[   15.118722]  r7:c0bb861c r6:20010193 r5:00000000 r4:c1053d10
[   15.124407] [<c020b7a8>] (show_stack) from [<c0931348>] (dump_stack+0x90/0xa4)
[   15.131664] [<c09312b8>] (dump_stack) from [<c02e2f10>] (bad_page+0x100/0x160)
[   15.138913]  r7:c0bb861c r6:efde0774 r5:c1002d00 r4:c108199c
[   15.144595] [<c02e2e10>] (bad_page) from [<c02e306c>] (check_new_page_bad+0x7c/0x80)
[   15.152367]  r7:efde0764 r6:0000000f r5:c1054480 r4:00000000
[   15.158049] [<c02e2ff0>] (check_new_page_bad) from [<c02e5cd4>] (get_page_from_freelist+0x63c/0x958)
[   15.167216]  r5:c1054480 r4:00000000
[   15.170804] [<c02e5698>] (get_page_from_freelist) from [<c02e6764>] (__alloc_pages_nodemask+0xcc/0xec0)
[   15.180234]  r10:edc9a040 r9:00000000 r8:c1003df8 r7:ededec30 r6:014200ca r5:00000081
[   15.188092]  r4:00000000
[   15.190635] [<c02e6698>] (__alloc_pages_nodemask) from [<c030aa90>] (wp_page_copy+0x6c/0x604)
[   15.199193]  r10:edc9a040 r9:edc9a000 r8:ffffe000 r7:ededec30 r6:f3fdb7df r5:efdf1acc
[   15.207051]  r4:ee87fe40
[   15.209593] [<c030aa24>] (wp_page_copy) from [<c030ca88>] (do_wp_page+0xa8/0x5a0)
[   15.217104]  r10:edc9a040 r9:00000055 r8:ffffe000 r7:00000000 r6:f3fdb7df r5:ededec30
[   15.224962]  r4:ee87fe40
[   15.227504] [<c030c9e0>] (do_wp_page) from [<c030f8cc>] (handle_mm_fault+0x774/0xc50)
[   15.235364]  r8:ffffe000 r7:00000000 r6:f3fdb7df r5:00000040 r4:f3fdb7df
[   15.242093] [<c030f158>] (handle_mm_fault) from [<c0213f34>] (do_page_fault+0x134/0x348)
[   15.250215]  r10:edc9a040 r9:00000055 r8:b6ca3060 r7:00000a0f r6:edc9a000 r5:ee880000
[   15.258072]  r4:ee87ffb0
[   15.260613] [<c0213e00>] (do_page_fault) from [<c020127c>] (do_DataAbort+0x38/0xb8)
[   15.268300]  r10:b6f788e0 r9:b6ca1000 r8:ee87ffb0 r7:b6ca3060 r6:c0213e00 r5:00000a0f
[   15.276157]  r4:c1008cbc
[   15.278698] [<c0201244>] (do_DataAbort) from [<c020c680>] (__dabt_usr+0x40/0x60)
[   15.286119] Exception stack(0xee87ffb0 to 0xee87fff8)
[   15.291188] ffa0:                                     00000001 b6ca3060 00000002 b6ca304c
[   15.299396] ffc0: 00000256 bee3f5d0 00000002 bee3f5e0 00000000 b6ca1000 b6f788e0 00000000
[   15.307604] ffe0: 00000078 bee3f5d0 b6c2854d b6c285f8 60010030 ffffffff
[   15.314243]  r8:30c5387d r7:30c5387d r6:ffffffff r5:60010030 r4:b6c285f8
ng Fast Webserver With Light System Requirements...
[  OK  ] Started Redis In-Memory Data Store.
         Starting Enable and configure wl18xx bluetooth stack...
         Starting Simple Network Management Protocol (SNMP) Daemon....
         Starting Permit User Sessions...
[   15.346627] Unable to handle kernel NULL pointer dereference at virtual address 0000080c
[   15.354756] pgd = edf900c0
[   15.357471] [0000080c] *pgd=ad930003, *pmd=00000000
[   15.362375] Internal error: Oops: 206 [#2] PREEMPT SMP ARM
[   15.367879] Modules linked in: dwc3 udc_core pruss snd_soc_simple_card snd_soc_simple_card_utils ahci_platform libahci_platform pvrsrvkm(O) omap_sham omap_aes_driver snd_soc_omap_hdmi_audio libahci libata pruss_soc_bus phy_omap_usb2 scsi_mod omap_wdt ti_vpe ti_sc ti_csc ti_vpdma dwc3_omap rtc_omap omap_remoteproc snd_soc_tlv320aic3x omap_des virtio_rpmsg_bus rpmsg_core remoteproc des_generic extcon_palmas crypto_engine omap_crypto rtc_ds1307 at24 pixcir_i2c_ts rtc_palmas sch_fq_codel uio_module_drv(O) uio ftdi_sio usbserial usbcore usb_common gdbserverproxy(O) cryptodev(O) cmemk(O)
[   15.419745] CPU: 0 PID: 91 Comm: systemd-journal Tainted: G    B D    O    4.14.79-gbde58ab01e #1
[   15.428649] Hardware name: Generic DRA74X (Flattened Device Tree)
[   15.434764] task: edf6af40 task.stack: ed92a000
[   15.439316] PC is at _raw_spin_lock_irqsave+0x34/0x70
[   15.444388] LR is at __pm_relax.part.1+0x20/0x7c
[   15.449020] pc : [<c0949c28>]    lr : [<c06637d8>]    psr: 200f0093
[   15.455309] sp : ed92be80  ip : ed92be90  fp : ed92be8c
[   15.460551] r10: 600f0013  r9 : 00000000  r8 : 00000004
[   15.465793] r7 : ed92bec0  r6 : edfc59b0  r5 : 0000080c  r4 : 00000800
[   15.472344] r3 : ed92a000  r2 : 0000080c  r1 : 00000002  r0 : 200f0093
[   15.478896] Flags: nzCv  IRQs off  FIQs on  Mode SVC_32  ISA ARM  Segment user
[   15.486144] Control: 30c5387d  Table: adf900c0  DAC: fffffffd
[   15.491910] Process systemd-journal (pid: 91, stack limit = 0xed92a210)
[   15.498548] Stack: (0xed92be80 to 0xed92c000)
[   15.502920] be80: ed92beac ed92be90 c06637d8 c0949c00 ed92a000 c038054c 00000000 edfc5980
[   15.511130] bea0: ed92bebc ed92beb0 c066384c c06637c4 ed92bef4 ed92bec0 c038126c c0663840
[   15.519339] bec0: ed92bec0 ed92bec0 ed975070 edf9ae40 0000001a bee3c578 edf9ae40 edfc5980
[   15.527548] bee0: 00000001 00000000 ed92bfa4 ed92bef8 c0382310 c038113c ed22b019 00000002
[   15.535756] bf00: c035b030 c0949f50 c034b538 000a0042 edf8f840 ed22b000 fffffffe ed22b000
[   15.543965] bf20: 00000000 c0207e44 00000000 00000000 c034b4e4 edfc59b0 fffffffe fffffffe
[   15.552174] bf40: ed92bf94 ed92bf50 c033a1f8 c034b490 0000001a bee3c578 ed92bf94 00020042
[   15.560383] bf60: 0000005b 0000040c ed92bf94 ed92bf78 c0246564 c0289620 00463130 00463130
[   15.568592] bf80: 00000001 00000000 000000fc c0207e44 ed92a000 000000fc 00000000 ed92bfa8
[   15.576800] bfa0: c0207c40 c038210c 00463130 00000001 00000007 bee3c578 0000001a 00000000
[   15.585009] bfc0: 00463130 00000001 00000000 000000fc 0000001a bee3c578 00000007 bee3c7ec
[   15.593217] bfe0: 00000000 bee3c56c b6e895d0 b6d4d5d8 600f0030 00000007 00000000 00000000
[   15.601423] Backtrace:
[   15.603880] [<c0949bf4>] (_raw_spin_lock_irqsave) from [<c06637d8>] (__pm_relax.part.1+0x20/0x7c)
[   15.612787] [<c06637b8>] (__pm_relax.part.1) from [<c066384c>] (__pm_relax+0x18/0x1c)
[   15.620646]  r5:edfc5980 r4:00000000
[   15.624239] [<c0663834>] (__pm_relax) from [<c038126c>] (ep_scan_ready_list.constprop.0+0x13c/0x1e0)
[   15.633411] [<c0381130>] (ep_scan_ready_list.constprop.0) from [<c0382310>] (SyS_epoll_wait+0x210/0x460)
[   15.642928]  r10:00000000 r9:00000001 r8:edfc5980 r7:edf9ae40 r6:bee3c578 r5:0000001a
[   15.650786]  r4:edf9ae40
[   15.653330] [<c0382100>] (SyS_epoll_wait) from [<c0207c40>] (ret_fast_syscall+0x0/0x4c)
[   15.661364]  r10:000000fc r9:ed92a000 r8:c0207e44 r7:000000fc r6:00000000 r5:00000001
[   15.669222]  r4:00463130
[   15.671762] Code: e5931004 e2811001 e5831004 f592f000 (e1923f9f)
[   15.677880] ---[ end trace 962b1cf5f5616f50 ]---

