[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 4.14.79-gbde58ab01e (oe-user@oe-host) (gcc version 7.2.1 20171011 (Linaro GCC 7.2-2017.11)) #1 SMP PREEMPT Thu Dec 20 04:51:24 UTC 2018
[    0.000000] CPU: ARMv7 Processor [412fc0f2] revision 2 (ARMv7), cr=30c5387d
[    0.000000] CPU: div instructions available: patching division code
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, PIPT instruction cache
[    0.000000] OF: fdt: Machine model: TI AM5728 EVM
[    0.000000] Memory policy: Data cache writealloc
[    0.000000] efi: Getting EFI parameters from FDT:
[    0.000000] efi: UEFI not found.
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000095800000, size 56 MiB
[    0.000000] OF: reserved mem: initialized node ipu2-memory@95800000, compatible id shared-dma-pool
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000099000000, size 64 MiB
[    0.000000] OF: reserved mem: initialized node dsp1-memory@99000000, compatible id shared-dma-pool
[    0.000000] Reserved memory: created CMA memory pool at 0x000000009d000000, size 32 MiB
[    0.000000] OF: reserved mem: initialized node ipu1-memory@9d000000, compatible id shared-dma-pool
[    0.000000] Reserved memory: created CMA memory pool at 0x000000009f000000, size 8 MiB
[    0.000000] OF: reserved mem: initialized node dsp2-memory@9f000000, compatible id shared-dma-pool
[    0.000000] cma: Reserved 24 MiB at 0x00000000fe400000
[    0.000000] OMAP4: Map 0x00000000ffd00000 to fe600000 for dram barrier
[    0.000000] DRA752 ES2.0
[    0.000000] percpu: Embedded 15 pages/cpu @eed29000 s31372 r8192 d21876 u61440
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 472640
[    0.000000] Kernel command line: console=ttyO2,115200n8 root=PARTUUID=07b1c964-02 rw rootfstype=ext4 rootwait
[    0.000000] PID hash table entries: 4096 (order: 2, 16384 bytes)
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes)
[    0.000000] Memory: 1675572K/1897472K available (8192K kernel code, 347K rwdata, 2628K rodata, 2048K init, 282K bss, 33484K reserved, 188416K cma-reserved, 1283072K highmem)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
[    0.000000]     fixmap  : 0xffc00000 - 0xfff00000   (3072 kB)
[    0.000000]     vmalloc : 0xf0800000 - 0xff800000   ( 240 MB)
[    0.000000]     lowmem  : 0xc0000000 - 0xf0000000   ( 768 MB)
[    0.000000]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
[    0.000000]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)
[    0.000000]       .text : 0xc0008000 - 0xc0a00000   (10208 kB)
[    0.000000]       .init : 0xc0e00000 - 0xc1000000   (2048 kB)
[    0.000000]       .data : 0xc1000000 - 0xc1056e98   ( 348 kB)
[    0.000000]        .bss : 0xc1058000 - 0xc109ebe0   ( 283 kB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=2, Nodes=1
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Tasks RCU enabled.
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] GIC: Using split EOI/Deactivate mode
[    0.000000] OMAP clockevent source: timer1 at 32786 Hz
[    0.000000] arch_timer: cp15 timer(s) running at 6.14MHz (phys).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x16af5adb9, max_idle_ns: 440795202250 ns
[    0.000005] sched_clock: 56 bits at 6MHz, resolution 162ns, wraps every 4398046511023ns
[    0.000016] Switching to timer-based delay loop, resolution 162ns
[    0.000359] clocksource: 32k_counter: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 58327039986419 ns
[    0.000367] OMAP clocksource: 32k_counter at 32768 Hz
[    0.000875] Console: colour dummy device 80x30
[    0.000892] WARNING: Your 'console=ttyO2' has been replaced by 'ttyS2'
[    0.000899] This ensures that you still see kernel messages. Please
[    0.000907] update your kernel commandline.
[    0.000928] Calibrating delay loop (skipped), value calculated using timer frequency.. 12.29 BogoMIPS (lpj=61475)
[    0.000943] pid_max: default: 32768 minimum: 301
[    0.001059] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.001073] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.001599] CPU: Testing write buffer coherency: ok
[    0.001636] CPU0: Spectre v2: using ICIALLU workaround
[    0.001831] /cpus/cpu@0 missing clock-frequency property
[    0.001850] /cpus/cpu@1 missing clock-frequency property
[    0.001862] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000
[    0.039847] Setting up static identity map for 0x80200000 - 0x80200060
[    0.059853] Hierarchical SRCU implementation.
[    0.080043] EFI services will not be available.
[    0.099917] smp: Bringing up secondary CPUs ...
[    0.170295] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001
[    0.170299] CPU1: Spectre v2: using ICIALLU workaround
[    0.170400] smp: Brought up 1 node, 2 CPUs
[    0.170411] SMP: Total of 2 processors activated (24.59 BogoMIPS).
[    0.170419] CPU: All CPU(s) started in HYP mode.
[    0.170427] CPU: Virtualization extensions available.
[    0.170960] devtmpfs: initialized
[    0.191742] random: get_random_u32 called from bucket_table_alloc+0x108/0x230 with crng_init=0
[    0.191992] VFP support v0.3: implementor 41 architecture 4 part 30 variant f rev 0
[    0.192187] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.192203] futex hash table entries: 512 (order: 3, 32768 bytes)
[    0.195965] pinctrl core: initialized pinctrl subsystem
[    0.196418] DMI not present or invalid.
[    0.196676] NET: Registered protocol family 16
[    0.197720] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.198671] omap_hwmod: l3_main_2 using broken dt data from ocp
[    0.307561] omap_hwmod: dcan1: _wait_target_disable failed
[    0.406011] cpuidle: using governor ladder
[    0.406043] cpuidle: using governor menu
[    0.414768] OMAP GPIO hardware version 0.1
[    0.443497] No ATAGs?
[    0.443569] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.443583] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.443979] omap4_sram_init:Unable to allocate sram needed to handle errata I688
[    0.443990] omap4_sram_init:Unable to get sram pool needed to handle errata I688
[    0.444526] OMAP DMA hardware revision 0.0
[    0.454288] edma 43300000.edma: memcpy is disabled
[    0.457516] edma 43300000.edma: TI EDMA DMA engine driver
[    0.464340] omap-dma-engine 4a056000.dma-controller: OMAP DMA engine driver (LinkedList1/2/3 supported)
[    0.465676] evm_5v0: supplied by main_12v0
[    0.466099] com_3v6: supplied by evm_5v0
[    0.469136] omap-iommu 40d01000.mmu: 40d01000.mmu registered
[    0.469339] omap-iommu 40d02000.mmu: 40d02000.mmu registered
[    0.469578] omap-iommu 58882000.mmu: 58882000.mmu registered
[    0.469811] omap-iommu 55082000.mmu: 55082000.mmu registered
[    0.470177] omap-iommu 41501000.mmu: 41501000.mmu registered
[    0.470384] omap-iommu 41502000.mmu: 41502000.mmu registered
[    0.470691] iommu: Adding device 58820000.ipu to group 1
[    0.470782] iommu: Adding device 55020000.ipu to group 2
[    0.470943] iommu: Adding device 40800000.dsp to group 0
[    0.471217] iommu: Adding device 41000000.dsp to group 3
[    0.473486] palmas 0-0058: Irq flag is 0x00000008
[    0.502716] palmas 0-0058: Muxing GPIO 2b, PWM 0, LED 0
[    0.504218] SMPS12: supplied by regulator-dummy
[    0.505920] SMPS3: supplied by regulator-dummy
[    0.507566] SMPS45: supplied by regulator-dummy
[    0.509386] SMPS6: supplied by regulator-dummy
[    0.510805] SMPS7: supplied by regulator-dummy
[    0.512236] SMPS8: supplied by regulator-dummy
[    0.513513] SMPS9: supplied by regulator-dummy
[    0.514233] LDO1: supplied by regulator-dummy
[    0.521311] LDO2: supplied by regulator-dummy
[    0.521505] random: fast init done
[    0.531181] LDO3: supplied by regulator-dummy
[    0.541196] LDO4: supplied by regulator-dummy
[    0.551235] LDO5: supplied by regulator-dummy
[    0.551968] LDO6: supplied by regulator-dummy
[    0.552689] LDO7: supplied by regulator-dummy
[    0.553429] LDO8: supplied by regulator-dummy
[    0.554169] LDO9: supplied by regulator-dummy
[    0.561267] LDOLN: supplied by regulator-dummy
[    0.571280] LDOUSB: supplied by regulator-dummy
[    0.583954] omap_i2c 48070000.i2c: bus 0 rev0.12 at 400 kHz
[    0.584515] omap_i2c 48060000.i2c: bus 2 rev0.12 at 400 kHz
[    0.585040] omap_i2c 4807c000.i2c: bus 4 rev0.12 at 400 kHz
[    0.585236] media: Linux media interface: v0.10
[    0.585274] Linux video capture interface: v2.00
[    0.585354] pps_core: LinuxPPS API ver. 1 registered
[    0.585362] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.585381] PTP clock support registered
[    0.585409] EDAC MC: Ver: 3.0.0
[    0.590706] dmi: Firmware registration failed.
[    0.591107] omap-mailbox 48840000.mailbox: omap mailbox rev 0x400
[    0.591385] omap-mailbox 48842000.mailbox: omap mailbox rev 0x400
[    0.591745] Advanced Linux Sound Architecture Driver Initialized.
[    0.600782] clocksource: Switched to clocksource arch_sys_counter
[    0.608676] NET: Registered protocol family 2
[    0.609198] TCP established hash table entries: 8192 (order: 3, 32768 bytes)
[    0.609262] TCP bind hash table entries: 8192 (order: 4, 65536 bytes)
[    0.609388] TCP: Hash tables configured (established 8192 bind 8192)
[    0.609455] UDP hash table entries: 512 (order: 2, 16384 bytes)
[    0.609489] UDP-Lite hash table entries: 512 (order: 2, 16384 bytes)
[    0.609614] NET: Registered protocol family 1
[    0.609898] RPC: Registered named UNIX socket transport module.
[    0.609907] RPC: Registered udp transport module.
[    0.609915] RPC: Registered tcp transport module.
[    0.609923] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.610914] hw perfevents: no interrupt-affinity property for /pmu, guessing.
[    0.611089] hw perfevents: enabled with armv7_cortex_a15 PMU driver, 7 counters available
[    0.612125] workingset: timestamp_bits=14 max_order=19 bucket_order=5
[    0.616173] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.616677] NFS: Registering the id_resolver key type
[    0.616700] Key type id_resolver registered
[    0.616708] Key type id_legacy registered
[    0.616749] ntfs: driver 2.1.32 [Flags: R/O].
[    0.618041] bounce: pool size: 64 pages
[    0.618086] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 245)
[    0.618097] io scheduler noop registered
[    0.618106] io scheduler deadline registered
[    0.618196] io scheduler cfq registered (default)
[    0.618206] io scheduler mq-deadline registered
[    0.618215] io scheduler kyber registered
[    0.622770] pinctrl-single 4a003400.pinmux: 282 pins at pa fc003400 size 1128
[    0.626124] dra7-pcie 51000000.pcie: Linked as a consumer to phy-4a094000.pciephy.1
[    0.626488] OF: PCI: host bridge /ocp/axi@0/pcie@51000000 ranges:
[    0.626523] OF: PCI:    IO 0x20003000..0x20012fff -> 0x00000000
[    0.626545] OF: PCI:   MEM 0x20013000..0x2fffffff -> 0x20013000
[    1.626812] dra7-pcie 51000000.pcie: phy link never came up
[    1.626948] dra7-pcie 51000000.pcie: PCI host bridge to bus 0000:00
[    1.626962] pci_bus 0000:00: root bus resource [bus 00-ff]
[    1.626973] pci_bus 0000:00: root bus resource [io  0x0000-0xffff]
[    1.626984] pci_bus 0000:00: root bus resource [mem 0x20013000-0x2fffffff]
[    1.627297] PCI: bus0: Fast back to back transfers disabled
[    1.627386] PCI: bus1: Fast back to back transfers enabled
[    1.627422] pci 0000:00:00.0: BAR 0: assigned [mem 0x20100000-0x201fffff 64bit]
[    1.627441] pci 0000:00:00.0: PCI bridge to [bus 01-ff]
[    1.627755] pcieport 0000:00:00.0: Sig
                                         [    2.848644] brd: module loaded
[    2.857118] loop: module loaded
[    2.863414] libphy: Fixed MDIO Bus: probed
[    2.920807] davinci_mdio 48485000.mdio: davinci mdio revision 1.6, bus freq 1000000
[    2.928502] libphy: 48485000.mdio: probed
[    2.936269] davinci_mdio: probe of 48485000.mdio failed with error -5
[    2.943307] cpsw 48484000.ethernet: Detected MACID = d8:a9:8b:41:ab:5a
[    2.949922] cpsw 48484000.ethernet: initialized cpsw ale version 1.4
[    2.956329] cpsw 48484000.ethernet: ALE Table size 1024
[    2.961627] cpsw 48484000.ethernet: device node lookup for pps timer failed
[    2.968657] cpsw 48484000.ethernet: cpts: overflow check period 500 (jiffies)
[    2.976567] cpsw 48484000.ethernet: cpsw: Detected MACID = d8:a9:8b:41:ab:5b
[    2.984849] i2c /dev entries driver
[    2.989301] IR NEC protocol handler initialized
[    2.993876] IR RC5(x/sz) protocol handler initialized
[    2.998951] IR RC6 protocol handler initialized
[    3.003541] IR JVC protocol handler initialized
[    3.008091] IR Sony protocol handler initialized
[    3.012747] IR SANYO protocol handler initialized
[    3.017472] IR Sharp protocol handler initialized
[    3.022229] IR MCE Keyboard/mouse protocol handler initialized
[    3.028088] IR XMP protocol handler initialized
[    3.035071] gpio-fan gpio_fan: GPIO fan initialized
[    3.040633] tmp102 0-0048: error reading config register
[    3.046127] tmp102: probe of 0-0048 failed with error -121
[    3.055969] sdhci: Secure Digital Host Controller Interface driver
[    3.062263] sdhci: Copyright(c) Pierre Ossman
[    3.067602] sdhci-pltfm: SDHCI platform and OF driver helper
[    3.074103] sdhci-omap 4809c000.mmc: Got CD GPIO
[    3.079476] sdhci-omap 4809c000.mmc: no pinctrl state for ddr_1_8v mode
[    3.086170] sdhci-omap 4809c000.mmc: no pinctrl state for hs200_1_8v mode
[    3.150990] mmc0: SDHCI controller on 4809c000.mmc [4809c000.mmc] using ADMA
[    3.220841] mmc1: SDHCI controller on 480b4000.mmc [480b4000.mmc] using ADMA
[    3.231948] sdhci-omap 480ad000.mmc: no pinctrl state for sdr104 mode
[    3.238437] sdhci-omap 480ad000.mmc: no pinctrl state for ddr50 mode
[    3.244902] sdhci-omap 480ad000.mmc: no pinctrl state for hs200_1_8v mode
[    3.289506] mmc0: host does not support reading read-only switch, assuming write-enable
[    3.301901] ti-iodelay 4844a000.padconf: Set reg 0x618 Delay(a: 1076 g: 330), Elements(C=2 F=7)0x29047
[    3.311377] ti-iodelay 4844a000.padconf: Set reg 0x620 Delay(a: 1271 g: 0), Elements(C=2 F=7)0x29047
[    3.320660] ti-iodelay 4844a000.padconf: Set reg 0x624 Delay(a: 722 g: 0), Elements(C=1 F=6)0x29026
[    3.320816] mmc2: SDHCI controller on 480ad000.mmc [480ad000.mmc] using PIO
[    3.329811] ledtrig-cpu: registered to indicate activity on CPUs
[    3.340117] NET: Registered protocol family 10
[    3.348126] ti-iodelay 4844a000.padconf: Set reg 0x628 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.350859] Segment Routing with IPv6
[    3.350907] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    3.351303] NET: Registered protocol family 17
[    3.351483] Key type dns_resolver registered
[    3.351583] omap_voltage_late_init: Voltage driver support not added
[    3.351586] Power Management for TI OMAP4+ devices.
[    3.351802] Registering SWP/SWPB emulation handler
[    3.371488] dmm 4e000000.dmm: workaround for errata i878 in use
[    3.372903] dmm 4e000000.dmm: initialized all PAT entries
[    3.405196] ti-iodelay 4844a000.padconf: Set reg 0x62c Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.414160] ti-iodelay 4844a000.padconf: Set reg 0x630 Delay(a: 751 g: 0), Elements(C=1 F=6)0x29026
[    3.423258] ti-iodelay 4844a000.padconf: Set reg 0x634 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.432187] ti-iodelay 4844a000.padconf: Set reg 0x638 Delay(a: 20 g: 0), Elements(C=0 F=0)0x29000
[    3.432962] [drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
[    3.432964] [drm] No driver support for vblank timestamp query.
[    3.441264] [drm] Enabling DMM ywrap scrolling
[    3.461673] ti-iodelay 4844a000.padconf: Set reg 0x63c Delay(a: 256 g: 0), Elements(C=0 F=6)0x29006
[    3.461681] ti-iodelay 4844a000.padconf: Set reg 0x640 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.461687] ti-iodelay 4844a000.padconf: Set reg 0x644 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.461694] ti-iodelay 4844a000.padconf: Set reg 0x648 Delay(a: 263 g: 0), Elements(C=0 F=7)0x29007
[    3.461701] ti-iodelay 4844a000.padconf: Set reg 0x64c Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.461706] ti-iodelay 4844a000.padconf: Set reg 0x650 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.461711] ti-iodelay 4844a000.padconf: Set reg 0x654 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.461717] ti-iodelay 4844a000.padconf: Set reg 0x658 Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.461723] ti-iodelay 4844a000.padconf: Set reg 0x65c Delay(a: 0 g: 0), Elements(C=0 F=0)0x29000
[    3.461857] mmc0: new ultra high speed DDR50 SDHC card at address aaaa
[    3.462147] mmcblk0: mmc0:aaaa SL08G 7.40 GiB
[    3.463358]  mmcblk0: p1 p2
[    3.533433] Console: switching to colour frame buffer device 100x30
[    3.640049] omapdrm omapdrm.0: fb0: omapdrm frame buffer device
[    3.647093] [drm] Initialized omapdrm 1.0.0 20110917 for omapdrm.0 on minor 0
[    3.655222] input: gpio_keys as /devices/platform/gpio_keys/input/input0
[    3.662301] hctosys: unable to open rtc device (rtc0)
[    3.667862] aic_dvdd_fixed: disabling
[    3.671749] ldousb: disabling
[    3.674990] ALSA device list:
[    3.678989]   No soundcards found.
[    7.899628] EXT4-fs (mmcblk0p2): warning: mounting fs with errors, running e2fsck is recommended
[    7.910515] EXT4-fs (mmcblk0p2): Errors on filesystem, clearing orphan list.
[    7.910515]
[    7.919195] EXT4-fs (mmcblk0p2): recovery complete
[    7.925559] EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Opts: (null)
[    7.933730] VFS: Mounted root (ext4 filesystem) on device 179:2.
[    7.942509] devtmpfs: mounted
[    7.946363] Freeing unused kernel memory: 2048K
[    8.104602] systemd[1]: System time before build time, advancing clock.
[    8.130292] systemd[1]: systemd 234 running in system mode. (+PAM -AUDIT -SELINUX +IMA -APPARMOR +SMACK +SYSVINIT +UTMP -LIBCRYPTSETUP -GCRYPT -GNUTLS +ACL +XZ -LZ4 -SECCOMP +BLKID -ELFUTILS +KMOD -IDN2 -IDN default-hierarchy=hybrid)
[    8.152274] systemd[1]: Detected architecture arm.

Welcome to Arago 2018.10!

[    8.191552] systemd[1]: Set hostname to <am57xx-evm>.
[    8.463934] random: systemd: uninitialized urandom read (16 bytes read)
[    8.471055] systemd[1]: Started Dispatch Password Requests to Console Directory Watch.
[  OK  ] Started Dispatch Password Requests to Console Directory Watch.
[    8.510904] random: systemd: uninitialized urandom read (16 bytes read)
[    8.517625] systemd[1]: Listening on udev Kernel Socket.
[  OK  ] Listening on udev Kernel Socket.
[    8.551049] random: systemd: uninitialized urandom read (16 bytes read)
[    8.557752] systemd[1]: Reached target Remote File Systems.
[  OK  ] Reached target Remote File Systems.
[    8.591090] systemd[1]: Listening on Network Service Netlink Socket.
[  OK  ] Listening on Network Service Netlink Socket.
[    8.631289] systemd[1]: Listening on udev Control Socket.
[  OK  ] Listening on udev Control Socket.
[    8.686996] systemd[1]: Created slice User and Session Slice.
[  OK  ] Created slice User and Session Slice.
[    8.722304] systemd[1]: Created slice System Slice.
[  OK  ] Created slice System Slice.
[  OK  ] Created slice system-serial\x2dgetty.slice.
[  OK  ] Created slice system-getty.slice.
[  OK  ] Reached target Slices.
[  OK  ] Listening on Syslog Socket.
[  OK  ] Reached target Swap.
         Mounting Temporary Directory (/tmp)...
         Mounting Kernel Debug File System...
         Mounting POSIX Message Queue File System...
[  OK  ] Listening on Journal Socket (/dev/log).
[  OK  ] Listening on Journal Socket.
         Starting Create list of required ste nodes for the current kernel...
         Starting Remount Root and Kernel File Systems...
[    9.115701] EXT4-fs (mmcblk0p2): re-mounted. Opts: (null)
         Starting Journal Service...
         Starting Load Kernel Modules...
[    9.168750] cmemk: loading out-of-tree module taints kernel.
[    9.176039] CMEMK module: reference Linux version 4.14.79
[  OK  ] Started Forward Password Requests to Wall Dir[    9.182799] allocated heap buffer 0x40500000 of size 0x100000
ectory Watch.
[    9.194104] cmemk initialized
[    9.210287] cryptodev: driver 1.9 loaded.
[  OK  ] Reached target Paths.
[    9.235995] usbcore: registered new interface driver usbfs
[    9.242119] usbcore: registered new interface driver hub
[    9.247604] usbcore: registered new device driver usb
[  OK  ] Listening on Process Core Dump Socket.
[    9.262949] usbcore: registered new interface driver usbserial
[    9.277265] usbcore: registered new interface driver ftdi_sio
[[    9.283791] usbserial: USB Serial support registered for FTDI USB Serial Device
  OK  ] Listening on /dev/initctl Compatibility Named Pipe.
[  OK  ] Mounted Kernel Debug File System.
[  OK  ] Mounted POSIX Message Queue File System.
[  OK  ] Mounted Temporary Directory (/tmp).
[  OK  ] Started Journal Service.
[  OK  ] Started Create list of required staice nodes for the current kernel.
[  OK  ] Started Remount Root and Kernel File Systems.
[  OK  ] Started Load Kernel Modules.
         Starting Apply Kernel Variables...
         Mounting Kernel Configuration File System...
         Starting Rebuild Hardware Database...
         Starting Create System Users...
         Starting Flush Journal to Persistent Storage...
[  OK  ] Mounted Kernel Configuration File System.
[  OK  ] Started Apply Kernel Variables.
[  OK  ] Started Create System Users.
[    9.787693] systemd-journald[90]: Received request to flush runtime journal from PID 1
         Starting Create Static Device Nodes in /dev...
[  OK  ] Started Flush Journal to Persistent Storage.
[  OK  ] Started Create Static Device Nodes in /dev.
[  OK  ] Reached target Local File Systems (Pre).
         Mounting /var/volatile...
         Mounting /media/ram...
         Starting udev Kernel Device Manager...
[  OK  ] Mounted /var/volatile.
[  OK  ] Mounted /media/ram.
         Starting Load/Save Random Seed...
[  OK  ] Reached target Local File Systems.
         Starting Rebuild Dynamic Linker Cache...
         Starting Rebuild Journal Catalog...
         Starting Create Volatile Files and Directories...
[  OK  ] Started udev Kernel Device Manager.
[  OK  ] Started Load/Save Random Seed.
[  OK  ] Started Rebuild Journal Catalog.
[   10.288036] EXT4-fs error (device mmcblk0p2): ext4_mb_generate_buddy:757: group 58, block bitmap and bg descriptor inconsistent: 4138 vs 4140 free clusters
[   10.303515] JBD2: Spotted dirty metadata buffer (dev = mmcblk0p2, blocknr = 0). There's a risk of filesystem corruption in case of system crash.
[  OK  ] Started Create Volatile Files and Directories.
[  OK  ] Started Rebuild Dynamic Linker Cache.
         Starting Network Time Synchronization...
         Starting Update UTMP about System Boot/Shutdown...
[   10.709551] EXT4-fs error (device mmcblk0p2): ext4_mb_generate_buddy:757: group 4, block bitmap and bg descriptor inconsistent: 14491 vs 14492 free clusters
[  OK  ] Started Update UTMP about System Boot/Shutdown.
[   10.741172] JBD2: Spotted dirty metadata buffer (dev = mmcblk0p2, blocknr = 0). There's a risk of filesystem corruption in case of system crash.
[  OK  ] Started Network Time Synchronization.
[  OK  ] Reached target System Time Synchronized.
[  OK  ] Started Rebuild Hardware Database.
         Starting Update is Completed...
         Starting udev Coldplug all Devices...
[  OK  ] Started Update is Completed.
[  OK  ] Started udev Coldplug all Devices.
[  OK  ] Reached target System Initialization.
         Starting Network Service...
[  OK  ] Listening on D-Bus System Message Bus Socket.
[   12.633112] palmas-rtc 48070000.i2c:tps659038@58:tps659038_rtc: rtc core: registered 48070000.i2c:tps659038@58:tps659038_rtc as rtc1
[  OK  ] Listening on dropbear.socket.
[   12.671105] rtc-ds1307: probe of 2-006f failed with error -121
[  OK  ] Listening on RPCbind Server Activation Socket.
[  OK  ] Started Daily Cleanup of Temporary Directories.
[   12.740720] omap-rproc 58820000.ipu: assigned reserved memory node ipu1-memory@9d000000
[  OK  ] Started Daily rotation of log files.
[   12.775616] remoteproc remoteproc0: 58820000.ipu is available
[  OK  ] Reached target Timers.
[   12.822408] omap-des 480a5000.des: OMAP DES hw accel rev: 2.2
[   12.832992] omap-des 480a5000.des: will run requests pump with realtime priority
[   12.843532] omap_rtc 48838000.rtc: registered as rtc2
[  OK  ] Listening on Avahi mDNS/DNS-SD Stack Activation Socket.
[   12.859130] omap-rproc 55020000.ipu: assigned reserved memory node ipu2-memory@95800000
[   12.872071] remoteproc remoteproc1: 55020000.ipu is available
[  OK  ] Reached target Sockets.
[   12.897811] omap-rproc 40800000.dsp: assigned reserved memory node dsp1-memory@99000000
[   12.913846] remoteproc remoteproc2: 40800000.dsp is available
[  OK  ] Reached target Basic System.
[   12.926551] omap-rproc 41000000.dsp: assigned reserved memory node dsp2-memory@9f000000
[   12.941083] remoteproc remoteproc3: 41000000.dsp is available
         Starting TI IPC Daemon...
         [   12.960878] pixcir_ts 4-005c: pixcir_set_power_mode: can't read reg 0x33 : -121
Starting uim-sysfs.service...
[   12.977953] pixcir_ts 4-005c: Failed to set IDLE mode
[   12.998534] pixcir_ts: probe of 4-005c failed with error -121
         Starting RPC Bind Service...
[   13.317039] remoteproc remoteproc0: powering up 58820000.ipu
[[   13.325619] remoteproc remoteproc0: Booting fw image dra7-ipu1-fw.xem4, size 6680920
  OK  ] Started D-Bus System Message Bus.
[   13.345198] omap-iommu 58882000.mmu: 58882000.mmu: version 2.1
[   13.354353] vpe 489d0000.vpe: loading firmware vpdma-1b8.bin
[   13.386569] SCSI subsystem initialized
[   13.422823] virtio_rpmsg_bus virtio0: rpmsg host is online
[   13.428390] remoteproc remoteproc0: registered virtio0 (type 7)
[   13.450333] remoteproc remoteproc1: powering up 55020000.ipu
[   13.450344] remoteproc remoteproc1: Booting fw image dra7-ipu2-fw.xem4, size 3747220
[   13.450411] omap-iommu 55082000.mmu: 55082000.mmu: version 2.1
[   13.462331] omap_wdt: OMAP Watchdog Timer Rev 0x01: initial timeout 60 sec
[   13.497063] omap-sham 4b101000.sham: hw accel on OMAP rev 4.3
[   13.543014] virtio_rpmsg_bus virtio0: creating channel rpmsg-proto addr 0x3d
[   13.610927] remoteproc remoteproc0: remote processor 58820000.ipu is now up
[   13.638540] [drm] Initialized pvr 1.14.3699939 20110701 for 56000000.gpu on minor 1
[   13.651157] ahci 4a140000.sata: SSS flag set, parallel bus scan disabled
[   13.657916] ahci 4a140000.sata: AHCI 0001.0300 32 slots 1 ports 3 Gbps 0x1 impl platform mode
[   13.695030] ahci 4a140000.sata: flags: 64bit ncq sntf stag pm led clo only pmp pio slum part ccc apst
[   13.710105] omap-hdmi-audio omap-hdmi-audio.0.auto: snd-soc-dummy-dai <-> 58040000.encoder mapping ok
[   13.710113] omap-hdmi-audio omap-hdmi-audio.0.auto: ASoC: no DMI vendor name!
[   13.828121] scsi host0: ahci
[   13.831554] virtio_rpmsg_bus virtio1: rpmsg host is online
[   13.831603] remoteproc remoteproc1: registered virtio1 (type 7)
[   13.831608] remoteproc remoteproc1: remote processor 55020000.ipu is now up
[   13.838057] virtio_rpmsg_bus virtio1: creating channel rpmsg-rpc addr 0x65
[   13.844150] virtio_rpmsg_bus virtio1: creating channel rpmsg-rpc addr 0x66
[   13.871880] vpe 489d0000.vpe: Device registered as /dev/video0
[   14.017861] ata1: SATA max UDMA/133 mmio [mem 0x4a140000-0x4a1410ff] port 0x100 irq 82
[   14.044883] omap-aes 4b500000.aes: OMAP AES hw accel rev: 3.3
[   14.056656] omap-aes 4b500000.aes: will run requests pump with realtime priority
[   14.100581] remoteproc remoteproc3: powering up 41000000.dsp
[   14.109078] remoteproc remoteproc3: Booting fw image dra7-dsp2-fw.xe66, size 20392652
[   14.123067] omap-aes 4b700000.aes: OMAP AES hw accel rev: 3.3
[   14.130646] omap-aes 4b700000.aes: will run requests pump with realtime priority
[   14.187865] omap_hwmod: mmu0_dsp2: _wait_target_disable failed
[   14.193767] omap-iommu 41501000.mmu: 41501000.mmu: version 3.0
[   14.199737] omap-iommu 41502000.mmu: 41502000.mmu: version 3.0
[   14.272447] asoc-simple-card sound0: tlv320aic3x-hifi <-> 48468000.mcasp mapping ok
[   14.290191] asoc-simple-card sound0: ASoC: no DMI vendor name!
[   14.318836] virtio_rpmsg_bus virtio2: rpmsg host is online
[   14.318907] virtio_rpmsg_bus virtio2: creating channel rpmsg-proto addr 0x3d
[   14.350898] remoteproc remoteproc3: registered virtio2 (type 7)
[   14.357794] remoteproc remoteproc3: remote processor 41000000.dsp is now up
[   14.374223] ata1: SATA link down (SStatus 0 SControl 300)
[   14.440148] remoteproc remoteproc2: powering up 40800000.dsp
[   14.457075] remoteproc remoteproc2: Booting fw image dra7-dsp1-fw.xe66, size 20392652
[   14.483775] omap_hwmod: mmu0_dsp1: _wait_target_disable failed
[   14.489671] omap-iommu 40d01000.mmu: 40d01000.mmu: version 3.0
[   14.495636] omap-iommu 40d02000.mmu: 40d02000.mmu: version 3.0
         Starting TI MultiCore Tools Daemon...
[  OK  ] Reached target Containers.
[   14.621286] net eth1: initializing cpsw version 1.15 (0)
         Starting Login Service...
[   14.680405] net eth1: phy "/ocp/ethernet@48484000/mdio@48485000/ethernet-phy@2" not found on slave 1
         Starting Print notice about GPLv3 packages...
[   14.764689] virtio_rpmsg_bus virtio3: rpmsg host is online
[   14.766080] virtio_rpmsg_bus virtio3: creating channel rpmsg-proto addr 0x3d
[   14.769146] IPv6: ADDRCONF(NETDEV_UP): eth1: link is not ready
[   14.798844] net eth0: initializing cpsw version 1.15 (0)
[   14.814966] net eth0: phy "/ocp/ethernet@48484000/mdio@48485000/ethernet-phy@1" not found on slave 0
[   14.828589] IPv6: ADDRCONF(NETDEV_UP): eth0: link is not ready
[   14.838416] random: crng init done
[   14.838420] random: 7 urandom warning(s) missed due to ratelimiting
[  OK  ] Started Hardware RNG Entropy Gatherer Daemon.[   14.971296] remoteproc remoteproc2: registered virtio3 (type 7)

         Starting Save/Restore Sound Card State...
[   14.996071] remoteproc remoteproc2: remote processor 40800000.dsp is now up
[  OK  ] Started Periodic Command Scheduler.
[  OK  ] Started Kernel Logging Service.
[  OK  ] Started Job spooling tools.
[  OK  ] Started System Logging Service.
         Starting Avahi mDNS/DNS-SD Stack...
[  OK  ] Started Network Service.
[  OK  ] Started TI IPC Daemon.
[  OK  ] Started uim-sysfs.service.
[  OK  ] Started RPC Bind Service.
[  OK  ] Started TI MultiCore Tools Daemon.
[  OK  ] Found device /dev/ttyS2.
[  OK  ] Started Save/Restore Sound Card State.
[   15.132982] FAT-fs (mmcblk0p1): Volume was not properly unmounted. Some data may be corrupt. Please run fsck.
[   15.600207] pruss 4b200000.pruss: creating PRU cores and other child platform devices
[   15.616630] NET: Registered protocol family 44
[   15.624164] rpmsg_rpc virtio1.rpmsg-rpc.-1.101: probing service dce-callback with src 1024 dst 101
[   15.624355] rpmsg_rpc virtio1.rpmsg-rpc.-1.102: probing service rpmsg-dce with src 1025 dst 102
[   15.625200] rpmsg_rpc virtio1.rpmsg-rpc.-1.101: published functions = 4
[   15.625223] rpmsg_rpc virtio1.rpmsg-rpc.-1.102: published functions = 9
[   15.689929] xhci-hcd xhci-hcd.1.auto: xHCI Host Controller
[   15.689950] xhci-hcd xhci-hcd.1.auto: new USB bus registered, assigned bus number 1
[   15.691677] xhci-hcd xhci-hcd.1.auto: hcc params 0x0220f04c hci version 0x100 quirks 0x02010010
[   15.692009] xhci-hcd xhci-hcd.1.auto: irq 189, io mem 0x48890000
[   15.692201] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002
[   15.692210] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[   15.692218] usb usb1: Product: xHCI Host Controller
[   15.692224] usb usb1: Manufacturer: Linux 4.14.79-gbde58ab01e xhci-hcd
[   15.692234] usb usb1: SerialNumber: xhci-hcd.1.auto
[   15.693232] hub 1-0:1.0: USB hub found
[   15.693268] hub 1-0:1.0: 1 port detected
[   15.693898] xhci-hcd xhci-hcd.1.auto: xHCI Host Controller
[   15.693913] xhci-hcd xhci-hcd.1.auto: new USB bus registered, assigned bus number 2
[   15.693923] xhci-hcd xhci-hcd.1.auto: Host supports USB 3.0  SuperSpeed
[   15.693987] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[   15.694322] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003
[   15.694326] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[   15.694330] usb usb2: Product: xHCI Host Controller
[   15.694333] usb usb2: Manufacturer: Linux 4.14.79-gbde58ab01e xhci-hcd
[   15.694336] usb usb2: SerialNumber: xhci-hcd.1.auto
[   15.694873] hub 2-0:1.0: USB hub found
[   15.694897] hub 2-0:1.0: 1 port detected
[   16.008457] pruss 4b280000.pruss: creating PRU cores and other child platform devices
[   16.060710] remoteproc remoteproc4: 4b234000.pru is available
[   16.069508] pru-rproc 4b234000.pru: PRU rproc node /ocp/pruss_soc_bus@4b226004/pruss@0/pru@34000 probed successfully
[   16.113940] remoteproc remoteproc5: 4b238000.pru is available
[   16.126612] pru-rproc 4b238000.pru: PRU rproc node /ocp/pruss_soc_bus@4b226004/pruss@0/pru@38000 probed successfully
[   16.139434] remoteproc remoteproc6: 4b2b4000.pru is available
[   16.146321] pru-rproc 4b2b4000.pru: PRU rproc node /ocp/pruss_soc_bus@4b2a6004/pruss@0/pru@34000 probed successfully
[   16.158647] remoteproc remoteproc7: 4b2b8000.pru is available
[   16.165667] pru-rproc 4b2b8000.pru: PRU rproc node /ocp/pruss_soc_bus@4b2a6004/pruss@0/pru@38000 probed successfully
[  OK  ] Started Avahi mDNS/DNS-SD Stack.
[  OK  ] Reached target Sound Card.
[  OK  ] Listening on Load/Save RF Kill Switch Status /dev/rfkill Watch.
[  OK  ] Created slice system-systemd\x2dbacklight.slice.
         Starting Load/Save Screen Backlightghtness of backlight:backlight...
         Starting rc.pvr.service...
         Starting Wait for Network to be Configured...
[  OK  ] Reached target Network.
[  OK  ] Started Redis In-Memory Data Store.
         Starting Simple Network Management Protocol (SNMP) Daemon....
         Starting Permit User Sessions...
         Starting Enable and configure wl18xx bluetooth stack...
         Starting Network Name Resolution...
         Starting Lightning Fast Webserver With Light System Requirements...
[  OK  ] Started Load/Save Screen Backlight Brightness of backlight:backlight.
[  OK  ] Started Login Service.
[  OK  ] Started Permit User Sessions.
[  OK  ] Started Getty on tty1.
[  OK  ] Started Serial Getty on ttyS2.
[  OK  ] Reached target Login Prompts.
         Starting Synchronize System and HW clocks...
[FAILED] Failed to start Synchronize System and HW clocks.
See 'systemctl status sync-clocks.service' for details.
[  OK  ] Started Lightning Fast Webserver With Light System Requirements.
[  OK  ] Started Network Name Resolution.
[  OK  ] Reached target Host and Network Name Lookups.
[  OK  ] Started NFS status monitor for NFSv2/3 locking..
[   16.935600] PVR_K: UM DDK-(3699939) and KM DDK-(3699939) match. [ OK ]
[  OK  ] Started rc.pvr.service.
         Starting weston.service...
[  OK  ] Started weston.service.
         Starting telnetd.service...
[  OK  ] Started telnetd.service.
         Starting cm_startup.service...
         Starting thttpd.service...
[  OK  ] Started thttpd.service.
[  OK  ] Started cm_startup.service.
         Starting rng-tools.service...
[  OK  ] Started Simple Network Management Protocol (SNMP) Daemon..
[  OK  ] Started rng-tools.service.
[  OK  ] Started Enable and configure wl18xx bluetooth stack.
[   18.210893] omapdss error: HDMI I2C Master Error
[   19.093096] BUG: Bad page state in process weston  pfn:f1685
[   19.098794] page:efd94ab4 count:2048 mapcount:0 mapping:  (null) index:0x1
[   19.105700] flags: 0x80000000()
[   19.108855] raw: 80000000 00000000 00000001 ffffffff 00000800 00000100 00000200 00000000
[   19.116977] raw: 00000000
[   19.119604] page dumped because: nonzero _count
[   19.124147] Modules linked in: m50ssc(O) bc_example(O) pru_rproc pruss_intc xhci_plat_hcd xhci_hcd rpmsg_rpc rpmsg_proto pruss dwc3 udc_core snd_soc_simple_card snd_soc_simple_card_utils omap_aes_driver pruss_soc_bus snd_soc_omap_hdmi_audio ahci_platform pvrsrvkm(O) libahci_platform libahci libata omap_sham omap_wdt scsi_mod ti_vpe phy_omap_usb2 ti_sc ti_csc ti_vpdma dwc3_omap rtc_omap omap_des omap_remoteproc pixcir_i2c_ts snd_soc_tlv320aic3x virtio_rpmsg_bus des_generic rpmsg_core crypto_engine omap_crypto at24 remoteproc rtc_ds1307 rtc_palmas extcon_palmas sch_fq_codel uio_module_drv(O) uio ftdi_sio usbserial usbcore usb_common gdbserverproxy(O) cryptodev(O) cmemk(O)
[   19.183886] CPU: 0 PID: 688 Comm: weston Tainted: G           O    4.14.79-gbde58ab01e #1
[   19.192093] Hardware name: Generic DRA74X (Flattened Device Tree)
[   19.198207] Backtrace:
[   19.200670] [<c020b4dc>] (dump_backtrace) from [<c020b7c0>] (show_stack+0x18/0x1c)
[   19.208270]  r7:c0bb861c r6:200f0193 r5:00000000 r4:c1053d10
[   19.213955] [<c020b7a8>] (show_stack) from [<c0931348>] (dump_stack+0x90/0xa4)
[   19.221209] [<c09312b8>] (dump_stack) from [<c02e2f10>] (bad_page+0x100/0x160)
[   19.228458]  r7:c0bb861c r6:efd94ab4 r5:c1002d00 r4:c108199c
[   19.234140] [<c02e2e10>] (bad_page) from [<c02e306c>] (check_new_page_bad+0x7c/0x80)
[   19.241913]  r7:efd94aa4 r6:0000001e r5:c1054480 r4:00000000
[   19.247594] [<c02e2ff0>] (check_new_page_bad) from [<c02e5cd4>] (get_page_from_freelist+0x63c/0x958)
[   19.256760]  r5:c1054480 r4:00000000
[   19.260348] [<c02e5698>] (get_page_from_freelist) from [<c02e6764>] (__alloc_pages_nodemask+0xcc/0xec0)
[   19.269778]  r10:edff2580 r9:00000000 r8:c1003df8 r7:014000c0 r6:014200ca r5:00000081
[   19.277637]  r4:00000000
[   19.280180] [<c02e6698>] (__alloc_pages_nodemask) from [<c030f6f4>] (handle_mm_fault+0x59c/0xc50)
[   19.289087]  r10:edff2580 r9:00000055 r8:ffffe000 r7:014000c0 r6:d56f9000 r5:00000040
[   19.296946]  r4:b4efe000
[   19.299488] [<c030f158>] (handle_mm_fault) from [<c0213f34>] (do_page_fault+0x134/0x348)
[   19.307610]  r10:edff2580 r9:00000055 r8:b4efe000 r7:00000a07 r6:edff2540 r5:ed050d80
[   19.315468]  r4:ec93bfb0
[   19.318009] [<c0213e00>] (do_page_fault) from [<c020127c>] (do_DataAbort+0x38/0xb8)
[   19.325695]  r10:b6ad7989 r9:00000400 r8:ec93bfb0 r7:b4efe000 r6:c0213e00 r5:00000a07
[   19.333552]  r4:c1008c3c
[   19.336093] [<c0201244>] (do_DataAbort) from [<c020c680>] (__dabt_usr+0x40/0x60)
[   19.343516] Exception stack(0xec93bfb0 to 0xec93bff8)
[   19.348585] bfa0:                                     00000001 b51fe000 00000400 0000024b
[   19.356794] bfc0: b51feffc b4efdffc ff7c7572 b4efd004 00000000 00000400 b6ad7989 0009d990
[   19.365002] bfe0: 00001000 be95f2e8 00001000 b6ad79b4 200f0030 ffffffff
[   19.371642]  r8:30c5387d r7:30c5387d r6:ffffffff r5:200f0030 r4:b6ad79b4
[   19.378367] Disabling lock debugging due to kernel taint
[   19.472845] BUG: Bad page state in process M50QT  pfn:f17cd
[   19.478454] page:efd978d4 count:2048 mapcount:0 mapping:  (null) index:0x1
[   19.485363] flags: 0x80000000()
[   19.488519] raw: 80000000 00000000 00000001 ffffffff 00000800 00000100 00000200 00000000
[   19.496638] raw: 00000000
[   19.499264] page dumped because: nonzero _count
[   19.503809] Modules linked in: m50ssc(O) bc_example(O) pru_rproc pruss_intc xhci_plat_hcd xhci_hcd rpmsg_rpc rpmsg_proto pruss dwc3 udc_core snd_soc_simple_card snd_soc_simple_card_utils omap_aes_driver pruss_soc_bus snd_soc_omap_hdmi_audio ahci_platform pvrsrvkm(O) libahci_platform libahci libata omap_sham omap_wdt scsi_mod ti_vpe phy_omap_usb2 ti_sc ti_csc ti_vpdma dwc3_omap rtc_omap omap_des omap_remoteproc pixcir_i2c_ts snd_soc_tlv320aic3x virtio_rpmsg_bus des_generic rpmsg_core crypto_engine omap_crypto at24 remoteproc rtc_ds1307 rtc_palmas extcon_palmas sch_fq_codel uio_module_drv(O) uio ftdi_sio usbserial usbcore usb_common gdbserverproxy(O) cryptodev(O) cmemk(O)
[   19.563546] CPU: 0 PID: 697 Comm: M50QT Tainted: G    B      O    4.14.79-gbde58ab01e #1
[   19.571666] Hardware name: Generic DRA74X (Flattened Device Tree)
[   19.577780] Backtrace:
[   19.580244] [<c020b4dc>] (dump_backtrace) from [<c020b7c0>] (show_stack+0x18/0x1c)
[   19.587843]  r7:c0bb861c r6:200d0193 r5:00000000 r4:c1053d10
[   19.593528] [<c020b7a8>] (show_stack) from [<c0931348>] (dump_stack+0x90/0xa4)
[   19.600784] [<c09312b8>] (dump_stack) from [<c02e2f10>] (bad_page+0x100/0x160)
[   19.608034]  r7:c0bb861c r6:efd978d4 r5:c1054480 r4:c108199c
[   19.613716] [<c02e2e10>] (bad_page) from [<c02e306c>] (check_new_page_bad+0x7c/0x80)
[   19.621488]  r7:eed33590 r6:00000000 r5:c1054480 r4:00000000
[   19.627169] [<c02e2ff0>] (check_new_page_bad) from [<c02e5cd4>] (get_page_from_freelist+0x63c/0x958)
[   19.636336]  r5:c1054480 r4:00000000
[   19.639923] [<c02e5698>] (get_page_from_freelist) from [<c02e6764>] (__alloc_pages_nodemask+0xcc/0xec0)
[   19.649354]  r10:00000001 r9:00000000 r8:c1003df8 r7:ec946000 r6:014200ca r5:00000081
[   19.657212]  r4:00000000
[   19.659754] [<c02e6698>] (__alloc_pages_nodemask) from [<c02f8ec4>] (shmem_getpage_gfp.constprop.4+0x574/0xae0)
[   19.669882]  r10:00000001 r9:00000176 r8:ec84a1d0 r7:ec946000 r6:ec943e40 r5:c1003ff8
[   19.677740]  r4:ed92f488
[   19.680281] [<c02f8950>] (shmem_getpage_gfp.constprop.4) from [<c02fac08>] (shmem_fault+0x6c/0x1a8)
[   19.689361]  r10:ec946040 r9:00000055 r8:ec943e40 r7:014200ca r6:ec943e40 r5:ec84a1d0
[   19.697219]  r4:dfc51c98
[   19.699763] [<c02fab9c>] (shmem_fault) from [<c030a934>] (__do_fault+0x20/0x70)
[   19.707099]  r9:00000055 r8:ec943e40 r7:014200ca r6:dfc51c98 r5:ec943e40 r4:edac6110
[   19.714873] [<c030a914>] (__do_fault) from [<c030f8e0>] (handle_mm_fault+0x788/0xc50)
[   19.722731]  r5:00000040 r4:edac6110
[   19.726319] [<c030f158>] (handle_mm_fault) from [<c0213f34>] (do_page_fault+0x134/0x348)
[   19.734440]  r10:ec946040 r9:00000055 r8:b2d42000 r7:00000a07 r6:ec946000 r5:ed054a40
[   19.742297]  r4:ec943fb0
[   19.744838] [<c0213e00>] (do_page_fault) from [<c020127c>] (do_DataAbort+0x38/0xb8)
[   19.752524]  r10:00049848 r9:00000320 r8:ec943fb0 r7:b2d42000 r6:c0213e00 r5:00000a07
[   19.760382]  r4:c1008c3c
[   19.762924] [<c0201244>] (do_DataAbort) from [<c020c680>] (__dabt_usr+0x40/0x60)
[   19.770346] Exception stack(0xec943fb0 to 0xec943ff8)
[   19.775415] 3fa0:                                     b2d42000 00000000 b2d43000 00000000
[   19.783624] 3fc0: 000001e0 00000000 00000000 000001e0 0006fa18 00000320 00049848 b3dcb42c
[   19.791832] 3fe0: 00000000 becaac98 b682466c b6922da8 200d0010 ffffffff
[   19.798470]  r8:30c5387d r7:30c5387d r6:ffffffff r5:200d0010 r4:b6922da8
[   19.821877] BUG: Bad page state in process systemd-journal  pfn:f1285
[   19.828354] page:efd8bab4 count:2048 mapcount:0 mapping:  (null) index:0x1
[   19.835268] flags: 0x80000000()
[   19.838437] raw: 80000000 00000000 00000001 ffffffff 00000800 00000100 00000200 00000000
[   19.846570] raw: 00000000
[   19.849203] page dumped because: nonzero _count
[   19.853748] Modules linked in: m50ssc(O) bc_example(O) pru_rproc pruss_intc xhci_plat_hcd xhci_hcd rpmsg_rpc rpmsg_proto pruss dwc3 udc_core snd_soc_simple_card snd_soc_simple_card_utils omap_aes_driver pruss_soc_bus snd_soc_omap_hdmi_audio ahci_platform pvrsrvkm(O) libahci_platform libahci libata omap_sham omap_wdt scsi_mod ti_vpe phy_omap_usb2 ti_sc ti_csc ti_vpdma dwc3_omap rtc_omap omap_des omap_remoteproc pixcir_i2c_ts snd_soc_tlv320aic3x virtio_rpmsg_bus des_generic rpmsg_core crypto_engine omap_crypto at24 remoteproc rtc_ds1307 rtc_palmas extcon_palmas sch_fq_codel uio_module_drv(O) uio ftdi_sio usbserial usbcore usb_common gdbserverproxy(O) cryptodev(O) cmemk(O)
[   19.913485] CPU: 0 PID: 90 Comm: systemd-journal Tainted: G    B      O    4.14.79-gbde58ab01e #1
[   19.922391] Hardware name: Generic DRA74X (Flattened Device Tree)
[   19.928505] Backtrace:
[   19.930969] [<c020b4dc>] (dump_backtrace) from [<c020b7c0>] (show_stack+0x18/0x1c)
[   19.938568]  r7:c0bb861c r6:200f0193 r5:00000000 r4:c1053d10
[   19.944253] [<c020b7a8>] (show_stack) from [<c0931348>] (dump_stack+0x90/0xa4)
[   19.951508] [<c09312b8>] (dump_stack) from [<c02e2f10>] (bad_page+0x100/0x160)
[   19.958757]  r7:c0bb861c r6:efd8bab4 r5:c1054480 r4:c108199c
[   19.964440] [<c02e2e10>] (bad_page) from [<c02e306c>] (check_new_page_bad+0x7c/0x80)
[   19.972213]  r7:efd8baa4 r6:0000000e r5:c1054480 r4:00000000
[   19.977894] [<c02e2ff0>] (check_new_page_bad) from [<c02e5cd4>] (get_page_from_freelist+0x63c/0x958)
[   19.987061]  r5:c1054480 r4:00000000
[   19.990649] [<c02e5698>] (get_page_from_freelist) from [<c02e6764>] (__alloc_pages_nodemask+0xcc/0xec0)
[   20.000078]  r10:edff23c0 r9:00000000 r8:c1003df8 r7:dfc519c0 r6:014200ca r5:00000081
[   20.007936]  r4:00000000
[   20.010479] [<c02e6698>] (__alloc_pages_nodemask) from [<c030aba0>] (wp_page_copy+0x17c/0x604)
[   20.019124]  r10:edff23c0 r9:edff2380 r8:b5fa6000 r7:dfc519c0 r6:affa27df r5:00000000
[   20.026982]  r4:ed961e40
[   20.029523] [<c030aa24>] (wp_page_copy) from [<c030ca88>] (do_wp_page+0xa8/0x5a0)
[   20.037034]  r10:edff23c0 r9:00000055 r8:ffffe000 r7:00000000 r6:affa27df r5:dfc519c0
[   20.044892]  r4:ed961e40
[   20.047434] [<c030c9e0>] (do_wp_page) from [<c030f8cc>] (handle_mm_fault+0x774/0xc50)
[   20.055293]  r8:ffffe000 r7:00000000 r6:affa27df r5:00000040 r4:affa27df
[   20.062022] [<c030f158>] (handle_mm_fault) from [<c0213f34>] (do_page_fault+0x134/0x348)
[   20.070143]  r10:edff23c0 r9:00000055 r8:b5fa6c04 r7:00000a0f r6:edff2380 r5:ed82a1c0
[   20.078001]  r4:ed961fb0
[   20.080541] [<c0213e00>] (do_page_fault) from [<c020127c>] (do_DataAbort+0x38/0xb8)
[   20.088226]  r10:b6171008 r9:0000003d r8:ed961fb0 r7:b5fa6c04 r6:c0213e00 r5:00000a0f
[   20.096084]  r4:c1008cbc
[   20.098625] [<c0201244>] (do_DataAbort) from [<c020c680>] (__dabt_usr+0x40/0x60)
[   20.106047] Exception stack(0xed961fb0 to 0xed961ff8)
[   20.111115] 1fa0:                                     0010003e 0010003e b6171045 00000000
[   20.119324] 1fc0: 0042ecb0 00441a9c 000001ff b5f6f008 b5b6e008 0000003d b6171008 00000000
[   20.127533] 1fe0: 0000deff bec6c620 00000080 b6c0cc34 800f0010 ffffffff
[   20.134171]  r8:30c5387d r7:30c5387d r6:ffffffff r5:800f0010 r4:b6c0cc34
[   20.159444] BUG: Bad page state in process weston  pfn:f1385
[   20.165145] page:efd8deb4 count:2048 mapcount:0 mapping:  (null) index:0x1
[   20.172057] flags: 0x80000000()
[   20.175216] raw: 80000000 00000000 00000001 ffffffff 00000800 00000100 00000200 00000000
[   20.183343] raw: 00000000
[   20.185972] page dumped because: nonzero _count
[   20.190519] Modules linked in: m50ssc(O) bc_example(O) pru_rproc pruss_intc xhci_plat_hcd xhci_hcd rpmsg_rpc rpmsg_proto pruss dwc3 udc_core snd_soc_simple_card snd_soc_simple_card_utils omap_aes_driver pruss_soc_bus snd_soc_omap_hdmi_audio ahci_platform pvrsrvkm(O) libahci_platform libahci libata omap_sham omap_wdt scsi_mod ti_vpe phy_omap_usb2 ti_sc ti_csc ti_vpdma dwc3_omap rtc_omap omap_des omap_remoteproc pixcir_i2c_ts snd_soc_tlv320aic3x virtio_rpmsg_bus des_generic rpmsg_core crypto_engine omap_crypto at24 remoteproc rtc_ds1307 rtc_palmas extcon_palmas sch_fq_codel uio_module_drv(O) uio ftdi_sio usbserial usbcore usb_common gdbserverproxy(O) cryptodev(O) cmemk(O)
[   20.250348] CPU: 0 PID: 688 Comm: weston Tainted: G    B      O    4.14.79-gbde58ab01e #1
[   20.258559] Hardware name: Generic DRA74X (Flattened Device Tree)
[   20.264672] Backtrace:
[   20.267136] [<c020b4dc>] (dump_backtrace) from [<c020b7c0>] (show_stack+0x18/0x1c)
[   20.274735]  r7:c0bb861c r6:20010193 r5:00000000 r4:c1053d10
[   20.280418] [<c020b7a8>] (show_stack) from [<c0931348>] (dump_stack+0x90/0xa4)
[   20.287672] [<c09312b8>] (dump_stack) from [<c02e2f10>] (bad_page+0x100/0x160)
[   20.294921]  r7:c0bb861c r6:efd8deb4 r5:c1054480 r4:c108199c
[   20.300602] [<c02e2e10>] (bad_page) from [<c02e306c>] (check_new_page_bad+0x7c/0x80)
[   20.308374]  r7:efd8dea4 r6:0000001c r5:c1054480 r4:00000000
[   20.314054] [<c02e2ff0>] (check_new_page_bad) from [<c02e5cd4>] (get_page_from_freelist+0x63c/0x958)
[   20.323221]  r5:c1054480 r4:00000000
[   20.326809] [<c02e5698>] (get_page_from_freelist) from [<c02e6764>] (__alloc_pages_nodemask+0xcc/0xec0)
[   20.336239]  r10:edff2580 r9:00000000 r8:c1003df8 r7:014000c0 r6:014200ca r5:00000081
[   20.344098]  r4:00000000
[   20.346642] [<c02e6698>] (__alloc_pages_nodemask) from [<c030f6f4>] (handle_mm_fault+0x59c/0xc50)
[   20.355549]  r10:edff2580 r9:00000055 r8:ffffe000 r7:014000c0 r6:dfc51a90 r5:00000040
[   20.363407]  r4:b46df000
[   20.365949] [<c030f158>] (handle_mm_fault) from [<c0213f34>] (do_page_fault+0x134/0x348)
[   20.374071]  r10:edff2580 r9:00000055 r8:b46df000 r7:00000a07 r6:edff2540 r5:ed050d80
[   20.381929]  r4:ec93bfb0
[   20.384470] [<c0213e00>] (do_page_fault) from [<c020127c>] (do_DataAbort+0x38/0xb8)
[   20.392156]  r10:b6ad7989 r9:00000320 r8:ec93bfb0 r7:b46df000 r6:c0213e00 r5:00000a07
[   20.400013]  r4:c1008c3c
[   20.402554] [<c0201244>] (do_DataAbort) from [<c020c680>] (__dabt_usr+0x40/0x60)
[   20.409977] Exception stack(0xec93bfb0 to 0xec93bff8)
[   20.415047] bfa0:                                     000002c1 b4c57e80 00000320 0000007b
[   20.423256] bfc0: b4c57ffc b46deffc ffefebe7 b46dee84 00000000 00000320 b6ad7989 000c4ad0
[   20.431464] bfe0: 00000c80 be95f2e8 00000c80 b6ad79b4 20010030 ffffffff
[   20.438103]  r8:30c5387d r7:30c5387d r6:ffffffff r5:20010030 r4:b6ad79b4
[   20.533433] Unable to handle kernel paging request at virtual address 40000000
[   20.540729] pgd = ed22b0c0
[   20.540733] [40000000] *pgd=00000000
[   20.540741] detected fb_set_par error, error code: -16
[   20.540745] Internal error: Oops: 205 [#1] PREEMPT SMP ARM
[   20.540749] Modules linked in: m50ssc(O) bc_example(O) pru_rproc pruss_intc xhci_plat_hcd xhci_hcd rpmsg_rpc rpmsg_proto pruss dwc3 udc_core snd_soc_simple_card snd_soc_simple_card_utils omap_aes_driver pruss_soc_bus snd_soc_omap_hdmi_audio ahci_platform pvrsrvkm(O) libahci_platform libahci libata omap_sham omap_wdt scsi_mod ti_vpe phy_omap_usb2 ti_sc ti_csc ti_vpdma dwc3_omap rtc_omap omap_des omap_remoteproc pixcir_i2c_ts snd_soc_tlv320aic3x virtio_rpmsg_bus des_generic rpmsg_core crypto_engine omap_crypto at24 remoteproc rtc_ds1307 rtc_palmas extcon_palmas sch_fq_codel uio_module_drv(O) uio ftdi_sio usbserial usbcore usb_common gdbserverproxy(O) cryptodev(O) cmemk(O)
[   20.540892] CPU: 1 PID: 802 Comm: basename Tainted: G    B      O    4.14.79-gbde58ab01e #1
[   20.540896] Hardware name: Generic DRA74X (Flattened Device Tree)
[   20.540899] task: d4fcde80 task.stack: d4fc2000
[   20.540912] PC is at handle_mm_fault+0x170/0xc50
[   20.540917] LR is at 0xbd000
[   20.540921] pc : [<c030f2c8>]    lr : [<000bd000>]    psr: 200a0113
[   20.540925] sp : d4fc3c60  ip : 00001000  fp : d4fc3cec
[   20.540929] r10: edb25c40  r9 : 00000015  r8 : 000bd686
[   20.540932] r7 : 014200ca  r6 : 00000000  r5 : 00000000  r4 : ed22b0c0
[   20.540936] r3 : 40000000  r2 : 40000000  r1 : 00000800  r0 : edb25c00
[   20.540941] Flags: nzCv  IRQs on  FIQs on  Mode SVC_32  ISA ARM  Segment user
[   20.540945] Control: 30c5387d  Table: ad22b0c0  DAC: 55555555
[   20.540948] Process basename (pid: 802, stack limit = 0xd4fc2210)
[   20.540953] Stack: (0xd4fc3c60 to 0xd4fc4000)
[   20.540958] 3c60: 00000000 00000002 c0e63d50 00000000 eed42554 01000200 5c15c7b2 19076d6d
[   20.540963] 3c80: d4f489c0 00000015 014200ca 0000009d 000bd000 40000000 ed22b0c0 00000000
[   20.540968] 3ca0: 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000
[   20.540973] 3cc0: d4fc3cec d4fc3e18 d4fcde80 edb25c00 00000a05 000bd686 00000015 edb25c40
[   20.540977] 3ce0: d4fc3d3c d4fc3cf0 c0213f34 c030f164 d4f489c0 c0c443c8 0000075f 04600000
[   20.540982] 3d00: edb25c00 d4f48d68 00000800 d4fc3d18 c031333c c1008c1c 00000a05 c02141d4
[   20.540987] 3d20: 000bd686 00000a05 d4fc2000 00000009 d4fc3d64 d4fc3d40 c02142a8 c0213e0c
[   20.540993] 3d40: c1008c1c 00000a05 c02141d4 000bd686 d4fc3e18 d4fc2000 d4fc3e14 d4fc3d68

