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Errors (9 items)

& first defined here board tdi0.c
G first defined here board kphy.c
& first defined here board tkphy.c
& first defined here tieschsp.c

G firs defined here teschsp.c

3 gmake: ** [all] Error 2 ethercat slave_demo_AM335x am
3 gmake[1L]: * [ethercat_slave_demo_AM335¢_ethercat slave_demo AM335x aim

G recipe for targetal faled makefile
@ recipe fortarget 'ethercat,_slave,demo_AM33. makefile
Warnings (4 items)

& nline function ‘bsp_get_pdl_sccess_perm’ de etherca slave_demo_AM335x arm
& inline function ‘bsp_pdi_access_perm_array'¢ ethercat_slave,demo AM335x_arm
& inline function ‘bsp_pdi_access_perm_dword' ethercat_slave_demo_AM335x_arm
line function 'bsp pdi access perm word' ¢ ethercat slave demo AM335x arm

Jethercat slave_demo ANB35x aim.
Jethercat slave_demo AM335x arm
Jethercat slave_demo AM335x arm
Jethercat slave_demo AM335x arm
Jethercat slave_demo AM335x arm

Jethercat slave_demo AM335x_arm/AMS.
Jethercat slave_demo AM335x_arm/AMS.
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71 void Board_phyLedConfig(uint32_t mdioBaseAddress, uint32_t phyllum,
2 uints T mode)

30

7

75
76 CSL_MDIO_phyRegRead(ndioBaseAddress, phylium, TLKPHY_PHYCR_REG, Sphyregval);
7

75 switch(mode)

uintls_t phyregval = 0;

7
a0 case LED_CFG_MODEL:

a1 phyregval |= (1 << 5);  //Set LeD_CF6[o] to 1

a2 break;

&3

& case LED_CFG_MoDE2:

a5 phyregval &= GxFFCF; //Set LED_CFG[0],LED_CFG[1] to 0

a6 break;

&7

& case LED_CFG_MODES:

a9 phyregval &= 6xFFDF; //Set LED_CFG[0] to 0

%0 phyregval |- 0x0040; //Set LeD CFo[1] to 1

o1 break;

2 3

o3

92 CSL_MDIO_ phyReghrite(ndioBaseAddress, phylum, TLKPHY_PHYCR_REG, phyregval);
o5

9%

97

93 void Board_TLK110_phyLedConfighode3(uint32_t mdioBaseAddress, uint32_t phylum)
99 {

100 uintls_t phyregval = 0;

101

102 CSL_MDIO_phyRegRead(ndioBaseAddress, phylium, TLKPHY_PHYCR_REG, Sphyregval);
103




