Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0000000000 [0x410fd034]
[    0.000000] Linux version 6.6.44-ti-01478-g541c20281af7-dirty (oe-user@oe-host) (aarch64-oe-linux-gcc (GCC) 13.3.0, GNU ld (GNU                                                                                                           Binutils) 2.42.0.20240723) #1 SMP PREEMPT Thu Nov 14 19:20:24 UTC 2024
[    0.000000] KASLR disabled due to lack of seed
[    0.000000] Machine model: Texas Instruments J722S ECU1270
[    0.000000] efi: UEFI not found.
[    0.000000] Reserved memory: created CMA memory pool at 0x00000008c8000000, size 896 MiB
[    0.000000] OF: reserved mem: initialized node linux,cma, compatible id shared-dma-pool
[    0.000000] OF: reserved mem: 0x00000008c8000000..0x00000008ffffffff (917504 KiB) map reusable linux,cma
[    0.000000] OF: reserved mem: 0x0000000080000000..0x000000008007ffff (512 KiB) nomap non-reusable tfa@80000000
[    0.000000] OF: reserved mem: 0x000000009e800000..0x000000009fffffff (24576 KiB) nomap non-reusable optee@9e800000
[    0.000000] Reserved memory: created DMA memory pool at 0x00000000a0000000, size 1 MiB
[    0.000000] OF: reserved mem: initialized node r5f-dma-memory@a0000000, compatible id shared-dma-pool
[    0.000000] OF: reserved mem: 0x00000000a0000000..0x00000000a00fffff (1024 KiB) nomap non-reusable r5f-dma-memory@a0000000
[    0.000000] Reserved memory: created DMA memory pool at 0x00000000a0100000, size 15 MiB
[    0.000000] OF: reserved mem: initialized node r5f-memory@a0100000, compatible id shared-dma-pool
[    0.000000] OF: reserved mem: 0x00000000a0100000..0x00000000a0ffffff (15360 KiB) nomap non-reusable r5f-memory@a0100000
[    0.000000] Reserved memory: created DMA memory pool at 0x00000000a1000000, size 1 MiB
[    0.000000] OF: reserved mem: initialized node mcu-r5fss-dma-memory-region@a1000000, compatible id shared-dma-pool
[    0.000000] OF: reserved mem: 0x00000000a1000000..0x00000000a10fffff (1024 KiB) nomap non-reusable mcu-r5fss-dma-memory-region@a                                                                                                          1000000
[    0.000000] Reserved memory: created DMA memory pool at 0x00000000a1100000, size 15 MiB
[    0.000000] OF: reserved mem: initialized node mcu-r5fss-memory-region@a1100000, compatible id shared-dma-pool
[    0.000000] OF: reserved mem: 0x00000000a1100000..0x00000000a1ffffff (15360 KiB) nomap non-reusable mcu-r5fss-memory-region@a110                                                                                                          0000
[    0.000000] Reserved memory: created DMA memory pool at 0x00000000a2000000, size 1 MiB
[    0.000000] OF: reserved mem: initialized node main-r5fss-dma-memory-region@a2000000, compatible id shared-dma-pool
[    0.000000] OF: reserved mem: 0x00000000a2000000..0x00000000a20fffff (1024 KiB) nomap non-reusable main-r5fss-dma-memory-region@                                                                                                          a2000000
[    0.000000] Reserved memory: created DMA memory pool at 0x00000000a2100000, size 15 MiB
[    0.000000] OF: reserved mem: initialized node main-r5fss-memory-region@a2100000, compatible id shared-dma-pool
[    0.000000] OF: reserved mem: 0x00000000a2100000..0x00000000a2ffffff (15360 KiB) nomap non-reusable main-r5fss-memory-region@a21                                                                                                          00000
[    0.000000] Reserved memory: created DMA memory pool at 0x00000000a3000000, size 1 MiB
[    0.000000] OF: reserved mem: initialized node c7x-dma-memory@a3000000, compatible id shared-dma-pool
[    0.000000] OF: reserved mem: 0x00000000a3000000..0x00000000a30fffff (1024 KiB) nomap non-reusable c7x-dma-memory@a3000000
[    0.000000] Reserved memory: created DMA memory pool at 0x00000000a3100000, size 15 MiB
[    0.000000] OF: reserved mem: initialized node c7x-memory@a3100000, compatible id shared-dma-pool
[    0.000000] OF: reserved mem: 0x00000000a3100000..0x00000000a3ffffff (15360 KiB) nomap non-reusable c7x-memory@a3100000
[    0.000000] Reserved memory: created DMA memory pool at 0x00000000a4000000, size 1 MiB
[    0.000000] OF: reserved mem: initialized node c7x-dma-memory@a4000000, compatible id shared-dma-pool
[    0.000000] OF: reserved mem: 0x00000000a4000000..0x00000000a40fffff (1024 KiB) nomap non-reusable c7x-dma-memory@a4000000
[    0.000000] Reserved memory: created DMA memory pool at 0x00000000a4100000, size 15 MiB
[    0.000000] OF: reserved mem: initialized node c7x-memory@a4100000, compatible id shared-dma-pool
[    0.000000] OF: reserved mem: 0x00000000a4100000..0x00000000a4ffffff (15360 KiB) nomap non-reusable c7x-memory@a4100000
[    0.000000] OF: reserved mem: 0x00000000a5000000..0x00000000a57fffff (8192 KiB) nomap non-reusable ipc-memories@a5000000
[    0.000000] Zone ranges:
[    0.000000]   DMA      [mem 0x0000000080000000-0x00000000ffffffff]
[    0.000000]   DMA32    empty
[    0.000000]   Normal   [mem 0x0000000100000000-0x00000008ffffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000080000000-0x000000008007ffff]
[    0.000000]   node   0: [mem 0x0000000080080000-0x000000009e7fffff]
[    0.000000]   node   0: [mem 0x000000009e800000-0x00000000a57fffff]
[    0.000000]   node   0: [mem 0x00000000a5800000-0x00000000ffffffff]
[    0.000000]   node   0: [mem 0x0000000880000000-0x00000008ffffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000080000000-0x00000008ffffffff]
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: Trusted OS migration not required
[    0.000000] psci: SMC Calling Convention v1.5
[    0.000000] percpu: Embedded 20 pages/cpu s43176 r8192 d30552 u81920
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: detected: GIC system register CPU interface
[    0.000000] CPU features: detected: ARM erratum 845719
[    0.000000] alternatives: applying boot alternatives
[    0.000000] Kernel command line: console=ttyS2,115200n8 root=/dev/mmcblk1p2 rauc.slot=system0 rw rootfstype=ext4 rootwait
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes, linear)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes, linear)
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1032192
[    0.000000] mem auto-init: stack:all(zero), heap alloc:off, heap free:off
[    0.000000] software IO TLB: area num 4.
[    0.000000] software IO TLB: mapped [mem 0x00000000fbfff000-0x00000000fffff000] (64MB)
[    0.000000] Memory: 2993576K/4194304K available (12608K kernel code, 1276K rwdata, 4220K rodata, 2496K init, 528K bss, 283224K r                                                                                                          eserved, 917504K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] rcu: Preemptible hierarchical RCU implementation.
[    0.000000] rcu:     RCU event tracing is enabled.
[    0.000000] rcu:     RCU restricting CPUs from NR_CPUS=256 to nr_cpu_ids=4.
[    0.000000]  Trampoline variant of Tasks RCU enabled.
[    0.000000]  Tracing variant of Tasks RCU enabled.
[    0.000000] rcu: RCU calculated value of scheduler-enlistment delay is 25 jiffies.
[    0.000000] rcu: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=4
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] GICv3: GIC: Using split EOI/Deactivate mode
[    0.000000] GICv3: 256 SPIs implemented
[    0.000000] GICv3: 0 Extended SPIs implemented
[    0.000000] Root IRQ handler: gic_handle_irq
[    0.000000] GICv3: GICv3 features: 16 PPIs
[    0.000000] GICv3: CPU0: found redistributor 0 region 0:0x0000000001880000
[    0.000000] ITS [mem 0x01820000-0x0182ffff]
[    0.000000] GIC: enabling workaround for ITS: Socionext Synquacer pre-ITS
[    0.000000] ITS@0x0000000001820000: Devices Table too large, reduce ids 20->19
[    0.000000] ITS@0x0000000001820000: allocated 524288 Devices @880800000 (flat, esz 8, psz 64K, shr 0)
[    0.000000] ITS: using cache flushing for cmd queue
[    0.000000] GICv3: using LPI property table @0x0000000880040000
[    0.000000] GIC: using cache flushing for LPI property table
[    0.000000] GICv3: CPU0: using allocated LPI pending table @0x0000000880050000
[    0.000000] rcu: srcu_init: Setting srcu_struct sizes based on contention.
[    0.000000] arch_timer: cp15 timer(s) running at 200.00MHz (phys).
[    0.000000] clocksource: arch_sys_counter: mask: 0x3ffffffffffffff max_cycles: 0x2e2049d3e8, max_idle_ns: 440795210634 ns
[    0.000001] sched_clock: 58 bits at 200MHz, resolution 5ns, wraps every 4398046511102ns
[    0.000350] Console: colour dummy device 80x25
[    0.000402] Calibrating delay loop (skipped), value calculated using timer frequency.. 400.00 BogoMIPS (lpj=800000)
[    0.000413] pid_max: default: 32768 minimum: 301
[    0.000498] LSM: initializing lsm=capability,selinux,integrity
[    0.000523] SELinux:  Initializing.
[    0.000650] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes, linear)
[    0.000668] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes, linear)
[    0.002400] RCU Tasks: Setting shift to 2 and lim to 1 rcu_task_cb_adjust=1.
[    0.002468] RCU Tasks Trace: Setting shift to 2 and lim to 1 rcu_task_cb_adjust=1.
[    0.002645] rcu: Hierarchical SRCU implementation.
[    0.002649] rcu:     Max phase no-delay instances is 1000.
[    0.002890] Platform MSI: msi-controller@1820000 domain created
[    0.003125] PCI/MSI: /bus@f0000/interrupt-controller@1800000/msi-controller@1820000 domain created
[    0.003402] EFI services will not be available.
[    0.003654] smp: Bringing up secondary CPUs ...
[    0.004317] Detected VIPT I-cache on CPU1
[    0.004392] GICv3: CPU1: found redistributor 1 region 0:0x00000000018a0000
[    0.004408] GICv3: CPU1: using allocated LPI pending table @0x0000000880060000
[    0.004458] CPU1: Booted secondary processor 0x0000000001 [0x410fd034]
[    0.005140] Detected VIPT I-cache on CPU2
[    0.005196] GICv3: CPU2: found redistributor 2 region 0:0x00000000018c0000
[    0.005210] GICv3: CPU2: using allocated LPI pending table @0x0000000880070000
[    0.005243] CPU2: Booted secondary processor 0x0000000002 [0x410fd034]
[    0.005837] Detected VIPT I-cache on CPU3
[    0.005893] GICv3: CPU3: found redistributor 3 region 0:0x00000000018e0000
[    0.005906] GICv3: CPU3: using allocated LPI pending table @0x0000000880080000
[    0.005936] CPU3: Booted secondary processor 0x0000000003 [0x410fd034]
[    0.006008] smp: Brought up 1 node, 4 CPUs
[    0.006015] SMP: Total of 4 processors activated.
[    0.006019] CPU features: detected: 32-bit EL0 Support
[    0.006023] CPU features: detected: CRC32 instructions
[    0.006081] CPU: All CPU(s) started at EL2
[    0.006084] alternatives: applying system-wide alternatives
[    0.007731] devtmpfs: initialized
[    0.018828] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 7645041785100000 ns
[    0.018852] futex hash table entries: 1024 (order: 4, 65536 bytes, linear)
[    0.041396] pinctrl core: initialized pinctrl subsystem
[    0.041930] DMI not present or invalid.
[    0.042531] NET: Registered PF_NETLINK/PF_ROUTE protocol family
[    0.043427] DMA: preallocated 512 KiB GFP_KERNEL pool for atomic allocations
[    0.043509] DMA: preallocated 512 KiB GFP_KERNEL|GFP_DMA pool for atomic allocations
[    0.043570] DMA: preallocated 512 KiB GFP_KERNEL|GFP_DMA32 pool for atomic allocations
[    0.043640] audit: initializing netlink subsys (disabled)
[    0.043834] audit: type=2000 audit(0.040:1): state=initialized audit_enabled=0 res=1
[    0.044303] thermal_sys: Registered thermal governor 'step_wise'
[    0.044308] thermal_sys: Registered thermal governor 'power_allocator'
[    0.044350] cpuidle: using governor menu
[    0.044521] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.044613] ASID allocator initialised with 65536 entries
[    0.059702] platform 30220000.dss: Fixed dependency cycle(s) with /bus@f0000/dsi@30500000
[    0.059937] platform 30220000.dss: Fixed dependency cycle(s) with /bus@f0000/dsi@30500000
[    0.060034] platform 30500000.dsi: Fixed dependency cycle(s) with /bus@f0000/dss@30220000
[    0.060093] platform 30500000.dsi: Fixed dependency cycle(s) with /bus@f0000/i2c@20000000/bridge@3d
[    0.063093] platform hdmi-out: Fixed dependency cycle(s) with /bus@f0000/i2c@20000000/bridge@3d
[    0.063509] Modules: 27440 pages in range for non-PLT usage
[    0.063515] Modules: 518960 pages in range for PLT usage
[    0.064242] HugeTLB: registered 1.00 GiB page size, pre-allocated 0 pages
[    0.064251] HugeTLB: 0 KiB vmemmap can be freed for a 1.00 GiB page
[    0.064256] HugeTLB: registered 32.0 MiB page size, pre-allocated 0 pages
[    0.064259] HugeTLB: 0 KiB vmemmap can be freed for a 32.0 MiB page
[    0.064263] HugeTLB: registered 2.00 MiB page size, pre-allocated 0 pages
[    0.064266] HugeTLB: 0 KiB vmemmap can be freed for a 2.00 MiB page
[    0.064270] HugeTLB: registered 64.0 KiB page size, pre-allocated 0 pages
[    0.064273] HugeTLB: 0 KiB vmemmap can be freed for a 64.0 KiB page
[    0.065721] k3-chipinfo 43000014.chipid: Family:J722S rev:SR1.0 JTAGID[0x0bba002f] Detected
[    0.066539] iommu: Default domain type: Translated
[    0.066551] iommu: DMA domain TLB invalidation policy: strict mode
[    0.066925] SCSI subsystem initialized
[    0.067254] usbcore: registered new interface driver usbfs
[    0.067280] usbcore: registered new interface driver hub
[    0.067316] usbcore: registered new device driver usb
[    0.067866] pps_core: LinuxPPS API ver. 1 registered
[    0.067870] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.067882] PTP clock support registered
[    0.068058] EDAC MC: Ver: 3.0.0
[    0.068629] scmi_core: SCMI protocol bus registered
[    0.068935] FPGA manager framework
[    0.069022] Advanced Linux Sound Architecture Driver Initialized.
[    0.069929] vgaarb: loaded
[    0.070314] clocksource: Switched to clocksource arch_sys_counter
[    0.070531] VFS: Disk quotas dquot_6.6.0
[    0.070556] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.076854] NET: Registered PF_INET protocol family
[    0.077063] IP idents hash table entries: 65536 (order: 7, 524288 bytes, linear)
[    0.079891] tcp_listen_portaddr_hash hash table entries: 2048 (order: 3, 32768 bytes, linear)
[    0.079939] Table-perturb hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.079952] TCP established hash table entries: 32768 (order: 6, 262144 bytes, linear)
[    0.080193] TCP bind hash table entries: 32768 (order: 8, 1048576 bytes, linear)
[    0.081070] TCP: Hash tables configured (established 32768 bind 32768)
[    0.081224] UDP hash table entries: 2048 (order: 4, 65536 bytes, linear)
[    0.081309] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes, linear)
[    0.081555] NET: Registered PF_UNIX/PF_LOCAL protocol family
[    0.082014] RPC: Registered named UNIX socket transport module.
[    0.082023] RPC: Registered udp transport module.
[    0.082025] RPC: Registered tcp transport module.
[    0.082028] RPC: Registered tcp-with-tls transport module.
[    0.082031] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.082038] NET: Registered PF_XDP protocol family
[    0.082060] PCI: CLS 0 bytes, default 64
[    0.083393] Initialise system trusted keyrings
[    0.083615] workingset: timestamp_bits=46 max_order=20 bucket_order=0
[    0.083910] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.084137] NFS: Registering the id_resolver key type
[    0.084163] Key type id_resolver registered
[    0.084166] Key type id_legacy registered
[    0.084184] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.084195] nfs4flexfilelayout_init: NFSv4 Flexfile Layout Driver Registering...
[    0.116823] Key type asymmetric registered
[    0.116834] Asymmetric key parser 'x509' registered
[    0.116891] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 244)
[    0.117055] io scheduler mq-deadline registered
[    0.117060] io scheduler kyber registered
[    0.117094] io scheduler bfq registered
[    0.120442] pinctrl-single 4084000.pinctrl: 34 pins, size 136
[    0.121020] pinctrl-single f4000.pinctrl: 171 pins, size 684
[    0.128737] Serial: 8250/16550 driver, 12 ports, IRQ sharing enabled
[    0.139809] loop: module loaded
[    0.158026] megasas: 07.725.01.00-rc1
[    0.161768] tun: Universal TUN/TAP device driver, 1.6
[    0.162836] VFIO - User Level meta-driver version: 0.3
[    0.164039] usbcore: registered new interface driver usb-storage
[    0.164618] i2c_dev: i2c /dev entries driver
[    0.165315] device-mapper: ioctl: 4.48.0-ioctl (2023-03-01) initialised: dm-devel@redhat.com
[    0.166547] sdhci: Secure Digital Host Controller Interface driver
[    0.166556] sdhci: Copyright(c) Pierre Ossman
[    0.166790] sdhci-pltfm: SDHCI platform and OF driver helper
[    0.167593] ledtrig-cpu: registered to indicate activity on CPUs
[    0.167904] SMCCC: SOC_ID: ARCH_SOC_ID not implemented, skipping ....
[    0.168566] usbcore: registered new interface driver usbhid
[    0.168570] usbhid: USB HID core driver
[    0.169853] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.170544] optee: probing for conduit method.
[    0.170573] optee: revision 4.4 (8f645256efc0dc66)
[    0.170863] optee: dynamic shared memory is enabled
[    0.171520] random: crng init done
[    0.171600] optee: initialized driver
[    0.173547] Initializing XFRM netlink socket
[    0.173580] NET: Registered PF_PACKET protocol family
[    0.173654] Key type dns_resolver registered
[    0.182255] registered taskstats version 1
[    0.182461] Loading compiled-in X.509 certificates
[    0.195349] ti-sci 44043000.system-controller: ABI: 4.0 (firmware rev 0x000a '10.1.6--v10.01.06 (Fiery Fox)')
[    0.243847] omap_i2c 2b200000.i2c: bus 1 rev0.12 at 400 kHz
[    0.245063] platform hdmi-out: Fixed dependency cycle(s) with /bus@f0000/i2c@20000000/bridge@3d
[    0.245138] platform 30500000.dsi: Fixed dependency cycle(s) with /bus@f0000/i2c@20000000/bridge@3d
[    0.245243] i2c 0-003d: Fixed dependency cycle(s) with /hdmi-out
[    0.245297] i2c 0-003d: Fixed dependency cycle(s) with /bus@f0000/dsi@30500000
[    0.245597] omap_i2c 20000000.i2c: bus 0 rev0.12 at 400 kHz
[    0.246947] omap_i2c 20030000.i2c: bus 3 rev0.12 at 400 kHz
[    0.247151] ti-sci-intr 4210000.interrupt-controller: Interrupt Router 5 domain created
[    0.247286] ti-sci-intr bus@f0000:interrupt-controller@a00000: Interrupt Router 3 domain created
[    0.247517] ti-sci-inta 48000000.interrupt-controller: Interrupt Aggregator domain 28 created
[    0.247770] ti-sci-inta 4e400000.interrupt-controller: Interrupt Aggregator domain 200 created
[    0.252945] ti-udma 485c0100.dma-controller: Number of rings: 82
[    0.255380] ti-udma 485c0100.dma-controller: Channels: 44 (bchan: 16, tchan: 12, rchan: 16)
[    0.257715] ti-udma 485c0000.dma-controller: Number of rings: 150
[    0.262469] ti-udma 485c0000.dma-controller: Channels: 35 (tchan: 20, rchan: 15)
[    0.264413] ti-udma 4e230000.dma-controller: Number of rings: 40
[    0.267149] ti-udma 4e230000.dma-controller: Channels: 40 (bchan: 0, tchan: 8, rchan: 32)
[    0.269924] printk: console [ttyS2] disabled
[    0.270231] 2800000.serial: ttyS2 at MMIO 0x2800000 (irq = 308, base_baud = 3000000) is a 8250
[    0.270276] printk: console [ttyS2] enabled
[    2.002317] davinci_mdio 8000f00.mdio: davinci mdio revision 17.7, bus freq 1000000
[    2.017168] davinci_mdio 8000f00.mdio: phy[0]: device 8000f00.mdio:00, driver TI DP83867
[    2.025273] davinci_mdio 8000f00.mdio: phy[9]: device 8000f00.mdio:09, driver TI DP83867
[    2.033394] am65-cpsw-nuss 8000000.ethernet: initializing am65 cpsw nuss version 0x6BA01903, cpsw version 0x6BA81903 Ports: 3 qu                                                                                                          irks:00000006
[    2.046540] am65-cpsw-nuss 8000000.ethernet: Use random MAC address
[    2.052820] am65-cpsw-nuss 8000000.ethernet: initialized cpsw ale version 1.5
[    2.059948] am65-cpsw-nuss 8000000.ethernet: ALE Table size 512
[    2.066535] am65-cpsw-nuss 8000000.ethernet: CPTS ver 0x4e8a010d, freq:500000000, add_val:1 pps:0
[    2.079914] am65-cpsw-nuss 8000000.ethernet: set new flow-id-base 19
[    2.090796] xhci-hcd xhci-hcd.0.auto: xHCI Host Controller
[    2.096321] xhci-hcd xhci-hcd.0.auto: new USB bus registered, assigned bus number 1
[    2.104073] xhci-hcd xhci-hcd.0.auto: USB3 root hub has no ports
[    2.110075] xhci-hcd xhci-hcd.0.auto: hcc params 0x0258fe6d hci version 0x110 quirks 0x0000008020000010
[    2.119502] xhci-hcd xhci-hcd.0.auto: irq 321, io mem 0x31000000
[    2.126382] hub 1-0:1.0: USB hub found
[    2.130158] hub 1-0:1.0: 1 port detected
[    2.134832] cpu cpu0: _of_add_opp_table_v2: no supported OPPs
[    2.140680] cpu cpu0: OPP table can't be empty
[    2.146504] mmc0: CQHCI version 5.10
[    2.159924] j721e-pcie f102000.pcie: host bridge /bus@f0000/pcie@f102000 ranges:
[    2.167389] j721e-pcie f102000.pcie:       IO 0x0068001000..0x0068010fff -> 0x0068001000
[    2.175486] j721e-pcie f102000.pcie:      MEM 0x0068011000..0x006fffffff -> 0x0068011000
[    2.183584] j721e-pcie f102000.pcie:   IB MEM 0x0000000000..0xffffffffffff -> 0x0000000000
[    2.186323] mmc0: SDHCI controller on fa10000.mmc [fa10000.mmc] using ADMA 64-bit
[    2.284803] mmc0: Command Queue Engine enabled
[    2.289280] mmc0: new HS400 MMC card at address 0001
[    2.294958] mmcblk0: mmc0:0001 C9A551 29.1 GiB
[    2.300835]  mmcblk0: p1 p2 p3 p4
[    2.304919] mmcblk0boot0: mmc0:0001 C9A551 4.00 MiB
[    2.310795] mmcblk0boot1: mmc0:0001 C9A551 4.00 MiB
[    2.316683] mmcblk0rpmb: mmc0:0001 C9A551 16.0 MiB, chardev (239:0)
[    3.302977] j721e-pcie f102000.pcie: PCI host bridge to bus 0000:00
[    3.309333] pci_bus 0000:00: root bus resource [bus 00-ff]
[    3.314820] pci_bus 0000:00: root bus resource [io  0x0000-0xffff] (bus address [0x68001000-0x68010fff])
[    3.324287] pci_bus 0000:00: root bus resource [mem 0x68011000-0x6fffffff]
[    3.331184] pci 0000:00:00.0: [104c:b010] type 01 class 0x060400
[    3.337258] pci 0000:00:00.0: supports D1
[    3.341264] pci 0000:00:00.0: PME# supported from D0 D1 D3hot
[    3.349323] pci 0000:00:00.0: bridge configuration invalid ([bus 00-00]), reconfiguring
[    3.357485] pci_bus 0000:01: busn_res: [bus 01-ff] end is updated to 01
[    3.364114] pci 0000:00:00.0: PCI bridge to [bus 01]
[    3.369202] pcieport 0000:00:00.0: of_irq_parse_pci: failed with rc=-22
[    3.376140] pcieport 0000:00:00.0: PME: Signaling with IRQ 495
[    3.382280] pcieport 0000:00:00.0: AER: enabled with IRQ 495
[    3.389340] 2810000.serial: ttyS3 at MMIO 0x2810000 (irq = 496, base_baud = 3000000) is a 8250
[    3.399350] 2820000.serial: ttyS4 at MMIO 0x2820000 (irq = 497, base_baud = 3000000) is a 8250
[    3.409299] 2830000.serial: ttyS5 at MMIO 0x2830000 (irq = 498, base_baud = 3000000) is a 8250
[    3.419295] 2840000.serial: ttyS6 at MMIO 0x2840000 (irq = 499, base_baud = 3000000) is a 8250
[    3.429195] 2850000.serial: ttyS7 at MMIO 0x2850000 (irq = 500, base_baud = 3000000) is a 8250
[    3.439230] 2860000.serial: ttyS8 at MMIO 0x2860000 (irq = 501, base_baud = 3000000) is a 8250
[    3.449191] sdhci-am654 fa00000.mmc: Got CD GPIO
[    3.454382] mmc1: CQHCI version 5.10
[    3.457906] clk: Disabling unused clocks
[    3.467794] ALSA device list:
[    3.470859]   No soundcards found.
[    3.497090] mmc1: SDHCI controller on fa00000.mmc [fa00000.mmc] using ADMA 64-bit
[    3.504844] Waiting for root device /dev/mmcblk1p2...
[    3.557359] mmc1: new ultra high speed SDR104 SDHC card at address aaaa
[    3.564597] mmcblk1: mmc1:aaaa SC16G 14.8 GiB
[    3.573665]  mmcblk1: p1 p2
[    3.624320] EXT4-fs (mmcblk1p2): recovery complete
[    3.630289] EXT4-fs (mmcblk1p2): mounted filesystem 1b835950-5d57-4989-84be-24c6ee3d8112 r/w with ordered data mode. Quota mode:                                                                                                           none.
[    3.642468] VFS: Mounted root (ext4 filesystem) on device 179:98.
[    3.651055] devtmpfs: mounted
[    3.654753] Freeing unused kernel memory: 2496K
[    3.659369] Run /sbin/init as init process
[    3.851834] systemd[1]: System time before build time, advancing clock.
[    3.897547] NET: Registered PF_INET6 protocol family
[    3.903558] Segment Routing with IPv6
[    3.907279] In-situ OAM (IOAM) with IPv6
[    3.940583] systemd[1]: systemd 255.4^ running in system mode (+PAM -AUDIT -SELINUX -APPARMOR +IMA -SMACK +SECCOMP -GCRYPT -GNUT                                                                                                          LS -OPENSSL +ACL +BLKID -CURL -ELFUTILS -FIDO2 -IDN2 -IDN -IPTC +KMOD -LIBCRYPTSETUP +LIBFDISK -PCRE2 -PWQUALITY -P11KIT -QRENCODE                                                                                                           -TPM2 -BZIP2 -LZ4 -XZ -ZLIB +ZSTD -BPF_FRAMEWORK -XKBCOMMON +UTMP +SYSVINIT default-hierarchy=unified)
[    3.972405] systemd[1]: Detected architecture arm64.
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[    3.998640] systemd[1]: Hostname set to <j722s-ecu1270>.
[    4.390479] systemd[1]: /etc/systemd/system/sync-clocks.service:11: Standard output type syslog is obsolete, automatically updat                                                                                                          ing to journal. Please update your unit file, and consider removing the setting altogether.
[    4.480164] systemd[1]: Queued start job for default target Multi-User System.
[    4.520427] systemd[1]: Created slice Slice /system/getty.
[  OK  ] Created slice Slice /system/getty.
[    4.544848] systemd[1]: Created slice Slice /system/modprobe.
[  OK  ] Created slice Slice /system/modprobe.
[    4.568839] systemd[1]: Created slice Slice /system/serial-getty.
[  OK  ] Created slice Slice /system/serial-getty.
[    4.592249] systemd[1]: Created slice User and Session Slice.
[  OK  ] Created slice User and Session Slice.
[    4.614813] systemd[1]: Started Dispatch Password Requests to Console Directory Watch.
[  OK  ] Started Dispatch Password Requests to Console Directory Watch.
[    4.638703] systemd[1]: Started Forward Password Requests to Wall Directory Watch.
[  OK  ] Started Forward Password Requests to Wall Directory Watch.
[    4.662494] systemd[1]: Expecting device /dev/ttyS2...
         Expecting device /dev/ttyS2...
[    4.678557] systemd[1]: Reached target Path Units.
[  OK  ] Reached target Path Units.
[    4.694473] systemd[1]: Reached target Remote File Systems.
[  OK  ] Reached target Remote File Systems.
[    4.714448] systemd[1]: Reached target Slice Units.
[  OK  ] Reached target Slice Units.
[    4.730468] systemd[1]: Reached target Swaps.
[  OK  ] Reached target Swaps.
[    4.783853] systemd[1]: Listening on RPCbind Server Activation Socket.
[  OK  ] Listening on RPCbind Server Activation Socket.
[    4.806608] systemd[1]: Reached target RPC Port Mapper.
[  OK  ] Reached target RPC Port Mapper.
[    4.835854] systemd[1]: Listening on Process Core Dump Socket.
[  OK  ] Listening on Process Core Dump Socket.
[    4.858886] systemd[1]: Listening on initctl Compatibility Named Pipe.
[  OK  ] Listening on initctl Compatibility Named Pipe.
[    4.883709] systemd[1]: Listening on Journal Audit Socket.
[  OK  ] Listening on Journal Audit Socket.
[    4.907230] systemd[1]: Listening on Journal Socket (/dev/log).
[  OK  ] Listening on Journal Socket (/dev/log).
[    4.931202] systemd[1]: Listening on Journal Socket.
[  OK  ] Listening on Journal Socket.
[    4.947389] systemd[1]: Listening on Network Service Netlink Socket.
[  OK  ] Listening on Network Service Netlink Socket.
[    4.973891] systemd[1]: Listening on udev Control Socket.
[  OK  ] Listening on udev Control Socket.
[    4.995065] systemd[1]: Listening on udev Kernel Socket.
[  OK  ] Listening on udev Kernel Socket.
[    5.015095] systemd[1]: Listening on User Database Manager Socket.
[  OK  ] Listening on User Database Manager Socket.
[    5.070701] systemd[1]: Mounting Huge Pages File System...
         Mounting Huge Pages File System...
[    5.090923] systemd[1]: Mounting POSIX Message Queue File System...
         Mounting POSIX Message Queue File System...
[    5.119162] systemd[1]: Mounting Kernel Debug File System...
         Mounting Kernel Debug File System...
[    5.135016] systemd[1]: Kernel Trace File System was skipped because of an unmet condition check (ConditionPathExists=/sys/kerne                                                                                                          l/tracing).
[    5.155042] systemd[1]: Mounting Temporary Directory /tmp...
         Mounting Temporary Directory /tmp...
[    5.176420] systemd[1]: Starting Create List of Static Device Nodes...
         Starting Create List of Static Device Nodes...
[    5.203407] systemd[1]: Starting Load Kernel Module configfs...
         Starting Load Kernel Module configfs...
[    5.223349] systemd[1]: Starting Load Kernel Module drm...
         Starting Load Kernel Module drm...
[    5.243321] systemd[1]: Starting Load Kernel Module fuse...
         Starting Load Kernel Module fuse...
[    5.263924] systemd[1]: Starting Start psplash boot splash screen...
         Starting Start psplash boot splash screen...
[    5.281806] fuse: init (API version 7.39)
[    5.294746] systemd[1]: Starting RPC Bind...
         Starting RPC Bind...
[    5.310796] systemd[1]: File System Check on Root Device was skipped because of an unmet condition check (ConditionPathIsReadWri                                                                                                          te=!/).
[    5.331628] systemd[1]: Starting Journal Service...
         Starting Journal Service...
[    5.353429] systemd[1]: Starting Load Kernel Modules...
         Starting Load Kernel Modules...
[    5.375798] systemd[1]: Starting Generate network units from Kernel command line...
         Starting Generate network units from Kernel command line...
[    5.404532] cryptodev: loading out-of-tree module taints kernel.
[    5.407248] systemd[1]: Starting Remount Root and Kernel File Systems...
[    5.422606] cryptodev: driver 1.14 loaded.
         Starting Remount Root and Kernel File Systems...
[    5.435013] systemd-journald[145]: Collecting audit messages is enabled.
[    5.447743] systemd[1]: Starting Coldplug All udev Devices...
         Starting Coldplug All udev Devices...
[    5.484789] systemd[1]: Started RPC Bind.
[  OK  ] Started RPC Bind.
[    5.505173] systemd[1]: Mounted Huge Pages File System.
[  OK  ] Mounted Huge Pages File System.
[    5.518956] EXT4-fs (mmcblk1p2): re-mounted 1b835950-5d57-4989-84be-24c6ee3d8112 r/w. Quota mode: none.
[    5.531212] systemd[1]: Mounted POSIX Message Queue File System.
[  OK  ] Mounted POSIX Message Queue File System.
[    5.555332] systemd[1]: Started Journal Service.
[  OK  ] Started Journal Service.
[  OK  ] Mounted Kernel Debug File System.
[  OK  ] Mounted Temporary Directory /tmp.
[  OK  ] Finished Create List of Static Device Nodes.
[  OK  ] Finished Load Kernel Module configfs.
[  OK  ] Finished Load Kernel Module drm.
[  OK  ] Finished Load Kernel Module fuse.
[FAILED] Failed to start Start psplash boot splash screen.
See 'systemctl status psplash-start.service' for details.
[DEPEND] Dependency failed for Start psplas…temd progress communication helper.
[  OK  ] Finished Load Kernel Modules.
[  OK  ] Finished Generate network units from Kernel command line.
[  OK  ] Finished Remount Root and Kernel File Systems.
         Mounting FUSE Control File System...
         Mounting Kernel Configuration File System...
         Starting Flush Journal to Persistent Storage...
         Starting Apply Kernel Variables...
         Starting Create Static Device Nodes in /dev gr[    5.965227] systemd-journald[145]: Received client request to flush runti                                                                                                          me journal.
acefully...
[  OK  ] Mounted FUSE Control File System.
[  OK  ] Mounted Kernel Configuration File System.
[  OK  ] Finished Flush Journal to Persistent Storage.
[  OK  ] Finished Apply Kernel Variables.
[  OK  ] Finished Create Static Device Nodes in /dev gracefully.
         Starting Create Static Device Nodes in /dev...
[  OK  ] Finished Create Static Device Nodes in /dev.
[  OK  ] Reached target Preparation for Local File Systems.
         Mounting /var/volatile...
[    6.198180] audit: type=1334 audit(1709054766.340:2): prog-id=6 op=LOAD
[    6.206248] audit: type=1334 audit(1709054766.348:3): prog-id=7 op=LOAD
         Starting Rule-based Manager for Device Events and Files...
[  OK  ] Mounted /var/volatile.
         Starting Load/Save OS Random Seed...
[  OK  ] Reached target Local File Systems.
         Starting Create Volatile Files and Directories...
[  OK  ] Finished Coldplug All udev Devices.
[  OK  ] Finished Load/Save OS Random Seed.
         Starting Wait for udev To Complete Device Initialization...
[  OK  ] Finished Create Volatile Files and Directories.
[    6.433391] audit: type=1334 audit(1709054766.576:4): prog-id=8 op=LOAD
         Starting Network Name Resolution...
[    6.474523] audit: type=1334 audit(1709054766.620:5): prog-id=9 op=LOAD
         Starting Network Time Synchronization...
         Starting Record System Boot/Shutdown in UTMP...
[    6.538509] audit: type=1334 audit(1709054766.684:6): prog-id=10 op=LOAD
[    6.545313] audit: type=1334 audit(1709054766.688:7): prog-id=11 op=LOAD
[    6.552075] audit: type=1334 audit(1709054766.696:8): prog-id=12 op=LOAD
         Starting User Database Manager...
[  OK  ] Finished Record System Boot/Shutdown in UTMP.
[  OK  ] Started User Database Manager.
[  OK  ] Started Rule-based Manager for Device Events and Files.
[  OK  ] Started Network Time Synchronization.
[  OK  ] Started Network Name Resolution.
[  OK  ] Reached target Host and Network Name Lookups.
[  OK  ] Reached target System Time Set.
[  OK  ] Found device /dev/ttyS2.
[    8.248824] omap-mailbox 29000000.mailbox: omap mailbox rev 0x66fca100
[    8.259031] CAN device driver interface
[    8.267298] omap-mailbox 29010000.mailbox: omap mailbox rev 0x66fca100
[    8.267521] mc: Linux media interface: v0.10
[    8.274755] omap-mailbox 29020000.mailbox: omap mailbox rev 0x66fca100
[    8.333167] omap-mailbox 29030000.mailbox: omap mailbox rev 0x66fca100
[    8.349461] videodev: Linux video capture interface: v2.00
[    8.349771] k3-dsp-rproc 7e000000.dsp: assigned reserved memory node c7x-dma-memory@a3000000
[    8.365101] k3-dsp-rproc 7e000000.dsp: configured DSP for remoteproc mode
[    8.402657] remoteproc remoteproc0: 7e000000.dsp is available
[    8.414434] k3-dsp-rproc 7e200000.dsp: assigned reserved memory node c7x-dma-memory@a4000000
[    8.414775] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[    8.429172] remoteproc remoteproc0: powering up 7e000000.dsp
[    8.433507] k3-dsp-rproc 7e200000.dsp: configured DSP for remoteproc mode
[    8.437233] remoteproc remoteproc0: Booting fw image j722s-c71_0-fw, size 2100488
[    8.454567] remoteproc remoteproc1: 7e200000.dsp is available
[    8.471528] remoteproc remoteproc1: powering up 7e200000.dsp
[    8.477284] remoteproc remoteproc1: Booting fw image j722s-c71_1-fw, size 2100488
[    8.488774] k3-dsp-rproc 7e000000.dsp: booting DSP core using boot addr = 0xa3600000
[    8.492940] platform 79000000.r5f: configured R5F for remoteproc mode
[    8.497362] k3-dsp-rproc 7e200000.dsp: booting DSP core using boot addr = 0xa4600000
[    8.503730] platform 79000000.r5f: assigned reserved memory node mcu-r5fss-dma-memory-region@a1000000
[    8.534760] rproc-virtio rproc-virtio.1.auto: assigned reserved memory node c7x-dma-memory@a3000000
[    8.543914] rproc-virtio rproc-virtio.2.auto: assigned reserved memory node c7x-dma-memory@a4000000
[    8.553961] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[    8.554905] virtio_rpmsg_bus virtio0: rpmsg host is online
[    8.555696] virtio_rpmsg_bus virtio0: creating channel ti.ipc4.ping-pong addr 0xd
[    8.555851] virtio_rpmsg_bus virtio0: creating channel rpmsg_chrdev addr 0xe
[    8.563279] remoteproc remoteproc2: 79000000.r5f is available
[    8.570019] rproc-virtio rproc-virtio.1.auto: registered virtio0 (type 7)
[    8.577911] remoteproc remoteproc2: powering up 79000000.r5f
[    8.582613] remoteproc remoteproc0: remote processor 7e000000.dsp is now up
[    8.585492] virtio_rpmsg_bus virtio1: rpmsg host is online
[    8.588648] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[    8.588677] virtio_rpmsg_bus virtio1: creating channel ti.ipc4.ping-pong addr 0xd
[    8.588884] remoteproc remoteproc2: Booting fw image j722s-mcu-r5f0_0-fw, size 50612
[    8.597310] virtio_rpmsg_bus virtio1: creating channel rpmsg_chrdev addr 0xe
[    8.602369] rproc-virtio rproc-virtio.2.auto: registered virtio1 (type 7)
[    8.605261] rtc-ti-k3 2b1f0000.rtc: registered as rtc0
[    8.605302] rtc-ti-k3 2b1f0000.rtc: setting system clock to 1970-01-01T00:00:00 UTC (0)
[    8.618650] rproc-virtio rproc-virtio.4.auto: assigned reserved memory node mcu-r5fss-dma-memory-region@a1000000
[    8.622230] remoteproc remoteproc1: remote processor 7e200000.dsp is now up
[    8.640927] platform 78000000.r5f: R5F core may have been powered on by a different host, programmed state (0) != actual state (                                                                                                          1)
[    8.693949] platform 78000000.r5f: configured R5F for IPC-only mode
[    8.700986] platform 78000000.r5f: assigned reserved memory node r5f-dma-memory@a0000000
[    8.715249] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[    8.722019] virtio_rpmsg_bus virtio2: rpmsg host is online
[    8.729273] virtio_rpmsg_bus virtio2: creating channel ti.ipc4.ping-pong addr 0xd
[    8.737032] Internal error: synchronous external abort: 0000000096000010 [#1] PREEMPT SMP
[    8.745216] Modules linked in: wave5(+) videobuf2_dma_contig k3_j72xx_bandgap videobuf2_memops rtc_ti_k3 v4l2_mem2mem ti_k3_r5_r                                                                                                          emoteproc(+) videobuf2_v4l2 tidss videobuf2_common mcrc64 ti_k3_dsp_remoteproc drm_dma_helper videodev m_can_platform cdns_dsi m_ca                                                                                                          n sa2ul drm_kms_helper mc cdns_dphy omap_hwspinlock omap_mailbox can_dev spi_omap2_mcspi cryptodev(O) fuse drm drm_panel_orientatio                                                                                                          n_quirks backlight ipv6
[    8.781567] CPU: 0 PID: 239 Comm: (udev-worker) Tainted: G           O       6.6.44-ti-01478-g541c20281af7-dirty #1
[    8.791987] Hardware name: Texas Instruments J722S ECU1270 (DT)
[    8.797892] pstate: 60000005 (nZCv daif -PAN -UAO -TCO -DIT -SSBS BTYPE=--)
[    8.804842] pc : wave5_vdi_read_register+0x8/0x20 [wave5]
[    8.810265] lr : wave5_vpu_probe+0x1d8/0x658 [wave5]
[    8.815236] sp : ffff80008263b830
[    8.818537] x29: ffff80008263b850 x28: 0000000000000000 x27: 0000000000000000
[    8.825665] x26: ffff80008146bb10 x25: ffff000802741120 x24: ffff800079784b78
[    8.832790] x23: ffff00080018b010 x22: ffff00080018b000 x21: ffff000802658880
[    8.839915] x20: 0000000000000001 x19: 0000000000000000 x18: ffffffffffffffff
[    8.847040] x17: 64646120676e6f70 x16: 2d676e69702e3463 x15: ffff800082513920
[    8.854165] x14: 00004edf32e576c6 x13: 000000000000031b x12: 0000000000000000
[    8.861290] x11: 0000000000000000 x10: ffff84007b9778b7 x9 : 0000000000000018
[    8.868414] x8 : 0101010101010101 x7 : 0000000000000000 x6 : 0000000000000001
[    8.875538] x5 : ffff00080016ee50 x4 : ffff80008055829c x3 : 0000000000000000
[    8.882663] x2 : 0000000000000000 x1 : 0000000000001044 x0 : ffff8000826e1044
[    8.889788] Call trace:
[bookmark: OLE_LINK4][    8.892225]  wave5_vdi_read_register+0x8/0x20 [wave5]
[    8.897282]  platform_probe+0x68/0xc4
[    8.900942]  really_probe+0x148/0x2b0
[    8.904599]  __driver_probe_device+0x78/0x12c
[    8.908949]  driver_probe_device+0xd8/0x15c
[    8.913123]  __driver_attach+0x90/0x19c
[    8.916952]  bus_for_each_dev+0x7c/0xdc
[    8.920780]  driver_attach+0x24/0x30
[    8.924348]  bus_add_driver+0xe4/0x208
[    8.928090]  driver_register+0x5c/0x124
[    8.931916]  __platform_driver_register+0x28/0x34
[    8.936609]  wave5_vpu_driver_init+0x20/0x1000 [wave5]
[    8.941752]  do_one_initcall+0x80/0x1c8
[    8.945581]  do_init_module+0x58/0x1e0
[    8.949326]  load_module+0x1c8c/0x1d18
[    8.953068]  init_module_from_file+0x88/0xcc
[    8.957330]  __arm64_sys_finit_module+0x1dc/0x2e4
[    8.962025]  invoke_syscall+0x48/0x114
[    8.965767]  el0_svc_common.constprop.0+0xc0/0xe0
[    8.970460]  do_el0_svc+0x1c/0x28
[    8.973767]  el0_svc+0x2c/0x84
[    8.976814]  el0t_64_sync_handler+0x120/0x12c
[    8.981161]  el0t_64_sync+0x190/0x194
[    8.984818] Code: b9000022 d65f03c0 f940b000 8b214000 (b9400000)
[    8.990896] ---[ end trace 0000000000000000 ]---
[    8.995823] virtio_rpmsg_bus virtio2: creating channel rpmsg_chrdev addr 0xe
[    9.003536] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[    9.003752] rproc-virtio rproc-virtio.4.auto: registered virtio2 (type 7)
[    9.018953] remoteproc remoteproc2: remote processor 79000000.r5f is now up
[    9.075342] remoteproc remoteproc3: 78000000.r5f is available
[    9.086083] remoteproc remoteproc3: attaching to 78000000.r5f
[    9.095119] rproc-virtio rproc-virtio.5.auto: assigned reserved memory node r5f-dma-memory@a0000000
[    9.134192] Internal error: synchronous external abort: 0000000096000010 [#2] PREEMPT SMP
[    9.142384] Modules linked in: e5010_jpeg_enc(+) v4l2_jpeg phy_can_transceiver rti_wdt(+) pci_endpoint_test cdns3_ti wave5(+) vi                                                                                                          deobuf2_dma_contig k3_j72xx_bandgap videobuf2_memops rtc_ti_k3 v4l2_mem2mem ti_k3_r5_remoteproc(+) videobuf2_v4l2 tidss videobuf2_c                                                                                                          ommon mcrc64 ti_k3_dsp_remoteproc drm_dma_helper videodev m_can_platform cdns_dsi m_can sa2ul drm_kms_helper mc cdns_dphy omap_hwsp                                                                                                          inlock omap_mailbox can_dev spi_omap2_mcspi cryptodev(O) fuse drm drm_panel_orientation_quirks backlight ipv6
[    9.151817] e5010 fd20000.e5010: Device registered as /dev/video0
[    9.182551] virtio_rpmsg_bus virtio3: rpmsg host is online
[    9.184973] rproc-virtio rproc-virtio.5.auto: registered virtio3 (type 7)
[    9.184991] remoteproc remoteproc3: remote processor 78000000.r5f is now attached
[    9.186213] CPU: 3 PID: 209 Comm: (udev-worker) Tainted: G      D    O       6.6.44-ti-01478-g541c20281af7-dirty #1
[    9.186227] Hardware name: Texas Instruments J722S ECU1270 (DT)
[    9.186231] pstate: 80000005 (Nzcv daif -PAN -UAO -TCO -DIT -SSBS BTYPE=--)
[    9.186239] pc : rti_wdt_probe+0x12c/0x5c0 [rti_wdt]
[    9.186265] lr : rti_wdt_probe+0x114/0x5c0 [rti_wdt]
[    9.186278] sp : ffff800082073800
[    9.186281] x29: ffff800082073850 x28: 0000000000000000 x27: 0000000000000000
[    9.186292] x26: ffff80008146bb10 x25: ffff800082073bb0 x24: 000000000000006e
[    9.186301] x23: ffff00080018ac00 x22: ffff0008013a4490 x21: ffff00080018ac10
[    9.186311] x20: ffff800082165090 x19: ffff0008013a4480 x18: 0000000000000000
[    9.186320] x17: ffff8007c6677000 x16: ffff8000814e0000 x15: 0000000000000000
[    9.186330] x14: 0000000000000000 x13: 0000000000000227 x12: ffff800082165fff
[    9.186340] x11: 0000000000002000 x10: ffff000847fff010 x9 : 0000000000000100
[    9.186350] x8 : ffff800082165000 x7 : ffff000847fff018 x6 : 00007fff8bf8b000
[    9.192520] virtio_rpmsg_bus virtio3: creating channel ti.ipc4.ping-pong addr 0xd
[    9.197904] x5 : 000000000e0f1000 x4 : ffff00080018ae10 x3 : ffff000809222540
[    9.197917] x2 : ffff000809222600 x1 : ffff00080251c740 x0 : ffff800082165000
[    9.197927] Call trace:
[    9.197931]  rti_wdt_probe+0x12c/0x5c0 [rti_wdt]
[    9.197948]  platform_probe+0x68/0xc4
[    9.203569] m_can_platform 20701000.can: m_can device registered (irq=513, version=32)
[    9.213390] m_can_platform 20711000.can: m_can device registered (irq=515, version=32)
[    9.222595]  really_probe+0x148/0x2b0
[    9.222626]  __driver_probe_device+0x78/0x12c
[    9.222635]  driver_probe_device+0xd8/0x15c
[    9.240611] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[    9.245386]  __driver_attach+0x90/0x19c
[    9.245399]  bus_for_each_dev+0x7c/0xdc
[    9.245408]  driver_attach+0x24/0x30
[    9.245417]  bus_add_driver+0xe4/0x208
[    9.245426]  driver_register+0x5c/0x124
[    9.245432]  __platform_driver_register+0x28/0x34
[    9.245439]  rti_wdt_driver_init+0x20/0x1000 [rti_wdt]
[    9.402925]  do_one_initcall+0x80/0x1c8
[    9.402949]  do_init_module+0x58/0x1e0
[    9.402960]  load_module+0x1c8c/0x1d18
[    9.402969]  init_module_from_file+0x88/0xcc
[    9.402978]  __arm64_sys_finit_module+0x1dc/0x2e4
[    9.402988]  invoke_syscall+0x48/0x114
[    9.402996]  el0_svc_common.constprop.0+0xc0/0xe0
[    9.403005]  do_el0_svc+0x1c/0x28
[    9.403012]  el0_svc+0x2c/0x84
[    9.403020]  el0t_64_sync_handler+0x120/0x12c
[    9.403027]  el0t_64_sync+0x190/0x194
[    9.403039] Code: b140041f 540010a8 91024014 a9096bf9 (b9400294)
[    9.403045] ---[ end trace 0000000000000000 ]---
[    9.463883] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[  OK  ] Created slice Slice /system/systemd[    9.479073] virtio_rpmsg_bus virtio3: creating channel rpmsg_chrdev addr 0xe
-fsck.
         Expecting device /dev/mmcblk0p1...
         Expecting device /dev/mmcblk0p2...
[  OK  ] Found device /dev/mmcblk0p1.
[    9.586896] platform 78400000.r5f: configured R5F for remoteproc mode
[    9.599845] platform 78400000.r5f: assigned reserved memory node main-r5fss-dma-memory-region@a2000000
[    9.623595] remoteproc remoteproc4: 78400000.r5f is available
[  OK  ] Found device /dev/mmcblk0p2.
[    9.632205] remoteproc remoteproc4: powering up 78400000.r5f
[    9.641831] remoteproc remoteproc4: Booting fw image j722s-main-r5f0_0-fw, size 46004
[    9.649819] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[    9.652844] rproc-virtio rproc-virtio.6.auto: assigned reserved memory node main-r5fss-dma-memory-region@a2000000
[    9.669341] virtio_rpmsg_bus virtio4: rpmsg host is online
[    9.675008] virtio_rpmsg_bus virtio4: creating channel ti.ipc4.ping-pong addr 0xd
[    9.682828] virtio_rpmsg_bus virtio4: creating channel rpmsg_chrdev addr 0xe
[    9.690107] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[    9.694564] rproc-virtio rproc-virtio.6.auto: registered virtio4 (type 7)
[    9.705677] remoteproc remoteproc4: remote processor 78400000.r5f is now up
[    9.713437] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
         Starting File System Check on /dev/mmcblk0p1...
[    9.752935] at25 spi1.0: 128 KByte fm25 fram, pagesize 4096
[    9.763963] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
         Starting File System Check on /dev/mmcblk0p2...
[    9.843267] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[    9.866468] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[    9.880299] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[    9.894929] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[  OK  ] Created slice Slice /system/tee-sup[    9.907015] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@                                                                                                          1/ports
plicant.
         Expecting device /dev/mmcblk0p3...
         Expecting device /dev/mmcblk0p4...
         Starting Start psplash boot splash screen...
         Starting Virtual Console Setup...
[   10.004693] m_can_platform 20701000.can main_mcan0: renamed from can0
[   10.042911] m_can_platform 20711000.can main_mcan1: renamed from can1
[  OK  ] Finished File System Check on /dev/mmcblk0p2.
[  OK  ] Finished File System Check on /dev/mmcblk0p1.
[   10.238898] xhci-hcd xhci-hcd.7.auto: xHCI Host Controller
[   10.244523] xhci-hcd xhci-hcd.7.auto: new USB bus registered, assigned bus number 2
[   10.252609] xhci-hcd xhci-hcd.7.auto: hcc params 0x200073c9 hci version 0x100 quirks 0x0000002000008010
[FAILED] Failed to start Start psplash boo[   10.264588] xhci-hcd xhci-hcd.7.auto: irq 516, io mem 0x31210000
t splash screen.
See 'systemctl status psplash-start.service' for details.
[   10.280308] xhci-hcd xhci-hcd.7.auto: xHCI Host Controller
[DEPEND] Dependency failed for Start[   10.286503] xhci-hcd xhci-hcd.7.auto: new USB bus registered, assigned bus number 3
 psplas…temd progress communication helper.
[   10.299773] xhci-hcd xhci-hcd.7.auto: Host supports USB 3.0 SuperSpeed
[   10.311744] hub 2-0:1.0: USB hub found
[   10.316363] hub 2-0:1.0: 1 port detected
[   10.321124] usb usb3: We don't know the algorithms for LPM for this host, disabling LPM.
[   10.330279] hub 3-0:1.0: USB hub found
[   10.334204] hub 3-0:1.0: 1 port detected
[   10.338626] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[  OK  ] Found device /dev/mmcblk0p3.
[   10.366788] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[  OK  ] Found device /dev/mmcblk0p4.
[  OK  ] Finished Virtual Console Setup.
         Mounting /run/media/mmcblk0p1...
         Mounting /run/media/rootfs-mmcblk0p2...
         Starting File System Check on /dev/mmcblk0p3...
         Starting File System Check on /dev/mmcblk0p4...
[   10.583589] EXT4-fs (mmcblk0p2): mounted filesystem 08ee7535-dd60-44e4-a611-b40b9214c440 r/w with ordered data mode. Quota mode:                                                                                                           none.
         Starting File System Check on /dev/mmcblk1p1...
[  OK  ] Mounted /run/media/mmcblk0p1.
[  OK  ] Mounted /run/media/rootfs-mmcblk0p2.
[  OK  ] Finished File System Check on /dev/mmcblk0p3.
         Mounting /run/media/recovery-mmcblk0p3...
[  OK  ] Finished File System Check on /dev/mmcblk0p4.
[   10.689745] EXT4-fs (mmcblk0p3): mounted filesystem dadc4dad-afec-4b10-acee-9b84c62caa4c r/w with ordered data mode. Quota mode:                                                                                                           none.
         Mounting /run/media/data-mmcblk0p4...
[  OK  ] Mounted /run/media/recovery-mmcblk0p3.
[  OK  ] Finished File System Check on /dev/[   10.740498] EXT4-fs (mmcblk0p4): mounted filesystem 3abe91c6-d23f-404c-8a24-6b7a3fc3                                                                                                          e572 r/w with ordered data mode. Quota mode: none.
mmcblk1p1.
[  OK  ] Mounted /run/media/data-mmcblk0p4.
         Mounting /run/media/boot-mmcblk1p1...
[  OK  ] Mounted /run/media/boot-mmcblk1p1.
[***   ] A start job is running for Wait for…ice Initialization (15s / 3min 1s)
[   20.452184] OF: graph: no port node found in /bus@f0000/dss@30220000/oldi-txes/oldi@1/ports
[     *] A start job is running for Wait for…nitialization (1min 18s / 3min 1s)
▒
