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Fig.1,2&3 (TFT Pins connection from the controller)
Fig.4 (interfacing the TFT connection from controller card to TFT Card)
[image: ]
Fig.5
[image: ]
	Fig.6
Fig.5( Connection from controller card to TFT Card)
[bookmark: _GoBack]Fig.6( Connection to TFT from TFT card)
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