/*
 * Copyright (C) 2012 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
/dts-v1/;

#include "am33xx.dtsi"
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/sound/sii9022-audio.h>

/ {
	model = "TI AM335x EVM";
	compatible = "ti,am335x-evm", "ti,am33xx";

	        aliases {
                display0 = &hdmi;
        };

        hdmi: connector {
                compatible = "hdmi-connector";
                label = "hdmi";

                type = "b";

                port {
                        hdmi_connector_in: endpoint {
                                remote-endpoint = <&sii9022_out>;
                        };
                };
        };

	cpus {
		cpu@0 {
			cpu0-supply = <&vdd1_reg>;
		};
	};

	memory {
		device_type = "memory";
		reg = <0x80000000 0x20000000>; /* 256 MB *//*our flash is 512MB*/
	};

	vbat: fixedregulator@0 {
		compatible = "regulator-fixed";
		regulator-name = "vbat";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-boot-on;
	};
        vmmcsd_fixed: fixedregulator@0 {
                compatible = "regulator-fixed";
                regulator-name = "vmmcsd_fixed";
                regulator-min-microvolt = <3300000>;
                regulator-max-microvolt = <3300000>;
        };


	lis3_reg: fixedregulator@1 {
		compatible = "regulator-fixed";
		regulator-name = "lis3_reg";
		regulator-boot-on;
	};



	backlight {
		compatible = "pwm-backlight";
		pwms = <&ecap2 0 50000 0>;
		brightness-levels = <0 51 53 56 62 75 101 152 255>;
		default-brightness-level = <8>;
	};

	panel {
		compatible = "ti,tilcdc,panel";
		status = "okay";
		pinctrl-names = "default";
		pinctrl-0 = <&lcd_pins_s0>;
		panel-info {
			ac-bias           = <255>;
			ac-bias-intrpt    = <0>;
			dma-burst-sz      = <16>;
			bpp               = <18>;/*<24>;*/
			fdd               = <0x80>;
			sync-edge         = <0>;
			sync-ctrl         = <1>;
			raster-order      = <0>;
			fifo-th           = <2>;
		};

		display-timings {
		/*	1024x768p62 {
				clock-frequency = <64900000>;
				hactive = <1024>;
				vactive = <768>;
				hfront-porch = <212>;
				hback-porch = <44>;
				hsync-len = <1>;
				vback-porch = <19>;
				vfront-porch = <26>;
				vsync-len = <4>;
				hsync-active = <0>;
				vsync-active = <0>;
			};*/
			800x480p62 {
				clock-frequency = <33300000>;
				hactive = <800>;
				vactive = <480>;
				hfront-porch = <212>;
				hback-porch = <44>;
				hsync-len = <1>;
				vback-porch = <19>;
				vfront-porch = <26>;
				vsync-len = <4>;
				hsync-active =  <0>;
				vsync-active = <0>;
			};
		};
	};
	/*add from SDK08*/
	kim {
		compatible = "kim";
		nshutdown_gpio = <117>; /* Bank3, pin21 */
		dev_name = "/dev/ttyO1";
		flow_cntrl = <1>;
		baud_rate = <3000000>;
	};
	
	/*add from SDK08*/
	btwilink {
		compatible = "btwilink";
	};

	sound {
		compatible = "simple-audio-card";
		simple-audio-card,name = "AM335x-EVM";
		simple-audio-card,widgets =
			"Microphone", "Microphone Jack",
			"Headphone", "Headphone Jack",
			"Line", "Line In",
			"Speaker", "Speaker External",
			"Line", "Line Out";
		simple-audio-card,routing =
			"Headphone Jack",	"HP_OUT",
			"MIC_IN", "Microphone Jack",
			"Speaker External", "LINE_OUT";
		simple-audio-card,format = "dsp_b";
//		simple-audio-card,hp-det-gpio = <&gpio1 31 GPIO_ACTIVE_LOW>;
		simple-audio-card,bitclock-master = <&sound_master>;
		simple-audio-card,frame-master = <&sound_master>;
		simple-audio-card,bitclock-inversion;

		simple-audio-card,cpu {
			sound-dai = <&mcasp1>;
		};

		sound_master: simple-audio-card,codec {
			sound-dai = <&sgtl5000>;
			system-clock-frequency = <12000000>;
		};
	};
        sound@1 {
                compatible = "simple-audio-card";
                simple-audio-card,name = "HDMI";
                simple-audio-card,format = "i2s";
                simple-audio-card,bitclock-master = <&hdmi_dailink_master>;
                simple-audio-card,frame-master = <&hdmi_dailink_master>;
                hdmi_dailink_master: simple-audio-card,cpu {
                        sound-dai = <&mcasp1>;
                        system-clock-frequency = <24000000>;
                        system-clock-direction = "out";
                };

                simple-audio-card,codec {
                        sound-dai = <&sii9022>;
                        system-clock-frequency = <12000000>;
                };
        };

};

&am33xx_pinmux {
	pinctrl-names = "default";
	pinctrl-0 = <&clkout1_2_pin>;


	hp_det_pins: pinmux_hp_det_pins {
		pinctrl-single,pins = <
			0x84 (PIN_INPUT | MUX_MODE7)	/* i2c0_sda.i2c0_sda */
		>;
	};
	i2c0_pins: pinmux_i2c0_pins {
		pinctrl-single,pins = <
			0x188 (PIN_INPUT_PULLUP | MUX_MODE0)	/* i2c0_sda.i2c0_sda */
			0x18c (PIN_INPUT_PULLUP | MUX_MODE0)	/* i2c0_scl.i2c0_scl */
		>;
	};


	i2c2_pins_default: i2c2_pins_default {
		pinctrl-single,pins = <
			0x154 ( PIN_INPUT | MUX_MODE2 ) /* (B17) spi0_d0.I2C2_SCL */
			0x150 ( PIN_INPUT | MUX_MODE2 ) /* (A17) spi0_sclk.I2C2_SDA */
		>;
	};

	uart0_pins: pinmux_uart0_pins {
		pinctrl-single,pins = <
			0x170 (PIN_INPUT_PULLUP | MUX_MODE0)	/* uart0_rxd.uart0_rxd */
			0x174 (PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* uart0_txd.uart0_txd */
		>;
	};

	uart1_pins: pinmux_uart1_pins {
		pinctrl-single,pins = <
			0x178 (PIN_INPUT | MUX_MODE0)		/* uart1_ctsn.uart1_ctsn */
			0x17C (PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* uart1_rtsn.uart1_rtsn */
			0x180 (PIN_INPUT_PULLUP | MUX_MODE0)	/* uart1_rxd.uart1_rxd */
			0x184 (PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* uart1_txd.uart1_txd */
		>;
	};

	uart3_pins_default: uart3_pins_default {
		pinctrl-single,pins = <
			0x160 ( PIN_INPUT | MUX_MODE1 ) /* (C15) spi0_cs1.uart3_rxd */
			0x164 ( PIN_OUTPUT | MUX_MODE1 ) /* (C18) eCAP0_in_PWM0_out.uart3_txd */
		>;
	};

	clkout1_2_pin: pinmux_clkout1_2_pin {
		pinctrl-single,pins = <
	/*		0x1b0 ( PIN_OUTPUT | MUX_MODE3 ) /* (A15) xdma_event_intr0.clkout1 */
			0x1b4 (PIN_OUTPUT_PULLDOWN | MUX_MODE3)	/* xdma_event_intr1.clkout2 */
		>;
	};


	nandflash_pins_s0: nandflash_pins_s0 {
		pinctrl-single,pins = <
			0x0 (PIN_INPUT_PULLUP | MUX_MODE0)	/* gpmc_ad0.gpmc_ad0 */
			0x4 (PIN_INPUT_PULLUP | MUX_MODE0)	/* gpmc_ad1.gpmc_ad1 */
			0x8 (PIN_INPUT_PULLUP | MUX_MODE0)	/* gpmc_ad2.gpmc_ad2 */
			0xc (PIN_INPUT_PULLUP | MUX_MODE0)	/* gpmc_ad3.gpmc_ad3 */
			0x10 (PIN_INPUT_PULLUP | MUX_MODE0)	/* gpmc_ad4.gpmc_ad4 */
			0x14 (PIN_INPUT_PULLUP | MUX_MODE0)	/* gpmc_ad5.gpmc_ad5 */
			0x18 (PIN_INPUT_PULLUP | MUX_MODE0)	/* gpmc_ad6.gpmc_ad6 */
			0x1c (PIN_INPUT_PULLUP | MUX_MODE0)	/* gpmc_ad7.gpmc_ad7 */
			0x70 (PIN_INPUT_PULLUP | MUX_MODE0)	/* gpmc_wait0.gpmc_wait0 */
			0x74 (PIN_INPUT_PULLUP | MUX_MODE7)	/* gpmc_wpn.gpio0_30 */
			0x7c (PIN_OUTPUT | MUX_MODE0)		/* gpmc_csn0.gpmc_csn0  */
			0x90 (PIN_OUTPUT | MUX_MODE0)		/* gpmc_advn_ale.gpmc_advn_ale */
			0x94 (PIN_OUTPUT | MUX_MODE0)		/* gpmc_oen_ren.gpmc_oen_ren */
			0x98 (PIN_OUTPUT | MUX_MODE0)		/* gpmc_wen.gpmc_wen */
			0x9c (PIN_OUTPUT | MUX_MODE0)		/* gpmc_be0n_cle.gpmc_be0n_cle */
		>;
	};

	ecap0_pins: backlight_pins {
		pinctrl-single,pins = <
			0x164 0x0	/* eCAP0_in_PWM0_out.eCAP0_in_PWM0_out MODE0 */
		>;
	};

	ecap2_pins_default: ecap2_pins_default {
		pinctrl-single,pins = <
			0x19c ( PIN_OUTPUT | MUX_MODE4 ) /* (C12) mcasp0_ahclkr.eCAP2_in_PWM2_out */
		>;
	};

	cpsw_default: cpsw_default {
		pinctrl-single,pins = <
			/* Slave 1 */
			0x114 (PIN_OUTPUT_PULLDOWN | MUX_MODE2)	/* mii1_txen.rgmii1_tctl */
			0x118 (PIN_INPUT_PULLDOWN | MUX_MODE2)	/* mii1_rxdv.rgmii1_rctl */
			0x11c (PIN_OUTPUT_PULLDOWN | MUX_MODE2)	/* mii1_txd3.rgmii1_td3 */
			0x120 (PIN_OUTPUT_PULLDOWN | MUX_MODE2)	/* mii1_txd2.rgmii1_td2 */
			0x124 (PIN_OUTPUT_PULLDOWN | MUX_MODE2)	/* mii1_txd1.rgmii1_td1 */
			0x128 (PIN_OUTPUT_PULLDOWN | MUX_MODE2)	/* mii1_txd0.rgmii1_td0 */
			0x12c (PIN_OUTPUT_PULLDOWN | MUX_MODE2)	/* mii1_txclk.rgmii1_tclk */
			0x130 (PIN_INPUT_PULLDOWN | MUX_MODE2)	/* mii1_rxclk.rgmii1_rclk */
			0x134 (PIN_INPUT_PULLDOWN | MUX_MODE2)	/* mii1_rxd3.rgmii1_rd3 */
			0x138 (PIN_INPUT_PULLDOWN | MUX_MODE2)	/* mii1_rxd2.rgmii1_rd2 */
			0x13c (PIN_INPUT_PULLDOWN | MUX_MODE2)	/* mii1_rxd1.rgmii1_rd1 */
			0x140 (PIN_INPUT_PULLDOWN | MUX_MODE2)	/* mii1_rxd0.rgmii1_rd0 */
		>;
	};

	cpsw_sleep: cpsw_sleep {
		pinctrl-single,pins = <
			/* Slave 1 reset value */
			0x114 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x118 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x11c (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x120 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x124 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x128 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x12c (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x130 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x134 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x138 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x13c (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x140 (PIN_INPUT_PULLDOWN | MUX_MODE7)
		>;
	};

	davinci_mdio_default: davinci_mdio_default {
		pinctrl-single,pins = <
			/* MDIO */
			0x148 (PIN_INPUT_PULLUP | SLEWCTRL_FAST | MUX_MODE0)	/* mdio_data.mdio_data */
			0x14c (PIN_OUTPUT_PULLUP | MUX_MODE0)			/* mdio_clk.mdio_clk */
		>;
	};

	davinci_mdio_sleep: davinci_mdio_sleep {
		pinctrl-single,pins = <
			/* MDIO reset value */
			0x148 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x14c (PIN_INPUT_PULLDOWN | MUX_MODE7)
		>;
	};


	mmc1_pins: pinmux_mmc1_pins {
		pinctrl-single,pins = <
			0x0F0 (PIN_INPUT_PULLUP | MUX_MODE0)    /* mmc0_dat3.mmc0_dat3 */
			0x0F4 (PIN_INPUT_PULLUP | MUX_MODE0)    /* mmc0_dat2.mmc0_dat2 */
			0x0F8 (PIN_INPUT_PULLUP | MUX_MODE0)    /* mmc0_dat1.mmc0_dat1 */
			0x0FC (PIN_INPUT_PULLUP | MUX_MODE0)    /* mmc0_dat0.mmc0_dat0 */
			0x100 (PIN_INPUT_PULLUP | MUX_MODE0)    /* mmc0_clk.mmc0_clk */
			0x104 (PIN_INPUT_PULLUP | MUX_MODE0)    /* mmc0_cmd.mmc0_cmd */
	/*		0x15C (PIN_INPUT_PULLUP | MUX_MODE7)           /* spi0_cs1.gpio0_6 *//*not set,if set,the cd pin can not high*/
		>;
	};

	mmc2_pins_default: mmc2_pins_default {
		pinctrl-single,pins = <
			0x8c ( PIN_INPUT_PULLUP | MUX_MODE3 ) /* (V12) gpmc_clk.mmc2_clk */
			0x88 ( PIN_INPUT_PULLUP | MUX_MODE3 ) /* (T13) gpmc_csn3.mmc2_cmd */
			0x44 ( PIN_INPUT_PULLUP | MUX_MODE3 ) /* (V14) gpmc_a1.mmc2_dat0 */
			0x48 ( PIN_INPUT_PULLUP | MUX_MODE3 ) /* (U14) gpmc_a2.mmc2_dat1 */
			0x4c ( PIN_INPUT_PULLUP | MUX_MODE3 ) /* (T14) gpmc_a3.mmc2_dat2 */
			0x78 ( PIN_INPUT_PULLUP | MUX_MODE3 ) /* (U18) gpmc_be1n.mmc2_dat3 */
		>;
	};


	lcd_pins_s0: lcd_pins_s0 {
		pinctrl-single,pins = <
			0x20 (PIN_OUTPUT | MUX_MODE1)		/* gpmc_ad8.lcd_data23 */
			0x24 (PIN_OUTPUT | MUX_MODE1)		/* gpmc_ad9.lcd_data22 */
			0x28 (PIN_OUTPUT | MUX_MODE1)		/* gpmc_ad10.lcd_data21 */
			0x2c (PIN_OUTPUT | MUX_MODE1)		/* gpmc_ad11.lcd_data20 */
			0x30 (PIN_OUTPUT | MUX_MODE1)		/* gpmc_ad12.lcd_data19 */
			0x34 (PIN_OUTPUT | MUX_MODE1)		/* gpmc_ad13.lcd_data18 */
			0x38 (PIN_OUTPUT | MUX_MODE1)		/* gpmc_ad14.lcd_data17 */
			0x3c (PIN_OUTPUT | MUX_MODE1)		/* gpmc_ad15.lcd_data16 */
			0xa0 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data0.lcd_data0 */
			0xa4 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data1.lcd_data1 */
			0xa8 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data2.lcd_data2 */
			0xac (PIN_OUTPUT | MUX_MODE0)		/* lcd_data3.lcd_data3 */
			0xb0 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data4.lcd_data4 */
			0xb4 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data5.lcd_data5 */
			0xb8 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data6.lcd_data6 */
			0xbc (PIN_OUTPUT | MUX_MODE0)		/* lcd_data7.lcd_data7 */
			0xc0 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data8.lcd_data8 */
			0xc4 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data9.lcd_data9 */
			0xc8 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data10.lcd_data10 */
			0xcc (PIN_OUTPUT | MUX_MODE0)		/* lcd_data11.lcd_data11 */
			0xd0 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data12.lcd_data12 */
			0xd4 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data13.lcd_data13 */
			0xd8 (PIN_OUTPUT | MUX_MODE0)		/* lcd_data14.lcd_data14 */
			0xdc (PIN_OUTPUT | MUX_MODE0)		/* lcd_data15.lcd_data15 */
			0xe0 (PIN_OUTPUT | MUX_MODE0)		/* lcd_vsync.lcd_vsync */
			0xe4 (PIN_OUTPUT | MUX_MODE0)		/* lcd_hsync.lcd_hsync */
			0xe8 (PIN_OUTPUT | MUX_MODE0)		/* lcd_pclk.lcd_pclk */
			0xec (PIN_OUTPUT | MUX_MODE0)		/* lcd_ac_bias_en.lcd_ac_bias_en */
		>;
	};

	mcasp1_pins: mcasp1_pins {
		pinctrl-single,pins = <
			0x10c (PIN_INPUT_PULLDOWN | MUX_MODE4) /* mii1_crs.mcasp1_aclkx */
			0x110 (PIN_INPUT_PULLDOWN | MUX_MODE4) /* mii1_rxerr.mcasp1_fsx */
			0x108 (PIN_OUTPUT_PULLDOWN | MUX_MODE4) /* mii1_col.mcasp1_axr2 */
			0x144 (PIN_INPUT_PULLDOWN | MUX_MODE4) /* rmii1_ref_clk.mcasp1_axr3 */
		>;
	};

	mcasp1_pins_sleep: mcasp1_pins_sleep {
		pinctrl-single,pins = <
			0x10c (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x110 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x108 (PIN_INPUT_PULLDOWN | MUX_MODE7)
			0x144 (PIN_INPUT_PULLDOWN | MUX_MODE7)
		>;
	};

	am335x_evm_bt_iis_pins_default: mymcasp0-bt-iis_pins_default {
		pinctrl-single,pins = <
			0x60 ( PIN_INPUT | MUX_MODE6 ) /* (V16) gpmc_a8.mcasp0_aclkx */
			0x64 ( PIN_INPUT | MUX_MODE6 ) /* (U16) gpmc_a9.mcasp0_fsx */
			0x68 ( PIN_INPUT | MUX_MODE6 ) /* (T16) gpmc_a10.mcasp0_axr0 */
			0x6c ( PIN_INPUT | MUX_MODE6 ) /* (V17) gpmc_a11.mcasp0_axr1 */
		>;
	};

	dcan0_pins_default: dcan0_pins_default {
		pinctrl-single,pins = <
			0x174 ( PIN_INPUT | MUX_MODE2 ) /* (E16) uart0_txd.dcan0_rx */
			0x170 ( PIN_OUTPUT | MUX_MODE2 ) /* (E15) uart0_rxd.dcan0_tx */
		>;
	};

	dcan1_pins_default: dcan1_pins_default {
		pinctrl-single,pins = <
			0x168 (PIN_OUTPUT | MUX_MODE2) /* uart0_ctsn.d_can1_tx */
			0x16c (PIN_INPUT_PULLDOWN | MUX_MODE2) /* uart0_rtsn.d_can1_rx */
		>;
	};

	usb0_pins_default: usb0_pins_default {
		pinctrl-single,pins = <
			0x21c ( PIN_OUTPUT | MUX_MODE0 ) /* (F16) USB0_DRVVBUS.USB0_DRVVBUS */
		>;
	};

	usb1_pins_default: usb1_pins_default {
		pinctrl-single,pins = <
			0x234 ( PIN_OUTPUT | MUX_MODE0 ) /* (F15) USB1_DRVVBUS.USB1_DRVVBUS */
		>;
	};

};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pins>;

	status = "disabled";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_pins>;

	status = "okay";
};

&uart3 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart3_pins_default>;
	status = "okay";
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0_pins>;

	status = "okay";
	clock-frequency = <400000>;
	
	sgtl5000: sgtl5000@0a {
		#sound-dai-cells = <0>;
        	compatible = "fsl,sgtl5000";
	        reg = <0x0a>;
        	micbias-resistor-k-ohms = <2>;
	        micbias-voltage-m-volts = <2250>;/*<2250>;*/
};

	tps: tps@2d {
		reg = <0x2d>;
	};
};

&i2c2 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c2_pins_default>;

	status = "okay";
	clock-frequency = <400000>;
	sii9022: sii9022@3b {
                #sound-dai-cells = <0>;
                compatible = "sil,sii9022";
                reg = <0x3b>;

                interrupt-parent = <&intc>;
                interrupts = <7>;       /* NNMI */

                i2s-fifo-routing = <
                        (ENABLE_BIT|CONNECT_SD0)
                        0
                        0
                        0
                >;

                ports {
                        #address-cells = <1>;
                        #size-cells = <0>;

                        port@0 {
                                reg = <0>;

                                sii9022_in: endpoint {
                                        /*remote-endpoint = <&dpi_out>;*/
                                        remote-endpoint = <&lcdc>;
                                };
                        };

                        port@1 {
                                reg = <1>;

                                sii9022_out: endpoint {
                                        remote-endpoint = <&hdmi_connector_in>;
                                };
                        };
                };
        };

//	tps: tps@2d {
//		reg = <0x3b>;
//	};
};
/*
&dss {
        port {
                dpi_out: endpoint@0 {
                        remote-endpoint = <&sii9022_in>;
                        data-lines = <24>;
                };
        };
};
*/

&usb {
	status = "okay";
};

&usb_ctrl_mod {
	status = "okay";
};

&usb0_phy {
	status = "okay";
};

&usb1_phy {
	status = "okay";
};

&usb0 {
	status = "okay";
};

&usb1 {
	status = "okay";
	dr_mode = "host";
};

&cppi41dma  {
	status = "okay";
};


&lcdc {
	status = "okay";

	blue-and-red-wiring = "crossed";
};

&elm {
	status = "okay";
};


&epwmss2 {
	status = "okay";

	ecap2: ecap@48304100 {
		status = "okay";
		pinctrl-names = "default";
		pinctrl-0 = <&ecap2_pins_default>;
	};
};

&gpmc {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&nandflash_pins_s0>;
	ranges = <0 0 0x08000000 0x1000000>;	/* CS0: 16MB for NAND */
	nand@0,0 {
		compatible = "ti,omap2-nand";
		reg = <0 0 4>; /* CS0, offset 0, IO size 4 */
		interrupt-parent = <&gpmc>;
		interrupts = <0 IRQ_TYPE_NONE>, /* fifoevent */
			     <1 IRQ_TYPE_NONE>;	/* termcount */
		rb-gpios = <&gpmc 0 GPIO_ACTIVE_HIGH>; /* gpmc_wait0 */
		ti,nand-ecc-opt = "bch8";
		ti,elm-id = <&elm>;
		nand-bus-width = <8>;
		gpmc,device-width = <1>;
		gpmc,sync-clk-ps = <0>;
		gpmc,cs-on-ns = <0>;
		gpmc,cs-rd-off-ns = <44>;
		gpmc,cs-wr-off-ns = <44>;
		gpmc,adv-on-ns = <6>;
		gpmc,adv-rd-off-ns = <34>;
		gpmc,adv-wr-off-ns = <44>;
		gpmc,we-on-ns = <0>;
		gpmc,we-off-ns = <40>;
		gpmc,oe-on-ns = <0>;
		gpmc,oe-off-ns = <54>;
		gpmc,access-ns = <64>;
		gpmc,rd-cycle-ns = <82>;
		gpmc,wr-cycle-ns = <82>;
		gpmc,bus-turnaround-ns = <0>;
		gpmc,cycle2cycle-delay-ns = <0>;
		gpmc,clk-activation-ns = <0>;
		gpmc,wr-access-ns = <40>;
		gpmc,wr-data-mux-bus-ns = <0>;
		/* MTD partition table */
		/* All SPL-* partitions are sized to minimal length
		 * which can be independently programmable. For
		 * NAND flash this is equal to size of erase-block */
		#address-cells = <1>;
		#size-cells = <1>;
		partition@0 {
			label = "NAND.SPL";
			reg = <0x00000000 0x000020000>;
		};
		partition@1 {
			label = "NAND.SPL.backup1";
			reg = <0x00020000 0x00020000>;
		};
		partition@2 {
			label = "NAND.SPL.backup2";
			reg = <0x00040000 0x00020000>;
		};
		partition@3 {
			label = "NAND.SPL.backup3";
			reg = <0x00060000 0x00020000>;
		};
		partition@4 {
			label = "NAND.u-boot-spl-os";
			reg = <0x00080000 0x00040000>;
		};
		partition@5 {
			label = "NAND.u-boot";
			reg = <0x000C0000 0x00200000>;
		};
		partition@6 {
			label = "NAND.u-boot-env";
			reg = <0x002C0000 0x00020000>;
		};
		partition@7 {
			label = "NAND.u-boot-env.backup1";
			reg = <0x002E0000 0x00020000>;
		};
		partition@8 {
			label = "NAND.kernel";
			reg = <0x00300000 0x00800000>;
		};
		partition@9 {
			label = "NAND.file-system";
			reg = <0x00b00000 0x2F500000>;
		};
	};
};

#include "tps65910.dtsi"

&mcasp0	{
	#sound-dai-cells = <0>;
	pinctrl-names = "default";
	pinctrl-0 = <&am335x_evm_bt_iis_pins_default>;
	status = "okay";
	op-mode = <0>;	/* MCASP_IIS_MODE */
	tdm-slots = <2>;
	serial-dir = <	/* 0: INACTIVE, 1: TX, 2: RX */
			0 0 1 0
		>;
	tx-num-evt = <32>;
	rx-num-evt = <32>;
};
&mcasp1 {
	#sound-dai-cells = <0>;
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&mcasp1_pins>;
	pinctrl-1 = <&mcasp1_pins_sleep>;

	status = "okay";

	op-mode = <0>;          /* MCASP_IIS_MODE */
	tdm-slots = <2>;
	/* 4 serializers */
	serial-dir = <  /* 0: INACTIVE, 1: TX, 2: RX */
		0 0 1 2
	>;
	tx-num-evt = <32>;
	rx-num-evt = <32>;
};

&tps {
	vcc1-supply = <&vbat>;
	vcc2-supply = <&vbat>;
	vcc3-supply = <&vbat>;
	vcc4-supply = <&vbat>;
	vcc5-supply = <&vbat>;
	vcc6-supply = <&vbat>;
	vcc7-supply = <&vbat>;
	vccio-supply = <&vbat>;

	regulators {
		vrtc_reg: regulator@0 {
			regulator-always-on;
		};

		vio_reg: regulator@1 {
			regulator-always-on;
		};

		vdd1_reg: regulator@2 {
			/* VDD_MPU voltage limits 0.95V - 1.26V with +/-4% tolerance */
			regulator-name = "vdd_mpu";
			regulator-min-microvolt = <912500>;
			regulator-max-microvolt = <1351500>;
			regulator-boot-on;
			regulator-always-on;
		};

		vdd2_reg: regulator@3 {
			/* VDD_CORE voltage limits 0.95V - 1.1V with +/-4% tolerance */
			regulator-name = "vdd_core";
			regulator-min-microvolt = <912500>;
			regulator-max-microvolt = <1150000>;
			regulator-boot-on;
			regulator-always-on;
		};

		vdd3_reg: regulator@4 {
			regulator-always-on;
		};

		vdig1_reg: regulator@5 {
			regulator-always-on;
		};

		vdig2_reg: regulator@6 {
			regulator-always-on;
		};

		vpll_reg: regulator@7 {
			regulator-always-on;
		};

		vdac_reg: regulator@8 {
			regulator-always-on;
		};

		vaux1_reg: regulator@9 {
			regulator-always-on;
		};

		vaux2_reg: regulator@10 {
			regulator-always-on;
		};

		vaux33_reg: regulator@11 {
			regulator-always-on;
		};

		vmmc_reg: regulator@12 {
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
		};
	};
};

&mac {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&cpsw_default>;
	pinctrl-1 = <&cpsw_sleep>;
	status = "okay";
	slaves = <1>;
};

&davinci_mdio {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&davinci_mdio_default>;
	pinctrl-1 = <&davinci_mdio_sleep>;
	status = "okay";
};

&cpsw_emac0 {
	phy_id = <&davinci_mdio>, <4>;
	phy-mode = "rgmii-txid";
};


&tscadc {
	status = "okay";
	tsc {
		ti,wires = <4>;
		ti,x-plate-resistance = <300>;
		ti,coordinate-readouts = <5>;
		ti,wire-config = <0x00 0x11 0x22 0x33>;
		ti,charge-delay = <0x400>;
	};

	adc {
		ti,adc-channels = <4 5 6 7>;
	};
};

&mmc1 {
	status = "okay";
//	vmmc-supply = <&vmmc_reg>;
	vmmc-supply = <&vmmcsd_fixed>;
	bus-width = <4>;
	pinctrl-names = "default";
	pinctrl-0 = <&mmc1_pins>;
	cd-gpios = <&gpio0 5 GPIO_ACTIVE_HIGH>;/*our cd pin is gpio0_5*/
};


&mmc3 {
       /* these are on the crossbar and are outlined in the
          xbar-event-map element */
       dmas = <&edma_xbar 12 0 1
               &edma_xbar 13 0 2>;
       dma-names = "tx", "rx";
       status = "okay";
       vmmc-supply = <&vmmcsd_fixed>;
       /*vmmc-supply = <&wlan_en_reg>;*/
       bus-width = <4>;
       pinctrl-names = "default";
       pinctrl-0 = <&mmc2_pins_default>;
       ti,non-removable;
       ti,needs-special-hs-handling;
       cap-power-off-card;
       keep-power-in-suspend;
       no-1-8-v;
       #address-cells = <1>;
       #size-cells = <0>;
       rtl8723bs_wifi: rtl8723bs_wifi@0 {
               compatible = "ti,rtl8723bs";
               reg = <2>;
/*               interrupt-parent = <&gpio3>;
               interrupts = <17 IRQ_TYPE_LEVEL_HIGH>;*/
       };
};




&edma {
	ti,edma-xbar-event-map = /bits/ 16 <1 12
					    2 13>;
};

&sham {
	status = "okay";
};

&aes {
	status = "okay";
};

&dcan0 {
	status = "okay";	/* Enable only if Profile 1 is selected */
	pinctrl-names = "default";
	pinctrl-0 = <&dcan0_pins_default>;
};

&dcan1 {
	status = "okay";	/* Enable only if Profile 1 is selected */
	pinctrl-names = "default";
	pinctrl-0 = <&dcan1_pins_default>;
};

&wkup_m3_ipc {
	ti,scale-data-fw = "am335x-evm-scale-data.bin";
};

&rtc {
	clocks = <&clk_32768_ck>, <&clkdiv32k_ick>;
	clock-names = "ext-clk", "int-clk";
};

&sgx {
	status = "okay";
};
