U-Boot SPL 2016.05 (Aug 16 2017 - 18:32:05)
DRA752-GP ES2.0
MMC Device 1 not found
*** Warning - No MMC card found, using default environment

Trying to boot from MMC1
MMC Device 1 not found
*** Warning - No MMC card found, using default environment

reading u-boot.img
reading u-boot.img
reading u-boot.img
reading u-boot.img


U-Boot 2016.05 (Aug 16 2017 - 18:32:05 +0800)

CPU  : DRA752-GP ES2.0
Model: TI DRA742
Board: DRA74x EVM REV 
DRAM:  256 MiB
NAND:  0 MiB
MMC:   OMAP SD/MMC: 0, OMAP SD/MMC: 1
** First descriptor is NOT a primary desc on 1:1 **
*** Warning - bad CRC, using default environment

Warning: fastboot.board_rev: unknown board revision
GUID Partition Table Header signature is wrong: 0x0 != 0x5452415020494645
part_get_info_efi: *** ERROR: Invalid GPT ***
GUID Partition Table Header signature is wrong: 0x0 != 0x5452415020494645
part_get_info_efi: *** ERROR: Invalid Backup GPT ***
ERROR: cannot find partition: 'userdata'

at arch/arm/cpu/armv7/omap-common/utils.c:195/mmc_get_part_size()
Warning: fastboot.userdata_size: unable to calc
SCSI:  SATA link 0 timeout.
AHCI 0001.0300 32 slots 1 ports 3 Gbps 0x1 impl SATA mode
flags: 64bit ncq stag pm led clo only pmp pio slum part ccc apst 
scanning bus for devices...
Found 0 device(s).
Net:   
Warning: ethernet@48484000 using MAC address from ROM
eth0: ethernet@48484000
@ADAPTER@
Hit any key to stop autoboot:  2  1  0 
switch to partitions #0, OK
mmc0 is current device
SD/MMC found on device 0
reading boot.scr
** Unable to read file boot.scr **
reading uEnv.txt
222 bytes read in 2 ms (108.4 KiB/s)
Loaded env from uEnv.txt
Importing environment from mmc0 ...
switch to partitions #0, OK
mmc0 is current device
SD/MMC found on device 0
3619768 bytes read in 345 ms (10 MiB/s)
109108 bytes read in 65 ms (1.6 MiB/s)
Booting from mmc0 ...
Kernel image @ 0x82000000 [ 0x000000 - 0x373bb8 ]
## Flattened Device Tree blob at 88000000
   Booting using the fdt blob at 0x88000000
   Loading Device Tree to 8eee0000, end 8eefda33 ... OK

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Initializing cgroup subsys cpuset
[    0.000000] Initializing cgroup subsys cpu
[    0.000000] Initializing cgroup subsys cpuacct
[    0.000000] Linux version 4.4.45 (hsuyz@hsuyz-VirtualBox) (gcc version 5.3.1 20160113 (Linaro GCC 5.3-2016.02) ) #10 SMP PREEMPT Wed Aug 16 18:32:11 CST 2017
[    0.000000] CPU: ARMv7 Processor [412fc0f2] revision 2 (ARMv7), cr=30c5387d
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, PIPT instruction cache
[    0.000000] Machine model: TI DRA742
[    0.000000] cma: Reserved 64 MiB at 0x000000008ac00000
[    0.000000] Forcing write-allocate cache policy for SMP
[    0.000000] Memory policy: Data cache writealloc
[    0.000000] DRA752 ES2.0
[    0.000000] PERCPU: Embedded 11 pages/cpu @cfb19000 s14848 r8192 d22016 u45056
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 64448
[    0.000000] Kernel command line: console=ttyO3,115200n8 elevator=noop root=PARTUUID=84346fd0-02 rw rootwait earlyprintk fixrtc omapdrm.num_crtc=2 consoleblank=0 cma=64M rootfstype=ext4 snd.slots_reserved=1,1
[    0.000000] PID hash table entries: 1024 (order: 0, 4096 bytes)
[    0.000000] Dentry cache hash table entries: 32768 (order: 5, 131072 bytes)
[    0.000000] Inode-cache hash table entries: 16384 (order: 4, 65536 bytes)
[    0.000000] Memory: 181200K/260096K available (6607K kernel code, 363K rwdata, 2464K rodata, 332K init, 290K bss, 13360K reserved, 65536K cma-reserved, 0K highmem)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
[    0.000000]     fixmap  : 0xffc00000 - 0xfff00000   (3072 kB)
[    0.000000]     vmalloc : 0xd0800000 - 0xff800000   ( 752 MB)
[    0.000000]     lowmem  : 0xc0000000 - 0xd0000000   ( 256 MB)
[    0.000000]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
[    0.000000]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)
[    0.000000]       .text : 0xc0008000 - 0xc08e4044   (9073 kB)
[    0.000000]       .init : 0xc08e5000 - 0xc0938000   ( 332 kB)
[    0.000000]       .data : 0xc0938000 - 0xc0992e90   ( 364 kB)
[    0.000000]        .bss : 0xc0994000 - 0xc09dc800   ( 290 kB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=2, Nodes=1
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000] 	Build-time adjustment of leaf fanout to 32.
[    0.000000] NR_IRQS:16 nr_irqs:16 16
[    0.000000] ti_dt_clocks_register: failed to lookup clock node gmac_gmii_ref_clk_div
[    0.000000] OMAP clockevent source: timer1 at 32786 Hz
[    0.000000] Architected cp15 timer(s) running at 6.14MHz (phys).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x16af5adb9, max_idle_ns: 440795202250 ns
[    0.000005] sched_clock: 56 bits at 6MHz, resolution 162ns, wraps every 4398046511023ns
[    0.000015] Switching to timer-based delay loop, resolution 162ns
[    0.000331] clocksource: 32k_counter: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 58327039986419 ns
[    0.000338] OMAP clocksource: 32k_counter at 32768 Hz
[    0.000806] Console: colour dummy device 80x30
[    0.000826] WARNING: Your 'console=ttyO3' has been replaced by 'ttyS3'
[    0.000833] This ensures that you still see kernel messages. Please
[    0.000838] update your kernel commandline.
[    0.000850] Calibrating delay loop (skipped), value calculated using timer frequency.. 12.29 BogoMIPS (lpj=61475)
[    0.000863] pid_max: default: 32768 minimum: 301
[    0.000959] Mount-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.000968] Mountpoint-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.001546] Initializing cgroup subsys io
[    0.001564] Initializing cgroup subsys memory
[    0.001591] Initializing cgroup subsys devices
[    0.001603] Initializing cgroup subsys freezer
[    0.001616] Initializing cgroup subsys perf_event
[    0.001627] Initializing cgroup subsys pids
[    0.001654] CPU: Testing write buffer coherency: ok
[    0.001883] /cpus/cpu@0 missing clock-frequency property
[    0.001899] /cpus/cpu@1 missing clock-frequency property
[    0.001910] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000
[    0.001946] Setting up static identity map for 0x800082c0 - 0x80008320
[    0.080123] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001
[    0.080183] Brought up 2 CPUs
[    0.080197] SMP: Total of 2 processors activated (24.59 BogoMIPS).
[    0.080204] CPU: All CPU(s) started in HYP mode.
[    0.080209] CPU: Virtualization extensions available.
[    0.080614] devtmpfs: initialized
[    0.110790] VFP support v0.3: implementor 41 architecture 4 part 30 variant f rev 0
[    0.111793] omap_hwmod: l3_main_2 using broken dt data from ocp
[    0.227209] omap_hwmod: dcan1: _wait_target_disable failed
[    0.325558] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.327210] pinctrl core: initialized pinctrl subsystem
[    0.328081] NET: Registered protocol family 16
[    0.329175] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.350221] cpuidle: using governor ladder
[    0.380246] cpuidle: using governor menu
[    0.388608] OMAP GPIO hardware version 0.1
[    0.392697] GPIO line 161 (radio_rst) hogged as output/low
[    0.395045] irq: no irq domain found for /ocp/l4@4a000000/scm@2000/pinmux@1400 !
[    0.410771] omap-gpmc 50000000.gpmc: could not find pctldev for node /ocp/l4@4a000000/scm@2000/pinmux@1400/nand_flash_x16, deferring probe
[    0.417767] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.417777] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.418598] OMAP DMA hardware revision 0.0
[    0.461596] omap-dma-engine 4a056000.dma-controller: OMAP DMA engine driver (LinkedList1/2/3 supported)
[    0.462725] edma 43300000.edma: memcpy is disabled
[    0.467601] edma 43300000.edma: TI EDMA DMA engine driver
[    0.474332] palmas 0-0058: IRQ missing: skipping irq request
[    0.491241] palmas 0-0058: Muxing GPIO a, PWM 0, LED 0
[    0.562942] omap_i2c 48070000.i2c: bus 0 rev0.12 at 400 kHz
[    0.563366] omap_i2c 48072000.i2c: bus 1 rev0.12 at 400 kHz
[    0.563735] omap_i2c 48060000.i2c: bus 2 rev0.12 at 400 kHz
[    0.564096] omap_i2c 4807a000.i2c: bus 3 rev0.12 at 400 kHz
[    0.564455] omap_i2c 4807c000.i2c: bus 4 rev0.12 at 400 kHz
[    0.564632] media: Linux media interface: v0.10
[    0.564687] Linux video capture interface: v2.00
[    0.564727] pps_core: LinuxPPS API ver. 1 registered
[    0.564734] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.564758] PTP clock support registered
[    0.564804] EDAC MC: Ver: 3.0.0
[    0.565564] Advanced Linux Sound Architecture Driver Initialized.
[    0.566476] clocksource: Switched to clocksource arch_sys_counter
[    0.577186] NET: Registered protocol family 2
[    0.577699] TCP established hash table entries: 2048 (order: 1, 8192 bytes)
[    0.577725] TCP bind hash table entries: 2048 (order: 2, 16384 bytes)
[    0.577763] TCP: Hash tables configured (established 2048 bind 2048)
[    0.577811] UDP hash table entries: 256 (order: 1, 8192 bytes)
[    0.577833] UDP-Lite hash table entries: 256 (order: 1, 8192 bytes)
[    0.578034] NET: Registered protocol family 1
[    0.578312] RPC: Registered named UNIX socket transport module.
[    0.578321] RPC: Registered udp transport module.
[    0.578327] RPC: Registered tcp transport module.
[    0.578334] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.579334] hw perfevents: enabled with armv7_cortex_a15 PMU driver, 7 counters available
[    0.581687] futex hash table entries: 512 (order: 3, 32768 bytes)
[    0.589553] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.590187] NFS: Registering the id_resolver key type
[    0.590217] Key type id_resolver registered
[    0.590226] Key type id_legacy registered
[    0.590281] ntfs: driver 2.1.32 [Flags: R/O].
[    0.592444] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 247)
[    0.592460] io scheduler noop registered (default)
[    0.592472] io scheduler deadline registered
[    0.592511] io scheduler cfq registered
[    0.597449] pinctrl-single 4a003400.pinmux: 282 pins at pa fc003400 size 1128
[    0.659391] Serial: 8250/16550 driver, 10 ports, IRQ sharing disabled
[    0.662841] 4806a000.serial: ttyS0 at MMIO 0x4806a000 (irq = 299, base_baud = 3000000) is a 8250
[    0.663716] 4806c000.serial: ttyS1 at MMIO 0x4806c000 (irq = 300, base_baud = 3000000) is a 8250
[    0.664567] 48020000.serial: ttyS2 at MMIO 0x48020000 (irq = 301, base_baud = 3000000) is a 8250
[    0.665410] console [ttyS3] disabled
[    0.665457] 4806e000.serial: ttyS3 at MMIO 0x4806e000 (irq = 302, base_baud = 3000000) is a 8250
[    1.449805] console [ttyS3] enabled
[    1.454124] 48422000.serial: ttyS7 at MMIO 0x48422000 (irq = 303, base_baud = 3000000) is a 8250
[    1.464077] [drm] Initialized drm 1.1.0 20060810
[    1.476020] loop: module loaded
[    1.484562] m25p80 spi32766.0: n25q128a13 (16384 Kbytes)
[    1.489981] 7 ofpart partitions found on MTD device spi32766.0
[    1.495840] Creating 7 MTD partitions on "spi32766.0":
[    1.501018] 0x000000000000-0x000000040000 : "QSPI.MLO"
[    1.507113] 0x000000040000-0x000000140000 : "QSPI.u-boot"
[    1.513402] 0x000000140000-0x0000001c0000 : "QSPI.DRA7-evm.dtb"
[    1.520243] 0x0000001c0000-0x0000001d0000 : "QSPI.u-boot-env"
[    1.526881] 0x0000001d0000-0x0000001e0000 : "QSPI.u-boot-env.backup1"
[    1.534210] 0x0000001e0000-0x0000009e0000 : "QSPI.uImage"
[    1.540531] 0x0000009e0000-0x000002000000 : "QSPI.IPU-exe"
[    1.546044] mtd: partition "QSPI.IPU-exe" extends beyond the end of device "spi32766.0" -- size truncated to 0x620000
[    1.558621] libphy: Fixed MDIO Bus: probed
[    1.606510] davinci_mdio 48485000.mdio: davinci mdio revision 1.6
[    1.612633] davinci_mdio 48485000.mdio: detected phy mask fffffffa
[    1.622829] libphy: 48485000.mdio: probed
[    1.626900] davinci_mdio 48485000.mdio: phy[0]: device 48485000.mdio:00, driver Micrel KSZ8081 or KSZ8091
[    1.636546] davinci_mdio 48485000.mdio: phy[2]: device 48485000.mdio:02, driver Micrel KSZ8081 or KSZ8091
[    1.646838] cpsw 48484000.ethernet: Detected MACID = c8:fd:19:b6:5e:f6
[    1.653485] cpsw 48484000.ethernet: cpts: overflow check period 800
[    1.660512] cpsw 48484000.ethernet: cpsw: Detected MACID = c8:fd:19:b6:5e:f7
[    1.669122] mousedev: PS/2 mouse device common for all mice
[    1.675280] i2c /dev entries driver
[    1.680279] vpe 489d0000.vpe: loading firmware vpdma-1b8.bin
[    1.690533] omap_hsmmc 4809c000.mmc: Got CD GPIO
[    1.696675] vpe 489d0000.vpe: Device registered as /dev/video0
[    1.747016] omap_hsmmc 480b4000.mmc: no pinctrl state for sdr25 mode
[    1.753400] omap_hsmmc 480b4000.mmc: no pinctrl state for sdr12 mode
[    1.776622] evm_3v3_sw: supplied by sysen1
[    1.817178] ledtrig-cpu: registered to indicate activity on CPUs
[    1.827433] hwspinlock_user gatemp: requested 10 hwspinlocks
[    1.833805] 
[    1.833805] [mcaspdrv_init]
[    1.838112] mcaspdrv_init called
[    1.842385] 
[    1.842385] ============[davinci_mcasp_probe]==============
[    1.849531] ====>pm_runtime_forbid
[    1.852950] davinci-mcasp 48460000.mcasp: DAI is shared
[    1.858252] =========> [davinci_mcasp_probe] mem->start  =	[00000000] <==
[    1.865069] =========> [davinci_mcasp_probe] mcasp->base =  [FA460000] <==
[    1.872003] =====[McASP1]====
[    1.874983] =====[mcasp->base][FA460000]=====
[    1.879455] 
[    1.879455] ============[davinci_mcasp_probe]==============
[    1.886589] ====>pm_runtime_forbid
[    1.890007] davinci-mcasp 48468000.mcasp: DAI is shared
[    1.895267] =========> [davinci_mcasp_probe] mem->start  =	[00000000] <==
[    1.902096] =========> [davinci_mcasp_probe] mcasp->base =  [FA468000] <==
[    1.909008] =====[McASP3]====
[    1.911985] =====[mcasp->base][FA468000]=====
[    1.911985] 
[    1.918960] NET: Registered protocol family 10
[    1.934391] sit: IPv6 over IPv4 tunneling driver
[    1.939639] NET: Registered protocol family 17
[    1.944320] Key type dns_resolver registered
[    1.948782] omap_voltage_late_init: Voltage driver support not added
[    1.955666] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    1.961888] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[    1.968149] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[    1.974753] Power Management for TI OMAP4+ devices.
[    1.979892] Registering SWP/SWPB emulation handler
[    1.987536] dmm 4e000000.dmm: initialized all PAT entries
[    2.003626] omap-gpmc 50000000.gpmc: GPMC revision 6.0
[    2.008832] gpmc_mem_init: disabling cs 0 mapped at 0x0-0x1000000
[    2.015187] omap-gpmc 50000000.gpmc: cannot remap GPMC CS 0 to 0x0000000000000000
[    2.022721] omap-gpmc 50000000.gpmc: GPMC CS 0 start cannot be lesser than 0x1000000
[    2.023650] mmc0: host does not support reading read-only switch, assuming write-enable
[    2.025584] mmc0: new high speed SDHC card at address b368
[    2.040784] mmcblk0: mmc0:b368 SDC   7.51 GiB 
[    2.047413]  mmcblk0: p1 p2
[    2.051371] omap-gpmc 50000000.gpmc: failed to probe DT children
[    2.057560] omap-gpmc: probe of 50000000.gpmc failed with error -16
[    2.064216] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    2.070450] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[    2.076718] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[    2.083663] hctosys: unable to open rtc device (rtc0)
[    2.100305] mmc1: MAN_BKOPS_EN bit is not set
[    2.101024] aic_dvdd: disabling
[    2.101029] vmmcwl_fixed: disabling
[    2.111416] ldousb: disabling
[    2.114891] ALSA device list:
[    2.117887]   No soundcards found.
[    2.153671] EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Opts: (null)
[    2.161852] VFS: Mounted root (ext4 filesystem) on device 179:2.
[    2.177830] mmc1: new HS200 MMC card at address 0001
[    2.183270] mmcblk1: mmc1:0001 MMC04G 3.57 GiB 
[    2.188009] devtmpfs: mounted
[    2.191298] Freeing unused kernel memory: 332K (c08e5000 - c0938000)
[    2.197700] This architecture does not have kernel memory protection.
[    2.204243] mmcblk1boot0: mmc1:0001 MMC04G partition 1 8.00 MiB
[    2.220492] mmcblk1boot1: mmc1:0001 MMC04G partition 2 8.00 MiB
[    2.228272] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    2.234622] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[    2.241004] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[    2.650725] systemd[1]: System time before build time, advancing clock.
[    2.732072] random: systemd: uninitialized urandom read (16 bytes read, 12 bits of entropy available)
[    2.745068] random: systemd: uninitialized urandom read (16 bytes read, 12 bits of entropy available)
[    2.759797] systemd[1]: systemd 229 running in system mode. (+PAM -AUDIT -SELINUX +IMA -APPARMOR +SMACK +SYSVINIT +UTMP -LIBCRYPTSETUP -GCRYPT +GNUTLS +ACL +XZ -LZ4 -SECCOMP +BLKID -ELFUTILS +KMOD -IDN)
[    2.778388] systemd[1]: Detected architecture arm.

Welcome to Arago 2016.12!

[    2.807744] systemd[1]: Set hostname to <dra7xx-evm>.
[    2.898847] random: systemd-sysv-ge: uninitialized urandom read (16 bytes read, 14 bits of entropy available)
[    2.910115] random: systemd-gpt-aut: uninitialized urandom read (16 bytes read, 14 bits of entropy available)
[    2.920337] random: systemd-gpt-aut: uninitialized urandom read (16 bytes read, 14 bits of entropy available)
[    2.948479] random: systemd-sysv-ge: uninitialized urandom read (16 bytes read, 14 bits of entropy available)
[    2.965363] random: systemd-sysv-ge: uninitialized urandom read (16 bytes read, 15 bits of entropy available)
[    3.116525] random: systemd: uninitialized urandom read (16 bytes read, 18 bits of entropy available)
[    3.126052] random: systemd: uninitialized urandom read (16 bytes read, 18 bits of entropy available)
[    3.136053] random: systemd: uninitialized urandom read (16 bytes read, 18 bits of entropy available)
[    3.506728] systemd[1]: Configuration file /etc/systemd/system/multi-user.target.wants/CAX50.service is marked executable. Please remove executable permission bits. Proceeding anyway.
[    3.523263] systemd[1]: Configuration file /etc/systemd/system/multi-user.target.wants/CAX50.service is marked world-writable. Please remove world writability permission bits. Proceeding anyway.
[    3.636126] systemd[1]: sysinit.target: Found ordering cycle on sysinit.target/start
[    3.643971] systemd[1]: sysinit.target: Found dependency on alignment.service/start
[    3.651759] systemd[1]: sysinit.target: Found dependency on basic.target/start
[    3.659053] systemd[1]: sysinit.target: Found dependency on sysinit.target/start
[    3.666505] systemd[1]: sysinit.target: Breaking ordering cycle by deleting job alignment.service/start
[    3.675946] systemd[1]: alignment.service: Job alignment.service/start deleted to break ordering cycle starting with sysinit.target/start
[ SKIP ] Ordering cycle found, skipping alignment.service
[    3.719303] systemd[1]: Listening on udev Kernel Socket.
[  OK  ] Listening on udev Kernel Socket.
[    3.746897] systemd[1]: Started Forward Password Requests to Wall Directory Watch.
[  OK  ] Started Forward Password Requests to Wall Directory Watch.
[    3.776640] systemd[1]: Reached target Remote File Systems.
[  OK  ] Reached target Remote File Systems.
[    3.806798] systemd[1]: Listening on Journal Socket.
[  OK  ] Listening on Journal Socket.
[    3.836709] systemd[1]: Listening on Syslog Socket.
[  OK  ] Listening on Syslog Socket.
[    3.858120] systemd[1]: Created slice System Slice.
[  OK  ] Created slice System Slice.
[    3.916727] systemd[1]: Mounting Debug File System...
         Mounting Debug File System...
[    3.949513] systemd[1]: Mounting POSIX Message Queue File System...
         Mounting POSIX Message Queue File System...
[    3.977456] systemd[1]: Created slice system-serial\x2dgetty.slice.
[  OK  ] Created slice system-serial\x2dgetty.slice.
[    4.006906] systemd[1]: Listening on Network Service Netlink Socket.
[  OK  ] Listening on Network Service Netlink Socket.
[    4.036762] systemd[1]: Listening on Journal Socket (/dev/log).
[  OK  ] Listening on Journal Socket (/dev/log).
[    4.066630] systemd[1]: Reached target Swap.
[  OK  ] Reached target Swap.
[    4.126909] systemd[1]: Starting Load Kernel Modules...
         Starting Load Kernel Modules...
[    4.159071] systemd[1]: Starting Remount Root and Kernel File Systems...
         Starting Remount Root and Kernel File Systems...
[    4.178022] EXT4-fs (mmcblk0p2): re-mounted. Opts: (null)
[    4.207152] systemd[1]: Starting Create list of required static device nodes for the current kernel...
         Starting Create list of required st... nodes for the current kernel...
[    4.236824] systemd[1]: Listening on udev Control Socket.
[  OK  ] Listening on udev Control Socket.
[    4.266842] systemd[1]: Listening on /dev/initctl Compatibility Named Pipe.
[  OK  ] Listening on /dev/initctl Compatibility Named Pipe.
[    4.336750] systemd[1]: Mounting Temporary Directory...
         Mounting Temporary Directory...
[    4.369052] systemd[1]: Starting Setup Virtual Console...
         Starting Setup Virtual Console...
[    4.396920] systemd[1]: Started Dispatch Password Requests to Console Directory Watch.
[  OK  ] Started Dispatch Password Requests to Console Directory Watch.
[    4.426669] systemd[1]: Reached target Paths.
[  OK  ] Reached target Paths.
[    4.447369] systemd[1]: Created slice User and Session Slice.
[  OK  ] Created slice User and Session Slice.
[    4.476718] systemd[1]: Reached target Slices.
[  OK  ] Reached target Slices.
[    4.536929] systemd[1]: Starting Journal Service...
         Starting Journal Service...
[    4.574389] systemd[1]: Mounted Debug File System.
[  OK  ] Mounted Debug File System.
[    4.596804] systemd[1]: Mounted POSIX Message Queue File System.
[  OK  ] Mounted POSIX Message Queue File System.
[    4.626743] systemd[1]: Mounted Temporary Directory.
[  OK  ] Mounted Temporary Directory.
[    4.647623] systemd[1]: systemd-modules-load.service: Main process exited, code=exited, status=1/FAILURE
[    4.658600] systemd[1]: Failed to start Load Kernel Modules.
[FAILED] Failed to start Load Kernel Modules.
See 'systemctl status systemd-modules-load.service' for details.
[    4.706623] systemd[1]: systemd-modules-load.service: Unit entered failed state.
[    4.714070] systemd[1]: systemd-modules-load.service: Failed with result 'exit-code'.
[    4.723110] systemd[1]: Started Remount Root and Kernel File Systems.
[  OK  ] Started Remount Root and Kernel File Systems.
[    4.747809] systemd[1]: Started Create list of required static device nodes for the current kernel.
[  OK  ] Started Create list of required sta...ce nodes for the current kernel.
[    4.778459] systemd[1]: Started Setup Virtual Console.
[  OK  ] Started Setup Virtual Console.
[    4.807137] systemd[1]: Started Journal Service.
[  OK  ] Started Journal Service.
         Starting Create Static Device Nodes in /dev...
         Starting Flush Journal to Persistent Storage...
         Starting udev Coldplug all Devices...
         Starting Apply Kernel Variables...
[  OK  ] Started Create Static Device Nodes in /dev.
[  OK  ] Started Apply Kernel Variables.
[    5.456807] systemd-journald[126]: Received request to flush runtime journal from PID 1
[  OK  ] Started Flush Journal to Persistent Storage.
[  OK  ] Reached target Local File Systems (Pre).
         Mounting /media/ram...
         Mounting /var/volatile...
         Starting udev Kernel Device Manager...
[  OK  ] Mounted /var/volatile.
[  OK  ] Mounted /media/ram.
[    5.809341] mmcblk0: error -110 sending status command, retrying
[    5.826539] mmcblk0: timed out sending r/w cmd command, card status 0x800b00
[  OK  ] Started udev Kernel Device Manager.
[  OK  ] Reached target Local File Systems.
         Starting Create Volatile Files and Directories...
         Starting Load/Save Random Seed...
[  OK  ] Started Create Volatile Files and Directories.
[  OK  ] Started udev Coldplug all Devices.
[  OK  ] Started Load/Save Random Seed.
[    6.283084] omap_rng 48090000.rng: OMAP Random Number Generator ver. 20
[    6.308742] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    6.314963] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[    6.363494] omap-des 480a5000.des: OMAP DES hw accel rev: 2.2
[    6.403142] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[    6.416985] alg: skcipher: setkey failed on test 5 for ecb-des-omap: flags=100
[    6.473082] alg: skcipher-ddst: setkey failed on test 5 for ecb-des-omap: flags=100
[    6.525854] alg: skcipher-ddst: setkey failed on test 5 for ecb-des-omap: flags=100
[  OK  ] Found device /dev/ttyS3.
[    6.586423] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    6.597852] omap_rtc 48838000.rtc: rtc core: registered 48838000.rtc as rtc0
[    6.625629] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[    6.650333] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[    6.664343] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    6.681809] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
         Starting Network Time Synchronization...
[    6.711105] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
         Starting Update UTMP about System Boot/Shutdown...
[    6.808863] SCSI subsystem initialized
[    6.859075] omap_wdt: OMAP Watchdog Timer Rev 0x01: initial timeout 60 sec
[    6.874043] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    6.889424] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[    6.904797] omap-sham 4b101000.sham: hw accel on OMAP rev 4.3
[  OK  ] Started Network Time Synchronization.[    6.925752] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517

[    6.950499] CAN device driver interface
[  OK  ] Started Update UTMP about System Boot/Shutdown.
[  OK  ] Reached target System Time Synchronized.
         Starting Synchronize System and HW clocks...
[  OK  ] Started Synchronize System and HW clocks.
[    7.681484] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[  OK  ] Reached target System Initialization.[    7.701303] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm

[    7.718277] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[    7.734960] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    7.757549] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[  OK  ] Listening on dropbear.socket.[    7.771282] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517

[  OK  ] Listening on Avahi mDNS/DNS-SD Stack Activation Socket.
[  OK  ] Listening on D-Bus System Message Bus Socket.
[    7.834213] omap-aes 4b500000.aes: OMAP AES hw accel rev: 3.3
[    7.835084] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    7.835089] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[    7.835148] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[  OK  ] Listening on RPCbind Server Activation Socket.
[  OK  ] Reached target Sockets.
[    7.894986] FAT-fs (mmcblk0p1): Volume was not properly unmounted. Some data may be corrupt. Please run fsck.
[  OK  ] Reached target Basic System.
[    7.911833] omap-aes 4b700000.aes: OMAP AES hw accel rev: 3.3
[    7.917981] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    7.925937] ahci 4a140000.sata: SSS flag set, parallel bus scan disabled
[    7.937220] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[    7.950289] ahci 4a140000.sata: AHCI 0001.0300 32 slots 1 ports 3 Gbps 0x1 impl platform mode
[  OK  ] Started Start helloworld.
[  OK  ] Started Kernel Logging Service.
[    7.989496] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
         Starting Avahi mDNS/DNS-SD Stack...


[INFO] VERSION: R0.2.0.0004
[    8.036577] ahci 4a140000.sata: flags: 64bit ncq sntf stag pm led clo only pmp pio slum part ccc apst 
[  OK  ] Started strongSwan IPsec IKEv1/IKEv2 daemon using ipsec.conf.
[    8.072175] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[  OK  ] Started System Logging Service.
         Starting Login Service...
         Starting Telephony service...[    8.117379] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm

         Starting Print notice about GPLv3 packages...
[    8.166843] scsi host0: ahci
[    8.170161] ata1: SATA max UDMA/133 mmio [mem 0x4a140000-0x4a1410ff] port 0x100 irq 335
         Starting uim-sysfs.service...
[  OK  ] Started Daily Cleanup of Temporary Directories.[    8.190769] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517

[  OK  ] Reached target Timers.
         Starting Permit User Sessions...
[  OK  ] Started D-Bus System Message Bus.
[    8.255597] [drm] Initialized pvr 1.14.3699939 20110701 on minor 0
[    8.264006] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    8.282364] c_can_platform 4ae3c000.can: c_can_platform device registered (regs=fce3c000, irq=349)
[    8.314637] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[INFO] memory test PASS
[    8.339212] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[SYS ] paring option: token=3, option=(null)
[INFO] R3 init, iface=/dev/ttyS7
[INFO] R2 init
[INFO] watchdog init
[INFO] CLIENT ready
[    8.368809] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    8.392511] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[    8.426773] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[    8.587332] ata1: SATA link down (SStatus 0 SControl 300)
[  OK  ] Started Telephony service.
[  OK  ] Started Avahi mDNS/DNS-SD Stack.
         Starting Network Service...
[  OK  ] Started Permit User Sessions.
[    8.841897] Bluetooth: Core ver 2.21
[    8.845542] NET: Registered protocol family 31
[    8.874959] Bluetooth: HCI device and connection manager initialized
[    8.907335] Bluetooth: HCI socket layer initialized
[    8.912248] Bluetooth: L2CAP socket layer initialized
[    8.921531] NET: Registered protocol family 15
[    8.966862] Bluetooth: SCO socket layer initialized
[  OK  ] Started Network Service.
[    9.099400] net eth1: initializing cpsw version 1.15 (0)
[    9.146203] net eth0: initialized cpsw ale version 1.4
[    9.193165] net eth0: ALE Table size 1024
[    9.204803] Initializing XFRM netlink socket
[    9.234006] libphy: PHY 48485000.mdio:03 not found
[    9.277110] net eth1: phy "48485000.mdio:03" not found on slave 1, err -19
[    9.363858] IPv6: ADDRCONF(NETDEV_UP): eth1: link is not ready
[    9.420417] net eth0: initializing cpsw version 1.15 (0)
[    9.522512] net eth0: phy found : id is : 0x221560
[    9.558081] IPv6: ADDRCONF(NETDEV_UP): eth0: link is not ready
[   10.159581] random: nonblocking pool is initialized
[   10.268262] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[   10.281357] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[   10.313735] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[   10.733915] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[   10.743101] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[   10.769511] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[   10.814689] usbcore: registered new interface driver usbfs
[   10.840238] usbcore: registered new interface driver hub
[   10.858937] usbcore: registered new device driver usb
[   10.900975] dwc3 48890000.usb: otg: primary host xhci-hcd.0.auto registered
[   10.912552] dwc3 48890000.usb: otg: shared host xhci-hcd.0.auto registered
[   10.931299] dwc3 48890000.usb: otg: can't start till gadget registers
[   10.952835] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[   10.959305] xhci-hcd xhci-hcd.1.auto: xHCI Host Controller
[   10.966007] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[   10.982594] xhci-hcd xhci-hcd.1.auto: new USB bus registered, assigned bus number 1
[   10.991341] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[   11.012916] xhci-hcd xhci-hcd.1.auto: hcc params 0x0220f04c hci version 0x100 quirks 0x00210010
[   11.040356] xhci-hcd xhci-hcd.1.auto: irq 424, io mem 0x488d0000
[   11.065466] hub 1-0:1.0: USB hub found
[   11.086827] hub 1-0:1.0: 1 port detected
[   11.101696] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[   11.108994] xhci-hcd xhci-hcd.1.auto: xHCI Host Controller
[   11.114519] xhci-hcd xhci-hcd.1.auto: new USB bus registered, assigned bus number 2
[   11.124399] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[   11.150155] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[   11.170655] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[   11.178657] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[   11.178662] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[   11.178717] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[   11.270892] hub 2-0:1.0: USB hub found
[   11.284839] hub 2-0:1.0: 1 port detected
[  OK  ] Listening on Load/Save RF Kill Switch Status /dev/rfkill Watch.
[  OK  ] Reached target Network.
[   11.344746] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[   11.355056] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
         Starting Network Name Resolution...
         Starting Lightning Fast Webserver With Light System Requirements...
[  OK  ] Started Serial Getty on ttyS3.
[  OK  ] Reached target Login Prompts.
[   11.414167] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[   11.426802] usb 1-1: new high-speed USB device number 2 using xhci-hcd
[  OK  ] Started Login Service.
[   11.457510] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[   11.463728] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[   11.496681] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[  OK  ] Started Lightning Fast Webserver With Light System Requirements.
[  OK  ] Started Network Name Resolution.
[   11.589756] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[   11.595974] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[   11.636735] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
[   11.793228] usbcore: registered new interface driver r8152
[   11.818290] usbcore: registered new interface driver cdc_ether
[   11.954740] usb 1-1: reset high-speed USB device number 2 using xhci-hcd
[  OK  ] Started uim-sysfs.service.
         Starting rc.pvr.service...
[   12.151874] r8152 1-1:1.0 eth2: v1.08.2
[   12.156172] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[   12.167061] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[   12.185679] ti_oppdm 4a003b20.oppdm: Unable to get vdd regulator:-517
***************************************************************
***************************************************************
NOTICE: This file system contains the following GPLv3 packages:
	autoconf
	binutils-dev
	binutils
	bison-dev
	bison
	cpp-symlinks
	cpp
	dosfstools
	g++-symlinks
	g++
	gawk-dev
	gawk
	gcc-symlinks
	gcc
	gdb
	gdbc6x
	gdbserver
	gstreamer1.0-libav
	libcairo-perf-utils
	libgmp10
	libidn11
	libmpc3
	libmpfr4
	m4-dev
	m4
	make
	nettle
	parted
	swig-dev
	swig

If you do not wish to distribute GPLv3 components please remove
the above packages prior to distribution.  This can be done using
the opkg remove command.  i.e.:
    opkg remove <package>
Where <package> is the name printed in the list above

NOTE: If the package is a dependency of another package you
      will be notified of the dependent packages.  You should
      use the --force-removal-of-dependent-packages option to
      also remove the dependent packages as well
***************************************************************
***************************************************************
[  OK  ] Started Print notice about GPLv3 packages.
   12.583905] PVR_K: UM DDK-(3699939) and KM DDK-(3699939) match. [ OK ]
[   12.647455] IPv6: ADDRCONF(NETDEV_UP): eth2: link is not ready
[[;32m  OK   ]Started rc.pvr.service.
         tSarting weston.service...
[[032m  OK   ]Started weston.service.
         tSarting telnetd.service...
         tSarting tiipclad-daemon.service...
[[032m  OK   ]Started telnetd.service.
[[;32m  OK   ]Started tiipclad-daemon.service.
         tSarting thttpd.service...
[[032m  OK   ]Started thttpd.service.
         tSarting rng-tools.service...
[[;32m  OK   ]Started rng-tools.service.
         tSarting gdbserverproxy.service...
[[;32m  OK   ]Started gdbserverproxy.service.
         tSarting matrix-gui-2.0.service...
[[0;2m  OK   ]Started matrix-gui-2.0.service.
         tSarting thermal-zone-init.service...
[[;32m  OK   ]Started thermal-zone-init.service.
[[;32m  OK   ]Reached target Multi-User System.
         tSarting Update UTMP about System Runlevel Changes...
[[032m  OK   ]Started Update UTMP about System Runlevel Chages.
 _____                    _____           _         _   
|  _  |___ ___ ___ ___   |  _  |___ ___  |_|___ ___| |_ 
|     |  _| .'| . | . |  |   __|  _| . | | | -_|  _|  _|
|__|__|_| |__,|_  |___|  |__|  |_| |___|_| |___|___|_|  
              |___|                    |___|            

Arago Project http://arago-project.org dra7xx-evm ttyS3

Arago 2016.12 dra7xx-evm ttyS3

dra7xx-evm login: root (automatic login)

[   13.522040] cpsw 48484000.ethernet eth0: Link is Up - 100Mbps/Full - flow control rx/tx
[   13.530389] IPv6: ADDRCONF(NETDEV_CHANGE): eth0: link becomes ready
root@dra7xx-evm:~# 