Terminal ready

U-Boot SPL 2016.05-00118-gdd926c6-dirty (Jan 23 2018 - 20:16:02)
DRA722-GP ES2.0
Trying to boot from MMC1
reading args
spl_load_image_fat_os: error reading image args, err - -1
reading u-boot.img
reading u-boot.img
reading u-boot.img
reading u-boot.img


U-Boot 2016.05-00118-gdd926c6-dirty (Jan 23 2018 - 20:16:02 +0800)

CPU  : DRA722-GP ES2.0
Model: TI AM5718 IDK
Board: AM571x IDK REV <NULL>
DRAM:  1 GiB
MMC:   no pinctrl for sdr104
no pinctrl for ddr50
no pinctrl for sdr50
no pinctrl for sdr25
no pinctrl for sdr12
OMAP SD/MMC: 0, OMAP SD/MMC: 1
reading uboot.env
SCSI:  omap_pipe3_wait_lock: DPLL failed to lock
ERROR: Sata phy enable failed

at drivers/block/dwc_ahci.c:57/dwc_ahci_probe()
ERROR: device probe error

at drivers/block/disk-uclass.c:27/scsi_get_device()
ERROR: scsi device not found

at drivers/block/disk-uclass.c:43/scsi_init()
Net:   
Warning: ethernet@48484000 MAC addresses don't match:
Address in SROM is         50:33:8b:b4:53:60
Address in environment is  50:33:8b:94:22:10
eth0: ethernet@48484000
Hit any key to stop autoboot:  1  0 
switch to partitions #0, OK
mmc0 is current device
reading uEnv.txt
574 bytes read in 4 ms (139.6 KiB/s)
Importing environment from mmc0 ...
3639232 bytes read in 171 ms (20.3 MiB/s)
99156 bytes read in 18 ms (5.3 MiB/s)
switch to partitions #0, OK
mmc0 is current device
SD/MMC found on device 0
reading uEnv.txt
574 bytes read in 3 ms (186.5 KiB/s)
Loaded environment from uEnv.txt
Importing environment from mmc0 ...
3639232 bytes read in 171 ms (20.3 MiB/s)
99156 bytes read in 17 ms (5.6 MiB/s)
Booting from mmc0 ...
Kernel image @ 0x82000000 [ 0x000000 - 0x3787c0 ]
## Flattened Device Tree blob at 88000000
   Booting using the fdt blob at 0x88000000
   Loading Device Tree to 8ffe4000, end 8ffff353 ... OK

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Initializing cgroup subsys cpuset
[    0.000000] Initializing cgroup subsys cpu
[    0.000000] Initializing cgroup subsys cpuacct
[    0.000000] Linux version 4.4.41 (root@ubuntu) (gcc version 5.3.1 20160113 (Linaro GCC 5.3-2016.02) ) #154 SMP PREEMPT Tue Jan 23 04:33:36 PST 2018
[    0.000000] CPU: ARMv7 Processor [412fc0f2] revision 2 (ARMv7), cr=30c5387d
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, PIPT instruction cache
[    0.000000] Machine model: TI AM5718 IDK
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000095800000, size 56 MiB
[    0.000000] Reserved memory: initialized node ipu2_cma@95800000, compatible id shared-dma-pool
[    0.000000] Reserved memory: created CMA memory pool at 0x0000000099000000, size 64 MiB
[    0.000000] Reserved memory: initialized node dsp1_cma@99000000, compatible id shared-dma-pool
[    0.000000] Reserved memory: created CMA memory pool at 0x000000009d000000, size 32 MiB
[    0.000000] Reserved memory: initialized node ipu1_cma@9d000000, compatible id shared-dma-pool
[    0.000000] cma: Reserved 24 MiB at 0x00000000be400000
[    0.000000] Forcing write-allocate cache policy for SMP
[    0.000000] Memory policy: Data cache writealloc
[    0.000000] OMAP4: Map 0x00000000bfd00000 to fe600000 for dram barrier
[    0.000000] DRA722 ES2.0
[    0.000000] PERCPU: Embedded 11 pages/cpu @ef646000 s14848 r8192 d22016 u45056
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 210496
[    0.000000] Kernel command line: console=ttyO2,115200n8 root=PARTUUID=00000780-02 rw rootfstype=ext4 rootwait
[    0.000000] PID hash table entries: 4096 (order: 2, 16384 bytes)
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes)
[    0.000000] Memory: 649404K/848896K available (6659K kernel code, 371K rwdata, 2456K rodata, 336K init, 302K bss, 19268K reserved, 180224K cma-reserved, 234496K highmem)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
[    0.000000]     fixmap  : 0xffc00000 - 0xfff00000   (3072 kB)
[    0.000000]     vmalloc : 0xf0800000 - 0xff800000   ( 240 MB)
[    0.000000]     lowmem  : 0xc0000000 - 0xf0000000   ( 768 MB)
[    0.000000]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
[    0.000000]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)
[    0.000000]       .text : 0xc0008000 - 0xc08ef094   (9117 kB)
[    0.000000]       .init : 0xc08f0000 - 0xc0944000   ( 336 kB)
[    0.000000]       .data : 0xc0944000 - 0xc09a0eb0   ( 372 kB)
[    0.000000]        .bss : 0xc09a2000 - 0xc09ed8d0   ( 303 kB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000] 	Build-time adjustment of leaf fanout to 32.
[    0.000000] 	RCU restricting CPUs from NR_CPUS=2 to nr_cpu_ids=1.
[    0.000000] RCU: Adjusting geometry for rcu_fanout_leaf=32, nr_cpu_ids=1
[    0.000000] NR_IRQS:16 nr_irqs:16 16
[    0.000000] ti_dt_clocks_register: failed to lookup clock node gmac_gmii_ref_clk_div
[    0.000000] OMAP clockevent source: timer1 at 32786 Hz
[    0.000000] Architected cp15 timer(s) running at 6.14MHz (virt).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x16af5adb9, max_idle_ns: 440795202250 ns
[    0.000004] sched_clock: 56 bits at 6MHz, resolution 162ns, wraps every 4398046511023ns
[    0.000015] Switching to timer-based delay loop, resolution 162ns
[    0.000334] clocksource: 32k_counter: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 58327039986419 ns
[    0.000343] OMAP clocksource: 32k_counter at 32768 Hz
[    0.000769] Console: colour dummy device 80x30
[    0.000786] WARNING: Your 'console=ttyO2' has been replaced by 'ttyS2'
[    0.000792] This ensures that you still see kernel messages. Please
[    0.000798] update your kernel commandline.
[    0.000810] Calibrating delay loop (skipped), value calculated using timer frequency.. 12.29 BogoMIPS (lpj=61475)
[    0.000824] pid_max: default: 32768 minimum: 301
[    0.000918] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.000928] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.001467] Initializing cgroup subsys io
[    0.001484] Initializing cgroup subsys memory
[    0.001509] Initializing cgroup subsys devices
[    0.001521] Initializing cgroup subsys freezer
[    0.001532] Initializing cgroup subsys perf_event
[    0.001544] Initializing cgroup subsys pids
[    0.001570] CPU: Testing write buffer coherency: ok
[    0.001776] /cpus/cpu@0 missing clock-frequency property
[    0.001788] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000
[    0.001823] Setting up static identity map for 0x800082c0 - 0x80008320
[    0.050028] Brought up 1 CPUs
[    0.050039] SMP: Total of 1 processors activated (12.29 BogoMIPS).
[    0.050046] CPU: All CPU(s) started in SVC mode.
[    0.050352] devtmpfs: initialized
[    0.080037] VFP support v0.3: implementor 41 architecture 4 part 30 variant f rev 0
[    0.081048] omap_hwmod: l3_main_2 using broken dt data from ocp
[    0.214255] omap_hwmod: gpu: _wait_target_ready failed: -16
[    0.214268] omap_hwmod: gpu: cannot be enabled for reset (3)
[    0.282228] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.293908] pinctrl core: initialized pinctrl subsystem
[    0.294823] NET: Registered protocol family 16
[    0.295747] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.320214] cpuidle: using governor ladder
[    0.350238] cpuidle: using governor menu
[    0.358690] OMAP GPIO hardware version 0.1
[    0.365223] irq: no irq domain found for /ocp/l4@4a000000/scm@2000/pinmux@1400 !
[    0.388287] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.388298] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.388781] omap4_sram_init:Unable to allocate sram needed to handle errata I688
[    0.388791] omap4_sram_init:Unable to get sram pool needed to handle errata I688
[    0.389380] OMAP DMA hardware revision 0.0
[    0.470908] omap-dma-engine 4a056000.dma-controller: OMAP DMA engine driver (LinkedList1/2/3 supported)
[    0.472085] edma 43300000.edma: memcpy is disabled
[    0.476846] edma 43300000.edma: TI EDMA DMA engine driver
[    0.480588] omap-iommu 40d01000.mmu: 40d01000.mmu registered
[    0.480779] omap-iommu 40d02000.mmu: 40d02000.mmu registered
[    0.480936] omap-iommu 58882000.mmu: 58882000.mmu registered
[    0.481098] omap-iommu 55082000.mmu: 55082000.mmu registered
[    0.484231] palmas 0-0058: Irq flag is 0x00000004
[    0.502306] palmas 0-0058: Muxing GPIO 2f, PWM 0, LED 0
[    0.584735] omap_i2c 48070000.i2c: bus 0 rev0.12 at 400 kHz
[    0.584959] media: Linux media interface: v0.10
[    0.585012] Linux video capture interface: v2.00
[    0.585055] pps_core: LinuxPPS API ver. 1 registered
[    0.585063] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.585089] PTP clock support registered
[    0.585135] EDAC MC: Ver: 3.0.0
[    0.591273] omap-mailbox 48840000.mailbox: omap mailbox rev 0x400
[    0.591469] omap-mailbox 48842000.mailbox: omap mailbox rev 0x400
[    0.591830] Advanced Linux Sound Architecture Driver Initialized.
[    0.592647] clocksource: Switched to clocksource arch_sys_counter
[    0.602736] NET: Registered protocol family 2
[    0.603240] TCP established hash table entries: 8192 (order: 3, 32768 bytes)
[    0.603303] TCP bind hash table entries: 8192 (order: 4, 65536 bytes)
[    0.603427] TCP: Hash tables configured (established 8192 bind 8192)
[    0.603480] UDP hash table entries: 512 (order: 2, 16384 bytes)
[    0.603512] UDP-Lite hash table entries: 512 (order: 2, 16384 bytes)
[    0.603725] NET: Registered protocol family 1
[    0.614025] RPC: Registered named UNIX socket transport module.
[    0.614034] RPC: Registered udp transport module.
[    0.614041] RPC: Registered tcp transport module.
[    0.614047] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.615040] hw perfevents: enabled with armv7_cortex_a15 PMU driver, 7 counters available
[    0.617408] futex hash table entries: 256 (order: 2, 16384 bytes)
[    0.635128] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.645803] NFS: Registering the id_resolver key type
[    0.645839] Key type id_resolver registered
[    0.645847] Key type id_legacy registered
[    0.645911] ntfs: driver 2.1.32 [Flags: R/O].
[    0.648167] bounce: pool size: 64 pages
[    0.648326] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 247)
[    0.648343] io scheduler noop registered
[    0.648357] io scheduler deadline registered
[    0.648393] io scheduler cfq registered (default)
[    0.650628] ldousb: supplied by VMAIN
[    1.940214] clock: dpll_pcie_ref_ck failed transition to 'locked'
[    1.941638] pinctrl-single 4a003400.pinmux: 282 pins at pa fc003400 size 1128
[    1.941758] pinctrl-single 4a002e8c.pinmux: 1 pins at pa fc002e8c size 4
[    2.010423] Serial: 8250/16550 driver, 10 ports, IRQ sharing disabled
[    2.013838] 48020000.serial: ttyS2 at MMIO 0x48020000 (irq = 299, base_baud = 3000000) is a 8250
[    2.848141] console [ttyS2] enabled
[    2.852840] [drm] Initialized drm 1.1.0 20060810
[    2.859023] ldoln: supplied by VMAIN
[    2.863232] OMAP DSS rev 6.1
[    2.867006] omapdss_dss 58000000.dss: bound 58001000.dispc (ops dispc_component_ops)
[    2.875531] omapdss_dss 58000000.dss: bound 58040000.encoder (ops hdmi5_component_ops)
[    2.971572] loop: module loaded
[    2.980290] m25p80 spi32766.0: s25fl256s1 (32768 Kbytes)
[    2.985733] 7 ofpart partitions found on MTD device spi32766.0
[    2.991591] Creating 7 MTD partitions on "spi32766.0":
[    2.996768] 0x000000000000-0x000000040000 : "QSPI.SPL"
[    3.012906] 0x000000040000-0x000000140000 : "QSPI.u-boot"
[    3.029236] 0x000000140000-0x0000001c0000 : "QSPI.u-boot-spl-os"
[    3.046209] 0x0000001c0000-0x0000001d0000 : "QSPI.u-boot-env"
[    3.062899] 0x0000001d0000-0x0000001e0000 : "QSPI.u-boot-env.backup1"
[    3.080257] 0x0000001e0000-0x0000009e0000 : "QSPI.kernel"
[    3.096588] 0x0000009e0000-0x000002000000 : "QSPI.file-system"
[    3.114376] libphy: Fixed MDIO Bus: probed
[    3.119070] CAN device driver interface
[    3.123117] ==mux spi1_clk = 0x50000
[    3.126707] ==mux spi1_d1 = 0x60000
[    3.130207] ==mux spi1_d0 = 0x20000
[    3.133727] ==mux spi1_cs0 = 0x20000
[    3.137316] ==mux gpio4_13 = 0x6000e
[    3.140902] ==mux spi2_clk = 0x50000
[    3.144502] ==mux spi2_d1 = 0x60000
[    3.148002] ==mux spi2_d0 = 0x20000
[    3.151501] ==mux spi2_cs0 = 0x20000
[    3.155101] ==mux gpio4_14 = 0x6000e
[    3.158687] ==mux spi3_clk = 0x50003
[    3.162273] ==mux spi3_d1 = 0x60003
[    3.165785] ==mux spi3_d0 = 0x20003
[    3.169284] ==mux spi3_cs0 = 0x20003
[    3.172881] ==mux gpio4_15 = 0x6000e
[    3.176469] ==mux spi4_clk = 0x50008
[    3.180054] ==mux spi4_d1 = 0x60008
[    3.183565] ==mux spi4_d0 = 0x20008
[    3.187064] ==mux spi4_cs0 = 0x20008
[    3.190650] ==mux gpio4_16 = 0x6000e
[    3.194438] smps9: supplied by VMAIN
[    3.198259] V3_3D: supplied by smps9
[    3.202165] *****[drivers/net/can/spi/mcp251x.c:1221]=====
[    3.217799] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_reset]:651 canstat=0x80====
[    3.225591] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:667 ====
[    3.232377] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:670 ctrl=0x87====
[    3.239904] *****[drivers/net/can/spi/mcp251x.c:1227]=====
[    3.245965] *****[drivers/net/can/spi/mcp251x.c:1234]=====
[    3.251474] *****[drivers/net/can/spi/mcp251x.c:1238]=====
[    3.257086] ==mux spi1_clk = 0x50000
[    3.260675] ==mux spi1_d1 = 0x60000
[    3.264190] ==mux spi1_d0 = 0x20000
[    3.267691] ==mux spi1_cs0 = 0x20000
[    3.271277] ==mux gpio4_13 = 0x6000e
[    3.274875] ==mux spi2_clk = 0x50000
[    3.278461] ==mux spi2_d1 = 0x60000
[    3.281961] ==mux spi2_d0 = 0x20000
[    3.285473] ==mux spi2_cs0 = 0x20000
[    3.289061] ==mux gpio4_14 = 0x6000e
[    3.292660] ==mux spi3_clk = 0x50003
[    3.296247] ==mux spi3_d1 = 0x60003
[    3.299746] ==mux spi3_d0 = 0x20003
[    3.303257] ==mux spi3_cs0 = 0x20003
[    3.306842] ==mux gpio4_15 = 0x6000e
[    3.310428] ==mux spi4_clk = 0x50008
[    3.314027] ==mux spi4_d1 = 0x60008
[    3.317526] ==mux spi4_d0 = 0x20008
[    3.321025] ==mux spi4_cs0 = 0x20008
[    3.324622] ==mux gpio4_16 = 0x6000e
[    3.328407] *****[drivers/net/can/spi/mcp251x.c:1221]=====
[    3.344038] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_reset]:651 canstat=0x80====
[    3.351813] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:667 ====
[    3.358609] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:670 ctrl=0x87====
[    3.366135] *****[drivers/net/can/spi/mcp251x.c:1227]=====
[    3.372141] *****[drivers/net/can/spi/mcp251x.c:1234]=====
[    3.377665] *****[drivers/net/can/spi/mcp251x.c:1238]=====
[    3.383260] ==mux spi1_clk = 0x50000
[    3.386849] ==mux spi1_d1 = 0x60000
[    3.390348] ==mux spi1_d0 = 0x20000
[    3.393863] ==mux spi1_cs0 = 0x20000
[    3.397449] ==mux gpio4_13 = 0x6000e
[    3.401035] ==mux spi2_clk = 0x50000
[    3.404633] ==mux spi2_d1 = 0x60000
[    3.408134] ==mux spi2_d0 = 0x20000
[    3.411632] ==mux spi2_cs0 = 0x20000
[    3.415230] ==mux gpio4_14 = 0x6000e
[    3.418817] ==mux spi3_clk = 0x50003
[    3.422404] ==mux spi3_d1 = 0x60003
[    3.425914] ==mux spi3_d0 = 0x20003
[    3.429414] ==mux spi3_cs0 = 0x20003
[    3.433012] ==mux gpio4_15 = 0x6000e
[    3.436599] ==mux spi4_clk = 0x50008
[    3.440185] ==mux spi4_d1 = 0x60008
[    3.443697] ==mux spi4_d0 = 0x20008
[    3.447196] ==mux spi4_cs0 = 0x20008
[    3.450782] ==mux gpio4_16 = 0x6000e
[    3.454560] *****[drivers/net/can/spi/mcp251x.c:1221]=====
[    3.470169] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_reset]:651 canstat=0x80====
[    3.477959] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:667 ====
[    3.484754] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:670 ctrl=0x87====
[    3.492267] *****[drivers/net/can/spi/mcp251x.c:1227]=====
[    3.498277] *****[drivers/net/can/spi/mcp251x.c:1234]=====
[    3.503804] *****[drivers/net/can/spi/mcp251x.c:1238]=====
[    3.509384] ==mux spi1_clk = 0x50000
[    3.512989] ==mux spi1_d1 = 0x60000
[    3.516489] ==mux spi1_d0 = 0x20000
[    3.519988] ==mux spi1_cs0 = 0x20000
[    3.523588] ==mux gpio4_13 = 0x6000e
[    3.527175] ==mux spi2_clk = 0x50000
[    3.530761] ==mux spi2_d1 = 0x60000
[    3.534273] ==mux spi2_d0 = 0x20000
[    3.537772] ==mux spi2_cs0 = 0x20000
[    3.541360] ==mux gpio4_14 = 0x6000e
[    3.544957] ==mux spi3_clk = 0x50003
[    3.548545] ==mux spi3_d1 = 0x60003
[    3.552044] ==mux spi3_d0 = 0x20003
[    3.555554] ==mux spi3_cs0 = 0x20003
[    3.559141] ==mux gpio4_15 = 0x6000e
[    3.562739] ==mux spi4_clk = 0x50008
[    3.566326] ==mux spi4_d1 = 0x60008
[    3.569826] ==mux spi4_d0 = 0x20008
[    3.573337] ==mux spi4_cs0 = 0x20008
[    3.576924] ==mux gpio4_16 = 0x6000e
[    3.580689] *****[drivers/net/can/spi/mcp251x.c:1221]=====
[    3.596317] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_reset]:651 canstat=0x80====
[    3.604107] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:667 ====
[    3.610891] ===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:670 ctrl=0x87====
[    3.618417] *****[drivers/net/can/spi/mcp251x.c:1227]=====
[    3.624427] *****[drivers/net/can/spi/mcp251x.c:1234]=====
[    3.629936] *****[drivers/net/can/spi/mcp251x.c:1238]=====
[    3.644603] omap_hwmod: dcan1: _wait_target_disable failed
[    3.650154] c_can_platform 4ae3c000.can: c_can_platform device registered (regs=fce3c000, irq=347)
[    3.659166] ===mapAddr can1_dx=0x20000
[    3.662940] ===mapAddr can1_rx=0x60000
[    3.666703] ===mapAddr can2_dx=0x20002
[    3.670463] ===mapAddr can2_rx=0x60002
[    3.674839] c_can_platform 48480000.can: c_can_platform device registered (regs=fa480000, irq=348)
[    3.683855] ===mapAddr can1_dx=0x20000
[    3.687617] ===mapAddr can1_rx=0x60000
[    3.691378] ===mapAddr can2_dx=0x20002
[    3.695153] ===mapAddr can2_rx=0x60002
[    3.742678] davinci_mdio 48485000.mdio: davinci mdio revision 1.6
[    3.748803] davinci_mdio 48485000.mdio: detected phy mask fffffffe
[    3.767270] libphy: 48485000.mdio: probed
[    3.771302] davinci_mdio 48485000.mdio: phy[0]: device 48485000.mdio:00, driver Micrel KSZ9031 Gigabit PHY
[    3.781613] cpsw 48484000.ethernet: No slave[1] phy_id, phy-handle, or fixed-link property
[    3.789991] cpsw 48484000.ethernet: Detected MACID = 50:33:8b:94:22:10
[    3.796696] cpsw 48484000.ethernet: cpts: overflow check period 800
[    3.804665] mousedev: PS/2 mouse device common for all mice
[    3.820777] i2c /dev entries driver
[    3.828663] omap_hsmmc 4809c000.mmc: Got CD GPIO
[    3.833834] ldo1: supplied by VMAIN
[    3.883194] omap_hsmmc 480b4000.mmc: no pinctrl state for sdr25 mode
[    3.889577] omap_hsmmc 480b4000.mmc: no pinctrl state for sdr12 mode
[    3.944253] ledtrig-cpu: registered to indicate activity on CPUs
[    3.964746] NET: Registered protocol family 10
[    3.992991] sit: IPv6 over IPv4 tunneling driver
[    3.998184] NET: Registered protocol family 17
[    4.012674] can: controller area network core (rev 20120528 abi 9)
[    4.018940] NET: Registered protocol family 29
[    4.032699] can: raw protocol (rev 20120528)
[    4.036991] can: broadcast manager protocol (rev 20120528 t)
[    4.052665] can: netlink gateway (rev 20130117) max_hops=1
[    4.058525] Key type dns_resolver registered
[    4.072794] omap_voltage_late_init: Voltage driver support not added
[    4.079753] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    4.102649] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[    4.112976] Adding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[    4.119185] Adding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[    4.143175] cpufreq: cpufreq_online: CPU0: Running at unlisted freq: 1000000 KHz
[    4.150618] cpu cpu0: dev_pm_opp_domain_set_rate: failed to find current OPP for freq 1000000000 (-34)
[    4.183142] cpufreq: cpufreq_online: CPU0: Unlisted initial frequency changed to: 500000 KHz
[    4.202681] Power Management for TI OMAP4+ devices.
[    4.207927] Registering SWP/SWPB emulation handler
[    4.227756] dmm 4e000000.dmm: initialized all PAT entries
[    4.236219] ldo3: supplied by VMAIN
[    4.249599] [drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
[    4.256360] [drm] No driver support for vblank timestamp query.
[    4.262359] omapdrm omapdrm.0: No connectors reported connected with modes
[    4.269386] [drm] Cannot find any crtc or sizes - going 1024x768
[    4.282408] mmc0: host does not support reading read-only switch, assuming write-enable
[    4.291496] [drm] Enabling DMM ywrap scrolling
[    4.298088] mmc0: new high speed SDHC card at address 59b4
[    4.309046] Console: switching to colour frame buffer device 128x48
[    4.326997] mmcblk0: mmc0:59b4 00000 7.35 GiB 
[    4.334235]  mmcblk0: p1 p2
[    4.343953] omapdrm omapdrm.0: fb0: omapdrm frame buffer device
[    4.374089] [drm] Initialized omapdrm 1.0.0 20110917 on minor 0
[    4.401573] hctosys: unable to open rtc device (rtc0)
[    4.407431] mmc1: MAN_BKOPS_EN bit is not set
[    4.430797] mmc1: new DDR MMC card at address 0001
[    4.441800] ALSA device list:
[    4.444839]   No soundcards found.
[    4.451551] mmcblk1: mmc1:0001 S10004 3.56 GiB 
[    4.466686] mmcblk1boot0: mmc1:0001 S10004 partition 1 4.00 MiB
[    4.483191] mmcblk1boot1: mmc1:0001 S10004 partition 2 4.00 MiB
[    4.490395]  mmcblk1: p1 p2
[    7.042528] EXT4-fs (mmcblk0p2): recovery complete
[    7.077355] EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Opts: (null)
[    7.085621] VFS: Mounted root (ext4 filesystem) on device 179:2.
[    7.100606] devtmpfs: mounted
[    7.104137] Freeing unused kernel memory: 336K (c08f0000 - c0944000)
[    7.110528] This architecture does not have kernel memory protection.
[    7.372469] systemd[1]: System time before build time, advancing clock.
[    7.426216] random: systemd: uninitialized urandom read (16 bytes read, 27 bits of entropy available)
[    7.442093] random: systemd: uninitialized urandom read (16 bytes read, 28 bits of entropy available)
[    7.456462] systemd[1]: systemd 229 running in system mode. (+PAM -AUDIT -SELINUX +IMA -APPARMOR +SMACK +SYSVINIT +UTMP -LIBCRYPTSETUP -GCRYPT -GNUTLS +ACL +XZ -LZ4 -SECCOMP +BLKID -ELFUTILS +KMOD -IDN)
[    7.475410] systemd[1]: Detected architecture arm.

Welcome to [1mArago 2016.12[0m!

[    7.504355] systemd[1]: Set hostname to <am57xx-evm>.
[    7.585746] random: systemd-sysv-ge: uninitialized urandom read (16 bytes read, 29 bits of entropy available)
[    7.609190] random: systemd-gpt-aut: uninitialized urandom read (16 bytes read, 30 bits of entropy available)
[    7.623690] random: systemd-gpt-aut: uninitialized urandom read (16 bytes read, 30 bits of entropy available)
[    7.642591] random: systemd-sysv-ge: uninitialized urandom read (16 bytes read, 30 bits of entropy available)
[    7.669110] random: systemd-sysv-ge: uninitialized urandom read (16 bytes read, 31 bits of entropy available)
[    7.775085] random: systemd: uninitialized urandom read (16 bytes read, 34 bits of entropy available)
[    7.785233] random: systemd: uninitialized urandom read (16 bytes read, 34 bits of entropy available)
[    7.796048] random: systemd: uninitialized urandom read (16 bytes read, 34 bits of entropy available)
[    8.498447] systemd[1]: sysinit.target: Found ordering cycle on sysinit.target/start
[    8.506368] systemd[1]: sysinit.target: Found dependency on alignment.service/start
[    8.514263] systemd[1]: sysinit.target: Found dependency on basic.target/start
[    8.521543] systemd[1]: sysinit.target: Found dependency on sockets.target/start
[    8.529071] systemd[1]: sysinit.target: Found dependency on dropbear.socket/stop
[    8.536552] systemd[1]: sysinit.target: Found dependency on sysinit.target/start
[    8.544032] systemd[1]: sysinit.target: Breaking ordering cycle by deleting job alignment.service/start
[    8.553518] systemd[1]: alignment.service: Job alignment.service/start deleted to break ordering cycle starting with sysinit.target/start
[[0;1;31m SKIP [0m] Ordering cycle found, skipping alignment.service
[    8.598698] systemd[1]: Listening on udev Control Socket.
[[0;32m  OK  [0m] Listening on udev Control Socket.
[    8.623473] systemd[1]: Listening on Journal Socket (/dev/log).
[[0;32m  OK  [0m] Listening on Journal Socket (/dev/log).
[    8.653372] systemd[1]: Listening on Journal Socket.
[[0;32m  OK  [0m] Listening on Journal Socket.
[    8.683550] systemd[1]: Reached target Remote File Systems.
[[0;32m  OK  [0m] Reached target Remote File Systems.
[    8.713106] systemd[1]: Reached target Swap.
[[0;32m  OK  [0m] Reached target Swap.
[    8.733576] systemd[1]: Listening on Network Service Netlink Socket.
[[0;32m  OK  [0m] Listening on Network Service Netlink Socket.
[    8.763245] systemd[1]: Listening on Syslog Socket.
[[0;32m  OK  [0m] Listening on Syslog Socket.
[    8.793222] systemd[1]: Listening on udev Kernel Socket.
[[0;32m  OK  [0m] Listening on udev Kernel Socket.
[    8.827365] systemd[1]: Created slice User and Session Slice.
[[0;32m  OK  [0m] Created slice User and Session Slice.
[    8.853548] systemd[1]: Started Dispatch Password Requests to Console Directory Watch.
[[0;32m  OK  [0m] Started Dispatch Password Requests to Console Directory Watch.
[    8.900332] systemd[1]: Started Forward Password Requests to Wall Directory Watch.
[[0;32m  OK  [0m] Started Forward Password Requests to Wall Directory Watch.
[    8.933142] systemd[1]: Reached target Paths.
[[0;32m  OK  [0m] Reached target Paths.
[    8.953318] systemd[1]: Listening on /dev/initctl Compatibility Named Pipe.
[[0;32m  OK  [0m] Listening on /dev/initctl Compatibility Named Pipe.
[    8.984523] systemd[1]: Created slice System Slice.
[[0;32m  OK  [0m] Created slice System Slice.
[    9.014635] systemd[1]: Created slice system-getty.slice.
[[0;32m  OK  [0m] Created slice system-getty.slice.
[    9.047563] systemd[1]: Mounting POSIX Message Queue File System...
         Mounting POSIX Message Queue File System...
[    9.088300] systemd[1]: Mounting Temporary Directory...
         Mounting Temporary Directory...
[    9.137632] systemd[1]: Starting Setup Virtual Console...
         Starting Setup Virtual Console...
[    9.177903] systemd[1]: Starting Journal Service...
         Starting Journal Service...
[    9.213329] systemd[1]: Reached target Slices.
[[0;32m  OK  [0m] Reached target Slices.
[    9.248097] systemd[1]: Starting Create list of required static device nodes for the current kernel...
         Starting Create list of required st... nodes for the current kernel...
[    9.343462] systemd[1]: Starting Load Kernel Modules...
         Starting Load Kernel Modules...
[    9.384923] systemd[1]: Created slice system-serial\x2dgetty.slice.
[    9.399063] CMEMK module: reference Linux version 4.4.41
[[0;32m  OK  [0m] Created slice system-serial\x2dgetty.slice.
[    9.412086] cmemk initialized
[    9.427919] systemd[1]: Mounting Debug File System...
         Mounting Debug File System...
[    9.463417] cryptodev: driver 1.8 loaded.
[    9.491552] systemd[1]: Starting Remount Root and Kernel File Systems...
         Starting Remount Root and Kernel File Systems...
[    9.577617] EXT4-fs (mmcblk0p2): re-mounted. Opts: (null)
[    9.643120] systemd[1]: Mounted Debug File System.
[[0;32m  OK  [0m] Mounted Debug File System.
[    9.673361] systemd[1]: Mounted POSIX Message Queue File System.
[[0;32m  OK  [0m] Mounted POSIX Message Queue File System.
[    9.703260] systemd[1]: Mounted Temporary Directory.
[[0;32m  OK  [0m] Mounted Temporary Directory.
[    9.737038] systemd[1]: Started Journal Service.
[[0;32m  OK  [0m] Started Journal Service.
[[0;32m  OK  [0m] Started Setup Virtual Console.
[[0;32m  OK  [0m] Started Create list of required sta...ce nodes for the current kernel.
[[0;32m  OK  [0m] Started Load Kernel Modules.
[[0;32m  OK  [0m] Started Remount Root and Kernel File Systems.
         Starting udev Coldplug all Devices...
         Starting Apply Kernel Variables...
         Starting Create Static Device Nodes in /dev...
         Starting Flush Journal to Persistent Storage...
[[0;32m  OK  [0m] Started Apply Kernel Variables.
[[0;32m  OK  [0m] Started Create Static Device Nodes in /dev.
[   11.283275] systemd-journald[123]: Received request to flush runtime journal from PID 1
[[0;32m  OK  [0m] Started Flush Journal to Persistent Storage.
         Starting udev Kernel Device Manager...
[[0;32m  OK  [0m] Reached target Local File Systems (Pre).
         Mounting /media/ram...
         Mounting /var/volatile...
[[0;32m  OK  [0m] Mounted /var/volatile.
[[0;32m  OK  [0m] Mounted /media/ram.
[[0;32m  OK  [0m] Started udev Kernel Device Manager.
[[0;32m  OK  [0m] Reached target Local File Systems.
         Starting Create Volatile Files and Directories...
         Starting Load/Save Random Seed...
[[0;32m  OK  [0m] Started Load/Save Random Seed.
[[0;32m  OK  [0m] Started Create Volatile Files and Directories.
         Starting Network Time Synchronization...
         Starting Update UTMP about System Boot/Shutdown...
[   13.761069] omap-rproc 58820000.ipu: assigned reserved memory node ipu1_cma@9d000000
[   13.856737]  remoteproc0: 58820000.ipu is available
[   13.902149]  remoteproc0: Note: remoteproc is still under development and considered experimental.
[[0;32m  OK  [0m] Started Network Time Synchronization.
[   13.990974]  remoteproc0: THE BINARY FORMAT IS NOT YET FINALIZED, and backward compatibility isn't yet guaranteed.
[   14.157249] omap-rproc 55020000.ipu: assigned reserved memory node ipu2_cma@95800000
[   14.269577]  remoteproc1: 55020000.ipu is available
[   14.339336]  remoteproc1: Note: remoteproc is still under development and considered experimental.
[   14.418742]  remoteproc0: registered virtio0 (type 7)
[   14.507895]  remoteproc1: THE BINARY FORMAT IS NOT YET FINALIZED, and backward compatibility isn't yet guaranteed.
[   14.645131] omap-rproc 40800000.dsp: assigned reserved memory node dsp1_cma@99000000
[   14.701731]  remoteproc2: 40800000.dsp is available
[   14.785726]  remoteproc2: Note: remoteproc is still under development and considered experimental.
[[0;32m  OK  [0m] Started udev Coldplug all Devices.
[   14.843640]  remoteproc1: registered virtio1 (type 7)
[   14.888001]  remoteproc2: THE BINARY FORMAT IS NOT YET FINALIZED, and backward compatibility isn't yet guaranteed.
[[0;32m  OK  [0m] Found device /dev/ttyS2.
[   14.950672] ov2659 0-0030: Sensor detection failed (3030, 0)
[   14.961495] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[   14.990099] omap_rng 48090000.rng: OMAP Random Number Generator ver. 20
[   15.019798] omap-des 480a5000.des: OMAP DES hw accel rev: 2.2
[   15.029782] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[   15.083354] alg: skcipher: setkey failed on test 5 for ecb-des-omap: flags=100
[   15.131641] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[   15.208044] alg: skcipher-ddst: setkey failed on test 5 for ecb-des-omap: flags=100
[   15.286715] alg: skcipher-ddst: setkey failed on test 5 for ecb-des-omap: flags=100
[   15.300566] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[   15.313324] palmas-rtc 48070000.i2c:tps659038@58:tps659038_rtc: rtc core: registered 48070000.i2c:tps659 as rtc0
[   15.476372] palmas-usb 48070000.i2c:tps659038@58:tps659038_usb: USB-HOST cable is attached
[   15.630114] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[[0;32m  OK  [0m] Started Update UTMP about System Boot/Shutdown.
[   15.759543] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[   15.832042] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[   15.960601] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[   16.070430] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[   16.174478] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[   16.306352]  remoteproc2: registered virtio2 (type 7)
[   16.361494] omap_rtc 48838000.rtc: rtc core: registered 48838000.rtc as rtc1
[   16.583240] vpe 489d0000.vpe: loading firmware vpdma-1b8.bin
         Starting Synchronize System and HW clocks...
[   16.663243] vpe 489d0000.vpe: Device registered as /dev/video0
[[0;32m  OK  [0m] Reached target System Time Synchronized.
[[0;32m  OK  [0m] Started Synchronize System and HW clocks.
[   16.962765] vip 48970000.vip: loading firmware vpdma-1b8.bin
[   16.982812] vip 48970000.vip: VPDMA firmware loaded
[[0;32m  OK  [0m] Reached target System Initialization.
[[0;32m  OK  [0m] Listening on Avahi mDNS/DNS-SD Stack Activation Socket.
[[0;32m  OK  [0m] Listening on RPCbind Server Activation Socket.
[[0;32m  OK  [0m] Started Daily Cleanup of Temporary Directories.
[[0;32m  OK  [0m] Reached target Timers.
[[0;32m  OK  [0m] Listening on D-Bus System Message Bus Socket.
[   18.198008] SCSI subsystem initialized
[[0;32m  OK  [0m] Listening on dropbear.socket.
[[0;32m  OK  [0m] Reached target Sockets.
[[0;32m  OK  [0m] Reached target Basic System.
[   18.367804] FAT-fs (mmcblk0p1): Volume was not properly unmounted. Some data may be corrupt. Please run fsck.
         Starting Print notice about GPLv3 packages...
         Starting Permit User Sessions...
[   18.537677] omap_wdt: OMAP Watchdog Timer Rev 0x01: initial timeout 60 sec
         Starting Telephony service...
         Starting Login Service...
[   18.647747] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[[0;32m  OK  [0m] Started Kernel Logging Service.
[   18.819740] ti-pipe3 4a096000.phy: DPLL failed to lock
[   18.845173] EXT4-fs (mmcblk1p2): recovery complete
[   18.850027] EXT4-fs (mmcblk1p2): mounted filesystem with ordered data mode. Opts: (null)
[   18.859293] FAT-fs (mmcblk1p1): Volume was not properly unmounted. Some data may be corrupt. Please run fsck.
[[0;32m  OK  [0m] Started strongSwan IPsec IKEv1/IKEv2 daemon using ipsec.conf.
[[0;32m  OK  [0m] Started D-Bus System Message Bus.
[   18.964983] phy phy-4a096000.phy.2: phy init failed --> -22
[   19.000877] can_dev: exports duplicate symbol alloc_can_err_skb (owned by kernel)
[   19.022924] ahci: probe of 4a140000.sata failed with error -22
[   19.142039] omap-sham 4b101000.sham: hw accel on OMAP rev 4.3
[   19.205741] r->name:nonblocking
[   19.208920] random: nonblocking pool is initialized
[[0;32m  OK  [0m] Started Telephony service.
         Starting Network Service...
[   20.260328] NET: Registered protocol family 15
         Starting uim-sysfs.service...
[   20.358919] Bluetooth: Core ver 2.21
[   20.362619] NET: Registered protocol family 31
[[0;32m  OK  [0m] Started System Logging Service.
[   20.615086] Bluetooth: HCI device and connection manager initialized
         Starting TI MultiCore Tools Daemon...
[   20.741382] Bluetooth: HCI socket layer initialized
[   20.761739] omap-aes 4b500000.aes: OMAP AES hw accel rev: 3.3
[   20.806186] Bluetooth: L2CAP socket layer initialized
[   20.811350] Bluetooth: SCO socket layer initialized
         Starting Avahi mDNS/DNS-SD Stack...
[   20.954570] omap_hwmod: dcan1: _wait_target_disable failed
[   21.327308] omap-hdmi-audio omap-hdmi-audio.0.auto: snd-soc-dummy-dai <-> 58040000.encoder mapping ok
[   21.347718] omap_hwmod: dcan1: _wait_target_disable failed
[   21.662580] omap_hwmod: dcan1: _wait_target_disable failed
[[0;32m  OK  [0m] Started Permit User Sessions.
[[0;32m  OK  [0m] Started TI MultiCore Tools Daemon.
[   21.761156] omap_hwmod: gpu: _wait_target_ready failed: -16
[   21.838821] PVR_K:(Error): EnableSGXClocks: pm_runtime_get_sync failed (16)
[   21.882341] Initializing XFRM netlink socket
[[0;32m  OK  [0m] Started Network Service.
[   21.951365] PVR_K:(Error): SysInitialise: Failed to Enable system clocks (175)
[   22.010923] net eth0: initializing cpsw version 1.15 (0)
[   22.052500] net eth0: initialized cpsw ale version 1.4
[   22.095657] omap-aes 4b700000.aes: OMAP AES hw accel rev: 3.3
[   22.153449] net eth0: ALE Table size 1024
[   22.435895] net eth0: phy found : id is : 0x221622
[   22.440948] libphy: PHY  not found
[   22.541217] net eth0: phy "" not found on slave 1, err -19
[   22.776714] IPv6: ADDRCONF(NETDEV_UP): eth0: link is not ready
[   24.937720] omap_hwmod: dcan1: _wait_target_disable failed
[   27.040636]  remoteproc0: powering up 58820000.ipu
[   27.311300]  remoteproc0: Booting fw image dra7-ipu1-fw.xem4, size 4890352
[   27.413007] omap-iommu 58882000.mmu: 58882000.mmu: version 2.1
[   27.576726]  remoteproc0: remote processor 58820000.ipu is now up
[   27.683903] virtio_rpmsg_bus virtio0: rpmsg host is online
[   27.689535] virtio_rpmsg_bus virtio0: creating channel rpmsg-client-sample addr 0x32
[   27.743904] virtio_rpmsg_bus virtio0: creating channel rpmsg-client-sample addr 0x33
[   27.825215] virtio_rpmsg_bus virtio0: creating channel rpmsg-omx addr 0x3c
[   27.903507] virtio_rpmsg_bus virtio0: creating channel rpmsg-rpc addr 0x65
[   27.993647]  remoteproc1: powering up 55020000.ipu
[   28.070343]  remoteproc1: Booting fw image dra7-ipu2-fw.xem4, size 3743116
[   28.158679] omap-iommu 55082000.mmu: 55082000.mmu: version 2.1
[   28.563734] ti-pipe3 4a084400.phy: DPLL failed to lock
[   28.610895] phy phy-4a084400.phy.4: phy init failed --> -22
[   28.669907] dwc3 48890000.usb: failed to initialize core
[   28.710250] dwc3: probe of 48890000.usb failed with error -22
[   29.187615]  remoteproc1: remote processor 55020000.ipu is now up
[   29.284918] virtio_rpmsg_bus virtio1: rpmsg host is online
[   29.290509] virtio_rpmsg_bus virtio1: creating channel rpmsg-rpc addr 0x65
[   29.333502] virtio_rpmsg_bus virtio1: creating channel rpmsg-rpc addr 0x66
[   29.354660]  remoteproc2: powering up 40800000.dsp
[   29.756768]  remoteproc2: Booting fw image dra7-dsp1-fw.xe66, size 21914156
[   29.847079] omap_hwmod: mmu0_dsp1: _wait_target_disable failed
[   29.853013] omap-iommu 40d01000.mmu: 40d01000.mmu: version 3.0
[   29.859022] omap-iommu 40d02000.mmu: 40d02000.mmu: version 3.0
[   30.211667]  remoteproc2: remote processor 40800000.dsp is now up
[   30.402343] virtio_rpmsg_bus virtio2: rpmsg host is online
[   30.408168] virtio_rpmsg_bus virtio2: creating channel rpmsg-proto addr 0x3d
[   30.519174] usbcore: registered new interface driver usbfs
[   30.584799] usbcore: registered new interface driver hub
[   30.641468] rpmsg_rpc rpmsg3: probing service rpc_example_2 with src 1024 dst 101
[   30.651979] NET: Registered protocol family 41
[   30.701311] usbcore: registered new device driver usb
[   30.735932] rpmsg_rpc rpmsg4: probing service dce-callback with src 1024 dst 101
[   30.743517] rpmsg_rpc rpmsg3: published functions = 8
[   30.805759] dwc3 488d0000.usb: otg: primary host xhci-hcd.1.auto registered
[   30.831767] rpmsg_rpc rpmsg5: probing service rpmsg-dce with src 1025 dst 102
[   30.839064] rpmsg_rpc rpmsg4: published functions = 4
[   30.887831] dwc3 488d0000.usb: otg: shared host xhci-hcd.1.auto registered
[   30.907311] rpmsg_rpc rpmsg5: published functions = 9
[   30.966226] dwc3 488d0000.usb: otg: can't start till gadget registers
***************************************************************
***************************************************************
NOTICE: This file system contains the following GPLv3 packages:
	autoconf
	binutils-dev
	binutils
	bison-dev
	bison
	cpp-symlinks
	cpp
	dosfstools
	g++-symlinks
	g++
	gawk-dev
	gawk
	gcc-symlinks
	gcc
	gdb
	gdbc6x
	gdbserver
	gstreamer1.0-libav
	hidapi
	libcairo-perf-utils
	libgmp10
	libidn11
	libmpc3
	libmpfr4
	m4-dev
	m4
	make
	nettle
	parted
	swig-dev
	swig

If you do not wish to distribute GPLv3 components please remove
the above packages prior to distribution.  This can be done using
the opkg remove command.  i.e.:
    opkg remove <package>
Where <package> is the name printed in the list above

NOTE: If the package is a dependency of another package you
      will be notified of the dependent packages.  You should
      use the --force-removal-of-dependent-packages option to
      also remove the dependent packages as well
***************************************************************
***************************************************************
[[0;32m  OK  [0m] Started Print notice about GPLv3 packages.
[[0;32m  OK  [0m] Started Avahi mDNS/DNS-SD Stack.
[[0;32m  OK  [0m] Started Login Service.
[[0;32m  OK  [0m] Reached target Sound Card.
[[0;32m  OK  [0m] Listening on Load/Save RF Kill Switch Status /dev/rfkill Watch.
[[0;32m  OK  [0m] Reached target Network.
         Starting Lightning Fast Webserver With Light System Requirements...
         Starting Network Name Resolution...
[[0;32m  OK  [0m] Started Serial Getty on ttyS2.
[[0;32m  OK  [0m] Started Getty on tty1.
[   33.888390] omap_hwmod: dcan1: _wait_target_disable failed
[[0;32m  OK  [0m] Started Lightning Fast Webserver With Light System Requirements.
[[0;32m  OK  [0m] Started Network Name Resolution.
[[0;32m  OK  [0m] Started uim-sysfs.service.
         Starting rc.pvr.service...
[[0;32m  OK  [0m] Started rc.pvr.service.
         Starting weston.service...
[[0;32m  OK  [0m] Started weston.service.
         Starting telnetd.service...
         Starting tiipclad-daemon.service...
[[0;32m  OK  [0m] Started telnetd.service.
[[0;32m  OK  [0m] Started tiipclad-daemon.service.
         Starting thttpd.service...
[[0;32m  OK  [0m] Started thttpd.service.
         Starting rng-tools.service...
[[0;32m  OK  [0m] Started rng-tools.service.
         Starting gdbserverproxy.service...


 _____                    _____           _         _   
|  _  |___ ___ ___ ___   |  _  |___ ___  |_|___ ___| |_ 
|     |  _| .'| . | . |  |   __|  _| . | | | -_|  _|  _|
|__|__|_| |__,|_  |___|  |__|  |_| |___|_| |___|___|_|  
              |___|                    |___|            

Arago Project http://arago-project.org am57xx-evm ttyS2

Arago 2016.12 am57xx-evm ttyS2

am57xx-evm login: [   41.051569] omap_hwmod: mmu1_dsp1: _wait_target_disable failed
[   41.067896] omap_hwmod: mmu0_dsp1: _wait_target_disable failed
root

7[r[999;999H[6n8root@am57xx-evm:~# dmesg
[32m[    0.000000] [0mBooting Linux on physical CPU 0x0
[32m[    0.000000] [0mInitializing cgroup subsys cpuset
[32m[    0.000000] [0mInitializing cgroup subsys cpu
[32m[    0.000000] [0mInitializing cgroup subsys cpuacct
[32m[    0.000000] [0mLinux version 4.4.41 (root@ubuntu) (gcc version 5.3.1 20160113 (Linaro GCC 5.3-2016.02) ) #154 SMP PREEMPT Tue Jan 23 04:33:36 PST 2018
[32m[    0.000000] [0m[33mCPU[0m: ARMv7 Processor [412fc0f2] revision 2 (ARMv7), cr=30c5387d
[32m[    0.000000] [0m[33mCPU[0m: PIPT / VIPT nonaliasing data cache, PIPT instruction cache
[32m[    0.000000] [0m[33mMachine model[0m: TI AM5718 IDK
[32m[    0.000000] [0m[33mReserved memory[0m: created CMA memory pool at 0x0000000095800000, size 56 MiB
[32m[    0.000000] [0m[33mReserved memory[0m: initialized node ipu2_cma@95800000, compatible id shared-dma-pool
[32m[    0.000000] [0m[33mReserved memory[0m: created CMA memory pool at 0x0000000099000000, size 64 MiB
[32m[    0.000000] [0m[33mReserved memory[0m: initialized node dsp1_cma@99000000, compatible id shared-dma-pool
[32m[    0.000000] [0m[33mReserved memory[0m: created CMA memory pool at 0x000000009d000000, size 32 MiB
[32m[    0.000000] [0m[33mReserved memory[0m: initialized node ipu1_cma@9d000000, compatible id shared-dma-pool
[32m[    0.000000] [0m[33mcma[0m: Reserved 24 MiB at 0x00000000be400000
[32m[    0.000000] [0m[1mForcing write-allocate cache policy for SMP[0m
[32m[    0.000000] [0m[33mMemory policy[0m: Data cache writealloc
[32m[    0.000000] [0m[33mOMAP4[0m: Map 0x00000000bfd00000 to fe600000 for dram barrier
[32m[    0.000000] [0m[33mOn node 0 totalpages[0m: 212224
[32m[    0.000000] [0m[33mfree_area_init_node[0m: node 0, pgdat c099e3c0, node_mem_map ef6a6000
[32m[    0.000000] [0m[33m  DMA zone[0m: 1728 pages used for memmap
[32m[    0.000000] [0m[33m  DMA zone[0m: 0 pages reserved
[32m[    0.000000] [0m[33m  DMA zone[0m: 147456 pages, LIFO batch:31
[32m[    0.000000] [0m[33m  HighMem zone[0m: 64768 pages, LIFO batch:15
[32m[    0.000000] [0mDRA722 ES2.0
[32m[    0.000000] [0m[33mPERCPU[0m: Embedded 11 pages/cpu @ef646000 s14848 r8192 d22016 u45056
[32m[    0.000000] [0m[33mpcpu-alloc[0m: s14848 r8192 d22016 u45056 alloc=11*4096
[32m[    0.000000] [0m[33mpcpu-alloc[0m: [0] 0 
[32m[    0.000000] [0m[33mBuilt 1 zonelists in Zone order, mobility grouping on.  Total pages[0m: 210496
[32m[    0.000000] [0m[33mKernel command line[0m: console=ttyO2,115200n8 root=PARTUUID=00000780-02 rw rootfstype=ext4 rootwait
[32m[    0.000000] [0m[33mPID hash table entries[0m: 4096 (order: 2, 16384 bytes)
[32m[    0.000000] [0m[33mDentry cache hash table entries[0m: 131072 (order: 7, 524288 bytes)
[32m[    0.000000] [0m[33mInode-cache hash table entries[0m: 65536 (order: 6, 262144 bytes)
[32m[    0.000000] [0m[33mMemory[0m: 649404K/848896K available (6659K kernel code, 371K rwdata, 2456K rodata, 336K init, 302K bss, 19268K reserved, 180224K cma-reserved, 234496K highmem)
[32m[    0.000000] [0m[33mVirtual kernel memory layout:
                   vector  [0m: 0xffff0000 - 0xffff1000   (   4 kB)
                   fixmap  : 0xffc00000 - 0xfff00000   (3072 kB)
                   vmalloc : 0xf0800000 - 0xff800000   ( 240 MB)
                   lowmem  : 0xc0000000 - 0xf0000000   ( 768 MB)
                   pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
                   modules : 0xbf000000 - 0xbfe00000   (  14 MB)
                     .text : 0xc0008000 - 0xc08ef094   (9117 kB)
                     .init : 0xc08f0000 - 0xc0944000   ( 336 kB)
                     .data : 0xc0944000 - 0xc09a0eb0   ( 372 kB)
                      .bss : 0xc09a2000 - 0xc09ed8d0   ( 303 kB)
[32m[    0.000000] [0m[33mSLUB[0m: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[32m[    0.000000] [0mPreemptible hierarchical RCU implementation.
[32m[    0.000000] [0m	Build-time adjustment of leaf fanout to 32.
[32m[    0.000000] [0m	RCU restricting CPUs from NR_CPUS=2 to nr_cpu_ids=1.
[32m[    0.000000] [0m[33mRCU[0m: Adjusting geometry for rcu_fanout_leaf=32, nr_cpu_ids=1
[32m[    0.000000] [0mNR_IRQS:16 nr_irqs:16 16
[32m[    0.000000] [0m[33mti_dt_clocks_register[0m[1m: failed to lookup clock node gmac_gmii_ref_clk_div[0m
[32m[    0.000000] [0m[33mOMAP clockevent source[0m: timer1 at 32786 Hz
[32m[    0.000000] [0mArchitected cp15 timer(s) running at 6.14MHz (virt).
[32m[    0.000000] [0m[33mclocksource[0m: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x16af5adb9, max_idle_ns: 440795202250 ns
[32m[    0.000004] [0m[33msched_clock[0m: 56 bits at 6MHz, resolution 162ns, wraps every 4398046511023ns
[32m[    0.000015] [0mSwitching to timer-based delay loop, resolution 162ns
[32m[    0.000334] [0m[33mclocksource[0m: 32k_counter: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 58327039986419 ns
[32m[    0.000343] [0m[33mOMAP clocksource[0m: 32k_counter at 32768 Hz
[32m[    0.000769] [0m[33mConsole[0m: colour dummy device 80x30
[32m[    0.000786] [0m[33mWARNING[0m[31m: Your 'console=ttyO2' has been replaced by 'ttyS2'[0m
[32m[    0.000792] [0m[31mThis ensures that you still see kernel messages. Please[0m
[32m[    0.000798] [0m[31mupdate your kernel commandline.[0m
[32m[    0.000810] [0mCalibrating delay loop (skipped), value calculated using timer frequency.. 12.29 BogoMIPS (lpj=61475)
[32m[    0.000824] [0m[33mpid_max[0m: default: 32768 minimum: 301
[32m[    0.000918] [0m[33mMount-cache hash table entries[0m: 2048 (order: 1, 8192 bytes)
[32m[    0.000928] [0m[33mMountpoint-cache hash table entries[0m: 2048 (order: 1, 8192 bytes)
[32m[    0.001467] [0mInitializing cgroup subsys io
[32m[    0.001484] [0mInitializing cgroup subsys memory
[32m[    0.001509] [0mInitializing cgroup subsys devices
[32m[    0.001521] [0mInitializing cgroup subsys freezer
[32m[    0.001532] [0mInitializing cgroup subsys perf_event
[32m[    0.001544] [0mInitializing cgroup subsys pids
[32m[    0.001570] [0m[33mCPU[0m: Testing write buffer coherency: ok
[32m[    0.001776] [0m[31m/cpus/cpu@0 missing clock-frequency property[0m
[32m[    0.001788] [0m[33mCPU0[0m: thread -1, cpu 0, socket 0, mpidr 80000000
[32m[    0.001823] [0mSetting up static identity map for 0x800082c0 - 0x80008320
[32m[    0.050028] [0mBrought up 1 CPUs
[32m[    0.050039] [0m[33mSMP[0m: Total of 1 processors activated (12.29 BogoMIPS).
[32m[    0.050046] [0m[33mCPU[0m: All CPU(s) started in SVC mode.
[32m[    0.050352] [0m[33mdevtmpfs[0m: initialized
[32m[    0.080037] [0m[33mVFP support v0.3[0m: implementor 41 architecture 4 part 30 variant f rev 0
[32m[    0.081048] [0m[33momap_hwmod[0m[1m: l3_main_2 using broken dt data from ocp[0m
[32m[    0.214255] [0m[33momap_hwmod[0m[31m: gpu: _wait_target_ready failed: -16[0m
[32m[    0.214268] [0m[33momap_hwmod[0m[1m: gpu: cannot be enabled for reset (3)[0m
[32m[    0.282228] [0m[33mclocksource[0m: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[32m[    0.293908] [0m[33mpinctrl core[0m: initialized pinctrl subsystem
[32m[    0.294823] [0m[33mNET[0m: Registered protocol family 16
[32m[    0.295747] [0m[33mDMA[0m: preallocated 256 KiB pool for atomic coherent allocations
[32m[    0.320214] [0m[33mcpuidle[0m: using governor ladder
[32m[    0.350238] [0m[33mcpuidle[0m: using governor menu
[32m[    0.358141] [0m[33mgpiochip_add[0m: registered GPIOs 0 to 31 on device: gpio
[32m[    0.358690] [0mOMAP GPIO hardware version 0.1
[32m[    0.359356] [0m[33mgpiochip_add[0m: registered GPIOs 32 to 63 on device: gpio
[32m[    0.360268] [0m[33mgpiochip_add[0m: registered GPIOs 64 to 95 on device: gpio
[32m[    0.361140] [0m[33mgpiochip_add[0m: registered GPIOs 96 to 127 on device: gpio
[32m[    0.362005] [0m[33mgpiochip_add[0m: registered GPIOs 128 to 159 on device: gpio
[32m[    0.362872] [0m[33mgpiochip_add[0m: registered GPIOs 160 to 191 on device: gpio
[32m[    0.363736] [0m[33mgpiochip_add[0m: registered GPIOs 192 to 223 on device: gpio
[32m[    0.364595] [0m[33mgpiochip_add[0m: registered GPIOs 224 to 255 on device: gpio
[32m[    0.365223] [0m[33mirq[0m[1m: no irq domain found for /ocp/l4@4a000000/scm@2000/pinmux@1400 ![0m
[32m[    0.388287] [0m[33mhw-breakpoint[0m: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[32m[    0.388298] [0m[33mhw-breakpoint[0m: maximum watchpoint size is 8 bytes.
[32m[    0.388781] [0m[1momap4_sram_init:Unable to allocate sram needed to handle errata I688[0m
[32m[    0.388791] [0m[1momap4_sram_init:Unable to get sram pool needed to handle errata I688[0m
[32m[    0.389380] [0mOMAP DMA hardware revision 0.0
[32m[    0.470908] [0m[33momap-dma-engine 4a056000.dma-controller[0m: OMAP DMA engine driver (LinkedList1/2/3 supported)
[32m[    0.472085] [0m[33medma 43300000.edma[0m: memcpy is disabled
[32m[    0.476846] [0m[33medma 43300000.edma[0m: TI EDMA DMA engine driver
[32m[    0.477243] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'gpio' property of node '/fixedregulator-vmain[0]'
[32m[    0.477477] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'gpio' property of node '/fixedregulator-v3_3d[0]'
[32m[    0.477696] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'gpio' property of node '/fixedregulator-vtt[0]'
[32m[    0.480588] [0m[33momap-iommu 40d01000.mmu[0m: 40d01000.mmu registered
[32m[    0.480779] [0m[33momap-iommu 40d02000.mmu[0m: 40d02000.mmu registered
[32m[    0.480936] [0m[33momap-iommu 58882000.mmu[0m: 58882000.mmu registered
[32m[    0.481098] [0m[33momap-iommu 55082000.mmu[0m: 55082000.mmu registered
[32m[    0.484231] [0m[33mpalmas 0-0058[0m: Irq flag is 0x00000004
[32m[    0.502306] [0m[33mpalmas 0-0058[0m: Muxing GPIO 2f, PWM 0, LED 0
[32m[    0.584207] [0m[33mgpiochip_find_base[0m: found new base at 504
[32m[    0.584314] [0m[33mgpiochip_add[0m: registered GPIOs 504 to 511 on device: 48070000.i2c:tps659038@58:tps659038_gpio
[32m[    0.584735] [0m[33momap_i2c 48070000.i2c[0m: bus 0 rev0.12 at 400 kHz
[32m[    0.584959] [0m[33mmedia[0m: Linux media interface: v0.10
[32m[    0.585012] [0m[33mLinux video capture interface[0m: v2.00
[32m[    0.585055] [0m[33mpps_core[0m: LinuxPPS API ver. 1 registered
[32m[    0.585063] [0m[33mpps_core[0m: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[32m[    0.585089] [0mPTP clock support registered
[32m[    0.585135] [0m[33mEDAC MC[0m: Ver: 3.0.0
[32m[    0.591273] [0m[33momap-mailbox 48840000.mailbox[0m: omap mailbox rev 0x400
[32m[    0.591469] [0m[33momap-mailbox 48842000.mailbox[0m: omap mailbox rev 0x400
[32m[    0.591830] [0mAdvanced Linux Sound Architecture Driver Initialized.
[32m[    0.592647] [0m[33mclocksource[0m: Switched to clocksource arch_sys_counter
[32m[    0.602736] [0m[33mNET[0m: Registered protocol family 2
[32m[    0.603240] [0m[33mTCP established hash table entries[0m: 8192 (order: 3, 32768 bytes)
[32m[    0.603303] [0m[33mTCP bind hash table entries[0m: 8192 (order: 4, 65536 bytes)
[32m[    0.603427] [0m[33mTCP[0m: Hash tables configured (established 8192 bind 8192)
[32m[    0.603480] [0m[33mUDP hash table entries[0m: 512 (order: 2, 16384 bytes)
[32m[    0.603512] [0m[33mUDP-Lite hash table entries[0m: 512 (order: 2, 16384 bytes)
[32m[    0.603725] [0m[33mNET[0m: Registered protocol family 1
[32m[    0.614025] [0m[33mRPC[0m: Registered named UNIX socket transport module.
[32m[    0.614034] [0m[33mRPC[0m: Registered udp transport module.
[32m[    0.614041] [0m[33mRPC[0m: Registered tcp transport module.
[32m[    0.614047] [0m[33mRPC[0m: Registered tcp NFSv4.1 backchannel transport module.
[32m[    0.614063] [0m[33mPCI[0m: CLS 0 bytes, default 64
[32m[    0.615040] [0m[33mhw perfevents[0m: enabled with armv7_cortex_a15 PMU driver, 7 counters available
[32m[    0.617408] [0m[33mfutex hash table entries[0m: 256 (order: 2, 16384 bytes)
[32m[    0.635128] [0m[33msquashfs[0m: version 4.0 (2009/01/31) Phillip Lougher
[32m[    0.645803] [0m[33mNFS[0m: Registering the id_resolver key type
[32m[    0.645839] [0mKey type id_resolver registered
[32m[    0.645847] [0mKey type id_legacy registered
[32m[    0.645911] [0m[33mntfs[0m: driver 2.1.32 [Flags: R/O].
[32m[    0.648167] [0m[33mbounce[0m: pool size: 64 pages
[32m[    0.648326] [0mBlock layer SCSI generic (bsg) driver version 0.4 loaded (major 247)
[32m[    0.648343] [0mio scheduler noop registered
[32m[    0.648357] [0mio scheduler deadline registered
[32m[    0.648393] [0mio scheduler cfq registered (default)
[32m[    0.650628] [0m[33mldousb[0m: supplied by VMAIN
[32m[    1.940214] [0m[33mclock[0m[31m: dpll_pcie_ref_ck failed transition to 'locked'[0m
[32m[    1.941638] [0m[33mpinctrl-single 4a003400.pinmux[0m: 282 pins at pa fc003400 size 1128
[32m[    1.941758] [0m[33mpinctrl-single 4a002e8c.pinmux[0m: 1 pins at pa fc002e8c size 4
[32m[    2.010423] [0m[33mSerial[0m: 8250/16550 driver, 10 ports, IRQ sharing disabled
[32m[    2.013838] [0m[33m48020000.serial[0m: ttyS2 at MMIO 0x48020000 (irq = 299, base_baud = 3000000) is a 8250
[32m[    2.848141] [0mconsole [ttyS2] enabled
[32m[    2.852840] [0m[drm] Initialized drm 1.1.0 20060810
[32m[    2.859023] [0m[33mldoln[0m: supplied by VMAIN
[32m[    2.863232] [0mOMAP DSS rev 6.1
[32m[    2.867006] [0m[33momapdss_dss 58000000.dss[0m: bound 58001000.dispc (ops dispc_component_ops)
[32m[    2.875531] [0m[33momapdss_dss 58000000.dss[0m: bound 58040000.encoder (ops hdmi5_component_ops)
[32m[    2.884429] [0m[33mtpd12s015 encoder@0[0m: GPIO lookup for consumer (null)
[32m[    2.884441] [0m[33mtpd12s015 encoder@0[0m: using device tree for GPIO lookup
[32m[    2.884452] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'gpios' property of node '/encoder@0[0]'
[32m[    2.884461] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'gpio' property of node '/encoder@0[0]'
[32m[    2.884469] [0m[33mtpd12s015 encoder@0[0m: using lookup tables for GPIO lookup
[32m[    2.884478] [0m[33mtpd12s015 encoder@0[0m: lookup for GPIO (null) failed
[32m[    2.884487] [0m[33mtpd12s015 encoder@0[0m: GPIO lookup for consumer (null)
[32m[    2.884495] [0m[33mtpd12s015 encoder@0[0m: using device tree for GPIO lookup
[32m[    2.884503] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'gpios' property of node '/encoder@0[1]'
[32m[    2.884511] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'gpio' property of node '/encoder@0[1]'
[32m[    2.884518] [0m[33mtpd12s015 encoder@0[0m: using lookup tables for GPIO lookup
[32m[    2.884526] [0m[33mtpd12s015 encoder@0[0m: lookup for GPIO (null) failed
[32m[    2.884535] [0m[33mtpd12s015 encoder@0[0m: GPIO lookup for consumer (null)
[32m[    2.884542] [0m[33mtpd12s015 encoder@0[0m: using device tree for GPIO lookup
[32m[    2.884571] [0m[33mof_get_named_gpiod_flags[0m: parsed 'gpios' property of node '/encoder@0[2]' - status (0)
[32m[    2.885265] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'hpd-gpios' property of node '/connector@0[0]'
[32m[    2.971572] [0m[33mloop[0m: module loaded
[32m[    2.980290] [0m[33mm25p80 spi32766.0[0m: s25fl256s1 (32768 Kbytes)
[32m[    2.985733] [0m7 ofpart partitions found on MTD device spi32766.0
[32m[    2.991591] [0mCreating 7 MTD partitions on "spi32766.0":
[32m[    2.996768] [0m[33m0x000000000000-0x000000040000 [0m: "QSPI.SPL"
[32m[    3.012906] [0m[33m0x000000040000-0x000000140000 [0m: "QSPI.u-boot"
[32m[    3.029236] [0m[33m0x000000140000-0x0000001c0000 [0m: "QSPI.u-boot-spl-os"
[32m[    3.046209] [0m[33m0x0000001c0000-0x0000001d0000 [0m: "QSPI.u-boot-env"
[32m[    3.062899] [0m[33m0x0000001d0000-0x0000001e0000 [0m: "QSPI.u-boot-env.backup1"
[32m[    3.080257] [0m[33m0x0000001e0000-0x0000009e0000 [0m: "QSPI.kernel"
[32m[    3.096588] [0m[33m0x0000009e0000-0x000002000000 [0m: "QSPI.file-system"
[32m[    3.114376] [0m[33mlibphy[0m: Fixed MDIO Bus: probed
[32m[    3.119070] [0mCAN device driver interface
[32m[    3.123117] [0m[1m==mux spi1_clk = 0x50000[0m
[32m[    3.126707] [0m[1m==mux spi1_d1 = 0x60000[0m
[32m[    3.130207] [0m[1m==mux spi1_d0 = 0x20000[0m
[32m[    3.133727] [0m[1m==mux spi1_cs0 = 0x20000[0m
[32m[    3.137316] [0m[1m==mux gpio4_13 = 0x6000e[0m
[32m[    3.140902] [0m[1m==mux spi2_clk = 0x50000[0m
[32m[    3.144502] [0m[1m==mux spi2_d1 = 0x60000[0m
[32m[    3.148002] [0m[1m==mux spi2_d0 = 0x20000[0m
[32m[    3.151501] [0m[1m==mux spi2_cs0 = 0x20000[0m
[32m[    3.155101] [0m[1m==mux gpio4_14 = 0x6000e[0m
[32m[    3.158687] [0m[1m==mux spi3_clk = 0x50003[0m
[32m[    3.162273] [0m[1m==mux spi3_d1 = 0x60003[0m
[32m[    3.165785] [0m[1m==mux spi3_d0 = 0x20003[0m
[32m[    3.169284] [0m[1m==mux spi3_cs0 = 0x20003[0m
[32m[    3.172881] [0m[1m==mux gpio4_15 = 0x6000e[0m
[32m[    3.176469] [0m[1m==mux spi4_clk = 0x50008[0m
[32m[    3.180054] [0m[1m==mux spi4_d1 = 0x60008[0m
[32m[    3.183565] [0m[1m==mux spi4_d0 = 0x20008[0m
[32m[    3.187064] [0m[1m==mux spi4_cs0 = 0x20008[0m
[32m[    3.190650] [0m[1m==mux gpio4_16 = 0x6000e[0m
[32m[    3.194438] [0m[33msmps9[0m: supplied by VMAIN
[32m[    3.198259] [0m[33mV3_3D[0m: supplied by smps9
[32m[    3.202165] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1221]=====[0m
[32m[    3.217799] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_reset]:651 canstat=0x80====[0m
[32m[    3.225591] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:667 ====[0m
[32m[    3.232377] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:670 ctrl=0x87====[0m
[32m[    3.239904] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1227]=====[0m
[32m[    3.245965] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1234]=====[0m
[32m[    3.251474] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1238]=====[0m
[32m[    3.257086] [0m[1m==mux spi1_clk = 0x50000[0m
[32m[    3.260675] [0m[1m==mux spi1_d1 = 0x60000[0m
[32m[    3.264190] [0m[1m==mux spi1_d0 = 0x20000[0m
[32m[    3.267691] [0m[1m==mux spi1_cs0 = 0x20000[0m
[32m[    3.271277] [0m[1m==mux gpio4_13 = 0x6000e[0m
[32m[    3.274875] [0m[1m==mux spi2_clk = 0x50000[0m
[32m[    3.278461] [0m[1m==mux spi2_d1 = 0x60000[0m
[32m[    3.281961] [0m[1m==mux spi2_d0 = 0x20000[0m
[32m[    3.285473] [0m[1m==mux spi2_cs0 = 0x20000[0m
[32m[    3.289061] [0m[1m==mux gpio4_14 = 0x6000e[0m
[32m[    3.292660] [0m[1m==mux spi3_clk = 0x50003[0m
[32m[    3.296247] [0m[1m==mux spi3_d1 = 0x60003[0m
[32m[    3.299746] [0m[1m==mux spi3_d0 = 0x20003[0m
[32m[    3.303257] [0m[1m==mux spi3_cs0 = 0x20003[0m
[32m[    3.306842] [0m[1m==mux gpio4_15 = 0x6000e[0m
[32m[    3.310428] [0m[1m==mux spi4_clk = 0x50008[0m
[32m[    3.314027] [0m[1m==mux spi4_d1 = 0x60008[0m
[32m[    3.317526] [0m[1m==mux spi4_d0 = 0x20008[0m
[32m[    3.321025] [0m[1m==mux spi4_cs0 = 0x20008[0m
[32m[    3.324622] [0m[1m==mux gpio4_16 = 0x6000e[0m
[32m[    3.328407] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1221]=====[0m
[32m[    3.344038] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_reset]:651 canstat=0x80====[0m
[32m[    3.351813] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:667 ====[0m
[32m[    3.358609] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:670 ctrl=0x87====[0m
[32m[    3.366135] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1227]=====[0m
[32m[    3.372141] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1234]=====[0m
[32m[    3.377665] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1238]=====[0m
[32m[    3.383260] [0m[1m==mux spi1_clk = 0x50000[0m
[32m[    3.386849] [0m[1m==mux spi1_d1 = 0x60000[0m
[32m[    3.390348] [0m[1m==mux spi1_d0 = 0x20000[0m
[32m[    3.393863] [0m[1m==mux spi1_cs0 = 0x20000[0m
[32m[    3.397449] [0m[1m==mux gpio4_13 = 0x6000e[0m
[32m[    3.401035] [0m[1m==mux spi2_clk = 0x50000[0m
[32m[    3.404633] [0m[1m==mux spi2_d1 = 0x60000[0m
[32m[    3.408134] [0m[1m==mux spi2_d0 = 0x20000[0m
[32m[    3.411632] [0m[1m==mux spi2_cs0 = 0x20000[0m
[32m[    3.415230] [0m[1m==mux gpio4_14 = 0x6000e[0m
[32m[    3.418817] [0m[1m==mux spi3_clk = 0x50003[0m
[32m[    3.422404] [0m[1m==mux spi3_d1 = 0x60003[0m
[32m[    3.425914] [0m[1m==mux spi3_d0 = 0x20003[0m
[32m[    3.429414] [0m[1m==mux spi3_cs0 = 0x20003[0m
[32m[    3.433012] [0m[1m==mux gpio4_15 = 0x6000e[0m
[32m[    3.436599] [0m[1m==mux spi4_clk = 0x50008[0m
[32m[    3.440185] [0m[1m==mux spi4_d1 = 0x60008[0m
[32m[    3.443697] [0m[1m==mux spi4_d0 = 0x20008[0m
[32m[    3.447196] [0m[1m==mux spi4_cs0 = 0x20008[0m
[32m[    3.450782] [0m[1m==mux gpio4_16 = 0x6000e[0m
[32m[    3.454560] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1221]=====[0m
[32m[    3.470169] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_reset]:651 canstat=0x80====[0m
[32m[    3.477959] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:667 ====[0m
[32m[    3.484754] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:670 ctrl=0x87====[0m
[32m[    3.492267] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1227]=====[0m
[32m[    3.498277] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1234]=====[0m
[32m[    3.503804] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1238]=====[0m
[32m[    3.509384] [0m[1m==mux spi1_clk = 0x50000[0m
[32m[    3.512989] [0m[1m==mux spi1_d1 = 0x60000[0m
[32m[    3.516489] [0m[1m==mux spi1_d0 = 0x20000[0m
[32m[    3.519988] [0m[1m==mux spi1_cs0 = 0x20000[0m
[32m[    3.523588] [0m[1m==mux gpio4_13 = 0x6000e[0m
[32m[    3.527175] [0m[1m==mux spi2_clk = 0x50000[0m
[32m[    3.530761] [0m[1m==mux spi2_d1 = 0x60000[0m
[32m[    3.534273] [0m[1m==mux spi2_d0 = 0x20000[0m
[32m[    3.537772] [0m[1m==mux spi2_cs0 = 0x20000[0m
[32m[    3.541360] [0m[1m==mux gpio4_14 = 0x6000e[0m
[32m[    3.544957] [0m[1m==mux spi3_clk = 0x50003[0m
[32m[    3.548545] [0m[1m==mux spi3_d1 = 0x60003[0m
[32m[    3.552044] [0m[1m==mux spi3_d0 = 0x20003[0m
[32m[    3.555554] [0m[1m==mux spi3_cs0 = 0x20003[0m
[32m[    3.559141] [0m[1m==mux gpio4_15 = 0x6000e[0m
[32m[    3.562739] [0m[1m==mux spi4_clk = 0x50008[0m
[32m[    3.566326] [0m[1m==mux spi4_d1 = 0x60008[0m
[32m[    3.569826] [0m[1m==mux spi4_d0 = 0x20008[0m
[32m[    3.573337] [0m[1m==mux spi4_cs0 = 0x20008[0m
[32m[    3.576924] [0m[1m==mux gpio4_16 = 0x6000e[0m
[32m[    3.580689] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1221]=====[0m
[32m[    3.596317] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_reset]:651 canstat=0x80====[0m
[32m[    3.604107] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:667 ====[0m
[32m[    3.610891] [0m[1m===[drivers/net/can/spi/mcp251x.c:mcp251x_hw_probe]:670 ctrl=0x87====[0m
[32m[    3.618417] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1227]=====[0m
[32m[    3.624427] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1234]=====[0m
[32m[    3.629936] [0m[1m*****[drivers/net/can/spi/mcp251x.c:1238]=====[0m
[32m[    3.644603] [0m[33momap_hwmod[0m[1m: dcan1: _wait_target_disable failed[0m
[32m[    3.650154] [0m[33mc_can_platform 4ae3c000.can[0m: c_can_platform device registered (regs=fce3c000, irq=347)
[32m[    3.659166] [0m[1m===mapAddr can1_dx=0x20000[0m
[32m[    3.662940] [0m[1m===mapAddr can1_rx=0x60000[0m
[32m[    3.666703] [0m[1m===mapAddr can2_dx=0x20002[0m
[32m[    3.670463] [0m[1m===mapAddr can2_rx=0x60002[0m
[32m[    3.674839] [0m[33mc_can_platform 48480000.can[0m: c_can_platform device registered (regs=fa480000, irq=348)
[32m[    3.683855] [0m[1m===mapAddr can1_dx=0x20000[0m
[32m[    3.687617] [0m[1m===mapAddr can1_rx=0x60000[0m
[32m[    3.691378] [0m[1m===mapAddr can2_dx=0x20002[0m
[32m[    3.695153] [0m[1m===mapAddr can2_rx=0x60002[0m
[32m[    3.742678] [0m[33mdavinci_mdio 48485000.mdio[0m: davinci mdio revision 1.6
[32m[    3.748803] [0m[33mdavinci_mdio 48485000.mdio[0m: detected phy mask fffffffe
[32m[    3.767270] [0m[33mlibphy[0m: 48485000.mdio: probed
[32m[    3.771302] [0m[33mdavinci_mdio 48485000.mdio[0m: phy[0]: device 48485000.mdio:00, driver Micrel KSZ9031 Gigabit PHY
[32m[    3.781613] [0m[33mcpsw 48484000.ethernet[0m[31m: No slave[1] phy_id, phy-handle, or fixed-link property
[0m[32m[    3.789991] [0m[33mcpsw 48484000.ethernet[0m: Detected MACID = 50:33:8b:94:22:10
[32m[    3.796696] [0m[33mcpsw 48484000.ethernet[0m: cpts: overflow check period 800
[32m[    3.804665] [0m[33mmousedev[0m: PS/2 mouse device common for all mice
[32m[    3.820777] [0mi2c /dev entries driver
[32m[    3.828603] [0m[33momap_hsmmc 4809c000.mmc[0m: GPIO lookup for consumer cd
[32m[    3.828615] [0m[33momap_hsmmc 4809c000.mmc[0m: using device tree for GPIO lookup
[32m[    3.828648] [0m[33mof_get_named_gpiod_flags[0m: parsed 'cd-gpios' property of node '/ocp/mmc@4809c000[0]' - status (0)
[32m[    3.828663] [0m[33momap_hsmmc 4809c000.mmc[0m: Got CD GPIO
[32m[    3.833358] [0m[33momap_hsmmc 4809c000.mmc[0m: GPIO lookup for consumer wp
[32m[    3.833367] [0m[33momap_hsmmc 4809c000.mmc[0m: using device tree for GPIO lookup
[32m[    3.833377] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'wp-gpios' property of node '/ocp/mmc@4809c000[0]'
[32m[    3.833387] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'wp-gpio' property of node '/ocp/mmc@4809c000[0]'
[32m[    3.833395] [0m[33momap_hsmmc 4809c000.mmc[0m: using lookup tables for GPIO lookup
[32m[    3.833404] [0m[33momap_hsmmc 4809c000.mmc[0m: lookup for GPIO wp failed
[32m[    3.833834] [0m[33mldo1[0m: supplied by VMAIN
[32m[    3.882916] [0m[33momap_hsmmc 480b4000.mmc[0m: GPIO lookup for consumer cd
[32m[    3.882927] [0m[33momap_hsmmc 480b4000.mmc[0m: using device tree for GPIO lookup
[32m[    3.882938] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'cd-gpios' property of node '/ocp/mmc@480b4000[0]'
[32m[    3.882947] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'cd-gpio' property of node '/ocp/mmc@480b4000[0]'
[32m[    3.882956] [0m[33momap_hsmmc 480b4000.mmc[0m: using lookup tables for GPIO lookup
[32m[    3.882964] [0m[33momap_hsmmc 480b4000.mmc[0m: lookup for GPIO cd failed
[32m[    3.882975] [0m[33momap_hsmmc 480b4000.mmc[0m: GPIO lookup for consumer wp
[32m[    3.882983] [0m[33momap_hsmmc 480b4000.mmc[0m: using device tree for GPIO lookup
[32m[    3.882992] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'wp-gpios' property of node '/ocp/mmc@480b4000[0]'
[32m[    3.883000] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'wp-gpio' property of node '/ocp/mmc@480b4000[0]'
[32m[    3.883008] [0m[33momap_hsmmc 480b4000.mmc[0m: using lookup tables for GPIO lookup
[32m[    3.883016] [0m[33momap_hsmmc 480b4000.mmc[0m: lookup for GPIO wp failed
[32m[    3.883194] [0m[33momap_hsmmc 480b4000.mmc[0m[31m: no pinctrl state for sdr25 mode
[0m[32m[    3.889577] [0m[33momap_hsmmc 480b4000.mmc[0m[31m: no pinctrl state for sdr12 mode
[0m[32m[    3.943152] [0m[33mof_get_named_gpiod_flags[0m: parsed 'gpios' property of node '/leds@1/led@0[0]' - status (0)
[32m[    3.943310] [0m[33mof_get_named_gpiod_flags[0m: parsed 'gpios' property of node '/leds@1/led@1[0]' - status (0)
[32m[    3.943424] [0m[33mof_get_named_gpiod_flags[0m: parsed 'gpios' property of node '/leds@1/led@2[0]' - status (0)
[32m[    3.943538] [0m[33mof_get_named_gpiod_flags[0m: parsed 'gpios' property of node '/leds@1/led@3[0]' - status (0)
[32m[    3.943659] [0m[33mof_get_named_gpiod_flags[0m: parsed 'gpios' property of node '/leds@1/led@4[0]' - status (0)
[32m[    3.943772] [0m[33mof_get_named_gpiod_flags[0m: parsed 'gpios' property of node '/leds@1/led@5[0]' - status (0)
[32m[    3.944253] [0m[33mledtrig-cpu[0m: registered to indicate activity on CPUs
[32m[    3.964746] [0m[33mNET[0m: Registered protocol family 10
[32m[    3.992991] [0m[33msit[0m: IPv6 over IPv4 tunneling driver
[32m[    3.998184] [0m[33mNET[0m: Registered protocol family 17
[32m[    4.012674] [0m[33mcan[0m: controller area network core (rev 20120528 abi 9)
[32m[    4.018940] [0m[33mNET[0m: Registered protocol family 29
[32m[    4.032699] [0m[33mcan[0m: raw protocol (rev 20120528)
[32m[    4.036991] [0m[33mcan[0m: broadcast manager protocol (rev 20120528 t)
[32m[    4.052665] [0m[33mcan[0m: netlink gateway (rev 20130117) max_hops=1
[32m[    4.058525] [0mKey type dns_resolver registered
[32m[    4.072794] [0m[33momap_voltage_late_init[0m[31m: Voltage driver support not added[0m
[32m[    4.079753] [0mAdding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[32m[    4.102649] [0mAdding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[32m[    4.112976] [0mAdding alias for supply vdd,cpu0 -> vdd,4a003b20.oppdm
[32m[    4.119185] [0mAdding alias for supply vbb,cpu0 -> vbb,4a003b20.oppdm
[32m[    4.143175] [0m[33mcpufreq[0m[1m: cpufreq_online: CPU0: Running at unlisted freq: 1000000 KHz[0m
[32m[    4.150618] [0m[33mcpu cpu0[0m[31m: dev_pm_opp_domain_set_rate: failed to find current OPP for freq 1000000000 (-34)
[0m[32m[    4.183142] [0m[33mcpufreq[0m[1m: cpufreq_online: CPU0: Unlisted initial frequency changed to: 500000 KHz[0m
[32m[    4.202681] [0mPower Management for TI OMAP4+ devices.
[32m[    4.207927] [0mRegistering SWP/SWPB emulation handler
[32m[    4.227756] [0m[33mdmm 4e000000.dmm[0m: initialized all PAT entries
[32m[    4.236219] [0m[33mldo3[0m: supplied by VMAIN
[32m[    4.249599] [0m[drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
[32m[    4.256360] [0m[drm] No driver support for vblank timestamp query.
[32m[    4.262359] [0m[33momapdrm omapdrm.0[0m: No connectors reported connected with modes
[32m[    4.269386] [0m[drm] Cannot find any crtc or sizes - going 1024x768
[32m[    4.282408] [0m[33mmmc0[0m[1m: host does not support reading read-only switch, assuming write-enable[0m
[32m[    4.291496] [0m[drm] Enabling DMM ywrap scrolling
[32m[    4.298088] [0m[33mmmc0[0m: new high speed SDHC card at address 59b4
[32m[    4.309046] [0m[33mConsole[0m: switching to colour frame buffer device 128x48
[32m[    4.326997] [0m[33mmmcblk0[0m: mmc0:59b4 00000 7.35 GiB 
[32m[    4.334235] [0m[33m mmcblk0[0m: p1 p2
[32m[    4.343953] [0m[33momapdrm omapdrm.0[0m: fb0: omapdrm frame buffer device
[32m[    4.374089] [0m[drm] Initialized omapdrm 1.0.0 20110917 on minor 0
[32m[    4.401573] [0m[33mhctosys[0m: unable to open rtc device (rtc0)
[32m[    4.407431] [0m[33mmmc1[0m: MAN_BKOPS_EN bit is not set
[32m[    4.430797] [0m[33mmmc1[0m: new DDR MMC card at address 0001
[32m[    4.441800] [0mALSA device list:
[32m[    4.444839] [0m  No soundcards found.
[32m[    4.451551] [0m[33mmmcblk1[0m: mmc1:0001 S10004 3.56 GiB 
[32m[    4.466686] [0m[33mmmcblk1boot0[0m: mmc1:0001 S10004 partition 1 4.00 MiB
[32m[    4.483191] [0m[33mmmcblk1boot1[0m: mmc1:0001 S10004 partition 2 4.00 MiB
[32m[    4.490395] [0m[33m mmcblk1[0m: p1 p2
[32m[    7.042528] [0m[33mEXT4-fs (mmcblk0p2)[0m: recovery complete
[32m[    7.077355] [0m[33mEXT4-fs (mmcblk0p2)[0m: mounted filesystem with ordered data mode. Opts: (null)
[32m[    7.085621] [0m[33mVFS[0m: Mounted root (ext4 filesystem) on device 179:2.
[32m[    7.100606] [0m[33mdevtmpfs[0m: mounted
[32m[    7.104137] [0m[33mFreeing unused kernel memory[0m: 336K (c08f0000 - c0944000)
[32m[    7.110528] [0m[1mThis architecture does not have kernel memory protection.[0m
[32m[    7.372469] [0m[33msystemd[1][0m: System time before build time, advancing clock.
[32m[    7.426216] [0m[33mrandom[0m: systemd: uninitialized urandom read (16 bytes read, 27 bits of entropy available)
[32m[    7.442093] [0m[33mrandom[0m: systemd: uninitialized urandom read (16 bytes read, 28 bits of entropy available)
[32m[    7.456462] [0m[33msystemd[1][0m: systemd 229 running in system mode. (+PAM -AUDIT -SELINUX +IMA -APPARMOR +SMACK +SYSVINIT +UTMP -LIBCRYPTSETUP -GCRYPT -GNUTLS +ACL +XZ -LZ4 -SECCOMP +BLKID -ELFUTILS +KMOD -IDN)
[32m[    7.475410] [0m[33msystemd[1][0m: Detected architecture arm.
[32m[    7.504355] [0m[33msystemd[1][0m: Set hostname to <am57xx-evm>.
[32m[    7.585746] [0m[33mrandom[0m: systemd-sysv-ge: uninitialized urandom read (16 bytes read, 29 bits of entropy available)
[32m[    7.609190] [0m[33mrandom[0m: systemd-gpt-aut: uninitialized urandom read (16 bytes read, 30 bits of entropy available)
[32m[    7.623690] [0m[33mrandom[0m: systemd-gpt-aut: uninitialized urandom read (16 bytes read, 30 bits of entropy available)
[32m[    7.642591] [0m[33mrandom[0m: systemd-sysv-ge: uninitialized urandom read (16 bytes read, 30 bits of entropy available)
[32m[    7.669110] [0m[33mrandom[0m: systemd-sysv-ge: uninitialized urandom read (16 bytes read, 31 bits of entropy available)
[32m[    7.775085] [0m[33mrandom[0m: systemd: uninitialized urandom read (16 bytes read, 34 bits of entropy available)
[32m[    7.785233] [0m[33mrandom[0m: systemd: uninitialized urandom read (16 bytes read, 34 bits of entropy available)
[32m[    7.796048] [0m[33mrandom[0m: systemd: uninitialized urandom read (16 bytes read, 34 bits of entropy available)
[32m[    8.498447] [0m[33msystemd[1][0m[1m: sysinit.target: Found ordering cycle on sysinit.target/start[0m
[32m[    8.506368] [0m[33msystemd[1][0m[1m: sysinit.target: Found dependency on alignment.service/start[0m
[32m[    8.514263] [0m[33msystemd[1][0m[1m: sysinit.target: Found dependency on basic.target/start[0m
[32m[    8.521543] [0m[33msystemd[1][0m[1m: sysinit.target: Found dependency on sockets.target/start[0m
[32m[    8.529071] [0m[33msystemd[1][0m[1m: sysinit.target: Found dependency on dropbear.socket/stop[0m
[32m[    8.536552] [0m[33msystemd[1][0m[1m: sysinit.target: Found dependency on sysinit.target/start[0m
[32m[    8.544032] [0m[33msystemd[1][0m[1m: sysinit.target: Breaking ordering cycle by deleting job alignment.service/start[0m
[32m[    8.553518] [0m[33msystemd[1][0m[31m: alignment.service: Job alignment.service/start deleted to break ordering cycle starting with sysinit.target/start[0m
[32m[    8.598698] [0m[33msystemd[1][0m: Listening on udev Control Socket.
[32m[    8.623473] [0m[33msystemd[1][0m: Listening on Journal Socket (/dev/log).
[32m[    8.653372] [0m[33msystemd[1][0m: Listening on Journal Socket.
[32m[    8.683550] [0m[33msystemd[1][0m: Reached target Remote File Systems.
[32m[    8.713106] [0m[33msystemd[1][0m: Reached target Swap.
[32m[    8.733576] [0m[33msystemd[1][0m: Listening on Network Service Netlink Socket.
[32m[    8.763245] [0m[33msystemd[1][0m: Listening on Syslog Socket.
[32m[    8.793222] [0m[33msystemd[1][0m: Listening on udev Kernel Socket.
[32m[    8.827365] [0m[33msystemd[1][0m: Created slice User and Session Slice.
[32m[    8.853548] [0m[33msystemd[1][0m: Started Dispatch Password Requests to Console Directory Watch.
[32m[    8.900332] [0m[33msystemd[1][0m: Started Forward Password Requests to Wall Directory Watch.
[32m[    8.933142] [0m[33msystemd[1][0m: Reached target Paths.
[32m[    8.953318] [0m[33msystemd[1][0m: Listening on /dev/initctl Compatibility Named Pipe.
[32m[    8.984523] [0m[33msystemd[1][0m: Created slice System Slice.
[32m[    9.014635] [0m[33msystemd[1][0m: Created slice system-getty.slice.
[32m[    9.047563] [0m[33msystemd[1][0m: Mounting POSIX Message Queue File System...
[32m[    9.088300] [0m[33msystemd[1][0m: Mounting Temporary Directory...
[32m[    9.137632] [0m[33msystemd[1][0m: Starting Setup Virtual Console...
[32m[    9.177903] [0m[33msystemd[1][0m: Starting Journal Service...
[32m[    9.213329] [0m[33msystemd[1][0m: Reached target Slices.
[32m[    9.248097] [0m[33msystemd[1][0m: Starting Create list of required static device nodes for the current kernel...
[32m[    9.343462] [0m[33msystemd[1][0m: Starting Load Kernel Modules...
[32m[    9.384923] [0m[33msystemd[1][0m: Created slice system-serial\x2dgetty.slice.
[32m[    9.399063] [0m[33mCMEMK module[0m: reference Linux version 4.4.41
[32m[    9.412086] [0mcmemk initialized
[32m[    9.427919] [0m[33msystemd[1][0m: Mounting Debug File System...
[32m[    9.463417] [0m[33mcryptodev[0m: driver 1.8 loaded.
[32m[    9.491552] [0m[33msystemd[1][0m: Starting Remount Root and Kernel File Systems...
[32m[    9.577617] [0m[33mEXT4-fs (mmcblk0p2)[0m: re-mounted. Opts: (null)
[32m[    9.643120] [0m[33msystemd[1][0m: Mounted Debug File System.
[32m[    9.673361] [0m[33msystemd[1][0m: Mounted POSIX Message Queue File System.
[32m[    9.703260] [0m[33msystemd[1][0m: Mounted Temporary Directory.
[32m[    9.737038] [0m[33msystemd[1][0m: Started Journal Service.
[32m[   11.283275] [0m[33msystemd-journald[123][0m: Received request to flush runtime journal from PID 1
[32m[   13.761069] [0m[33momap-rproc 58820000.ipu[0m: assigned reserved memory node ipu1_cma@9d000000
[32m[   13.856737] [0m[33m remoteproc0[0m: 58820000.ipu is available
[32m[   13.902149] [0m[33m remoteproc0[0m: Note: remoteproc is still under development and considered experimental.
[32m[   13.990974] [0m[33m remoteproc0[0m: THE BINARY FORMAT IS NOT YET FINALIZED, and backward compatibility isn't yet guaranteed.
[32m[   14.157249] [0m[33momap-rproc 55020000.ipu[0m: assigned reserved memory node ipu2_cma@95800000
[32m[   14.269577] [0m[33m remoteproc1[0m: 55020000.ipu is available
[32m[   14.339336] [0m[33m remoteproc1[0m: Note: remoteproc is still under development and considered experimental.
[32m[   14.418742] [0m[33m remoteproc0[0m: registered virtio0 (type 7)
[32m[   14.507895] [0m[33m remoteproc1[0m: THE BINARY FORMAT IS NOT YET FINALIZED, and backward compatibility isn't yet guaranteed.
[32m[   14.645131] [0m[33momap-rproc 40800000.dsp[0m: assigned reserved memory node dsp1_cma@99000000
[32m[   14.701731] [0m[33m remoteproc2[0m: 40800000.dsp is available
[32m[   14.785726] [0m[33m remoteproc2[0m: Note: remoteproc is still under development and considered experimental.
[32m[   14.843640] [0m[33m remoteproc1[0m: registered virtio1 (type 7)
[32m[   14.888001] [0m[33m remoteproc2[0m: THE BINARY FORMAT IS NOT YET FINALIZED, and backward compatibility isn't yet guaranteed.
[32m[   14.946479] [0m[33mov2659 0-0030[0m: GPIO lookup for consumer pwrdn
[32m[   14.946508] [0m[33mov2659 0-0030[0m: using device tree for GPIO lookup
[32m[   14.946578] [0m[33mof_get_named_gpiod_flags[0m: parsed 'pwrdn-gpios' property of node '/ocp/i2c@48070000/ov2659@30[0]' - status (0)
[32m[   14.950672] [0m[33mov2659 0-0030[0m[31m: Sensor detection failed (3030, 0)
[0m[32m[   14.961495] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   14.990099] [0m[33momap_rng 48090000.rng[0m: OMAP Random Number Generator ver. 20
[32m[   15.019798] [0m[33momap-des 480a5000.des[0m: OMAP DES hw accel rev: 2.2
[32m[   15.029782] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   15.083354] [0m[33malg[0m[31m: skcipher: setkey failed on test 5 for ecb-des-omap: flags=100[0m
[32m[   15.131641] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   15.208044] [0m[33malg[0m[31m: skcipher-ddst: setkey failed on test 5 for ecb-des-omap: flags=100[0m
[32m[   15.286715] [0m[33malg[0m[31m: skcipher-ddst: setkey failed on test 5 for ecb-des-omap: flags=100[0m
[32m[   15.300566] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   15.313276] [0m[33mrtc rtc0[0m: 48070000.i2c:tps659: dev (254:0)
[32m[   15.313324] [0m[33mpalmas-rtc 48070000.i2c:tps659038@58:tps659038_rtc[0m: rtc core: registered 48070000.i2c:tps659 as rtc0
[32m[   15.431213] [0m[33mgpiochip_find_base[0m: found new base at 496
[32m[   15.431464] [0m[33mgpiochip_add[0m: registered GPIOs 496 to 503 on device: tpic2810
[32m[   15.438292] [0m[33mpalmas-usb 48070000.i2c:tps659038@58:tps659038_usb[0m: GPIO lookup for consumer id
[32m[   15.438321] [0m[33mpalmas-usb 48070000.i2c:tps659038@58:tps659038_usb[0m: using device tree for GPIO lookup
[32m[   15.438344] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'id-gpios' property of node '/ocp/i2c@48070000/tps659038@58/tps659038_usb[0]'
[32m[   15.438467] [0m[33mof_get_named_gpiod_flags[0m: parsed 'id-gpio' property of node '/ocp/i2c@48070000/tps659038@58/tps659038_usb[0]' - status (0)
[32m[   15.438550] [0m[33mpalmas-usb 48070000.i2c:tps659038@58:tps659038_usb[0m: GPIO lookup for consumer vbus
[32m[   15.438570] [0m[33mpalmas-usb 48070000.i2c:tps659038@58:tps659038_usb[0m: using device tree for GPIO lookup
[32m[   15.438590] [0m[33mof_get_named_gpiod_flags[0m: can't parse 'vbus-gpios' property of node '/ocp/i2c@48070000/tps659038@58/tps659038_usb[0]'
[32m[   15.438648] [0m[33mof_get_named_gpiod_flags[0m: parsed 'vbus-gpio' property of node '/ocp/i2c@48070000/tps659038@58/tps659038_usb[0]' - status (0)
[32m[   15.476372] [0m[33mpalmas-usb 48070000.i2c:tps659038@58:tps659038_usb[0m: USB-HOST cable is attached
[32m[   15.630114] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   15.759543] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   15.832042] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   15.960601] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   16.070430] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   16.174478] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   16.306352] [0m[33m remoteproc2[0m: registered virtio2 (type 7)
[32m[   16.361460] [0m[33mrtc rtc1[0m: 48838000.rtc: dev (254:1)
[32m[   16.361494] [0m[33momap_rtc 48838000.rtc[0m: rtc core: registered 48838000.rtc as rtc1
[32m[   16.583240] [0m[33mvpe 489d0000.vpe[0m: loading firmware vpdma-1b8.bin
[32m[   16.663243] [0m[33mvpe 489d0000.vpe[0m: Device registered as /dev/video0
[32m[   16.962765] [0m[33mvip 48970000.vip[0m: loading firmware vpdma-1b8.bin
[32m[   16.982812] [0m[33mvip 48970000.vip[0m: VPDMA firmware loaded
[32m[   18.198008] [0mSCSI subsystem initialized
[32m[   18.367804] [0m[33mFAT-fs (mmcblk0p1)[0m[1m: Volume was not properly unmounted. Some data may be corrupt. Please run fsck.[0m
[32m[   18.537677] [0m[33momap_wdt[0m: OMAP Watchdog Timer Rev 0x01: initial timeout 60 sec
[32m[   18.564945] [0mlibata version 3.00 loaded.
[32m[   18.647747] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   18.819740] [0m[33mti-pipe3 4a096000.phy[0m[31m: DPLL failed to lock
[0m[32m[   18.845173] [0m[33mEXT4-fs (mmcblk1p2)[0m: recovery complete
[32m[   18.850027] [0m[33mEXT4-fs (mmcblk1p2)[0m: mounted filesystem with ordered data mode. Opts: (null)
[32m[   18.859293] [0m[33mFAT-fs (mmcblk1p1)[0m[1m: Volume was not properly unmounted. Some data may be corrupt. Please run fsck.[0m
[32m[   18.964983] [0m[33mphy phy-4a096000.phy.2[0m[31m: phy init failed --> -22
[0m[32m[   19.000877] [0m[33mcan_dev[0m[31m: exports duplicate symbol alloc_can_err_skb (owned by kernel)[0m
[32m[   19.022924] [0m[33mahci[0m[1m: probe of 4a140000.sata failed with error -22[0m
[32m[   19.142039] [0m[33momap-sham 4b101000.sham[0m: hw accel on OMAP rev 4.3
[32m[   19.205741] [0m[1mr->name:nonblocking[0m
[32m[   19.208920] [0m[33mrandom[0m: nonblocking pool is initialized
[32m[   20.260328] [0m[33mNET[0m: Registered protocol family 15
[32m[   20.358919] [0m[33mBluetooth[0m: Core ver 2.21
[32m[   20.362619] [0m[33mNET[0m: Registered protocol family 31
[32m[   20.615086] [0m[33mBluetooth[0m: HCI device and connection manager initialized
[32m[   20.741382] [0m[33mBluetooth[0m: HCI socket layer initialized
[32m[   20.761739] [0m[33momap-aes 4b500000.aes[0m: OMAP AES hw accel rev: 3.3
[32m[   20.806186] [0m[33mBluetooth[0m: L2CAP socket layer initialized
[32m[   20.811350] [0m[33mBluetooth[0m: SCO socket layer initialized
[32m[   20.954570] [0m[33momap_hwmod[0m[1m: dcan1: _wait_target_disable failed[0m
[32m[   21.327308] [0m[33momap-hdmi-audio omap-hdmi-audio.0.auto[0m: snd-soc-dummy-dai <-> 58040000.encoder mapping ok
[32m[   21.347718] [0m[33momap_hwmod[0m[1m: dcan1: _wait_target_disable failed[0m
[32m[   21.662580] [0m[33momap_hwmod[0m[1m: dcan1: _wait_target_disable failed[0m
[32m[   21.761156] [0m[33momap_hwmod[0m[31m: gpu: _wait_target_ready failed: -16[0m
[32m[   21.838821] [0m[33mPVR_K:(Error)[0m: EnableSGXClocks: pm_runtime_get_sync failed (16)
[32m[   21.882341] [0mInitializing XFRM netlink socket
[32m[   21.951365] [0m[33mPVR_K:(Error)[0m: SysInitialise: Failed to Enable system clocks (175)
[32m[   22.010923] [0m[33mnet eth0[0m: initializing cpsw version 1.15 (0)
[32m[   22.052500] [0m[33mnet eth0[0m: initialized cpsw ale version 1.4
[32m[   22.095657] [0m[33momap-aes 4b700000.aes[0m: OMAP AES hw accel rev: 3.3
[32m[   22.153449] [0m[33mnet eth0[0m: ALE Table size 1024
[32m[   22.435895] [0m[33mnet eth0[0m: phy found : id is : 0x221622
[32m[   22.440948] [0m[33mlibphy[0m[31m: PHY  not found[0m
[32m[   22.541217] [0m[33mnet eth0[0m[31m: phy "" not found on slave 1, err -19
[0m[32m[   22.776714] [0m[33mIPv6[0m: ADDRCONF(NETDEV_UP): eth0: link is not ready
[32m[   24.937720] [0m[33momap_hwmod[0m[1m: dcan1: _wait_target_disable failed[0m
[32m[   27.040636] [0m[33m remoteproc0[0m: powering up 58820000.ipu
[32m[   27.311300] [0m[33m remoteproc0[0m: Booting fw image dra7-ipu1-fw.xem4, size 4890352
[32m[   27.413007] [0m[33momap-iommu 58882000.mmu[0m: 58882000.mmu: version 2.1
[32m[   27.576726] [0m[33m remoteproc0[0m: remote processor 58820000.ipu is now up
[32m[   27.683903] [0m[33mvirtio_rpmsg_bus virtio0[0m: rpmsg host is online
[32m[   27.689535] [0m[33mvirtio_rpmsg_bus virtio0[0m: creating channel rpmsg-client-sample addr 0x32
[32m[   27.743904] [0m[33mvirtio_rpmsg_bus virtio0[0m: creating channel rpmsg-client-sample addr 0x33
[32m[   27.825215] [0m[33mvirtio_rpmsg_bus virtio0[0m: creating channel rpmsg-omx addr 0x3c
[32m[   27.903507] [0m[33mvirtio_rpmsg_bus virtio0[0m: creating channel rpmsg-rpc addr 0x65
[32m[   27.993647] [0m[33m remoteproc1[0m: powering up 55020000.ipu
[32m[   28.070343] [0m[33m remoteproc1[0m: Booting fw image dra7-ipu2-fw.xem4, size 3743116
[32m[   28.158679] [0m[33momap-iommu 55082000.mmu[0m: 55082000.mmu: version 2.1
[32m[   28.563734] [0m[33mti-pipe3 4a084400.phy[0m[31m: DPLL failed to lock
[0m[32m[   28.610895] [0m[33mphy phy-4a084400.phy.4[0m[31m: phy init failed --> -22
[0m[32m[   28.669907] [0m[33mdwc3 48890000.usb[0m[31m: failed to initialize core
[0m[32m[   28.710250] [0m[33mdwc3[0m[1m: probe of 48890000.usb failed with error -22[0m
[32m[   29.187615] [0m[33m remoteproc1[0m: remote processor 55020000.ipu is now up
[32m[   29.284918] [0m[33mvirtio_rpmsg_bus virtio1[0m: rpmsg host is online
[32m[   29.290509] [0m[33mvirtio_rpmsg_bus virtio1[0m: creating channel rpmsg-rpc addr 0x65
[32m[   29.333502] [0m[33mvirtio_rpmsg_bus virtio1[0m: creating channel rpmsg-rpc addr 0x66
[32m[   29.354660] [0m[33m remoteproc2[0m: powering up 40800000.dsp
[32m[   29.756768] [0m[33m remoteproc2[0m: Booting fw image dra7-dsp1-fw.xe66, size 21914156
[32m[   29.847079] [0m[33momap_hwmod[0m[1m: mmu0_dsp1: _wait_target_disable failed[0m
[32m[   29.853013] [0m[33momap-iommu 40d01000.mmu[0m: 40d01000.mmu: version 3.0
[32m[   29.859022] [0m[33momap-iommu 40d02000.mmu[0m: 40d02000.mmu: version 3.0
[32m[   30.211667] [0m[33m remoteproc2[0m: remote processor 40800000.dsp is now up
[32m[   30.402343] [0m[33mvirtio_rpmsg_bus virtio2[0m: rpmsg host is online
[32m[   30.408168] [0m[33mvirtio_rpmsg_bus virtio2[0m: creating channel rpmsg-proto addr 0x3d
[32m[   30.519174] [0m[33musbcore[0m: registered new interface driver usbfs
[32m[   30.584799] [0m[33musbcore[0m: registered new interface driver hub
[32m[   30.641468] [0m[33mrpmsg_rpc rpmsg3[0m: probing service rpc_example_2 with src 1024 dst 101
[32m[   30.651979] [0m[33mNET[0m: Registered protocol family 41
[32m[   30.701311] [0m[33musbcore[0m: registered new device driver usb
[32m[   30.735932] [0m[33mrpmsg_rpc rpmsg4[0m: probing service dce-callback with src 1024 dst 101
[32m[   30.743517] [0m[33mrpmsg_rpc rpmsg3[0m: published functions = 8
[32m[   30.805759] [0m[33mdwc3 488d0000.usb[0m: otg: primary host xhci-hcd.1.auto registered
[32m[   30.831767] [0m[33mrpmsg_rpc rpmsg5[0m: probing service rpmsg-dce with src 1025 dst 102
[32m[   30.839064] [0m[33mrpmsg_rpc rpmsg4[0m: published functions = 4
[32m[   30.887831] [0m[33mdwc3 488d0000.usb[0m: otg: shared host xhci-hcd.1.auto registered
[32m[   30.907311] [0m[33mrpmsg_rpc rpmsg5[0m: published functions = 9
[32m[   30.966226] [0m[33mdwc3 488d0000.usb[0m: otg: can't start till gadget registers
[32m[   33.888390] [0m[33momap_hwmod[0m[1m: dcan1: _wait_target_disable failed[0m
[32m[   41.051569] [0m[33momap_hwmod[0m[1m: mmu1_dsp1: _wait_target_disable failed[0m
[32m[   41.067896] [0m[33momap_hwmod[0m[1m: mmu0_dsp1: _wait_target_disable failed[0m
root@am57xx-evm:~# 
Thanks for using picocom
picocom v1.7

port is        : /dev/ttyUSB0
flowcontrol    : none
baudrate is    : 115200
parity is      : none
databits are   : 8
escape is      : C-a
local echo is  : no
noinit is      : no
noreset is     : no
nolock is      : no
send_cmd is    : sz -vv
receive_cmd is : rz -vv
imap is        : 
omap is        : 
emap is        : crcrlf,delbs,

