1. Remove the link to your firmware, this will make sure that the R5 SPL doesn't load it, we can then load it 
   using the u-boot.

2. Reboot and stop at the u-boot prompt, you should see in the SPL prints
   ** File not found /lib/firmware/j7-mcu-r5f0_0-fw **

   this means that the R5 SPL did not find any valid firmware image for MCU R5F0_0

3. Load the firmware using u-boot

4. Launch CCS and connect to MCU R5F0_0
   This should be in main(), looping on the while(1)

   Type boot at u-boot prompt and boot to linux too (optional)

5  You are now in your application! Load the symbols and start debugging.
