Parsing the input object file, /home/user/ti_sdk_8.0/ti-processor-sdk-rtos-j721e-evm-08_00_00_12/pdk_jacinto_08_00_00_37/packages/ti/binary/csl_uart_test_app/bin/j721e_evm/csl_uart_test_app_mcu1_0_release.xer5f.
File conversion complete!
WARNING: The runtime version supported by this application is unavailable.
Using default runtime: v4.0.30319
Number of Input Files 1

Number of Input Files 1

Parsing the input object file, /home/user/ti_sdk_8.0/ti-processor-sdk-rtos-j721e-evm-08_00_00_12/pdk_jacinto_08_00_00_37/packages/ti/binary/csl_uart_test_app/bin/j721e_evm/csl_uart_test_app_mcu1_0_release.xer5f.
File conversion complete!
WARNING: The runtime version supported by this application is unavailable.
Using default runtime: v4.0.30319
Number of Input Files 1

Number of Input Files 1

Parsing the input object file, /home/user/ti_sdk_8.0/ti-processor-sdk-rtos-j721e-evm-08_00_00_12/pdk_jacinto_08_00_00_37/packages/ti/binary/csl_uart_test_app/bin/j721e_evm/csl_uart_test_app_mcu1_0_release.xer5f.
File conversion complete!
WARNING: The runtime version supported by this application is unavailable.
Using default runtime: v4.0.30319
Number of Input Files 1

Number of Input Files 1

