<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<configurations XML_version="1.2" id="configurations_0">
    <configuration XML_version="1.2" id="configuration_0">
        <instance XML_version="1.2" desc="Texas Instruments XDS2xx USB Debug Probe" href="connections/TIXDS2XXUSB_Connection.xml" id="Texas Instruments XDS2xx USB Debug Probe" xml="TIXDS2XXUSB_Connection.xml" xmlpath="connections"/>
        <connection XML_version="1.2" id="Texas Instruments XDS2xx USB Debug Probe">
            <instance XML_version="1.2" href="drivers/tixds560icepick_d.xml" id="drivers" xml="tixds560icepick_d.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560arm9.xml" id="drivers" xml="tixds560arm9.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560cs_dap.xml" id="drivers" xml="tixds560cs_dap.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560cortexM.xml" id="drivers" xml="tixds560cortexM.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560cs_child.xml" id="drivers" xml="tixds560cs_child.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560c66xx.xml" id="drivers" xml="tixds560c66xx.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560dap_pc.xml" id="drivers" xml="tixds560dap_pc.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560cortexA15.xml" id="drivers" xml="tixds560cortexA15.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560csstm.xml" id="drivers" xml="tixds560csstm.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560etbcs.xml" id="drivers" xml="tixds560etbcs.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560pru.xml" id="drivers" xml="tixds560pru.xml" xmlpath="drivers"/>
            <property Type="choicelist" Value="0" id="The JTAG TCLK Frequency (MHz)">
                <choice Name="Fixed with user specified faster value" value="SPECIFIC">
                    <property Type="stringfield" Value="10.368MHz" id="-- Enter a value from 0.5MHz to 20.0MHz"/>
                </choice>
            </property>
            <platform XML_version="1.2" id="platform_0">
                <instance XML_version="1.2" desc="GPEVM_AM572X" href="boards/gpevm_am572x.xml" id="GPEVM_AM572X" xml="gpevm_am572x.xml" xmlpath="boards"/>
            <board XML_version="1.2" description="AM572x General Purpose Evaluation Module with silicon revision 2.x" id="GPEVM_AM572X">
                    <device HW_revision="1.1" XML_version="1.2" description="AM5728 - Cortex A15 Embedded Processor&#10;Silicon Revision 2.x" id="AM5728_0" partnum="AM5728" simulation="no">
                        <router HW_revision="1.0" XML_version="1.2" description="ICEPick_D Router" id="IcePick_D_0" isa="ICEPICK_D">
                            <subpath id="IPU_2_C0">
                                <router HW_revision="1.0" XML_version="1.2" description="CS_DAP Router" id="CS_DAP_3" isa="CS_DAP">
                                    <subpath id="CortexM4_IPU_2_C0">
                                        <cpu HW_revision="1.0" XML_version="1.2" desc="ICECrusherCS_2" description="Cross Triggering" deviceSim="false" id="ICECrusherCS_0" isa="cs_child"/>
                                    </subpath>
                                </router>
                            </subpath>
                            <subpath id="IPU_2_C1">
                                <router HW_revision="1.0" XML_version="1.2" description="CS_DAP Router" id="CS_DAP_4" isa="CS_DAP">
                                    <subpath id="CortexM4_IPU_2_C1">
                                        <cpu HW_revision="1.0" XML_version="1.2" desc="ICECrusherCS_3" description="Cross Triggering" deviceSim="false" id="ICECrusherCS_0" isa="cs_child"/>
                                    </subpath>
                                </router>
                            </subpath>
                        </router>
                    </device>
                </board>
            </platform>
        </connection>
    </configuration>
</configurations>
