
U-Boot 2013.01.01 (Sep 05 2016 - 02:36:30)

I2C:   ready
DRAM:  1 GiB
WARNING: Caches not enabled
NAND:  No NAND device found!!!
0 MiB
MMC:   OMAP SD/MMC: 0, OMAP SD/MMC: 1
SF: Detected N25Q128 with page size 64 KiB, total 16 MiB
musb-hdrc: ConfigData=0xde (UTMI-8, dyn FIFOs, bulk combine, bulk split, HB-ISO Rx, HB-ISO Tx, SoftConn)
musb-hdrc: MHDRC RTL version 2.0 
musb-hdrc: setup fifo_mode 4
musb-hdrc: 28/31 max ep, 16384/16384 memory
USB Peripheral mode controller at 47401000 using PIO, IRQ 0
musb-hdrc: ConfigData=0xde (UTMI-8, dyn FIFOs, bulk combine, bulk split, HB-ISO Rx, HB-ISO Tx, SoftConn)
musb-hdrc: MHDRC RTL version 2.0 
musb-hdrc: setup fifo_mode 4
musb-hdrc: 28/31 max ep, 16384/16384 memory
USB Host mode controller at 47401800 using PIO, IRQ 0
Net:   register M88E1512_driver
init cpsw_slaves RGMII 
trying to get phy id
trying to get phy id ok, id:0x1410dd1
phy driver:Marvell 88E1512 compare duid:0X1410DD1 mask0XFFFFFF1 phy_id0X1410DD1
cpsw, usb_ether
Hit any key to stop autoboot:  0 
U-Boot# 
U-Boot# 
U-Boot# 
U-Boot# 
U-Boot# tftp 0x83000000 uImage;tftp 0x80F80000 am335x-evm.dtb;bootm 0x83000000 - 0x80F80000
link up on port 0, speed 1000, full duplex
Using cpsw device
TFTP from server 192.168.8.100; our IP address is 192.168.8.11
Filename 'uImage'.
Load address: 0x83000000
Loading: #################################################################
         #################################################################
         #################################################################
         #######################################################
         808.6 KiB/s
done
Bytes transferred = 3656736 (37cc20 hex)
link up on port 0, speed 1000, full duplex
Using cpsw device
TFTP from server 192.168.8.100; our IP address is 192.168.8.11
Filename 'am335x-evm.dtb'.
Load address: 0x80f80000
Loading: ###
         689.5 KiB/s
done
Bytes transferred = 43077 (a845 hex)
## Booting kernel from Legacy Image at 83000000 ...
   Image Name:   Linux-4.4.20-dirty
   Image Type:   ARM Linux Kernel Image (uncompressed)
   Data Size:    3656672 Bytes = 3.5 MiB
   Load Address: 80008000
   Entry Point:  80008000
   Verifying Checksum ... OK
## Flattened Device Tree blob at 80f80000
   Booting using the fdt blob at 0x80f80000
   Loading Kernel Image ... OK
OK
   Using Device Tree in place at 80f80000, end 80f8d844

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Initializing cgroup subsys cpu
[    0.000000] Initializing cgroup subsys cpuacct
[    0.000000] Linux version 4.4.20-dirty (eware@ubuntu) (gcc version 5.3.1 20160113 (Linaro GCC 5.3-2016.02) ) #29 PREEMPT Thu Dec 14 15:56:51 CST 2017
[    0.000000] CPU: ARMv7 Processor [413fc082] revision 2 (ARMv7), cr=10c5387d
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] Machine model: TI AM335x EVM
[    0.000000] cma: Reserved 24 MiB at 0xbe800000
[    0.000000] Memory policy: Data cache writeback
[    0.000000] CPU: All CPU(s) started in SVC mode.
[    0.000000] AM335X ES2.1 (neon )
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 260416
[    0.000000] Kernel command line: console=ttyS0,115200 root=/dev/sda1 rw rootdelay=10
[    0.000000] PID hash table entries: 4096 (order: 2, 16384 bytes)
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes)
[    0.000000] Memory: 1003368K/1048576K available (7107K kernel code, 291K rwdata, 2408K rodata, 280K init, 260K bss, 20632K reserved, 24576K cma-reserved, 237568K highmem)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
[    0.000000]     fixmap  : 0xffc00000 - 0xfff00000   (3072 kB)
[    0.000000]     vmalloc : 0xf0800000 - 0xff800000   ( 240 MB)
[    0.000000]     lowmem  : 0xc0000000 - 0xf0000000   ( 768 MB)
[    0.000000]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
[    0.000000]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)
[    0.000000]       .text : 0xc0008000 - 0xc09530ac   (9517 kB)
[    0.000000]       .init : 0xc0954000 - 0xc099a000   ( 280 kB)
[    0.000000]       .data : 0xc099a000 - 0xc09e2c98   ( 292 kB)
[    0.000000]        .bss : 0xc09e2c98 - 0xc0a23e38   ( 261 kB)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000]  Build-time adjustment of leaf fanout to 32.
[    0.000000] NR_IRQS:16 nr_irqs:16 16
[    0.000000] IRQ: Found an INTC at 0xfa200000 (revision 5.0) with 128 interrupts
[    0.000000] OMAP clockevent source: timer2 at 24000000 Hz
[    0.000012] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 89478484971ns
[    0.000033] clocksource: timer1: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.000042] OMAP clocksource: timer1 at 24000000 Hz
[    0.000197] Console: colour dummy device 80x30
[    0.000230] Calibrating delay loop... 996.14 BogoMIPS (lpj=4980736)
[    0.089240] pid_max: default: 32768 minimum: 301
[    0.089353] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.089364] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.089981] Initializing cgroup subsys io
[    0.090009] Initializing cgroup subsys memory
[    0.090043] Initializing cgroup subsys devices
[    0.090058] Initializing cgroup subsys freezer
[    0.090070] Initializing cgroup subsys perf_event
[    0.090080] Initializing cgroup subsys pids
[    0.090105] CPU: Testing write buffer coherency: ok
[    0.090456] Setting up static identity map for 0x800082c0 - 0x80008318
[    0.092211] devtmpfs: initialized
[    0.103198] VFP support v0.3: implementor 41 architecture 3 part 30 variant c rev 3
[    0.117717] omap_hwmod: debugss: _wait_target_disable failed
[    0.172273] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.174198] pinctrl core: initialized pinctrl subsystem
[    0.175369] NET: Registered protocol family 16
[    0.177067] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.199228] cpuidle: using governor ladder
[    0.229219] cpuidle: using governor menu
[    0.233149] OMAP GPIO hardware version 0.1
[    0.238276] platform 44e3e000.rtc: Cannot lookup hwmod 'rtc'
[    0.240691] omap-gpmc 50000000.gpmc: could not find pctldev for node /ocp/l4_wkup@44c00000/scm@210000/pinmux@800/nandflash_pins_s0, deferring probe
[    0.243270] hw-breakpoint: debug architecture 0x4 unsupported.
[    0.287004] edma 49000000.edma: TI EDMA DMA engine driver
[    0.289923] vgaarb: loaded
[    0.290432] SCSI subsystem initialized
[    0.290709] usbcore: registered new interface driver usbfs
[    0.290773] usbcore: registered new interface driver hub
[    0.290869] usbcore: registered new device driver usb
[    0.291500] omap_i2c 44e0b000.i2c: could not find pctldev for node /ocp/l4_wkup@44c00000/scm@210000/pinmux@800/pinmux_i2c0_pins, deferring probe
[    0.291548] omap_i2c 4802a000.i2c: could not find pctldev for node /ocp/l4_wkup@44c00000/scm@210000/pinmux@800/pinmux_i2c1_pins, deferring probe
[    0.291667] media: Linux media interface: v0.10
[    0.291723] Linux video capture interface: v2.00
[    0.291778] pps_core: LinuxPPS API ver. 1 registered
[    0.291785] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.291812] PTP clock support registered
[    0.292001] EDAC MC: Ver: 3.0.0
[    0.293011] omap-mailbox 480c8000.mailbox: omap mailbox rev 0x400
[    0.293324] Advanced Linux Sound Architecture Driver Initialized.
[    0.294117] clocksource: Switched to clocksource timer1
[    0.303385] NET: Registered protocol family 2
[    0.304055] TCP established hash table entries: 8192 (order: 3, 32768 bytes)
[    0.304192] TCP bind hash table entries: 8192 (order: 3, 32768 bytes)
[    0.304260] TCP: Hash tables configured (established 8192 bind 8192)
[    0.304353] UDP hash table entries: 512 (order: 1, 8192 bytes)
[    0.304375] UDP-Lite hash table entries: 512 (order: 1, 8192 bytes)
[    0.304518] NET: Registered protocol family 1
[    0.304882] RPC: Registered named UNIX socket transport module.
[    0.304896] RPC: Registered udp transport module.
[    0.304902] RPC: Registered tcp transport module.
[    0.304908] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.305793] hw perfevents: enabled with armv7_cortex_a8 PMU driver, 5 counters available
[    0.307464] futex hash table entries: 256 (order: -1, 3072 bytes)
[    0.314018] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.314991] NFS: Registering the id_resolver key type
[    0.315052] Key type id_resolver registered
[    0.315059] Key type id_legacy registered
[    0.315131] ntfs: driver 2.1.32 [Flags: R/O].
[    0.316686] bounce: pool size: 64 pages
[    0.316887] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 248)
[    0.316906] io scheduler noop registered
[    0.316917] io scheduler deadline registered
[    0.317053] io scheduler cfq registered (default)
[    0.318371] pinctrl-single 44e10800.pinmux: bad data for mux matrix_keypad_s0
[    0.318388] pinctrl-single 44e10800.pinmux: no pins entries for matrix_keypad_s0
[    0.318456] pinctrl-single 44e10800.pinmux: 142 pins at pa f9e10800 size 568
[    0.319809] ecap 48300100.ecap: failed to get clock
[    0.319856] ecap: probe of 48300100.ecap failed with error -2
[    0.320587] backlight supply power not found, using dummy regulator
[    0.371312] Serial: 8250/16550 driver, 10 ports, IRQ sharing disabled
[    0.374753] console [ttyS0] disabled
[    0.374838] 44e09000.serial: ttyS0 at MMIO 0x44e09000 (irq = 158, base_baud = 3000000) is a 8250
[    1.036015] console [ttyS0] enabled
[    1.040567] 48022000.serial: ttyS1 at MMIO 0x48022000 (irq = 159, base_baud = 3000000) is a 8250
[    1.050425] [drm] Initialized drm 1.1.0 20060810
[    1.055686] of_graph_get_next_endpoint(): no port node found in /ocp/lcdc@4830e000
[    1.063887] of_graph_get_next_endpoint(): no port node found in /ocp/lcdc@4830e000
[    1.071997] [drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
[    1.078709] [drm] No driver support for vblank timestamp query.
[    1.129077] Console: switching to colour frame buffer device 100x30
[    1.140178] tilcdc 4830e000.lcdc: fb0:  frame buffer device
[    1.174137] [drm] Initialized tilcdc 1.0.0 20121205 on minor 0
[    1.186990] brd: module loaded
[    1.195689] loop: module loaded
[    1.201420] m25p80 spi1.0: found n25q128a13, expected m25p80
[    1.207246] m25p80 spi1.0: n25q128a13 (16384 Kbytes)
[    1.212273] 6 ofpart partitions found on MTD device spi1.0
[    1.217812] Creating 6 MTD partitions on "spi1.0":
[    1.222630] 0x000000000000-0x000000020000 : "MLO"
[    1.228508] 0x000000020000-0x0000000c0000 : "uboot"
[    1.234388] 0x0000000c0000-0x000000100000 : "uboot env"
[    1.240510] 0x000000100000-0x000000900000 : "linux uImage"
[    1.246972] 0x000000900000-0x000000a00000 : "linux dtb"
[    1.253109] 0x000000a00000-0x000001000000 : "user data"
[    1.260478] libphy: Fixed MDIO Bus: probed
[    1.324151] davinci_mdio 4a101000.mdio: davinci mdio revision 1.6
[    1.330286] davinci_mdio 4a101000.mdio: detected phy mask fffffffc
[    1.337881] libphy: 4a101000.mdio: probed
[    1.341923] davinci_mdio 4a101000.mdio: phy[0]: device 4a101000.mdio:00, driver Marvell 88E1512
[    1.350747] davinci_mdio 4a101000.mdio: phy[1]: device 4a101000.mdio:01, driver Marvell 88E1512
[    1.360225] cpsw 4a100000.ethernet: Detected MACID = 00:e0:ee:00:05:2e
[    1.367785] cpsw 4a100000.ethernet: cpsw: Detected MACID = 98:5d:ad:61:51:41
[    1.375571] pegasus: v0.9.3 (2013/04/25), Pegasus/Pegasus II USB Ethernet driver
[    1.383090] usbcore: registered new interface driver pegasus
[    1.388905] usbcore: registered new interface driver r8152
[    1.394498] usbcore: registered new interface driver asix
[    1.399962] usbcore: registered new interface driver ax88179_178a
[    1.406142] usbcore: registered new interface driver cdc_ether
[    1.412053] usbcore: registered new interface driver smsc75xx
[    1.417892] usbcore: registered new interface driver smsc95xx
[    1.423710] usbcore: registered new interface driver net1080
[    1.429450] usbcore: registered new interface driver cdc_subset
[    1.435447] usbcore: registered new interface driver zaurus
[    1.441136] usbcore: registered new interface driver cdc_ncm
[    1.447541] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    1.454150] ehci-pci: EHCI PCI platform driver
[    1.458665] ehci-platform: EHCI generic platform driver
[    1.464085] ehci-omap: OMAP-EHCI Host Controller driver
[    1.469462] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver
[    1.475727] ohci-pci: OHCI PCI platform driver
[    1.480246] ohci-platform: OHCI generic platform driver
[    1.486035] usbcore: registered new interface driver usb-storage
[    1.493476] 47401300.usb-phy supply vcc not found, using dummy regulator
[    1.526292] musb-hdrc musb-hdrc.0.auto: MUSB HDRC host driver
[    1.532089] musb-hdrc musb-hdrc.0.auto: new USB bus registered, assigned bus number 1
[    1.540848] hub 1-0:1.0: USB hub found
[    1.544723] hub 1-0:1.0: 1 port detected
[    1.574825] 47401b00.usb-phy supply vcc not found, using dummy regulator
[    1.606183] musb-hdrc musb-hdrc.1.auto: MUSB HDRC host driver
[    1.611977] musb-hdrc musb-hdrc.1.auto: new USB bus registered, assigned bus number 2
[    1.620694] hub 2-0:1.0: USB hub found
[    1.624569] hub 2-0:1.0: 1 port detected
[    1.660161] mousedev: PS/2 mouse device common for all mice
[    1.666893] i2c /dev entries driver
[    1.671794] /cpus/cpu@0: unsupported enable-method property: ti,am3352
[    1.678482] CPUidle arm: CPU 0 failed to init idle CPU ops
[    1.684071] sdhci: Secure Digital Host Controller Interface driver
[    1.690357] sdhci: Copyright(c) Pierre Ossman
[    1.695332] omap_hsmmc 48060000.mmc: Got CD GPIO
[    1.724417] pinctrl-single 44e10800.pinmux: pin 44e1084c.0 already requested by 4a100000.ethernet; cannot claim for 47810000.mmc
[    1.736240] pinctrl-single 44e10800.pinmux: pin-19 (47810000.mmc) status -22
[    1.743327] pinctrl-single 44e10800.pinmux: could not request pin 19 (44e1084c.0) from group pinmux_mmc3_pins  on device pinctrl-single
[    1.755598] omap_hsmmc 47810000.mmc: Error applying setting, reverse things back
[    1.874433] Synopsys Designware Multimedia Card Interface Driver
[    1.884307] sdhci-pltfm: SDHCI platform and OF driver helper
[    1.891688] ledtrig-cpu: registered to indicate activity on CPUs
[    1.898090] usbcore: registered new interface driver usbhid
[    1.903741] usbhid: USB HID core driver
[    1.911947] NET: Registered protocol family 10
[    1.917808] sit: IPv6 over IPv4 tunneling driver
[    1.923160] NET: Registered protocol family 17
[    1.927837] bridge: automatic filtering via arp/ip/ip6tables has been deprecated. Update your scripts to load br_netfilter if you need this.
[    1.940610] 8021q: 802.1Q VLAN Support v1.8
[    1.944859] usb 1-1: new high-speed USB device number 2 using musb-hdrc
[    1.951650] Key type dns_resolver registered
[    1.956224] omap_voltage_late_init: Voltage driver support not added
[    1.963146] ThumbEE CPU extension supported.
[    1.967605] Registering SWP/SWPB emulation handler
[    1.974538] pinctrl-single 44e10800.pinmux: pin 44e1089c.0 already requested by leds; cannot claim for 50000000.gpmc
[    1.985225] pinctrl-single 44e10800.pinmux: pin-39 (50000000.gpmc) status -22
[    1.992398] pinctrl-single 44e10800.pinmux: could not request pin 39 (44e1089c.0) from group nandflash_pins_s0  on device pinctrl-single
[    2.004856] omap-gpmc 50000000.gpmc: Error applying setting, reverse things back
[    2.012413] omap-gpmc 50000000.gpmc: GPMC revision 6.0
[    2.017692] gpmc_mem_init: disabling cs 0 mapped at 0x0-0x1000000
[    2.024173] usb 2-1: new high-speed USB device number 2 using musb-hdrc
[    2.185456] usb-storage 2-1:1.0: USB Mass Storage device detected
[    2.204514] scsi host0: usb-storage 2-1:1.0
[    2.214207] usb 1-1: reset high-speed USB device number 2 using musb-hdrc
[    2.274336] nand: No NAND device found
[    2.278108] omap2-nand omap2-nand.0: scan failed, may be bus-width mismatch
[    2.304276] tps65910 0-002d: No interrupt support, no core IRQ
[    2.310848] tps65910 0-002d: Error in configuring external control EN1
[    2.317444] tps65910 0-002d: Failed to initialise ext control config
[    2.324096] vrtc: failed to enable
[    2.327629] tps65910 0-002d: failed to register tps65910-pmic regulator
[    2.334304] tps65910-pmic: probe of tps65910-pmic failed with error -121
[    2.341422] omap_i2c 44e0b000.i2c: bus 0 rev0.11 at 400 kHz
[    2.347242] pinctrl-single 44e10800.pinmux: bad data for mux pinmux_i2c1_pins
[    2.354538] pinctrl-single 44e10800.pinmux: no pins entries for pinmux_i2c1_pins
[    2.363249] omap_i2c 4802a000.i2c: bus 1 rev0.11 at 100 kHz
[    2.369180] backlight supply power not found, using dummy regulator
[    2.377107] omap_hsmmc 48060000.mmc: Got CD GPIO
[    2.406348] input: volume_keys@0 as /devices/platform/volume_keys@0/input/input0
[    2.415047] backlight supply power not found, using dummy regulator
[    2.422164] omap_hsmmc 48060000.mmc: Got CD GPIO
[    2.427334] hctosys: unable to open rtc device (rtc0)
[    2.433554] r8152 1-1:1.0 eth2: v1.08.2
[    2.440712] vbat: disabling
[    2.443545] lis3_reg: disabling
[    2.447651] wlan-en-regulator: disabling
[    2.451713] ALSA device list:
[    2.454778]   No soundcards found.
[    2.459181] Waiting 10 sec before mounting root device...
[    2.474803] backlight supply power not found, using dummy regulator
[    2.481853] omap_hsmmc 48060000.mmc: Got CD GPIO
[    3.204917] scsi 0:0:0:0: Direct-Access     ATA      UB31TMM4000YS1-B 0529 PQ: 0 ANSI: 6
[    3.213975] sd 0:0:0:0: [sda] 7733248 512-byte logical blocks: (3.96 GB/3.69 GiB)
[    3.222291] backlight supply power not found, using dummy regulator
[    3.228894] sd 0:0:0:0: [sda] Write Protect is off
[    3.235372] sd 0:0:0:0: [sda] Write cache: enabled, read cache: enabled, doesn't support DPO or FUA
[    3.245229] omap_hsmmc 48060000.mmc: Got CD GPIO
[    3.254826]  sda: sda1
[    3.261088] sd 0:0:0:0: [sda] Attached SCSI disk
[   12.475244] EXT4-fs (sda1): couldn't mount as ext3 due to feature incompatibilities
[   12.483784] EXT4-fs (sda1): mounting ext2 file system using the ext4 subsystem
[   12.505083] EXT4-fs (sda1): warning: mounting unchecked fs, running e2fsck is recommended
[   12.519779] EXT4-fs (sda1): mounted filesystem without journal. Opts: (null)
[   12.526970] VFS: Mounted root (ext2 filesystem) on device 8:1.
[   12.541940] devtmpfs: mounted
[   12.546434] Freeing unused kernel memory: 280K (c0954000 - c099a000)
[   12.789238] random: nonblocking pool is initialized
[   13.055334] systemd[1]: System time before build time, advancing clock.
[   13.110977] systemd[1]: systemd 229 running in system mode. (+PAM -AUDIT -SELINUX +IMA -APPARMOR +SMACK +SYSVINIT +UTMP -LIBCRYPTSETUP -GCRYPT +GNUTLS +ACL +XZ -LZ4 -SECCOMP +BLKID -ELFUTILS +KMOD -IDN)
[   13.129880] systemd[1]: Detected architecture arm.

Welcome to Arago 2016.10!

[   13.155538] systemd[1]: Set hostname to <am335x-evm>.
[   13.515256] systemd[1]: [/lib/systemd/system/gadget-init.service:15] Unknown lvalue 'ExecStopPre' in section 'Service'
[   13.762970] systemd[1]: basic.target: Found ordering cycle on basic.target/start
[   13.770631] systemd[1]: basic.target: Found dependency on sockets.target/start
[   13.778039] systemd[1]: basic.target: Found dependency on avahi-daemon.socket/start
[   13.785809] systemd[1]: basic.target: Found dependency on sysinit.target/start
[   13.793073] systemd[1]: basic.target: Found dependency on alignment.service/start
[   13.800623] systemd[1]: basic.target: Found dependency on basic.target/start
[   13.807725] systemd[1]: basic.target: Breaking ordering cycle by deleting job sockets.target/start
[   13.816786] systemd[1]: sockets.target: Job sockets.target/start deleted to break ordering cycle starting with basic.target/start
[ SKIP ] Ordering cycle found, skipping Sockets
[   13.854797] systemd[1]: alignment.service: Found ordering cycle on alignment.service/start
[   13.863131] systemd[1]: alignment.service: Found dependency on sysinit.target/start
[   13.870917] systemd[1]: alignment.service: Found dependency on alignment.service/start
[   13.878928] systemd[1]: alignment.service: Breaking ordering cycle by deleting job alignment.service/start
[   13.888709] systemd[1]: alignment.service: Job alignment.service/start deleted to break ordering cycle starting with alignment.service/start
[ SKIP ] Ordering cycle found, skipping alignment.service
[   13.956781] systemd[1]: Reached target Swap.
[  OK  ] Reached target Swap.
[   13.986723] systemd[1]: Created slice User and Session Slice.
[  OK  ] Created slice User and Session Slice.
[   14.014554] systemd[1]: Reached target Remote File Systems.
[  OK  ] Reached target Remote File Systems.
[   14.065818] systemd[1]: Listening on Journal Socket (/dev/log).
[  OK  ] Listening on Journal Socket (/dev/log).
[   14.095179] systemd[1]: Listening on Network Service Netlink Socket.
[  OK  ] Listening on Network Service Netlink Socket.
[   14.124702] systemd[1]: Listening on /dev/initctl Compatibility Named Pipe.
[  OK  ] Listening on /dev/initctl Compatibility Named Pipe.
[   14.144636] systemd[1]: Listening on udev Kernel Socket.
[  OK  ] Listening on udev Kernel Socket.
[   14.164737] systemd[1]: Listening on udev Control Socket.
[  OK  ] Listening on udev Control Socket.
[   14.184774] systemd[1]: Listening on Journal Socket.
[  OK  ] Listening on Journal Socket.
[   14.205793] systemd[1]: Created slice System Slice.
[  OK  ] Created slice System Slice.
[   14.235794] systemd[1]: Created slice system-serial\x2dgetty.slice.
[  OK  ] Created slice system-serial\x2dgetty.slice.
[   14.268250] systemd[1]: Mounting Debug File System...
         Mounting Debug File System...
[   14.294813] systemd[1]: Reached target Slices.
[  OK  ] Reached target Slices.
[   14.362709] systemd[1]: Mounting Temporary Directory...
         Mounting Temporary Directory...
[   14.398595] systemd[1]: Starting Setup Virtual Console...
         Starting Setup Virtual Console...
[   14.439206] systemd[1]: Starting Create Static Device Nodes in /dev...
         Starting Create Static Device Nodes in /dev...
[   14.531866] systemd[1]: Starting Remount Root and Kernel File Systems...
         Starting Remount Root and Kernel File Systems...
[   14.658728] systemd[1]: Mounting POSIX Message Queue File System...
         Mounting POSIX Message Queue File System...
[   14.736018] systemd[1]: Created slice system-getty.slice.
[  OK  ] Created slice system-getty.slice.[   14.743266] EXT4-fs (sda1): re-mounted. Opts: (null)

[   14.784808] systemd[1]: Starting Load Kernel Modules...
         Starting Load Kernel Modules...
[   14.805081] systemd[1]: Started Forward Password Requests to Wall Directory Watch.
[  OK  ] Started Forward Password Requests to Wall Directory Watch.
[   14.854877] systemd[1]: Listening on Syslog Socket.
[  OK  ] Listening on Syslog Socket.
[   14.888554] systemd[1]: Starting Journal Service...
         Starting Journal Service...
[   14.927159] systemd[1]: Started Dispatch Password Requests to Console Directory Watch.
[  OK  ] Started Dispatch Password Requests to Console Directory Watch.
[   14.994708] systemd[1]: Reached target Paths.
[  OK  ] Reached target Paths.
[   15.047411] systemd[1]: Mounted POSIX Message Queue File System.
[  OK  ] Mounted POSIX Message Queue File System.
[   15.084879] systemd[1]: Mounted Debug File System.
[  OK  ] Mounted Debug File System.
[   15.114619] systemd[1]: Mounted Temporary Directory.
[  OK  ] Mounted Temporary Directory.
[   15.145231] systemd[1]: Started Journal Service.
[  OK  ] Started Journal Service.
[  OK  ] Started Setup Virtual Console.
[  OK  ] Started Create Static Device Nodes in /dev.
[  OK  ] Started Remount Root and Kernel File Systems.
[FAILED] Failed to start Load Kernel Modules.
See 'systemctl status systemd-modules-load.service' for details.
         Starting Apply Kernel Variables...
         Starting udev Coldplug all Devices...
[  OK  ] Reached target Local File Systems (Pre).
         Mounting /media/ram...
         Mounting /var/volatile...
         Starting udev Kernel Device Manager...
         Starting Flush Journal to Persistent Storage...
[  OK  ] Mounted /var/volatile.
[  OK  ] Mounted /media/ram.
[  OK  ] Started Apply Kernel Variables.
[  OK  ] Started udev Kernel Device Manager.
[   17.369741] systemd-journald[117]: Received request to flush runtime journal from PID 1
[  OK  ] Started Flush Journal to Persistent Storage.
         Starting Load/Save Random Seed...
[  OK  ] Reached target Local File Systems.
         Starting Create Volatile Files and Directories...
[  OK  ] Started Load/Save Random Seed.
[  OK  ] Started Create Volatile Files and Directories.
         Starting Update UTMP about System Boot/Shutdown...
         Starting Network Time Synchronization...
[  OK  ] Found device /dev/ttyS0.
[  OK  ] Started udev Coldplug all Devices.
[  OK  ] Started Network Time Synchronization.
[  OK  ] Started Update UTMP about System Boot/Shutdown.
[  OK  ] Found device /dev/ttyS3.
         Starting Synchronize System and HW clocks...
[  OK  ] Reached target System Time Synchronized.
[FAILED] Failed to start Synchronize System and HW clocks.
See 'systemctl status sync-clocks.service' for details.
[  OK  ] Reached target System Initialization.
[  OK  ] Reached target Basic System.
         Starting Permit User Sessions...
[  OK  ] Started strongSwan IPsec IKEv1/IKEv2 daemon using ipsec.conf.
[  OK  ] Listening on D-Bus System Message Bus Socket.
[  OK  ] Started Kernel Logging Service.
         Starting Telephony service...
[  OK  ] Listening on dropbear.socket.
         Starting Print notice about GPLv3 packages...
[  OK  ] Listening on RPCbind Server Activation Socket.
[  OK  ] Started D-Bus System Message Bus.
[  OK  ] Started Telephony service.
         Starting Network Service...
         Starting Login Service...
[  OK  ] Listening on Avahi mDNS/DNS-SD Stack Activation Socket.
         Starting Avahi mDNS/DNS-SD Stack...
[  OK  ] Started System Logging Service.
         Starting uim-sysfs.service...
[  OK  ] Started Daily Cleanup of Temporary Directories.
[  OK  ] Reached target Timers.
[  OK  ] Started Permit User Sessions.
[  OK  ] Started Network Service.
[   25.394568] IPv6: ADDRCONF(NETDEV_UP): eth2: link is not ready
[   25.540812] net eth1: initializing cpsw version 1.12 (0)
[   25.675827] net eth1: phy found : id is : 0x1410dd1
[   25.791890] IPv6: ADDRCONF(NETDEV_UP): eth1: link is not ready
[   25.863986] 8021q: adding VLAN 0 to HW filter on device eth1
[   25.967380] net eth0: initializing cpsw version 1.12 (0)
[   26.125621] net eth0: phy found : id is : 0x1410dd1
[   26.193347] IPv6: ADDRCONF(NETDEV_UP): eth0: link is not ready
[   26.278419] 8021q: adding VLAN 0 to HW filter on device eth0
[   29.674903] cpsw 4a100000.ethernet eth1: Link is Up - 1Gbps/Full - flow control off
[   29.717969] IPv6: ADDRCONF(NETDEV_CHANGE): eth1: link becomes ready
[   30.124960] cpsw 4a100000.ethernet eth0: Link is Up - 1Gbps/Full - flow control off
[   30.164722] IPv6: ADDRCONF(NETDEV_CHANGE): eth0: link becomes ready
***************************************************************
***************************************************************
NOTICE: This file system contains the following GPLv3 packages:
        autoconf
        binutils
        bison-dev
        bison
        cpp-symlinks
        cpp
        dosfstools
        g++-symlinks
        g++
        gawk-dev
        gawk
        gcc-symlinks
        gcc
        gdb
        gdbserver
        gstreamer1.0-libav
        hidapi
        libcairo-perf-utils
        libgmp10
        libidn11
        libmpc3
        libmpfr4
        m4-dev
        m4
        make
        nettle
        swig-dev
        swig

If you do not wish to distribute GPLv3 components please remove
the above packages prior to distribution.  This can be done using
the opkg remove command.  i.e.:
    opkg remove <package>
Where <package> is the name printed in the list above

NOTE: If the package is a dependency of another package you
      will be notified of the dependent packages.  You should
      use the --force-removal-of-dependent-packages option to
      also remove the dependent packages as well
***************************************************************
***************************************************************
[  OK  ] Started Print notice about GPLv3 packages.
[  OK  ] Started uim-sysfs.service.
[  OK  ] Started Avahi mDNS/DNS-SD Stack.
[  OK  ] Started Login Service.
         Starting rc.pvr.service...
[  OK  ] Reached target Network.
         Starting Lightning Fast Webserver With Light System Requirements...
         Starting Network Name Resolution...
[  OK  ] Started Serial Getty on ttyS3.
[  OK  ] Started Getty on tty1.
[  OK  ] Started Serial Getty on ttyS0.
[  OK  ] Started rc.pvr.service.
[  OK  ] Started Lightning Fast Webserver With Light System Requirements.
[  OK  ] Started Network Name Resolution.
         Starting weston.service...
[  OK  ] Started weston.service.
         Starting telnetd.service...
[  OK  ] Started telnetd.service.
         Starting busybox-udhcpd.service...
         Starting thttpd.service...
[  OK  ] Started busybox-udhcpd.service.
         Starting rng-tools.service...
[  OK  ] Started rng-tools.service.
         Starting matrix-gui-2.0.service...
[  OK  ] Started matrix-gui-2.0.service.
         Starting thermal-zone-init.service...
         Starting parse-ip.service...
[  OK  ] Started thermal-zone-init.service.
[  OK  ] Started parse-ip.service.

 _____                    _____           _         _   
|  _  |___ ___ ___ ___   |  _  |___ ___  |_|___ ___| |_ 
|     |  _| .'| . | . |  |   __|  _| . | | | -_|  _|  _|
|__|__|_| |__,|_  |___|  |__|  |_| |___|_| |___|___|_|  
              |___|                    |___|            

Arago Project http://arago-project.org am335x-evm ttyS0

Arago 2016.10 am335x-evm ttyS0

am335x-evm login: root
root@am335x-evm:~# 