/*
 * Copyright (C) 2013 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */

#include "dra7-evm.dts"

&pcf_gpio_21 {
	status = "disabled";
};

&evm_3v3_sd {
	gpio = <>;
};

&extcon_usb1 {
	id-gpio = <>;
};

&extcon_usb2 {
	id-gpio = <>;
};

/ {
	chosen {
		stdout-path = &uart4;
	};

	memory {
		reg = <0x80000000 0x10000000>; /* 256 MB */
	};
};

&uart4 {
 	status = "okay";
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart4_pins>;
};

&dra7_pmx_core {
	uart4_pins: pinmux_uart4_pins {
		pinctrl-single,pins = <
		0x33C (PIN_INPUT_SLEW | MUX_MODE4) /* uart4_rxd */
		0x340 (PIN_INPUT_SLEW | MUX_MODE4) /* uart4_txd */
		>;
	};
};