[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 4.14.40 (root@andy-Aspire-E5-571G) (gcc version 7.4.0 (Buildroot 2019.02-git-g89a55c58ae-dirty)) #4 SMP Fri Mar 15 12:15:31 MSK 2019
[    0.000000] CPU: ARMv7 Processor [413fc082] revision 2 (ARMv7), cr=10c5387d
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] OF: fdt: Machine model: TI AM335x BeagleBone Black
[    0.000000] Memory policy: Data cache writeback
[    0.000000] cma: Reserved 16 MiB at 0x9e800000
[    0.000000] On node 0 totalpages: 130560
[    0.000000] free_area_init_node: node 0, pgdat c17c5480, node_mem_map df971000
[    0.000000]   Normal zone: 1148 pages used for memmap
[    0.000000]   Normal zone: 0 pages reserved
[    0.000000]   Normal zone: 130560 pages, LIFO batch:31
[    0.000000] CPU: All CPU(s) started in SVC mode.
[    0.000000] AM335X ES2.1 (sgx neon)
[    0.000000] percpu: Embedded 17 pages/cpu @df93c000 s40872 r8192 d20568 u69632
[    0.000000] pcpu-alloc: s40872 r8192 d20568 u69632 alloc=17*4096
[    0.000000] pcpu-alloc: [0] 0 
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 129412
[    0.000000] Kernel command line: root=/dev/ram rw rootwait console=ttyO0,115200
[    0.000000] PID hash table entries: 2048 (order: 1, 8192 bytes)
[    0.000000] Dentry cache hash table entries: 65536 (order: 6, 262144 bytes)
[    0.000000] Inode-cache hash table entries: 32768 (order: 5, 131072 bytes)
[    0.000000] Memory: 469632K/522240K available (8192K kernel code, 818K rwdata, 2424K rodata, 11264K init, 7548K bss, 36224K reserved, 16384K cma-reserved, 0K highmem)
[    0.000000] Virtual kernel memory layout:
[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
[    0.000000]     fixmap  : 0xffc00000 - 0xfff00000   (3072 kB)
[    0.000000]     vmalloc : 0xe0000000 - 0xff800000   ( 504 MB)
[    0.000000]     lowmem  : 0xc0000000 - 0xdfe00000   ( 510 MB)
[    0.000000]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
[    0.000000]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)
[    0.000000]       .text : 0xc0008000 - 0xc0900000   (9184 kB)
[    0.000000]       .init : 0xc0c00000 - 0xc1700000   (11264 kB)
[    0.000000]       .data : 0xc1700000 - 0xc17cc838   ( 819 kB)
[    0.000000]        .bss : 0xc17ce000 - 0xc1f2d094   (7549 kB)
[    0.000000] Running RCU self tests
[    0.000000] Hierarchical RCU implementation.
[    0.000000] 	RCU event tracing is enabled.
[    0.000000] 	RCU lockdep checking is enabled.
[    0.000000] 	RCU restricting CPUs from NR_CPUS=2 to nr_cpu_ids=1.
[    0.000000] RCU: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=1
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] IRQ: Found an INTC at 0xfa200000 (revision 5.0) with 128 interrupts
[    0.000000] OMAP clockevent source: timer2 at 24000000 Hz
[    0.000018] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 89478484971ns
[    0.000048] clocksource: timer1: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.000106] OMAP clocksource: timer1 at 24000000 Hz
[    0.000658] timer_probe: no matching timers found
[    0.001638] Console: colour dummy device 80x30
[    0.001691] Lock dependency validator: Copyright (c) 2006 Red Hat, Inc., Ingo Molnar
[    0.001704] ... MAX_LOCKDEP_SUBCLASSES:  8
[    0.001716] ... MAX_LOCK_DEPTH:          48
[    0.001728] ... MAX_LOCKDEP_KEYS:        8191
[    0.001740] ... CLASSHASH_SIZE:          4096
[    0.001753] ... MAX_LOCKDEP_ENTRIES:     32768
[    0.001765] ... MAX_LOCKDEP_CHAINS:      65536
[    0.001777] ... CHAINHASH_SIZE:          32768
[    0.001788]  memory used by lock dependency info: 4655 kB
[    0.001801]  per task-struct memory footprint: 1536 bytes
[    0.001837] Calibrating delay loop... 996.14 BogoMIPS (lpj=4980736)
[    0.078604] pid_max: default: 32768 minimum: 301
[    0.079034] Security Framework initialized
[    0.079180] Mount-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.079204] Mountpoint-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.082506] CPU: Testing write buffer coherency: ok
[    0.084152] CPU0: thread -1, cpu 0, socket -1, mpidr 0
[    0.085784] Setting up static identity map for 0x80100000 - 0x80100078
[    0.086401] Hierarchical SRCU implementation.
[    0.088119] smp: Bringing up secondary CPUs ...
[    0.088143] smp: Brought up 1 node, 1 CPU
[    0.088160] SMP: Total of 1 processors activated (996.14 BogoMIPS).
[    0.088175] CPU: All CPU(s) started in SVC mode.
[    0.092398] devtmpfs: initialized
[    0.119092] random: get_random_u32 called from bucket_table_alloc+0xe4/0x23c with crng_init=0
[    0.120176] VFP support v0.3: implementor 41 architecture 3 part 30 variant c rev 3
[    0.121002] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.121075] futex hash table entries: 256 (order: 2, 16384 bytes)
[    0.122957] pinctrl core: initialized pinctrl subsystem
[    0.124732] reg-dummy reg-dummy: no of_node; not parsing pinctrl DT
[    0.127769] NET: Registered protocol family 16
[    0.135269] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.172173] omap_hwmod: tptc0 using broken dt data from edma
[    0.172677] omap_hwmod: tptc1 using broken dt data from edma
[    0.173151] omap_hwmod: tptc2 using broken dt data from edma
[    0.233961] cpuidle: using governor menu
[    0.243411] gpio gpiochip0: (gpio): added GPIO chardev (254:0)
[    0.243842] gpiochip_setup_dev: registered GPIOs 0 to 31 on device: gpiochip0 (gpio)
[    0.244094] OMAP GPIO hardware version 0.1
[    0.246362] gpio gpiochip1: (gpio): added GPIO chardev (254:1)
[    0.246607] gpiochip_setup_dev: registered GPIOs 32 to 63 on device: gpiochip1 (gpio)
[    0.248835] gpio gpiochip2: (gpio): added GPIO chardev (254:2)
[    0.249073] gpiochip_setup_dev: registered GPIOs 64 to 95 on device: gpiochip2 (gpio)
[    0.251157] gpio gpiochip3: (gpio): added GPIO chardev (254:3)
[    0.251375] gpiochip_setup_dev: registered GPIOs 96 to 127 on device: gpiochip3 (gpio)
[    0.272088] No ATAGs?
[    0.272117] hw-breakpoint: debug architecture 0x4 unsupported.
[    0.272476] omap4_sram_init:Unable to allocate sram needed to handle errata I688
[    0.272498] omap4_sram_init:Unable to get sram pool needed to handle errata I688
[    0.296990] edma 49000000.edma: Legacy memcpy is enabled, things might not work
[    0.308249] edma 49000000.edma: TI EDMA DMA engine driver
[    0.309434] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/fixedregulator@0[0]'
[    0.313942] SCSI subsystem initialized
[    0.315043] libata version 3.00 loaded.
[    0.315879] omap_i2c 44e0b000.i2c: could not find pctldev for node /ocp/l4_wkup@44c00000/scm@210000/pinmux@800/pinmux_i2c0_pins, deferring probe
[    0.316234] pps_core: LinuxPPS API ver. 1 registered
[    0.316251] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.316302] PTP clock support registered
[    0.320781] clocksource: Switched to clocksource timer1
[    0.458174] VFS: Disk quotas dquot_6.6.0
[    0.458387] VFS: Dquot-cache hash table entries: 1024 (order 0, 4096 bytes)
[    0.483529] NET: Registered protocol family 2
[    0.485521] TCP established hash table entries: 4096 (order: 2, 16384 bytes)
[    0.485633] TCP bind hash table entries: 4096 (order: 5, 147456 bytes)
[    0.486804] TCP: Hash tables configured (established 4096 bind 4096)
[    0.487265] UDP hash table entries: 256 (order: 2, 20480 bytes)
[    0.487450] UDP-Lite hash table entries: 256 (order: 2, 20480 bytes)
[    0.488222] NET: Registered protocol family 1
[    0.490526] RPC: Registered named UNIX socket transport module.
[    0.490577] RPC: Registered udp transport module.
[    0.490591] RPC: Registered tcp transport module.
[    0.490787] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    1.681610] hw perfevents: no interrupt-affinity property for /pmu, guessing.
[    1.682763] hw perfevents: enabled with armv7_cortex_a8 PMU driver, 5 counters available
[    1.684602] alarmtimer alarmtimer: no of_node; not parsing pinctrl DT
[    1.685449] audit: initializing netlink subsys (disabled)
[    1.688171] audit: type=2000 audit(1.680:1): state=initialized audit_enabled=0 res=1
[    1.688537] workingset: timestamp_bits=14 max_order=17 bucket_order=3
[    1.691998] NFS: Registering the id_resolver key type
[    1.692430] Key type id_resolver registered
[    1.692471] Key type id_legacy registered
[    1.692631] jffs2: version 2.2. (NAND) (SUMMARY)  © 2001-2006 Red Hat, Inc.
[    1.699387] io scheduler noop registered
[    1.699420] io scheduler deadline registered
[    1.699561] io scheduler cfq registered (default)
[    1.699580] io scheduler mq-deadline registered
[    1.699596] io scheduler kyber registered
[    1.701310] pinctrl-single 44e10800.pinmux: please update dts to use #pinctrl-cells = <1>
[    1.701442] pinctrl-single 44e10800.pinmux: allocating 142 pins
[    1.701490] pinctrl-single 44e10800.pinmux: try to register 142 pins ...
[    1.701512] pinctrl core: registered pin 0 (PIN0) on pinctrl-single
[    1.701532] pinctrl core: registered pin 1 (PIN1) on pinctrl-single
[    1.701546] pinctrl core: registered pin 2 (PIN2) on pinctrl-single
[    1.701560] pinctrl core: registered pin 3 (PIN3) on pinctrl-single
[    1.701574] pinctrl core: registered pin 4 (PIN4) on pinctrl-single
[    1.701588] pinctrl core: registered pin 5 (PIN5) on pinctrl-single
[    1.701601] pinctrl core: registered pin 6 (PIN6) on pinctrl-single
[    1.701615] pinctrl core: registered pin 7 (PIN7) on pinctrl-single
[    1.701629] pinctrl core: registered pin 8 (PIN8) on pinctrl-single
[    1.701643] pinctrl core: registered pin 9 (PIN9) on pinctrl-single
[    1.701657] pinctrl core: registered pin 10 (PIN10) on pinctrl-single
[    1.701671] pinctrl core: registered pin 11 (PIN11) on pinctrl-single
[    1.701685] pinctrl core: registered pin 12 (PIN12) on pinctrl-single
[    1.701699] pinctrl core: registered pin 13 (PIN13) on pinctrl-single
[    1.701713] pinctrl core: registered pin 14 (PIN14) on pinctrl-single
[    1.701727] pinctrl core: registered pin 15 (PIN15) on pinctrl-single
[    1.701741] pinctrl core: registered pin 16 (PIN16) on pinctrl-single
[    1.701755] pinctrl core: registered pin 17 (PIN17) on pinctrl-single
[    1.701769] pinctrl core: registered pin 18 (PIN18) on pinctrl-single
[    1.701783] pinctrl core: registered pin 19 (PIN19) on pinctrl-single
[    1.701798] pinctrl core: registered pin 20 (PIN20) on pinctrl-single
[    1.701812] pinctrl core: registered pin 21 (PIN21) on pinctrl-single
[    1.701826] pinctrl core: registered pin 22 (PIN22) on pinctrl-single
[    1.701840] pinctrl core: registered pin 23 (PIN23) on pinctrl-single
[    1.701854] pinctrl core: registered pin 24 (PIN24) on pinctrl-single
[    1.701869] pinctrl core: registered pin 25 (PIN25) on pinctrl-single
[    1.701883] pinctrl core: registered pin 26 (PIN26) on pinctrl-single
[    1.701897] pinctrl core: registered pin 27 (PIN27) on pinctrl-single
[    1.701912] pinctrl core: registered pin 28 (PIN28) on pinctrl-single
[    1.701929] pinctrl core: registered pin 29 (PIN29) on pinctrl-single
[    1.701943] pinctrl core: registered pin 30 (PIN30) on pinctrl-single
[    1.701957] pinctrl core: registered pin 31 (PIN31) on pinctrl-single
[    1.701971] pinctrl core: registered pin 32 (PIN32) on pinctrl-single
[    1.701985] pinctrl core: registered pin 33 (PIN33) on pinctrl-single
[    1.701999] pinctrl core: registered pin 34 (PIN34) on pinctrl-single
[    1.702013] pinctrl core: registered pin 35 (PIN35) on pinctrl-single
[    1.702028] pinctrl core: registered pin 36 (PIN36) on pinctrl-single
[    1.702042] pinctrl core: registered pin 37 (PIN37) on pinctrl-single
[    1.702056] pinctrl core: registered pin 38 (PIN38) on pinctrl-single
[    1.702070] pinctrl core: registered pin 39 (PIN39) on pinctrl-single
[    1.702084] pinctrl core: registered pin 40 (PIN40) on pinctrl-single
[    1.702098] pinctrl core: registered pin 41 (PIN41) on pinctrl-single
[    1.702112] pinctrl core: registered pin 42 (PIN42) on pinctrl-single
[    1.702127] pinctrl core: registered pin 43 (PIN43) on pinctrl-single
[    1.702141] pinctrl core: registered pin 44 (PIN44) on pinctrl-single
[    1.702155] pinctrl core: registered pin 45 (PIN45) on pinctrl-single
[    1.702169] pinctrl core: registered pin 46 (PIN46) on pinctrl-single
[    1.702183] pinctrl core: registered pin 47 (PIN47) on pinctrl-single
[    1.702197] pinctrl core: registered pin 48 (PIN48) on pinctrl-single
[    1.702219] pinctrl core: registered pin 49 (PIN49) on pinctrl-single
[    1.702233] pinctrl core: registered pin 50 (PIN50) on pinctrl-single
[    1.702247] pinctrl core: registered pin 51 (PIN51) on pinctrl-single
[    1.702261] pinctrl core: registered pin 52 (PIN52) on pinctrl-single
[    1.702275] pinctrl core: registered pin 53 (PIN53) on pinctrl-single
[    1.702289] pinctrl core: registered pin 54 (PIN54) on pinctrl-single
[    1.702303] pinctrl core: registered pin 55 (PIN55) on pinctrl-single
[    1.702317] pinctrl core: registered pin 56 (PIN56) on pinctrl-single
[    1.702331] pinctrl core: registered pin 57 (PIN57) on pinctrl-single
[    1.702345] pinctrl core: registered pin 58 (PIN58) on pinctrl-single
[    1.702359] pinctrl core: registered pin 59 (PIN59) on pinctrl-single
[    1.702373] pinctrl core: registered pin 60 (PIN60) on pinctrl-single
[    1.702387] pinctrl core: registered pin 61 (PIN61) on pinctrl-single
[    1.702401] pinctrl core: registered pin 62 (PIN62) on pinctrl-single
[    1.702416] pinctrl core: registered pin 63 (PIN63) on pinctrl-single
[    1.702433] pinctrl core: registered pin 64 (PIN64) on pinctrl-single
[    1.702447] pinctrl core: registered pin 65 (PIN65) on pinctrl-single
[    1.702461] pinctrl core: registered pin 66 (PIN66) on pinctrl-single
[    1.702476] pinctrl core: registered pin 67 (PIN67) on pinctrl-single
[    1.702490] pinctrl core: registered pin 68 (PIN68) on pinctrl-single
[    1.702504] pinctrl core: registered pin 69 (PIN69) on pinctrl-single
[    1.702518] pinctrl core: registered pin 70 (PIN70) on pinctrl-single
[    1.702532] pinctrl core: registered pin 71 (PIN71) on pinctrl-single
[    1.702546] pinctrl core: registered pin 72 (PIN72) on pinctrl-single
[    1.702560] pinctrl core: registered pin 73 (PIN73) on pinctrl-single
[    1.702574] pinctrl core: registered pin 74 (PIN74) on pinctrl-single
[    1.702588] pinctrl core: registered pin 75 (PIN75) on pinctrl-single
[    1.702602] pinctrl core: registered pin 76 (PIN76) on pinctrl-single
[    1.702616] pinctrl core: registered pin 77 (PIN77) on pinctrl-single
[    1.702630] pinctrl core: registered pin 78 (PIN78) on pinctrl-single
[    1.702646] pinctrl core: registered pin 79 (PIN79) on pinctrl-single
[    1.702660] pinctrl core: registered pin 80 (PIN80) on pinctrl-single
[    1.702681] pinctrl core: registered pin 81 (PIN81) on pinctrl-single
[    1.702695] pinctrl core: registered pin 82 (PIN82) on pinctrl-single
[    1.702710] pinctrl core: registered pin 83 (PIN83) on pinctrl-single
[    1.702724] pinctrl core: registered pin 84 (PIN84) on pinctrl-single
[    1.702738] pinctrl core: registered pin 85 (PIN85) on pinctrl-single
[    1.702752] pinctrl core: registered pin 86 (PIN86) on pinctrl-single
[    1.702766] pinctrl core: registered pin 87 (PIN87) on pinctrl-single
[    1.702780] pinctrl core: registered pin 88 (PIN88) on pinctrl-single
[    1.702795] pinctrl core: registered pin 89 (PIN89) on pinctrl-single
[    1.702809] pinctrl core: registered pin 90 (PIN90) on pinctrl-single
[    1.702823] pinctrl core: registered pin 91 (PIN91) on pinctrl-single
[    1.702837] pinctrl core: registered pin 92 (PIN92) on pinctrl-single
[    1.702851] pinctrl core: registered pin 93 (PIN93) on pinctrl-single
[    1.702865] pinctrl core: registered pin 94 (PIN94) on pinctrl-single
[    1.702879] pinctrl core: registered pin 95 (PIN95) on pinctrl-single
[    1.702893] pinctrl core: registered pin 96 (PIN96) on pinctrl-single
[    1.702907] pinctrl core: registered pin 97 (PIN97) on pinctrl-single
[    1.702921] pinctrl core: registered pin 98 (PIN98) on pinctrl-single
[    1.702935] pinctrl core: registered pin 99 (PIN99) on pinctrl-single
[    1.702950] pinctrl core: registered pin 100 (PIN100) on pinctrl-single
[    1.702964] pinctrl core: registered pin 101 (PIN101) on pinctrl-single
[    1.702978] pinctrl core: registered pin 102 (PIN102) on pinctrl-single
[    1.702993] pinctrl core: registered pin 103 (PIN103) on pinctrl-single
[    1.703007] pinctrl core: registered pin 104 (PIN104) on pinctrl-single
[    1.703021] pinctrl core: registered pin 105 (PIN105) on pinctrl-single
[    1.703035] pinctrl core: registered pin 106 (PIN106) on pinctrl-single
[    1.703049] pinctrl core: registered pin 107 (PIN107) on pinctrl-single
[    1.703063] pinctrl core: registered pin 108 (PIN108) on pinctrl-single
[    1.703077] pinctrl core: registered pin 109 (PIN109) on pinctrl-single
[    1.703092] pinctrl core: registered pin 110 (PIN110) on pinctrl-single
[    1.703107] pinctrl core: registered pin 111 (PIN111) on pinctrl-single
[    1.703122] pinctrl core: registered pin 112 (PIN112) on pinctrl-single
[    1.703143] pinctrl core: registered pin 113 (PIN113) on pinctrl-single
[    1.703157] pinctrl core: registered pin 114 (PIN114) on pinctrl-single
[    1.703172] pinctrl core: registered pin 115 (PIN115) on pinctrl-single
[    1.703186] pinctrl core: registered pin 116 (PIN116) on pinctrl-single
[    1.703200] pinctrl core: registered pin 117 (PIN117) on pinctrl-single
[    1.703214] pinctrl core: registered pin 118 (PIN118) on pinctrl-single
[    1.703228] pinctrl core: registered pin 119 (PIN119) on pinctrl-single
[    1.703242] pinctrl core: registered pin 120 (PIN120) on pinctrl-single
[    1.703256] pinctrl core: registered pin 121 (PIN121) on pinctrl-single
[    1.703271] pinctrl core: registered pin 122 (PIN122) on pinctrl-single
[    1.703285] pinctrl core: registered pin 123 (PIN123) on pinctrl-single
[    1.703299] pinctrl core: registered pin 124 (PIN124) on pinctrl-single
[    1.703313] pinctrl core: registered pin 125 (PIN125) on pinctrl-single
[    1.703327] pinctrl core: registered pin 126 (PIN126) on pinctrl-single
[    1.703341] pinctrl core: registered pin 127 (PIN127) on pinctrl-single
[    1.703357] pinctrl core: registered pin 128 (PIN128) on pinctrl-single
[    1.703371] pinctrl core: registered pin 129 (PIN129) on pinctrl-single
[    1.703385] pinctrl core: registered pin 130 (PIN130) on pinctrl-single
[    1.703399] pinctrl core: registered pin 131 (PIN131) on pinctrl-single
[    1.703414] pinctrl core: registered pin 132 (PIN132) on pinctrl-single
[    1.703428] pinctrl core: registered pin 133 (PIN133) on pinctrl-single
[    1.703442] pinctrl core: registered pin 134 (PIN134) on pinctrl-single
[    1.703456] pinctrl core: registered pin 135 (PIN135) on pinctrl-single
[    1.703470] pinctrl core: registered pin 136 (PIN136) on pinctrl-single
[    1.703484] pinctrl core: registered pin 137 (PIN137) on pinctrl-single
[    1.703498] pinctrl core: registered pin 138 (PIN138) on pinctrl-single
[    1.703513] pinctrl core: registered pin 139 (PIN139) on pinctrl-single
[    1.703527] pinctrl core: registered pin 140 (PIN140) on pinctrl-single
[    1.703541] pinctrl core: registered pin 141 (PIN141) on pinctrl-single
[    1.703652] pinctrl-single 44e10800.pinmux: 142 pins at pa f9e10800 size 568
[    1.703683] pinctrl-single 44e10800.pinmux: no hogs found
[    1.705784] platform 48300100.ecap: Cannot lookup hwmod 'ecap0'
[    1.710154] Serial: 8250/16550 driver, 6 ports, IRQ sharing enabled
[    1.715137] serial8250 serial8250: no of_node; not parsing pinctrl DT
[    1.716169] pinctrl-single 44e10800.pinmux: pinmux_uart0_pins index: 0x170 value: 0x30
[    1.716190] pinctrl-single 44e10800.pinmux: pinmux_uart0_pins index: 0x174 value: 0x0
[    1.716220] pinctrl core: add 1 pinctrl maps
[    1.716350] pinctrl-single 44e10800.pinmux: found group selector 0 for pinmux_uart0_pins
[    1.716399] pinctrl-single 44e10800.pinmux: request pin 92 (PIN92) for 44e09000.serial
[    1.716414] pinctrl-single 44e10800.pinmux: request pin 93 (PIN93) for 44e09000.serial
[    1.716430] pinctrl-single 44e10800.pinmux: enabling (null) function0
[    1.716874] omap_uart 44e09000.serial: no wakeirq for uart0
[    1.716915] of_get_named_gpiod_flags: can't parse 'rts-gpio' property of node '/ocp/serial@44e09000[0]'
[    1.717465] 44e09000.serial: ttyO0 at MMIO 0x44e09000 (irq = 27, base_baud = 3000000) is a OMAP UART0
[    2.468082] console [ttyO0] enabled
[    2.473316] pinctrl-single 44e10800.pinmux: pinmux_uart1_pins index: 0x180 value: 0x30
[    2.473340] pinctrl-single 44e10800.pinmux: pinmux_uart1_pins index: 0x184 value: 0x0
[    2.473377] pinctrl core: add 1 pinctrl maps
[    2.473422] pinctrl-single 44e10800.pinmux: found group selector 1 for pinmux_uart1_pins
[    2.473447] pinctrl-single 44e10800.pinmux: request pin 96 (PIN96) for 48022000.serial
[    2.473462] pinctrl-single 44e10800.pinmux: request pin 97 (PIN97) for 48022000.serial
[    2.473478] pinctrl-single 44e10800.pinmux: enabling (null) function1
[    2.473714] omap_uart 48022000.serial: no wakeirq for uart1
[    2.479581] of_get_named_gpiod_flags: can't parse 'rts-gpio' property of node '/ocp/serial@48022000[0]'
[    2.479908] 48022000.serial: ttyO1 at MMIO 0x48022000 (irq = 28, base_baud = 3000000) is a OMAP UART1
[    2.490778] pinctrl-single 44e10800.pinmux: pinmux_uart2_pins index: 0x10c value: 0x36
[    2.490801] pinctrl-single 44e10800.pinmux: pinmux_uart2_pins index: 0x110 value: 0x6
[    2.490844] pinctrl core: add 1 pinctrl maps
[    2.490888] pinctrl-single 44e10800.pinmux: found group selector 2 for pinmux_uart2_pins
[    2.490911] pinctrl-single 44e10800.pinmux: request pin 67 (PIN67) for 48024000.serial
[    2.490925] pinctrl-single 44e10800.pinmux: request pin 68 (PIN68) for 48024000.serial
[    2.490939] pinctrl-single 44e10800.pinmux: enabling (null) function2
[    2.491144] omap_uart 48024000.serial: no wakeirq for uart2
[    2.496987] of_get_named_gpiod_flags: can't parse 'rts-gpio' property of node '/ocp/serial@48024000[0]'
[    2.497280] 48024000.serial: ttyO2 at MMIO 0x48024000 (irq = 29, base_baud = 3000000) is a OMAP UART2
[    2.507905] pinctrl-single 44e10800.pinmux: pinmux_uart4_pins index: 0x168 value: 0x31
[    2.507925] pinctrl-single 44e10800.pinmux: pinmux_uart4_pins index: 0x16c value: 0x1
[    2.507950] pinctrl core: add 1 pinctrl maps
[    2.507990] pinctrl-single 44e10800.pinmux: found group selector 3 for pinmux_uart4_pins
[    2.508011] pinctrl-single 44e10800.pinmux: request pin 90 (PIN90) for 481a8000.serial
[    2.508024] pinctrl-single 44e10800.pinmux: request pin 91 (PIN91) for 481a8000.serial
[    2.508039] pinctrl-single 44e10800.pinmux: enabling (null) function3
[    2.508225] omap_uart 481a8000.serial: no wakeirq for uart4
[    2.514185] of_get_named_gpiod_flags: can't parse 'rts-gpio' property of node '/ocp/serial@481a8000[0]'
[    2.514483] 481a8000.serial: ttyO4 at MMIO 0x481a8000 (irq = 30, base_baud = 3000000) is a OMAP UART4
[    2.554807] brd: module loaded
[    2.584588] loop: module loaded
[    2.590563] mtdoops: mtd device (mtddev=name/number) must be supplied
[    2.599051] pinctrl-single 44e10800.pinmux: pinmux_spi0 index: 0x150 value: 0x30
[    2.599073] pinctrl-single 44e10800.pinmux: pinmux_spi0 index: 0x154 value: 0x10
[    2.599088] pinctrl-single 44e10800.pinmux: pinmux_spi0 index: 0x158 value: 0x30
[    2.599103] pinctrl-single 44e10800.pinmux: pinmux_spi0 index: 0x15c value: 0x10
[    2.599135] pinctrl core: add 1 pinctrl maps
[    2.599186] pinctrl-single 44e10800.pinmux: found group selector 4 for pinmux_spi0
[    2.599213] pinctrl-single 44e10800.pinmux: request pin 84 (PIN84) for 48030000.spi
[    2.599227] pinctrl-single 44e10800.pinmux: request pin 85 (PIN85) for 48030000.spi
[    2.599240] pinctrl-single 44e10800.pinmux: request pin 86 (PIN86) for 48030000.spi
[    2.599252] pinctrl-single 44e10800.pinmux: request pin 87 (PIN87) for 48030000.spi
[    2.599268] pinctrl-single 44e10800.pinmux: enabling (null) function4
[    2.604204] mdio_bus fixed-0: GPIO lookup for consumer reset
[    2.604227] mdio_bus fixed-0: using lookup tables for GPIO lookup
[    2.604327] mdio_bus fixed-0: lookup for GPIO reset failed
[    2.604547] libphy: Fixed MDIO Bus: probed
[    2.612080] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x114 value: 0x2
[    2.612102] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x118 value: 0x22
[    2.612117] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x11c value: 0x2
[    2.612132] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x120 value: 0x2
[    2.612147] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x124 value: 0x2
[    2.612162] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x128 value: 0x2
[    2.612177] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x12c value: 0x2
[    2.612192] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x130 value: 0x22
[    2.612207] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x134 value: 0x22
[    2.612221] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x138 value: 0x22
[    2.612236] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x13c value: 0x22
[    2.612251] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x140 value: 0x22
[    2.612266] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x40 value: 0x2
[    2.612281] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x44 value: 0x22
[    2.612295] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x48 value: 0x2
[    2.612310] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x4c value: 0x2
[    2.612325] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x50 value: 0x2
[    2.612340] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x54 value: 0x2
[    2.612354] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x58 value: 0x2
[    2.612369] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x5c value: 0x22
[    2.612384] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x60 value: 0x22
[    2.612398] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x64 value: 0x22
[    2.612413] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x68 value: 0x22
[    2.612428] pinctrl-single 44e10800.pinmux: cpsw_default index: 0x6c value: 0x22
[    2.612460] pinctrl core: add 1 pinctrl maps
[    2.612510] pinctrl-single 44e10800.pinmux: found group selector 5 for cpsw_default
[    2.612534] pinctrl-single 44e10800.pinmux: request pin 69 (PIN69) for 4a100000.ethernet
[    2.612549] pinctrl-single 44e10800.pinmux: request pin 70 (PIN70) for 4a100000.ethernet
[    2.612562] pinctrl-single 44e10800.pinmux: request pin 71 (PIN71) for 4a100000.ethernet
[    2.612574] pinctrl-single 44e10800.pinmux: request pin 72 (PIN72) for 4a100000.ethernet
[    2.612587] pinctrl-single 44e10800.pinmux: request pin 73 (PIN73) for 4a100000.ethernet
[    2.612599] pinctrl-single 44e10800.pinmux: request pin 74 (PIN74) for 4a100000.ethernet
[    2.612611] pinctrl-single 44e10800.pinmux: request pin 75 (PIN75) for 4a100000.ethernet
[    2.612623] pinctrl-single 44e10800.pinmux: request pin 76 (PIN76) for 4a100000.ethernet
[    2.612636] pinctrl-single 44e10800.pinmux: request pin 77 (PIN77) for 4a100000.ethernet
[    2.612648] pinctrl-single 44e10800.pinmux: request pin 78 (PIN78) for 4a100000.ethernet
[    2.612661] pinctrl-single 44e10800.pinmux: request pin 79 (PIN79) for 4a100000.ethernet
[    2.612673] pinctrl-single 44e10800.pinmux: request pin 80 (PIN80) for 4a100000.ethernet
[    2.612686] pinctrl-single 44e10800.pinmux: request pin 16 (PIN16) for 4a100000.ethernet
[    2.612699] pinctrl-single 44e10800.pinmux: request pin 17 (PIN17) for 4a100000.ethernet
[    2.612711] pinctrl-single 44e10800.pinmux: request pin 18 (PIN18) for 4a100000.ethernet
[    2.612723] pinctrl-single 44e10800.pinmux: request pin 19 (PIN19) for 4a100000.ethernet
[    2.612735] pinctrl-single 44e10800.pinmux: request pin 20 (PIN20) for 4a100000.ethernet
[    2.612748] pinctrl-single 44e10800.pinmux: request pin 21 (PIN21) for 4a100000.ethernet
[    2.612760] pinctrl-single 44e10800.pinmux: request pin 22 (PIN22) for 4a100000.ethernet
[    2.612772] pinctrl-single 44e10800.pinmux: request pin 23 (PIN23) for 4a100000.ethernet
[    2.612785] pinctrl-single 44e10800.pinmux: request pin 24 (PIN24) for 4a100000.ethernet
[    2.612798] pinctrl-single 44e10800.pinmux: request pin 25 (PIN25) for 4a100000.ethernet
[    2.612810] pinctrl-single 44e10800.pinmux: request pin 26 (PIN26) for 4a100000.ethernet
[    2.612822] pinctrl-single 44e10800.pinmux: request pin 27 (PIN27) for 4a100000.ethernet
[    2.612838] pinctrl-single 44e10800.pinmux: enabling (null) function5
[    2.626002] random: fast init done
[    2.631025] pinctrl-single 44e10800.pinmux: davinci_mdio_default index: 0x148 value: 0x30
[    2.631058] pinctrl-single 44e10800.pinmux: davinci_mdio_default index: 0x14c value: 0x10
[    2.631090] pinctrl core: add 1 pinctrl maps
[    2.631143] pinctrl-single 44e10800.pinmux: found group selector 6 for davinci_mdio_default
[    2.631173] pinctrl-single 44e10800.pinmux: request pin 82 (PIN82) for 4a101000.mdio
[    2.631187] pinctrl-single 44e10800.pinmux: request pin 83 (PIN83) for 4a101000.mdio
[    2.631201] pinctrl-single 44e10800.pinmux: enabling (null) function6
[    2.631729] mdio_bus 4a101000.mdio: GPIO lookup for consumer reset
[    2.631743] mdio_bus 4a101000.mdio: using lookup tables for GPIO lookup
[    2.631759] mdio_bus 4a101000.mdio: lookup for GPIO reset failed
[    2.690823] davinci_mdio 4a101000.mdio: davinci mdio revision 1.6, bus freq 1000000
[    2.698869] davinci_mdio 4a101000.mdio: detected phy mask ffffffef
[    2.739872] Atheros 8035 ethernet 4a101000.mdio:04: no of_node; not parsing pinctrl DT
[    2.740408] libphy: 4a101000.mdio: probed
[    2.744925] davinci_mdio 4a101000.mdio: phy[4]: device 4a101000.mdio:04, driver Atheros 8035 ethernet
[    2.756189] cpsw 4a100000.ethernet: Detected MACID = 88:c2:55:80:fe:b6
[    2.763696] cpsw 4a100000.ethernet: initialized cpsw ale version 1.4
[    2.770346] cpsw 4a100000.ethernet: ALE Table size 1024
[    2.775962] cpsw 4a100000.ethernet: device node lookup for pps timer failed
[    2.783374] cpsw 4a100000.ethernet: cpts: overflow check period 500 (jiffies)
[    2.793586] cpsw 4a100000.ethernet: cpsw: Detected MACID = 88:c2:55:80:fe:b8
[    2.803833] i2c /dev entries driver
[    2.808554] ti-cpufreq ti-cpufreq: no of_node; not parsing pinctrl DT
[    2.808651] cpu cpu0: OPP-v2 not supported, cpufreq-dt will attempt to use legacy tables.
[    2.818967] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins index: 0xf0 value: 0x30
[    2.818991] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins index: 0xf4 value: 0x30
[    2.819006] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins index: 0xf8 value: 0x30
[    2.819021] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins index: 0xfc value: 0x30
[    2.819037] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins index: 0x100 value: 0x30
[    2.819052] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins index: 0x104 value: 0x30
[    2.819067] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins index: 0x1a0 value: 0x37
[    2.819082] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins index: 0x160 value: 0x2f
[    2.819126] pinctrl core: add 1 pinctrl maps
[    2.819183] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins_sleep index: 0xf0 value: 0x27
[    2.819199] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins_sleep index: 0xf4 value: 0x27
[    2.819214] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins_sleep index: 0xf8 value: 0x27
[    2.819229] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins_sleep index: 0xfc value: 0x27
[    2.819244] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins_sleep index: 0x100 value: 0x27
[    2.819259] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins_sleep index: 0x104 value: 0x27
[    2.819274] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins_sleep index: 0x1a0 value: 0x27
[    2.819289] pinctrl-single 44e10800.pinmux: pinmux_mmc1_pins_sleep index: 0x160 value: 0x27
[    2.819309] pinctrl core: add 1 pinctrl maps
[    2.819357] pinctrl-single 44e10800.pinmux: found group selector 7 for pinmux_mmc1_pins
[    2.819380] pinctrl-single 44e10800.pinmux: found group selector 8 for pinmux_mmc1_pins_sleep
[    2.819402] pinctrl-single 44e10800.pinmux: request pin 60 (PIN60) for 48060000.mmc
[    2.819417] pinctrl-single 44e10800.pinmux: request pin 61 (PIN61) for 48060000.mmc
[    2.819429] pinctrl-single 44e10800.pinmux: request pin 62 (PIN62) for 48060000.mmc
[    2.819441] pinctrl-single 44e10800.pinmux: request pin 63 (PIN63) for 48060000.mmc
[    2.819454] pinctrl-single 44e10800.pinmux: request pin 64 (PIN64) for 48060000.mmc
[    2.819466] pinctrl-single 44e10800.pinmux: request pin 65 (PIN65) for 48060000.mmc
[    2.819479] pinctrl-single 44e10800.pinmux: request pin 104 (PIN104) for 48060000.mmc
[    2.819492] pinctrl-single 44e10800.pinmux: request pin 88 (PIN88) for 48060000.mmc
[    2.819507] pinctrl-single 44e10800.pinmux: enabling (null) function7
[    2.819794] omap_hsmmc 48060000.mmc: GPIO lookup for consumer cd
[    2.819808] omap_hsmmc 48060000.mmc: using device tree for GPIO lookup
[    2.819858] of_get_named_gpiod_flags: parsed 'cd-gpios' property of node '/ocp/mmc@48060000[0]' - status (0)
[    2.819994] omap_hsmmc 48060000.mmc: Got CD GPIO
[    2.824995] omap_hsmmc 48060000.mmc: GPIO lookup for consumer wp
[    2.825007] omap_hsmmc 48060000.mmc: using device tree for GPIO lookup
[    2.825027] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/ocp/mmc@48060000[0]'
[    2.825042] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/ocp/mmc@48060000[0]'
[    2.825054] omap_hsmmc 48060000.mmc: using lookup tables for GPIO lookup
[    2.825071] omap_hsmmc 48060000.mmc: lookup for GPIO wp failed
[    2.882572] pinctrl-single 44e10800.pinmux: emmc_pins_default index: 0x0 value: 0x31
[    2.882599] pinctrl-single 44e10800.pinmux: emmc_pins_default index: 0x4 value: 0x31
[    2.882614] pinctrl-single 44e10800.pinmux: emmc_pins_default index: 0x8 value: 0x31
[    2.882629] pinctrl-single 44e10800.pinmux: emmc_pins_default index: 0xc value: 0x31
[    2.882645] pinctrl-single 44e10800.pinmux: emmc_pins_default index: 0x10 value: 0x31
[    2.882661] pinctrl-single 44e10800.pinmux: emmc_pins_default index: 0x14 value: 0x31
[    2.882676] pinctrl-single 44e10800.pinmux: emmc_pins_default index: 0x18 value: 0x31
[    2.882690] pinctrl-single 44e10800.pinmux: emmc_pins_default index: 0x1c value: 0x31
[    2.882705] pinctrl-single 44e10800.pinmux: emmc_pins_default index: 0x80 value: 0x32
[    2.882720] pinctrl-single 44e10800.pinmux: emmc_pins_default index: 0x84 value: 0x32
[    2.882751] pinctrl core: add 1 pinctrl maps
[    2.882809] pinctrl-single 44e10800.pinmux: found group selector 9 for emmc_pins_default
[    2.882834] pinctrl-single 44e10800.pinmux: request pin 0 (PIN0) for 481d8000.mmc
[    2.882848] pinctrl-single 44e10800.pinmux: request pin 1 (PIN1) for 481d8000.mmc
[    2.882860] pinctrl-single 44e10800.pinmux: request pin 2 (PIN2) for 481d8000.mmc
[    2.882872] pinctrl-single 44e10800.pinmux: request pin 3 (PIN3) for 481d8000.mmc
[    2.882884] pinctrl-single 44e10800.pinmux: request pin 4 (PIN4) for 481d8000.mmc
[    2.882896] pinctrl-single 44e10800.pinmux: request pin 5 (PIN5) for 481d8000.mmc
[    2.882908] pinctrl-single 44e10800.pinmux: request pin 6 (PIN6) for 481d8000.mmc
[    2.882921] pinctrl-single 44e10800.pinmux: request pin 7 (PIN7) for 481d8000.mmc
[    2.882934] pinctrl-single 44e10800.pinmux: request pin 32 (PIN32) for 481d8000.mmc
[    2.882946] pinctrl-single 44e10800.pinmux: request pin 33 (PIN33) for 481d8000.mmc
[    2.882962] pinctrl-single 44e10800.pinmux: enabling (null) function9
[    2.883284] omap_hsmmc 481d8000.mmc: GPIO lookup for consumer cd
[    2.883299] omap_hsmmc 481d8000.mmc: using device tree for GPIO lookup
[    2.883320] of_get_named_gpiod_flags: can't parse 'cd-gpios' property of node '/ocp/mmc@481d8000[0]'
[    2.883335] of_get_named_gpiod_flags: can't parse 'cd-gpio' property of node '/ocp/mmc@481d8000[0]'
[    2.883347] omap_hsmmc 481d8000.mmc: using lookup tables for GPIO lookup
[    2.883364] omap_hsmmc 481d8000.mmc: lookup for GPIO cd failed
[    2.883386] omap_hsmmc 481d8000.mmc: GPIO lookup for consumer wp
[    2.883397] omap_hsmmc 481d8000.mmc: using device tree for GPIO lookup
[    2.883411] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/ocp/mmc@481d8000[0]'
[    2.883425] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/ocp/mmc@481d8000[0]'
[    2.883436] omap_hsmmc 481d8000.mmc: using lookup tables for GPIO lookup
[    2.883448] omap_hsmmc 481d8000.mmc: lookup for GPIO wp failed
[    2.941404] ledtrig-cpu: registered to indicate activity on CPUs
[    2.950607] oprofile-perf oprofile-perf.0: no of_node; not parsing pinctrl DT
[    2.950974] oprofile: using arm/armv7
[    2.955629] Initializing XFRM netlink socket
[    2.960595] NET: Registered protocol family 10
[    2.970022] Segment Routing with IPv6
[    2.974210] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    2.982454] NET: Registered protocol family 17
[    2.987183] NET: Registered protocol family 15
[    2.992564] Key type dns_resolver registered
[    2.997176] omap_voltage_late_init: Voltage driver support not added
[    3.003950] sr_dev_init: No voltage domain specified for smartreflex0. Cannot initialize
[    3.012462] sr_dev_init: No voltage domain specified for smartreflex1. Cannot initialize
[    3.021429] ThumbEE CPU extension supported.
[    3.025923] Registering SWP/SWPB emulation handler
[    3.031023] SmartReflex Class3 initialized
[    3.063258] pinctrl-single 44e10800.pinmux: pinmux_i2c0_pins index: 0x188 value: 0x30
[    3.063316] pinctrl-single 44e10800.pinmux: pinmux_i2c0_pins index: 0x18c value: 0x30
[    3.063353] pinctrl core: add 1 pinctrl maps
[    3.063451] pinctrl-single 44e10800.pinmux: found group selector 10 for pinmux_i2c0_pins
[    3.063487] pinctrl-single 44e10800.pinmux: request pin 98 (PIN98) for 44e0b000.i2c
[    3.063503] pinctrl-single 44e10800.pinmux: request pin 99 (PIN99) for 44e0b000.i2c
[    3.063518] pinctrl-single 44e10800.pinmux: enabling (null) function10
[    3.069924] tps65217-pmic tps65217-pmic: no of_node; not parsing pinctrl DT
[    3.114553] vdd_1v8: Bringing 3300000uV into 1800000-1800000uV
[    3.127784] mmc1: new high speed MMC card at address 0001
[    3.134400] mmcblk mmc1:0001: no of_node; not parsing pinctrl DT
[    3.136935] mmcblk1: mmc1:0001 MMC04G 3.66 GiB 
[    3.143536] mmcblk1boot0: mmc1:0001 MMC04G partition 1 1.00 MiB
[    3.151192] mmcblk1boot1: mmc1:0001 MMC04G partition 2 1.00 MiB
[    3.158763] mmcblk1rpmb: mmc1:0001 MMC04G partition 3 128 KiB
[    3.171911] tps65217 0-0024: TPS65217 ID 0xe version 1.2
[    3.179257] omap_i2c 44e0b000.i2c: bus 0 rev0.11 at 400 kHz
[    3.185932]  mmcblk1: p1 p2
[    3.198304] hctosys: unable to open rtc device (rtc0)
[    3.203861] sr_init: No PMIC hook to init smartreflex
[    3.209427] sr_init: platform driver register failed for SR
[    3.238700] Freeing unused kernel memory: 11264K
[    3.530985] random: dd: uninitialized urandom read (512 bytes read)
[    4.090271] net eth0: initializing cpsw version 1.12 (0)
[    4.213336] Atheros 8035 ethernet 4a101000.mdio:04: attached PHY driver [Atheros 8035 ethernet] (mii_bus:phy_addr=4a101000.mdio:04, irq=POLL)
[    4.252894] cpts ptp bc clkid 0
[    4.261137] IPv6: ADDRCONF(NETDEV_UP): eth0: link is not ready
[    4.437770] net eth1: initializing cpsw version 1.12 (0)
[    4.446112] libphy: PHY 4a101000.mdio:06 not found
[    4.451230] net eth1: phy "4a101000.mdio:06" not found on slave 1, err -19
[    4.463010] IPv6: ADDRCONF(NETDEV_UP): eth1: link is not ready
[    4.633509] random: dropbear: uninitialized urandom read (32 bytes read)
[    6.323220] cpsw 4a100000.ethernet eth0: Link is Up - 100Mbps/Full - flow control rx/tx
[    6.342031] IPv6: ADDRCONF(NETDEV_CHANGE): eth0: link becomes ready
[    7.337950] random: dropbear: uninitialized urandom read (32 bytes read)
[    7.381544] random: dropbear: uninitialized urandom read (32 bytes read)
[    7.466631] random: dropbear: uninitialized urandom read (32 bytes read)
[    7.822819] random: crng init done
[   11.214260] device eth0 entered promiscuous mode
[   11.399600] pinctrl-single 44e10800.pinmux: user_leds index: 0x88 value: 0x7
[   11.399634] pinctrl-single 44e10800.pinmux: user_leds index: 0x78 value: 0x7
[   11.399665] pinctrl core: add 1 pinctrl maps
[   11.399731] pinctrl-single 44e10800.pinmux: found group selector 11 for user_leds
[   11.399757] pinctrl-single 44e10800.pinmux: request pin 34 (PIN34) for 4a300000.pruss
[   11.399772] pinctrl-single 44e10800.pinmux: request pin 30 (PIN30) for 4a300000.pruss
[   11.399787] pinctrl-single 44e10800.pinmux: enabling (null) function11
[   11.400353] pruss 4a300000.pruss: creating PRU cores and other child platform devices
[   11.415536] remoteproc remoteproc0: 4a334000.pru is available
[   11.422417] pru-rproc 4a334000.pru: PRU rproc node /ocp/pruss_soc_bus@4a326004/pruss@0/pru@34000 probed successfully
[   11.435477] remoteproc remoteproc1: 4a338000.pru is available
[   11.441885] pru-rproc 4a338000.pru: PRU rproc node /ocp/pruss_soc_bus@4a326004/pruss@0/pru@38000 probed successfully
[   11.475076] pps_gen_gpio: loading out-of-tree module taints kernel.
[   11.483032] GPIO PPS signal generator
[   11.487563] pps_gen_gpio pps-gen: GPIO lookup for consumer pps-gen
[   11.487582] pps_gen_gpio pps-gen: using device tree for GPIO lookup
[   11.487609] of_get_named_gpiod_flags: can't parse 'pps-gen-gpios' property of node '/pps-gen[0]'
[   11.487645] of_get_named_gpiod_flags: parsed 'pps-gen-gpio' property of node '/pps-gen[0]' - status (0)
[   11.488190] PPS GPIO set on the average takes 2450ns
[   11.503063] remoteproc remoteproc0: powering up 4a334000.pru
[   11.510488] remoteproc remoteproc0: Direct firmware load for /lib/firmware/pru/pps_gen.out failed with error -2
[   11.521763] remoteproc remoteproc0: request_firmware failed: -2
[   11.527971] remoteproc remoteproc0: Boot failed: -2
[   11.537733] remoteproc remoteproc1: powering up 4a338000.pru
[   11.546884] remoteproc remoteproc1: Direct firmware load for /lib/firmware/pru/pps_gen.out failed with error -2
[   11.557634] remoteproc remoteproc1: request_firmware failed: -2
[   11.563900] remoteproc remoteproc1: Boot failed: -2
[   18.000601] We are late this time [17.999970710]
[   24.000599] We are late this time [23.999969377]
