Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 6.1.83-ti-gc1c2f1971fbf (oe-user@oe-host) (arm-poky-linux-gnueabi-gcc (GCC) 11.4.0, GNU ld (GNU Binutils) 2.38.20220708) #1 PREEMPT Mon May 13 20:19:51 UTC 2024
[    0.000000] CPU: ARMv7 Processor [413fc082] revision 2 (ARMv7), cr=10c5387d
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] OF: fdt: Machine model: TI AM335x BeagleTest
[    0.000000] earlycon: omap8250 at MMIO 0x44e09000 (options '')
[    0.000000] printk: bootconsole [omap8250] enabled
[    0.000000] Memory policy: Data cache writeback
[    0.000000] efi: UEFI not found.
[    0.000000] cma: Reserved 64 MiB at 0x9b800000
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x0000000080000000-0x000000009fdfffff]
[    0.000000]   HighMem  empty
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000080000000-0x000000009fdfffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000080000000-0x000000009fdfffff]
[    0.000000] CPU: All CPU(s) started in SVC mode.
[    0.000000] AM335X ES2.1 (neon)
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 129540
[    0.000000] Kernel command line: root=PARTUUID=2a114b52-02 rootwait rw earlycon console=ttyO0,115200n8,115200
[    0.000000] Dentry cache hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.000000] Inode-cache hash table entries: 32768 (order: 5, 131072 bytes, linear)
[    0.000000] mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.000000] Memory: 433576K/522240K available (11264K kernel code, 1467K rwdata, 3200K rodata, 1024K init, 281K bss, 23128K reserved, 65536K cma-reserved, 0K highmem)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] trace event string verifier disabled
[    0.000000] rcu: Preemptible hierarchical RCU implementation.
[    0.000000] rcu:     RCU event tracing is enabled.
[    0.000000]  Trampoline variant of Tasks RCU enabled.
[    0.000000] rcu: RCU calculated value of scheduler-enlistment delay is 10 jiffies.
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] IRQ: Found an INTC at 0x(ptrval) (revision 5.0) with 128 interrupts
[    0.000000] rcu: srcu_init: Setting srcu_struct sizes based on contention.
[    0.000000] TI gptimer clocksource: always-on /ocp/interconnect@44c00000/segment@200000/target-module@31000
[    0.000003] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 89478484971ns
[    0.008084] clocksource: dmtimer: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.018280] TI gptimer clockevent: 24000000 Hz at /ocp/interconnect@48000000/segment@0/target-module@40000
[    0.030631] Console: colour dummy device 80x30
[    0.035257] WARNING: Your 'console=ttyO0' has been replaced by 'ttyS0'
[    0.042073] This ensures that you still see kernel messages. Please
[    0.048536] update your kernel commandline.
[    0.052879] Calibrating delay loop... 597.60 BogoMIPS (lpj=2988032)
[    0.114719] CPU: Testing write buffer coherency: ok
[    0.119841] CPU0: Spectre v2: using BPIALL workaround
[    0.125043] pid_max: default: 32768 minimum: 301
[    0.130126] Mount-cache hash table entries: 1024 (order: 0, 4096 bytes, linear)
[    0.137670] Mountpoint-cache hash table entries: 1024 (order: 0, 4096 bytes, linear)
[    0.148066] cblist_init_generic: Setting adjustable number of callback queues.
[    0.155632] cblist_init_generic: Setting shift to 0 and lim to 1.
[    0.162141] Setting up static identity map for 0x80100000 - 0x80100060
[    0.169119] rcu: Hierarchical SRCU implementation.
[    0.174056] rcu:     Max phase no-delay instances is 1000.
[    0.182127] EFI services will not be available.
[    0.187612] devtmpfs: initialized
[    0.211437] VFP support v0.3: implementor 41 architecture 3 part 30 variant c rev 3
[    0.219844] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.230028] futex hash table entries: 256 (order: -1, 3072 bytes, linear)
[    0.244091] pinctrl core: initialized pinctrl subsystem
[    0.251103] DMI not present or invalid.
[    0.256081] NET: Registered PF_NETLINK/PF_ROUTE protocol family
[    0.265435] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.274215] thermal_sys: Registered thermal governor 'step_wise'
[    0.274360] cpuidle: using governor menu
[    0.301467] OF: /ocp/target-module@47400000/usb@1400: could not get #interrupt-cells for /ocp/interconnect@44c00000/segment@200000/target-module@b000/i2c@0/tps@2D
[    0.316724] OF: /ocp/target-module@47400000/usb@1400: could not get #interrupt-cells for /ocp/interconnect@44c00000/segment@200000/target-module@b000/i2c@0/tps@2D
[    0.334894] No ATAGs?
[    0.337262] hw-breakpoint: debug architecture 0x4 unsupported.
[    0.381427] iommu: Default domain type: Translated
[    0.386487] iommu: DMA domain TLB invalidation policy: strict mode
[    0.400524] SCSI subsystem initialized
[    0.418879] usbcore: registered new interface driver usbfs
[    0.424600] usbcore: registered new interface driver hub
[    0.438381] usbcore: registered new device driver usb
[    0.444184] pps_core: LinuxPPS API ver. 1 registered
[    0.458300] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.467740] PTP clock support registered
[    0.488597] EDAC MC: Ver: 3.0.0
[    0.498833] clocksource: Switched to clocksource dmtimer
[    0.529691] NET: Registered PF_INET protocol family
[    0.549024] IP idents hash table entries: 8192 (order: 4, 65536 bytes, linear)
[    0.569587] tcp_listen_portaddr_hash hash table entries: 1024 (order: 0, 4096 bytes, linear)
[    0.578340] Table-perturb hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.598865] TCP established hash table entries: 4096 (order: 2, 16384 bytes, linear)
[    0.606905] TCP bind hash table entries: 4096 (order: 3, 32768 bytes, linear)
[    0.628914] TCP: Hash tables configured (established 4096 bind 4096)
[    0.635614] UDP hash table entries: 256 (order: 0, 4096 bytes, linear)
[    0.658852] UDP-Lite hash table entries: 256 (order: 0, 4096 bytes, linear)
[    0.666268] NET: Registered PF_UNIX/PF_LOCAL protocol family
[    0.689297] RPC: Registered named UNIX socket transport module.
[    0.695415] RPC: Registered udp transport module.
[    0.708842] RPC: Registered tcp transport module.
[    0.713687] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.728850] PCI: CLS 0 bytes, default 64
[    0.734838] Initialise system trusted keyrings
[    0.749682] workingset: timestamp_bits=30 max_order=17 bucket_order=0
[    0.774174] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.799366] NFS: Registering the id_resolver key type
[    0.804665] Key type id_resolver registered
[    0.809058] Key type id_legacy registered
[    0.813341] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.838842] nfs4flexfilelayout_init: NFSv4 Flexfile Layout Driver Registering...
[    0.846524] ntfs: driver 2.1.32 [Flags: R/O].
[    0.859942] Key type asymmetric registered
[    0.864187] Asymmetric key parser 'x509' registered
[    0.879135] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 247)
[    0.886764] io scheduler mq-deadline registered
[    0.908845] io scheduler kyber registered
[    1.058209] Serial: 8250/16550 driver, 5 ports, IRQ sharing enabled
[    1.080490] STMicroelectronics ASC driver initialized
[    1.123941] brd: module loaded
[    1.143355] loop: module loaded
[    1.164434] CAN device driver interface
[    1.179009] e1000e: Intel(R) PRO/1000 Network Driver
[    1.184132] e1000e: Copyright(c) 1999 - 2015 Intel Corporation.
[    1.198980] igb: Intel(R) Gigabit Ethernet Network Driver
[    1.204544] igb: Copyright (c) 2007-2014 Intel Corporation.
[    1.219021] ksz8895_init
[    1.222741] pegasus: Pegasus/Pegasus II USB Ethernet driver
[    1.228551] usbcore: registered new interface driver pegasus
[    1.248917] usbcore: registered new interface driver asix
[    1.254531] usbcore: registered new interface driver ax88179_178a
[    1.278893] usbcore: registered new interface driver cdc_ether
[    1.284965] usbcore: registered new interface driver smsc75xx
[    1.298917] usbcore: registered new interface driver smsc95xx
[    1.304880] usbcore: registered new interface driver net1080
[    1.318892] usbcore: registered new interface driver cdc_subset
[    1.325029] usbcore: registered new interface driver zaurus
[    1.348949] usbcore: registered new interface driver cdc_ncm
[    1.355806] usbcore: registered new interface driver usb-storage
[    1.379937] i2c_dev: i2c /dev entries driver
[    1.387042] cpuidle: enable-method property 'ti,am3352' found operations
[    1.409713] sdhci: Secure Digital Host Controller Interface driver
[    1.416096] sdhci: Copyright(c) Pierre Ossman
[    1.429125] Synopsys Designware Multimedia Card Interface Driver
[    1.435539] sdhci-pltfm: SDHCI platform and OF driver helper
[    1.449527] ledtrig-cpu: registered to indicate activity on CPUs
[    1.456285] usbcore: registered new interface driver usbhid
[    1.478837] usbhid: USB HID core driver
[    1.485478] NET: Registered PF_PACKET protocol family
[    1.508932] can: controller area network core
[    1.513576] NET: Registered PF_CAN protocol family
[    1.518516] can: raw protocol
[    1.528855] can: broadcast manager protocol
[    1.533182] can: netlink gateway - max_hops=1
[    1.537953] 8021q: 802.1Q VLAN Support v1.8
[    1.559192] Key type dns_resolver registered
[    1.563786] ThumbEE CPU extension supported.
[    1.568200] Registering SWP/SWPB emulation handler
[    1.589465] omap_voltage_late_init: Voltage driver support not added
[    1.597315] Loading compiled-in X.509 certificates
[    1.703181] platform 44e10800.pinmux: Fixed dependency cycle(s) with /ocp/interconnect@44c00000/segment@200000/target-module@10000/scm@0/pinmux@800/pinmux_clkout2_pin
[    1.739673] pinctrl-single 44e10800.pinmux: 142 pins, size 568
[    1.763444] ti-sysc: probe of 44e31000.target-module failed with error -16
[    1.807015] ti-sysc: probe of 48040000.target-module failed with error -16
[    1.856985] gpio gpiochip0: (gpio-0-31): not an immutable chip, please consider fixing it!
[    1.879348] OMAP GPIO hardware version 0.1
[    1.920395] at24 2-0054: supply vcc not found, using dummy regulator
[    1.973269] at24 2-0055: supply vcc not found, using dummy regulator
[    2.023016] at24 2-0056: supply vcc not found, using dummy regulator
[    2.072875] at24 2-0057: supply vcc not found, using dummy regulator
[    2.122441] omap_i2c 4819c000.i2c: bus 2 rev0.11 at 100 kHz
[    2.144622] gpio gpiochip1: (gpio-32-63): not an immutable chip, please consider fixing it!
[    2.171823] gpio gpiochip2: (gpio-64-95): not an immutable chip, please consider fixing it!
[    2.213991] omap_rng 48310000.rng: Random Number Generator ver. 20
[    2.220629] random: crng init done
[    2.251472] cpsw 4a100000.ethernet: initialized cpsw ale version 1.4
[    2.258070] cpsw 4a100000.ethernet: ALE Table size 1024
[    2.279111] cpsw 4a100000.ethernet: cpts: overflow check period 500 (jiffies)
[    2.286536] cpsw 4a100000.ethernet: Detected MACID = 68:c9:0b:80:64:81
[    2.310094] cpsw 4a100000.ethernet: cpsw: Detected MACID = 68:c9:0b:80:64:83
[    2.350782] debugfs: Directory '49000000.dma' with parent 'dmaengine' already present!
[    2.368862] edma 49000000.dma: TI EDMA DMA engine driver
[    2.445091] omap_reset_deassert: timedout waiting for gfx:0
[    2.458914] ti-sysc: probe of 5600fe00.target-module failed with error -110
[    2.482309] hw perfevents: enabled with armv7_cortex_a8 PMU driver, 5 counters available
[    2.504027] l3-aon-clkctrl:0000:0: failed to disable
[    2.510468] gpio gpiochip3: (gpio-96-127): not an immutable chip, please consider fixing it!
[    2.539908] 44e09000.serial: ttyS0 at MMIO 0x44e09000 (irq = 35, base_baud = 3000000) is a 8250
[    2.559028] printk: console [ttyS0] enabled
[    2.559028] printk: console [ttyS0] enabled
[    2.567552] printk: bootconsole [omap8250] disabled
[    2.567552] printk: bootconsole [omap8250] disabled
[    2.629258] tps65910 0-002d: No interrupt support, no core IRQ
[    2.699318] at24 0-0050: supply vcc not found, using dummy regulator
[    2.719440] at24 0-0050: 32768 byte 24c256 EEPROM, writable, 1 bytes/write
[    2.726542] omap_i2c 44e0b000.i2c: bus 0 rev0.11 at 100 kHz
[    2.751791] ksz8895_probe
[    2.754874]  gpio_reset 74 gpio_irq 73
[    2.809145] KSZ8895: Chip Family 95  Chip ID 4  Revision ID 0
[    2.815032] ksz8895_create_sysfs_nodes
[    2.829061] KSZ8895: user0 ksz8895_probe1#############
[    2.834570] KSZ8895: user0 ksz8895_probe2#############
[    2.848912] ksz8895_reset
[    2.855628] ksz8895_reconfigure
[    2.868922] KSZ8895: user0 init_vlan#############
[    2.873773] set_vlan_table_entry vid 0  membership 0x0  fid 0  valid 0
[    2.888889] read_vlan_table_entry  iac0 0x14 iac1 0x0   0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0   table_entry 0x0
[    2.908836] read_vlan_table_entry  vid 0 : valid 0 membership 0x0  FID 0
[    2.915700] set_vlan_table_entry post iac0 0x4 iac1 0x0   0x4 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 table_entry 0x0
[    2.948837] set_vlan_table_entry  vid 0 : membership 0x0  FID 0  valid 0
[    2.955583] set_vlan_table_entry vid 0  membership 0x0  fid 0  valid 0
[    2.968892] read_vlan_table_entry  iac0 0x14 iac1 0x0   0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0   table_entry 0x0
[    2.988842] read_vlan_table_entry  vid 0 : valid 0 membership 0x0  FID 0
[    2.995708] set_vlan_table_entry post iac0 0x4 iac1 0x0   0x4 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 table_entry 0x0
[    3.028835] set_vlan_table_entry  vid 0 : membership 0x0  FID 0  valid 0
[    3.035579] set_vlan_table_entry vid 0  membership 0x0  fid 0  valid 0
[    3.058882] read_vlan_table_entry  iac0 0x14 iac1 0x0   0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0   table_entry 0x0
[    3.078838] read_vlan_table_entry  vid 0 : valid 0 membership 0x0  FID 0
[    3.085704] set_vlan_table_entry post iac0 0x4 iac1 0x0   0x4 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 table_entry 0x0
[    3.108837] set_vlan_table_entry  vid 0 : membership 0x0  FID 0  valid 0
[    3.115577] set_vlan_table_entry vid 0  membership 0x0  fid 0  valid 0
[    3.138884] read_vlan_table_entry  iac0 0x14 iac1 0x0   0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0   table_entry 0x0
[    3.158848] read_vlan_table_entry  vid 0 : valid 0 membership 0x0  FID 0
[    3.165716] set_vlan_table_entry post iac0 0x4 iac1 0x0   0x4 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 table_entry 0x0
[    3.188837] set_vlan_table_entry  vid 0 : membership 0x0  FID 0  valid 0
[    3.195640] set_default_port_vid port 1 addr 0x13   soll 14 ist 0/14
[    3.218896] set_default_port_vid port 2 addr 0x23   soll a ist 0/a
[    3.225345] set_default_port_vid port 3 addr 0x33   soll a ist 0/a
[    3.238930] set_default_port_vid port 4 addr 0x43   soll a ist 0/a
[    3.245370] remove_vlan_tag_on_outgoing_port port 1 remove 1  addr 0x10  reg 0x2
[    3.268882] remove_vlan_tag_on_outgoing_port port 2 remove 1  addr 0x20  reg 0x2
[    3.276453] remove_vlan_tag_on_outgoing_port port 3 remove 1  addr 0x30  reg 0x2
[    3.298884] remove_vlan_tag_on_outgoing_port port 4 remove 1  addr 0x40  reg 0x2
[    3.306456] insert_vlan_tag_on_outgoing_port port 5 insert 1  addr 0x50  reg 0x4
[    3.328915] set_ports_vlan_membership port 1  port_mask 0x11 addr 0x11  reg 0x11
[    3.336488] set_ports_vlan_membership port 2  port_mask 0x1e addr 0x21  reg 0x1e
[    3.358882] set_ports_vlan_membership port 3  port_mask 0x1e addr 0x31  reg 0x1e
[    3.366453] set_ports_vlan_membership port 4  port_mask 0x1e addr 0x41  reg 0x1e
[    3.388891] set_ports_vlan_membership port 5  port_mask 0x1f addr 0x51  reg 0x1f
[    3.396426] set_vlan_table_entry vid 20  membership 0x11  fid 1  valid 1
[    3.418879] read_vlan_table_entry  iac0 0x14 iac1 0x5   0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0   table_entry 0x0
[    3.438840] read_vlan_table_entry  vid 20 : valid 0 membership 0x0  FID 0
[    3.445799] set_vlan_table_entry post iac0 0x4 iac1 0x5   0x4 0x5 0x0 0x0 0x0 0x0 0x0 0x18 0x81 table_entry 0x1881
[    3.478832] set_vlan_table_entry  vid 20 : membership 0x11  FID 1  valid 1
[    3.485793] read_vlan_table_entry  iac0 0x14 iac1 0x5   0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x18 0x81   table_entry 0x1881
[    3.508836] read_vlan_table_entry  vid 20 : valid 1 membership 0x11  FID 1
[    3.515839] set_vlan_table_entry vid 10  membership 0x1e  fid 2  valid 1
[    3.538890] read_vlan_table_entry  iac0 0x14 iac1 0x2   0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0 0x0   table_entry 0x0
[    3.558836] read_vlan_table_entry  vid 10 : valid 0 membership 0x0  FID 0
[    3.565789] set_vlan_table_entry post iac0 0x4 iac1 0x2   0x4 0x2 0x0 0x0 0x7c 0x8 0x0 0x0 0x0 table_entry 0x1f02
[    3.588834] set_vlan_table_entry  vid 10 : membership 0x1e  FID 2  valid 1
[    3.595796] read_vlan_table_entry  iac0 0x14 iac1 0x2   0x0 0x0 0x0 0x0 0x7c 0x8 0x0 0x0 0x0   table_entry 0x1f02
[    3.628835] read_vlan_table_entry  vid 10 : valid 1 membership 0x1e  FID 2
[    3.636167] set_rstp_support_bits port 1 addr 0x12 reg 0x1   symbol D
[    3.658870] set_rstp_support_bits port 2 addr 0x22 reg 0x1   symbol D
[    3.665468] set_rstp_support_bits port 3 addr 0x32 reg 0x1   symbol D
[    3.678871] set_rstp_support_bits port 4 addr 0x42 reg 0x1   symbol D
[    3.685469] set_rstp_support_bits port 5 addr 0x52 reg 0x1   symbol D
[    3.708914] flush_dynamic_mac_table  port 1..5 -XXX-
[    3.714063] flush_static_mac_table  port 1..5 -XXX-
[    3.728878] set_rstp_support_bits port 1 addr 0x12 reg 0x6   symbol F
[    3.735473] set_rstp_support_bits port 2 addr 0x22 reg 0x1   symbol D
[    3.758878] set_rstp_support_bits port 3 addr 0x32 reg 0x1   symbol D
[    3.765476] set_rstp_support_bits port 4 addr 0x42 reg 0x1   symbol D
[    3.778887] set_rstp_support_bits port 5 addr 0x52 reg 0x6   symbol F
[    3.785457] KSZ_DEFAULT_WAN_PORT 1
[    3.798855] KSZ_DEFAULT_LAN_PORT1 2
[    3.802457] KSZ_DEFAULT_LAN_PORT2 2
[    3.806048] KSZ_DEFAULT_LAN_PORT3 2
[    3.828846] KSZ_DEFAULT_WAN_PORT 20
[    3.832454] KSZ_DEFAULT_LAN_PORT1 10
[    3.836134] KSZ_DEFAULT_LAN_PORT2 10
[    3.848849] KSZ_DEFAULT_LAN_PORT3 10
[    3.871042] omap_gpio 44e07000.gpio: Could not set line 17 debounce to 200000 microseconds (-22)
[    3.898991] sdhci-omap 48060000.mmc: Got CD GPIO
[    3.904026] sdhci-omap 48060000.mmc: supply pbias not found, using dummy regulator
[    3.919740] sdhci-omap 48060000.mmc: supply vqmmc not found, using dummy regulator
[    3.966494] mmc0: SDHCI controller on 48060000.mmc [48060000.mmc] using External DMA
[    3.975689] Waiting for root device PARTUUID=2a114b52-02...
[    4.013945] mmc0: new high speed SDHC card at address 59b4
[    4.021356] mmcblk0: mmc0:59b4 USD   3.75 GiB
[    4.030475]  mmcblk0: p1 p2
[    4.184505] EXT4-fs (mmcblk0p2): recovery complete
[    4.193579] EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Quota mode: disabled.
[    4.202789] VFS: Mounted root (ext4 filesystem) on device 179:2.
[    4.211778] devtmpfs: mounted
[    4.216785] Freeing unused kernel image (initmem) memory: 1024K
[    4.223563] Run /sbin/init as init process
INIT: version 3.01 booting
[    4.595626] ksz8895_interrupt: queue_work ok ......
[    4.600866] KSZ8895: user0 ksz8895_work_queue_func#############
[    4.606913] ksz8895_work_queue_func
[    4.613920] KSZ8895: user0 ksz8895_work_queue_func2#############
[    4.629164]  port 1 goes up
[    4.632107] KSZ8895: user0 ksz8895_work_queue_func2#############
[    4.638226] KSZ8895: user0 ksz8895_work_queue_func2#############
[    4.655643] KSZ8895: user0 ksz8895_work_queue_func2#############
[    4.669534] KSZ8895: user0 ksz8895_work_queue_func2#############
Starting udev
[    4.850303] udevd[95]: starting version 3.2.10
[    4.908667] udevd[96]: starting eudev-3.2.10
[    6.811073] EXT4-fs (mmcblk0p2): re-mounted. Quota mode: disabled.
hwclock: can't open '/dev/misc/rtc': No such file or directory
Fri Mar  9 12:36:16 UTC 2018
hwclock: can't open '/dev/misc/rtc': No such file or directory
INIT: Entering runlevel: 5
Configuring network interfaces... ip: can't find device 'usb0'
ip: SIOCGIFFLAGS: No such device
ip: can't find device 'vlan20'
ip: SIOCGIFFLAGS: No such device
/bin/sh: /usr/sbin/avahi-autoipd: not found
Starting OpenBSD Secure Shell server: sshd
done.
hwclock: can't open '/dev/misc/rtc': No such file or directory
Starting syslogd/klogd: done
Poky (Yocto Project Reference Distro) 4.0.20 beagletest /dev/ttyS0

beagletest login: root
root@beagletest:~# 
root@beagletest:~# ifconfig
lo        Link encap:Local Loopback  
          inet addr:127.0.0.1  Mask:255.0.0.0
          UP LOOPBACK RUNNING  MTU:65536  Metric:1
          RX packets:0 errors:0 dropped:0 overruns:0 frame:0
          TX packets:0 errors:0 dropped:0 overruns:0 carrier:0
          collisions:0 txqueuelen:1000 
          RX bytes:0 (0.0 B)  TX bytes:0 (0.0 B)

root@beagletest:~# ifconfig eth1 up
[  140.719217] net eth1: initializing cpsw version 1.12 (0)
[  140.745491] Generic PHY fixed-0:01: attached PHY driver (mii_bus:phy_addr=fixed-0:01, irq=POLL)
[  140.756923] cpsw 4a100000.ethernet eth1: Link is Up - 100Mbps/Full - flow control off
[  140.774247] 8021q: adding VLAN 0 to HW filter on device eth1
root@beagletest:~# ifconfig
eth1      Link encap:Ethernet  HWaddr 68:C9:0B:80:64:83  
          UP BROADCAST RUNNING MULTICAST  MTU:1500  Metric:1
          RX packets:0 errors:0 dropped:0 overruns:0 frame:0
          TX packets:0 errors:0 dropped:0 overruns:0 carrier:0
          collisions:0 txqueuelen:1000 
          RX bytes:0 (0.0 B)  TX bytes:0 (0.0 B)

lo        Link encap:Local Loopback  
          inet addr:127.0.0.1  Mask:255.0.0.0
          UP LOOPBACK RUNNING  MTU:65536  Metric:1
          RX packets:0 errors:0 dropped:0 overruns:0 frame:0
          TX packets:0 errors:0 dropped:0 overruns:0 carrier:0
          collisions:0 txqueuelen:1000 
          RX bytes:0 (0.0 B)  TX bytes:0 (0.0 B)

root@beagletest:~#