<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_4-0-3.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE UUID="ECUC:AUTOSAR">
      <SHORT-NAME>TI_TMS570LSx</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-DEF UUID="ECUC:cce1bea0-f990-4c41-b8fd-2b0f0e590935">
          <SHORT-NAME>Lin</SHORT-NAME>
          <DESC>
            <L-2 L="EN">Configuration of the Lin (LIN driver) module.</L-2>
          </DESC>
          <ADMIN-DATA>
            <DOC-REVISIONS>
              <DOC-REVISION>
                <REVISION-LABEL>4.2.0</REVISION-LABEL>
                <ISSUED-BY>AUTOSAR</ISSUED-BY>
                <DATE>2011-11-09</DATE>
              </DOC-REVISION>
            </DOC-REVISIONS>
          </ADMIN-DATA>
          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
          <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
          <REFINED-MODULE-DEF-REF DEST="ECUC-MODULE-DEF">/AUTOSAR/EcucDefs/Lin</REFINED-MODULE-DEF-REF>
          <SUPPORTED-CONFIG-VARIANTS>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-POST-BUILD</SUPPORTED-CONFIG-VARIANT>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-PRE-COMPILE</SUPPORTED-CONFIG-VARIANT>
          </SUPPORTED-CONFIG-VARIANTS>
          <CONTAINERS>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:1d543976-f649-42c3-b4ac-ad3abf68201a">
              <SHORT-NAME>LinGeneral</SHORT-NAME>
              <DESC>
                <L-2 L="EN">This container contains the parameters related to each LIN Driver Unit.</L-2>
              </DESC>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:6f7825c9-bce4-4f50-8643-1f8fcef24d80">
                  <SHORT-NAME>LinDevErrorDetect</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Switches the Development Error Detection and Notification ON or OFF.</L-2>
                  </DESC>
                  <IMPLEMENTATION-CONFIG-CLASSES>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                  </IMPLEMENTATION-CONFIG-CLASSES>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:6d8fcd10-4bde-4582-99fd-4e98b7c25839">
                  <SHORT-NAME>LinIndex</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Specifies the InstanceId of this module instance. If only one instance is present it shall have the Id 0.</L-2>
                  </DESC>
                  <IMPLEMENTATION-CONFIG-CLASSES>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                  </IMPLEMENTATION-CONFIG-CLASSES>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:4c279681-63d2-4125-b3a0-36aabd53153b">
                  <SHORT-NAME>LinTimeoutDuration</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Specifies the maximum number of loops for blocking function until a timeout is raised in short term wait loops</L-2>
                  </DESC>
                  <IMPLEMENTATION-CONFIG-CLASSES>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                  </IMPLEMENTATION-CONFIG-CLASSES>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>65535</DEFAULT-VALUE>
                  <MAX>65535</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:33f40783-f5c3-4caf-9f02-aec048208445">
                  <SHORT-NAME>VCLK</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Peripheral clock frequency (in MHz)</L-2>
                  </DESC>
                  <IMPLEMENTATION-CONFIG-CLASSES>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                  </IMPLEMENTATION-CONFIG-CLASSES>
                  <ORIGIN>Texas Instruments</ORIGIN>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>90</DEFAULT-VALUE>
                  <MAX>100</MAX>
                  <MIN>8</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:03f6c9e0-e3b7-4907-84c0-a96e099b4431">
                  <SHORT-NAME>LinVersionInfoApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Switches the Lin_GetVersionInfo function ON or OFF.</L-2>
                  </DESC>
                  <IMPLEMENTATION-CONFIG-CLASSES>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                  </IMPLEMENTATION-CONFIG-CLASSES>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:d9d0695d-0b1f-4a63-b4cf-0bcc86102e58">
                  <SHORT-NAME>LinTypeofInterruptFunction</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Type of ISR function</L-2>
                  </DESC>
                  <IMPLEMENTATION-CONFIG-CLASSES>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                  </IMPLEMENTATION-CONFIG-CLASSES>
                  <ORIGIN>Texas Instruments</ORIGIN>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>LIN_ISR_CAT1</DEFAULT-VALUE>
                  <LITERALS>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>LIN_ISR_VOID</SHORT-NAME>
                      <ORIGIN>Texas Instruments</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>LIN_ISR_CAT1</SHORT-NAME>
                      <ORIGIN>Texas Instruments</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>LIN_ISR_CAT2</SHORT-NAME>
                      <ORIGIN>Texas Instruments</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                  </LITERALS>
                </ECUC-ENUMERATION-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:af84be2a-4649-4e74-b644-c9d4a7497889">
                  <SHORT-NAME>LinSafeTIApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Switches the Lin_ConfigRegReadBack function ON or OFF.</L-2>
                  </DESC>
                  <IMPLEMENTATION-CONFIG-CLASSES>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                  </IMPLEMENTATION-CONFIG-CLASSES>
                  <ORIGIN>Texas Instruments</ORIGIN>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:55d75bee-8515-48f5-ae55-ca73d842a3a0">
                  <SHORT-NAME>LinLoopBackTestEnable</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Switch to enable loopback mode.</L-2>
                  </DESC>
                  <IMPLEMENTATION-CONFIG-CLASSES>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                  </IMPLEMENTATION-CONFIG-CLASSES>
                  <ORIGIN>Texas Instruments</ORIGIN>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:8c14b8ff-560d-46b2-b94b-c09489fa5a75">
                  <SHORT-NAME>LinCallUserCallout</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Switches the user callout API. If OFF, DEM API will be called, else user callout API will be called.</L-2>
                  </DESC>
                  <IMPLEMENTATION-CONFIG-CLASSES>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                  </IMPLEMENTATION-CONFIG-CLASSES>
                  <ORIGIN>Texas Instruments</ORIGIN>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-FUNCTION-NAME-DEF UUID="ECUC:f43bffda-8d3a-4520-b424-b558fcbe752c">
                  <SHORT-NAME>LinCallOutAPIDeclaration</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">User callout API function declaration.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <IMPLEMENTATION-CONFIG-CLASSES>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                    <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                  </IMPLEMENTATION-CONFIG-CLASSES>
                  <ORIGIN>Texas Instruments</ORIGIN>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                    <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>Lin_AvoidCallOut</DEFAULT-VALUE>
                    </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                  </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                </ECUC-FUNCTION-NAME-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:5bf7d5c4-2ce3-45ef-9aa4-694ae888aef1">
              <SHORT-NAME>LinGlobalConfig</SHORT-NAME>
              <DESC>
                <L-2 L="EN">This container contains the global configuration parameter of the Lin driver. This container is a MultipleConfigurationContainer, i.e. this container and its sub-containers exit once per configuration set.</L-2>
              </DESC>
              <MULTIPLE-CONFIGURATION-CONTAINER>true</MULTIPLE-CONFIGURATION-CONTAINER>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:5068d91d-ca0a-460f-9f6a-21f7ad18d591">
                  <SHORT-NAME>LinChannel</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">This container contains the configuration (parameters) of the LIN Controller(s).</L-2>
                  </DESC>
                  <PARAMETERS>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:16748716-3f59-4064-a8ef-ca1ab0b00deb">
                      <SHORT-NAME>LinChannelBaudRate</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Specifies the baud rate of the LIN channel</L-2>
                      </DESC>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>20000</DEFAULT-VALUE>
                      <MAX>20000</MAX>
                      <MIN>1000</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:c3ebc9ff-d623-4c49-ac91-241dec476a8d">
                      <SHORT-NAME>LinChannelId</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Identifies the LIN channel. Replaces LIN_CHANNEL_INDEX_NAME from the LIN SWS.</L-2>
                      </DESC>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <SYMBOLIC-NAME-VALUE>true</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>10</DEFAULT-VALUE>
                      <MAX>65535</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:644aeda6-9c40-4e6d-945f-555f9c2b0c56">
                      <SHORT-NAME>LinChannelWakeupSupport</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Specifies if the LIN hardware channel supports wake up functionality</L-2>
                      </DESC>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:1459b26a-9994-46ad-a37b-7cf7b1642d7c">
                      <SHORT-NAME>LinBaseAddress</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Address of LIN config registers</L-2>
                      </DESC>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>Texas Instruments</ORIGIN>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>4294435840</DEFAULT-VALUE>
                      <MAX>4294967295</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:1f62bb1a-6b38-47e3-b016-2478eea9de5b">
                      <SHORT-NAME>LinSyncBreak</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Synchronization break of the LIN Header </L-2>
                      </DESC>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>Texas Instruments</ORIGIN>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>14</DEFAULT-VALUE>
                      <MAX>20</MAX>
                      <MIN>13</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:916ba542-865e-499a-b473-d7b7adc63fb6">
                      <SHORT-NAME>LinSyncBreakDelimiter</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Synchronization break delimiter of the LIN Header </L-2>
                      </DESC>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>Texas Instruments</ORIGIN>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>2</DEFAULT-VALUE>
                      <MAX>4</MAX>
                      <MIN>1</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:df926436-58ac-4912-beb2-b6a951d5f244">
                      <SHORT-NAME>LinClockRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Reference to the LIN clock source configuration, which is set in the MCU driver configuration.</L-2>
                      </DESC>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                    <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:c24ae6cb-a145-4c7d-a7e1-7493da1e0df8">
                      <SHORT-NAME>LinChannelEcuMWakeupSource</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">This parameter contains a reference to the Wakeup Source for this controller as defined in the ECU State Manager.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMWakeupSource</DESTINATION-REF>
                    </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:4d8e20c9-6d9d-4ed9-8556-977fd239ecbf">
                  <SHORT-NAME>LinDemEventParameterRefs</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Container for the references to DemEventParameter elements which shall be invoked using the API Dem_ReportErrorStatus API in case the corresponding error occurs. The EventId is taken from the referenced DemEventParameter&apos;s DemEventId value. The standardized errors are provided in the container and can be extended by vendor specific error references.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <REFERENCES>
                    <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:479d9631-3cd7-4995-ada9-6163ae75fd71">
                      <SHORT-NAME>LIN_E_TIMEOUT</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Timeout caused by hardware error&quot; has occured. If the reference is not configured the error shall be reported as DET error.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                    </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                    <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:1628f973-fcc8-4f8b-bb9e-6f186e361524">
                      <SHORT-NAME>LIN_E_NORESPONSE</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;NoResponse caused by hardware error&quot; has occured. If the reference is not configured the error shall not be reported.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>Texas Instruments</ORIGIN>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                    </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                    <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:114789be-23fb-4d7a-9ba2-9dc214925c5a">
                      <SHORT-NAME>LIN_E_CHKSUM</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;CheckSum caused by hardware error&quot; has occured. If the reference is not configured the error shall not be reported.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>Texas Instruments</ORIGIN>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                    </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                    <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:e24c5d8a-0c81-4099-9a3d-1accb114a253">
                      <SHORT-NAME>LIN_E_OVRRUN</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;OverRun caused by hardware error&quot; has occured. If the reference is not configured the error shall not be reported.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>Texas Instruments</ORIGIN>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                    </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                    <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:427c625e-3bf6-4117-bff9-a7ac7539d543">
                      <SHORT-NAME>LIN_E_PHYBUS</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;PhysicalBus caused by hardware error&quot; has occured. If the reference is not configured the error shall not be reported.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>Texas Instruments</ORIGIN>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                    </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                    <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:a84b4c10-3485-4d8e-a1d3-cbec4165b404">
                      <SHORT-NAME>LIN_E_BIT</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;BITError caused by hardware error&quot; has occured. If the reference is not configured the error shall not be reported.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>Texas Instruments</ORIGIN>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                    </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                    <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:fe4e5c4c-edeb-4d02-952d-524b9a8f774c">
                      <SHORT-NAME>LIN_E_FRM</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;FrameError caused by hardware error&quot; has occured. If the reference is not configured the error shall not be reported.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>Texas Instruments</ORIGIN>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                    </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                    <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:76af5980-6208-4794-97a1-ba165c8bb647">
                      <SHORT-NAME>LIN_E_SYNCFIELD</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;SyncField caused by hardware error&quot; has occured. If the reference is not configured the error shall not be reported.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>Texas Instruments</ORIGIN>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                    </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                    <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:46df11ed-883c-4e06-88c0-59f6fa5c05f1">
                      <SHORT-NAME>LIN_E_PARITY</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;ParityError caused by hardware error&quot; has occured. If the reference is not configured the error shall not be reported.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <IMPLEMENTATION-CONFIG-CLASSES>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                        <ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-IMPLEMENTATION-CONFIGURATION-CLASS>
                      </IMPLEMENTATION-CONFIG-CLASSES>
                      <ORIGIN>Texas Instruments</ORIGIN>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                    </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
          </CONTAINERS>
        </ECUC-MODULE-DEF>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
