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Configured Device : Texas Instruments XDS2xx USB Debug Probe > TIVA TMA4C1294NCPDT [more info] [downlosd ccxmi] CORTEX_M4.0
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5/27/2020, 10:05:13 AM] [ERROR] CS_DAP_0: Error initializing emulator: (Error -2083 @ 0x0) Unable to communicate with the debug probe. Confirm debug probe configuration and connections, reset the debug [l

Jprobe, and retry the operation. (Emulation package 9.1.1.00002)
(5/27/2020, 10:05:22 AMI [ERROR] CS_DAP._0: Error initalizing emulator: (Error 2083 @ 0x0) Unable to communicate with the debug probe. Confirm debug probe configuration and connections, reset the debug
Jprobe, and retry the operation. (Emulation package 9.1.1.00002)

(5/27/2020, 10:05:42 AMI [ERROR] CS_DAP._0: Error initalizing emulator: (Error 2083 @ 0x0) Unable to communicate with the debug probe. Confirm debug probe configuration and connections, reset the debug
Jprobe, and retry the operation. (Emulation package 9.1.1.00002)
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