#

# Hercules Safety Microcontrollers

##

###

### Key benefits

### Key applications

- Up to 160 MHz, ARM Cortex-R4F CPU
- Lock-Step CPUs with fail safe detection logic
- Up to 2 MB of Embedded Flash Memory with ECC
- Dual 12-bit ADC, 8 redundant channels
- FlexRay, CAN, LIN, Multi-Buffered SPIs, and DMA
- Timer Co-Processer for PWM and input capture
- Package options: 144 QFP and 337 BGA

- Architected for safety critical transportation applications
- ARM Cortex-R4F with Floating Point (single and double precision)
- Automotive qualified across full temperature range
- Flexible real-time control peripherals
- Robust communication interfaces
- Development network and support

- Braking systems (ABS and ESC)
- Electric power steering (EPS)
- HEV/EV inverter systems
- Battery management systems
- Active driver assistance systems
- Aerospace and avionics
- Railway communications
- Off road vehicles

#

### Copyright © 2013 Texas Instruments Incorporated. All rights reserved.