# TMS570LC4357ZWT 10/18/23 08:47:14
# 
ARCH=TMS570LC4357ZWT
# 
DRIVER.TOOLS.VAR.GCC.VALUE=0
DRIVER.TOOLS.VAR.ARM.VALUE=0
DRIVER.TOOLS.VAR.IAR.VALUE=0
DRIVER.TOOLS.VAR.GHS.VALUE=0
DRIVER.TOOLS.VAR.TI.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_AVCLK4_DIVIDER.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_PERMISSION.VALUE=PRIV_RW_USER_RW_NOEXEC
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_TYPE.VALUE=NORMAL_OIWTNOWA_NONSHARED
DRIVER.SYSTEM.VAR.VIM_CHANNEL_122_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_114_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_106_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_70_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_62_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_54_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_46_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_38_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CAPTURE_EVENT_SOURCE_0.VALUE=0
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_1_WAIT_STATE_FREQ.VALUE=32.0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_PERMISSION_VALUE.VALUE=0x1300
DRIVER.SYSTEM.VAR.VIM_CHANNEL_81_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_73_NAME.VALUE=het2LowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_65_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_57_NAME.VALUE=adc2Group2Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_49_NAME.VALUE=mibspi4HighLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_2_MAPPING.VALUE=2
DRIVER.SYSTEM.VAR.VIM_CAPTURE_EVENT_SOURCE_1.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_SIZE.VALUE=32_BYTES
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_111_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_103_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.EQEP2_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.FLASH_DATA_3_WAIT_STATE_FREQ.VALUE=180.0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_96_MAPPING.VALUE=96
DRIVER.SYSTEM.VAR.VIM_CHANNEL_88_MAPPING.VALUE=88
DRIVER.SYSTEM.VAR.VIM_CHANNEL_1_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_END_ADDRESS.VALUE=0x0000001f
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_SUB_5_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_DATA_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_11_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.LIN2_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.SPI3_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_PLL1_BYPASS_ON_SLIP.VALUE=0x20000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_TYPE_VALUE.VALUE=0x0008
DRIVER.SYSTEM.VAR.VIM_CHANNEL_124_NAME.VALUE=epcFullInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_116_NAME.VALUE=sci4HighLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_108_NAME.VALUE=ecap5Interrupt
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_BASE_ADDRESS.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_SIZE.VALUE=128_MB
DRIVER.SYSTEM.VAR.VIM_CHANNEL_100_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_98_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_20_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_12_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_2_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.CRC_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.MIBSPI1_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_HCLK_FREQ.VALUE=150.000
DRIVER.SYSTEM.VAR.CLKT_PLL2_FREQ.VALUE=300.00
DRIVER.SYSTEM.VAR.VIM_CHANNEL_81_MAPPING.VALUE=81
DRIVER.SYSTEM.VAR.VIM_CHANNEL_73_MAPPING.VALUE=73
DRIVER.SYSTEM.VAR.VIM_CHANNEL_65_MAPPING.VALUE=65
DRIVER.SYSTEM.VAR.VIM_CHANNEL_57_MAPPING.VALUE=57
DRIVER.SYSTEM.VAR.VIM_CHANNEL_49_MAPPING.VALUE=49
DRIVER.SYSTEM.VAR.VIM_CHANNEL_40_NAME.VALUE=dmaBTCAInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_32_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_24_NAME.VALUE=het1LowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_16_NAME.VALUE=can1HighLevelInterrupt
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_92_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_84_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_76_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_68_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_31_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_23_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_15_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.ECLK_CLKSRC.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_TYPE_VALUE.VALUE=0x0006
DRIVER.SYSTEM.VAR.CLKT_PLL2_OUTPUT_DIV.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_EXT2_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CLKT_PLL1_SOURCE_ENABLE.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_END_ADDRESS.VALUE=0x6fffffff
DRIVER.SYSTEM.VAR.VIM_CHANNEL_96_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_88_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_9_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_4_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_RTI2_PRE_SOURCE.VALUE=PLL1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_SIZE_VALUE.VALUE=0x1A
DRIVER.SYSTEM.VAR.VIM_CHANNEL_99_NAME.VALUE=etpwm5TripZoneInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_50_MAPPING.VALUE=50
DRIVER.SYSTEM.VAR.VIM_CHANNEL_42_MAPPING.VALUE=42
DRIVER.SYSTEM.VAR.VIM_CHANNEL_34_MAPPING.VALUE=34
DRIVER.SYSTEM.VAR.VIM_CHANNEL_26_MAPPING.VALUE=26
DRIVER.SYSTEM.VAR.VIM_CHANNEL_18_MAPPING.VALUE=18
DRIVER.SYSTEM.VAR.CLKT_VCLK3_DOMAIN_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.FLASH_ECC_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.FLASH_BANKS.VALUE=4
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_TYPE.VALUE=NORMAL_OIWTNOWA_SHARED
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_IRQ_DISP_ENTRY.VALUE=_irqDispatch
DRIVER.SYSTEM.VAR.VIM_CHANNEL_111_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_103_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_92_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_84_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_76_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_68_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CAN3_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_AVCLK1_SOURCE.VALUE=VCLK
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.ETPWM4_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.DCC2_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_PLL1_RESET_ON_OSCILLATOR_FAIL.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_PERMISSION_VALUE.VALUE=0x0600
DRIVER.SYSTEM.VAR.VIM_CHANNEL_11_MAPPING.VALUE=11
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_PERMISSION.VALUE=PRIV_RW_USER_RW_NOEXEC
DRIVER.SYSTEM.VAR.LBIST_ENA.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_AVCLK2_DOMAIN_ENABLE.VALUE=TRUE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_TYPE.VALUE=NORMAL_OIWBWA_NONSHARED
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_END_ADDRESS.VALUE=0x003fffff
DRIVER.SYSTEM.VAR.VIM_CHANNEL_41_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_33_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_25_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_17_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_3_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ECAP6_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.SCI_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.FLASH_DATA_1_WAIT_STATE_FREQ.VALUE=90.0
DRIVER.SYSTEM.VAR.RAM_STACK_IRQ_BASE.VALUE=0x08001200
DRIVER.SYSTEM.VAR.VIM_CHANNEL_125_MAPPING.VALUE=125
DRIVER.SYSTEM.VAR.VIM_CHANNEL_117_MAPPING.VALUE=117
DRIVER.SYSTEM.VAR.VIM_CHANNEL_109_MAPPING.VALUE=109
DRIVER.SYSTEM.VAR.VIM_CHANNEL_90_NAME.VALUE=etpwm1Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_82_NAME.VALUE=dcc1DoneInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_74_NAME.VALUE=sciLowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_66_NAME.VALUE=i2cInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_58_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.CLKT_AVCLK3_DOMAIN_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_PMU_GLOBAL_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_SIZE.VALUE=512_KB
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_END_ADDRESS.VALUE=0x0000001f
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_BASE_ADDRESS.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_97_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_89_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_81_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_73_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_70_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_65_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_62_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_57_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_54_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_49_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_46_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_38_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.EMAC_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_8_MAPPING.VALUE=8
DRIVER.SYSTEM.VAR.VIM_CHANNEL_2_NAME.VALUE=rtiCompare0Interrupt
DRIVER.SYSTEM.VAR.CORE_PMU_COUNTER0_EVENT.VALUE=0x11
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_PERMISSION.VALUE=PRIV_RO_USER_RO_NOEXEC
DRIVER.SYSTEM.VAR.FLASH_ADDRESS_WAIT_STATES.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_RESET_ENTRY.VALUE=_c_int00
DRIVER.SYSTEM.VAR.VIM_CHANNEL_127_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_122_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_119_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_114_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_106_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_9_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.ADC1_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.MIBSPI_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ECLK_VCLK1_FREQ.VALUE=75.000
DRIVER.SYSTEM.VAR.CLKT_EXTERNAL_FREQ.VALUE=00.0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_SIZE_VALUE.VALUE=0x04
DRIVER.SYSTEM.VAR.VIM_CHANNEL_125_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_117_NAME.VALUE=can4LowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_110_MAPPING.VALUE=110
DRIVER.SYSTEM.VAR.VIM_CHANNEL_109_NAME.VALUE=ecap6Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_102_MAPPING.VALUE=102
DRIVER.SYSTEM.VAR.CLKT_AVCLK3_DIVIDER.VALUE=1
DRIVER.SYSTEM.VAR.RAM_LENGTH.VALUE=0x00080000
DRIVER.SYSTEM.VAR.CLKT_VCLK1_DOMAIN_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_SIZE.VALUE=256_MB
DRIVER.SYSTEM.VAR.VIM_CHANNEL_124_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_116_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_108_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.I2C2_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_41_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_33_NAME.VALUE=dmaFTCAInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_25_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_17_NAME.VALUE=spi2HighLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_1_MAPPING.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_EXTERNAL_SOURCE_ENABLE.VALUE=0x00000008
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_END_ADDRESS.VALUE=0x0000001f
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_BASE_ADDRESS.VALUE=0xF0000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_40_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_32_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_24_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_16_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_5_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_PERMISSION_VALUE.VALUE=0x1200
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_TYPE_VALUE.VALUE=0x0006
DRIVER.SYSTEM.VAR.VIM_CHANNEL_95_MAPPING.VALUE=95
DRIVER.SYSTEM.VAR.VIM_CHANNEL_87_MAPPING.VALUE=87
DRIVER.SYSTEM.VAR.VIM_CHANNEL_79_MAPPING.VALUE=79
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_SUB_4_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_IRQ_VIC_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_121_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_113_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_105_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_70_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_62_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_54_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_50_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_46_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_42_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_38_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_34_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_26_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_18_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.SPI1_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_8_WAIT_STATE_FREQ.VALUE=144.0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_100_NAME.VALUE=etpwm6Interrupt
DRIVER.SYSTEM.VAR.CLKT_RTI2_DIVIDER.VALUE=1
DRIVER.SYSTEM.VAR.RAM_ECC_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_TYPE.VALUE=NORMAL_OIWTNOWA_SHARED
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_SUB_7_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_99_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.CLKT_EXTERNAL_FREQ_INPUT.VALUE=16.0
DRIVER.SYSTEM.VAR.STC_INTERVAL.VALUE=40
DRIVER.SYSTEM.VAR.CLKT_LPO_HIGH_TRIM_VALUE.VALUE=16
DRIVER.SYSTEM.VAR.CLKT_GCLK_FREQ.VALUE=300.000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_PERMISSION_VALUE.VALUE=0x1000
DRIVER.SYSTEM.VAR.VIM_CHANNEL_80_MAPPING.VALUE=80
DRIVER.SYSTEM.VAR.VIM_CHANNEL_72_MAPPING.VALUE=72
DRIVER.SYSTEM.VAR.VIM_CHANNEL_64_MAPPING.VALUE=64
DRIVER.SYSTEM.VAR.VIM_CHANNEL_56_MAPPING.VALUE=56
DRIVER.SYSTEM.VAR.VIM_CHANNEL_48_MAPPING.VALUE=48
DRIVER.SYSTEM.VAR.CLKT_PLL1_REF_CLOCK_DIV.VALUE=8
DRIVER.SYSTEM.VAR.FLASHW_BASE_ADDRESS.VALUE=0xFFF87000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_FIQ_ENTRY.VALUE="ldr pc,[pc,#-0x1b0]"
DRIVER.SYSTEM.VAR.VIM_CHANNEL_10_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.SCILIN_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.SPI_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ALL_DVR_ENA.VALUE=0
DRIVER.SYSTEM.VAR.CCM_MENU_VALUE.VALUE=0x0001
DRIVER.SYSTEM.VAR.PBIST_ENA1.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_VCLK4_DIVIDER.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_TYPE.VALUE=DEVICE_NONSHAREABLE
DRIVER.SYSTEM.VAR.VIM_CHANNEL_97_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_89_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_OSCILLATOR_FREQ.VALUE=16.0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_91_NAME.VALUE=etpwm1TripZoneInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_83_NAME.VALUE=dcc2DoneInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_75_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_67_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_59_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_41_MAPPING.VALUE=41
DRIVER.SYSTEM.VAR.VIM_CHANNEL_33_MAPPING.VALUE=33
DRIVER.SYSTEM.VAR.VIM_CHANNEL_25_MAPPING.VALUE=25
DRIVER.SYSTEM.VAR.VIM_CHANNEL_17_MAPPING.VALUE=17
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_IRQ_MODE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_11_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_11_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.PMM_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.EMIF_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CAN1_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CAN_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_TYPE_VALUE.VALUE=0x0006
DRIVER.SYSTEM.VAR.VIM_CHANNEL_3_NAME.VALUE=rtiCompare1Interrupt
DRIVER.SYSTEM.VAR.CLKT_PLL1_OUTPUT_DIV.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_PERMISSION.VALUE=PRIV_RW_USER_RO_NOEXEC
DRIVER.SYSTEM.VAR.CLKT_PLL2_FM_ENABLE.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_BASE_ADDRESS.VALUE=0xF8000000
DRIVER.SYSTEM.VAR.VIM_CHANNEL_92_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_91_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_84_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_83_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_76_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_75_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_68_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_67_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_59_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_8_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ETPWM2_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.HET1_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_RTI1_PRE_SOURCE.VALUE=PLL1
DRIVER.SYSTEM.VAR.FLASH_MODE_VALUE.VALUE=3
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_SIZE_VALUE.VALUE=0x1B
DRIVER.SYSTEM.VAR.VIM_CHANNEL_126_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_118_NAME.VALUE=lin2LowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_10_MAPPING.VALUE=10
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_SIZE.VALUE=128_MB
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_125_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_117_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_109_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_91_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_83_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_75_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_67_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_59_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_3_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.ECAP4_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_PLL2_BYPASS_ON_SLIP.VALUE=0x20000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_PERMISSION_VALUE.VALUE=0x1600
DRIVER.SYSTEM.VAR.VIM_CHANNEL_124_MAPPING.VALUE=124
DRIVER.SYSTEM.VAR.VIM_CHANNEL_116_MAPPING.VALUE=116
DRIVER.SYSTEM.VAR.VIM_CHANNEL_108_MAPPING.VALUE=108
DRIVER.SYSTEM.VAR.VIM_CHANNEL_50_NAME.VALUE=adc2Group0Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_42_NAME.VALUE=can2LowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_34_NAME.VALUE=dmaLFSAInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_26_NAME.VALUE=mibspi1LowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_18_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.FLASH_ARBITRATION.VALUE=FIX
DRIVER.SYSTEM.VAR.CLKT_LPO_HIGH_SOURCE_ENABLE.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_110_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_102_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.SCI4_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.PBIST_ALGO_9_10.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_EXTERNAL2_FREQ_INPUT.VALUE=16.0
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_6_WAIT_STATE_FREQ.VALUE=112.0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_SIZE_VALUE.VALUE=0x12
DRIVER.SYSTEM.VAR.VIM_CHANNEL_7_MAPPING.VALUE=7
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_PERMISSION.VALUE=PRIV_RW_USER_RW_NOEXEC
DRIVER.SYSTEM.VAR.CLKT_RTI2_DOMAIN_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_BACKGROUND_REGION_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_8_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_2_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CONFIG.VALUE=TRUE
DRIVER.SYSTEM.VAR.CRC2_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_101_MAPPING.VALUE=101
DRIVER.SYSTEM.VAR.VIM_CHANNEL_101_NAME.VALUE=etpwm6TripZoneInterrupt
DRIVER.SYSTEM.VAR.RAM_STACK_ABORT_LENGTH.VALUE=0x00000100
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_WAIT_STATES.VALUE=9
DRIVER.SYSTEM.VAR.FLASH_DATA_MAX_WAIT_STATES.VALUE=3
DRIVER.SYSTEM.VAR.FLASH_MODE.VALUE=PIPELINE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_TYPE.VALUE=DEVICE_NONSHAREABLE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_61_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_61_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_53_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_53_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_45_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_45_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_40_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_37_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_37_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_32_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_29_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_29_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_24_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_16_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.MINIT_VALUE.VALUE=0x1E57F
DRIVER.SYSTEM.VAR.VIM_CHANNEL_0_MAPPING.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_PLL1_DIV.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_PERMISSION.VALUE=PRIV_RO_USER_RO_NOEXEC
DRIVER.SYSTEM.VAR.CLKT_VCLK4_DOMAIN_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_PLL2_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.RAM_BASE_ADDRESS.VALUE=0x08000000
DRIVER.SYSTEM.VAR.CORE_PMU_EVENT_EXPORT_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_SUB_2_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_126_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_118_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_110_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_102_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_96_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_88_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.GIO_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_SIZE_VALUE.VALUE=0x04
DRIVER.SYSTEM.VAR.VIM_CHANNEL_94_MAPPING.VALUE=94
DRIVER.SYSTEM.VAR.VIM_CHANNEL_86_MAPPING.VALUE=86
DRIVER.SYSTEM.VAR.VIM_CHANNEL_78_MAPPING.VALUE=78
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_TYPE.VALUE=STRONGLYORDERED_SHAREABLE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_SUB_3_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_BASE_ADDRESS.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_UNDEF_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_8_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.MIBSPI4_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.RAM_STACK_ABORT_BASE.VALUE=0x08001300
DRIVER.SYSTEM.VAR.VIM_CHANNEL_92_NAME.VALUE=etpwm2Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_84_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_76_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_68_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.CLKT_RTI1_DIVIDER.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_AVCLK4_DOMAIN_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_SUB_6_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_123_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_115_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_107_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_31_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_23_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_15_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_1_INT_TYPE.VALUE=FIQ
DRIVER.SYSTEM.VAR.CLKT_GHV_WAKUP_SOURCE.VALUE=PLL1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_TYPE_VALUE.VALUE=0x0000
DRIVER.SYSTEM.VAR.VIM_CHANNEL_71_MAPPING.VALUE=71
DRIVER.SYSTEM.VAR.VIM_CHANNEL_63_MAPPING.VALUE=63
DRIVER.SYSTEM.VAR.VIM_CHANNEL_55_MAPPING.VALUE=55
DRIVER.SYSTEM.VAR.VIM_CHANNEL_47_MAPPING.VALUE=47
DRIVER.SYSTEM.VAR.VIM_CHANNEL_39_MAPPING.VALUE=39
DRIVER.SYSTEM.VAR.VIM_CHANNEL_4_NAME.VALUE=rtiCompare2Interrupt
DRIVER.SYSTEM.VAR.CLKT_HCLK_DIVIDER.VALUE=1
DRIVER.SYSTEM.VAR.CORE_PMU_COUNTER1_EVENT.VALUE=0x11
DRIVER.SYSTEM.VAR.EFUSE_SELFTEST_ENA.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_AVCLK4_DOMAIN_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.RAM_LINK_BASE_ADDRESS.VALUE=0x08001500
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_BASE_ADDRESS.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_120_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_112_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_104_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_30_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_22_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_14_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_PERMISSION_VALUE.VALUE=0x1600
DRIVER.SYSTEM.VAR.VIM_CHANNEL_127_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_119_NAME.VALUE=sci4LowLevelInterrupt
DRIVER.SYSTEM.VAR.CLKT_PLL2_DIV.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_VCLK3_DIVIDER.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_LPO_TRIM_OTP_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_SIZE.VALUE=8_MB
DRIVER.SYSTEM.VAR.VIM_CHANNEL_95_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_87_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_79_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_61_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_53_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_45_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_37_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_29_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_AVCLK4_SOURCE.VALUE=VCLK
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_4_WAIT_STATE_FREQ.VALUE=80.0
DRIVER.SYSTEM.VAR.FLASH_ADDRESS_WAIT_STATES_FREQ.VALUE=120.0
DRIVER.SYSTEM.VAR.RAM_STACK_BASE.VALUE=0x08000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_TYPE_VALUE.VALUE=0x0010
DRIVER.SYSTEM.VAR.VIM_CHANNEL_51_NAME.VALUE=adc2Group1Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_43_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_40_MAPPING.VALUE=40
DRIVER.SYSTEM.VAR.VIM_CHANNEL_35_NAME.VALUE=can2HighLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_32_MAPPING.VALUE=32
DRIVER.SYSTEM.VAR.VIM_CHANNEL_27_NAME.VALUE=lin1LowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_24_MAPPING.VALUE=24
DRIVER.SYSTEM.VAR.VIM_CHANNEL_19_NAME.VALUE=crcInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_16_MAPPING.VALUE=16
DRIVER.SYSTEM.VAR.CLKT_VCLK3_DOMAIN_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_END_ADDRESS.VALUE=0xf07fffff
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.ETPWM7_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_1.VALUE=0
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_2.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_96_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_88_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_3.VALUE=0
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_4.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_110_NAME.VALUE=eqep1Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_102_NAME.VALUE=etpwm7Interrupt
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_5.VALUE=0
DRIVER.SYSTEM.VAR.LBIST_STT.VALUE=1
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_6.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_ECC_AVAILABLE.VALUE=TRUE
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_7.VALUE=0
DRIVER.SYSTEM.VAR.ECAP2_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_8.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_TYPE_VALUE.VALUE=0x000C
DRIVER.SYSTEM.VAR.VIM_CHANNEL_123_MAPPING.VALUE=123
DRIVER.SYSTEM.VAR.VIM_CHANNEL_115_MAPPING.VALUE=115
DRIVER.SYSTEM.VAR.VIM_CHANNEL_107_MAPPING.VALUE=107
DRIVER.SYSTEM.VAR.VIM_CHANNEL_10_NAME.VALUE=het1HighLevelInterrupt
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_9.VALUE=0
DRIVER.SYSTEM.VAR.RAM_STACK_USER_LENGTH.VALUE=0x00001000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_PERMISSION.VALUE=PRIV_RW_USER_RO_NOEXEC
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_END_ADDRESS.VALUE=0xffffffff
DRIVER.SYSTEM.VAR.CORE_CACHE_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_80_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_72_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_64_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_56_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_48_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_10_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_7_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.SCI2_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.LIN_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_RTI1_FREQ.VALUE=75.000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_SIZE_VALUE.VALUE=0x1A
DRIVER.SYSTEM.VAR.VIM_CHANNEL_6_MAPPING.VALUE=6
DRIVER.SYSTEM.VAR.CLKT_PLL2_SPEADING_AMOUNT.VALUE=61
DRIVER.SYSTEM.VAR.CLKT_PLL2_SPEADING_RATE.VALUE=255
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_BASE_ADDRESS.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_TYPE.VALUE=NORMAL_OIWTNOWA_SHARED
DRIVER.SYSTEM.VAR.VIM_CHANNEL_121_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_113_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_105_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_90_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_90_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_82_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_82_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_74_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_74_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_66_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_66_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_58_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_58_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_PLL2_RESET_ON_SLIP.VALUE=0x00000000
DRIVER.SYSTEM.VAR.ECLK_FREQ.VALUE=9.375
DRIVER.SYSTEM.VAR.CLKT_AVCLK1_FREQ.VALUE=75.000
DRIVER.SYSTEM.VAR.VIM_CHANNEL_100_MAPPING.VALUE=100
DRIVER.SYSTEM.VAR.VIM_CHANNEL_93_NAME.VALUE=etpwm2TripZoneInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_85_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_77_NAME.VALUE=EMACTxIntISR
DRIVER.SYSTEM.VAR.VIM_CHANNEL_69_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.RAM_STACK_IRQ_LENGTH.VALUE=0x00000100
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_2_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_RTI2_POST_SOURCE.VALUE=VCLK
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_10_WAIT_STATE_FREQ.VALUE=176.0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_SIZE_VALUE.VALUE=0x04
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_PERMISSION_VALUE.VALUE=0x1600
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_PERMISSION_VALUE.VALUE=0x1200
DRIVER.SYSTEM.VAR.VIM_CHANNEL_5_NAME.VALUE=rtiCompare3Interrupt
DRIVER.SYSTEM.VAR.RAM_STACK_LENGTH.VALUE=0x00001500
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_PERMISSION.VALUE=PRIV_RO_USER_RO_EXEC
DRIVER.SYSTEM.VAR.CLKT_LPO_BIAS.VALUE=true
DRIVER.SYSTEM.VAR.CLKT_AVCLK3_DIVIDER1.VALUE=4
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_SUB_1_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_END_ADDRESS.VALUE=0xffffffff
DRIVER.SYSTEM.VAR.CORE_PRAGMA_ENA.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_101_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_4_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_1_INT_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.SPI4_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_AVCLK4_POST_SOURCE.VALUE=VCLKA4_DIVR
DRIVER.SYSTEM.VAR.CLKT_VCLK1_FREQ.VALUE=75.000
DRIVER.SYSTEM.VAR.CLKT_AVCLK3_FREQ1.VALUE=75.000
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_2_WAIT_STATE_FREQ.VALUE=48.0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_93_MAPPING.VALUE=93
DRIVER.SYSTEM.VAR.VIM_CHANNEL_85_MAPPING.VALUE=85
DRIVER.SYSTEM.VAR.VIM_CHANNEL_77_MAPPING.VALUE=77
DRIVER.SYSTEM.VAR.VIM_CHANNEL_69_MAPPING.VALUE=69
DRIVER.SYSTEM.VAR.CLKT_AVCLK3_FREQ2.VALUE=18.750
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_END_ADDRESS.VALUE=0x0000001f
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_SIZE.VALUE=32_BYTES
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_BASE_ADDRESS.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_SUB_2_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_60_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_52_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_44_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_41_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_36_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_33_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_28_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_25_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_17_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.MIBSPI2_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_PLL1_MUL.VALUE=150
DRIVER.SYSTEM.VAR.VIM_CHANNEL_60_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_52_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_44_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_36_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_28_NAME.VALUE=adc1Group2Interrupt
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_PERMISSION.VALUE=PRIV_RO_USER_RO_NOEXEC
DRIVER.SYSTEM.VAR.CLKT_OSC_ENABLE.VALUE=TRUE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_SIZE.VALUE=32_BYTES
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_SVC_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_125_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_117_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_109_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_98_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_31_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_23_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_15_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.PINMUX_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.PBIST_ALGO_3_4.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_LPO_BIAS_VALUE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_70_MAPPING.VALUE=70
DRIVER.SYSTEM.VAR.VIM_CHANNEL_62_MAPPING.VALUE=62
DRIVER.SYSTEM.VAR.VIM_CHANNEL_54_MAPPING.VALUE=54
DRIVER.SYSTEM.VAR.VIM_CHANNEL_46_MAPPING.VALUE=46
DRIVER.SYSTEM.VAR.VIM_CHANNEL_38_MAPPING.VALUE=38
DRIVER.SYSTEM.VAR.CLKT_AVCLK1_DOMAIN_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CLKT_EXTERNAL2_SOURCE_ENABLE.VALUE=0x00000080
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_PREFETCH_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_95_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_87_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_79_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.PBIST_ALGO_15.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_111_NAME.VALUE=eqep2Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_103_NAME.VALUE=etpwm7TripZoneInterrupt
DRIVER.SYSTEM.VAR.PBIST_ALGO_16.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_VCLK2_DIVIDER.VALUE=1
DRIVER.SYSTEM.VAR.RAM_LINK_LENGTH.VALUE=0x0007EB00
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_END_ADDRESS.VALUE=0x0000001f
DRIVER.SYSTEM.VAR.VIM_CHANNEL_30_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_22_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_14_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_7_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CAN4_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_LPO_OSCFRQCONFIGCNT_VALUE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_AVCLK2_SOURCE.VALUE=VCLK
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_TYPE_VALUE.VALUE=0x0010
DRIVER.SYSTEM.VAR.VIM_CHANNEL_31_MAPPING.VALUE=31
DRIVER.SYSTEM.VAR.VIM_CHANNEL_23_MAPPING.VALUE=23
DRIVER.SYSTEM.VAR.VIM_CHANNEL_15_MAPPING.VALUE=15
DRIVER.SYSTEM.VAR.VIM_CHANNEL_11_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.PBIST_ALGO_5_6.VALUE=0
DRIVER.SYSTEM.VAR.PBIST_ENA.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_HCLK_DOMAIN_ENABLE.VALUE=TRUE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_122_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_114_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_111_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_106_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_103_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_10_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.ETPWM5_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.ETPWM_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_PLL2_MUL.VALUE=150
DRIVER.SYSTEM.VAR.CLKT_RTI2_FREQ.VALUE=0.0
DRIVER.SYSTEM.VAR.CLKT_LPO_LOW_FREQ.VALUE=0.080
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_TYPE.VALUE=NORMAL_OINC_NONSHARED
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_PREFETCH_ENTRY.VALUE=_prefetch
DRIVER.SYSTEM.VAR.VIM_CHANNEL_91_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_83_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_75_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_67_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_59_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.CLKT_AVCLK2_FREQ.VALUE=0.000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_TYPE_VALUE.VALUE=0x0006
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_PERMISSION_VALUE.VALUE=0x1600
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_PERMISSION_VALUE.VALUE=0x1200
DRIVER.SYSTEM.VAR.VIM_CHANNEL_94_NAME.VALUE=etpwm3Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_86_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_78_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.ECLK_PORT_BIT0_PULDIS.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_OSCILLATOR_SOURCE_ENABLE.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_BASE_ADDRESS.VALUE=0x60000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_124_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_116_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_108_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_60_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_52_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_44_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_36_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_28_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.PBIST_ALGO_7_8.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_PLL2_RESET_ON_OSCILLATOR_FAIL.VALUE=0x00000000
DRIVER.SYSTEM.VAR.FLASH_BANK_LINK_BASE_ADDRESS_0.VALUE=0x00000020
DRIVER.SYSTEM.VAR.FLASH_BANK_LINK_BASE_ADDRESS_1.VALUE=0x00200000
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_0_WAIT_STATE_FREQ.VALUE=16.0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_SIZE_VALUE.VALUE=0x04
DRIVER.SYSTEM.VAR.VIM_CHANNEL_122_MAPPING.VALUE=122
DRIVER.SYSTEM.VAR.VIM_CHANNEL_114_MAPPING.VALUE=114
DRIVER.SYSTEM.VAR.VIM_CHANNEL_106_MAPPING.VALUE=106
DRIVER.SYSTEM.VAR.VIM_CHANNEL_6_NAME.VALUE=rtiOverflow0Interrupt
DRIVER.SYSTEM.VAR.CORE_PMU_COUNTER2_EVENT.VALUE=0x11
DRIVER.SYSTEM.VAR.FLASH_DATA_WAIT_STATES.VALUE=3
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_95_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_87_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_79_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ADC2_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_VCLK2_FREQ.VALUE=75.000
DRIVER.SYSTEM.VAR.FLASH_DATA_2_WAIT_STATE_FREQ.VALUE=135.0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_5_MAPPING.VALUE=5
DRIVER.SYSTEM.VAR.VIM_CHANNELS.VALUE=128
DRIVER.SYSTEM.VAR.FLASH_BANK_LINK_BASE_ADDRESS_7.VALUE=0xF0200000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_SIZE.VALUE=32_BYTES
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_7_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.ESM_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_99_MAPPING.VALUE=99
DRIVER.SYSTEM.VAR.VIM_CHANNEL_61_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_53_NAME.VALUE=mibspi5HighLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_45_NAME.VALUE=can3HighLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_37_NAME.VALUE=mibspi3HighInterruptLevel
DRIVER.SYSTEM.VAR.VIM_CHANNEL_29_NAME.VALUE=can1LowLevelInterrupt
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_PERMISSION.VALUE=PRIV_RW_USER_RO_NOEXEC
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_SIZE.VALUE=32_BYTES
DRIVER.SYSTEM.VAR.VIM_CHANNEL_127_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_119_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_60_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_52_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_44_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_36_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_28_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_6_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.EQEP1_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_LPO_HIGH_FREQ.VALUE=10.000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_SIZE_VALUE.VALUE=0x12
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_SUB_0_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_IRQ_ENTRY.VALUE="ldr pc,[pc,#-0x1b0]"
DRIVER.SYSTEM.VAR.VIM_CHANNEL_101_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_81_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_73_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_65_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_57_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_49_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ECAP_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.LIN1_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.SPI2_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_GHV_POWER_DOWN_SOURCE.VALUE=PLL1
DRIVER.SYSTEM.VAR.RAM_STACK_USER_BASE.VALUE=0x08000000
DRIVER.SYSTEM.VAR.VIM_CHANNEL_120_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_112_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_104_NAME.VALUE=ecap1Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_92_MAPPING.VALUE=92
DRIVER.SYSTEM.VAR.VIM_CHANNEL_84_MAPPING.VALUE=84
DRIVER.SYSTEM.VAR.VIM_CHANNEL_76_MAPPING.VALUE=76
DRIVER.SYSTEM.VAR.VIM_CHANNEL_68_MAPPING.VALUE=68
DRIVER.SYSTEM.VAR.CLKT_GCLK_DOMAIN_ENABLE.VALUE=TRUE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_SUB_1_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_81_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_73_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_65_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_57_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_49_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.SYSTEM_INIT.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_SIZE_VALUE.VALUE=0x04
DRIVER.SYSTEM.VAR.VIM_CHANNEL_20_NAME.VALUE=esmLowInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_12_NAME.VALUE=mibspi1HighLevelInterrupt
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_PERMISSION.VALUE=PRIV_NA_USER_NA_NOEXEC
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_BASE_ADDRESS.VALUE=0x00000000
DRIVER.SYSTEM.VAR.VIM_CHANNEL_1_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_0_INT_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_0_INT_TYPE.VALUE=FIQ
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_9_WAIT_STATE_FREQ.VALUE=160.0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_PERMISSION_VALUE.VALUE=0x0600
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_PERMISSION_VALUE.VALUE=0x1200
DRIVER.SYSTEM.VAR.VIM_CHANNEL_61_MAPPING.VALUE=61
DRIVER.SYSTEM.VAR.VIM_CHANNEL_53_MAPPING.VALUE=53
DRIVER.SYSTEM.VAR.VIM_CHANNEL_45_MAPPING.VALUE=45
DRIVER.SYSTEM.VAR.VIM_CHANNEL_37_MAPPING.VALUE=37
DRIVER.SYSTEM.VAR.VIM_CHANNEL_29_MAPPING.VALUE=29
DRIVER.SYSTEM.VAR.ECLK_PORT_BIT0_DIR.VALUE=1
DRIVER.SYSTEM.VAR.FLASH_LENGTH.VALUE=0x00400000
DRIVER.SYSTEM.VAR.RAM_STACK_FIQ_LENGTH.VALUE=0x00000100
DRIVER.SYSTEM.VAR.CLKT_EXT1_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_TYPE.VALUE=DEVICE_NONSHAREABLE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_100_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_51_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_43_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_35_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_27_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_21_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_19_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_13_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_ECC_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_AVCLK3_FREQ.VALUE=75.000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_TYPE_VALUE.VALUE=0x0006
DRIVER.SYSTEM.VAR.VIM_CHANNEL_95_NAME.VALUE=etpwm3TripZoneInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_87_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_79_NAME.VALUE=EMACRxIntISR
DRIVER.SYSTEM.VAR.CLKT_VCLK1_DIVIDER.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_PERMISSION.VALUE=PRIV_RO_USER_RO_NOEXEC
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_BASE_ADDRESS.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_TYPE.VALUE=NORMAL_OIWTNOWA_SHARED
DRIVER.SYSTEM.VAR.VIM_CHANNEL_124_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_116_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_108_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_94_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_86_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_78_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.CAN2_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ECLK_PORT_BIT0_DOUT.VALUE=0
DRIVER.SYSTEM.VAR.PBIST_ALGO_1.VALUE=0
DRIVER.SYSTEM.VAR.FLASH_DATA_0_WAIT_STATE_FREQ.VALUE=45.0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_30_MAPPING.VALUE=30
DRIVER.SYSTEM.VAR.VIM_CHANNEL_22_MAPPING.VALUE=22
DRIVER.SYSTEM.VAR.VIM_CHANNEL_14_MAPPING.VALUE=14
DRIVER.SYSTEM.VAR.VIM_CHANNEL_7_NAME.VALUE=rtiOverflow1Interrupt
DRIVER.SYSTEM.VAR.PBIST_ALGO_2.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_RTI1_DOMAIN_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CLKT_AVCLK1_DOMAIN_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_127_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_119_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_30_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_22_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_14_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.ETPWM3_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.DCC1_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.HET2_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_VCLK3_FREQ.VALUE=75.000
DRIVER.SYSTEM.VAR.CLKT_AVCLK4_FREQ1.VALUE=75.000
DRIVER.SYSTEM.VAR.PBIST_ALGO_11_12.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_PLL2_SOURCE_ENABLE.VALUE=0x00000000
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_MAX_WAIT_STATES.VALUE=11
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_END_ADDRESS.VALUE=0x0000001f
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_94_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_86_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_78_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_21_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_13_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ECAP5_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.ADC_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_TYPE_VALUE.VALUE=0x000B
DRIVER.SYSTEM.VAR.VIM_CHANNEL_70_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_62_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_54_NAME.VALUE=mibspi4LowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_46_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_38_NAME.VALUE=mibspi3LowLevelInterrupt
DRIVER.SYSTEM.VAR.FEE_FLASH_ECC_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_SIZE.VALUE=32_BYTES
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_RESET_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_110_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_102_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_6_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_121_MAPPING.VALUE=121
DRIVER.SYSTEM.VAR.VIM_CHANNEL_113_MAPPING.VALUE=113
DRIVER.SYSTEM.VAR.VIM_CHANNEL_105_MAPPING.VALUE=105
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_RESERVED_ENTRY.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_121_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_113_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_105_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_71_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_63_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_55_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_47_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_39_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_TYPE_VALUE.VALUE=0x0006
DRIVER.SYSTEM.VAR.VIM_CHANNEL_121_NAME.VALUE=crc2Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_113_NAME.VALUE=can4HighLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_105_NAME.VALUE=ecap2Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_4_MAPPING.VALUE=4
DRIVER.SYSTEM.VAR.CLKT_AVCLK3_DOMAIN_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_END_ADDRESS.VALUE=0x87ffffff
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_SIZE.VALUE=4_GB
DRIVER.SYSTEM.VAR.VIM_CHANNEL_120_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_112_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_104_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.I2C1_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_7_WAIT_STATE_FREQ.VALUE=128.0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_PERMISSION_VALUE.VALUE=0x1300
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_SIZE_VALUE.VALUE=0x04
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_PERMISSION_VALUE.VALUE=0x0300
DRIVER.SYSTEM.VAR.VIM_CHANNEL_98_MAPPING.VALUE=98
DRIVER.SYSTEM.VAR.VIM_CHANNEL_21_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_13_NAME.VALUE=lin1HighLevelInterrupt
DRIVER.SYSTEM.VAR.ECLK_PORT_BIT0_FUN.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_BASE_ADDRESS.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_SUB_7_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_94_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_86_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_78_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_51_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_43_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_35_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_27_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_19_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.HET_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.PBIST_ALGO_13_14.VALUE=0
DRIVER.SYSTEM.VAR.RAM_STACK_UNDEF_BASE.VALUE=0x08001400
DRIVER.SYSTEM.VAR.RAM_STACK_SVC_BASE.VALUE=0x08001000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_TYPE.VALUE=NORMAL_OIWTNOWA_SHARED
DRIVER.SYSTEM.VAR.VIM_CHANNEL_99_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_3_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.DMM_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.MIBSPI5_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.FLASH_BANK_CONFIG_0.VALUE=ACTIVE
DRIVER.SYSTEM.VAR.CLKT_AVCLK4_FREQ.VALUE=75.000
DRIVER.SYSTEM.VAR.FLASH_BANK_CONFIG_1.VALUE=ACTIVE
DRIVER.SYSTEM.VAR.VIM_CHANNEL_96_NAME.VALUE=etpwm4Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_91_MAPPING.VALUE=91
DRIVER.SYSTEM.VAR.VIM_CHANNEL_88_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_83_MAPPING.VALUE=83
DRIVER.SYSTEM.VAR.VIM_CHANNEL_75_MAPPING.VALUE=75
DRIVER.SYSTEM.VAR.VIM_CHANNEL_67_MAPPING.VALUE=67
DRIVER.SYSTEM.VAR.VIM_CHANNEL_59_MAPPING.VALUE=59
DRIVER.SYSTEM.VAR.FLASH_BANK_CONFIG_2.VALUE=SLEEP
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_PERMISSION.VALUE=PRIV_RW_USER_RW_EXEC
DRIVER.SYSTEM.VAR.CLKT_VCLK2_DOMAIN_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.FLASH_BANK_CONFIG_3.VALUE=SLEEP
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_TYPE.VALUE=NORMAL_OIWTNOWA_SHARED
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_END_ADDRESS.VALUE=0x0807ffff
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_SUB_0_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_40_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_32_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_24_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_16_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_5_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ECLK_PORT_BIT0_PDR.VALUE=0
DRIVER.SYSTEM.VAR.FLASH_BANK_CONFIG_4.VALUE=SLEEP
DRIVER.SYSTEM.VAR.FLASH_BANK_CONFIG_5.VALUE=SLEEP
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_SIZE_VALUE.VALUE=0x15
DRIVER.SYSTEM.VAR.VIM_CHANNEL_8_NAME.VALUE=rtiTimebaseInterrupt
DRIVER.SYSTEM.VAR.ECLK_PRESCALER.VALUE=8
DRIVER.SYSTEM.VAR.FLASH_BANK_CONFIG_6.VALUE=SLEEP
DRIVER.SYSTEM.VAR.FLASH_BANK_CONFIG_7.VALUE=ACTIVE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_END_ADDRESS.VALUE=0xffffffff
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_BASE_ADDRESS.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_126_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_118_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_97_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_89_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_80_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_72_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_64_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_56_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_48_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_VCLK4_FREQ.VALUE=75.0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_60_MAPPING.VALUE=60
DRIVER.SYSTEM.VAR.VIM_CHANNEL_52_MAPPING.VALUE=52
DRIVER.SYSTEM.VAR.VIM_CHANNEL_44_MAPPING.VALUE=44
DRIVER.SYSTEM.VAR.VIM_CHANNEL_36_MAPPING.VALUE=36
DRIVER.SYSTEM.VAR.VIM_CHANNEL_28_MAPPING.VALUE=28
DRIVER.SYSTEM.VAR.CLKT_PLL1_BAND_WIDTH_ADJUSTMENT.VALUE=7
DRIVER.SYSTEM.VAR.CLKT_LPO_LOW_SOURCE_ENABLE.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_PLL2_MUL_VAL.VALUE=9500
DRIVER.SYSTEM.VAR.CLKT_RTI1_POST_SOURCE.VALUE=VCLK
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_SIZE_VALUE.VALUE=0x04
DRIVER.SYSTEM.VAR.VIM_CHANNEL_71_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_63_NAME.VALUE=het2HighLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_55_NAME.VALUE=can3LowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_47_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_39_NAME.VALUE=dmaHBCAInterrupt
DRIVER.SYSTEM.VAR.CLKT_PLL2_BAND_WIDTH_ADJUSTMENT.VALUE=7
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_SIZE.VALUE=32_BYTES
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_DATA_ENTRY.VALUE=_dabort
DRIVER.SYSTEM.VAR.VIM_CHANNEL_80_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_72_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_64_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_56_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_48_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_21_MAPPING.VALUE=21
DRIVER.SYSTEM.VAR.VIM_CHANNEL_13_MAPPING.VALUE=13
DRIVER.SYSTEM.VAR.CLKT_PLL2_REF_CLOCK_DIV.VALUE=8
DRIVER.SYSTEM.VAR.CLKT_PLL1_SPEADING_RATE.VALUE=255
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_END_ADDRESS.VALUE=0x0000001f
DRIVER.SYSTEM.VAR.VIM_CHANNEL_50_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_42_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_34_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_26_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_18_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_0_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.ETPWM1_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_PLL1_RESET_ON_SLIP.VALUE=0x00000000
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_5_WAIT_STATE_FREQ.VALUE=96.0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_TYPE_VALUE.VALUE=0x0010
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_PERMISSION_VALUE.VALUE=0x0300
DRIVER.SYSTEM.VAR.VIM_CHANNEL_127_MAPPING.VALUE=127
DRIVER.SYSTEM.VAR.VIM_CHANNEL_122_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_119_MAPPING.VALUE=119
DRIVER.SYSTEM.VAR.VIM_CHANNEL_114_NAME.VALUE=i2c2Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_106_NAME.VALUE=ecap3nterrupt
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_PERMISSION.VALUE=PRIV_RO_USER_RO_EXEC
DRIVER.SYSTEM.VAR.CLKT_PLL1_FM_ENABLE.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_SIZE.VALUE=4_MB
DRIVER.SYSTEM.VAR.VIM_CHANNEL_123_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_115_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_107_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_90_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_82_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_74_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_66_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_58_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.ECAP3_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_30_NAME.VALUE=mibspi2LowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_22_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_14_NAME.VALUE=adc1Group0Interrupt
DRIVER.SYSTEM.VAR.CLKT_LPOLO_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_123_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_115_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_107_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.SCI3_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.ECLK_PORT_BIT0_PSL.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_120_MAPPING.VALUE=120
DRIVER.SYSTEM.VAR.VIM_CHANNEL_112_MAPPING.VALUE=112
DRIVER.SYSTEM.VAR.VIM_CHANNEL_104_MAPPING.VALUE=104
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_END_ADDRESS.VALUE=0x0000001f
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_BASE_ADDRESS.VALUE=0x80000000
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_SVC_ENTRY.VALUE=_svc
DRIVER.SYSTEM.VAR.VIM_CHANNEL_21_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_20_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_13_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_12_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CONFIG_NEW.VALUE=1
DRIVER.SYSTEM.VAR.CRC1_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_EXTERNAL2_FREQ.VALUE=00.0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_TYPE_VALUE.VALUE=0x0002
DRIVER.SYSTEM.VAR.VIM_CHANNEL_97_NAME.VALUE=etpwm4TripZoneInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_89_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_3_MAPPING.VALUE=3
DRIVER.SYSTEM.VAR.CLKT_LPOHI_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_TYPE.VALUE=NORMAL_OIWTNOWA_SHARED
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_101_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_99_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_93_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_85_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_77_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_69_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_6_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.CLKT_GHV_NORMAL_SOURCE.VALUE=PLL1
DRIVER.SYSTEM.VAR.CLKT_AVCLK3_DIV_FREQ.VALUE=75.0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_97_MAPPING.VALUE=97
DRIVER.SYSTEM.VAR.VIM_CHANNEL_89_MAPPING.VALUE=89
DRIVER.SYSTEM.VAR.VIM_CHANNEL_9_NAME.VALUE=gioHighLevelInterrupt
DRIVER.SYSTEM.VAR.CLKT_PLL1_ENABLE.VALUE=TRUE
DRIVER.SYSTEM.VAR.FLASH_BASE_ADDRESS.VALUE=0x00000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_11_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_SUB_6_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_51_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_43_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_35_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_27_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_19_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_5_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.SPI5_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_TYPE_VALUE.VALUE=0x0006
DRIVER.SYSTEM.VAR.CLKT_AVCLK2_DOMAIN_DISABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_15_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_TYPE.VALUE=NORMAL_OINC_NONSHARED
DRIVER.SYSTEM.VAR.VIM_CHANNEL_120_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_112_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_104_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_100_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.RTP_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.MIBSPI3_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.FLASH_BANK_LINK_LENGTH_0.VALUE=0x001FFFE0
DRIVER.SYSTEM.VAR.FLASH_BANK_LINK_LENGTH_1.VALUE=0x00200000
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_11_WAIT_STATE_FREQ.VALUE=192.0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_SIZE_VALUE.VALUE=0x16
DRIVER.SYSTEM.VAR.VIM_CHANNEL_90_MAPPING.VALUE=90
DRIVER.SYSTEM.VAR.VIM_CHANNEL_82_MAPPING.VALUE=82
DRIVER.SYSTEM.VAR.VIM_CHANNEL_80_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_74_MAPPING.VALUE=74
DRIVER.SYSTEM.VAR.VIM_CHANNEL_72_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_66_MAPPING.VALUE=66
DRIVER.SYSTEM.VAR.VIM_CHANNEL_64_NAME.VALUE=sci3HighLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_58_MAPPING.VALUE=58
DRIVER.SYSTEM.VAR.VIM_CHANNEL_56_NAME.VALUE=mibspi5LowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_48_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_14_SIZE.VALUE=32_BYTES
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_8_SUB_1_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_93_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_85_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_77_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_69_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.EQEP_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.RTI_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.STC_MAX_TIMEOUT.VALUE=0xFFFFFFFF
DRIVER.SYSTEM.VAR.CLKT_LPO_LOW_TRIM.VALUE=100.00
DRIVER.SYSTEM.VAR.FLASH_EEPROM_DATA_3_WAIT_STATE_FREQ.VALUE=64.0
DRIVER.SYSTEM.VAR.RAM_STACK_FIQ_BASE.VALUE=0x08001100
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_PERMISSION_VALUE.VALUE=0x1300
DRIVER.SYSTEM.VAR.VIM_CHANNEL_0_NAME.VALUE=esmHighInterrupt
DRIVER.SYSTEM.VAR.FLASH_BANK_LINK_LENGTH_7.VALUE=0x000020000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_SUB_2_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_50_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_42_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_34_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_26_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_18_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.FEE_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_10.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_LPO_LOW_TRIM_VALUE.VALUE=16
DRIVER.SYSTEM.VAR.VIM_CHANNEL_123_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_115_NAME.VALUE=lin2HighLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_107_NAME.VALUE=ecap4Interrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_51_MAPPING.VALUE=51
DRIVER.SYSTEM.VAR.VIM_CHANNEL_43_MAPPING.VALUE=43
DRIVER.SYSTEM.VAR.VIM_CHANNEL_35_MAPPING.VALUE=35
DRIVER.SYSTEM.VAR.VIM_CHANNEL_27_MAPPING.VALUE=27
DRIVER.SYSTEM.VAR.VIM_CHANNEL_19_MAPPING.VALUE=19
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_11.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_5_PERMISSION.VALUE=PRIV_RW_USER_RW_EXEC
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_12.VALUE=0
DRIVER.SYSTEM.VAR.CCM_MENU.VALUE=NONE
DRIVER.SYSTEM.VAR.CLKT_RESERVED_SOURCE_ENABLE.VALUE=0x00000004
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_9_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_SIZE.VALUE=512_KB
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_BASE_ADDRESS.VALUE=0x08000000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_2_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_98_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_20_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_12_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_4_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_13.VALUE=0
DRIVER.SYSTEM.VAR.POM_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_PLL1_MUL_VAL.VALUE=9500
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_14.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_AVCLK3_SOURCE.VALUE=VCLK
DRIVER.SYSTEM.VAR.CLKT_PLL1_FREQ.VALUE=300.00
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_1_SIZE_VALUE.VALUE=0x1F
DRIVER.SYSTEM.VAR.VIM_CHANNEL_31_NAME.VALUE=phantomInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_23_NAME.VALUE=gioLowLevelInterrupt
DRIVER.SYSTEM.VAR.VIM_CHANNEL_15_NAME.VALUE=adc1Group1Interrupt
DRIVER.SYSTEM.VAR.ERRATA_WORKAROUND_15.VALUE=0
DRIVER.SYSTEM.VAR.RAM_STACK_UNDEF_LENGTH.VALUE=0x00000100
DRIVER.SYSTEM.VAR.RAM_STACK_SVC_LENGTH.VALUE=0x00000100
DRIVER.SYSTEM.VAR.CLKT_LPO_TRIM_OTP_LOC.VALUE=0xF00801B4
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_SUB_3_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_6_SUB_6_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_HANDLER_TABLE_UNDEF_ENTRY.VALUE=_undef
DRIVER.SYSTEM.VAR.VIM_CHANNEL_93_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_85_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_77_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_71_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_69_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_63_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_55_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_47_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_39_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ETPWM6_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.DCC_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_20_MAPPING.VALUE=20
DRIVER.SYSTEM.VAR.VIM_CHANNEL_12_MAPPING.VALUE=12
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_PERMISSION.VALUE=PRIV_RW_USER_RO_NOEXEC
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_16_BASE_ADDRESS.VALUE=0xFFF80000
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_SUB_4_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_SUB_7_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_ENDIAN_LITTLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_126_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_125_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_118_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.VIM_CHANNEL_117_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_109_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.OS_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_12_SIZE_VALUE.VALUE=0x04
DRIVER.SYSTEM.VAR.VIM_CHANNEL_126_MAPPING.VALUE=126
DRIVER.SYSTEM.VAR.VIM_CHANNEL_118_MAPPING.VALUE=118
DRIVER.SYSTEM.VAR.VIM_CHANNEL_98_NAME.VALUE=etpwm5Interrupt
DRIVER.SYSTEM.VAR.ECLK_PORT_BIT0_PULL.VALUE=2
DRIVER.SYSTEM.VAR.ECLK_SUSPEND.VALUE=0
DRIVER.SYSTEM.VAR.CLKT_PLL1_SPEADING_AMOUNT.VALUE=61
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_13_TYPE.VALUE=NORMAL_OIWTNOWA_SHARED
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_10_SUB_5_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_4_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CORE_VFP_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.ECAP1_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.I2C_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.AJSM_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.ECLK_OSCILLATOR_FREQ.VALUE=16.000
DRIVER.SYSTEM.VAR.CLKT_LPO_HIGH_TRIM.VALUE=100.00
DRIVER.SYSTEM.VAR.CLKT_AVCLK4_SPL_SOURCE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_9_MAPPING.VALUE=9
DRIVER.SYSTEM.VAR.VIM_ECC_INTERRUPT_MAPPED_TO_VIM.VALUE=FALSE
DRIVER.SYSTEM.VAR.CLKT_VCLK4_DOMAIN_ENABLE.VALUE=FALSE
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_3_SUB_0_DISABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_71_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_63_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_55_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_47_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_41_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_39_INT_PRAGMA_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.VIM_CHANNEL_33_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_25_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_17_INT_ENABLE.VALUE=0
DRIVER.SYSTEM.VAR.VIM_CHANNEL_9_INT_TYPE.VALUE=IRQ
DRIVER.SYSTEM.VAR.SCI1_ENABLE.VALUE=1
DRIVER.SYSTEM.VAR.CLKT_CRYSTAL_FREQ.VALUE=16.0
DRIVER.SYSTEM.VAR.CORE_MPU_REGION_7_TYPE_VALUE.VALUE=0x0008
DRIVER.SYSTEM.VAR.VIM_CHANNEL_111_MAPPING.VALUE=111
DRIVER.SYSTEM.VAR.VIM_CHANNEL_103_MAPPING.VALUE=103
DRIVER.SYSTEM.VAR.VIM_PHANTOM_NAME.VALUE=phantomInterrupt
DRIVER.OS.VAR.OS_USERECERSIVEMUTEXES.VALUE=0
DRIVER.OS.VAR.OS_USETIMERS.VALUE=0
DRIVER.OS.VAR.OS_USECNTSEMAPHORE.VALUE=0
DRIVER.OS.VAR.OS_GENERATERUNTIMESTATS.VALUE=0
DRIVER.OS.VAR.OS_USEMPU.VALUE=0
DRIVER.OS.VAR.OS_TOTALHEAPSIZE.VALUE=8192
DRIVER.OS.VAR.OS_USEVERBOSESTACK.VALUE=2
DRIVER.OS.VAR.OS_TIMERPRIORITY.VALUE=0
DRIVER.OS.VAR.OS_SVCENABLE.VALUE=0
DRIVER.OS.VAR.OS_MAXTASKNAMELEN.VALUE=16
DRIVER.OS.VAR.OS_MAXPRIORITIES.VALUE=5
DRIVER.OS.VAR.OS_TIMERTASKSTACKDEPTH.VALUE=0
DRIVER.OS.VAR.OS_COROUTINEPRIORITIES.VALUE=2
DRIVER.OS.VAR.OS_USECOROUTINES.VALUE=0
DRIVER.OS.VAR.OS_USEMUTEXES.VALUE=0
DRIVER.OS.VAR.OS_CPUCLOCKHZ.VALUE=80000000
DRIVER.OS.VAR.OS_USEMALLOCFAILEDHOOK.VALUE=0
DRIVER.OS.VAR.OS_MINSTACKSIZE.VALUE=128
DRIVER.OS.VAR.OS_SYSTEM_MODE.VALUE=0x1F
DRIVER.OS.VAR.OS_USEPREEMPTION.VALUE=1
DRIVER.OS.VAR.OS_IDLESHOULDYIELD.VALUE=1
DRIVER.OS.VAR.OS_USEIDLEHOOK.VALUE=0
DRIVER.OS.VAR.OS_TICKRATEHZ.VALUE=1000
DRIVER.OS.VAR.OS_TIMERPQUEUELENGTH.VALUE=0
DRIVER.OS.VAR.OS_USETRACE.VALUE=0
DRIVER.OS.VAR.OS_USESTACK.VALUE=0
DRIVER.OS.VAR.OS_USETICKHOOK.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL93_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL85_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL77_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL69_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL0_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL21_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL13_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL71_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL63_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL55_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL47_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL39_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL94_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL86_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL78_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL3_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL41_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL33_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL25_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL17_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL88_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL9_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL50_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL42_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL34_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL26_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL18_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL81_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL73_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL65_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL57_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL49_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL2_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL11_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL50_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL42_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL34_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL26_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL18_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL8_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL5_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL11_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL71_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL63_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL55_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL47_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL39_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL92_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL84_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL76_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL68_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL11_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL70_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL62_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL54_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL46_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL38_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL92_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL84_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL76_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL68_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL1_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL94_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL86_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL78_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL7_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL40_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL32_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL24_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL16_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL71_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL63_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL55_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL47_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL39_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL0_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL40_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL32_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL24_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL16_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL40_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL32_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL24_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL16_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL10_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL89_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL6_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL89_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL4_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL61_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL53_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL45_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL37_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL29_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL91_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL83_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL75_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL67_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL59_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL61_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL53_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL45_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL37_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL29_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL92_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL84_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL76_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL68_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL5_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL61_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL53_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL45_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL37_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL29_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL90_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL82_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL74_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL66_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL58_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_LOW_TIME.VALUE=218.453
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL30_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL22_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL14_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL31_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL23_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL15_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL9_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL30_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL22_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL14_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL95_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL87_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL79_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL4_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL88_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL3_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL51_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL43_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL35_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL27_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL19_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL90_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL82_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL74_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL66_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL58_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL89_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL90_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL82_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL74_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL66_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL58_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL3_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL9_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL51_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL43_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL35_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL27_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL19_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL60_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL52_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL44_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL36_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL28_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL20_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL12_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL80_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL72_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL64_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL56_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL48_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_VCLK_FREQ.VALUE=75
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL30_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL22_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL14_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL8_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL20_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL12_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL93_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL85_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL77_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL69_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL2_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL95_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL87_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL79_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL2_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL95_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL87_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL79_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL8_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL80_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL72_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL64_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL56_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL48_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL1_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL41_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL33_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL25_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL17_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL81_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL73_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL65_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL57_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL49_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL41_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL33_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL25_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL17_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL10_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL7_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL51_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL43_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL35_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL27_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL19_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL70_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL62_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL54_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL46_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL38_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL21_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL13_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL7_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL10_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL93_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL85_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL77_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL69_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL6_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL91_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL83_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL75_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL67_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL59_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL0_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL94_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL86_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL78_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL1_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL70_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL62_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL54_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL46_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL38_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_BASE.VALUE=0xFFFFF500
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL31_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL23_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL15_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL31_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL23_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL15_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL80_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL72_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL64_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL56_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL48_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL88_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL5_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL50_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL42_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL34_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL26_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL18_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL60_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL52_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL44_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL36_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL28_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL20_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL12_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL6_INT_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL91_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL83_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL75_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL67_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL59_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL4_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL60_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL52_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL44_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL36_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL28_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_LPC.VALUE=16384
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL21_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL13_ENABLE.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL81_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL73_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL65_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL57_INT_LEVEL.VALUE=0
DRIVER.ESM.VAR.ESM_GROUP0_CHANNEL49_INT_LEVEL.VALUE=0
DRIVER.RTI.VAR.RTI_1_COMPARE_2_SOURCE.VALUE=0x00000100
DRIVER.RTI.VAR.RTI_1_COMPARE_3_FREQ.VALUE=0.000100000
DRIVER.RTI.VAR.RTI_1_FREQ.VALUE=75.000
DRIVER.RTI.VAR.RTI_1_COMPARE_1_ACTUALTIME.VALUE=5.000
DRIVER.RTI.VAR.RTI_1_COUNTER_1_UC_COMPARE.VALUE=7
DRIVER.RTI.VAR.RTI_1_COMPARE_1_TIME.VALUE=5.000
DRIVER.RTI.VAR.RTI_1_COMPARE_3_UPDATE.VALUE=93750
DRIVER.RTI.VAR.RTI_1_CONTINUE_ON_SUSPEND_ENABLE.VALUE=0x00000000
DRIVER.RTI.VAR.RTI_1_COMPARE_1_INPUT_FREQ.VALUE=9.375000000
DRIVER.RTI.VAR.RTI_1_COMPARE_0_SOURCE.VALUE=0x00000000
DRIVER.RTI.VAR.RTI_1_COMPARE_2_TIME.VALUE=8.000
DRIVER.RTI.VAR.RTI_1_COMPARE_0_ACTUALTIME.VALUE=1.000
DRIVER.RTI.VAR.RTI_1_COUNTER_0_UC_COMPARE.VALUE=7
DRIVER.RTI.VAR.RTI_1_COMPARE_1_UPDATE.VALUE=46875
DRIVER.RTI.VAR.RTI_1_COMPARE_3_TIME.VALUE=10.000
DRIVER.RTI.VAR.RTI_1_COUNTER_0_NTU_SOURCE.VALUE=1
DRIVER.RTI.VAR.RTI_1_COMPARE_0_INPUT_FREQ.VALUE=9.375000000
DRIVER.RTI.VAR.RTI_1_COUNTER_0_RTI_FREQ.VALUE=0.0
DRIVER.RTI.VAR.RTI_1_COUNTER_0_FREQ.VALUE=9.375000000
DRIVER.RTI.VAR.RTI_1_COUNTER_1_FREQUENCY.VALUE=10.000
DRIVER.RTI.VAR.RTI_1_COMPARE_3_SOURCE.VALUE=0x00001000
DRIVER.RTI.VAR.RTI_1_COUNTER_1_FREQ.VALUE=9.375000000
DRIVER.RTI.VAR.RTI_1_COUNTER_0_NTU_SOURCE_REG.VALUE=0x5
DRIVER.RTI.VAR.RTI_1_COMPARE_1_SOURCE.VALUE=0x00000000
DRIVER.RTI.VAR.RTI_1_NTU_1_FREQ.VALUE=0.0
DRIVER.RTI.VAR.RTI_1_COMPARE_3_ACTUALTIME.VALUE=10.000
DRIVER.RTI.VAR.RTI_1_COMPARE_0_FREQ.VALUE=0.001000000
DRIVER.RTI.VAR.RTI_1_COMPARE_2_UPDATE.VALUE=75000
DRIVER.RTI.VAR.RTI_1_BASE.VALUE=0xFFFFFC00
DRIVER.RTI.VAR.RTI_1_NTU_2_FREQ.VALUE=0.0
DRIVER.RTI.VAR.RTI_1_COMPARE_3_INPUT_FREQ.VALUE=9.375000000
DRIVER.RTI.VAR.RTI_1_COMPARE_1_FREQ.VALUE=0.000200000
DRIVER.RTI.VAR.RTI_1_COUNTER_0_CAPTURE_SOURCE_ENABLE.VALUE=0
DRIVER.RTI.VAR.RTI_1_COUNTER_1_CAPTURE_SOURCE_ENABLE.VALUE=0
DRIVER.RTI.VAR.RTI_1_COMPARE_0_UPDATE.VALUE=9375
DRIVER.RTI.VAR.RTI_1_NTU_3_FREQ.VALUE=300.000
DRIVER.RTI.VAR.RTI_1_COMPARE_0.VALUE=9375
DRIVER.RTI.VAR.RTI_1_COMPARE_2_ACTUALTIME.VALUE=8.000
DRIVER.RTI.VAR.RTI_1_COMPARE_1.VALUE=46875
DRIVER.RTI.VAR.RTI_1_COMPARE_2.VALUE=75000
DRIVER.RTI.VAR.RTI_1_COMPARE_3.VALUE=93750
DRIVER.RTI.VAR.RTI_1_COUNTER_0_NTU_FREQ.VALUE=0.000
DRIVER.RTI.VAR.RTI_1_COMPARE_2_FREQ.VALUE=0.000125000
DRIVER.RTI.VAR.RTI_1_COMPARE_0_TIME.VALUE=1.000
DRIVER.RTI.VAR.RTI_1_NTU_4_FREQ.VALUE=0.000
DRIVER.RTI.VAR.RTI_1_COMPARE_2_INPUT_FREQ.VALUE=9.375000000
DRIVER.RTI.VAR.RTI_1_COUNTER_0_FREQUENCY.VALUE=10.000
DRIVER.GIO.VAR.GIO_PORT1_BIT4_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT0_BIT5_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT4_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT7_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT2_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT7_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT3_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT2_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT6_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT2_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT6_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT2_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT3_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT4_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT3_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT5_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT7_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT3_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT5_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT0_BIT7_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT4_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT5_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT4_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT2_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT4_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT0_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT0_BIT3_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT5_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT6_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT5_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT5_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT6_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT0_BIT6_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT3_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT7_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT6_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT0_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT6_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT1_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT0_BIT4_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT7_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT7_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT7_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT0_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT7_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT7_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT1_BIT1_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT2_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT1_BIT1_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT5_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT0_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT5_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT0_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT2_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT3_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT1_BIT1_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT6_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT1_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT6_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT2_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT2_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT0_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT0_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT0_BIT3_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT3_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT4_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT1_BIT3_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT7_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT3_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT0_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT1_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT0_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT4_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT0_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT4_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT4_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_BASE_PORTA.VALUE=0xFFF7BC34
DRIVER.GIO.VAR.GIO_BASE_PORTB.VALUE=0xFFF7BC54
DRIVER.GIO.VAR.GIO_PORT1_BIT1_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT2_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT1_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT1_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT1_BIT4_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT5_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT1_BIT5_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT1_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT5_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT2_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT1_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT0_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT3_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT2_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT0_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT6_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT2_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT6_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_BASE.VALUE=0xFFF7BC00
DRIVER.GIO.VAR.GIO_PORT1_BIT3_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT1_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT4_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT3_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT2_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT0_BIT1_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT5_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT6_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT1_BIT7_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT2_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT3_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT7_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT4_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT2_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT5_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT4_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT2_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT0_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT6_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT4_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT0_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORTB_ENABLE.VALUE=1
DRIVER.GIO.VAR.GIO_PORT1_BIT5_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT3_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT6_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT5_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT3_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT0_BIT3_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT6_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT7_PULL.VALUE=1
DRIVER.GIO.VAR.GIO_PORT0_BIT0_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT5_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT1_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT0_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT6_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT7_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT4_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT7_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT6_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT0_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT4_DIR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT0_PULDIS.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT1_DOUT.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT1_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT6_PSL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT2_PDR.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT1_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT7_LVL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT5_ENA.VALUE=0
DRIVER.GIO.VAR.GIO_PORT1_BIT7_POL.VALUE=0
DRIVER.GIO.VAR.GIO_PORT0_BIT1_PSL.VALUE=0
DRIVER.SCI.VAR.SCI4_PORT_BIT2_PULL.VALUE=2
DRIVER.SCI.VAR.SCI1_PORT_BIT2_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI4_BASE.VALUE=0xFFF7E700
DRIVER.SCI.VAR.SCI4_LENGTH.VALUE=8
DRIVER.SCI.VAR.SCI3_BREAKINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT0_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT2_PSL.VALUE=1
DRIVER.SCI.VAR.SCI3_PORT_BIT0_FUN.VALUE=0
DRIVER.SCI.VAR.SCI4_ACTUALBAUDRATE.VALUE=114329
DRIVER.SCI.VAR.SCI4_FEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI3_PORT_BIT2_DIR.VALUE=0
DRIVER.SCI.VAR.SCI1_BAUDRATE.VALUE=115200
DRIVER.SCI.VAR.SCI4_OEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI4_TXINTENA.VALUE=0
DRIVER.SCI.VAR.SCI3_PORT_BIT0_PDR.VALUE=0
DRIVER.SCI.VAR.SCI2_PEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI1_STOPBITS.VALUE=2
DRIVER.SCI.VAR.SCI3_PORT_BIT1_FUN.VALUE=1
DRIVER.SCI.VAR.SCI3_WAKEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT0_PULDIS.VALUE=0
DRIVER.SCI.VAR.SCI1_RXINTENA.VALUE=0
DRIVER.SCI.VAR.SCI4_WAKEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI1_FEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT0_PULL.VALUE=2
DRIVER.SCI.VAR.SCI3_PORT_BIT1_PDR.VALUE=0
DRIVER.SCI.VAR.SCI1_TXINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT1_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI3_PORT_BIT2_FUN.VALUE=1
DRIVER.SCI.VAR.SCI4_TIMMINGMODE.VALUE=1
DRIVER.SCI.VAR.SCI3_CLKMODE.VALUE=1
DRIVER.SCI.VAR.SCI3_PORT_BIT0_PSL.VALUE=1
DRIVER.SCI.VAR.SCI2_LENGTH.VALUE=8
DRIVER.SCI.VAR.SCI1_BASE_PORT.VALUE=0xFFF7E440
DRIVER.SCI.VAR.SCI4_BAUDRATE.VALUE=115200
DRIVER.SCI.VAR.SCI3_OEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI2_PARITYENA.VALUE=0
DRIVER.SCI.VAR.SCI1_EVENPARITY.VALUE=0
DRIVER.SCI.VAR.SCI3_PORT_BIT2_PDR.VALUE=0
DRIVER.SCI.VAR.SCI2_BREAKINTENA.VALUE=0
DRIVER.SCI.VAR.SCI1_PEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI1_TIMMINGMODE.VALUE=1
DRIVER.SCI.VAR.SCI3_PORT_BIT1_PSL.VALUE=1
DRIVER.SCI.VAR.SCI4_STOPBITS.VALUE=2
DRIVER.SCI.VAR.SCI4_RXINTENA.VALUE=0
DRIVER.SCI.VAR.SCI4_FEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT1_PULL.VALUE=2
DRIVER.SCI.VAR.SCI4_PORT_BIT1_PULDIS.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT2_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI4_TXINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI3_PORT_BIT2_PSL.VALUE=1
DRIVER.SCI.VAR.SCI3_PORT_BIT0_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI2_WAKEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI3_WAKEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI1_RXINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI2_CLKMODE.VALUE=1
DRIVER.SCI.VAR.SCI1_PRESCALE.VALUE=40
DRIVER.SCI.VAR.SCI4_PEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT0_DIR.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT2_PULL.VALUE=2
DRIVER.SCI.VAR.SCI3_PORT_BIT1_PULDIS.VALUE=0
DRIVER.SCI.VAR.SCI3_FEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT0_PULL.VALUE=2
DRIVER.SCI.VAR.SCI3_OEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI3_TXINTENA.VALUE=0
DRIVER.SCI.VAR.SCI1_ACTUALBAUDRATE.VALUE=114329
DRIVER.SCI.VAR.SCI3_PORT_BIT1_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI2_BREAKINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI1_PEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT1_DIR.VALUE=0
DRIVER.SCI.VAR.SCI4_RXINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI4_BASE_PORT.VALUE=0xFFF7E740
DRIVER.SCI.VAR.SCI4_PRESCALE.VALUE=40
DRIVER.SCI.VAR.SCI2_PORT_BIT0_FUN.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT1_PULDIS.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT2_DIR.VALUE=0
DRIVER.SCI.VAR.SCI1_WAKEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI1_CLKMODE.VALUE=1
DRIVER.SCI.VAR.SCI2_PORT_BIT1_PULL.VALUE=2
DRIVER.SCI.VAR.SCI2_WAKEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT0_PDR.VALUE=0
DRIVER.SCI.VAR.SCI3_BAUDRATE.VALUE=115200
DRIVER.SCI.VAR.SCI2_OEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI3_PORT_BIT2_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT1_FUN.VALUE=1
DRIVER.SCI.VAR.SCI4_PORT_BIT0_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI4_PEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI4_BREAKINTENA.VALUE=0
DRIVER.SCI.VAR.SCI3_TIMMINGMODE.VALUE=1
DRIVER.SCI.VAR.SCI3_STOPBITS.VALUE=2
DRIVER.SCI.VAR.SCI3_RXINTENA.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT1_PDR.VALUE=0
DRIVER.SCI.VAR.SCI3_FEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT1_PULDIS.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT2_FUN.VALUE=1
DRIVER.SCI.VAR.SCI1_BREAKINTENA.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT0_PSL.VALUE=1
DRIVER.SCI.VAR.SCI3_TXINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI4_PORT_BIT0_DIR.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT2_PULL.VALUE=2
DRIVER.SCI.VAR.SCI2_PORT_BIT2_PDR.VALUE=0
DRIVER.SCI.VAR.SCI3_PORT_BIT0_PULL.VALUE=2
DRIVER.SCI.VAR.SCI2_BASE_PORT.VALUE=0xFFF7E640
DRIVER.SCI.VAR.SCI3_PARITYENA.VALUE=0
DRIVER.SCI.VAR.SCI2_ACTUALBAUDRATE.VALUE=114329
DRIVER.SCI.VAR.SCI4_PORT_BIT1_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT1_PSL.VALUE=1
DRIVER.SCI.VAR.SCI3_LENGTH.VALUE=8
DRIVER.SCI.VAR.SCI3_PEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI4_PORT_BIT1_DIR.VALUE=0
DRIVER.SCI.VAR.SCI1_WAKEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI2_FEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT2_PSL.VALUE=1
DRIVER.SCI.VAR.SCI4_PORT_BIT0_FUN.VALUE=0
DRIVER.SCI.VAR.SCI2_OEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI4_EVENPARITY.VALUE=0
DRIVER.SCI.VAR.SCI2_TXINTENA.VALUE=0
DRIVER.SCI.VAR.SCI4_PORT_BIT2_DIR.VALUE=0
DRIVER.SCI.VAR.SCI4_PORT_BIT2_PULDIS.VALUE=0
DRIVER.SCI.VAR.SCI4_BREAKINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI3_PORT_BIT1_PULL.VALUE=2
DRIVER.SCI.VAR.SCI4_PORT_BIT0_PDR.VALUE=0
DRIVER.SCI.VAR.SCI3_RXINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI4_PORT_BIT2_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI1_BASE.VALUE=0xFFF7E400
DRIVER.SCI.VAR.SCI4_PORT_BIT1_FUN.VALUE=1
DRIVER.SCI.VAR.SCI3_PRESCALE.VALUE=40
DRIVER.SCI.VAR.SCI1_PORT_BIT0_DIR.VALUE=0
DRIVER.SCI.VAR.SCI1_BREAKINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI4_PORT_BIT1_PDR.VALUE=0
DRIVER.SCI.VAR.SCI1_LENGTH.VALUE=8
DRIVER.SCI.VAR.SCI4_PORT_BIT2_FUN.VALUE=1
DRIVER.SCI.VAR.SCI3_PORT_BIT2_PULDIS.VALUE=0
DRIVER.SCI.VAR.SCI2_BAUDRATE.VALUE=115200
DRIVER.SCI.VAR.SCI1_PARITYENA.VALUE=0
DRIVER.SCI.VAR.SCI1_OEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI4_PORT_BIT0_PSL.VALUE=1
DRIVER.SCI.VAR.SCI1_PORT_BIT1_DIR.VALUE=0
DRIVER.SCI.VAR.SCI3_PORT_BIT2_PULL.VALUE=2
DRIVER.SCI.VAR.SCI3_PEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI4_PORT_BIT2_PDR.VALUE=0
DRIVER.SCI.VAR.SCI2_STOPBITS.VALUE=2
DRIVER.SCI.VAR.SCI4_PORT_BIT0_PULL.VALUE=2
DRIVER.SCI.VAR.SCI2_RXINTENA.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT0_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI2_BASE.VALUE=0xFFF7E600
DRIVER.SCI.VAR.SCI2_FEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT0_FUN.VALUE=0
DRIVER.SCI.VAR.SCI4_PORT_BIT0_PULDIS.VALUE=0
DRIVER.SCI.VAR.SCI3_ACTUALBAUDRATE.VALUE=114329
DRIVER.SCI.VAR.SCI4_PORT_BIT1_PSL.VALUE=1
DRIVER.SCI.VAR.SCI1_PORT_BIT2_DIR.VALUE=0
DRIVER.SCI.VAR.SCI3_EVENPARITY.VALUE=0
DRIVER.SCI.VAR.SCI2_TXINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI3_BREAKINTENA.VALUE=0
DRIVER.SCI.VAR.SCI2_TIMMINGMODE.VALUE=1
DRIVER.SCI.VAR.SCI1_PORT_BIT0_PDR.VALUE=0
DRIVER.SCI.VAR.SCI2_PORT_BIT2_PULDIS.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT1_FUN.VALUE=1
DRIVER.SCI.VAR.SCI4_PORT_BIT2_PSL.VALUE=1
DRIVER.SCI.VAR.SCI4_OEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI2_PEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT1_PDR.VALUE=0
DRIVER.SCI.VAR.SCI4_PORT_BIT1_PULL.VALUE=2
DRIVER.SCI.VAR.SCI3_PORT_BIT0_PULDIS.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT1_DOUT.VALUE=0
DRIVER.SCI.VAR.SCI3_BASE.VALUE=0xFFF7E500
DRIVER.SCI.VAR.SCI1_PORT_BIT2_FUN.VALUE=1
DRIVER.SCI.VAR.SCI4_WAKEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI1_FEINTENA.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT0_PSL.VALUE=1
DRIVER.SCI.VAR.SCI3_PORT_BIT0_DIR.VALUE=0
DRIVER.SCI.VAR.SCI1_OEINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT2_PULDIS.VALUE=0
DRIVER.SCI.VAR.SCI1_TXINTENA.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT2_PDR.VALUE=0
DRIVER.SCI.VAR.SCI1_PORT_BIT1_PSL.VALUE=1
DRIVER.SCI.VAR.SCI2_RXINTLVL.VALUE=0
DRIVER.SCI.VAR.SCI3_PORT_BIT1_DIR.VALUE=0
DRIVER.SCI.VAR.SCI3_BASE_PORT.VALUE=0xFFF7E540
DRIVER.SCI.VAR.SCI4_PARITYENA.VALUE=0
DRIVER.SCI.VAR.SCI4_CLKMODE.VALUE=1
DRIVER.SCI.VAR.SCI2_EVENPARITY.VALUE=0
DRIVER.SCI.VAR.SCI2_PRESCALE.VALUE=40
DRIVER.SCI.VAR.SCI2_PORT_BIT0_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PARITYENA2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_DLENERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI2_BASE_PORT.VALUE=0xFFF7F618
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT17_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT25_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_BITERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PARITYENA3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_RXINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT25_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT17_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT8_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_BUF_CSNR.VALUE=CS_1
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT1_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_CLKMOD.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT11_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT5_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PHASE0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI1_PHASE1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT27_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT19_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT3_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT9_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PHASE2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT8_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI1_PHASE3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT25_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT17_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_BUF_CSNR.VALUE=CS_2
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT1_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT11_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_BASE.VALUE=0xFFF7FA00
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT5_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT1_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT17_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT25_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_C2TDELAYACTUAL.VALUE=26.667
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT1_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT11_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TXINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TIMEOUTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT27_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT19_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_WDELAY0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT3_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI4_WDELAY1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI4_WDELAY2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PARERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT8_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_WDELAY3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT9_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT8_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT4_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT26_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT18_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT2_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_ACTUALBAUDRATE0.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI2_T2EDELAYACTUAL.VALUE=0.000
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI3_ACTUALBAUDRATE1.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT0_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT10_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_ACTUALBAUDRATE2.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT3_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_LENGTH.VALUE=8
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_ACTUALBAUDRATE3.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT9_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_C2EDELAYACTUAL.VALUE=0.000
DRIVER.MIBSPI.VAR.MIBSPI2_BAUDRATE0.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT8_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_BUF_CSNR.VALUE=CS_1
DRIVER.MIBSPI.VAR.MIBSPI2_BAUDRATE1.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT2_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT1_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI2_BAUDRATE2.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI2_BAUDRATE3.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_T2CDELAYACTUAL.VALUE=13.333
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT4_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT4_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_BUF_CSNR.VALUE=CS_2
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT9_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PARERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI3_OVRNINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT8_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT26_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT18_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT0_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT10_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT2_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_BUF_CSNR.VALUE=CS_3
DRIVER.MIBSPI.VAR.MIBSPI2_POLARITY0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT17_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT25_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_POLARITY1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_C2TDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT10_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_OVRNINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT5_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI2_POLARITY2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_RXINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT17_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT25_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT4_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_DEYSNCENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_POLARITY3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT11_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT1_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT27_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT19_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT0_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_BUF_CSNR.VALUE=CS_4
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT3_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_WAITENA0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_BASE.VALUE=0xFFF7FC00
DRIVER.MIBSPI.VAR.MIBSPI2_WAITENA1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT1_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_DEYSNCLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PARPOL0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT11_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT17_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT25_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_WAITENA2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT10_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PARPOL1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI2_WAITENA3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_BUF_CSNR.VALUE=CS_5
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PARPOL2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT9_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PARPOL3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT3_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT0_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI1_TXINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT5_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PRESCALE0.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI1_CLKMOD.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI1_PRESCALE1.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TXINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PRESCALE2.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT9_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TIMEOUTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_DLENERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PRESCALE3.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT1_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT11_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PARITYENA0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT8_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_ACTUALBAUDRATE0.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_PARITYENA1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_ACTUALBAUDRATE1.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT9_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI3_PARITYENA2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_DLENERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_ACTUALBAUDRATE2.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT2_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PARITYENA3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_BITERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_ACTUALBAUDRATE3.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT4_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI3_T2EDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT2_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_BITERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_SHIFTDIR0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT8_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_RXINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_CSDEF.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT4_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_SHIFTDIR1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT0_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_SHIFTDIR2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT10_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_WDELAY0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT17_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT25_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_T2CDELAYACTUAL.VALUE=13.333
DRIVER.MIBSPI.VAR.MIBSPI4_SHIFTDIR3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_WDELAY1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI4_MASTER.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_WDELAY2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT2_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT1_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_WDELAY3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT8_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_ENABLEHIGHZ.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT5_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_BUF_CSNR.VALUE=CS_4
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT10_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT0_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT10_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT4_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT27_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT19_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT2_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT3_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_BUF_CSNR.VALUE=CS_5
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT9_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI2_C2EDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT11_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT17_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT25_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT1_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT5_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_BUF_CSNR.VALUE=CS_6
DRIVER.MIBSPI.VAR.MIBSPI4_C2TDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT3_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_BASE_PORT.VALUE=0xFFF7FC18
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT9_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT0_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT1_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_WAITENA0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_BUF_CSNR.VALUE=CS_7
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT11_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_WAITENA1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_WAITENA2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT2_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_WAITENA3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT9_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT10_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT17_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT25_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_C2TDELAYACTUAL.VALUE=26.667
DRIVER.MIBSPI.VAR.MIBSPI2_T2CDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT11_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT2_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TXINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT3_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT0_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_BASE_RAM.VALUE=0xFF080000
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT8_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_PARPOL0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_CHARLEN0.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PARPOL1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PARERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_CHARLEN1.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI2_OVRNINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PHASE0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PARPOL2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_CHARLEN2.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI4_PHASE1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PARPOL3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_CHARLEN3.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI5_PARERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT8_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_PHASE2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_OVRNINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT1_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT5_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI4_PHASE3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_DEYSNCENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_RXINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT2_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_BUF_CSNR.VALUE=CS_0
DRIVER.MIBSPI.VAR.MIBSPI3_T2EDELAYACTUAL.VALUE=0.000
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT8_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_RXINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT10_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_DEYSNCLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT3_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT3_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT4_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT9_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_BUF_CSNR.VALUE=CS_1
DRIVER.MIBSPI.VAR.MIBSPI4_C2EDELAYACTUAL.VALUE=0.000
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT8_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT25_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT17_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT1_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT11_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT0_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT10_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_BAUDRATE0.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT4_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT1_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_BUF_CSNR.VALUE=CS_7
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_BAUDRATE1.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI5_BAUDRATE2.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT9_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TXINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_BAUDRATE3.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TIMEOUTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI1_DLENERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT10_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT2_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT17_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT25_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_WDELAY0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PARITYENA0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_C2EDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_WDELAY1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PARITYENA1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TIMEOUTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT2_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_WDELAY2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PARITYENA2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_DLENERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_MASTER.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT9_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_WDELAY3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PARITYENA3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_BITERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT3_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT0_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_POLARITY0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT10_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT0_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_POLARITY1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_POLARITY2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT11_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_BITERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT4_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_SHIFTDIR0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT26_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT18_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_POLARITY3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT2_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_SHIFTDIR1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT11_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT9_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_SHIFTDIR2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_SHIFTDIR3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT0_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT11_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT2_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_BUF_CSNR.VALUE=CS_0
DRIVER.MIBSPI.VAR.MIBSPI5_T2CDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_LENGTH.VALUE=8
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT11_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PRESCALE0.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT8_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_BUF_CSNR.VALUE=CS_1
DRIVER.MIBSPI.VAR.MIBSPI5_BASE_RAM.VALUE=0xFF0A0000
DRIVER.MIBSPI.VAR.MIBSPI4_PRESCALE1.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_CHARLEN0.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT9_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_PRESCALE2.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI3_CSDEF.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT3_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_CHARLEN1.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI4_PRESCALE3.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT4_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_CHARLEN2.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_BUF_CSNR.VALUE=CS_2
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT1_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT9_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_CHARLEN3.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT8_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_BASE_PORT.VALUE=0xFFF7F818
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT5_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT4_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT0_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_RXINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT10_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_BUF_CSNR.VALUE=CS_3
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_T2CDELAYACTUAL.VALUE=13.333
DRIVER.MIBSPI.VAR.MIBSPI1_WAITENA0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI1_WAITENA1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT26_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT18_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT1_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT2_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI2_PARPOL0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_WAITENA2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PARPOL1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_WAITENA3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_BUF_CSNR.VALUE=CS_4
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_CLKMOD.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT5_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT3_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PARPOL2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PHASE0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI2_PARPOL3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PHASE1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT10_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT0_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PHASE2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT9_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PHASE3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT3_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT9_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT10_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT0_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TXINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT4_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT2_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI1_PARERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_OVRNINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT1_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT11_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT2_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT9_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT0_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PARERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_OVRNINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT11_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI2_T2EDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT2_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_DEYSNCLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_RXINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_C2TDELAYACTUAL.VALUE=26.667
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT4_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_WDELAY0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_WDELAY1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT11_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_WDELAY2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT17_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT25_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_WDELAY3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT0_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_BAUDRATE0.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_BUF_CSNR.VALUE=CS_3
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI3_BAUDRATE1.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT8_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_BAUDRATE2.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT5_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT17_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT25_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT0_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI3_BAUDRATE3.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_TIMEOUTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT10_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_ENABLEHIGHZ.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT3_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_BUF_CSNR.VALUE=CS_4
DRIVER.MIBSPI.VAR.MIBSPI1_PARITYENA0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_C2EDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PARITYENA1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT8_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT1_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TIMEOUTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT5_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_PARITYENA2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_DLENERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI1_PARITYENA3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_T2EDELAYACTUAL.VALUE=0.000
DRIVER.MIBSPI.VAR.MIBSPI4_ACTUALBAUDRATE0.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_BUF_CSNR.VALUE=CS_5
DRIVER.MIBSPI.VAR.MIBSPI3_POLARITY0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT8_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_ACTUALBAUDRATE1.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_C2TDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_POLARITY1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT27_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT19_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT10_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT3_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_ACTUALBAUDRATE2.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT3_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI3_POLARITY2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT10_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT0_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_BITERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI4_ACTUALBAUDRATE3.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI4_DEYSNCENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_POLARITY3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT9_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT8_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_C2EDELAYACTUAL.VALUE=0.000
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_BUF_CSNR.VALUE=CS_6
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_WAITENA0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT5_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_WAITENA1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT1_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_WAITENA2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT5_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_WAITENA3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT2_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_BUF_CSNR.VALUE=CS_7
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT17_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT25_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT4_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT1_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_ENABLEHIGHZ.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT11_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT1_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI1_T2CDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT9_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_LENGTH.VALUE=8
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT11_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TXINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT10_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT2_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT4_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PRESCALE0.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PRESCALE1.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI1_BASE_RAM.VALUE=0xFF0E0000
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT10_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT2_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT8_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PRESCALE2.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI1_PARPOL0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_CHARLEN0.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI2_PRESCALE3.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI1_PARPOL1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_CHARLEN1.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT0_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_CLKMOD.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PARPOL2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_CHARLEN2.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI1_PARPOL3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_CHARLEN3.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT11_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT17_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT25_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT4_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT11_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT1_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_BASE_PORT.VALUE=0xFFF7F418
DRIVER.MIBSPI.VAR.MIBSPI4_BITERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT9_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_T2EDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_SHIFTDIR0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_RXINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT3_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_SHIFTDIR1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT0_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_BUF_CSNR.VALUE=CS_0
DRIVER.MIBSPI.VAR.MIBSPI5_SHIFTDIR2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT2_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_SHIFTDIR3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_CSDEF.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT8_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT11_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT8_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT5_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_ACTUALBAUDRATE0.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_BUF_CSNR.VALUE=CS_6
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_ACTUALBAUDRATE1.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT9_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI5_MASTER.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT3_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT9_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_ACTUALBAUDRATE2.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT10_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT0_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI2_ACTUALBAUDRATE3.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT1_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT9_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_BUF_CSNR.VALUE=CS_7
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_C2EDELAYACTUAL.VALUE=0.000
DRIVER.MIBSPI.VAR.MIBSPI4_C2EDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT5_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT4_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT2_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PARERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_OVRNINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_DLENERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT5_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT10_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_T2CDELAYACTUAL.VALUE=13.333
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT17_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT25_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT2_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT5_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT3_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT10_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT2_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT0_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT0_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT10_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT8_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT9_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT3_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT0_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_BAUDRATE0.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI4_T2CDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI1_BAUDRATE1.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT11_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT17_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT25_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT4_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT11_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT1_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_BAUDRATE2.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI2_TIMEOUTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT17_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT25_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_BAUDRATE3.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT2_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG5_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_BUF_CSNR.VALUE=CS_0
DRIVER.MIBSPI.VAR.MIBSPI4_BASE_RAM.VALUE=0xFF060000
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_CHARLEN0.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI3_TIMEOUTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT3_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT3_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_CHARLEN1.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI4_PARERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT10_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT0_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT11_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_CHARLEN2.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_BUF_CSNR.VALUE=CS_1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT8_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_POLARITY0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_CHARLEN3.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI1_POLARITY1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_BASE.VALUE=0xFFF7F400
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_POLARITY2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_RXINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_DEYSNCENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_POLARITY3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PHASE0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT17_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT25_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT4_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_BUF_CSNR.VALUE=CS_2
DRIVER.MIBSPI.VAR.MIBSPI4_C2TDELAYACTUAL.VALUE=26.667
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT11_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT1_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PHASE1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PHASE2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_DEYSNCLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT9_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT9_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_PHASE3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_BUF_CSNR.VALUE=CS_3
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT5_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_LENGTH.VALUE=8
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT2_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT8_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT5_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT3_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT10_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT0_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT5_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI3_TXINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT4_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT1_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_ENABLE.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT11_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_T2EDELAYACTUAL.VALUE=0.000
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT8_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT9_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG4_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT3_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT0_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT10_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT10_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT0_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_OVRNINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_BITERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT5_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT3_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT2_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_T2EDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT1_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI4_BITERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT11_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI3_SHIFTDIR0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_MASTER.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_SHIFTDIR1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_SHIFTDIR2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT8_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT1_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI3_SHIFTDIR3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT3_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT27_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT19_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT3_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT17_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT25_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT4_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT11_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT1_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_BUF_CSNR.VALUE=CS_2
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT8_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT5_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG4_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PRESCALE0.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT10_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_BUF_CSNR.VALUE=CS_3
DRIVER.MIBSPI.VAR.MIBSPI5_PRESCALE1.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI2_BASE.VALUE=0xFFF7F600
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT25_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT17_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PRESCALE2.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT1_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT11_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PRESCALE3.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI4_DLENERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.MIBSPI.VAR.MIBSPI5_PARITYENA0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_BUF_CSNR.VALUE=CS_4
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT3_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PARITYENA1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI2_C2TDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PARITYENA2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_DLENERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_CSDEF.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI4_BASE_PORT.VALUE=0xFFF7FA18
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_PARITYENA3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT8_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT5_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_BUF_CSNR.VALUE=CS_5
DRIVER.MIBSPI.VAR.MIBSPI3_WAITENA0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT9_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_WAITENA1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_WAITENA2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT8_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT4_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG7_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT1_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_WAITENA3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_BUF_CSNR.VALUE=CS_6
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT5_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT2_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_T2EDELAYACTUAL.VALUE=0.000
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT9_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT0_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT10_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI2_TG1_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TXINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TIMEOUTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG1_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_CLKMOD.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_ENABLEHIGHZ.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT9_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PHASE0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_C2EDELAYACTUAL.VALUE=0.000
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI3_PHASE1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT26_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT18_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT17_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT25_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT4_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT2_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PHASE2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TIMEOUTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT11_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT1_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PHASE3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PARERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI4_T2CDELAYACTUAL.VALUE=13.333
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT4_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT4_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT2_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI4_TG3_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PARERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT3_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG4_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT0_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT10_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT2_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG6_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_T2EDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT8_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_RXINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG7_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_DEYSNCLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT5_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_WDELAY0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT0_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT10_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT3_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_ENABLEHIGHZ.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_WDELAY1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT25_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT17_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG5_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_WDELAY2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT1_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT11_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_LENGTH.VALUE=8
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT17_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT25_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_WDELAY3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT11_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_BAUDRATE0.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI1_TG5_BUF_CSNR.VALUE=CS_5
DRIVER.MIBSPI.VAR.MIBSPI4_BAUDRATE1.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_BASE.VALUE=0xFFF7F800
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT27_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT19_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_BAUDRATE2.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT3_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_MASTER.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_BAUDRATE3.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT8_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT8_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_BUF_CSNR.VALUE=CS_6
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT5_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG0_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG4_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI3_C2EDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG7_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI2_TG2_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG2_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT25_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT17_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_BUF_LOCK.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_OVRNINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT1_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT11_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT25_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT17_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_C2TDELAYACTUAL.VALUE=26.667
DRIVER.MIBSPI.VAR.MIBSPI4_POLARITY0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT1_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG7_BUF_CSNR.VALUE=CS_7
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT11_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_TG3_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_C2TDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_POLARITY1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_OVRNINTLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT9_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_TG0_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI4_POLARITY2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT9_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI2_TG0_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_BITERRLVL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_SHIFTDIR0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT10_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG6_BUF_MODE.VALUE=4
DRIVER.MIBSPI.VAR.MIBSPI5_DEYSNCENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG6_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI4_POLARITY3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_SHIFTDIR1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG1_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT4_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_SHIFTDIR2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_TG6_TRGSRC.VALUE=TRG_DISABLED
DRIVER.MIBSPI.VAR.MIBSPI1_SHIFTDIR3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT26_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT18_FUN.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_TG0_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT2_FUN.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT17_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT25_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT8_DIR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG2_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT0_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT10_PSL.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI2_TG4_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_T2CDELAY.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT5_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT4_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG2_TRGEVT.VALUE=TRG_ALWAYS
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_BUF_CSHOLD_LASTBUF.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT2_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI1_CSDEF.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_CS_ENCODE.VALUE=0xFF
DRIVER.MIBSPI.VAR.MIBSPI5_TG7_USE_CS_ENCODE.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TXINTENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT3_PULDIS.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG3_BUF_WDEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_TG2_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_ACTUALBAUDRATE0.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT9_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PORT_BIT8_DOUT.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG6_PRST.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PRESCALE0.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI2_TG3_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI1_PORT_BIT5_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_ACTUALBAUDRATE1.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI3_PRESCALE1.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI3_BASE_RAM.VALUE=0xFF0C0000
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT3_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT0_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_ACTUALBAUDRATE2.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_PARPOL0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG1_LENGTH.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT10_DIR.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI3_TG3_BUF_CSHOLD.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PRESCALE2.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI3_CHARLEN0.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT0_PULL.VALUE=2
DRIVER.MIBSPI.VAR.MIBSPI5_ACTUALBAUDRATE3.VALUE=1000.000
DRIVER.MIBSPI.VAR.MIBSPI5_PARPOL1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PRESCALE3.VALUE=74
DRIVER.MIBSPI.VAR.MIBSPI3_CHARLEN1.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI3_DLENERRENA.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT26_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PORT_BIT18_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI5_PARPOL2.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_TG5_ONESHOT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI4_PARITYENA0.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_PORT_BIT2_PDR.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG5_BUF_DFSEL.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_TG0_BUF_CSNR.VALUE=CS_0
DRIVER.MIBSPI.VAR.MIBSPI3_CHARLEN2.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI2_PORT_BIT3_DOUT.VALUE=1
DRIVER.MIBSPI.VAR.MIBSPI5_PARPOL3.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI4_PARITYENA1.VALUE=0
DRIVER.MIBSPI.VAR.MIBSPI3_CHARLEN3.VALUE=16
DRIVER.MIBSPI.VAR.MIBSPI1_TG1_TRGSRC.VALUE=TRG_DISABLED
DRIVER.SPI.VAR.SPI5_PORT_BIT26_DIR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT18_DIR.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT4_PULL.VALUE=2
DRIVER.SPI.VAR.SPI3_PHASE2.VALUE=0
DRIVER.SPI.VAR.SPI2_TIMEOUTLVL.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT1_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_PORT_BIT25_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT17_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI3_PHASE3.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT11_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_T2CDELAYACTUAL.VALUE=13.333
DRIVER.SPI.VAR.SPI4_POLARITY0.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT1_PDR.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT4_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI4_POLARITY1.VALUE=0
DRIVER.SPI.VAR.SPI2_T2EDELAY.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT2_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_PORT_BIT9_FUN.VALUE=1
DRIVER.SPI.VAR.SPI4_POLARITY2.VALUE=0
DRIVER.SPI.VAR.SPI2_BITERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI1_SHIFTDIR0.VALUE=0
DRIVER.SPI.VAR.SPI1_RXINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT10_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_DEYSNCENA.VALUE=0
DRIVER.SPI.VAR.SPI4_POLARITY3.VALUE=0
DRIVER.SPI.VAR.SPI1_SHIFTDIR1.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT5_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT10_PDR.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT2_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT4_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_SHIFTDIR2.VALUE=0
DRIVER.SPI.VAR.SPI1_SHIFTDIR3.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT2_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT10_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_PORT_BIT8_DIR.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT0_PSL.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT0_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT25_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT17_FUN.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT11_PULL.VALUE=2
DRIVER.SPI.VAR.SPI3_PORT_BIT4_DIR.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT11_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT25_DIR.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT17_DIR.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT0_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT9_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_PRESCALE0.VALUE=74
DRIVER.SPI.VAR.SPI3_PRESCALE1.VALUE=74
DRIVER.SPI.VAR.SPI1_C2EDELAY.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT27_DIR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT19_DIR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT0_DIR.VALUE=1
DRIVER.SPI.VAR.SPI3_PRESCALE2.VALUE=74
DRIVER.SPI.VAR.SPI1_MASTER.VALUE=1
DRIVER.SPI.VAR.SPI3_PRESCALE3.VALUE=74
DRIVER.SPI.VAR.SPI3_PORT_BIT2_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_C2TDELAY.VALUE=0
DRIVER.SPI.VAR.SPI2_BASE_PORT.VALUE=0xFFF7F618
DRIVER.SPI.VAR.SPI5_BITERRENA.VALUE=0
DRIVER.SPI.VAR.SPI4_OVRNINTENA.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT9_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT25_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT17_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_C2TDELAYACTUAL.VALUE=26.667
DRIVER.SPI.VAR.SPI4_PORT_BIT10_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT8_PSL.VALUE=1
DRIVER.SPI.VAR.SPI4_WAITENA0.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT11_PDR.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT5_PSL.VALUE=1
DRIVER.SPI.VAR.SPI4_WAITENA1.VALUE=0
DRIVER.SPI.VAR.SPI5_OVRNINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI4_WAITENA2.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT3_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT9_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_PORT_BIT9_DIR.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT5_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_WAITENA3.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT2_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT1_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_T2CDELAY.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT26_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT18_FUN.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT5_DIR.VALUE=1
DRIVER.SPI.VAR.SPI3_TXINTENA.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT10_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_BASE_RAM.VALUE=0xFF0E0000
DRIVER.SPI.VAR.SPI5_PORT_BIT1_DIR.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT5_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_PORT_BIT2_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_CHARLEN0.VALUE=16
DRIVER.SPI.VAR.SPI1_CHARLEN1.VALUE=16
DRIVER.SPI.VAR.SPI4_PORT_BIT8_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT3_PDR.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT5_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI1_CHARLEN2.VALUE=16
DRIVER.SPI.VAR.SPI1_CHARLEN3.VALUE=16
DRIVER.SPI.VAR.SPI5_PORT_BIT3_PULL.VALUE=2
DRIVER.SPI.VAR.SPI3_PORT_BIT10_DIR.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT0_PULL.VALUE=2
DRIVER.SPI.VAR.SPI2_PARERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT8_FUN.VALUE=1
DRIVER.SPI.VAR.SPI3_DLENERRENA.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT26_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT18_PDR.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT9_PSL.VALUE=1
DRIVER.SPI.VAR.SPI4_PARITYENA0.VALUE=0
DRIVER.SPI.VAR.SPI4_ENABLEHIGHZ.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT3_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI5_T2EDELAY.VALUE=0
DRIVER.SPI.VAR.SPI4_PARITYENA1.VALUE=0
DRIVER.SPI.VAR.SPI4_PARITYENA2.VALUE=0
DRIVER.SPI.VAR.SPI4_DLENERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI4_RXINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT4_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT25_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT17_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT11_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_PORT_BIT3_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_PARITYENA3.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT0_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT2_PSL.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT1_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI3_CLKMOD.VALUE=1
DRIVER.SPI.VAR.SPI1_PHASE0.VALUE=0
DRIVER.SPI.VAR.SPI1_PHASE1.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT27_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT19_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT0_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_PHASE2.VALUE=0
DRIVER.SPI.VAR.SPI1_PHASE3.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT25_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT17_PSL.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT11_PSL.VALUE=1
DRIVER.SPI.VAR.SPI2_BAUDRATE0.VALUE=1000.000
DRIVER.SPI.VAR.SPI1_PORT_BIT8_PDR.VALUE=0
DRIVER.SPI.VAR.SPI2_BAUDRATE1.VALUE=1000.000
DRIVER.SPI.VAR.SPI5_PORT_BIT2_DIR.VALUE=1
DRIVER.SPI.VAR.SPI2_BAUDRATE2.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_BAUDRATE3.VALUE=1000.000
DRIVER.SPI.VAR.SPI5_WDELAY0.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT4_PDR.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT10_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT25_PDR.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT17_PDR.VALUE=0
DRIVER.SPI.VAR.SPI1_C2TDELAYACTUAL.VALUE=26.667
DRIVER.SPI.VAR.SPI1_ENABLEHIGHZ.VALUE=0
DRIVER.SPI.VAR.SPI5_WDELAY1.VALUE=0
DRIVER.SPI.VAR.SPI4_C2EDELAY.VALUE=0
DRIVER.SPI.VAR.SPI5_WDELAY2.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT11_DIR.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT9_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_TIMEOUTLVL.VALUE=0
DRIVER.SPI.VAR.SPI5_WDELAY3.VALUE=0
DRIVER.SPI.VAR.SPI5_PARERRENA.VALUE=0
DRIVER.SPI.VAR.SPI4_RAM_PARITY_ENA.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT5_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT27_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT19_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT0_PDR.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT11_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI2_POLARITY0.VALUE=0
DRIVER.SPI.VAR.SPI2_POLARITY1.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT5_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_POLARITY2.VALUE=0
DRIVER.SPI.VAR.SPI3_DEYSNCENA.VALUE=0
DRIVER.SPI.VAR.SPI2_POLARITY3.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT11_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT3_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT1_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_DEYSNCLVL.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT8_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_PORT_BIT10_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT26_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT18_PSL.VALUE=1
DRIVER.SPI.VAR.SPI2_T2EDELAYACTUAL.VALUE=0.000
DRIVER.SPI.VAR.SPI1_PORT_BIT9_PDR.VALUE=0
DRIVER.SPI.VAR.SPI4_T2CDELAY.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT3_DIR.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT10_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT0_DIR.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT3_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_PORT_BIT9_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT5_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_C2EDELAYACTUAL.VALUE=0.000
DRIVER.SPI.VAR.SPI1_PRESCALE0.VALUE=74
DRIVER.SPI.VAR.SPI4_BASE_RAM.VALUE=0xFF060000
DRIVER.SPI.VAR.SPI1_PRESCALE1.VALUE=74
DRIVER.SPI.VAR.SPI5_PORT_BIT4_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_CHARLEN0.VALUE=16
DRIVER.SPI.VAR.SPI2_PORT_BIT1_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_PRESCALE2.VALUE=74
DRIVER.SPI.VAR.SPI4_PORT_BIT3_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_CHARLEN1.VALUE=16
DRIVER.SPI.VAR.SPI1_PORT_BIT0_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI1_PRESCALE3.VALUE=74
DRIVER.SPI.VAR.SPI5_PORT_BIT1_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_T2CDELAYACTUAL.VALUE=13.333
DRIVER.SPI.VAR.SPI4_CHARLEN2.VALUE=16
DRIVER.SPI.VAR.SPI1_PORT_BIT8_PSL.VALUE=1
DRIVER.SPI.VAR.SPI4_CHARLEN3.VALUE=16
DRIVER.SPI.VAR.SPI1_BASE.VALUE=0xFFF7F400
DRIVER.SPI.VAR.SPI3_BITERRENA.VALUE=0
DRIVER.SPI.VAR.SPI3_OVRNINTENA.VALUE=0
DRIVER.SPI.VAR.SPI3_RXINTENA.VALUE=0
DRIVER.SPI.VAR.SPI5_ACTUALBAUDRATE0.VALUE=1000.000
DRIVER.SPI.VAR.SPI3_PORT_BIT10_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT4_PSL.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT2_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT25_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT17_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_ACTUALBAUDRATE1.VALUE=1000.000
DRIVER.SPI.VAR.SPI5_PORT_BIT2_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_ACTUALBAUDRATE2.VALUE=1000.000
DRIVER.SPI.VAR.SPI5_PARPOL0.VALUE=0
DRIVER.SPI.VAR.SPI5_BITERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI4_SHIFTDIR0.VALUE=0
DRIVER.SPI.VAR.SPI4_OVRNINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT8_DIR.VALUE=0
DRIVER.SPI.VAR.SPI5_ACTUALBAUDRATE3.VALUE=1000.000
DRIVER.SPI.VAR.SPI5_PARPOL1.VALUE=0
DRIVER.SPI.VAR.SPI4_SHIFTDIR1.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT27_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT19_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT0_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_PARPOL2.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT0_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI4_SHIFTDIR2.VALUE=0
DRIVER.SPI.VAR.SPI5_PARPOL3.VALUE=0
DRIVER.SPI.VAR.SPI4_SHIFTDIR3.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT4_DIR.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT11_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT1_DIR.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT8_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT25_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT17_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT11_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI3_TXINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT1_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT2_PDR.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT9_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_CLKMOD.VALUE=1
DRIVER.SPI.VAR.SPI5_TIMEOUTENA.VALUE=0
DRIVER.SPI.VAR.SPI2_DLENERRENA.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT11_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT5_PSL.VALUE=1
DRIVER.SPI.VAR.SPI3_PARITYENA0.VALUE=0
DRIVER.SPI.VAR.SPI3_PARITYENA1.VALUE=0
DRIVER.SPI.VAR.SPI1_T2EDELAY.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT3_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_BASE_PORT.VALUE=0xFFF7FC18
DRIVER.SPI.VAR.SPI3_PORT_BIT9_PULL.VALUE=2
DRIVER.SPI.VAR.SPI3_PORT_BIT9_DIR.VALUE=1
DRIVER.SPI.VAR.SPI3_PARITYENA2.VALUE=0
DRIVER.SPI.VAR.SPI3_DLENERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT0_FUN.VALUE=1
DRIVER.SPI.VAR.SPI3_PARITYENA3.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT1_PSL.VALUE=1
DRIVER.SPI.VAR.SPI4_WDELAY0.VALUE=0
DRIVER.SPI.VAR.SPI4_WDELAY1.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT5_DIR.VALUE=1
DRIVER.SPI.VAR.SPI4_WDELAY2.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT2_DIR.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT4_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_WDELAY3.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT3_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT10_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_T2CDELAYACTUAL.VALUE=13.333
DRIVER.SPI.VAR.SPI5_PORT_BIT5_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_MASTER.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT2_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_PORT_BIT8_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT3_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_ACTUALBAUDRATE0.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_PORT_BIT0_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_ACTUALBAUDRATE1.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_BASE.VALUE=0xFFF7F600
DRIVER.SPI.VAR.SPI4_PORT_BIT10_DIR.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT8_FUN.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT0_PULL.VALUE=2
DRIVER.SPI.VAR.SPI3_ACTUALBAUDRATE2.VALUE=1000.000
DRIVER.SPI.VAR.SPI3_ACTUALBAUDRATE3.VALUE=1000.000
DRIVER.SPI.VAR.SPI3_PARERRENA.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT3_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI2_C2TDELAY.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT4_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_PARERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT1_FUN.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT8_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT5_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI1_DEYSNCENA.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT2_PSL.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT1_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI3_WAITENA0.VALUE=0
DRIVER.SPI.VAR.SPI3_WAITENA1.VALUE=0
DRIVER.SPI.VAR.SPI3_WAITENA2.VALUE=0
DRIVER.SPI.VAR.SPI3_DEYSNCLVL.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT3_DIR.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT1_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI3_WAITENA3.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT26_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT18_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT11_PSL.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT8_PDR.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT10_PULL.VALUE=2
DRIVER.SPI.VAR.SPI3_PORT_BIT10_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI2_TXINTENA.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT4_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_BAUDRATE0.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_PORT_BIT1_PDR.VALUE=0
DRIVER.SPI.VAR.SPI2_C2TDELAYACTUAL.VALUE=26.667
DRIVER.SPI.VAR.SPI5_BAUDRATE1.VALUE=1000.000
DRIVER.SPI.VAR.SPI5_BAUDRATE2.VALUE=1000.000
DRIVER.SPI.VAR.SPI4_PORT_BIT11_DIR.VALUE=0
DRIVER.SPI.VAR.SPI4_PARPOL0.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT9_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_BAUDRATE3.VALUE=1000.000
DRIVER.SPI.VAR.SPI5_RAM_PARITY_ENA.VALUE=0
DRIVER.SPI.VAR.SPI4_PARPOL1.VALUE=0
DRIVER.SPI.VAR.SPI4_PARPOL2.VALUE=0
DRIVER.SPI.VAR.SPI4_PARPOL3.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT5_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT2_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT3_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI2_OVRNINTENA.VALUE=0
DRIVER.SPI.VAR.SPI1_BITERRENA.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT3_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_POLARITY0.VALUE=0
DRIVER.SPI.VAR.SPI4_PHASE0.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT0_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_POLARITY1.VALUE=0
DRIVER.SPI.VAR.SPI4_T2EDELAY.VALUE=0
DRIVER.SPI.VAR.SPI4_PHASE1.VALUE=0
DRIVER.SPI.VAR.SPI5_POLARITY2.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT8_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_PHASE2.VALUE=0
DRIVER.SPI.VAR.SPI3_BITERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI3_OVRNINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI3_RXINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI2_SHIFTDIR0.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT5_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_PORT_BIT26_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT18_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_POLARITY3.VALUE=0
DRIVER.SPI.VAR.SPI4_PHASE3.VALUE=0
DRIVER.SPI.VAR.SPI2_SHIFTDIR1.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT9_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_T2EDELAYACTUAL.VALUE=0.000
DRIVER.SPI.VAR.SPI2_SHIFTDIR2.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT8_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI1_ACTUALBAUDRATE0.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_SHIFTDIR3.VALUE=0
DRIVER.SPI.VAR.SPI1_ACTUALBAUDRATE1.VALUE=1000.000
DRIVER.SPI.VAR.SPI4_PORT_BIT10_FUN.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT0_DIR.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT3_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_ACTUALBAUDRATE2.VALUE=1000.000
DRIVER.SPI.VAR.SPI5_PORT_BIT11_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI1_ACTUALBAUDRATE3.VALUE=1000.000
DRIVER.SPI.VAR.SPI5_PORT_BIT9_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT5_PDR.VALUE=0
DRIVER.SPI.VAR.SPI4_C2EDELAYACTUAL.VALUE=0.000
DRIVER.SPI.VAR.SPI2_PORT_BIT2_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_BASE.VALUE=0xFFF7F800
DRIVER.SPI.VAR.SPI3_PORT_BIT1_PULL.VALUE=2
DRIVER.SPI.VAR.SPI3_PORT_BIT8_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_PRESCALE0.VALUE=74
DRIVER.SPI.VAR.SPI3_PORT_BIT8_PSL.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT4_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI3_WDELAY0.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT25_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT17_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI4_PRESCALE1.VALUE=74
DRIVER.SPI.VAR.SPI3_C2EDELAY.VALUE=0
DRIVER.SPI.VAR.SPI3_WDELAY1.VALUE=0
DRIVER.SPI.VAR.SPI4_PRESCALE2.VALUE=74
DRIVER.SPI.VAR.SPI3_WDELAY2.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT3_FUN.VALUE=1
DRIVER.SPI.VAR.SPI4_PRESCALE3.VALUE=74
DRIVER.SPI.VAR.SPI4_TIMEOUTENA.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT1_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI3_WDELAY3.VALUE=0
DRIVER.SPI.VAR.SPI1_DLENERRENA.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT4_PSL.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT10_PDR.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT2_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI3_ENABLEHIGHZ.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT1_PSL.VALUE=1
DRIVER.SPI.VAR.SPI2_PARITYENA0.VALUE=0
DRIVER.SPI.VAR.SPI5_C2TDELAY.VALUE=0
DRIVER.SPI.VAR.SPI2_PARITYENA1.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT8_DIR.VALUE=0
DRIVER.SPI.VAR.SPI5_TIMEOUTLVL.VALUE=0
DRIVER.SPI.VAR.SPI3_BASE_PORT.VALUE=0xFFF7F818
DRIVER.SPI.VAR.SPI2_PORT_BIT10_PULL.VALUE=2
DRIVER.SPI.VAR.SPI2_PARITYENA2.VALUE=0
DRIVER.SPI.VAR.SPI2_DLENERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI2_MASTER.VALUE=1
DRIVER.SPI.VAR.SPI2_PARITYENA3.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT27_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT19_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT0_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT11_FUN.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT11_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_PORT_BIT1_DIR.VALUE=1
DRIVER.SPI.VAR.SPI1_RAM_PARITY_ENA.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT3_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_T2CDELAY.VALUE=0
DRIVER.SPI.VAR.SPI5_TXINTENA.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT3_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT9_PSL.VALUE=1
DRIVER.SPI.VAR.SPI3_BASE_RAM.VALUE=0xFF0C0000
DRIVER.SPI.VAR.SPI3_CHARLEN0.VALUE=16
DRIVER.SPI.VAR.SPI3_CHARLEN1.VALUE=16
DRIVER.SPI.VAR.SPI1_PARERRENA.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT10_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT5_PSL.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT11_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_CHARLEN2.VALUE=16
DRIVER.SPI.VAR.SPI2_PORT_BIT2_PSL.VALUE=1
DRIVER.SPI.VAR.SPI3_CHARLEN3.VALUE=16
DRIVER.SPI.VAR.SPI5_PORT_BIT9_DIR.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT9_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_PORT_BIT0_FUN.VALUE=1
DRIVER.SPI.VAR.SPI3_PARERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI2_RXINTENA.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT9_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT2_DIR.VALUE=1
DRIVER.SPI.VAR.SPI3_PARPOL0.VALUE=0
DRIVER.SPI.VAR.SPI1_DEYSNCLVL.VALUE=0
DRIVER.SPI.VAR.SPI3_PARPOL1.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT8_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT10_PSL.VALUE=1
DRIVER.SPI.VAR.SPI3_PARPOL2.VALUE=0
DRIVER.SPI.VAR.SPI2_T2CDELAYACTUAL.VALUE=13.333
DRIVER.SPI.VAR.SPI4_BASE.VALUE=0xFFF7FA00
DRIVER.SPI.VAR.SPI3_PARPOL3.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT2_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_PORT_BIT4_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT1_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT0_PDR.VALUE=0
DRIVER.SPI.VAR.SPI4_CLKMOD.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT5_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI3_BAUDRATE0.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_PHASE0.VALUE=0
DRIVER.SPI.VAR.SPI3_BAUDRATE1.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_PHASE1.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT10_DIR.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT8_FUN.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT0_PULL.VALUE=2
DRIVER.SPI.VAR.SPI3_BAUDRATE2.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_PHASE2.VALUE=0
DRIVER.SPI.VAR.SPI2_TXINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI3_BAUDRATE3.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_PORT_BIT10_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI2_PHASE3.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT3_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT3_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT0_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT25_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_PORT_BIT17_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_PORT_BIT1_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT11_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_OVRNINTENA.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT1_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI3_POLARITY0.VALUE=0
DRIVER.SPI.VAR.SPI3_POLARITY1.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT3_DIR.VALUE=1
DRIVER.SPI.VAR.SPI3_POLARITY2.VALUE=0
DRIVER.SPI.VAR.SPI2_OVRNINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT0_DIR.VALUE=1
DRIVER.SPI.VAR.SPI1_BITERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI4_DEYSNCENA.VALUE=0
DRIVER.SPI.VAR.SPI3_POLARITY3.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT8_PDR.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT11_PSL.VALUE=1
DRIVER.SPI.VAR.SPI2_WDELAY0.VALUE=0
DRIVER.SPI.VAR.SPI2_WDELAY1.VALUE=0
DRIVER.SPI.VAR.SPI2_WDELAY2.VALUE=0
DRIVER.SPI.VAR.SPI2_WDELAY3.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT1_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT10_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI3_C2TDELAYACTUAL.VALUE=26.667
DRIVER.SPI.VAR.SPI5_PORT_BIT11_DIR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT9_FUN.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT11_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT11_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI2_PRESCALE0.VALUE=74
DRIVER.SPI.VAR.SPI2_PRESCALE1.VALUE=74
DRIVER.SPI.VAR.SPI4_PORT_BIT2_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT8_DIR.VALUE=0
DRIVER.SPI.VAR.SPI2_PRESCALE2.VALUE=74
DRIVER.SPI.VAR.SPI3_TIMEOUTENA.VALUE=0
DRIVER.SPI.VAR.SPI2_PRESCALE3.VALUE=74
DRIVER.SPI.VAR.SPI1_PORT_BIT8_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT0_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_PARITYENA0.VALUE=0
DRIVER.SPI.VAR.SPI1_C2TDELAY.VALUE=0
DRIVER.SPI.VAR.SPI1_PARITYENA1.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT8_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_PORT_BIT4_DIR.VALUE=1
DRIVER.SPI.VAR.SPI4_TIMEOUTLVL.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT1_DIR.VALUE=1
DRIVER.SPI.VAR.SPI1_PARITYENA2.VALUE=0
DRIVER.SPI.VAR.SPI1_DLENERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI1_BASE_PORT.VALUE=0xFFF7F418
DRIVER.SPI.VAR.SPI5_RXINTENA.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT4_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_BITERRENA.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT1_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI1_PARITYENA3.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT9_PDR.VALUE=0
DRIVER.SPI.VAR.SPI4_T2EDELAYACTUAL.VALUE=0.000
DRIVER.SPI.VAR.SPI2_PORT_BIT8_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI2_WAITENA0.VALUE=0
DRIVER.SPI.VAR.SPI5_BASE.VALUE=0xFFF7FC00
DRIVER.SPI.VAR.SPI2_WAITENA1.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT10_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_SHIFTDIR0.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT3_PULL.VALUE=2
DRIVER.SPI.VAR.SPI2_WAITENA2.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT10_DIR.VALUE=1
DRIVER.SPI.VAR.SPI5_SHIFTDIR1.VALUE=0
DRIVER.SPI.VAR.SPI2_WAITENA3.VALUE=0
DRIVER.SPI.VAR.SPI5_C2EDELAYACTUAL.VALUE=0.000
DRIVER.SPI.VAR.SPI5_SHIFTDIR2.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT2_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_SHIFTDIR3.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT1_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_TXINTENA.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT8_PSL.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT4_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT1_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT26_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_PORT_BIT18_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_TXINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT3_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT9_DIR.VALUE=1
DRIVER.SPI.VAR.SPI2_PARPOL0.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT0_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT9_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI2_PARPOL1.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT10_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT2_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT1_PSL.VALUE=1
DRIVER.SPI.VAR.SPI2_PARPOL2.VALUE=0
DRIVER.SPI.VAR.SPI2_PARPOL3.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT5_DIR.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT2_DIR.VALUE=1
DRIVER.SPI.VAR.SPI1_PARERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT2_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI2_CLKMOD.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT10_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI3_T2EDELAY.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT11_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_RXINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT11_DIR.VALUE=0
DRIVER.SPI.VAR.SPI2_RAM_PARITY_ENA.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT3_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT11_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT0_PDR.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT8_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT9_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_BAUDRATE0.VALUE=1000.000
DRIVER.SPI.VAR.SPI1_BAUDRATE1.VALUE=1000.000
DRIVER.SPI.VAR.SPI4_PORT_BIT4_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT8_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_PORT_BIT1_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_BAUDRATE2.VALUE=1000.000
DRIVER.SPI.VAR.SPI3_PORT_BIT4_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT25_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT17_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI1_BAUDRATE3.VALUE=1000.000
DRIVER.SPI.VAR.SPI5_PORT_BIT11_PDR.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT2_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_WDELAY0.VALUE=0
DRIVER.SPI.VAR.SPI2_C2EDELAY.VALUE=0
DRIVER.SPI.VAR.SPI1_WDELAY1.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT9_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_MASTER.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT10_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT3_DIR.VALUE=1
DRIVER.SPI.VAR.SPI1_WDELAY2.VALUE=0
DRIVER.SPI.VAR.SPI4_PARERRENA.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT10_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI1_WDELAY3.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT9_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT8_PDR.VALUE=0
DRIVER.SPI.VAR.SPI1_C2EDELAYACTUAL.VALUE=0.000
DRIVER.SPI.VAR.SPI1_POLARITY0.VALUE=0
DRIVER.SPI.VAR.SPI4_C2TDELAY.VALUE=0
DRIVER.SPI.VAR.SPI1_POLARITY1.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT4_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_PORT_BIT25_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_PORT_BIT17_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_POLARITY2.VALUE=0
DRIVER.SPI.VAR.SPI1_OVRNINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI5_DLENERRENA.VALUE=0
DRIVER.SPI.VAR.SPI2_DEYSNCENA.VALUE=0
DRIVER.SPI.VAR.SPI1_POLARITY3.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT10_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_WAITENA0.VALUE=0
DRIVER.SPI.VAR.SPI5_ENABLEHIGHZ.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT4_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_T2CDELAYACTUAL.VALUE=13.333
DRIVER.SPI.VAR.SPI1_PORT_BIT1_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_WAITENA1.VALUE=0
DRIVER.SPI.VAR.SPI5_WAITENA2.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT2_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_DEYSNCLVL.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT9_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_WAITENA3.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT9_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT5_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI4_ACTUALBAUDRATE0.VALUE=1000.000
DRIVER.SPI.VAR.SPI1_PORT_BIT10_PDR.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT2_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI4_ACTUALBAUDRATE1.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_T2CDELAY.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT27_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_PORT_BIT19_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_PORT_BIT0_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_PORT_BIT5_FUN.VALUE=1
DRIVER.SPI.VAR.SPI4_ACTUALBAUDRATE2.VALUE=1000.000
DRIVER.SPI.VAR.SPI1_PORT_BIT2_FUN.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT2_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_ACTUALBAUDRATE3.VALUE=1000.000
DRIVER.SPI.VAR.SPI4_TXINTENA.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT3_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT3_PSL.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT0_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT0_PSL.VALUE=1
DRIVER.SPI.VAR.SPI2_BASE_RAM.VALUE=0xFF080000
DRIVER.SPI.VAR.SPI2_CHARLEN0.VALUE=16
DRIVER.SPI.VAR.SPI1_PORT_BIT11_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT4_DIR.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT11_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI2_CHARLEN1.VALUE=16
DRIVER.SPI.VAR.SPI2_TIMEOUTENA.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT9_PDR.VALUE=0
DRIVER.SPI.VAR.SPI2_CHARLEN2.VALUE=16
DRIVER.SPI.VAR.SPI2_ENABLEHIGHZ.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT11_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI2_CHARLEN3.VALUE=16
DRIVER.SPI.VAR.SPI3_PORT_BIT0_DIR.VALUE=1
DRIVER.SPI.VAR.SPI3_TIMEOUTLVL.VALUE=0
DRIVER.SPI.VAR.SPI2_BITERRENA.VALUE=0
DRIVER.SPI.VAR.SPI1_RXINTENA.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT11_PSL.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT5_PDR.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT2_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT10_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_RXINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI4_BITERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI3_SHIFTDIR0.VALUE=0
DRIVER.SPI.VAR.SPI1_PARPOL0.VALUE=0
DRIVER.SPI.VAR.SPI3_SHIFTDIR1.VALUE=0
DRIVER.SPI.VAR.SPI1_PARPOL1.VALUE=0
DRIVER.SPI.VAR.SPI5_PHASE0.VALUE=0
DRIVER.SPI.VAR.SPI4_C2TDELAYACTUAL.VALUE=26.667
DRIVER.SPI.VAR.SPI3_SHIFTDIR2.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT8_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT11_PDR.VALUE=0
DRIVER.SPI.VAR.SPI1_PARPOL2.VALUE=0
DRIVER.SPI.VAR.SPI5_PHASE1.VALUE=0
DRIVER.SPI.VAR.SPI3_SHIFTDIR3.VALUE=0
DRIVER.SPI.VAR.SPI1_PARPOL3.VALUE=0
DRIVER.SPI.VAR.SPI5_PHASE2.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT9_PULL.VALUE=2
DRIVER.SPI.VAR.SPI1_PORT_BIT3_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT27_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT19_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT0_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_PHASE3.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT4_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT1_PSL.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT8_DIR.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT5_DIR.VALUE=1
DRIVER.SPI.VAR.SPI1_TXINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI5_PRESCALE0.VALUE=74
DRIVER.SPI.VAR.SPI1_PORT_BIT10_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_C2EDELAY.VALUE=0
DRIVER.SPI.VAR.SPI5_PRESCALE1.VALUE=74
DRIVER.SPI.VAR.SPI5_PRESCALE2.VALUE=74
DRIVER.SPI.VAR.SPI3_PORT_BIT5_PULL.VALUE=2
DRIVER.SPI.VAR.SPI3_PORT_BIT1_DIR.VALUE=1
DRIVER.SPI.VAR.SPI5_PRESCALE3.VALUE=74
DRIVER.SPI.VAR.SPI3_PORT_BIT9_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_T2EDELAYACTUAL.VALUE=0.000
DRIVER.SPI.VAR.SPI3_PORT_BIT8_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI2_ACTUALBAUDRATE0.VALUE=1000.000
DRIVER.SPI.VAR.SPI1_PORT_BIT3_PDR.VALUE=0
DRIVER.SPI.VAR.SPI2_ACTUALBAUDRATE1.VALUE=1000.000
DRIVER.SPI.VAR.SPI4_PORT_BIT3_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_BASE_PORT.VALUE=0xFFF7FA18
DRIVER.SPI.VAR.SPI2_PORT_BIT10_DIR.VALUE=1
DRIVER.SPI.VAR.SPI2_ACTUALBAUDRATE2.VALUE=1000.000
DRIVER.SPI.VAR.SPI1_PORT_BIT0_PULL.VALUE=2
DRIVER.SPI.VAR.SPI5_OVRNINTENA.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT2_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI2_ACTUALBAUDRATE3.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_PORT_BIT9_PSL.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT3_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT1_PULL.VALUE=2
DRIVER.SPI.VAR.SPI3_MASTER.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT4_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT4_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT5_PSL.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT1_DOUT.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT2_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_T2CDELAY.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT9_DIR.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT0_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_PORT_BIT11_PSL.VALUE=1
DRIVER.SPI.VAR.SPI5_BASE_RAM.VALUE=0xFF0A0000
DRIVER.SPI.VAR.SPI5_CHARLEN0.VALUE=16
DRIVER.SPI.VAR.SPI3_PORT_BIT10_PULL.VALUE=2
DRIVER.SPI.VAR.SPI3_PORT_BIT2_DIR.VALUE=1
DRIVER.SPI.VAR.SPI5_CHARLEN1.VALUE=16
DRIVER.SPI.VAR.SPI2_PARERRENA.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT4_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI5_CHARLEN2.VALUE=16
DRIVER.SPI.VAR.SPI1_PORT_BIT4_PDR.VALUE=0
DRIVER.SPI.VAR.SPI5_CHARLEN3.VALUE=16
DRIVER.SPI.VAR.SPI5_PORT_BIT25_DIR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT17_DIR.VALUE=0
DRIVER.SPI.VAR.SPI5_PORT_BIT11_PULL.VALUE=2
DRIVER.SPI.VAR.SPI4_PARERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI2_PORT_BIT11_DIR.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT0_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_DLENERRENA.VALUE=0
DRIVER.SPI.VAR.SPI4_RXINTENA.VALUE=0
DRIVER.SPI.VAR.SPI3_RAM_PARITY_ENA.VALUE=0
DRIVER.SPI.VAR.SPI5_PARITYENA0.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT0_PDR.VALUE=0
DRIVER.SPI.VAR.SPI1_WAITENA0.VALUE=0
DRIVER.SPI.VAR.SPI5_PARITYENA1.VALUE=0
DRIVER.SPI.VAR.SPI1_WAITENA1.VALUE=0
DRIVER.SPI.VAR.SPI5_PARITYENA2.VALUE=0
DRIVER.SPI.VAR.SPI5_DLENERRLVL.VALUE=0
DRIVER.SPI.VAR.SPI4_PORT_BIT8_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_DEYSNCLVL.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT5_FUN.VALUE=1
DRIVER.SPI.VAR.SPI1_WAITENA2.VALUE=0
DRIVER.SPI.VAR.SPI5_PARITYENA3.VALUE=0
DRIVER.SPI.VAR.SPI1_WAITENA3.VALUE=0
DRIVER.SPI.VAR.SPI1_PORT_BIT3_PSL.VALUE=1
DRIVER.SPI.VAR.SPI3_PORT_BIT1_FUN.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT8_PULL.VALUE=2
DRIVER.SPI.VAR.SPI2_PORT_BIT9_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_BAUDRATE0.VALUE=1000.000
DRIVER.SPI.VAR.SPI1_T2EDELAYACTUAL.VALUE=0.000
DRIVER.SPI.VAR.SPI4_BAUDRATE1.VALUE=1000.000
DRIVER.SPI.VAR.SPI4_BAUDRATE2.VALUE=1000.000
DRIVER.SPI.VAR.SPI4_TXINTLVL.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT3_DIR.VALUE=1
DRIVER.SPI.VAR.SPI2_PORT_BIT10_FUN.VALUE=1
DRIVER.SPI.VAR.SPI5_PORT_BIT5_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI4_BAUDRATE3.VALUE=1000.000
DRIVER.SPI.VAR.SPI2_PORT_BIT2_PULDIS.VALUE=0
DRIVER.SPI.VAR.SPI1_TIMEOUTENA.VALUE=0
DRIVER.SPI.VAR.SPI5_CLKMOD.VALUE=1
DRIVER.SPI.VAR.SPI4_PORT_BIT8_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_PORT_BIT9_DOUT.VALUE=0
DRIVER.SPI.VAR.SPI3_PHASE0.VALUE=0
DRIVER.SPI.VAR.SPI2_C2EDELAYACTUAL.VALUE=0.000
DRIVER.SPI.VAR.SPI1_PORT_BIT5_PDR.VALUE=0
DRIVER.SPI.VAR.SPI3_PHASE1.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_51_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_51_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_43_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_43_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_35_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_35_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_27_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_27_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_19_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_19_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_51_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_43_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_35_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_27_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_19_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_21_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_21_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_13_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_13_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_59_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_9_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_30_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_22_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_14_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_4_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_61_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_53_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_45_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_37_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_29_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_6_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.CAN.VAR.CAN_1_MESSAGE_59_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_64_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_56_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_48_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_SYNC.VALUE=1
DRIVER.CAN.VAR.CAN_4_MESSAGE_62_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_54_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_46_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_38_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_SHIFT.VALUE=0
DRIVER.CAN.VAR.CAN_4_AUTO_BUS_ON.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_4_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_4_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_40_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_32_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_24_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_16_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_57_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_49_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_64_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_56_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_48_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_31_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_23_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_15_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_51_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_43_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_35_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_27_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_19_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_BAUDRATE.VALUE=500
DRIVER.CAN.VAR.CAN_2_PORT_RX_PDR.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_63_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_55_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_47_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_39_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_30_ID.VALUE=30
DRIVER.CAN.VAR.CAN_2_MESSAGE_22_ID.VALUE=22
DRIVER.CAN.VAR.CAN_2_MESSAGE_14_ID.VALUE=14
DRIVER.CAN.VAR.CAN_2_MESSAGE_9_ID.VALUE=9
DRIVER.CAN.VAR.CAN_1_MESSAGE_57_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_49_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_60_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_52_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_44_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_36_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_28_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_RAMBASE.VALUE=0xFF1C0000
DRIVER.CAN.VAR.CAN_1_MESSAGE_30_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_22_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_14_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_51_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_43_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_35_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_27_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_19_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_9_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_PORT_RX_PULDIS.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_57_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_49_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_4_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_2_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_64_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_56_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_48_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_NOMINAL_BIT_RATE.VALUE=500.000
DRIVER.CAN.VAR.CAN_1_MESSAGE_51_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_43_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_35_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_27_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_19_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_1_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_57_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_51_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_49_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_43_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_35_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_27_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_19_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_10_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_5_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_64_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_64_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_56_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_56_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_48_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_48_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_40_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_32_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_24_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_16_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_9_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_60_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_52_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_50_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_44_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_42_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_36_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_34_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_28_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_26_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_18_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_60_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_58_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_52_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_44_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_36_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_28_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_PIN_MODE.VALUE=1
DRIVER.CAN.VAR.CAN_2_PHASE_SEG.VALUE=4
DRIVER.CAN.VAR.CAN_1_MESSAGE_30_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_22_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_20_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_14_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_12_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_31_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_23_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_15_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_7_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_51_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_43_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_35_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_31_ID.VALUE=31
DRIVER.CAN.VAR.CAN_2_MESSAGE_27_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_23_ID.VALUE=23
DRIVER.CAN.VAR.CAN_2_MESSAGE_19_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_15_ID.VALUE=15
DRIVER.CAN.VAR.CAN_4_MESSAGE_1_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_NOMINAL_BIT_TIME.VALUE=15
DRIVER.CAN.VAR.CAN_4_MESSAGE_60_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_60_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_52_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_52_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_51_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_44_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_44_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_43_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_36_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_36_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_35_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_28_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_28_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_27_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_19_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_9_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_30_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_30_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_22_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_22_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_21_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_14_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_14_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_13_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_AUTO_BUS_ON.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_60_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_52_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_44_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_36_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_28_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_63_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_55_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_47_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_39_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_31_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_23_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_15_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_10_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_5_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_PORT_TX_PULDIS.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_30_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_22_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_14_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_51_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_43_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_35_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_27_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_19_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_7_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_21_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_13_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_57_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_49_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_BASE.VALUE=0xFFF7DC00
DRIVER.CAN.VAR.CAN_4_MESSAGE_9_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_40_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_32_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_24_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_16_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_10_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_10_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_5_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_5_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_6_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_40_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_32_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_24_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_16_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_11_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_1_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_8_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_3_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_3_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_10_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_4_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_21_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_13_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_64_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_56_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_48_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_40_ID.VALUE=40
DRIVER.CAN.VAR.CAN_2_MESSAGE_32_ID.VALUE=32
DRIVER.CAN.VAR.CAN_2_MESSAGE_24_ID.VALUE=24
DRIVER.CAN.VAR.CAN_2_MESSAGE_16_ID.VALUE=16
DRIVER.CAN.VAR.CAN_1_MESSAGE_1_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_61_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_53_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_45_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_37_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_29_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_31_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_23_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_15_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_1_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_1_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_21_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_13_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_6_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_6_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_IDENTIFIER_MODE.VALUE=0x40000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_57_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_49_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_11_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_57_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_49_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_40_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_32_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_24_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_16_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_3_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_60_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_52_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_44_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_36_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_28_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_11_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_6_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_PORT_RX_PULL.VALUE=1
DRIVER.CAN.VAR.CAN_4_MESSAGE_40_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_32_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_24_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_16_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_57_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_57_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_49_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_49_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_6_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_PORT_TX_DIN.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_10_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_61_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_53_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_45_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_37_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_29_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_59_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_51_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_43_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_35_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_27_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_19_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_1_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_31_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_23_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_15_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_40_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_32_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_24_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_16_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_8_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_PORT_RX_PSL.VALUE=1
DRIVER.CAN.VAR.CAN_2_MESSAGE_41_ID.VALUE=41
DRIVER.CAN.VAR.CAN_2_MESSAGE_33_ID.VALUE=33
DRIVER.CAN.VAR.CAN_2_MESSAGE_25_ID.VALUE=25
DRIVER.CAN.VAR.CAN_2_MESSAGE_17_ID.VALUE=17
DRIVER.CAN.VAR.CAN_1_MESSAGE_10_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_2_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_BRP_FREQ.VALUE=7.500
DRIVER.CAN.VAR.CAN_4_MESSAGE_61_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_61_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_53_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_53_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_45_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_45_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_37_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_37_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_29_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_29_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_6_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_21_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_13_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_PORT_TX_DIR.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_31_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_31_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_23_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_23_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_15_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_15_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_3_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_21_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_13_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_5_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_11_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_6_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_4_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_PROP_SEG.VALUE=6
DRIVER.CAN.VAR.CAN_3_MESSAGE_1_ID.VALUE=1
DRIVER.CAN.VAR.CAN_2_MESSAGE_64_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_56_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_48_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_1_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_SYNC.VALUE=1
DRIVER.CAN.VAR.CAN_3_MESSAGE_58_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_11_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_11_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_10_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_6_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_6_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_3_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_2_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_60_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_52_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_44_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_36_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_28_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_57_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_49_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_NOMINAL_BIT_RATE.VALUE=500.000
DRIVER.CAN.VAR.CAN_1_MESSAGE_64_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_56_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_48_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_64_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_56_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_48_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_57_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_50_ID.VALUE=50
DRIVER.CAN.VAR.CAN_2_MESSAGE_49_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_42_ID.VALUE=42
DRIVER.CAN.VAR.CAN_2_MESSAGE_34_ID.VALUE=34
DRIVER.CAN.VAR.CAN_2_MESSAGE_26_ID.VALUE=26
DRIVER.CAN.VAR.CAN_2_MESSAGE_18_ID.VALUE=18
DRIVER.CAN.VAR.CAN_1_MESSAGE_50_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_42_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_34_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_26_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_18_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_62_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_54_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_46_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_38_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_PROPAGATION_DELAY.VALUE=700
DRIVER.CAN.VAR.CAN_1_MESSAGE_40_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_32_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_24_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_16_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_21_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_13_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_2_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_2_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_3_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_58_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_BAUDRATE.VALUE=500
DRIVER.CAN.VAR.CAN_3_MESSAGE_58_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_50_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_42_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_34_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_26_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_18_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_60_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_57_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_52_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_49_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_44_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_36_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_28_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_10_ID.VALUE=10
DRIVER.CAN.VAR.CAN_4_MESSAGE_9_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_61_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_53_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_50_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_45_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_42_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_37_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_34_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_29_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_26_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_18_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_2_ID.VALUE=2
DRIVER.CAN.VAR.CAN_1_MESSAGE_6_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_NOMINAL_BIT_TIME.VALUE=15
DRIVER.CAN.VAR.CAN_2_MESSAGE_20_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_12_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_7_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_3_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_58_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_58_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_10_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_SAMPLE_POINT.VALUE=73.333
DRIVER.CAN.VAR.CAN_4_MESSAGE_62_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_54_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_46_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_38_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_8_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_7_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_61_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_53_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_45_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_37_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_29_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_21_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_20_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_13_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_12_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_40_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_32_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_24_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_16_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_5_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_4_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_41_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_33_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_25_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_17_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_9_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_51_ID.VALUE=51
DRIVER.CAN.VAR.CAN_2_MESSAGE_43_ID.VALUE=43
DRIVER.CAN.VAR.CAN_2_MESSAGE_35_ID.VALUE=35
DRIVER.CAN.VAR.CAN_2_MESSAGE_27_ID.VALUE=27
DRIVER.CAN.VAR.CAN_2_MESSAGE_20_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_19_ID.VALUE=19
DRIVER.CAN.VAR.CAN_2_MESSAGE_12_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_3_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_11_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_3_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_62_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_62_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_54_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_54_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_46_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_46_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_38_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_38_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_40_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_40_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_32_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_32_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_24_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_24_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_16_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_16_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_64_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_56_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_48_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_40_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_32_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_24_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_20_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_16_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_12_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_7_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_50_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_42_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_34_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_26_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_18_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_20_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_12_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_11_ID.VALUE=11
DRIVER.CAN.VAR.CAN_3_MESSAGE_3_ID.VALUE=3
DRIVER.CAN.VAR.CAN_2_PORT_RX_DOUT.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_2_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_59_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_BASE.VALUE=0xFFF7DE00
DRIVER.CAN.VAR.CAN_1_RAMBASE.VALUE=0xFF1E0000
DRIVER.CAN.VAR.CAN_4_MESSAGE_10_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_20_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_20_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_12_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_12_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_7_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_7_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_PORT_RX_PULL.VALUE=2
DRIVER.CAN.VAR.CAN_4_MESSAGE_63_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_55_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_47_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_41_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_39_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_33_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_25_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_17_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_3_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_1_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_9_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_IDENTIFIER_MODE.VALUE=0x40000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_41_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_33_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_25_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_17_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_11_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_60_ID.VALUE=60
DRIVER.CAN.VAR.CAN_2_MESSAGE_58_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_52_ID.VALUE=52
DRIVER.CAN.VAR.CAN_2_MESSAGE_44_ID.VALUE=44
DRIVER.CAN.VAR.CAN_2_MESSAGE_36_ID.VALUE=36
DRIVER.CAN.VAR.CAN_2_MESSAGE_28_ID.VALUE=28
DRIVER.CAN.VAR.CAN_4_MESSAGE_63_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_55_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_47_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_39_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_41_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_33_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_25_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_17_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_PORT_RX_DIN.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_3_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_3_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_41_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_33_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_25_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_17_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_7_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_59_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_20_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_12_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_9_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_11_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_6_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_11_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_4_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_20_ID.VALUE=20
DRIVER.CAN.VAR.CAN_4_MESSAGE_12_ID.VALUE=12
DRIVER.CAN.VAR.CAN_3_MESSAGE_62_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_54_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_46_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_38_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_4_ID.VALUE=4
DRIVER.CAN.VAR.CAN_1_MESSAGE_63_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_55_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_47_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_39_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_21_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_13_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_8_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_PORT_RX_DIR.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_59_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_59_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_AUTO_RETRANSMISSION.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_PORT_TX_FUN.VALUE=1
DRIVER.CAN.VAR.CAN_1_MESSAGE_59_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_63_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_55_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_47_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_39_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_62_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_54_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_46_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_38_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_2_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_41_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_33_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_25_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_17_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_PORT_TX_DOUT.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_50_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_42_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_34_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_26_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_18_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_AUTO_BUS_ON_TR.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_63_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_55_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_47_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_39_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_61_ID.VALUE=61
DRIVER.CAN.VAR.CAN_2_MESSAGE_53_ID.VALUE=53
DRIVER.CAN.VAR.CAN_2_MESSAGE_45_ID.VALUE=45
DRIVER.CAN.VAR.CAN_2_MESSAGE_37_ID.VALUE=37
DRIVER.CAN.VAR.CAN_2_MESSAGE_29_ID.VALUE=29
DRIVER.CAN.VAR.CAN_1_MESSAGE_20_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_12_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_4_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_1_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_63_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_63_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_55_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_55_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_47_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_47_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_39_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_39_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_PORT_TX_PULL.VALUE=2
DRIVER.CAN.VAR.CAN_1_MESSAGE_41_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_41_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_33_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_33_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_25_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_25_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_17_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_17_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_10_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_62_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_54_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_46_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_38_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_2_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_21_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_13_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_8_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_NOMINAL_BIT_RATE.VALUE=500.000
DRIVER.CAN.VAR.CAN_4_MESSAGE_21_ID.VALUE=21
DRIVER.CAN.VAR.CAN_4_MESSAGE_13_ID.VALUE=13
DRIVER.CAN.VAR.CAN_3_MESSAGE_5_ID.VALUE=5
DRIVER.CAN.VAR.CAN_2_MESSAGE_41_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_33_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_25_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_17_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_8_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_3_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_BRPE_FREQ.VALUE=7.500
DRIVER.CAN.VAR.CAN_2_MESSAGE_59_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_21_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_21_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_13_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_13_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_8_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_8_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_PORT_RX_DIN.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_40_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_32_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_24_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_16_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_4_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_PROP_SEG.VALUE=6
DRIVER.CAN.VAR.CAN_3_MESSAGE_8_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_58_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_31_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_23_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_15_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.CAN.VAR.CAN_1_MESSAGE_10_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_1_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_41_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_33_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_25_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_17_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_5_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_PORT_TX_PDR.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_62_ID.VALUE=62
DRIVER.CAN.VAR.CAN_2_MESSAGE_59_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_54_ID.VALUE=54
DRIVER.CAN.VAR.CAN_2_MESSAGE_46_ID.VALUE=46
DRIVER.CAN.VAR.CAN_2_MESSAGE_38_ID.VALUE=38
DRIVER.CAN.VAR.CAN_1_MESSAGE_11_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_64_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_56_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_48_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_NOMINAL_BIT_TIME.VALUE=15
DRIVER.CAN.VAR.CAN_1_MESSAGE_50_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_42_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_34_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_26_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_18_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_4_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_4_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_PORT_RX_DIR.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_64_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_56_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_48_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_1_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_1_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_59_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_58_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_61_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_59_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_53_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_45_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_37_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_29_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_TQ.VALUE=133.333
DRIVER.CAN.VAR.CAN_4_MESSAGE_30_ID.VALUE=30
DRIVER.CAN.VAR.CAN_4_MESSAGE_22_ID.VALUE=22
DRIVER.CAN.VAR.CAN_4_MESSAGE_14_ID.VALUE=14
DRIVER.CAN.VAR.CAN_4_MESSAGE_2_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_63_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_55_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_47_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_39_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_11_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_6_ID.VALUE=6
DRIVER.CAN.VAR.CAN_2_MESSAGE_30_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_22_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_14_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_9_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_59_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_64_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_56_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_48_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_62_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_54_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_46_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_38_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_61_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_53_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_45_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_37_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_29_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_3_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_50_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_42_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_34_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_26_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_18_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_51_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_43_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_35_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_27_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_19_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_63_ID.VALUE=63
DRIVER.CAN.VAR.CAN_2_MESSAGE_55_ID.VALUE=55
DRIVER.CAN.VAR.CAN_2_MESSAGE_47_ID.VALUE=47
DRIVER.CAN.VAR.CAN_2_MESSAGE_39_ID.VALUE=39
DRIVER.CAN.VAR.CAN_1_MESSAGE_21_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_13_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_5_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_10_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_2_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_64_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_64_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_56_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_56_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_48_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_48_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_64_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_56_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_48_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_50_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_50_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_42_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_42_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_34_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_34_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_26_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_26_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_18_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_18_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_51_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_43_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_35_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_31_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_27_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_23_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_19_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_15_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_41_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_33_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_30_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_25_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_22_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_17_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_14_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_9_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_TQ.VALUE=133.333
DRIVER.CAN.VAR.CAN_1_MESSAGE_7_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_BRPE.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_31_ID.VALUE=31
DRIVER.CAN.VAR.CAN_4_MESSAGE_23_ID.VALUE=23
DRIVER.CAN.VAR.CAN_4_MESSAGE_15_ID.VALUE=15
DRIVER.CAN.VAR.CAN_3_MESSAGE_7_ID.VALUE=7
DRIVER.CAN.VAR.CAN_2_MESSAGE_4_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_BASE.VALUE=0xFFF7E000
DRIVER.CAN.VAR.CAN_4_MESSAGE_59_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_30_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_30_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_22_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_22_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_14_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_14_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_9_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_9_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_61_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_53_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_45_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_37_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_29_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_50_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_42_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_34_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_26_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_18_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_5_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_10_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_1_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_PORT_TX_PULDIS.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_64_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_56_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_48_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_20_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_12_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_2_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_64_ID.VALUE=64
DRIVER.CAN.VAR.CAN_2_MESSAGE_62_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_56_ID.VALUE=56
DRIVER.CAN.VAR.CAN_2_MESSAGE_54_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_48_ID.VALUE=48
DRIVER.CAN.VAR.CAN_2_MESSAGE_46_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_38_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_PORT_TX_DOUT.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_57_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_49_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_51_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_43_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_35_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_27_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_19_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_PORT_RX_FUN.VALUE=1
DRIVER.CAN.VAR.CAN_4_MESSAGE_5_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_5_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_64_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_56_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_48_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_10_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_10_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_2_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_2_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_58_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_8_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_7_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_21_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_20_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_13_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_12_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_TQ.VALUE=133.333
DRIVER.CAN.VAR.CAN_1_MESSAGE_60_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_52_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_44_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_36_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_28_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_5_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_4_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_62_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_54_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_46_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_40_ID.VALUE=40
DRIVER.CAN.VAR.CAN_4_MESSAGE_38_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_32_ID.VALUE=32
DRIVER.CAN.VAR.CAN_4_MESSAGE_24_ID.VALUE=24
DRIVER.CAN.VAR.CAN_4_MESSAGE_16_ID.VALUE=16
DRIVER.CAN.VAR.CAN_3_MESSAGE_64_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_56_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_48_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_8_ID.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_40_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_32_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_24_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_16_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_10_ID.VALUE=10
DRIVER.CAN.VAR.CAN_2_MESSAGE_31_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_23_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_15_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_61_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_53_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_45_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_37_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_29_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_63_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_57_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_55_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_49_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_47_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_39_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_30_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_22_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_14_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_9_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_3_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_51_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_43_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_41_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_35_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_33_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_27_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_25_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_19_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_17_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_60_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_52_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_44_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_36_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_28_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_7_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_40_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_32_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_24_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_16_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_PORT_TX_PSL.VALUE=1
DRIVER.CAN.VAR.CAN_2_MESSAGE_57_ID.VALUE=57
DRIVER.CAN.VAR.CAN_2_MESSAGE_49_ID.VALUE=49
DRIVER.CAN.VAR.CAN_1_MESSAGE_30_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_22_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_14_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_4_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_6_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_11_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_3_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_SAMPLE_POINT_REFERENCE.VALUE=75
DRIVER.CAN.VAR.CAN_1_PROPAGATION_DELAY.VALUE=700
DRIVER.CAN.VAR.CAN_4_MESSAGE_64_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_57_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_57_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_56_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_49_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_49_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_48_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_51_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_51_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_50_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_43_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_43_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_42_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_35_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_35_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_34_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_27_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_27_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_26_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_19_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_19_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_18_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_3_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_TQ.VALUE=133.333
DRIVER.CAN.VAR.CAN_3_MESSAGE_1_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_31_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_23_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_15_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_PORT_RX_PDR.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_41_ID.VALUE=41
DRIVER.CAN.VAR.CAN_4_MESSAGE_33_ID.VALUE=33
DRIVER.CAN.VAR.CAN_4_MESSAGE_25_ID.VALUE=25
DRIVER.CAN.VAR.CAN_4_MESSAGE_17_ID.VALUE=17
DRIVER.CAN.VAR.CAN_3_MESSAGE_9_ID.VALUE=9
DRIVER.CAN.VAR.CAN_2_MESSAGE_10_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_10_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_5_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_1_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_11_ID.VALUE=11
DRIVER.CAN.VAR.CAN_1_NOMINAL_BIT_TIME.VALUE=15
DRIVER.CAN.VAR.CAN_3_MESSAGE_61_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_53_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_45_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_37_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_29_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_31_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_31_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_23_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_23_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_15_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_15_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_PORT_RX_FUN.VALUE=1
DRIVER.CAN.VAR.CAN_4_MESSAGE_40_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_32_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_24_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_16_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_6_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_57_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_49_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_11_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_8_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_ENABLE.VALUE=1
DRIVER.CAN.VAR.CAN_2_MESSAGE_59_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_10_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_3_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_PIN_MODE.VALUE=1
DRIVER.CAN.VAR.CAN_4_MESSAGE_10_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_1_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_58_ID.VALUE=58
DRIVER.CAN.VAR.CAN_4_MESSAGE_58_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_SAMPLE_POINT_REFERENCE.VALUE=75
DRIVER.CAN.VAR.CAN_1_MESSAGE_60_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_52_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_44_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_36_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_28_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_6_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_6_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_11_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_11_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_50_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_42_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_34_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_26_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_18_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_3_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_3_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_51_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_43_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_35_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_27_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_19_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_61_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_53_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_45_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_37_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_29_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_PORT_RX_PULDIS.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_62_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_54_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_46_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_38_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_21_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_13_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_50_ID.VALUE=50
DRIVER.CAN.VAR.CAN_4_MESSAGE_42_ID.VALUE=42
DRIVER.CAN.VAR.CAN_4_MESSAGE_34_ID.VALUE=34
DRIVER.CAN.VAR.CAN_4_MESSAGE_26_ID.VALUE=26
DRIVER.CAN.VAR.CAN_4_MESSAGE_18_ID.VALUE=18
DRIVER.CAN.VAR.CAN_3_MESSAGE_57_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_49_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_59_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_20_ID.VALUE=20
DRIVER.CAN.VAR.CAN_1_MESSAGE_12_ID.VALUE=12
DRIVER.CAN.VAR.CAN_2_MESSAGE_40_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_32_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_24_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_16_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_61_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_53_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_45_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_37_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_29_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_AUTO_BUS_ON.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_31_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_23_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_15_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_58_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_63_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_55_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_47_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_39_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_1_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_2_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_60_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_52_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_44_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_36_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_28_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_61_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_59_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_53_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_45_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_37_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_29_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_59_ID.VALUE=59
DRIVER.CAN.VAR.CAN_1_PORT_RX_PDR.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_61_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_53_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_45_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_37_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_31_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_29_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_23_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_15_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_7_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_20_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_12_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_SAMPLE_POINT_REFERENCE.VALUE=75
DRIVER.CAN.VAR.CAN_1_MESSAGE_4_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_58_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_58_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_50_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_42_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_34_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_26_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_18_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_60_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_60_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_52_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_52_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_44_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_44_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_36_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_36_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_28_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_28_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_8_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_SHIFT.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_64_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_56_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_50_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_48_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_42_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_40_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_34_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_32_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_30_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_26_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_24_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_22_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_18_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_16_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_14_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_9_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_BRPE.VALUE=0
DRIVER.CAN.VAR.CAN_1_MASK.VALUE=0x1FFFFFFF
DRIVER.CAN.VAR.CAN_4_MESSAGE_51_ID.VALUE=51
DRIVER.CAN.VAR.CAN_4_MESSAGE_43_ID.VALUE=43
DRIVER.CAN.VAR.CAN_4_MESSAGE_35_ID.VALUE=35
DRIVER.CAN.VAR.CAN_4_MESSAGE_27_ID.VALUE=27
DRIVER.CAN.VAR.CAN_4_MESSAGE_19_ID.VALUE=19
DRIVER.CAN.VAR.CAN_3_MESSAGE_61_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_53_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_45_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_37_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_29_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_11_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_6_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_21_ID.VALUE=21
DRIVER.CAN.VAR.CAN_1_MESSAGE_13_ID.VALUE=13
DRIVER.CAN.VAR.CAN_1_MESSAGE_9_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_BASE.VALUE=0xFFF7E200
DRIVER.CAN.VAR.CAN_2_MESSAGE_40_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_40_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_32_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_32_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_31_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_24_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_24_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_23_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_16_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_16_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_15_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_8_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_51_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_43_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_35_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_27_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_19_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_7_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_57_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_50_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_49_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_42_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_34_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_26_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_20_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_18_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_12_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_21_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_13_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_4_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_2_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_31_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_23_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_15_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_6_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_59_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_SAMPLE_POINT_REFERENCE.VALUE=75
DRIVER.CAN.VAR.CAN_1_MESSAGE_61_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_53_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_45_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_37_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_29_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_BRPE_FREQ.VALUE=7.500
DRIVER.CAN.VAR.CAN_1_BRP_FREQ.VALUE=7.500
DRIVER.CAN.VAR.CAN_4_PORT_TX_DIN.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_50_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_42_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_34_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_26_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_18_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_7_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_7_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_20_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_20_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_12_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_12_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_8_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_20_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_12_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_4_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_4_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_20_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_12_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_9_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_30_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_22_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_14_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_4_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_2_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_6_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_PORT_RX_PSL.VALUE=1
DRIVER.CAN.VAR.CAN_4_MESSAGE_60_ID.VALUE=60
DRIVER.CAN.VAR.CAN_4_MESSAGE_52_ID.VALUE=52
DRIVER.CAN.VAR.CAN_4_MESSAGE_44_ID.VALUE=44
DRIVER.CAN.VAR.CAN_4_MESSAGE_36_ID.VALUE=36
DRIVER.CAN.VAR.CAN_4_MESSAGE_31_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_28_ID.VALUE=28
DRIVER.CAN.VAR.CAN_4_MESSAGE_23_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_15_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_58_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_3_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_30_ID.VALUE=30
DRIVER.CAN.VAR.CAN_1_MESSAGE_22_ID.VALUE=22
DRIVER.CAN.VAR.CAN_1_MESSAGE_14_ID.VALUE=14
DRIVER.CAN.VAR.CAN_2_MESSAGE_41_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_33_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_25_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_17_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_PORT_TX_DIR.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_8_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_31_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_23_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_15_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_5_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_59_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_50_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_42_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_34_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_26_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_18_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_4_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_63_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_61_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_55_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_53_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_47_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_45_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_39_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_37_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_29_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_62_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_54_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_46_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_38_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_1_ID.VALUE=1
DRIVER.CAN.VAR.CAN_1_MESSAGE_40_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_32_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_24_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_16_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_8_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_21_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_13_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_5_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_59_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_59_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_20_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_12_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_5_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_61_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_61_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_53_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_53_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_45_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_45_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_37_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_37_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_29_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_29_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_10_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_2_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_BAUDRATE.VALUE=500
DRIVER.CAN.VAR.CAN_2_MESSAGE_41_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_41_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_33_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_33_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_25_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_25_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_17_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_17_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_63_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_55_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_47_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_39_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_61_ID.VALUE=61
DRIVER.CAN.VAR.CAN_4_MESSAGE_53_ID.VALUE=53
DRIVER.CAN.VAR.CAN_4_MESSAGE_45_ID.VALUE=45
DRIVER.CAN.VAR.CAN_4_MESSAGE_37_ID.VALUE=37
DRIVER.CAN.VAR.CAN_4_MESSAGE_29_ID.VALUE=29
DRIVER.CAN.VAR.CAN_2_MESSAGE_20_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_12_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_7_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_58_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_31_ID.VALUE=31
DRIVER.CAN.VAR.CAN_1_MESSAGE_23_ID.VALUE=23
DRIVER.CAN.VAR.CAN_1_MESSAGE_15_ID.VALUE=15
DRIVER.CAN.VAR.CAN_3_MESSAGE_1_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_31_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_23_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_15_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_5_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_41_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_41_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_33_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_33_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_25_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_25_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_17_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_17_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_PORT_TX_DIN.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_8_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_6_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_6_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_21_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_13_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_11_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_11_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_5_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_3_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_3_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_3_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_2_ID.VALUE=2
DRIVER.CAN.VAR.CAN_3_MESSAGE_58_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_PORT_RX_PSL.VALUE=1
DRIVER.CAN.VAR.CAN_4_AUTO_BUS_ON_TIME.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_62_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_54_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_46_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_38_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_8_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_8_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_5_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_AUTO_RETRANSMISSION.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_21_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_21_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_20_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_13_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_13_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_12_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_SAMPLE_POINT.VALUE=73.333
DRIVER.CAN.VAR.CAN_1_PORT_TX_DIR.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_5_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_5_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_2_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_62_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_54_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_46_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_38_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_PIN_MODE.VALUE=1
DRIVER.CAN.VAR.CAN_3_MESSAGE_1_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.CAN.VAR.CAN_3_PHASE_SEG.VALUE=4
DRIVER.CAN.VAR.CAN_1_MESSAGE_63_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_55_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_47_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_40_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_39_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_32_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_24_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_16_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_62_ID.VALUE=62
DRIVER.CAN.VAR.CAN_4_MESSAGE_54_ID.VALUE=54
DRIVER.CAN.VAR.CAN_4_MESSAGE_46_ID.VALUE=46
DRIVER.CAN.VAR.CAN_4_MESSAGE_38_ID.VALUE=38
DRIVER.CAN.VAR.CAN_3_MESSAGE_59_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_60_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_52_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_44_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_36_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_28_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_40_ID.VALUE=40
DRIVER.CAN.VAR.CAN_1_MESSAGE_32_ID.VALUE=32
DRIVER.CAN.VAR.CAN_1_MESSAGE_24_ID.VALUE=24
DRIVER.CAN.VAR.CAN_1_MESSAGE_16_ID.VALUE=16
DRIVER.CAN.VAR.CAN_2_MESSAGE_50_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_42_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_34_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_26_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_18_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_1_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_1_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_2_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_62_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_54_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_46_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_38_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_64_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_56_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_48_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_59_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_62_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_54_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_46_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_40_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_38_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_32_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_24_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_16_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_63_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_60_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_55_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_52_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_47_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_44_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_39_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_36_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_28_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_3_ID.VALUE=3
DRIVER.CAN.VAR.CAN_3_PORT_RX_DOUT.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_8_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_41_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_33_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_30_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_25_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_22_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_17_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_14_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_9_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_30_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_22_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_14_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_6_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_20_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_12_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_2_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_PORT_RX_PULL.VALUE=2
DRIVER.CAN.VAR.CAN_1_MESSAGE_62_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_62_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_54_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_54_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_46_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_46_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_38_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_38_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_31_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_23_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_15_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_7_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_BRPE.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_51_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_50_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_43_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_42_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_35_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_34_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_27_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_26_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_19_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_18_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_10_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_5_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MASK.VALUE=0x1FFFFFFF
DRIVER.CAN.VAR.CAN_4_MESSAGE_63_ID.VALUE=63
DRIVER.CAN.VAR.CAN_4_MESSAGE_55_ID.VALUE=55
DRIVER.CAN.VAR.CAN_4_MESSAGE_47_ID.VALUE=47
DRIVER.CAN.VAR.CAN_4_MESSAGE_39_ID.VALUE=39
DRIVER.CAN.VAR.CAN_4_MESSAGE_5_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_30_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_22_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_14_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_21_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_13_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_8_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_41_ID.VALUE=41
DRIVER.CAN.VAR.CAN_1_MESSAGE_33_ID.VALUE=33
DRIVER.CAN.VAR.CAN_1_MESSAGE_25_ID.VALUE=25
DRIVER.CAN.VAR.CAN_1_MESSAGE_17_ID.VALUE=17
DRIVER.CAN.VAR.CAN_1_MESSAGE_2_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_10_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_2_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_2_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_50_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_50_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_42_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_42_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_34_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_34_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_26_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_26_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_18_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_18_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_60_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_52_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_44_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_36_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_28_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_9_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_30_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_22_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_14_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_60_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_59_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_52_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_44_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_36_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_28_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_30_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_22_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_14_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_6_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_4_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_4_ID.VALUE=4
DRIVER.CAN.VAR.CAN_1_MESSAGE_1_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_1_ID.VALUE=1
DRIVER.CAN.VAR.CAN_1_MESSAGE_63_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_55_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_47_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_39_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_PORT_TX_FUN.VALUE=1
DRIVER.CAN.VAR.CAN_4_MESSAGE_9_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_9_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_30_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_30_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_22_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_22_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_14_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_14_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_6_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_6_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_10_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_PORT_TX_PULDIS.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_61_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_53_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_45_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_37_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_31_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_29_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_23_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_15_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_2_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_7_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_64_ID.VALUE=64
DRIVER.CAN.VAR.CAN_4_MESSAGE_56_ID.VALUE=56
DRIVER.CAN.VAR.CAN_4_MESSAGE_48_ID.VALUE=48
DRIVER.CAN.VAR.CAN_1_MESSAGE_50_ID.VALUE=50
DRIVER.CAN.VAR.CAN_1_MESSAGE_42_ID.VALUE=42
DRIVER.CAN.VAR.CAN_1_MESSAGE_34_ID.VALUE=34
DRIVER.CAN.VAR.CAN_1_MESSAGE_26_ID.VALUE=26
DRIVER.CAN.VAR.CAN_1_MESSAGE_18_ID.VALUE=18
DRIVER.CAN.VAR.CAN_4_BRP_FREQ.VALUE=7.500
DRIVER.CAN.VAR.CAN_2_MESSAGE_51_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_43_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_35_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_27_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_19_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_PORT_TX_PULL.VALUE=2
DRIVER.CAN.VAR.CAN_4_MESSAGE_10_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_10_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_2_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_2_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_BRP.VALUE=9
DRIVER.CAN.VAR.CAN_4_MESSAGE_31_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_23_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_15_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_7_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_PROP_SEG.VALUE=6
DRIVER.CAN.VAR.CAN_2_MESSAGE_21_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_13_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_10_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_8_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_5_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_63_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_55_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_47_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_39_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_64_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_56_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_48_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_5_ID.VALUE=5
DRIVER.CAN.VAR.CAN_3_MESSAGE_10_ID.VALUE=10
DRIVER.CAN.VAR.CAN_2_MESSAGE_57_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_49_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_50_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_42_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_34_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_26_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_18_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_2_ID.VALUE=2
DRIVER.CAN.VAR.CAN_1_AUTO_BUS_ON_TR.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_31_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_23_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_15_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_7_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_PORT_RX_DIN.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_63_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_63_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_55_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_55_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_47_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_47_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_39_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_39_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_11_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_64_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_56_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_48_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_3_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_51_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_43_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_35_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_27_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_19_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_58_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_PORT_TX_PDR.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_57_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_57_ID.VALUE=57
DRIVER.CAN.VAR.CAN_4_MESSAGE_49_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_49_ID.VALUE=49
DRIVER.CAN.VAR.CAN_2_MESSAGE_30_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_22_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_14_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_9_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_51_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_51_ID.VALUE=51
DRIVER.CAN.VAR.CAN_1_MESSAGE_43_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_43_ID.VALUE=43
DRIVER.CAN.VAR.CAN_1_MESSAGE_35_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_35_ID.VALUE=35
DRIVER.CAN.VAR.CAN_1_MESSAGE_27_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_27_ID.VALUE=27
DRIVER.CAN.VAR.CAN_1_MESSAGE_19_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_19_ID.VALUE=19
DRIVER.CAN.VAR.CAN_4_MESSAGE_11_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_3_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_AUTO_BUS_ON_TIME.VALUE=0
DRIVER.CAN.VAR.CAN_3_PORT_RX_DIR.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_51_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_51_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_43_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_43_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_35_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_35_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_27_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_27_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_19_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_19_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_PORT_TX_FUN.VALUE=1
DRIVER.CAN.VAR.CAN_1_MESSAGE_58_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_1_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_31_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_23_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_15_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_60_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_52_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_44_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_36_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_28_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_1_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_7_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_6_ID.VALUE=6
DRIVER.CAN.VAR.CAN_4_MESSAGE_5_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_51_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_43_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_35_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_27_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_19_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_11_ID.VALUE=11
DRIVER.CAN.VAR.CAN_3_MESSAGE_10_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_7_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_3_ID.VALUE=3
DRIVER.CAN.VAR.CAN_1_MESSAGE_2_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_64_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_56_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_48_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_31_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_31_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_23_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_23_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_15_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_15_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_7_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_7_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_11_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_9_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_41_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_33_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_30_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_25_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_22_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_17_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_14_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_3_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_64_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_56_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_48_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_9_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_6_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_58_ID.VALUE=58
DRIVER.CAN.VAR.CAN_2_MESSAGE_21_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_13_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_4_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_60_ID.VALUE=60
DRIVER.CAN.VAR.CAN_1_MESSAGE_52_ID.VALUE=52
DRIVER.CAN.VAR.CAN_1_MESSAGE_44_ID.VALUE=44
DRIVER.CAN.VAR.CAN_1_MESSAGE_36_ID.VALUE=36
DRIVER.CAN.VAR.CAN_1_MESSAGE_28_ID.VALUE=28
DRIVER.CAN.VAR.CAN_2_MESSAGE_60_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_52_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_44_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_36_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_28_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_11_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_11_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_3_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_3_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_58_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_BRP.VALUE=9
DRIVER.CAN.VAR.CAN_3_MESSAGE_57_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_49_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_PORT_RX_PULDIS.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_64_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_62_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_56_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_54_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_48_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_46_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_38_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_57_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_49_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_21_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_13_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_7_ID.VALUE=7
DRIVER.CAN.VAR.CAN_3_MESSAGE_20_ID.VALUE=20
DRIVER.CAN.VAR.CAN_3_MESSAGE_12_ID.VALUE=12
DRIVER.CAN.VAR.CAN_3_MESSAGE_1_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_PORT_TX_PDR.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_51_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_43_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_35_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_27_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_19_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_4_ID.VALUE=4
DRIVER.CAN.VAR.CAN_3_MESSAGE_40_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_32_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_24_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_16_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_8_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_NOMINAL_AUTO_BUS_ON_TIME.VALUE=0.000
DRIVER.CAN.VAR.CAN_2_SHIFT.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_64_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_64_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_63_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_56_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_56_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_55_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_48_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_48_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_47_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_39_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_57_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_49_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_5_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_BRPE.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_10_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MASK.VALUE=0x1FFFFFFF
DRIVER.CAN.VAR.CAN_2_MESSAGE_60_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_60_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_52_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_52_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_44_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_44_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_36_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_36_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_28_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_28_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_51_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_43_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_35_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_27_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_19_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_2_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_59_ID.VALUE=59
DRIVER.CAN.VAR.CAN_2_PORT_TX_DOUT.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_31_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_23_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_15_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_61_ID.VALUE=61
DRIVER.CAN.VAR.CAN_1_MESSAGE_53_ID.VALUE=53
DRIVER.CAN.VAR.CAN_1_MESSAGE_45_ID.VALUE=45
DRIVER.CAN.VAR.CAN_1_MESSAGE_37_ID.VALUE=37
DRIVER.CAN.VAR.CAN_1_MESSAGE_29_ID.VALUE=29
DRIVER.CAN.VAR.CAN_4_MESSAGE_20_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_12_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_4_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_58_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_60_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_60_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_52_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_52_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_44_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_44_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_36_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_36_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_28_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_28_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_PORT_TX_PULL.VALUE=2
DRIVER.CAN.VAR.CAN_4_MESSAGE_61_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_61_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_53_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_53_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_45_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_45_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_37_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_37_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_29_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_29_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_40_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_32_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_24_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_16_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_21_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_13_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_8_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_31_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_31_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_23_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_23_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_15_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_15_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_8_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_8_ID.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_6_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_21_ID.VALUE=21
DRIVER.CAN.VAR.CAN_3_MESSAGE_13_ID.VALUE=13
DRIVER.CAN.VAR.CAN_3_MESSAGE_11_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_64_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_56_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_48_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_5_ID.VALUE=5
DRIVER.CAN.VAR.CAN_1_MESSAGE_3_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_57_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_49_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_40_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_40_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_32_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_32_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_24_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_24_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_16_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_16_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_63_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_55_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_47_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_39_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_8_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_8_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_20_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_12_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_2_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_40_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_32_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_24_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_16_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_4_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_58_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_8_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_PORT_TX_PSL.VALUE=1
DRIVER.CAN.VAR.CAN_3_MESSAGE_64_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_56_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_48_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_62_ID.VALUE=62
DRIVER.CAN.VAR.CAN_1_MESSAGE_54_ID.VALUE=54
DRIVER.CAN.VAR.CAN_1_MESSAGE_46_ID.VALUE=46
DRIVER.CAN.VAR.CAN_1_MESSAGE_38_ID.VALUE=38
DRIVER.CAN.VAR.CAN_2_MESSAGE_61_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_53_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_45_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_37_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_29_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_58_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_20_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_20_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_12_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_12_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_4_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_4_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_BRP.VALUE=9
DRIVER.CAN.VAR.CAN_1_MESSAGE_60_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_52_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_44_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_36_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_28_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_30_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_22_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_14_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_64_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_56_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_48_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_6_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_IDENTIFIER_MODE.VALUE=0x40000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_11_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_6_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_57_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_49_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_PHASE_SEG.VALUE=4
DRIVER.CAN.VAR.CAN_4_MESSAGE_58_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_9_ID.VALUE=9
DRIVER.CAN.VAR.CAN_3_MESSAGE_30_ID.VALUE=30
DRIVER.CAN.VAR.CAN_3_MESSAGE_22_ID.VALUE=22
DRIVER.CAN.VAR.CAN_3_MESSAGE_14_ID.VALUE=14
DRIVER.CAN.VAR.CAN_2_MESSAGE_50_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_42_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_34_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_26_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_18_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_9_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_60_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_52_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_44_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_36_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_28_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_6_ID.VALUE=6
DRIVER.CAN.VAR.CAN_4_BRPE_FREQ.VALUE=7.500
DRIVER.CAN.VAR.CAN_3_MESSAGE_41_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_33_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_25_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_17_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_AUTO_BUS_ON_TIME.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_9_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_PORT_RX_FUN.VALUE=1
DRIVER.CAN.VAR.CAN_3_MESSAGE_63_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_55_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_47_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_39_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_57_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_57_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_49_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_49_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_50_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_42_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_34_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_26_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_20_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_18_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_12_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_4_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_61_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_53_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_51_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_45_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_43_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_37_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_35_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_29_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_27_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_19_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_20_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_12_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_50_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_42_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_34_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_26_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_18_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_6_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_40_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_32_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_24_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_16_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_63_ID.VALUE=63
DRIVER.CAN.VAR.CAN_1_MESSAGE_55_ID.VALUE=55
DRIVER.CAN.VAR.CAN_1_MESSAGE_47_ID.VALUE=47
DRIVER.CAN.VAR.CAN_1_MESSAGE_39_ID.VALUE=39
DRIVER.CAN.VAR.CAN_1_MESSAGE_20_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_12_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_21_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_13_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_5_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_61_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_61_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_60_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_53_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_53_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_52_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_45_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_45_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_44_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_37_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_37_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_36_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_29_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_29_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_28_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_2_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_41_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_33_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_25_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_17_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_1_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_9_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_7_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_3_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_31_ID.VALUE=31
DRIVER.CAN.VAR.CAN_3_MESSAGE_23_ID.VALUE=23
DRIVER.CAN.VAR.CAN_3_MESSAGE_20_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_20_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_15_ID.VALUE=15
DRIVER.CAN.VAR.CAN_3_MESSAGE_12_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_12_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_PORT_TX_PSL.VALUE=1
DRIVER.CAN.VAR.CAN_1_MESSAGE_7_ID.VALUE=7
DRIVER.CAN.VAR.CAN_1_MESSAGE_4_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_58_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_63_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_55_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_47_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_39_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_41_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_41_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_33_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_33_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_25_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_25_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_17_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_17_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_41_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_33_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_25_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_17_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_9_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_9_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_21_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_13_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_5_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_63_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_55_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_47_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_39_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_20_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_12_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_7_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_57_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_49_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_PORT_RX_PDR.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_64_ID.VALUE=64
DRIVER.CAN.VAR.CAN_1_MESSAGE_56_ID.VALUE=56
DRIVER.CAN.VAR.CAN_1_MESSAGE_48_ID.VALUE=48
DRIVER.CAN.VAR.CAN_2_MESSAGE_62_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_54_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_46_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_38_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_21_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_21_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_13_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_13_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_BRP.VALUE=9
DRIVER.CAN.VAR.CAN_3_MESSAGE_60_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_52_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_44_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_36_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_28_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_5_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_5_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.CAN.VAR.CAN_3_MESSAGE_63_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_58_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_55_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_47_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_41_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_39_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_33_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_25_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_17_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_58_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_9_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_59_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_40_ID.VALUE=40
DRIVER.CAN.VAR.CAN_3_MESSAGE_32_ID.VALUE=32
DRIVER.CAN.VAR.CAN_3_MESSAGE_24_ID.VALUE=24
DRIVER.CAN.VAR.CAN_3_MESSAGE_16_ID.VALUE=16
DRIVER.CAN.VAR.CAN_1_MESSAGE_61_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_53_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_45_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_37_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_29_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_8_ID.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_50_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_42_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_34_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_26_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_18_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_NOMINAL_AUTO_BUS_ON_TIME.VALUE=0.000
DRIVER.CAN.VAR.CAN_2_MESSAGE_41_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_33_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_25_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_17_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_58_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_58_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_AUTO_RETRANSMISSION.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_11_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MASK.VALUE=0x1FFFFFFF
DRIVER.CAN.VAR.CAN_3_MESSAGE_3_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_62_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_61_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_54_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_53_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_46_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_45_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_38_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_37_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_29_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_63_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_55_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_47_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_41_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_39_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_33_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_25_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_17_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_57_ID.VALUE=57
DRIVER.CAN.VAR.CAN_1_MESSAGE_49_ID.VALUE=49
DRIVER.CAN.VAR.CAN_4_MESSAGE_30_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_22_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_14_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_6_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_60_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_52_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_44_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_36_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_28_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_62_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_62_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_54_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_54_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_46_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_46_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_38_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_38_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_AUTO_BUS_ON.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_30_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_22_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_14_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_62_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_54_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_46_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_38_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_50_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_42_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_40_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_34_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_32_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_26_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_24_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_18_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_16_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_62_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_54_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_46_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_40_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_38_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_32_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_24_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_16_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_8_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_63_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_55_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_47_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_39_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_8_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_41_ID.VALUE=41
DRIVER.CAN.VAR.CAN_3_MESSAGE_33_ID.VALUE=33
DRIVER.CAN.VAR.CAN_3_MESSAGE_25_ID.VALUE=25
DRIVER.CAN.VAR.CAN_3_MESSAGE_21_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_17_ID.VALUE=17
DRIVER.CAN.VAR.CAN_3_MESSAGE_13_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_41_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_33_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_25_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_17_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_9_ID.VALUE=9
DRIVER.CAN.VAR.CAN_1_MESSAGE_5_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_59_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_SJW.VALUE=4
DRIVER.CAN.VAR.CAN_3_MESSAGE_50_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_50_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_42_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_42_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_41_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_34_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_34_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_33_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_26_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_26_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_25_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_18_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_18_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_17_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_7_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_59_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_30_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_22_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_14_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_41_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_33_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_25_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_17_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_6_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_40_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_32_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_24_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_16_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_BAUDRATE.VALUE=500
DRIVER.CAN.VAR.CAN_1_MESSAGE_61_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_53_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_45_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_37_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_29_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_9_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_IDENTIFIER_MODE.VALUE=0x40000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_8_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_41_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_33_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_25_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_17_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_1_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_58_ID.VALUE=58
DRIVER.CAN.VAR.CAN_1_MESSAGE_5_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_RAMBASE.VALUE=0xFF180000
DRIVER.CAN.VAR.CAN_2_MESSAGE_63_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_55_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_47_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_39_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_AUTO_BUS_ON_TIME.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_30_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_30_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_22_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_22_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_14_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_14_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_6_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_6_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_30_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_22_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_14_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_7_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_PORT_TX_PULDIS.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_5_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_4_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_10_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_20_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_12_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_7_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_59_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_2_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_1_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_50_ID.VALUE=50
DRIVER.CAN.VAR.CAN_3_MESSAGE_42_ID.VALUE=42
DRIVER.CAN.VAR.CAN_3_MESSAGE_34_ID.VALUE=34
DRIVER.CAN.VAR.CAN_3_MESSAGE_26_ID.VALUE=26
DRIVER.CAN.VAR.CAN_3_MESSAGE_18_ID.VALUE=18
DRIVER.CAN.VAR.CAN_2_MESSAGE_11_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_2_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_62_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_54_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_46_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_38_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_51_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_43_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_35_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_27_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_19_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_41_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_33_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_25_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_17_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_PORT_TX_DIN.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_7_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_59_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_59_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_11_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_60_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_52_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_44_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_36_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_28_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_21_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_13_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_59_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_5_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_PIN_MODE.VALUE=1
DRIVER.CAN.VAR.CAN_2_MESSAGE_63_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_55_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_47_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_39_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_30_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_22_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_14_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_11_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_PORT_RX_PSL.VALUE=1
DRIVER.CAN.VAR.CAN_2_MESSAGE_50_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_42_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_34_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_26_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_18_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_AUTO_BUS_ON_TR.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_59_ID.VALUE=59
DRIVER.CAN.VAR.CAN_4_MESSAGE_31_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_23_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_15_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_PROPAGATION_DELAY.VALUE=700
DRIVER.CAN.VAR.CAN_3_MESSAGE_7_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_7_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_SAMPLE_POINT.VALUE=73.333
DRIVER.CAN.VAR.CAN_3_PORT_TX_DIR.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_30_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_22_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_14_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_63_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_63_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_55_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_55_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_47_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_47_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_39_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_39_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_4_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_61_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_53_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_45_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_37_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_29_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_3_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_ENABLE.VALUE=1
DRIVER.CAN.VAR.CAN_3_MESSAGE_51_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_43_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_35_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_27_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_19_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_57_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_49_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_31_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_23_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_15_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_9_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_51_ID.VALUE=51
DRIVER.CAN.VAR.CAN_3_MESSAGE_43_ID.VALUE=43
DRIVER.CAN.VAR.CAN_3_MESSAGE_35_ID.VALUE=35
DRIVER.CAN.VAR.CAN_3_MESSAGE_30_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_27_ID.VALUE=27
DRIVER.CAN.VAR.CAN_3_MESSAGE_22_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_19_ID.VALUE=19
DRIVER.CAN.VAR.CAN_3_MESSAGE_14_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_6_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_SJW.VALUE=4
DRIVER.CAN.VAR.CAN_3_MESSAGE_51_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_51_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_43_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_43_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_35_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_35_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_27_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_27_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_19_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_19_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_11_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_4_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_31_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_23_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_21_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_15_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_13_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_7_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_5_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_4_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_58_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_PORT_RX_DOUT.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_10_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_2_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_62_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_54_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_46_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_38_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_64_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_56_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_48_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_31_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_31_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_30_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_23_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_23_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_22_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_15_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_15_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_14_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_PORT_RX_PULL.VALUE=1
DRIVER.CAN.VAR.CAN_3_MESSAGE_7_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_7_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_4_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_59_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_58_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_50_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_42_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_34_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_26_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_18_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_62_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_60_ID.VALUE=60
DRIVER.CAN.VAR.CAN_3_MESSAGE_54_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_52_ID.VALUE=52
DRIVER.CAN.VAR.CAN_3_MESSAGE_46_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_44_ID.VALUE=44
DRIVER.CAN.VAR.CAN_3_MESSAGE_38_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_36_ID.VALUE=36
DRIVER.CAN.VAR.CAN_3_MESSAGE_28_ID.VALUE=28
DRIVER.CAN.VAR.CAN_1_MESSAGE_63_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_55_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_47_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_39_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_60_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_52_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_44_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_36_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_28_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_NOMINAL_AUTO_BUS_ON_TIME.VALUE=0.000
DRIVER.CAN.VAR.CAN_1_SYNC.VALUE=1
DRIVER.CAN.VAR.CAN_4_MESSAGE_4_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_11_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_SHIFT.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_1_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_PORT_RX_PULDIS.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_60_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_52_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_44_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_36_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_28_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_64_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_62_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_56_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_54_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_48_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_46_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_38_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_51_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_43_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_40_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_35_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_32_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_27_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_24_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_19_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_16_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_7_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_1_ID.VALUE=1
DRIVER.CAN.VAR.CAN_4_MESSAGE_40_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_32_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_24_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_16_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_8_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_BRP_FREQ.VALUE=7.500
DRIVER.CAN.VAR.CAN_2_BRPE_FREQ.VALUE=7.500
DRIVER.CAN.VAR.CAN_1_MESSAGE_10_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_64_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_64_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_56_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_56_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_48_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_48_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_1_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_63_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_55_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_47_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_39_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_30_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_22_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_14_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_60_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_52_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_44_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_36_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_28_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_6_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_11_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_6_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_PROP_SEG.VALUE=6
DRIVER.CAN.VAR.CAN_1_MESSAGE_41_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_33_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_25_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_17_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_40_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_32_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_24_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_16_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_61_ID.VALUE=61
DRIVER.CAN.VAR.CAN_3_MESSAGE_53_ID.VALUE=53
DRIVER.CAN.VAR.CAN_3_MESSAGE_45_ID.VALUE=45
DRIVER.CAN.VAR.CAN_3_MESSAGE_37_ID.VALUE=37
DRIVER.CAN.VAR.CAN_3_MESSAGE_31_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_29_ID.VALUE=29
DRIVER.CAN.VAR.CAN_3_MESSAGE_23_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_15_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_4_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_10_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_7_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_SJW.VALUE=4
DRIVER.CAN.VAR.CAN_2_MESSAGE_1_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_11_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_60_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_60_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_52_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_52_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_44_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_44_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_36_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_36_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_28_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_28_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_1_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_40_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_32_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_24_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_16_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_62_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_54_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_50_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_46_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_42_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_38_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_34_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_26_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_18_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_8_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_57_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_49_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_10_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_11_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_1_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_10_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_3_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_2_ID.VALUE=2
DRIVER.CAN.VAR.CAN_2_MESSAGE_57_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_49_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_40_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_40_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_32_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_32_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_24_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_24_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_16_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_16_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_1_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_8_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_8_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_10_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_10_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_SAMPLE_POINT.VALUE=73.333
DRIVER.CAN.VAR.CAN_2_MESSAGE_51_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_43_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_35_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_27_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_21_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_19_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_13_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_8_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_1_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_59_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_62_ID.VALUE=62
DRIVER.CAN.VAR.CAN_3_MESSAGE_54_ID.VALUE=54
DRIVER.CAN.VAR.CAN_3_MESSAGE_46_ID.VALUE=46
DRIVER.CAN.VAR.CAN_3_MESSAGE_38_ID.VALUE=38
DRIVER.CAN.VAR.CAN_1_MESSAGE_64_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_59_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_56_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_48_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_61_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_53_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_45_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_37_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_29_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_PORT_TX_FUN.VALUE=1
DRIVER.CAN.VAR.CAN_2_MESSAGE_1_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_1_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_30_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_22_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_14_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_8_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_31_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_23_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_21_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_15_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_13_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_6_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_57_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_49_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_7_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_5_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_59_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_60_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_52_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_44_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_36_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_28_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_3_ID.VALUE=3
DRIVER.CAN.VAR.CAN_1_PORT_RX_DOUT.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_41_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_33_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_25_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_17_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_9_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_11_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_57_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_57_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_49_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_49_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_58_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_4_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_PHASE_SEG.VALUE=4
DRIVER.CAN.VAR.CAN_3_MESSAGE_61_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_53_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_45_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_37_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_29_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_60_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_52_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_44_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_36_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_28_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_1_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_63_ID.VALUE=63
DRIVER.CAN.VAR.CAN_3_MESSAGE_55_ID.VALUE=55
DRIVER.CAN.VAR.CAN_3_MESSAGE_47_ID.VALUE=47
DRIVER.CAN.VAR.CAN_3_MESSAGE_40_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_39_ID.VALUE=39
DRIVER.CAN.VAR.CAN_3_MESSAGE_32_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_24_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_16_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_61_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_53_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_45_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_37_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_29_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_8_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_SJW.VALUE=4
DRIVER.CAN.VAR.CAN_3_RAMBASE.VALUE=0xFF1A0000
DRIVER.CAN.VAR.CAN_2_MESSAGE_2_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_61_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_61_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_53_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_53_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_45_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_45_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_37_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_37_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_29_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_29_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_PORT_RX_DIN.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_64_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_56_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_48_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_41_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_33_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_25_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_17_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_3_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_9_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_59_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_50_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_42_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_34_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_26_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_18_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_11_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_61_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_53_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_45_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_37_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_29_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_20_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_12_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_PORT_TX_PDR.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_9_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_4_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_4_ID.VALUE=4
DRIVER.CAN.VAR.CAN_1_MESSAGE_31_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_23_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_15_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_58_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_41_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_41_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_33_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_33_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_25_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_25_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_17_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_17_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_9_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_9_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_PORT_RX_DIR.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_57_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_49_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_11_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_11_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_51_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_43_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_35_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_27_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_19_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_20_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_12_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_7_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_2_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_21_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_13_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_6_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_PORT_TX_DOUT.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_64_ID.VALUE=64
DRIVER.CAN.VAR.CAN_3_MESSAGE_56_ID.VALUE=56
DRIVER.CAN.VAR.CAN_3_MESSAGE_48_ID.VALUE=48
DRIVER.CAN.VAR.CAN_3_MESSAGE_31_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_23_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_15_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_57_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_49_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_3_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_NOMINAL_AUTO_BUS_ON_TIME.VALUE=0.000
DRIVER.CAN.VAR.CAN_3_MESSAGE_62_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_54_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_46_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_38_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_SYNC.VALUE=1
DRIVER.CAN.VAR.CAN_2_PORT_TX_PULL.VALUE=2
DRIVER.CAN.VAR.CAN_2_MESSAGE_2_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_2_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_1_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_64_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_63_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_58_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_56_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_55_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_48_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_47_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_39_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_61_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_53_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_45_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_37_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_29_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_10_ID.VALUE=10
DRIVER.CAN.VAR.CAN_2_MESSAGE_5_ID.VALUE=5
DRIVER.CAN.VAR.CAN_4_MESSAGE_50_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_42_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_34_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_26_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_18_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_20_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_12_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_58_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_58_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_57_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_49_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_64_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_56_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_48_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_20_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_12_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_63_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_62_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_55_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_54_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_47_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_46_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_39_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_38_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_4_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_50_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_42_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_34_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_26_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_18_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_57_ID.VALUE=57
DRIVER.CAN.VAR.CAN_3_MESSAGE_49_ID.VALUE=49
DRIVER.CAN.VAR.CAN_3_MESSAGE_41_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_33_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_25_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_17_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_9_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_3_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_62_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_62_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_54_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_54_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_46_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_46_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_38_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_38_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_62_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_54_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_46_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_38_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_50_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_42_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_41_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_34_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_33_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_26_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_25_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_18_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_17_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_NOMINAL_BIT_RATE.VALUE=500.000
DRIVER.CAN.VAR.CAN_3_MESSAGE_51_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_43_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_35_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_27_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_19_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_9_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_41_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_33_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_25_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_17_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_20_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_12_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_11_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_4_MESSAGE_21_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_13_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_5_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_58_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_11_ID.VALUE=11
DRIVER.CAN.VAR.CAN_2_MESSAGE_6_ID.VALUE=6
DRIVER.CAN.VAR.CAN_3_PROPAGATION_DELAY.VALUE=700
DRIVER.CAN.VAR.CAN_2_MESSAGE_59_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_50_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_50_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_42_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_42_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_34_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_34_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_26_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_26_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_18_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_18_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_57_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_49_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_AUTO_RETRANSMISSION.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_20_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_20_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_12_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_12_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_30_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_22_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_14_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_9_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_3_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_58_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_58_ID.VALUE=58
DRIVER.CAN.VAR.CAN_1_MESSAGE_60_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_58_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_52_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_44_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_36_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_28_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_63_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_55_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_47_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_39_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_2_MESSAGE_62_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_54_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_46_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_38_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_3_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_3_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_31_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_23_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_4_MESSAGE_15_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_7_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_2_MESSAGE_62_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_59_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_54_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_46_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_38_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_10_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_5_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_PORT_TX_PSL.VALUE=1
DRIVER.CAN.VAR.CAN_3_MESSAGE_60_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_52_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_44_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_36_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_28_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_62_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_54_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_46_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_38_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_20_ID.VALUE=20
DRIVER.CAN.VAR.CAN_2_MESSAGE_12_ID.VALUE=12
DRIVER.CAN.VAR.CAN_2_MESSAGE_7_ID.VALUE=7
DRIVER.CAN.VAR.CAN_1_MESSAGE_8_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_51_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_43_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_35_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_27_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_19_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_21_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_1_MESSAGE_13_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_4_MESSAGE_57_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_49_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_59_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_59_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_51_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_43_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_35_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_27_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_19_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_5_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_63_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_61_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_55_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_53_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_47_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_45_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_40_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_39_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_37_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_32_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_29_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_24_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_16_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_10_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_1_MESSAGE_8_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_2_MASK.VALUE=0x000007FF
DRIVER.CAN.VAR.CAN_3_MESSAGE_59_ID.VALUE=59
DRIVER.CAN.VAR.CAN_3_MESSAGE_50_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_42_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_34_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_26_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_18_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_AUTO_BUS_ON_TR.VALUE=0
DRIVER.CAN.VAR.CAN_2_MESSAGE_30_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_22_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_14_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_5_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_4_DLC.VALUE=8
DRIVER.CAN.VAR.CAN_3_MESSAGE_63_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_63_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_62_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_55_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_55_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_54_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_47_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_47_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_46_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_39_EOB.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_39_DIR.VALUE=0x20000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_38_INT_ENA_REF.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_PORT_RX_FUN.VALUE=1
DRIVER.CAN.VAR.CAN_4_MESSAGE_51_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_43_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_35_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_27_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_19_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_10_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_3_MESSAGE_2_BOOL_ENA.VALUE=0
DRIVER.CAN.VAR.CAN_1_MESSAGE_58_INT_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_21_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_1_MESSAGE_13_ENA.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_30_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_30_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_22_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_22_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_14_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_4_MESSAGE_14_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_6_RTR.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_3_MESSAGE_2_INT_LEVEL.VALUE=0x00000000
DRIVER.CAN.VAR.CAN_2_MESSAGE_21_ID.VALUE=21
DRIVER.CAN.VAR.CAN_2_MESSAGE_13_ID.VALUE=13
DRIVER.CAN.VAR.CAN_2_MESSAGE_8_ID.VALUE=8
DRIVER.ADC.VAR.ADC2_GROUP1_DISCHARGE_PRESCALER.VALUE=0
DRIVER.ADC.VAR.ADC1_GROUP1_PIN21_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN13_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_ACTUAL_DISCHARGE_TIME.VALUE=0.00
DRIVER.ADC.VAR.ADC2_GROUP1_RESOLUTION.VALUE=12_BIT
DRIVER.ADC.VAR.ADC2_GROUP0_PIN3_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_PARITY_ENABLE.VALUE=0x00000005
DRIVER.ADC.VAR.ADC1_GROUP2_PIN25_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN17_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_ACTUAL_DISCHARGE_TIME.VALUE=0.00
DRIVER.ADC.VAR.ADC1_GROUP2_RESOLUTION.VALUE=12_BIT
DRIVER.ADC.VAR.ADC2_GROUP2_PIN7_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN10_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_TRIGGER_EDGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_RAM_PARITY_ENA.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP1_EXTENDED_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC2_GROUP2_PIN0_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_RAM_PARITY_ENA.VALUE=0
DRIVER.ADC.VAR.ADC1_GROUP1_PIN3_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_CHANNEL_TOTAL_TIME.VALUE=0.000000
DRIVER.ADC.VAR.ADC1_GROUP1_FIFO_SIZE.VALUE=16
DRIVER.ADC.VAR.ADC1_GROUP2_DISCHARGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_SAMPLE_PRESCALER.VALUE=1
DRIVER.ADC.VAR.ADC1_GROUP1_LENGTH.VALUE=16
DRIVER.ADC.VAR.ADC2_GROUP1_ID_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN18_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_CONVERSION_TIME.VALUE=1.300
DRIVER.ADC.VAR.ADC2_PORT_BIT0_DIR.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP1_PIN4_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN11_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN7_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_ALT_TRIG.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP1_PIN23_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_PIN15_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN29_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN0_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_CONVERSION_TIME.VALUE=1.300
DRIVER.ADC.VAR.ADC2_GROUP2_LENGTH.VALUE=32
DRIVER.ADC.VAR.ADC2_GROUP2_PIN19_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_DISCHARGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN4_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN30_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN22_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN14_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_ACTUAL_SAMPLE_TIME.VALUE=320.01
DRIVER.ADC.VAR.ADC2_GROUP2_SAMPLE_PRESCALER.VALUE=1
DRIVER.ADC.VAR.ADC2_GROUP2_PIN20_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_PIN12_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN26_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN18_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN8_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN11_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_BND.VALUE=2
DRIVER.ADC.VAR.ADC2_GROUP0_PIN1_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN31_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN23_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN15_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_DISCHARGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_SAMPLE_PRESCALER.VALUE=1
DRIVER.ADC.VAR.ADC2_PORT_BIT0_PULDIS.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP2_PIN5_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN8_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_ID_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_EXTENDED_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC1_GROUP0_CONVERSION_TIME.VALUE=1.300
DRIVER.ADC.VAR.ADC2_GROUP0_RESOLUTION.VALUE=12_BIT
DRIVER.ADC.VAR.ADC1_GROUP1_PIN1_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_RESOLUTION.VALUE=12_BIT
DRIVER.ADC.VAR.ADC2_GROUP1_TRIGGER_EDGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_CONVERSION_TIME.VALUE=1.300
DRIVER.ADC.VAR.ADC2_BND.VALUE=2
DRIVER.ADC.VAR.ADC2_GROUP1_DISCHARGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_PORT_BIT0_PDR.VALUE=0
DRIVER.ADC.VAR.ADC2_ACTUAL_CYCLE_TIME.VALUE=106.67
DRIVER.ADC.VAR.ADC2_GROUP1_SAMPLE_PRESCALER.VALUE=1
DRIVER.ADC.VAR.ADC2_GROUP1_PIN9_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN24_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN16_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC2_GROUP1_PIN2_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_TRIGGER_MODE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN5_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_DISCHARGE_PRESCALER.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP1_PIN21_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_PIN13_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN9_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN27_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN19_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_DISCHARGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.ADC.VAR.ADC2_GROUP1_SCAN_TIME.VALUE=0.000
DRIVER.ADC.VAR.ADC2_GROUP0_CHANNEL_TOTAL_TIME.VALUE=0.000000
DRIVER.ADC.VAR.ADC1_GROUP2_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC2_GROUP0_LENGTH.VALUE=16
DRIVER.ADC.VAR.ADC1_GROUP0_SAMPLE_PRESCALER.VALUE=1
DRIVER.ADC.VAR.ADC2_GROUP2_PIN17_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_PORT_BIT0_PULDIS.VALUE=0
DRIVER.ADC.VAR.ADC1_GROUP2_PIN2_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN20_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN12_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_PIN10_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN24_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN16_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_ACTUAL_SAMPLE_TIME.VALUE=320.01
DRIVER.ADC.VAR.ADC2_GROUP0_PIN6_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN28_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_TRIGGER_MODE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_PORT_BIT0_PSL.VALUE=1
DRIVER.ADC.VAR.ADC1_GROUP2_CHANNEL_TOTAL_TIME.VALUE=0.000000
DRIVER.ADC.VAR.ADC1_GROUP0_DISCHARGE_TIME.VALUE=0.00
DRIVER.ADC.VAR.ADC2_LENGTH.VALUE=64
DRIVER.ADC.VAR.ADC2_GROUP0_DISCHARGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN21_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN13_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PINS.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP0_DISCHARGE_TIME.VALUE=0.00
DRIVER.ADC.VAR.ADC2_GROUP0_SAMPLE_PRESCALER.VALUE=1
DRIVER.ADC.VAR.ADC1_GROUP0_DISCHARGE_PRESCALER.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP2_PIN3_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN6_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_RAMBASE.VALUE=0xFF3A0000
DRIVER.ADC.VAR.ADC2_GROUP0_BND.VALUE=8
DRIVER.ADC.VAR.ADC1_PORT_BIT0_DOUT.VALUE=0
DRIVER.ADC.VAR.ADC1_GROUP1_SCAN_TIME.VALUE=0.000
DRIVER.ADC.VAR.ADC1_GROUP0_RESOLUTION.VALUE=12_BIT
DRIVER.ADC.VAR.ADC2_GROUP2_FIFO_SIZE.VALUE=16
DRIVER.ADC.VAR.ADC2_GROUP1_PIN7_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN22_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN14_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_HW_TRIGGER_SOURCE.VALUE=EVENT
DRIVER.ADC.VAR.ADC2_GROUP1_BND.VALUE=8
DRIVER.ADC.VAR.ADC2_GROUP0_HW_TRIGGER_SOURCE_ALT.VALUE=EVENT
DRIVER.ADC.VAR.ADC2_GROUP1_PIN18_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_PIN0_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN3_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_ALT_TRIG_COMP.VALUE=1
DRIVER.ADC.VAR.ADC2_GROUP1_HW_TRIGGER_SOURCE_ALT.VALUE=EVENT
DRIVER.ADC.VAR.ADC2_GROUP1_PIN11_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN7_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN25_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN17_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_PARITY_ENABLE.VALUE=0x00000005
DRIVER.ADC.VAR.ADC1_ACTUAL_CYCLE_TIME.VALUE=106.67
DRIVER.ADC.VAR.ADC2_GROUP2_HW_TRIGGER_SOURCE_ALT.VALUE=EVENT
DRIVER.ADC.VAR.ADC2_GROUP2_PIN23_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_PIN15_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN0_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_CONTINUOUS_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN29_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN10_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_PINS.VALUE=0
DRIVER.ADC.VAR.ADC1_GROUP1_PIN30_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN22_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN14_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN4_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN26_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN18_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_PIN8_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_TRIGGER_EDGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN11_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_PIN1_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_FIFO_SIZE.VALUE=16
DRIVER.ADC.VAR.ADC1_GROUP1_PIN4_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_RAMBASE.VALUE=0xFF3E0000
DRIVER.ADC.VAR.ADC1_BASE.VALUE=0xFFF7C000
DRIVER.ADC.VAR.ADC1_PORT_BIT0_DIR.VALUE=0
DRIVER.ADC.VAR.ADC2_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.ADC.VAR.ADC2_GROUP2_HW_TRIGGER_SOURCE.VALUE=EVENT
DRIVER.ADC.VAR.ADC2_GROUP2_ID_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_ACTUAL_SAMPLE_TIME.VALUE=320.01
DRIVER.ADC.VAR.ADC1_GROUP2_LENGTH.VALUE=32
DRIVER.ADC.VAR.ADC1_GROUP0_BND.VALUE=8
DRIVER.ADC.VAR.ADC2_GROUP0_PIN19_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_CHANNEL_TOTAL_TIME.VALUE=0.000000
DRIVER.ADC.VAR.ADC2_GROUP2_CONTINUOUS_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_PIN5_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN20_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN12_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN8_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_TRIGGER_EDGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_PINS.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP0_EXTENDED_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC1_GROUP1_DISCHARGE_TIME.VALUE=0.00
DRIVER.ADC.VAR.ADC2_GROUP1_PIN24_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_PIN16_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN1_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_EXTENDED_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC2_GROUP1_DISCHARGE_TIME.VALUE=0.00
DRIVER.ADC.VAR.ADC2_GROUP2_TRIGGER_MODE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_FIFO_SIZE.VALUE=16
DRIVER.ADC.VAR.ADC1_GROUP2_PIN5_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN31_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN23_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN15_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_BND.VALUE=8
DRIVER.ADC.VAR.ADC2_GROUP2_PIN21_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_PIN13_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN27_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN19_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_PORT_BIT0_DOUT.VALUE=0
DRIVER.ADC.VAR.ADC2_CYCLE_TIME.VALUE=100.00
DRIVER.ADC.VAR.ADC1_GROUP1_HW_TRIGGER_SOURCE.VALUE=EVENT
DRIVER.ADC.VAR.ADC1_GROUP1_DISCHARGE_PRESCALER.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP0_PIN9_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_PRESCALE.VALUE=7
DRIVER.ADC.VAR.ADC1_GROUP1_PIN20_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN12_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_RAM_PARITY_ENA.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP0_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC2_BASE.VALUE=0xFFF7C200
DRIVER.ADC.VAR.ADC2_GROUP0_PIN2_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_RAM_PARITY_ENA.VALUE=0
DRIVER.ADC.VAR.ADC1_GROUP2_PIN24_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN16_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_ID_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_PIN6_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN9_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_CONTINUOUS_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_PORT_BIT0_PDR.VALUE=0
DRIVER.ADC.VAR.ADC1_GROUP1_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC1_GROUP1_PIN2_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_CONVERSION_TIME.VALUE=1.300
DRIVER.ADC.VAR.ADC1_GROUP0_FIFO_SIZE.VALUE=16
DRIVER.ADC.VAR.ADC1_PORT_BIT0_PULL.VALUE=2
DRIVER.ADC.VAR.ADC1_GROUP0_LENGTH.VALUE=16
DRIVER.ADC.VAR.ADC2_GROUP0_PIN17_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_CONVERSION_TIME.VALUE=1.300
DRIVER.ADC.VAR.ADC1_GROUP0_PINS.VALUE=0
DRIVER.ADC.VAR.ADC1_GROUP0_ACTUAL_SAMPLE_TIME.VALUE=320.01
DRIVER.ADC.VAR.ADC2_GROUP1_PIN3_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN10_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_ID_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN6_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_SCAN_TIME.VALUE=0.000
DRIVER.ADC.VAR.ADC2_GROUP1_HW_TRIGGER_SOURCE.VALUE=EVENT
DRIVER.ADC.VAR.ADC1_GROUP1_CHANNEL_TOTAL_TIME.VALUE=0.000000
DRIVER.ADC.VAR.ADC1_GROUP0_EXTENDED_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC1_GROUP0_HW_TRIGGER_SOURCE_ALT.VALUE=EVENT
DRIVER.ADC.VAR.ADC2_GROUP1_PIN22_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_PIN14_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN28_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_PORT_BIT0_PSL.VALUE=1
DRIVER.ADC.VAR.ADC1_GROUP2_EXTENDED_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC2_GROUP1_LENGTH.VALUE=16
DRIVER.ADC.VAR.ADC1_GROUP1_HW_TRIGGER_SOURCE_ALT.VALUE=EVENT
DRIVER.ADC.VAR.ADC2_GROUP2_PIN18_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN3_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN21_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN13_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_ACTUAL_DISCHARGE_TIME.VALUE=0.00
DRIVER.ADC.VAR.ADC1_GROUP2_HW_TRIGGER_SOURCE_ALT.VALUE=EVENT
DRIVER.ADC.VAR.ADC2_GROUP2_PIN11_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_CONTINUOUS_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN25_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN17_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_ACTUAL_DISCHARGE_TIME.VALUE=0.00
DRIVER.ADC.VAR.ADC2_GROUP0_PIN7_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN29_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN10_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_ACTUAL_DISCHARGE_TIME.VALUE=0.00
DRIVER.ADC.VAR.ADC2_GROUP0_PIN0_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN30_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN22_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN14_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_CYCLE_TIME.VALUE=100.00
DRIVER.ADC.VAR.ADC2_GROUP0_DISCHARGE_PRESCALER.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP2_PIN4_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN7_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_DISCHARGE_TIME.VALUE=0.00
DRIVER.ADC.VAR.ADC1_GROUP0_HW_TRIGGER_SOURCE.VALUE=EVENT
DRIVER.ADC.VAR.ADC1_GROUP1_PIN0_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_ID_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_DISCHARGE_TIME.VALUE=0.00
DRIVER.ADC.VAR.ADC1_GROUP2_SCAN_TIME.VALUE=0.000
DRIVER.ADC.VAR.ADC1_GROUP1_PINS.VALUE=0
DRIVER.ADC.VAR.ADC1_GROUP1_TRIGGER_EDGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_ALT_TRIG_COMP.VALUE=1
DRIVER.ADC.VAR.ADC1_GROUP0_CONTINUOUS_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_PIN8_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN23_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN15_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_ALT_TRIG.VALUE=0
DRIVER.ADC.VAR.ADC1_GROUP1_RAM_PARITY_ENA.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP1_PIN19_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_PIN1_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_RAM_PARITY_ENA.VALUE=0
DRIVER.ADC.VAR.ADC1_GROUP0_PIN4_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_DISCHARGE_PRESCALER.VALUE=0
DRIVER.ADC.VAR.ADC2_GROUP1_PIN20_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_PIN12_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN8_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN26_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN18_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_RESOLUTION.VALUE=12_BIT
DRIVER.ADC.VAR.ADC2_GROUP2_PIN24_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_PIN16_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN1_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN11_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_SCAN_TIME.VALUE=0.000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN31_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN23_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN15_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_HW_TRIGGER_SOURCE.VALUE=EVENT
DRIVER.ADC.VAR.ADC2_GROUP0_PIN5_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN27_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN19_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_PRESCALE.VALUE=7
DRIVER.ADC.VAR.ADC2_GROUP0_ACTUAL_SAMPLE_TIME.VALUE=320.01
DRIVER.ADC.VAR.ADC1_GROUP2_PINS.VALUE=0
DRIVER.ADC.VAR.ADC2_PORT_BIT0_PULL.VALUE=2
DRIVER.ADC.VAR.ADC1_LENGTH.VALUE=64
DRIVER.ADC.VAR.ADC2_GROUP2_PIN9_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN20_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN12_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC2_GROUP1_CHANNEL_TOTAL_TIME.VALUE=0.000000
DRIVER.ADC.VAR.ADC2_GROUP2_PIN2_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_CONTINUOUS_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN5_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_ACTUAL_SAMPLE_TIME.VALUE=320.01
DRIVER.ADC.VAR.ADC1_GROUP0_SCAN_TIME.VALUE=0.000
DRIVER.ADC.VAR.ADC2_GROUP1_PIN6_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN21_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_PIN13_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP0_TRIGGER_EDGE_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN9_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_SAMPLE_TIME.VALUE=300.00
DRIVER.ADC.VAR.ADC2_GROUP1_PIN17_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_FIFO_SIZE.VALUE=16
DRIVER.ADC.VAR.ADC1_GROUP0_PIN2_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP1_PIN10_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP2_PIN6_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN24_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_PIN16_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_PIN22_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC2_GROUP2_PIN14_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_PIN28_ENABLE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP1_TRIGGER_MODE.VALUE=0x00000000
DRIVER.ADC.VAR.ADC1_GROUP0_ACTUAL_DISCHARGE_TIME.VALUE=0.00
DRIVER.LIN.VAR.LIN2_PORT_BIT1_PDR.VALUE=0
DRIVER.LIN.VAR.LIN1_TOAWUSINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_TOA3WUSINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT2_DOUT.VALUE=0
DRIVER.LIN.VAR.LIN2_PORT_BIT2_FUN.VALUE=4
DRIVER.LIN.VAR.LIN1_HGENCTRL.VALUE=1
DRIVER.LIN.VAR.LIN2_PORT_BIT0_PSL.VALUE=1
DRIVER.LIN.VAR.LIN2_PORT_BIT0_DOUT.VALUE=0
DRIVER.LIN.VAR.LIN1_PBEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_PORT_BIT0_PULDIS.VALUE=0
DRIVER.LIN.VAR.LIN2_PORT_BIT2_PDR.VALUE=0
DRIVER.LIN.VAR.LIN1_BASE_PORT.VALUE=0xFFF7E440
DRIVER.LIN.VAR.LIN2_PARITYENA.VALUE=0
DRIVER.LIN.VAR.LIN2_WAKEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_FEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_CEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_PORT_BIT1_PSL.VALUE=2
DRIVER.LIN.VAR.LIN2_OEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_TXINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT0_PULL.VALUE=2
DRIVER.LIN.VAR.LIN1_MAXPRESCALE.VALUE=3370
DRIVER.LIN.VAR.LIN2_IDINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT0_PULDIS.VALUE=0
DRIVER.LIN.VAR.LIN1_RX_MASK.VALUE=0xFF
DRIVER.LIN.VAR.LIN2_PORT_BIT2_PSL.VALUE=4
DRIVER.LIN.VAR.LIN2_PORT_BIT1_DOUT.VALUE=0
DRIVER.LIN.VAR.LIN1_BREAKINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_NREINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_TOINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_TOAWUSINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_TOA3WUSINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_BAUDRATE.VALUE=20.000
DRIVER.LIN.VAR.LIN1_OEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT0_DIR.VALUE=0
DRIVER.LIN.VAR.LIN1_PORT_BIT1_PULL.VALUE=2
DRIVER.LIN.VAR.LIN2_RXINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_WAKEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_PORT_BIT2_DOUT.VALUE=0
DRIVER.LIN.VAR.LIN2_WAKEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_FEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT1_DIR.VALUE=0
DRIVER.LIN.VAR.LIN1_CEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_PBEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_TXINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT0_FUN.VALUE=0
DRIVER.LIN.VAR.LIN2_IDINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT2_DIR.VALUE=0
DRIVER.LIN.VAR.LIN2_SBREAK.VALUE=13
DRIVER.LIN.VAR.LIN2_TOAWUSINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT2_PULL.VALUE=2
DRIVER.LIN.VAR.LIN1_BREAKINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_PEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT0_PDR.VALUE=0
DRIVER.LIN.VAR.LIN1_BASE.VALUE=0xFFF7E400
DRIVER.LIN.VAR.LIN2_PORT_BIT0_PULL.VALUE=2
DRIVER.LIN.VAR.LIN1_LENGTH.VALUE=8
DRIVER.LIN.VAR.LIN2_TOINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT1_FUN.VALUE=2
DRIVER.LIN.VAR.LIN2_BEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_ACTUALBAUDRATE.VALUE=20.032
DRIVER.LIN.VAR.LIN1_FEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_OEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_NREINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_TXINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT1_PDR.VALUE=0
DRIVER.LIN.VAR.LIN1_MSTMOD.VALUE=1
DRIVER.LIN.VAR.LIN2_ISFEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT2_FUN.VALUE=4
DRIVER.LIN.VAR.LIN2_TX_MASK.VALUE=0xFF
DRIVER.LIN.VAR.LIN1_PORT_BIT0_PSL.VALUE=1
DRIVER.LIN.VAR.LIN2_RXINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_WAKEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_IDINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_PRESCALE.VALUE=233
DRIVER.LIN.VAR.LIN1_PORT_BIT2_PDR.VALUE=0
DRIVER.LIN.VAR.LIN2_BASE.VALUE=0xFFF7E600
DRIVER.LIN.VAR.LIN2_PORT_BIT1_PULL.VALUE=2
DRIVER.LIN.VAR.LIN2_PBEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_PORT_BIT1_PULDIS.VALUE=0
DRIVER.LIN.VAR.LIN1_TOINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT1_PSL.VALUE=2
DRIVER.LIN.VAR.LIN2_BASE_PORT.VALUE=0xFFF7E640
DRIVER.LIN.VAR.LIN1_BAUDRATE.VALUE=20.000
DRIVER.LIN.VAR.LIN2_TOAWUSINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_PEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT2_PSL.VALUE=4
DRIVER.LIN.VAR.LIN2_MAXBAUDRATE.VALUE=22.255
DRIVER.LIN.VAR.LIN1_RXINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_BEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_FEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_PORT_BIT2_PULL.VALUE=2
DRIVER.LIN.VAR.LIN1_PORT_BIT1_PULDIS.VALUE=0
DRIVER.LIN.VAR.LIN1_TX_MASK.VALUE=0xFF
DRIVER.LIN.VAR.LIN2_NREINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_TXINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_ISFEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_ISFEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_ACTUALBAUDRATE.VALUE=20.032
DRIVER.LIN.VAR.LIN1_IDINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_TOA3WUSINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_TOINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PARITYENA.VALUE=0
DRIVER.LIN.VAR.LIN1_BEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_RXINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_HGENCTRL.VALUE=1
DRIVER.LIN.VAR.LIN1_PRESCALE.VALUE=233
DRIVER.LIN.VAR.LIN1_ISFEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_SDEL.VALUE=1
DRIVER.LIN.VAR.LIN2_LENGTH.VALUE=8
DRIVER.LIN.VAR.LIN2_MAXPRESCALE.VALUE=3370
DRIVER.LIN.VAR.LIN2_CEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_BREAKINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT0_DOUT.VALUE=0
DRIVER.LIN.VAR.LIN2_TOA3WUSINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_MSTMOD.VALUE=1
DRIVER.LIN.VAR.LIN2_PORT_BIT0_DIR.VALUE=0
DRIVER.LIN.VAR.LIN1_BEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PBEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_SDEL.VALUE=1
DRIVER.LIN.VAR.LIN2_PORT_BIT1_DIR.VALUE=0
DRIVER.LIN.VAR.LIN1_MAXBAUDRATE.VALUE=22.255
DRIVER.LIN.VAR.LIN2_PORT_BIT2_PULDIS.VALUE=0
DRIVER.LIN.VAR.LIN1_SBREAK.VALUE=13
DRIVER.LIN.VAR.LIN2_OEINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_PORT_BIT1_DOUT.VALUE=0
DRIVER.LIN.VAR.LIN2_PORT_BIT0_FUN.VALUE=0
DRIVER.LIN.VAR.LIN2_PORT_BIT2_DIR.VALUE=0
DRIVER.LIN.VAR.LIN2_PORT_BIT0_PDR.VALUE=0
DRIVER.LIN.VAR.LIN2_PORT_BIT1_FUN.VALUE=2
DRIVER.LIN.VAR.LIN2_CEINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN1_NREINTENA.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_BREAKINTLVL.VALUE=0x00000000
DRIVER.LIN.VAR.LIN2_RX_MASK.VALUE=0xFF
DRIVER.LIN.VAR.LIN1_PORT_BIT2_PULDIS.VALUE=0
DRIVER.HET.VAR.HET2_EDGE5_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM5_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET2_PWM0_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT0_PULL.VALUE=1
DRIVER.HET.VAR.HET2_INT_X0.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE4_BOTH.VALUE=0
DRIVER.HET.VAR.HET1_BIT1_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT6_HRSHARE.VALUE=0x00000008
DRIVER.HET.VAR.HET2_INT_X1.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM2_DUTY.VALUE=50
DRIVER.HET.VAR.HET1_BIT29_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT0_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_IGNORE_SUSPEND_ENABLE.VALUE=0x00020000
DRIVER.HET.VAR.HET2_PWM3_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET2_PWM1_PIN_SELECT.VALUE=10
DRIVER.HET.VAR.HET2_BIT20_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT12_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT3_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_INT_X2.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X3.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM2_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_INT_X4.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM6_ACTION.VALUE=3
DRIVER.HET.VAR.HET1_PWM0_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT4_PULL.VALUE=1
DRIVER.HET.VAR.HET2_PWM3_ENA.VALUE=0
DRIVER.HET.VAR.HET2_BIT4_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X5.VALUE=0x00000000
DRIVER.HET.VAR.HET2_IGNORE_SUSPEND_ENABLE.VALUE=0x00020000
DRIVER.HET.VAR.HET1_BIT30_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT26_HRSHARE.VALUE=0x00002000
DRIVER.HET.VAR.HET1_BIT22_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT18_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT14_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM4_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET2_BIT3_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X6.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE0_PIN_SELECT.VALUE=9
DRIVER.HET.VAR.HET1_BIT28_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT7_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_INT_X7.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT7_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X8.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM3_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT26_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT18_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT10_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X9.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT11_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT11_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_PWM4_PIN_SELECT.VALUE=16
DRIVER.HET.VAR.HET2_PWM4_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET1_RAM_BASE.VALUE=0xFF460000
DRIVER.HET.VAR.HET2_EDGE6_BOTH.VALUE=0
DRIVER.HET.VAR.HET2_PWM2_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT31_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT23_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT15_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE2_EVENT.VALUE=1
DRIVER.HET.VAR.HET2_BIT11_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PIN_ENABLE.VALUE=0
DRIVER.HET.VAR.HET1_CAP3_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_BIT24_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT16_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT5_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT27_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT19_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE6_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT24_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT16_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT2_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM6_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE3_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_EDGE5_PIN_SELECT.VALUE=21
DRIVER.HET.VAR.HET2_BIT21_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT13_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM7_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET1_BIT27_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT19_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_CAP5_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_PWM4_ENA.VALUE=0
DRIVER.HET.VAR.HET2_BIT8_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM1_POLARITY.VALUE=3
DRIVER.HET.VAR.HET2_CAP2_PIN_SELECT.VALUE=4
DRIVER.HET.VAR.HET2_BIT4_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM0_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET1_BIT29_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT0_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT8_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM4_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET2_BIT1_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT20_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT12_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM7_ACTION.VALUE=3
DRIVER.HET.VAR.HET2_PWM4_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET2_BIT26_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT24_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT18_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT16_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM3_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM3_POLARITY.VALUE=3
DRIVER.HET.VAR.HET2_BIT28_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT0_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM1_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET2_BIT29_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT6_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_CAP5_PIN_SELECT.VALUE=26
DRIVER.HET.VAR.HET1_BIT28_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT10_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_EDGE7_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM0_ACTION.VALUE=3
DRIVER.HET.VAR.HET2_BIT1_PULL.VALUE=1
DRIVER.HET.VAR.HET1_EDGE7_EVENT.VALUE=1
DRIVER.HET.VAR.HET1_EDGE5_BOTH.VALUE=0
DRIVER.HET.VAR.HET1_PWM5_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET1_BIT3_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE7_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_EDGE1_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM3_DUTY.VALUE=50
DRIVER.HET.VAR.HET1_PWM1_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT30_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT22_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT14_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT4_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_EDGE4_EVENT.VALUE=1
DRIVER.HET.VAR.HET1_BIT5_PULL.VALUE=1
DRIVER.HET.VAR.HET1_MASTER.VALUE=1
DRIVER.HET.VAR.HET2_EDGE5_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM5_ENA.VALUE=0
DRIVER.HET.VAR.HET2_PWM0_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT2_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT5_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM7_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET1_BIT8_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT1_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_LR_ACTUALTIME.VALUE=853.333
DRIVER.HET.VAR.HET1_PWM5_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_PWM5_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM4_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET2_BIT9_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM3_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM0_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT5_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM6_PIN_SELECT.VALUE=18
DRIVER.HET.VAR.HET2_BIT21_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT20_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT13_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT12_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_EDGE7_BOTH.VALUE=0
DRIVER.HET.VAR.HET2_BIT25_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT17_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM6_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM0_ENA.VALUE=0
DRIVER.HET.VAR.HET1_BIT30_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT27_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT22_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT19_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT14_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM1_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET2_BIT7_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE5_PIN_SELECT.VALUE=21
DRIVER.HET.VAR.HET1_BIT29_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT0_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET_DIS_BLACKBOX.VALUE=0
DRIVER.HET.VAR.HET2_PWM7_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_HR_ACTUALFREQUENCY.VALUE=75.000
DRIVER.HET.VAR.HET2_PWM5_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM4_ACTION.VALUE=3
DRIVER.HET.VAR.HET1_BIT25_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT17_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT4_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE0_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_CAP6_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_BIT20_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT12_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT31_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT23_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT15_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X10.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT28_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_INT_X11.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X20.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X12.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM3_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET2_PWM6_ENA.VALUE=0
DRIVER.HET.VAR.HET2_BIT24_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT16_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X21.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X13.VALUE=0x00000000
DRIVER.HET.VAR.HET2_HR_PRESCALE.VALUE=0
DRIVER.HET.VAR.HET1_EDGE6_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_PWM6_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_LR_PRESCALE.VALUE=6
DRIVER.HET.VAR.HET2_PWM0_PIN_SELECT.VALUE=8
DRIVER.HET.VAR.HET2_BIT6_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X30.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X22.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X14.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT2_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X31.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X23.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X15.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM3_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET2_INT_X24.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X16.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BASE_PORT.VALUE=0xFFF7B84C
DRIVER.HET.VAR.HET2_PWM5_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT0_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X25.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X17.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM4_POLARITY.VALUE=3
DRIVER.HET.VAR.HET1_PWM3_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT10_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT30_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT22_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT14_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X26.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X18.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X27.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X19.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT27_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT26_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT19_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT18_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X28.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM2_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM1_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET2_PWM0_DUTY.VALUE=50
DRIVER.HET.VAR.HET2_BIT26_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT18_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_INT_X29.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM1_ENA.VALUE=0
DRIVER.HET.VAR.HET2_CAP7_PIN_SELECT.VALUE=30
DRIVER.HET.VAR.HET2_BIT8_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM5_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET1_PWM4_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET1_PWM3_PIN_SELECT.VALUE=14
DRIVER.HET.VAR.HET1_BIT11_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT1_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM0_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_BIT2_PULL.VALUE=1
DRIVER.HET.VAR.HET1_EDGE6_BOTH.VALUE=0
DRIVER.HET.VAR.HET1_BIT5_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM6_POLARITY.VALUE=3
DRIVER.HET.VAR.HET2_BIT30_HRSHARE.VALUE=0x00008000
DRIVER.HET.VAR.HET2_BIT22_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT14_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT6_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM4_DUTY.VALUE=50
DRIVER.HET.VAR.HET1_BIT20_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT12_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PIN_ENABLE.VALUE=0
DRIVER.HET.VAR.HET2_BIT24_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT16_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT5_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_PWM0_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET1_BIT6_PULL.VALUE=1
DRIVER.HET.VAR.HET2_PWM7_ENA.VALUE=0
DRIVER.HET.VAR.HET1_PWM0_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT8_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE4_PIN_SELECT.VALUE=20
DRIVER.HET.VAR.HET2_BIT7_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT9_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT3_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM5_ACTION.VALUE=3
DRIVER.HET.VAR.HET2_BIT10_PULL.VALUE=1
DRIVER.HET.VAR.HET2_CAP1_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_EDGE6_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_CAP1_PIN_SELECT.VALUE=2
DRIVER.HET.VAR.HET2_BIT31_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT23_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT21_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT15_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT13_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT27_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT19_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE3_EVENT.VALUE=1
DRIVER.HET.VAR.HET1_PWM6_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM2_ENA.VALUE=0
DRIVER.HET.VAR.HET2_BIT9_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT2_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE0_EVENT.VALUE=1
DRIVER.HET.VAR.HET1_PWM2_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET1_BIT26_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT18_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT6_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE3_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT24_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT16_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT25_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT17_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_CAP4_PIN_SELECT.VALUE=24
DRIVER.HET.VAR.HET1_BIT29_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT0_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_PWM2_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET2_EDGE3_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_BIT3_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT2_HRSHARE.VALUE=0x00000002
DRIVER.HET.VAR.HET2_PWM6_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET2_BIT8_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM1_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET1_BIT4_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT4_HRSHARE.VALUE=0x00000004
DRIVER.HET.VAR.HET1_BIT25_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT17_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT24_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT16_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM1_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_PWM4_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT28_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT28_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM2_ACTION.VALUE=3
DRIVER.HET.VAR.HET2_PWM1_DUTY.VALUE=50
DRIVER.HET.VAR.HET2_BIT29_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM7_POLARITY.VALUE=3
DRIVER.HET.VAR.HET1_PWM3_ENA.VALUE=0
DRIVER.HET.VAR.HET1_BIT24_HRSHARE.VALUE=0x00001000
DRIVER.HET.VAR.HET1_BIT16_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT10_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM5_PIN_SELECT.VALUE=17
DRIVER.HET.VAR.HET1_BIT20_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT12_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT3_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X10.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X11.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT3_PULL.VALUE=1
DRIVER.HET.VAR.HET1_EDGE7_BOTH.VALUE=0
DRIVER.HET.VAR.HET1_EDGE0_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT7_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X20.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X12.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT30_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT22_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT14_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM5_DUTY.VALUE=50
DRIVER.HET.VAR.HET1_BIT10_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X21.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X13.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM5_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET2_BIT26_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT18_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT6_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_EDGE4_PIN_SELECT.VALUE=20
DRIVER.HET.VAR.HET1_INT_X30.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X22.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X14.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM3_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET1_INT_X31.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X23.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X15.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE5_EVENT.VALUE=1
DRIVER.HET.VAR.HET2_PWM1_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM7_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM6_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET1_BIT7_PULL.VALUE=1
DRIVER.HET.VAR.HET1_INT_X24.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X16.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT28_HRSHARE.VALUE=0x00004000
DRIVER.HET.VAR.HET1_CAP2_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_PWM3_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT6_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X25.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X17.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT9_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT5_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X26.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X18.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X27.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X19.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT11_PULL.VALUE=1
DRIVER.HET.VAR.HET1_INT_X28.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM2_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_RAM_SIZE.VALUE=160
DRIVER.HET.VAR.HET1_EDGE2_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_INT_X29.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT30_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT25_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT22_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT17_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT14_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_PWM3_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET2_PWM5_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET2_BIT29_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM1_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET1_BIT10_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_CAP4_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_BIT8_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT4_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM4_ENA.VALUE=0
DRIVER.HET.VAR.HET1_PWM0_POLARITY.VALUE=3
DRIVER.HET.VAR.HET1_BIT4_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM1_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET1_EDGE1_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM1_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT27_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT19_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT8_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT30_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT22_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT14_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_CAP6_PIN_SELECT.VALUE=28
DRIVER.HET.VAR.HET2_BIT27_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT19_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM2_PIN_SELECT.VALUE=12
DRIVER.HET.VAR.HET1_BIT1_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_PWM3_ACTION.VALUE=3
DRIVER.HET.VAR.HET2_PWM2_POLARITY.VALUE=3
DRIVER.HET.VAR.HET1_EDGE4_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT28_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT6_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE0_BOTH.VALUE=0
DRIVER.HET.VAR.HET2_EDGE6_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_PWM5_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT8_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT4_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE3_PIN_SELECT.VALUE=15
DRIVER.HET.VAR.HET2_PWM2_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET2_BIT26_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT18_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT29_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT11_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT10_PULL.VALUE=1
DRIVER.HET.VAR.HET2_EDGE1_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM7_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM2_DUTY.VALUE=50
DRIVER.HET.VAR.HET1_PWM5_ENA.VALUE=0
DRIVER.HET.VAR.HET1_BIT8_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_CAP0_PIN_SELECT.VALUE=0
DRIVER.HET.VAR.HET1_BIT21_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT13_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT5_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM4_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_BIT4_PULL.VALUE=1
DRIVER.HET.VAR.HET1_EDGE2_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM2_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM2_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET1_BIT9_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT6_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM6_DUTY.VALUE=50
DRIVER.HET.VAR.HET1_BIT1_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM4_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET2_BIT28_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT7_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_PWM7_ACTION.VALUE=3
DRIVER.HET.VAR.HET1_BIT8_PULL.VALUE=1
DRIVER.HET.VAR.HET2_PWM2_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT20_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT12_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT31_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT23_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT15_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_CAP3_PIN_SELECT.VALUE=6
DRIVER.HET.VAR.HET1_BIT7_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM6_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_PWM4_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM1_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET2_BIT20_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT12_PULL.VALUE=1
DRIVER.HET.VAR.HET1_PWM0_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET1_PWM0_ACTION.VALUE=3
DRIVER.HET.VAR.HET2_BIT27_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT19_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_CAP5_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_BIT26_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT18_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT31_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT27_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT23_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT19_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT15_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_PWM0_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET1_EDGE4_EVENT.VALUE=1
DRIVER.HET.VAR.HET1_BIT20_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT12_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT20_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT12_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE5_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_PWM6_ENA.VALUE=0
DRIVER.HET.VAR.HET1_BIT6_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE1_EVENT.VALUE=1
DRIVER.HET.VAR.HET2_PWM3_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE3_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT28_PULL.VALUE=1
DRIVER.HET.VAR.HET2_CAP7_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_PWM3_POLARITY.VALUE=3
DRIVER.HET.VAR.HET2_PWM4_PIN_SELECT.VALUE=16
DRIVER.HET.VAR.HET2_BIT29_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT10_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT2_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT9_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM5_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM0_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE3_PIN_SELECT.VALUE=15
DRIVER.HET.VAR.HET1_PWM1_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET1_BIT8_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BASE.VALUE=0xFFF7B800
DRIVER.HET.VAR.HET2_EDGE1_BOTH.VALUE=0
DRIVER.HET.VAR.HET1_PWM6_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM5_POLARITY.VALUE=3
DRIVER.HET.VAR.HET2_BIT20_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT12_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT2_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT2_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT28_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM7_PIN_SELECT.VALUE=19
DRIVER.HET.VAR.HET1_PWM5_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET1_LR_ACTUALTIME.VALUE=853.333
DRIVER.HET.VAR.HET1_BIT21_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT13_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT11_PULL.VALUE=1
DRIVER.HET.VAR.HET2_PWM3_DUTY.VALUE=50
DRIVER.HET.VAR.HET1_PWM7_ENA.VALUE=0
DRIVER.HET.VAR.HET1_HR_PRESCALE.VALUE=0
DRIVER.HET.VAR.HET1_BIT30_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT22_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT14_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT7_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_HR_ACTUALFREQUENCY.VALUE=75.000
DRIVER.HET.VAR.HET2_PWM1_ACTION.VALUE=3
DRIVER.HET.VAR.HET2_BIT5_PULL.VALUE=1
DRIVER.HET.VAR.HET1_EDGE4_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_CAP0_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_BIT4_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE2_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM7_DUTY.VALUE=50
DRIVER.HET.VAR.HET1_PWM2_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT8_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT11_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM7_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_EDGE6_EVENT.VALUE=1
DRIVER.HET.VAR.HET2_MASTER.VALUE=1
DRIVER.HET.VAR.HET1_PWM5_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM0_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT9_PULL.VALUE=1
DRIVER.HET.VAR.HET2_EDGE6_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT10_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_CAP5_PIN_SELECT.VALUE=26
DRIVER.HET.VAR.HET1_PWM1_PIN_SELECT.VALUE=10
DRIVER.HET.VAR.HET1_BIT9_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT21_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT13_PULL.VALUE=1
DRIVER.HET.VAR.HET1_PWM7_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET1_PWM5_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT24_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT16_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT6_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.HET.VAR.HET2_BIT29_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT24_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT16_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT10_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM7_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE0_BOTH.VALUE=0
DRIVER.HET.VAR.HET1_BIT30_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT22_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT14_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X0.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE2_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_PWM4_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT28_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT0_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT0_HRSHARE.VALUE=0x00000001
DRIVER.HET.VAR.HET1_INT_X1.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE2_PIN_SELECT.VALUE=13
DRIVER.HET.VAR.HET2_PWM2_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET1_BIT8_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X2.VALUE=0x00000000
DRIVER.HET.VAR.HET1_DIS_BLACKBOX.VALUE=0
DRIVER.HET.VAR.HET2_LR_TIME.VALUE=800.000
DRIVER.HET.VAR.HET1_INT_X3.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM6_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET1_EDGE5_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM5_ACTION.VALUE=3
DRIVER.HET.VAR.HET1_BIT29_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT0_PULL.VALUE=1
DRIVER.HET.VAR.HET1_INT_X4.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT2_HRSHARE.VALUE=0x00000002
DRIVER.HET.VAR.HET1_BIT21_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT13_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X5.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM2_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET1_BIT20_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT12_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT3_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_INT_X6.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM0_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET1_INT_X7.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BASE_PORT.VALUE=0xFFF7B94C
DRIVER.HET.VAR.HET1_INT_X8.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT25_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT17_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT2_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM6_POLARITY.VALUE=3
DRIVER.HET.VAR.HET1_BIT30_HRSHARE.VALUE=0x00008000
DRIVER.HET.VAR.HET1_BIT22_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT14_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_INT_X9.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BASE.VALUE=0xFFF7B900
DRIVER.HET.VAR.HET2_EDGE2_BOTH.VALUE=0
DRIVER.HET.VAR.HET1_EDGE0_EVENT.VALUE=1
DRIVER.HET.VAR.HET2_BIT28_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT10_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_CAP2_PIN_SELECT.VALUE=4
DRIVER.HET.VAR.HET1_BIT11_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM2_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_PWM0_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT31_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT23_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT20_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT15_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT12_PULL.VALUE=1
DRIVER.HET.VAR.HET2_PWM4_DUTY.VALUE=50
DRIVER.HET.VAR.HET2_BIT26_HRSHARE.VALUE=0x00002000
DRIVER.HET.VAR.HET2_BIT18_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_CAP1_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_BIT30_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT22_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT14_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM6_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET1_PWM6_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET1_BIT31_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT23_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT15_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT9_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT6_PULL.VALUE=1
DRIVER.HET.VAR.HET1_EDGE6_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT7_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE1_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_RAM_SIZE.VALUE=160
DRIVER.HET.VAR.HET2_BIT9_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT21_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT13_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM2_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT0_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM3_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET2_CAP3_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_BIT0_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM3_PIN_SELECT.VALUE=14
DRIVER.HET.VAR.HET2_PWM6_ACTION.VALUE=3
DRIVER.HET.VAR.HET2_BIT30_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT22_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT14_PULL.VALUE=1
DRIVER.HET.VAR.HET1_EDGE7_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT25_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT17_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_EDGE2_PIN_SELECT.VALUE=13
DRIVER.HET.VAR.HET1_BIT20_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT12_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_HR_FREQUENCY.VALUE=110.000
DRIVER.HET.VAR.HET2_PWM2_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET1_EDGE5_EVENT.VALUE=1
DRIVER.HET.VAR.HET1_EDGE1_BOTH.VALUE=0
DRIVER.HET.VAR.HET1_PWM5_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT24_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT16_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM1_POLARITY.VALUE=3
DRIVER.HET.VAR.HET2_BIT26_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT18_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE0_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT0_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_PWM6_PIN_SELECT.VALUE=18
DRIVER.HET.VAR.HET2_EDGE2_EVENT.VALUE=1
DRIVER.HET.VAR.HET1_EDGE7_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT1_PULL.VALUE=1
DRIVER.HET.VAR.HET2_EDGE5_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_EDGE4_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT6_HRSHARE.VALUE=0x00000008
DRIVER.HET.VAR.HET1_BIT30_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT22_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT14_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT4_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT1_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM7_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT8_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT0_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT4_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE7_PIN_SELECT.VALUE=23
DRIVER.HET.VAR.HET2_PWM7_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET2_PWM3_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET1_PWM3_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_EDGE3_BOTH.VALUE=0
DRIVER.HET.VAR.HET1_PWM1_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM2_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT28_HRSHARE.VALUE=0x00004000
DRIVER.HET.VAR.HET1_BIT26_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT18_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_CAP4_PIN_SELECT.VALUE=24
DRIVER.HET.VAR.HET2_PWM0_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET1_PWM0_PIN_SELECT.VALUE=8
DRIVER.HET.VAR.HET1_BIT21_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT13_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_LR_TIME.VALUE=800.000
DRIVER.HET.VAR.HET2_EDGE0_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM3_ACTION.VALUE=3
DRIVER.HET.VAR.HET1_BIT25_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT21_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT17_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT13_PULL.VALUE=1
DRIVER.HET.VAR.HET2_PWM5_DUTY.VALUE=50
DRIVER.HET.VAR.HET2_PWM1_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT20_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT12_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT11_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT24_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT16_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_PWM5_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_RAM_BASE.VALUE=0xFF440000
DRIVER.HET.VAR.HET2_PWM3_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT7_PULL.VALUE=1
DRIVER.HET.VAR.HET2_PWM4_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT31_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT23_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT15_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_CAP4_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_BIT8_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE1_PIN_SELECT.VALUE=11
DRIVER.HET.VAR.HET1_CAP7_PIN_SELECT.VALUE=30
DRIVER.HET.VAR.HET1_BIT31_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT23_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT15_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE7_EVENT.VALUE=1
DRIVER.HET.VAR.HET2_BIT2_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE4_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_BIT31_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT23_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT15_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT10_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_CAP6_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_PWM2_POLARITY.VALUE=3
DRIVER.HET.VAR.HET2_BIT26_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT18_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT0_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM4_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET1_BIT30_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT22_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT14_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE1_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM7_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE2_BOTH.VALUE=0
DRIVER.HET.VAR.HET1_BIT26_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT18_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM1_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT24_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT16_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT5_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_RAM_PARITY_ENA.VALUE=0x00000005
DRIVER.HET.VAR.HET1_PWM7_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM0_DUTY.VALUE=50
DRIVER.HET.VAR.HET2_PWM0_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET2_BIT1_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_CAP1_PIN_SELECT.VALUE=2
DRIVER.HET.VAR.HET1_PWM7_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET1_BIT2_PULL.VALUE=1
DRIVER.HET.VAR.HET2_PWM6_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM4_POLARITY.VALUE=3
DRIVER.HET.VAR.HET2_BIT10_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM7_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT10_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE7_PIN_SELECT.VALUE=23
DRIVER.HET.VAR.HET1_BIT24_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT16_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT5_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_PWM7_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET2_PWM7_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET2_PWM4_ACTION.VALUE=3
DRIVER.HET.VAR.HET2_BIT3_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE5_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT6_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM6_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET2_EDGE4_BOTH.VALUE=0
DRIVER.HET.VAR.HET2_PWM1_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT11_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE1_EVENT.VALUE=1
DRIVER.HET.VAR.HET2_LR_PRESCALE.VALUE=6
DRIVER.HET.VAR.HET2_PWM2_PIN_SELECT.VALUE=12
DRIVER.HET.VAR.HET2_BIT1_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT31_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT23_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT15_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM6_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_EDGE2_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM4_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT30_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT27_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT22_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT19_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT14_PULL.VALUE=1
DRIVER.HET.VAR.HET2_EDGE2_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM6_DUTY.VALUE=50
DRIVER.HET.VAR.HET2_BIT8_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM4_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT9_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE1_PIN_SELECT.VALUE=11
DRIVER.HET.VAR.HET1_BIT25_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT17_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT8_PULL.VALUE=1
DRIVER.HET.VAR.HET1_PWM4_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM0_ENA.VALUE=0
DRIVER.HET.VAR.HET2_BIT30_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT22_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT14_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT2_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM5_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET2_BIT0_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM5_PIN_SELECT.VALUE=17
DRIVER.HET.VAR.HET1_BIT25_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT17_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM6_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT4_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE1_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_CAP7_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_BIT28_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT24_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT16_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT24_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT20_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT16_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT12_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM4_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET1_PWM1_ACTION.VALUE=3
DRIVER.HET.VAR.HET2_BIT28_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT0_HRSHARE.VALUE=0x00000001
DRIVER.HET.VAR.HET1_EDGE7_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_PWM1_DUTY_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE6_PIN_SELECT.VALUE=22
DRIVER.HET.VAR.HET2_BIT27_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT19_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT2_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_DIS_BLACKBOX.VALUE=0
DRIVER.HET.VAR.HET1_BIT24_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT16_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE3_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE6_EVENT.VALUE=1
DRIVER.HET.VAR.HET1_EDGE3_BOTH.VALUE=0
DRIVER.HET.VAR.HET1_PWM6_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET1_BIT28_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT21_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT13_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM5_POLARITY.VALUE=3
DRIVER.HET.VAR.HET1_PWM1_DUTY.VALUE=50
DRIVER.HET.VAR.HET1_BIT20_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT12_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_CAP3_PIN_SELECT.VALUE=6
DRIVER.HET.VAR.HET2_BIT10_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT2_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_PWM3_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET2_EDGE3_EVENT.VALUE=1
DRIVER.HET.VAR.HET2_PWM6_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET2_PWM3_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET1_BIT3_PULL.VALUE=1
DRIVER.HET.VAR.HET2_PWM1_ENA.VALUE=0
DRIVER.HET.VAR.HET2_BIT1_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT26_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT18_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT6_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_PWM1_DUTYTIME.VALUE=500.053
DRIVER.HET.VAR.HET2_BIT5_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM7_POLARITY.VALUE=3
DRIVER.HET.VAR.HET2_BIT24_HRSHARE.VALUE=0x00001000
DRIVER.HET.VAR.HET2_BIT16_HRSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_CAP0_POLARITY.VALUE=0
DRIVER.HET.VAR.HET1_BIT4_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE0_PIN_SELECT.VALUE=9
DRIVER.HET.VAR.HET2_BIT10_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_CAP6_PIN_SELECT.VALUE=28
DRIVER.HET.VAR.HET1_PWM2_PERIOD.VALUE=1000.000
DRIVER.HET.VAR.HET2_EDGE5_BOTH.VALUE=0
DRIVER.HET.VAR.HET2_BIT21_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT13_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT3_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE0_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_PWM7_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET2_BIT3_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT25_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT17_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_EDGE4_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT31_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT29_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT23_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT15_PULL.VALUE=1
DRIVER.HET.VAR.HET1_BIT0_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_CAP2_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_PWM7_DUTY.VALUE=50
DRIVER.HET.VAR.HET2_BIT6_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM4_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT11_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT26_DOUT.VALUE=0
DRIVER.HET.VAR.HET1_BIT18_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_PWM6_PERIOD_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM2_ACTION.VALUE=3
DRIVER.HET.VAR.HET2_BIT9_PULL.VALUE=1
DRIVER.HET.VAR.HET1_PWM7_DUTY_LVL.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM3_PERIOD_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM2_ENA.VALUE=0
DRIVER.HET.VAR.HET2_BIT20_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT12_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE3_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM7_PIN_SELECT.VALUE=19
DRIVER.HET.VAR.HET2_BIT2_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_CAP0_PIN_SELECT.VALUE=0
DRIVER.HET.VAR.HET1_BIT27_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT19_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT6_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM0_DUTY_PRESCALER.VALUE=75136
DRIVER.HET.VAR.HET2_EDGE7_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET2_PWM0_POLARITY.VALUE=3
DRIVER.HET.VAR.HET1_BIT26_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT18_XORSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT10_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_EDGE6_PIN_SELECT.VALUE=22
DRIVER.HET.VAR.HET1_PWM0_ACTUALPERIOD.VALUE=1000.106
DRIVER.HET.VAR.HET2_HR_FREQUENCY.VALUE=110.000
DRIVER.HET.VAR.HET2_BIT30_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT25_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT22_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT17_PULL.VALUE=1
DRIVER.HET.VAR.HET2_BIT14_DIR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_PWM5_PERIOD_PRESCALER.VALUE=149888
DRIVER.HET.VAR.HET2_EDGE4_POLARITY.VALUE=0
DRIVER.HET.VAR.HET2_EDGE0_INTENA.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT7_PULDIS.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT4_HRSHARE.VALUE=0x00000004
DRIVER.HET.VAR.HET1_BIT2_ANDSHARE.VALUE=0x00000000
DRIVER.HET.VAR.HET2_BIT28_DOUT.VALUE=0
DRIVER.HET.VAR.HET2_BIT4_PDR.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT26_PSL.VALUE=0x00000000
DRIVER.HET.VAR.HET1_BIT18_PSL.VALUE=0x00000000
DRIVER.RTP.VAR.RTP_PORT_BIT1_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT3_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT1_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT5_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT14_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT11_DIR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT3_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT8_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT4_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT6_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT2_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT10_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT6_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT14_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT12_DIR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT17_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT4_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT10_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT2_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT5_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT3_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT11_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT7_DIR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT13_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT5_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT11_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT9_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT6_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT12_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT4_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT12_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT8_DIR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT10_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT15_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT14_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT18_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT6_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT0_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT4_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT12_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT3_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT7_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT5_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT13_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT9_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT11_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT15_DIR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT7_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT13_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT8_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT6_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT14_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT12_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT16_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT16_DIR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT17_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT8_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT1_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT10_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT14_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT4_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT9_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT7_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT15_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT9_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT13_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT10_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT17_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT2_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT9_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT15_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT8_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT16_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT14_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT18_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT17_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_BASE_PORT.VALUE=0xFFFFFA38
DRIVER.RTP.VAR.RTP_PORT_BIT2_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT16_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT5_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT9_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT17_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT15_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT15_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT11_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT17_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT7_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT18_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT0_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT16_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT18_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT3_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT18_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT6_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT17_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT12_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT13_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT18_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT4_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT5_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT7_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT10_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT13_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT18_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT5_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT11_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT8_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT0_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT11_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT14_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT3_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT1_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT6_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT0_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT9_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT2_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT12_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT16_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT15_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT0_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT0_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT1_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_BASE.VALUE=0xFFFFFA00
DRIVER.RTP.VAR.RTP_PORT_BIT3_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT8_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT1_PULDIS.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT1_PDR.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT7_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT2_FUN.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT0_PSL.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT4_DIR.VALUE=0
DRIVER.RTP.VAR.RTP_BASE_RAM.VALUE=0xFFF83000
DRIVER.RTP.VAR.RTP_PORT_BIT13_PULL.VALUE=2
DRIVER.RTP.VAR.RTP_PORT_BIT10_DIR.VALUE=1
DRIVER.RTP.VAR.RTP_PORT_BIT16_DOUT.VALUE=0
DRIVER.RTP.VAR.RTP_PORT_BIT2_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT14_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT17_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT17_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT4_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT1_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT18_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT0_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT15_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT4_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT2_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT7_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT15_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT18_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT0_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_BASE.VALUE=0xFFFFF700
DRIVER.DMM.VAR.DMM_PORT_BIT1_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT3_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT9_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT1_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT2_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT2_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT0_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT5_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT4_DIR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT8_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT16_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT2_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT13_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT3_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_BASE_PORT.VALUE=0xFFFFF770
DRIVER.DMM.VAR.DMM_PORT_BIT1_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT5_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT10_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT3_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT4_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT2_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT6_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT6_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT7_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT9_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT17_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT0_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT4_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT5_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT3_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT0_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT7_DIR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT18_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT11_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT11_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT5_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT6_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT4_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT8_DIR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT7_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT18_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT6_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT10_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT7_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT5_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT5_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT1_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT9_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT12_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT7_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT11_DIR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT8_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT16_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT6_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT8_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT10_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT8_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT12_DIR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT9_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT10_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT7_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT2_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT10_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT13_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT11_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT9_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT13_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT3_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT11_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT8_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT9_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT12_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT10_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT14_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT14_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT0_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT12_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT9_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT3_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT11_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT14_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT13_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT11_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT15_DIR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT13_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT8_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT14_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT1_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT12_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT16_DIR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT1_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT14_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT4_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT12_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT15_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT15_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT12_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT13_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT17_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT15_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT16_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT14_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT18_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT2_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT6_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT16_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT5_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT13_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT16_DOUT.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT17_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT15_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT17_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT17_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT10_PULDIS.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT18_FUN.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT16_PSL.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT3_PULL.VALUE=2
DRIVER.DMM.VAR.DMM_PORT_BIT0_DIR.VALUE=1
DRIVER.DMM.VAR.DMM_PORT_BIT18_PDR.VALUE=0
DRIVER.DMM.VAR.DMM_PORT_BIT6_DOUT.VALUE=0
DRIVER.I2C.VAR.I2C1_STOPBITS.VALUE=2
DRIVER.I2C.VAR.I2C1_PORT_BIT0_PULDIS.VALUE=0
DRIVER.I2C.VAR.I2C1_BASE_PORT.VALUE=0xFFF7D44C
DRIVER.I2C.VAR.I2C2_PARITYENA.VALUE=0
DRIVER.I2C.VAR.I2C1_DATACOUNT.VALUE=8
DRIVER.I2C.VAR.I2C2_PORT_BIT0_PULL.VALUE=2
DRIVER.I2C.VAR.I2C1_IGNACK.VALUE=0
DRIVER.I2C.VAR.I2C1_ADDRMODE.VALUE=7BIT_AMODE
DRIVER.I2C.VAR.I2C2_ALINTLVL.VALUE=0
DRIVER.I2C.VAR.I2C2_TXDMA.VALUE=0
DRIVER.I2C.VAR.I2C1_BC_VALUE.VALUE=0x0003
DRIVER.I2C.VAR.I2C1_TXRX_VALUE.VALUE=0
DRIVER.I2C.VAR.I2C2_ICXRDYINTLVL.VALUE=0
DRIVER.I2C.VAR.I2C2_MODCLK.VALUE=8
DRIVER.I2C.VAR.I2C2_PORT_BIT1_PULL.VALUE=2
DRIVER.I2C.VAR.I2C2_PORT_BIT0_DIR.VALUE=0
DRIVER.I2C.VAR.I2C1_ALINTENA.VALUE=0
DRIVER.I2C.VAR.I2C1_PRESCALE.VALUE=8
DRIVER.I2C.VAR.I2C2_ARDYINTENA.VALUE=0
DRIVER.I2C.VAR.I2C2_PORT_BIT1_DIR.VALUE=0
DRIVER.I2C.VAR.I2C2_PORT_BIT0_FUN.VALUE=0
DRIVER.I2C.VAR.I2C1_MSMODE.VALUE=1
DRIVER.I2C.VAR.I2C1_AASLVL.VALUE=0
DRIVER.I2C.VAR.I2C2_PORT_BIT0_PDR.VALUE=0
DRIVER.I2C.VAR.I2C2_RM_ENA.VALUE=0
DRIVER.I2C.VAR.I2C2_PORT_BIT1_FUN.VALUE=0
DRIVER.I2C.VAR.I2C2_PORT_BIT1_PULDIS.VALUE=0
DRIVER.I2C.VAR.I2C2_SCDLVL.VALUE=0
DRIVER.I2C.VAR.I2C2_PORT_BIT1_PDR.VALUE=0
DRIVER.I2C.VAR.I2C2_STPCND.VALUE=1
DRIVER.I2C.VAR.I2C1_ALINTLVL.VALUE=0
DRIVER.I2C.VAR.I2C2_PORT_BIT0_PSL.VALUE=1
DRIVER.I2C.VAR.I2C1_ARDYINTENA.VALUE=0
DRIVER.I2C.VAR.I2C2_ARDYINTLVL.VALUE=0
DRIVER.I2C.VAR.I2C1_ICRRDYINTENA.VALUE=0
DRIVER.I2C.VAR.I2C2_BASE_PORT.VALUE=0xFFF7D54C
DRIVER.I2C.VAR.I2C1_PORT_BIT1_PULDIS.VALUE=0
DRIVER.I2C.VAR.I2C2_PORT_BIT1_PSL.VALUE=1
DRIVER.I2C.VAR.I2C2_DATACOUNT.VALUE=8
DRIVER.I2C.VAR.I2C1_LENGTH.VALUE=8
DRIVER.I2C.VAR.I2C1_TXRX.VALUE=TRANSMITTER
DRIVER.I2C.VAR.I2C2_NACKINTENA.VALUE=0
DRIVER.I2C.VAR.I2C2_IGNACK.VALUE=0
DRIVER.I2C.VAR.I2C1_PORT_BIT0_DOUT.VALUE=0
DRIVER.I2C.VAR.I2C1_STACND.VALUE=1
DRIVER.I2C.VAR.I2C2_TXRX.VALUE=TRANSMITTER
DRIVER.I2C.VAR.I2C1_PORT_BIT0_DIR.VALUE=0
DRIVER.I2C.VAR.I2C1_ARDYINTLVL.VALUE=0
DRIVER.I2C.VAR.I2C1_ICRRDYINTLVL.VALUE=0
DRIVER.I2C.VAR.I2C1_PARITYENA.VALUE=0
DRIVER.I2C.VAR.I2C1_BASE.VALUE=0xFFF7D400
DRIVER.I2C.VAR.I2C1_PORT_BIT1_DIR.VALUE=0
DRIVER.I2C.VAR.I2C1_PORT_BIT1_DOUT.VALUE=0
DRIVER.I2C.VAR.I2C1_ICXRDYINTENA.VALUE=0
DRIVER.I2C.VAR.I2C1_PORT_BIT0_FUN.VALUE=0
DRIVER.I2C.VAR.I2C1_NACKINTENA.VALUE=0
DRIVER.I2C.VAR.I2C2_NACKINTLVL.VALUE=0
DRIVER.I2C.VAR.I2C2_BAUDRATE.VALUE=100
DRIVER.I2C.VAR.I2C1_AAS.VALUE=0
DRIVER.I2C.VAR.I2C1_BCM.VALUE=0
DRIVER.I2C.VAR.I2C1_PORT_BIT0_PDR.VALUE=0
DRIVER.I2C.VAR.I2C2_MSMODE.VALUE=1
DRIVER.I2C.VAR.I2C2_STOPBITS.VALUE=2
DRIVER.I2C.VAR.I2C1_BC.VALUE=8_BIT
DRIVER.I2C.VAR.I2C1_PORT_BIT1_FUN.VALUE=0
DRIVER.I2C.VAR.I2C2_EVENPARITY.VALUE=0
DRIVER.I2C.VAR.I2C2_ICRRDYINTENA.VALUE=0
DRIVER.I2C.VAR.I2C1_FDF.VALUE=0
DRIVER.I2C.VAR.I2C2_BASE.VALUE=0xFFF7D500
DRIVER.I2C.VAR.I2C2_AASLVL.VALUE=0
DRIVER.I2C.VAR.I2C2_AAS.VALUE=0
DRIVER.I2C.VAR.I2C1_ICCH.VALUE=37
DRIVER.I2C.VAR.I2C2_BCM.VALUE=0
DRIVER.I2C.VAR.I2C2_BC.VALUE=2_BIT
DRIVER.I2C.VAR.I2C1_MODCLK.VALUE=8
DRIVER.I2C.VAR.I2C1_ADDRMODE_VALUE.VALUE=0x0001
DRIVER.I2C.VAR.I2C2_PORT_BIT0_DOUT.VALUE=0
DRIVER.I2C.VAR.I2C1_ICCL.VALUE=37
DRIVER.I2C.VAR.I2C1_PORT_BIT1_PDR.VALUE=0
DRIVER.I2C.VAR.I2C2_ADDRMODE.VALUE=7BIT_AMODE
DRIVER.I2C.VAR.I2C2_FDF.VALUE=0
DRIVER.I2C.VAR.I2C1_PORT_BIT0_PSL.VALUE=1
DRIVER.I2C.VAR.I2C1_RXDMA.VALUE=0
DRIVER.I2C.VAR.I2C1_PORT_BIT1_PSL.VALUE=1
DRIVER.I2C.VAR.I2C2_BC_VALUE.VALUE=0x0003
DRIVER.I2C.VAR.I2C1_PORT_BIT0_PULL.VALUE=2
DRIVER.I2C.VAR.I2C1_ICXRDYINTLVL.VALUE=0
DRIVER.I2C.VAR.I2C2_ICCH.VALUE=37
DRIVER.I2C.VAR.I2C1_NACKINTLVL.VALUE=0
DRIVER.I2C.VAR.I2C2_ICCL.VALUE=37
DRIVER.I2C.VAR.I2C2_PORT_BIT1_DOUT.VALUE=0
DRIVER.I2C.VAR.I2C1_SCD.VALUE=0
DRIVER.I2C.VAR.I2C1_TXDMA.VALUE=0
DRIVER.I2C.VAR.I2C2_LENGTH.VALUE=8
DRIVER.I2C.VAR.I2C1_EVENPARITY.VALUE=0
DRIVER.I2C.VAR.I2C1_RM_ENA.VALUE=0
DRIVER.I2C.VAR.I2C2_ICRRDYINTLVL.VALUE=0
DRIVER.I2C.VAR.I2C2_ALINTENA.VALUE=0
DRIVER.I2C.VAR.I2C2_PRESCALE.VALUE=8
DRIVER.I2C.VAR.I2C2_PORT_BIT0_PULDIS.VALUE=0
DRIVER.I2C.VAR.I2C1_SCDLVL.VALUE=0
DRIVER.I2C.VAR.I2C2_SCD.VALUE=0
DRIVER.I2C.VAR.I2C1_PORT_BIT1_PULL.VALUE=2
DRIVER.I2C.VAR.I2C2_TXRX_VALUE.VALUE=0
DRIVER.I2C.VAR.I2C1_STPCND.VALUE=1
DRIVER.I2C.VAR.I2C2_ICXRDYINTENA.VALUE=0
DRIVER.I2C.VAR.I2C2_ADDRMODE_VALUE.VALUE=0x0001
DRIVER.I2C.VAR.I2C1_BAUDRATE.VALUE=100
DRIVER.I2C.VAR.I2C2_STACND.VALUE=1
DRIVER.I2C.VAR.I2C2_RXDMA.VALUE=0
DRIVER.DCC.VAR.DCC1_ENABLE_KEY.VALUE=10
DRIVER.DCC.VAR.PINMUX_BASE.VALUE=0xFFFFEA00
DRIVER.DCC.VAR.DCC1_DETECTION_TIME.VALUE=2500.00
DRIVER.DCC.VAR.DCC1_CLOCK_SOURCE1_VALUE.VALUE=0x0002
DRIVER.DCC.VAR.DCC1_ENABLE_ERROR_INTERRUPT.VALUE=0xA
DRIVER.DCC.VAR.DCC2_ENABLE.VALUE=0xA
DRIVER.DCC.VAR.PINMUX_BASE_PORT.VALUE=0xFFFFEA40
DRIVER.DCC.VAR.DCC2_ENABLE_ERROR_INTERRUPT.VALUE=0xA
DRIVER.DCC.VAR.DCC2_CLOCK_SOURCE0_VALUE.VALUE=0x0001
DRIVER.DCC.VAR.DCC2_CLOCK_SOURCE0_FREQ.VALUE=0
DRIVER.DCC.VAR.DCC2_VALID0_SEED.VALUE=0
DRIVER.DCC.VAR.DCC2_CLKT_N2HET2_0_FREQ.VALUE=1
DRIVER.DCC.VAR.DCC2_CLOCK_SOURCE1_FREQ.VALUE=0
DRIVER.DCC.VAR.DCC2_DETECTION_TIME.VALUE=2500.00
DRIVER.DCC.VAR.DCC2_CLOCK_DRIFT.VALUE=1.0
DRIVER.DCC.VAR.DCC2_CLOCK_SOURCE1_VALUE.VALUE=0x0002
DRIVER.DCC.VAR.DCC1_CLKT_N2HET1_31_FREQ.VALUE=1
DRIVER.DCC.VAR.DCC2_COUNT0_SEED.VALUE=0
DRIVER.DCC.VAR.DCC2_CLOCK_SOURCE0.VALUE=OSCIN
DRIVER.DCC.VAR.DCC2_CLOCK_SOURCE1.VALUE=VCLK
DRIVER.DCC.VAR.DCC1_CLOCK_SOURCE0_FREQ.VALUE=16.0
DRIVER.DCC.VAR.DCC1_VALID0_SEED.VALUE=792
DRIVER.DCC.VAR.DCC1_BASE.VALUE=0xFFFFEC00
DRIVER.DCC.VAR.DCC2_COUNT1_SEED.VALUE=0
DRIVER.DCC.VAR.DCC1_CLOCK_SOURCE1_FREQ.VALUE=300.0
DRIVER.DCC.VAR.DCC1_CLOCK_DRIFT.VALUE=1.0
DRIVER.DCC.VAR.DCC1_ENABLE.VALUE=0xA
DRIVER.DCC.VAR.DCC1_ENABLE_SINGLESHOT_MODE.VALUE=0x5
DRIVER.DCC.VAR.DCC2_ENABLE_SINGLESHOT_MODE.VALUE=0x5
DRIVER.DCC.VAR.DCC2_BASE.VALUE=0xFFFFF400
DRIVER.DCC.VAR.DCC1_DONE_INTERRUPT_ENABLE.VALUE=0xA
DRIVER.DCC.VAR.DCC2_DONE_INTERRUPT_ENABLE.VALUE=0xA
DRIVER.DCC.VAR.DCC2_ENABLE_KEY.VALUE=0xA
DRIVER.DCC.VAR.DCC1_COUNT0_SEED.VALUE=39204
DRIVER.DCC.VAR.DCC1_CLOCK_SOURCE0_VALUE.VALUE=0x0001
DRIVER.DCC.VAR.DCC1_CLOCK_SOURCE0.VALUE=OSCIN
DRIVER.DCC.VAR.DCC1_CLOCK_SOURCE1.VALUE=PLL1
DRIVER.DCC.VAR.CLKT_TCK_FREQ.VALUE=12.0
DRIVER.DCC.VAR.DCC1_COUNT1_SEED.VALUE=742500
DRIVER.PINMUX.VAR.EQEP2A_FILTER.VALUE=0
DRIVER.PINMUX.VAR.MUX61_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX53_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX45_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX37_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX29_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX7_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX61_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX53_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX45_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX37_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX29_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX7_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_SOC4A_SELECT.VALUE=ON
DRIVER.PINMUX.VAR.ETPWM_TIME_BASE_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX61_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX53_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX50_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX45_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX42_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX37_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX34_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX29_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX26_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX18_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX61_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX53_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX45_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX37_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX29_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX61_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX53_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX45_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX37_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX29_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX61_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX53_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX45_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX37_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX29_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX99_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_96_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_88_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_5_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX30_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX22_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX14_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX30_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX22_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX14_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX30_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX22_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX14_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_81_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_73_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_65_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_57_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_49_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX30_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX22_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX14_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL5_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX30_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX22_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX14_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL5_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX30_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX22_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX14_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX101_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL55_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL47_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL39_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_50_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_42_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_34_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_26_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_18_SELECT.VALUE=0
DRIVER.PINMUX.VAR.ECAP5_FILTER.VALUE=0
DRIVER.PINMUX.VAR.EMIF_OUTPUT_ENABLE_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.PINMUX10.VALUE="PINMUX_BALL_K17_EMIF_nCS_3 | PINMUX_BALL_M17_EMIF_nCS_4 | PINMUX_BALL_R3_EMIF_nRAS | PINMUX_BALL_P3_EMIF_nWAIT"
DRIVER.PINMUX.VAR.MUX11_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL40_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL32_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL24_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL16_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_11_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PINMUX11.VALUE="PINMUX_BALL_D17_EMIF_nWE | PINMUX_BALL_E9_ETMDATA_08 | PINMUX_BALL_E8_ETMDATA_09 | PINMUX_BALL_E7_ETMDATA_10"
DRIVER.PINMUX.VAR.PINMUX20.VALUE="PINMUX_BALL_M1_GIOA_7 | PINMUX_BALL_F2_GIOB_2 | PINMUX_BALL_W10_GIOB_3 | PINMUX_BALL_J2_GIOB_6"
DRIVER.PINMUX.VAR.PINMUX12.VALUE="PINMUX_BALL_E6_ETMDATA_11 | PINMUX_BALL_E13_ETMDATA_12 | PINMUX_BALL_E12_ETMDATA_13 | PINMUX_BALL_E11_ETMDATA_14"
DRIVER.PINMUX.VAR.PINMUX21.VALUE="PINMUX_BALL_F1_GIOB_7 | PINMUX_BALL_R2_MIBSPI1NCS_0 | PINMUX_BALL_F3_MIBSPI1NCS_1 | PINMUX_BALL_G3_MIBSPI1NCS_2"
DRIVER.PINMUX.VAR.PINMUX13.VALUE="PINMUX_BALL_E10_ETMDATA_15 | PINMUX_BALL_K15_ETMDATA_16 | PINMUX_BALL_L15_ETMDATA_17 | PINMUX_BALL_M15_ETMDATA_18"
DRIVER.PINMUX.VAR.ECAP3_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.PINMUX30.VALUE="PINMUX_BALL_E18_N2HET1_08 | PINMUX_BALL_V7_N2HET1_09 | PINMUX_BALL_D19_N2HET1_10 | PINMUX_BALL_E3_N2HET1_11"
DRIVER.PINMUX.VAR.PINMUX22.VALUE="PINMUX_BALL_J3_MIBSPI1NCS_3 | PINMUX_BALL_G19_MIBSPI1NENA | PINMUX_BALL_V9_MIBSPI3CLK | PINMUX_BALL_V10_MIBSPI3NCS_0"
DRIVER.PINMUX.VAR.PINMUX14.VALUE="PINMUX_BALL_N15_ETMDATA_19 | PINMUX_BALL_E5_ETMDATA_20 | PINMUX_BALL_F5_ETMDATA_21 | PINMUX_BALL_G5_ETMDATA_22"
DRIVER.PINMUX.VAR.MUX92_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX84_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX76_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX68_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PINMUX31.VALUE="PINMUX_BALL_B4_N2HET1_12 | PINMUX_BALL_N2_SCI3TX | PINMUX_BALL_N1_N2HET1_15 | PINMUX_BALL_A4_N2HET1_16"
DRIVER.PINMUX.VAR.PINMUX23.VALUE="PINMUX_BALL_V5_MIBSPI3NCS_1 | PINMUX_BALL_B2_MIBSPI3NCS_2 | PINMUX_BALL_C3_MIBSPI3NCS_3 | PINMUX_BALL_W9_MIBSPI3NENA"
DRIVER.PINMUX.VAR.PINMUX15.VALUE="PINMUX_BALL_K5_ETMDATA_23 | PINMUX_BALL_L5_ETMDATA_24 | PINMUX_BALL_M5_ETMDATA_25 | PINMUX_BALL_N5_ETMDATA_26"
DRIVER.PINMUX.VAR.PINMUX32.VALUE="PINMUX_BALL_A13_SCI4RX | PINMUX_BALL_J1_N2HET1_18 | PINMUX_BALL_B13_SCI4TX | PINMUX_BALL_P2_N2HET1_20"
DRIVER.PINMUX.VAR.PINMUX24.VALUE="PINMUX_BALL_W8_MIBSPI3SIMO | PINMUX_BALL_V8_MIBSPI3SOMI | PINMUX_BALL_H19_MIBSPI5CLK | PINMUX_BALL_E19_MIBSPI5NCS_0"
DRIVER.PINMUX.VAR.PINMUX16.VALUE="PINMUX_BALL_P5_ETMDATA_27 | PINMUX_BALL_R5_ETMDATA_28 | PINMUX_BALL_R6_ETMDATA_29 | PINMUX_BALL_R7_ETMDATA_30"
DRIVER.PINMUX.VAR.SIGNAL56_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL48_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX131_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX123_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX115_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX107_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.PINMUX33.VALUE="PINMUX_BALL_H4_N2HET1_21 | PINMUX_BALL_B3_N2HET1_22 | PINMUX_BALL_J4_N2HET1_23 | PINMUX_BALL_P1_N2HET1_24"
DRIVER.PINMUX.VAR.PINMUX25.VALUE="PINMUX_BALL_B6_MIBSPI5NCS_1 | PINMUX_BALL_W6_MIBSPI5NCS_2 | PINMUX_BALL_T12_MIBSPI5NCS_3 | PINMUX_BALL_H18_MIBSPI5NENA"
DRIVER.PINMUX.VAR.PINMUX17.VALUE="PINMUX_BALL_R8_ETMDATA_31 | PINMUX_BALL_R9_ETMTRACECLKIN | PINMUX_BALL_R10_ETMTRACECLKOUT | PINMUX_BALL_R11_ETMTRACECTL"
DRIVER.PINMUX.VAR.SIGNAL56_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL48_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX131_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX123_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX115_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX107_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.GIOB6_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.EQEP2B_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.ETPWM7_EQEPERR_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.PINMUX34.VALUE="PINMUX_BALL_A14_N2HET1_26 | PINMUX_BALL_K19_N2HET1_28 | PINMUX_BALL_B11_N2HET1_30 | PINMUX_BALL_D8_N2HET2_01"
DRIVER.PINMUX.VAR.PINMUX26.VALUE="PINMUX_BALL_J19_MIBSPI5SIMO_0 | PINMUX_BALL_E16_MIBSPI5SIMO_1 | PINMUX_BALL_H17_MIBSPI5SIMO_2 | PINMUX_BALL_G17_MIBSPI5SIMO_3"
DRIVER.PINMUX.VAR.PINMUX18.VALUE="PINMUX_BALL_B15_FRAYTX1 | PINMUX_BALL_B8_FRAYTX2 | PINMUX_BALL_B16_FRAYTXEN1 | PINMUX_BALL_B9_FRAYTXEN2"
DRIVER.PINMUX.VAR.MUX131_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX123_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX115_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX107_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.PINMUX35.VALUE="PINMUX_BALL_D7_N2HET2_02 | PINMUX_BALL_D3_N2HET2_12 | PINMUX_BALL_D2_N2HET2_13 | PINMUX_BALL_D1_N2HET2_14"
DRIVER.PINMUX.VAR.PINMUX27.VALUE="PINMUX_BALL_J18_MIBSPI5SOMI_0 | PINMUX_BALL_E17_MIBSPI5SOMI_1 | PINMUX_BALL_H16_MIBSPI5SOMI_2 | PINMUX_BALL_G16_MIBSPI5SOMI_3"
DRIVER.PINMUX.VAR.PINMUX19.VALUE="PINMUX_BALL_C1_GIOA_2 | PINMUX_BALL_E1_GIOA_3 | PINMUX_BALL_B5_GIOA_5 | PINMUX_BALL_H3_GIOA_6"
DRIVER.PINMUX.VAR.MUX131_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX123_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX115_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX107_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.PINMUX36.VALUE="PINMUX_BALL_P4_N2HET2_19 | PINMUX_BALL_T5_N2HET2_20 | PINMUX_BALL_T4_MII_RXCLK | PINMUX_BALL_U7_MII_TX_CLK"
DRIVER.PINMUX.VAR.PINMUX28.VALUE="PINMUX_BALL_K18_N2HET1_00 | PINMUX_BALL_V2_N2HET1_01 | PINMUX_BALL_W5_N2HET1_02 | PINMUX_BALL_U1_N2HET1_03"
DRIVER.PINMUX.VAR.MUX131_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX123_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX115_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX107_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX98_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.PINMUX37.VALUE="PINMUX_BALL_E2_N2HET2_03 | PINMUX_BALL_N3_N2HET2_07"
DRIVER.PINMUX.VAR.PINMUX29.VALUE="PINMUX_BALL_B12_N2HET1_04 | PINMUX_BALL_V6_N2HET1_05 | PINMUX_BALL_W3_SCI3RX | PINMUX_BALL_T1_N2HET1_07"
DRIVER.PINMUX.VAR.MUX131_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX123_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX115_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX107_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX98_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX98_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX7_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL3_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX98_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.PINMUX80.VALUE=SIGNAL_AD2EVT_T10
DRIVER.PINMUX.VAR.SIGNAL41_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL33_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL25_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL17_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX100_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX98_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.TEMP2_ENABLE.VALUE=0
DRIVER.PINMUX.VAR.PINMUX81.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL41_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL33_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL25_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL17_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX100_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX98_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.PINMUX90.VALUE="SIGNAL_MII_RX_DV_U6 | SIGNAL_MII_RX_ER_U5 | SIGNAL_MII_RXCLK_T4 | SIGNAL_MII_RXD_0_U4"
DRIVER.PINMUX.VAR.PINMUX82.VALUE=0
DRIVER.PINMUX.VAR.MUX127_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX119_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX100_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_133_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_125_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_117_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_109_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PINMUX91.VALUE="SIGNAL_MII_RXD_1_T3 | SIGNAL_MII_RXD_2_U3 | SIGNAL_MII_RXD_3_V3 | SIGNAL_MII_TX_CLK_U7"
DRIVER.PINMUX.VAR.PINMUX83.VALUE=SIGNAL_GIOA_0_A5
DRIVER.PINMUX.VAR.MUX100_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.PINMUX92.VALUE="SIGNAL_N2HET1_17_A13 | SIGNAL_N2HET1_19_B13 | SIGNAL_N2HET1_21_H4 | SIGNAL_N2HET1_23_J4"
DRIVER.PINMUX.VAR.PINMUX84.VALUE="SIGNAL_GIOA_1_C2 | SIGNAL_GIOA_2_C1 | SIGNAL_GIOA_3_E1 | SIGNAL_GIOA_4_A6"
DRIVER.PINMUX.VAR.MUX100_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX91_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX83_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX75_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX67_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX59_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.PINMUX93.VALUE="SIGNAL_N2HET1_25_M3 | SIGNAL_N2HET1_27_A9 | SIGNAL_N2HET1_29_A3 | SIGNAL_N2HET1_31_J17"
DRIVER.PINMUX.VAR.PINMUX85.VALUE="SIGNAL_GIOA_5_B5 | SIGNAL_GIOA_6_H3 | SIGNAL_GIOA_7_M1 | SIGNAL_GIOB_0_M2"
DRIVER.PINMUX.VAR.MUX100_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX91_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX83_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX75_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX67_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX59_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.GIOB0_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.GIOA2_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.PINMUX94.VALUE="SIGNAL_N2HET2_00_D6 | SIGNAL_N2HET2_01_D8 | SIGNAL_N2HET2_02_D7 | SIGNAL_N2HET2_03_E2"
DRIVER.PINMUX.VAR.PINMUX86.VALUE="SIGNAL_GIOB_1_K2 | SIGNAL_GIOB_2_F2 | SIGNAL_GIOB_3_W10 | SIGNAL_GIOB_4_G1"
DRIVER.PINMUX.VAR.MUX91_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX83_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX75_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX67_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX61_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX59_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX53_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX45_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX37_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX29_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_110_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_102_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PINMUX95.VALUE="SIGNAL_N2HET2_04_D13 | SIGNAL_N2HET2_05_D12 | SIGNAL_N2HET2_06_D11 | SIGNAL_N2HET2_07_N3"
DRIVER.PINMUX.VAR.PINMUX87.VALUE="SIGNAL_GIOB_5_G2 | SIGNAL_GIOB_6_J2 | SIGNAL_GIOB_7_F1 | SIGNAL_MDIO_F4"
DRIVER.PINMUX.VAR.MUX91_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX83_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX75_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX67_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX59_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.ETPWM2_EQEPERR12.VALUE=EQEPERR12
DRIVER.PINMUX.VAR.PINMUX96.VALUE="SIGNAL_N2HET2_08_K16 | SIGNAL_N2HET2_09_L16 | SIGNAL_N2HET2_10_M16 | SIGNAL_N2HET2_11_N16"
DRIVER.PINMUX.VAR.PINMUX88.VALUE="SIGNAL_MIBSPI1NCS_4_U10 | SIGNAL_MIBSPI1NCS_5_U9"
DRIVER.PINMUX.VAR.SIGNAL10_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX91_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX83_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX75_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX67_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX59_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX6_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.PINMUX97.VALUE="SIGNAL_N2HET2_12_D3 | SIGNAL_N2HET2_13_D2 | SIGNAL_N2HET2_14_D1 | SIGNAL_N2HET2_15_K4"
DRIVER.PINMUX.VAR.PINMUX89.VALUE="SIGNAL_MII_COL_W4 | SIGNAL_MII_CRS_V4"
DRIVER.PINMUX.VAR.SIGNAL10_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX91_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX83_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX75_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX67_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX59_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX6_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.PINMUX98.VALUE="SIGNAL_N2HET2_16_L4 | SIGNAL_N2HET2_18_N4 | SIGNAL_N2HET2_20_T5 | SIGNAL_N2HET2_22_T7"
DRIVER.PINMUX.VAR.MUX6_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.PINMUX99.VALUE="SIGNAL_nTZ1_1_N19 | SIGNAL_nTZ1_2_F1 | SIGNAL_nTZ1_3_J3"
DRIVER.PINMUX.VAR.MUX6_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.EQEP1A_FILTER.VALUE=0
DRIVER.PINMUX.VAR.MUX60_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX52_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX44_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX36_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX28_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX6_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX60_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX52_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX44_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX36_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX28_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX6_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.EQEP1I_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.ETPWM_SOC3A_SELECT.VALUE=ON
DRIVER.PINMUX.VAR.MUX60_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX52_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX44_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX36_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX28_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX60_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX52_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX44_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX36_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX28_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX60_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX52_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX44_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX36_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX28_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX60_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX52_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX44_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX36_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX28_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.TEMP3_ENABLE_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX120_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX112_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX104_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_94_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_86_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_78_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_3_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX21_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX13_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX21_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX13_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.ETPWM3_EQEPERR_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.GIOA_DISABLE_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX30_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX22_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX21_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX14_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX13_OPTION2.VALUE=1
DRIVER.PINMUX.VAR.PIN_MUX_71_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_63_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_55_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_47_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_39_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX21_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX13_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL4_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX21_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX13_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL4_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX21_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX13_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX95_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX87_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX79_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL61_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL53_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL45_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL37_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL29_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_40_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_32_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_24_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_16_SELECT.VALUE=0
DRIVER.PINMUX.VAR.ECAP3_FILTER.VALUE=0
DRIVER.PINMUX.VAR.ETPWM7_EQEPERR12.VALUE=EQEPERR12
DRIVER.PINMUX.VAR.MUX129_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX129_OPTION1.VALUE=1
DRIVER.PINMUX.VAR.ETPWM_TBCLK_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX129_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL30_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL22_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL14_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX129_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX129_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX129_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.I2C1.VALUE=0
DRIVER.PINMUX.VAR.I2C2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL55_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL47_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL39_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX130_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX122_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX114_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX106_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL55_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL47_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL39_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX130_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX122_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX114_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX106_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX130_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX122_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX114_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX106_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL8_SELECT.VALUE=0
DRIVER.PINMUX.VAR.GATE_EMIF_CLK.VALUE=0
DRIVER.PINMUX.VAR.MUX130_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX122_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX114_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX106_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX130_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX122_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX114_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX106_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX97_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX89_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX130_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX122_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX114_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX106_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX97_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX89_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.EQEP1A_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX97_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX89_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX80_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX72_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX64_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX56_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX48_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL1_SELECT.VALUE=0
DRIVER.PINMUX.VAR.GIOA0_DMA.VALUE=0
DRIVER.PINMUX.VAR.MUX97_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX89_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL40_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL32_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL24_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL16_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX97_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX89_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL40_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL32_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL24_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL16_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX97_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX89_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.GIOB5_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.GIOA7_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.PIN_MUX_131_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_123_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_115_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_107_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX90_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX82_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX74_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX66_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX58_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX90_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX82_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX74_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX66_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX58_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX90_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX82_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX74_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX66_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX58_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX3_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_100_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX90_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX82_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX74_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX66_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX58_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX90_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX82_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX74_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX66_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX58_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX5_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX90_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX82_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX74_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX66_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX58_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX5_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.EQEP1S_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX131_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX123_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX115_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX107_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX5_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX5_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX51_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX43_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX35_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX27_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX19_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX5_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX51_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX43_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX35_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX27_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX19_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX5_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.GIOA1_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.ECAP5_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.ETPWM_SOC2A_SELECT.VALUE=ON
DRIVER.PINMUX.VAR.MUX51_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX43_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX41_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX35_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX33_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX27_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX25_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX19_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX17_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_99_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_8_SELECT.VALUE=0
DRIVER.PINMUX.VAR.GIOA1_DMA.VALUE=0
DRIVER.PINMUX.VAR.MUX51_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX43_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX35_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX27_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX19_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX51_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX43_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX35_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX27_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX19_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX51_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX43_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX35_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX27_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX19_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.ALT_ADC_SELECT.VALUE=1
DRIVER.PINMUX.VAR.MUX98_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_92_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_84_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_76_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_68_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_1_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX20_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX12_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX20_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX12_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX20_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX12_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL58_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_61_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_53_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_45_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_37_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_29_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX20_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX12_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL3_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX20_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX12_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL3_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX20_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX12_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX100_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL51_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL43_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL35_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL27_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL19_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_30_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_22_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_14_SELECT.VALUE=0
DRIVER.PINMUX.VAR.ECAP1_FILTER.VALUE=0
DRIVER.PINMUX.VAR.CAN4.VALUE=0
DRIVER.PINMUX.VAR.MUX128_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX128_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX128_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX10_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL20_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL12_SELECT.VALUE=0
DRIVER.PINMUX.VAR.GIOB0_DMA.VALUE=0
DRIVER.PINMUX.VAR.GIOA2_DMA.VALUE=0
DRIVER.PINMUX.VAR.MUX128_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX128_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX128_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.ETHERNET_SELECT.VALUE=MII
DRIVER.PINMUX.VAR.MUX91_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX83_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX75_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX67_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX59_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.ETPWM5_EQEPERR12.VALUE=EQEPERR12
DRIVER.PINMUX.VAR.CONCOUNT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL54_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL46_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL38_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX121_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX113_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX105_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL54_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL46_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL38_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX121_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX113_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX105_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.EQEP2I_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX121_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX113_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX105_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL6_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX121_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX113_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX105_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX121_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX113_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX105_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX96_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX88_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX121_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX113_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX105_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX96_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX88_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX96_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX88_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX6_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_128_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX96_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX88_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL31_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL23_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL15_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX96_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX88_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.TEMP_CHECK.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL31_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL23_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL15_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX96_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX88_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.ETPWM4_EQEPERR_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.GIOB_DISABLE_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX134_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX126_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX118_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_121_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_113_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_105_SELECT.VALUE=0
DRIVER.PINMUX.VAR.GIOB1_DMA.VALUE=0
DRIVER.PINMUX.VAR.GIOA3_DMA.VALUE=0
DRIVER.PINMUX.VAR.EQEP2I_FILTER.VALUE=0
DRIVER.PINMUX.VAR.MUX81_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX73_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX65_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX57_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX49_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX81_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX73_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX65_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX57_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX49_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_TZ2_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX81_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX73_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX65_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX60_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX57_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX52_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX49_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX44_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX36_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX28_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX81_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX73_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX65_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX57_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX49_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.EQEP2B_FILTER.VALUE=0
DRIVER.PINMUX.VAR.MUX81_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX73_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX65_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX57_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX49_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX4_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX81_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX73_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX65_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX57_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX49_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX4_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.GIOB4_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.GIOA6_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.ECAP.VALUE=0
DRIVER.PINMUX.VAR.MUX4_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX4_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX50_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX42_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX34_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX26_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX18_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX4_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX50_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX42_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX34_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX26_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX18_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX4_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_SOC1A_SELECT.VALUE=ON
DRIVER.PINMUX.VAR.MUX50_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX42_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX34_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX26_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX18_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_97_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_89_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_6_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX50_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX42_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX34_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX26_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX18_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL9_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX50_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX42_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX34_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX26_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX18_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL9_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX50_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX42_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX34_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX26_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX18_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.ECAP2_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX111_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX103_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_90_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_82_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_74_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_66_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_58_SELECT.VALUE=0
DRIVER.PINMUX.VAR.GIOB2_DMA.VALUE=0
DRIVER.PINMUX.VAR.GIOA4_DMA.VALUE=0
DRIVER.PINMUX.VAR.MUX11_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX11_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.GIOA0_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.EQEP2A_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX21_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX13_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX11_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL56_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL48_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_51_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_43_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_35_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_27_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_19_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX11_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.ECAP6_FILTER.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL2_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX11_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_TBCLK_SYNC_ENABLE.VALUE=0
DRIVER.PINMUX.VAR.AD1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL2_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX11_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.AD2.VALUE=0
DRIVER.PINMUX.VAR.MUX94_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX86_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX78_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL41_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL33_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL25_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL17_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_20_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_12_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX127_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX119_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX127_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX119_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX127_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX119_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL10_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX127_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX119_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX127_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX119_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX127_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX119_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.EQEP2S_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX9_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.GIOB3_DMA.VALUE=0
DRIVER.PINMUX.VAR.GIOA5_DMA.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL61_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL53_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL45_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL37_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL29_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX120_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX112_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX104_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL61_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL53_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL45_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL37_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL29_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX120_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX112_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX104_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX129_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX120_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX112_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX104_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL4_SELECT.VALUE=0
DRIVER.PINMUX.VAR.ALT_ADC.VALUE=0
DRIVER.PINMUX.VAR.I2C.VALUE=0
DRIVER.PINMUX.VAR.MUX120_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX112_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX104_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX120_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX112_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX104_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX95_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX87_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX79_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.TEMP3_ENABLE.VALUE=0
DRIVER.PINMUX.VAR.MUX120_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX112_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX104_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX95_OPTION1.VALUE=1
DRIVER.PINMUX.VAR.MUX87_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX79_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX95_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX87_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX79_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX71_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX63_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX55_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX47_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX39_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_134_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_126_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_118_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX95_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX87_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX79_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.ETPWM3_EQEPERR12.VALUE=EQEPERR12
DRIVER.PINMUX.VAR.SIGNAL30_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL22_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL14_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX95_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX87_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX79_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL30_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL22_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL14_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX95_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX87_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX79_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.TEMP2_ENABLE_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.PIN_MUX_111_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_103_SELECT.VALUE=0
DRIVER.PINMUX.VAR.EQEP1I_FILTER.VALUE=0
DRIVER.PINMUX.VAR.MUX80_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX72_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX64_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX56_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX48_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.HET1.VALUE=0
DRIVER.PINMUX.VAR.MUX80_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX72_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX64_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX56_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX48_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_SOC7A_SELECT.VALUE=ON
DRIVER.PINMUX.VAR.HET2.VALUE=0
DRIVER.PINMUX.VAR.MUX80_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX72_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX64_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX56_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX48_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX2_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.GIOB4_DMA.VALUE=0
DRIVER.PINMUX.VAR.GIOA6_DMA.VALUE=0
DRIVER.PINMUX.VAR.MUX80_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX72_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX64_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX56_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX48_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.EQEP1B_FILTER.VALUE=0
DRIVER.PINMUX.VAR.MUX80_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX72_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX64_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX56_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX48_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX3_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX80_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX72_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX64_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX56_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX48_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX3_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX130_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX122_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX114_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX106_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX3_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX3_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.EMIF.VALUE=0
DRIVER.PINMUX.VAR.MUX41_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX33_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX25_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX17_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX3_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_TZ1.VALUE=ASYNC
DRIVER.PINMUX.VAR.MUX41_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX33_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX25_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX17_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX3_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_TZ2.VALUE=ASYNC
DRIVER.PINMUX.VAR.MUX41_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX40_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX33_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX32_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX25_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX24_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX17_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX16_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_95_SELECT.VALUE=1
DRIVER.PINMUX.VAR.PIN_MUX_87_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_79_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_4_SELECT.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_TZ3.VALUE=ASYNC
DRIVER.PINMUX.VAR.MUX41_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX33_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX25_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX17_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL8_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX41_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX33_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX25_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX17_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL8_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX41_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX33_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX25_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX17_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.GIOB3_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.GIOA5_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX97_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX89_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_80_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_72_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_64_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_56_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_48_SELECT.VALUE=0
DRIVER.PINMUX.VAR.GIOA.VALUE=0
DRIVER.PINMUX.VAR.GIOB.VALUE=0
DRIVER.PINMUX.VAR.MUX10_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.GIOB_DISABLE.VALUE=0
DRIVER.PINMUX.VAR.MUX10_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX10_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL54_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL46_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL38_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_41_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_33_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_25_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_17_SELECT.VALUE=0
DRIVER.PINMUX.VAR.GIOB5_DMA.VALUE=0
DRIVER.PINMUX.VAR.GIOA7_DMA.VALUE=0
DRIVER.PINMUX.VAR.MUX10_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.ECAP4_FILTER.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL1_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX10_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL1_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX10_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.ETPWM5_EQEPERR_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.SIGNAL31_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL23_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL15_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_10_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL59_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX134_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX126_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX118_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL59_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX134_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX126_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX118_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.EQEP.VALUE=0
DRIVER.PINMUX.VAR.MUX134_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX126_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX118_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX134_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX126_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX118_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX134_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX126_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX118_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX134_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX126_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX118_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX90_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX82_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX74_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX66_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX58_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL9_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MIBSPI1.VALUE=0
DRIVER.PINMUX.VAR.MIBSPI2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL60_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL52_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL44_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL36_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL28_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX111_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX103_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MIBSPI3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL60_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL52_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL44_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL36_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL28_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX111_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX103_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MIBSPI4.VALUE=0
DRIVER.PINMUX.VAR.OHCI0.VALUE=0
DRIVER.PINMUX.VAR.MUX111_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX103_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL2_SELECT.VALUE=0
DRIVER.PINMUX.VAR.GIOB6_DMA.VALUE=0
DRIVER.PINMUX.VAR.MIBSPI5.VALUE=0
DRIVER.PINMUX.VAR.W2FC.VALUE=0
DRIVER.PINMUX.VAR.OHCI1.VALUE=0
DRIVER.PINMUX.VAR.MUX111_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX103_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.EQEP2S_FILTER.VALUE=0
DRIVER.PINMUX.VAR.MUX111_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX103_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX94_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX86_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX78_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.TEMP1_ENABLE.VALUE=0
DRIVER.PINMUX.VAR.MUX111_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX103_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX94_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX86_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX78_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.ECAP4_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX94_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX86_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX78_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX5_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_132_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_124_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_116_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_108_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX94_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX86_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX78_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL21_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL13_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX94_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX86_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX78_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX9_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL21_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL13_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX94_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX86_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX78_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX9_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX133_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX125_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX117_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX109_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX9_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_101_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX9_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX71_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX63_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX55_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX47_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX39_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX9_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX71_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX63_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX55_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX47_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX39_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX9_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_SOC6A_SELECT.VALUE=ON
DRIVER.PINMUX.VAR.MUX71_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX63_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX55_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX51_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX47_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX43_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX39_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX35_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX27_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX19_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX71_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX63_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX55_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX47_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX39_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.ETPWM1_EQEPERR12.VALUE=EQEPERR12
DRIVER.PINMUX.VAR.MUX71_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX63_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX55_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX47_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX39_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX2_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.EMIF_OUTPUT_ENABLE.VALUE=0
DRIVER.PINMUX.VAR.MUX71_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX63_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX55_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX47_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX39_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX2_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.ETPWM1_EQEPERR_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX2_OPTION2.VALUE=1
DRIVER.PINMUX.VAR.PIN_MUX_9_SELECT.VALUE=0
DRIVER.PINMUX.VAR.GIOB7_DMA.VALUE=0
DRIVER.PINMUX.VAR.MUX2_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX40_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX32_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX24_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX16_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX2_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX40_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX32_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX24_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX16_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX2_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_EPWM1SYNCI_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX40_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX32_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX24_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX16_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_93_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_85_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_77_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_69_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_2_SELECT.VALUE=2
DRIVER.PINMUX.VAR.MUX40_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX32_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX24_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX16_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL7_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX40_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX32_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX24_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX16_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL7_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX40_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX32_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX24_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX16_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX110_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX102_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL59_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_70_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_62_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_54_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_46_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_38_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MII.VALUE=0
DRIVER.PINMUX.VAR.SCI2.VALUE=0
DRIVER.PINMUX.VAR.GIOA_DISABLE.VALUE=0
DRIVER.PINMUX.VAR.SCI3.VALUE=1
DRIVER.PINMUX.VAR.GATE_EMIF_CLK_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.SCI4.VALUE=1
DRIVER.PINMUX.VAR.MUX20_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX12_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL60_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL52_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL44_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL36_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL28_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_31_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_23_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_15_SELECT.VALUE=0
DRIVER.PINMUX.VAR.ECAP2_FILTER.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_TIME_BASE_SYNC_ENABLE.VALUE=0
DRIVER.PINMUX.VAR.GIOB2_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.GIOA4_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX93_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX85_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX77_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX69_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL21_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL13_SELECT.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_EPWM1SYNCI.VALUE=ASYNC
DRIVER.PINMUX.VAR.ETPWM6_EQEPERR12.VALUE=EQEPERR12
DRIVER.PINMUX.VAR.SIGNAL58_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX133_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX125_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX117_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX109_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL58_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX133_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX125_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX117_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX109_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX133_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX125_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX117_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX109_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_SOC1A.VALUE=1
DRIVER.PINMUX.VAR.SCI.VALUE=0
DRIVER.PINMUX.VAR.MUX133_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX125_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX117_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX109_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX133_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX125_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX117_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX109_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_SOC2A.VALUE=1
DRIVER.PINMUX.VAR.MUX133_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX125_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX117_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX109_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX8_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL7_SELECT.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_SOC3A.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL51_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL43_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL35_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL27_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL19_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX110_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX102_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_SOC4A.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL51_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL43_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL35_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL27_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL19_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX110_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX102_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX128_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX110_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX102_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_129_SELECT.VALUE=1
DRIVER.PINMUX.VAR.ETPWM_SOC5A.VALUE=1
DRIVER.PINMUX.VAR.ETPWM.VALUE=0
DRIVER.PINMUX.VAR.MUX110_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX102_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.EQEP1S_FILTER.VALUE=0
DRIVER.PINMUX.VAR.MUX110_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX102_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX93_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX85_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX77_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX69_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_SOC6A.VALUE=1
DRIVER.PINMUX.VAR.MUX110_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX102_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX93_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX85_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX77_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX69_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX93_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX85_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX77_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX70_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX69_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX62_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX54_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX46_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX38_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_130_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_122_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_114_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_106_SELECT.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_SOC7A.VALUE=1
DRIVER.PINMUX.VAR.MUX93_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX85_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX77_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX69_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL20_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL12_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX93_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX85_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX77_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX69_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX8_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL20_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL12_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX93_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX85_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX77_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX69_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX8_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.ECAP1_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.ETPWM_TZ3_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX8_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX8_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX70_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX62_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX54_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX46_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX38_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX8_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX70_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX62_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX54_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX46_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX38_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX8_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.EQEP1B_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.ETPWM_SOC5A_SELECT.VALUE=ON
DRIVER.PINMUX.VAR.ETPWM6_EQEPERR_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX70_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX62_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX54_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX46_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX38_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX1_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX70_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX62_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX54_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX46_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX38_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX70_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX62_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX54_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX46_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX38_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX1_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX70_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX62_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX54_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX46_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX38_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX1_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX121_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX113_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX105_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX1_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_98_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_7_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX1_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX31_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX23_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX15_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX1_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX31_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX23_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX15_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX1_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX31_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX31_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX23_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX23_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX15_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX15_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_91_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_83_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_75_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_67_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_59_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX31_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX23_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX15_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL6_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX31_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX23_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX15_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL6_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX31_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX23_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX15_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX96_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX88_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL57_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL49_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_60_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_52_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_44_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_36_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_28_SELECT.VALUE=0
DRIVER.PINMUX.VAR.GIOB7_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.ECAP6_FILTER_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.SIGNAL50_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL42_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL34_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL26_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL18_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_21_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_13_SELECT.VALUE=2
DRIVER.PINMUX.VAR.SIGNAL11_SELECT.VALUE=0
DRIVER.PINMUX.VAR.SPI2.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL57_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL49_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX132_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX124_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX116_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX108_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL57_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL49_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX132_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX124_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX116_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX108_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.TEMP1_ENABLE_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.SPI4.VALUE=0
DRIVER.PINMUX.VAR.MUX132_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX124_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX116_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX108_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.RMII.VALUE=0
DRIVER.PINMUX.VAR.MUX132_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX124_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX116_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX108_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.PINMUX0.VALUE="PINMUX_BALL_N19_AD1EVT | PINMUX_BALL_D4_EMIF_ADDR_00 | PINMUX_BALL_D5_EMIF_ADDR_01 | PINMUX_BALL_C4_EMIF_ADDR_06"
DRIVER.PINMUX.VAR.MUX132_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX124_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX116_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX108_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX99_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.PINMUX1.VALUE="PINMUX_BALL_C5_EMIF_ADDR_07 | PINMUX_BALL_C6_EMIF_ADDR_08 | PINMUX_BALL_C7_EMIF_ADDR_09 | PINMUX_BALL_C8_EMIF_ADDR_10"
DRIVER.PINMUX.VAR.MUX132_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX124_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX116_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX108_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX99_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.GIOB1_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.GIOA3_DMA_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.ETPWM2_EQEPERR_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.PINMUX2.VALUE="PINMUX_BALL_C9_EMIF_ADDR_11 | PINMUX_BALL_C10_EMIF_ADDR_12 | PINMUX_BALL_C11_EMIF_ADDR_13 | PINMUX_BALL_C12_EMIF_ADDR_14"
DRIVER.PINMUX.VAR.MUX99_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX81_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX73_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX65_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX57_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX49_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL5_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PINMUX3.VALUE="PINMUX_BALL_C13_EMIF_ADDR_15 | PINMUX_BALL_D14_EMIF_ADDR_16 | PINMUX_BALL_C14_EMIF_ADDR_17 | PINMUX_BALL_D15_EMIF_ADDR_18"
DRIVER.PINMUX.VAR.MUX99_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.ETPWM4_EQEPERR12.VALUE=EQEPERR12
DRIVER.PINMUX.VAR.PINMUX4.VALUE="PINMUX_BALL_C15_EMIF_ADDR_19 | PINMUX_BALL_C16_EMIF_ADDR_20 | PINMUX_BALL_C17_EMIF_ADDR_21"
DRIVER.PINMUX.VAR.SIGNAL50_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL42_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL34_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL26_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.SIGNAL18_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX101_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX99_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.PINMUX5.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL50_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL42_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL34_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL26_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL18_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX101_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX99_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.PINMUX6.VALUE=0
DRIVER.PINMUX.VAR.MUX101_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_127_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_119_SELECT.VALUE=0
DRIVER.PINMUX.VAR.ALT_ADC_A.VALUE=0
DRIVER.PINMUX.VAR.PINMUX7.VALUE=0
DRIVER.PINMUX.VAR.MUX101_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.ALT_ADC_B.VALUE=0
DRIVER.PINMUX.VAR.PINMUX8.VALUE=PINMUX_BALL_D16_EMIF_BA_1
DRIVER.PINMUX.VAR.MUX101_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX92_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX84_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX76_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.MUX68_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.PINMUX9.VALUE="PINMUX_BALL_R4_EMIF_nCAS | PINMUX_BALL_N17_EMIF_nCS_0 | PINMUX_BALL_L17_EMIF_nCS_2"
DRIVER.PINMUX.VAR.MUX101_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX92_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX84_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX76_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX68_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX92_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX84_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX76_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX68_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX4_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_120_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_112_SELECT.VALUE=0
DRIVER.PINMUX.VAR.PIN_MUX_104_SELECT.VALUE=0
DRIVER.PINMUX.VAR.MUX92_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX84_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX76_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.MUX68_OPTION3.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL11_OPTION0.VALUE=1
DRIVER.PINMUX.VAR.MUX92_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX84_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX76_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX68_OPTION4.VALUE=0
DRIVER.PINMUX.VAR.MUX7_OPTION0.VALUE=0
DRIVER.PINMUX.VAR.SIGNAL11_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.MUX92_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX84_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX76_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX68_OPTION5.VALUE=0
DRIVER.PINMUX.VAR.MUX7_OPTION1.VALUE=0
DRIVER.PINMUX.VAR.ETPWM_TZ1_SELECT.VALUE=OFF
DRIVER.PINMUX.VAR.MUX132_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX124_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX116_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX108_CONFLICT.VALUE=0
DRIVER.PINMUX.VAR.MUX7_OPTION2.VALUE=0
DRIVER.PINMUX.VAR.MUX7_OPTION3.VALUE=0
DRIVER.CRC.VAR.HTU_CPB_7_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC1_CH1_URI.VALUE=0x00000000
DRIVER.CRC.VAR.CRC1_CH2_TOE.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_DCP0_TRDIR_1.VALUE=HET_TO_MAIN_MEM
DRIVER.CRC.VAR.CRC2_CH2_WDTO.VALUE=0
DRIVER.CRC.VAR.HTU_ICPBL_7_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.HTU_ICPA_5_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_ICPB_1_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_DEBMOD_1.VALUE=0
DRIVER.CRC.VAR.CRC1_CH2_URI.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_ICPAL_1_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.HTU_ENABUS_1.VALUE=0
DRIVER.CRC.VAR.CRC1_CH2_MODE.VALUE=FULL_CPU
DRIVER.CRC.VAR.HTU_CPA_2_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC2_CH1_PSSIH.VALUE=0
DRIVER.CRC.VAR.CRC2_CH1_PSSIL.VALUE=0
DRIVER.CRC.VAR.HTU_MP1_ACC_1.VALUE=READ_ONLY
DRIVER.CRC.VAR.HTU_CONTPAR_1.VALUE=0
DRIVER.CRC.VAR.HTU_ICPB_6_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_DCP0_EC_1.VALUE=0
DRIVER.CRC.VAR.HTU_DCP0_CPBFULADD_1.VALUE=0
DRIVER.CRC.VAR.HTU_ICPAL_6_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.CRC1_CH1_PSIH.VALUE=0
DRIVER.CRC.VAR.HTU_CPA_7_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_CPB_3_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC1_BASE.VALUE=0xFE000000
DRIVER.CRC.VAR.CRC1_CH1_PSIL.VALUE=0
DRIVER.CRC.VAR.HTU_DCP0_FC_1.VALUE=0
DRIVER.CRC.VAR.HTU_BASE.VALUE=0xFFF7A400
DRIVER.CRC.VAR.HTU_ICPBL_3_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.HTU_ICPA_1_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC1_CH1_WDTO.VALUE=0x00000000
DRIVER.CRC.VAR.CRC1_CH2_PSIH.VALUE=0
DRIVER.CRC.VAR.CRC2_BASE.VALUE=0xFB000000
DRIVER.CRC.VAR.CRC1_CH2_PSIL.VALUE=0
DRIVER.CRC.VAR.HTU_ICPA_6_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_ICPB_2_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_DCP0_CPAFULADD_1.VALUE=0
DRIVER.CRC.VAR.HTU_ICPAL_2_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.HTU_CPA_3_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC2_CH2_PSSIH.VALUE=0
DRIVER.CRC.VAR.CRC2_CH2_PSSIL.VALUE=0
DRIVER.CRC.VAR.HTU_MP1_STADD_1.VALUE=0
DRIVER.CRC.VAR.HTU_ICPB_7_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC1_CH2_WDTO.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_ICPAL_7_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.HTU_CPB_4_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC2_CH1_BCTO.VALUE=0
DRIVER.CRC.VAR.HTU_MP0_ENA_1.VALUE=0
DRIVER.CRC.VAR.HTU_ICPBL_4_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.HTU_ICPA_2_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_PAR_1.VALUE=0
DRIVER.CRC.VAR.HTU_CONT_1.VALUE=0
DRIVER.CRC.VAR.HTU_ENAREQ_1.VALUE=0
DRIVER.CRC.VAR.CRC2_CH2_BCTO.VALUE=0
DRIVER.CRC.VAR.HTU_MP1_ERRENA_1.VALUE=0
DRIVER.CRC.VAR.HTU_MP0_STADD_1.VALUE=0
DRIVER.CRC.VAR.HTU_ICPA_7_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_ICPB_3_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_ICPAL_3_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.HTU_CPA_4_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_CPB_0_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_DCP0_MMADD_1.VALUE=POST_INCREMENT
DRIVER.CRC.VAR.CRC2_CH1_CCI.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_ENAINTMAP_1.VALUE=0
DRIVER.CRC.VAR.CRC2_CH1_CFI.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_ICPBL_0_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.HTU_CPB_5_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC2_CH2_CCI.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_MP1_ENA_1.VALUE=0
DRIVER.CRC.VAR.CRC1_CH2_MODE_VALUE.VALUE=0x0001
DRIVER.CRC.VAR.HTU_DCP0_HETADD.VALUE=0
DRIVER.CRC.VAR.CRC2_CH2_CFI.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_ICPBL_5_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.HTU_ICPA_3_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC2_CH1_DTE.VALUE=0
DRIVER.CRC.VAR.CRC2_CH1_CVH.VALUE=0
DRIVER.CRC.VAR.HTU_CPA_0_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_RES_1.VALUE=0
DRIVER.CRC.VAR.CRC1_CH1_BCTO.VALUE=0x00000000
DRIVER.CRC.VAR.CRC2_CH1_CVL.VALUE=0
DRIVER.CRC.VAR.HTU_DCP0_CPATMOD_1.VALUE=POST_INCREMENT
DRIVER.CRC.VAR.CRC1_CH1_CCI.VALUE=0x00000000
DRIVER.CRC.VAR.CRC2_CH1_MODE.VALUE=FULL_CPU
DRIVER.CRC.VAR.CRC1_CH1_PSSIH.VALUE=0
DRIVER.CRC.VAR.CRC2_CH2_DTE.VALUE=1
DRIVER.CRC.VAR.CRC1_CH1_CFI.VALUE=0x00000000
DRIVER.CRC.VAR.CRC1_CH1_PSSIL.VALUE=0
DRIVER.CRC.VAR.HTU_MP1_ENDADD_1.VALUE=0
DRIVER.CRC.VAR.HTU_ICPB_4_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC2_CH2_CVH.VALUE=0
DRIVER.CRC.VAR.HTU_ICPAL_4_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.CRC2_CH2_CVL.VALUE=0
DRIVER.CRC.VAR.CRC2_CH1_PCP.VALUE=0
DRIVER.CRC.VAR.HTU_CPA_5_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_CPB_1_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC1_CH2_CCI.VALUE=0x00000000
DRIVER.CRC.VAR.CRC1_CH2_CFI.VALUE=0x00000000
DRIVER.CRC.VAR.CRC2_CH1_SCP.VALUE=0
DRIVER.CRC.VAR.HTU_VBHOLD_1.VALUE=0
DRIVER.CRC.VAR.CRC1_CH2_BCTO.VALUE=0x00000000
DRIVER.CRC.VAR.CRC1_CH1_MODE_VALUE.VALUE=0x0001
DRIVER.CRC.VAR.CRC2_CH2_PCP.VALUE=0
DRIVER.CRC.VAR.HTU_MP0_ERRENA_1.VALUE=0
DRIVER.CRC.VAR.HTU_ICPBL_1_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.CRC2_CH1_PSA.VALUE=1
DRIVER.CRC.VAR.CRC2_CH2_MODE.VALUE=FULL_CPU
DRIVER.CRC.VAR.CRC2_CH1_ORI.VALUE=0x00000000
DRIVER.CRC.VAR.CRC1_CH1_DTE.VALUE=0
DRIVER.CRC.VAR.HTU_CPB_6_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC1_CH1_CVH.VALUE=0x00000000
DRIVER.CRC.VAR.CRC1_CH1_CVL.VALUE=0x00000000
DRIVER.CRC.VAR.CRC2_CH2_SCP.VALUE=0
DRIVER.CRC.VAR.CRC2_CH2_MODE_VALUE.VALUE=0x0001
DRIVER.CRC.VAR.CRC2_CH1_TOE.VALUE=0x00000000
DRIVER.CRC.VAR.CRC2_CH2_PSA.VALUE=1
DRIVER.CRC.VAR.CRC2_CH2_ORI.VALUE=0x00000000
DRIVER.CRC.VAR.CRC1_CH2_DTE.VALUE=1
DRIVER.CRC.VAR.HTU_DCP0_TRDAT_1.VALUE=32BIT
DRIVER.CRC.VAR.HTU_ICPBL_6_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.HTU_ICPA_4_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_ICPB_0_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC1_CH2_CVH.VALUE=0x00000000
DRIVER.CRC.VAR.CRC2_CH1_PSIH.VALUE=0
DRIVER.CRC.VAR.HTU_ICPAL_0_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.CRC1_CH2_CVL.VALUE=0x00000000
DRIVER.CRC.VAR.CRC2_CH1_URI.VALUE=0x00000000
DRIVER.CRC.VAR.CRC2_CH1_PSIL.VALUE=0
DRIVER.CRC.VAR.CRC1_CH1_PCP.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_CPA_1_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC2_CH2_TOE.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_DCP0_CPBTMOD_1.VALUE=POST_INCREMENT
DRIVER.CRC.VAR.CRC1_CH2_PSSIH.VALUE=0
DRIVER.CRC.VAR.HTU_MP0_ACC_1.VALUE=READ_ONLY
DRIVER.CRC.VAR.CRC1_CH2_PSSIL.VALUE=0
DRIVER.CRC.VAR.CRC1_CH1_SCP.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_ICPB_5_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC2_CH2_URI.VALUE=0x00000000
DRIVER.CRC.VAR.CRC1_CH2_PCP.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_ICPAL_5_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.CRC1_CH1_PSA.VALUE=1
DRIVER.CRC.VAR.CRC1_CH1_ORI.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_DCP0_ADMOD_1.VALUE=INCREMENT_16BIT
DRIVER.CRC.VAR.HTU_CPA_6_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.HTU_CPB_2_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC2_CH1_WDTO.VALUE=0
DRIVER.CRC.VAR.CRC2_CH2_PSIH.VALUE=0
DRIVER.CRC.VAR.CRC1_CH2_SCP.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_ENA_1.VALUE=0
DRIVER.CRC.VAR.CRC1_CH1_TOE.VALUE=0x00000000
DRIVER.CRC.VAR.CRC1_CH1_MODE.VALUE=FULL_CPU
DRIVER.CRC.VAR.CRC2_CH2_PSIL.VALUE=0
DRIVER.CRC.VAR.CRC1_CH2_PSA.VALUE=1
DRIVER.CRC.VAR.CRC1_CH2_ORI.VALUE=0x00000000
DRIVER.CRC.VAR.HTU_MP0_ENDADD_1.VALUE=0
DRIVER.CRC.VAR.HTU_ICPBL_2_SEL_1.VALUE=HIGH
DRIVER.CRC.VAR.HTU_ICPA_0_SEL_1.VALUE=ENABLE
DRIVER.CRC.VAR.CRC2_CH1_MODE_VALUE.VALUE=0x0001
DRIVER.EMAC.VAR.EMAC_PHY_CUSTOM.VALUE=0
DRIVER.EMAC.VAR.EMAC_ADD1.VALUE=FF
DRIVER.EMAC.VAR.EMAC_ADD2.VALUE=FF
DRIVER.EMAC.VAR.EMAC_ADD3.VALUE=FF
DRIVER.EMAC.VAR.EMAC_ADD4.VALUE=FF
DRIVER.EMAC.VAR.EMAC_ADD5.VALUE=FF
DRIVER.EMAC.VAR.EMAC_ADD6.VALUE=FF
DRIVER.EMAC.VAR.EMAC_CTRL_BASE.VALUE=0xFCF78800
DRIVER.EMAC.VAR.EMAC_PHY_DP83640.VALUE=1
DRIVER.EMAC.VAR.EMAC_LOOPBACK_ENA.VALUE=0
DRIVER.EMAC.VAR.MDIO_BASE.VALUE=0xFCF78900
DRIVER.EMAC.VAR.EMAC_BASE.VALUE=0xFCF78000
DRIVER.EMAC.VAR.EMAC_BASE_PORT.VALUE=0xFFFFFFFF
DRIVER.EMAC.VAR.EMAC_TRANSMIT_ENA.VALUE=1
DRIVER.EMAC.VAR.EMAC_PHY_TLK111.VALUE=0
DRIVER.EMAC.VAR.EMAC_CHANNELNUMBER.VALUE=0
DRIVER.EMAC.VAR.EMAC_RX_PBUF_ALLOC.VALUE=10
DRIVER.EMAC.VAR.EMAC_UNICAST_ENA.VALUE=1
DRIVER.EMAC.VAR.EMAC_FULL_DUPLEX_ENA.VALUE=1
DRIVER.EMAC.VAR.EMAC_PHYADDRESS.VALUE=1
DRIVER.EMAC.VAR.EMAC_MII_ENA.VALUE=1
DRIVER.EMAC.VAR.EMAC_CTRL_RAM_BASE.VALUE=0xFC520000
DRIVER.EMAC.VAR.EMAC_BROADCAST_ENA.VALUE=1
DRIVER.EMAC.VAR.EMAC_RECEIVE_ENA.VALUE=1
DRIVER.EMIF.VAR.EMIF_ASYNC2_TAVAV.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_TD.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_EXTENDED_WAIT.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_TH.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_TA.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_WAIT.VALUE=pin0
DRIVER.EMIF.VAR.EMIF_ASYNC2_TD.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_NOR_FLASH.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_TEHQZ.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_TH.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_TA.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_TD.VALUE=0
DRIVER.EMIF.VAR.EMIF_ENA_SDRAM.VALUE=1
DRIVER.EMIF.VAR.EMIF_ASYNC3_TH.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_TELQV.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_PAGE_MODE.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_ENA.VALUE=1
DRIVER.EMIF.VAR.EMIF_SDRAM_REFRESH_CYCLES.VALUE=0
DRIVER.EMIF.VAR.EMIF_AVAILABLE.VALUE=1
DRIVER.EMIF.VAR.EMIF_SDRAM_TRC_MAX.VALUE=213
DRIVER.EMIF.VAR.EMIF_ASYNC3_TEHEL.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_ENA.VALUE=1
DRIVER.EMIF.VAR.EMIF_ASYNC1_R_STROBE.VALUE=63
DRIVER.EMIF.VAR.EMIF_SDRAM_TRAS_MAX.VALUE=213
DRIVER.EMIF.VAR.EMIF_ASYNC3_TELEH.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_TRRD_MAX.VALUE=107
DRIVER.EMIF.VAR.EMIF_ASYNC3_STROBE_MODE.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_ENA.VALUE=1
DRIVER.EMIF.VAR.EMIF_ASYNC1_ASIZE.VALUE=8_bit
DRIVER.EMIF.VAR.EMIF_SDRAM_TRC_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_TAVAV.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_BANKS.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_PAGE_DELAY_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_TRAS_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_TRRD_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_BASE.VALUE=0xFCFFE800
DRIVER.EMIF.VAR.EMIF_ASYNC3_TEHQZ.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_W_STROBE.VALUE=63
DRIVER.EMIF.VAR.EMIF_ASYNC3_TELQV.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_TXSR_MAX.VALUE=427
DRIVER.EMIF.VAR.EMIF_ASYNC2_PAGE_SIZE.VALUE=4_words
DRIVER.EMIF.VAR.EMIF_CLKFRQ.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_W_HOLD.VALUE=7
DRIVER.EMIF.VAR.EMIF_ASYNC2_R_HOLD.VALUE=7
DRIVER.EMIF.VAR.EMIF_SDRAM_TREFRESH_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_R_SETUP.VALUE=15
DRIVER.EMIF.VAR.EMIF_SDRAM_TXSR_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_TSU.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_EXTENDED_WAIT.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_ASIZE.VALUE=8_bit
DRIVER.EMIF.VAR.EMIF_ASYNC2_TSU.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_W_SETUP.VALUE=15
DRIVER.EMIF.VAR.EMIF_ASYNC3_NOR_FLASH.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_TWR_MAX.VALUE=107
DRIVER.EMIF.VAR.EMIF_ASYNC2_PAGE_DELAY_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_W_HOLD.VALUE=7
DRIVER.EMIF.VAR.EMIF_SDRAM_INIT_TIME.VALUE=200
DRIVER.EMIF.VAR.EMIF_SDRAM_TREFRESH_DEFAULT.VALUE=1605
DRIVER.EMIF.VAR.EMIF_ASYNC3_TSU.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_PAGE_MODE.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_STROBE_MODE.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_R_SETUP.VALUE=15
DRIVER.EMIF.VAR.EMIF_SDRAM_TWR_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_R_STROBE.VALUE=63
DRIVER.EMIF.VAR.EMIF_SDRAM_TRCD_MAX.VALUE=107
DRIVER.EMIF.VAR.EMIF_CLK.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_TRCD.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_W_SETUP.VALUE=15
DRIVER.EMIF.VAR.EMIF_SDRAM_TRFC.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_ASIZE.VALUE=8_bit
DRIVER.EMIF.VAR.EMIF_SDRAM_TRAS.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_NOR_FLASH.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_PAGE_DELAY.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_CAS_LATENCY.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC_WAIT_POLARITY0.VALUE=pin_low
DRIVER.EMIF.VAR.EMIF_SDRAM_TRCD_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC_WAIT_POLARITY1.VALUE=pin_high
DRIVER.EMIF.VAR.EMIF_ASYNC1_PAGE_MODE.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_R_SETUP.VALUE=15
DRIVER.EMIF.VAR.EMIF_SDRAM_TRC.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_TRRD.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_PAGE_DELAY_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_W_STROBE.VALUE=63
DRIVER.EMIF.VAR.EMIF_ASYNC1_TEHEL.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC_MAX_EXT_WAIT.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_TRP.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_PAGE_SIZE.VALUE=4_words
DRIVER.EMIF.VAR.EMIF_ASYNC1_W_SETUP.VALUE=15
DRIVER.EMIF.VAR.EMIF_ASYNC1_TELEH.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_REFRESH_CYCLES_MAX.VALUE=0
DRIVER.EMIF.VAR.EMIF_MS.VALUE=0.001
DRIVER.EMIF.VAR.EMIF_NS.VALUE=0.000000001
DRIVER.EMIF.VAR.EMIF_SDRAM_TWR.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_EXTENDED_WAIT.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_REFRESH_PERIOD.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC3_R_HOLD.VALUE=7
DRIVER.EMIF.VAR.EMIF_ASYNC1_TAVAV.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_PAGE_DELAY.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_WAIT.VALUE=pin0
DRIVER.EMIF.VAR.EMIF_SDRAM_TRP_MAX.VALUE=107
DRIVER.EMIF.VAR.EMIF_SDRAM_TXSR.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_TEHQZ.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_TRFC_MAX.VALUE=427
DRIVER.EMIF.VAR.EMIF_ASYNC2_R_STROBE.VALUE=63
DRIVER.EMIF.VAR.EMIF_ASYNC1_TELQV.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_STROBE_MODE.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_TRP_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_REFRESH_PERIOD_MAX.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_W_HOLD.VALUE=7
DRIVER.EMIF.VAR.EMIF_ASYNC1_PAGE_SIZE.VALUE=4_words
DRIVER.EMIF.VAR.EMIF_ASYNC2_WAIT.VALUE=pin0
DRIVER.EMIF.VAR.EMIF_ASYNC2_TEHEL.VALUE=0
DRIVER.EMIF.VAR.EMIF_SDRAM_TRFC_VAL.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_R_HOLD.VALUE=7
DRIVER.EMIF.VAR.EMIF_SDRAM_PAGE_SIZE.VALUE=elements_256
DRIVER.EMIF.VAR.EMIF_ASYNC2_TELEH.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC1_PAGE_DELAY.VALUE=0
DRIVER.EMIF.VAR.EMIF_IBANK.VALUE=0
DRIVER.EMIF.VAR.EMIF_ASYNC2_W_STROBE.VALUE=63
DRIVER.EMIF.VAR.EMIF_ASYNC1_TA.VALUE=0
DRIVER.POM.VAR.POM_OVRLY_START_ADD28.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD29.VALUE=0x00000000
DRIVER.POM.VAR.POM_REGION_10_ENA.VALUE=0
DRIVER.POM.VAR.POM_TIMEOUT_ENABLE.VALUE=0
DRIVER.POM.VAR.POM_REGION_11_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_20_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_12_ENA.VALUE=0
DRIVER.POM.VAR.POM_NO_OF_REGION.VALUE=1
DRIVER.POM.VAR.POM_REGION_21_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_13_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_30_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_22_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_14_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_31_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_23_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_15_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_1_ENA.VALUE=1
DRIVER.POM.VAR.POM_REGION_32_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_24_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_16_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_2_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_25_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_17_ENA.VALUE=0
DRIVER.POM.VAR.POM_OVRLY_START_ADD1.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD2.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD3.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD4.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD5.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD6.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD7.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD8.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVLY_TRG_REGION.VALUE=INTERNAL_RAM
DRIVER.POM.VAR.POM_OVRLY_START_ADD9.VALUE=0x00000000
DRIVER.POM.VAR.POM_REGION_3_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_26_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_18_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_4_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_27_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_19_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_5_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_28_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_6_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_SIZE10.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE11.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE20.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE12.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_29_ENA.VALUE=0
DRIVER.POM.VAR.POM_REGION_SIZE21.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE13.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE30.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE22.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE14.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE31.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE23.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE15.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE32.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE24.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE16.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE25.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE17.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE26.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE18.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE27.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE19.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE28.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE29.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_7_ENA.VALUE=0
DRIVER.POM.VAR.POM_BASE.VALUE=0xFFA04000
DRIVER.POM.VAR.POM_PROG_START_ADD10.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD11.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD20.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD12.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD21.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD13.VALUE=0x00000000
DRIVER.POM.VAR.POM_REGION_8_ENA.VALUE=0
DRIVER.POM.VAR.POM_PROG_START_ADD30.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD22.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD14.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD31.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD23.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD15.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD32.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD24.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD16.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD25.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD17.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD26.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD18.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD27.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD19.VALUE=0x00000000
DRIVER.POM.VAR.POM_REGION_SIZE1.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_PROG_START_ADD28.VALUE=0x00000000
DRIVER.POM.VAR.POM_REGION_SIZE2.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_PROG_START_ADD29.VALUE=0x00000000
DRIVER.POM.VAR.POM_REGION_SIZE3.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE4.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE5.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE6.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE7.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE8.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_SIZE9.VALUE=SIZE_64BYTES
DRIVER.POM.VAR.POM_REGION_9_ENA.VALUE=0
DRIVER.POM.VAR.POM_PROG_START_ADD1.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD2.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD3.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD4.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD5.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD6.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD7.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD8.VALUE=0x00000000
DRIVER.POM.VAR.POM_PROG_START_ADD9.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD10.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD11.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD20.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD12.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD21.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD13.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD30.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD22.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD14.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD31.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD23.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD15.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD32.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD24.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD16.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD25.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD17.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD26.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD18.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD27.VALUE=0x00000000
DRIVER.POM.VAR.POM_OVRLY_START_ADD19.VALUE=0x00000000
DRIVER.PMM.VAR.PMM_RAM_PWR_DOMAIN2_ENABLE.VALUE=0
DRIVER.PMM.VAR.PMM_PWR_DOMAIN5_ENABLE.VALUE=0
DRIVER.PMM.VAR.PMM_PWR_DOMAIN3_ENABLE.VALUE=0
DRIVER.PMM.VAR.PMM_RAM_PWR_DOMAIN3_ENABLE.VALUE=0
DRIVER.PMM.VAR.PMM_RAM_PWR_DOMAIN1_ENABLE.VALUE=0
DRIVER.PMM.VAR.PMM_PWR_DOMAIN4_ENABLE.VALUE=0
DRIVER.PMM.VAR.PMM_PWR_DOMAIN2_ENABLE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_OSHT_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM3_PWMA_PERIOD_REG.VALUE=1000
DRIVER.ETPWM.VAR.ETPWM2_PWMA_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM5_CHOPPER_PERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM3_PWMA_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM3_PWMA_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM7_PWMB_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM3_PWMB_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_HSPCLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_CLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_SOCA_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_DEADBAND_INPUT.VALUE=PWMA_RED_FED
DRIVER.ETPWM.VAR.ETPWM7_BASE.VALUE=0xFCF79200
DRIVER.ETPWM.VAR.ETPWM5_TB_ACTUALFREQUENCY.VALUE=80.000
DRIVER.ETPWM.VAR.ETPWM6_DCBEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_DCBEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_ENABLE_SOCA.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_CBC.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_ENABLE_SOCB.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_PWMA_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_CHOPPER_PERIOD_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_PWMA_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_PWMB_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM6_RDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_PWMA_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM1_CHOPPER_DUTY_NEW.VALUE=50.0
DRIVER.ETPWM.VAR.ETPWM7_SOCB_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_OSHT_ACTUAL_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM7_PWMB_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_PWMB_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM2_PWMB_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM1_OSHT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_OSHT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_PWMA_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_ENABLE_SOCA.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_OSHT3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_ENABLE_SOCB.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_OSHT4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_OSHT_WIDTH_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_OSHT5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_PWMA_PERIOD_REG.VALUE=1000
DRIVER.ETPWM.VAR.ETPWM1_OSHT6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_CHOPPER_PERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM1_PWMB_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM2_CBC.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_CLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_PWMB_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_SOCB_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM7_CHOPPER_MODE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_PWMB_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM7_DEADBAND_OUTPUT.VALUE=PWMA_PWMB_NIL
DRIVER.ETPWM.VAR.ETPWM4_PWMB_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM1_ENABLE_SOCA.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_PWMB_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM1_ENABLE_SOCB.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_CHOPPER_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM5_DCAEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_HSPCLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_DCAEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_CHOPPER_DUTYTIME.VALUE=50.000
DRIVER.ETPWM.VAR.ETPWM6_OSHT_ACTUAL_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM4_PWMB_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_PWMB_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_OSHT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_PWMA_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_OSHT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_PWMA_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM1_SOCB_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_OSHT3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_PWMB_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM3_CBC.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_TB_ACTUALFREQUENCY.VALUE=80.000
DRIVER.ETPWM.VAR.ETPWM1_FDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_OSHT4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_PWMB_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_OSHT5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_PWMB_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM2_PWMB_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_OSHT6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_DEADBAND_INPUT.VALUE=PWMA_RED_FED
DRIVER.ETPWM.VAR.ETPWM6_SELECT_SOCA.VALUE=DCAEVT1
DRIVER.ETPWM.VAR.ETPWM6_SELECT_SOCB.VALUE=DCBEVT1
DRIVER.ETPWM.VAR.ETPWM6_SELECT_EVENT.VALUE=NO_EVENT
DRIVER.ETPWM.VAR.ETPWM5_OSHT_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM1_PWMA_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_PWMA_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM3_CHOPPER_PERIOD_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_PWMA_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_PWMB_PERIOD_REG.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM5_DCBEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_OSHT_WIDTH_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_PWMA_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM5_DCBEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_PWMA_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM5_PWMA_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_HSPCLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_PWMA_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_PWMA_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_CHOPPER_MODE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_CLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_PWMB_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_TB_FREQUENCY.VALUE=110.000
DRIVER.ETPWM.VAR.ETPWM4_CBC.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_SELECT_SOCA.VALUE=DCAEVT1
DRIVER.ETPWM.VAR.ETPWM7_PWMA_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_SELECT_SOCB.VALUE=DCBEVT1
DRIVER.ETPWM.VAR.ETPWM6_PWMB_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM5_PWMA_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_CHOPPER_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM5_DEADBAND_OUTPUT.VALUE=PWMA_PWMB_NIL
DRIVER.ETPWM.VAR.ETPWM6_FDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_RDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_PWMA_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM6_PWMB_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_PWMA_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM5_PWMB_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_CHOPPER_PERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM6_CHOPPER_DUTYTIME.VALUE=50.000
DRIVER.ETPWM.VAR.ETPWM1_PWMB_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM3_SELECT_EVENT.VALUE=NO_EVENT
DRIVER.ETPWM.VAR.ETPWM2_CLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_PWMA_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM7_PWMA_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM2_DEADBAND_INPUT.VALUE=PWMA_RED_FED
DRIVER.ETPWM.VAR.ETPWM5_CBC.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_CBC1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_CBC2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_CBC3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_CHOPPER_DUTYTIME_REG.VALUE=3
DRIVER.ETPWM.VAR.ETPWM7_PWMB_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM1_CBC4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_CBC5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_CBC6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_DCAEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_PWMB_PERIOD_REG.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM3_CHOPPER_DUTYTIME_REG.VALUE=3
DRIVER.ETPWM.VAR.ETPWM1_CHOPPER_MODE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_PWMA_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM4_DCAEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_TB_ACTUALFREQUENCY.VALUE=80.000
DRIVER.ETPWM.VAR.ETPWM3_TB_FREQUENCY.VALUE=110.000
DRIVER.ETPWM.VAR.ETPWM2_PWMB_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM5_CHOPPER_DUTYTIME_REG.VALUE=3
DRIVER.ETPWM.VAR.ETPWM2_OSHT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_CHOPPER_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM1_PWMB_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM1_HSPCLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_INTERRUPT_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM2_OSHT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_OSHT3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_OSHT4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_CHOPPER_DUTYTIME_REG.VALUE=3
DRIVER.ETPWM.VAR.ETPWM4_PWMB_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_PWMA_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM2_OSHT5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_DEADBAND_OUTPUT.VALUE=PWMA_PWMB_NIL
DRIVER.ETPWM.VAR.ETPWM3_PWMB_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM2_OSHT6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_CBC.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_PWMB_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM6_OSHT_WIDTH_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM2_CHOPPER_PERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM2_PWMA_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM5_CHOPPER_DUTYTIME.VALUE=50.000
DRIVER.ETPWM.VAR.ETPWM5_OSHT_ACTUAL_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM4_DCBEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_SOCA_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM5_PWMA_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_DCBEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_PWMB_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM4_OSHT_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM5_PWMA_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_PWMA_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_PWMA_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM7_OSHT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_PWMB_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM6_PWMA_PERIOD_REG.VALUE=1000
DRIVER.ETPWM.VAR.ETPWM6_HSPCLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_PWMB_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM7_OSHT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_PWMB_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM7_CBC.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_OSHT3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_CBC1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_OSHT4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_CBC2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_HSPCLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_OSHT5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_PWMB_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM2_CBC3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_PWMB_PERIOD_REG.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM2_PWMA_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_CLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_OSHT6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_SOCA_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM2_CBC4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_OST.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_CHOPPER_ACTUALPERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM1_PWMA_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM7_PWMB_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM3_FDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_CBC5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_CLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_CBC6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_PWMB_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM7_DEADBAND_INPUT.VALUE=PWMA_RED_FED
DRIVER.ETPWM.VAR.ETPWM6_INTERRUPT_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM3_CHOPPER_ACTUALPERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM1_PWMB_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_ENABLE_SOCA.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_PWMB_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM1_BASE.VALUE=0xFCF78C00
DRIVER.ETPWM.VAR.ETPWM6_ENABLE_SOCB.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_PWMB_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM5_CHOPPER_ACTUALPERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM3_PWMB_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM1_DEADBAND_OUTPUT.VALUE=PWMA_PWMB_NIL
DRIVER.ETPWM.VAR.ETPWM4_TB_ACTUALFREQUENCY.VALUE=80.000
DRIVER.ETPWM.VAR.ETPWM2_OSHT_WIDTH_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM7_CHOPPER_ACTUALPERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM6_SOCB_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_CHOPPER_DUTYTIME.VALUE=50.000
DRIVER.ETPWM.VAR.ETPWM5_CHOPPER_PERIOD_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_PWMA_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM3_DCAEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_DCAEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_OST.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_ENABLE_SOCA.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_HSPCLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_ENABLE_SOCB.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_PWMA_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_PWMA_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_PWMA_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM5_RDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_PWMB_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM5_PWMA_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM4_PWMA_PERIOD_REG.VALUE=1000
DRIVER.ETPWM.VAR.ETPWM7_CHOPPER_PERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM6_PWMB_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_SOCB_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_PWMB_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM4_PWMA_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM2_PWMB_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_PWMB_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_CBC1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_SELECT_EVENT.VALUE=NO_EVENT
DRIVER.ETPWM.VAR.ETPWM3_CBC2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_DCBEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_CBC3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_INTERRUPT_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM3_OST.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_DCBEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_CBC4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_DEADBAND_INPUT.VALUE=PWMA_RED_FED
DRIVER.ETPWM.VAR.ETPWM3_CBC5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_CBC6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_PWMA_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM2_PWMB_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM6_PWMB_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM2_BASE.VALUE=0xFCF78D00
DRIVER.ETPWM.VAR.ETPWM7_CHOPPER_DUTY_NEW.VALUE=50.0
DRIVER.ETPWM.VAR.ETPWM7_CLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_CHOPPER_MODE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_OSHT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_OSHT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_TB_FREQUENCY.VALUE=110.000
DRIVER.ETPWM.VAR.ETPWM5_SELECT_SOCA.VALUE=DCAEVT1
DRIVER.ETPWM.VAR.ETPWM3_OSHT3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_CHOPPER_DUTYTIME.VALUE=50.000
DRIVER.ETPWM.VAR.ETPWM5_SELECT_SOCB.VALUE=DCBEVT1
DRIVER.ETPWM.VAR.ETPWM4_OSHT_ACTUAL_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM3_OSHT4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_OSHT_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM5_CHOPPER_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM4_PWMB_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_PWMB_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM3_OSHT5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_HSPCLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_PWMA_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_OSHT6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_TB_ACTUALFREQUENCY.VALUE=80.000
DRIVER.ETPWM.VAR.ETPWM5_CLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_PWMA_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM6_PWMB_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_PWMB_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM4_OST.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_PWMB_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM7_OSHT_WIDTH_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM2_CHOPPER_PERIOD_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_PWMA_PERIOD_REG.VALUE=1000
DRIVER.ETPWM.VAR.ETPWM1_PWMB_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM1_CLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_CHOPPER_PERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM7_PWMB_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM2_SELECT_SOCA.VALUE=DCAEVT1
DRIVER.ETPWM.VAR.ETPWM4_SELECT_EVENT.VALUE=NO_EVENT
DRIVER.ETPWM.VAR.ETPWM2_SELECT_SOCB.VALUE=DCBEVT1
DRIVER.ETPWM.VAR.ETPWM7_PWMB_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM2_DCAEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_INTERRUPT_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM2_DCAEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_CBC1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_PWMB_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM4_CBC2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_PWMA_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_CBC3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_CHOPPER_MODE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM1_PWMA_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM7_PWMA_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM5_OST.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_CBC4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_CBC5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_TB_FREQUENCY.VALUE=110.000
DRIVER.ETPWM.VAR.ETPWM4_CBC6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_CHOPPER_DUTY_NEW.VALUE=50.0
DRIVER.ETPWM.VAR.ETPWM4_PWMA_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_CHOPPER_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM2_PWMA_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM5_FDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_BASE.VALUE=0xFCF78E00
DRIVER.ETPWM.VAR.ETPWM2_CHOPPER_DUTYTIME.VALUE=50.000
DRIVER.ETPWM.VAR.ETPWM2_RDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_PWMB_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM2_PWMA_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM1_PWMA_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM4_HSPCLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_PWMA_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM1_PWMB_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_PWMB_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_PWMA_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM2_DCBEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_PWMA_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM4_PWMA_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM2_DCBEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_PWMB_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM3_PWMB_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM1_SELECT_EVENT.VALUE=NO_EVENT
DRIVER.ETPWM.VAR.ETPWM7_PWMB_PERIOD_REG.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM7_PWMB_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM7_PWMB_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM3_OSHT_WIDTH_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM3_PWMA_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM7_SOCA_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_OST.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_PWMB_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_PWMB_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_TB_ACTUALFREQUENCY.VALUE=80.000
DRIVER.ETPWM.VAR.ETPWM4_PWMB_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM2_PWMA_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM7_PWMB_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_PWMA_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM3_PWMB_FALLING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_DEADBAND_OUTPUT.VALUE=PWMA_PWMB_NIL
DRIVER.ETPWM.VAR.ETPWM3_INTERRUPT_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_PWMA_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM7_RDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_PWMA_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM1_TB_FREQUENCY.VALUE=110.000
DRIVER.ETPWM.VAR.ETPWM3_CLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_PWMA_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_CHOPPER_PERIOD_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_CLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_SOCA_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_PWMB_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM5_CBC1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_PWMB_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM5_CBC2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_PWMA_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_OSHT_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM5_CBC3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_CHOPPER_DUTY_NEW.VALUE=50.0
DRIVER.ETPWM.VAR.ETPWM3_PWMB_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM1_PWMA_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM7_OST.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_CBC4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_CBC5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_CHOPPER_DUTYTIME.VALUE=50.000
DRIVER.ETPWM.VAR.ETPWM1_PWMB_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM6_PWMA_DEADBAND_INVERT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_CBC6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_OSHT_ACTUAL_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM2_PWMB_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM5_PWMB_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM4_DEADBAND_INPUT.VALUE=PWMA_RED_FED
DRIVER.ETPWM.VAR.ETPWM3_PWMA_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_PWMB_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM4_BASE.VALUE=0xFCF78F00
DRIVER.ETPWM.VAR.ETPWM3_PWMA_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM4_OSHT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_DCAEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_PWMA_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_OSHT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_SOCA_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_DCAEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_OSHT3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_OSHT4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_PWMB_PERIOD_REG.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM4_OSHT5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_PWMB_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_OSHT6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_PWMB_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM5_ENABLE_SOCA.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_ENABLE_SOCB.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_HSPCLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_PWMB_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM2_PWMB_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM3_PWMA_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_PWMA_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_SOCB_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_DEADBAND_OUTPUT.VALUE=PWMA_PWMB_NIL
DRIVER.ETPWM.VAR.ETPWM2_INTERRUPT_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_PWMB_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM4_PWMA_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM2_FDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM1_PWMA_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM7_PWMB_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM5_PWMB_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM5_PWMA_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM2_CHOPPER_DUTYTIME_REG.VALUE=3
DRIVER.ETPWM.VAR.ETPWM1_DCBEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_CHOPPER_PERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM1_DCBEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_TB_ACTUALFREQUENCY.VALUE=80.000
DRIVER.ETPWM.VAR.ETPWM2_ENABLE_SOCA.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_ENABLE_SOCB.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_HSPCLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_PWMB_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_CHOPPER_DUTYTIME_REG.VALUE=3
DRIVER.ETPWM.VAR.ETPWM4_CHOPPER_DUTY_NEW.VALUE=50.0
DRIVER.ETPWM.VAR.ETPWM6_CBC1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_PWMA_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM6_CBC2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_CBC3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_CHOPPER_DUTYTIME_REG.VALUE=3
DRIVER.ETPWM.VAR.ETPWM4_CHOPPER_PERIOD_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_CBC4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_SOCB_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_CBC5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_CBC6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_PWMA_PERIOD_REG.VALUE=1000
DRIVER.ETPWM.VAR.ETPWM6_CHOPPER_MODE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_PWMB_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_PWMA_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM7_SELECT_SOCA.VALUE=DCAEVT1
DRIVER.ETPWM.VAR.ETPWM5_PWMA_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM5_BASE.VALUE=0xFCF79000
DRIVER.ETPWM.VAR.ETPWM3_PWMA_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM7_SELECT_SOCB.VALUE=DCBEVT1
DRIVER.ETPWM.VAR.ETPWM7_OSHT_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM1_CLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_CHOPPER_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM6_PWMA_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM3_PWMB_PERIOD_REG.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM4_PWMB_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_FDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_RDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM4_PWMA_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM7_DCAEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_PWMA_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM7_DCAEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_PWMA_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM7_HSPCLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_CLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_PWMB_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM2_DEADBAND_OUTPUT.VALUE=PWMA_PWMB_NIL
DRIVER.ETPWM.VAR.ETPWM1_INTERRUPT_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM4_SELECT_SOCA.VALUE=DCAEVT1
DRIVER.ETPWM.VAR.ETPWM5_SELECT_EVENT.VALUE=NO_EVENT
DRIVER.ETPWM.VAR.ETPWM4_SELECT_SOCB.VALUE=DCBEVT1
DRIVER.ETPWM.VAR.ETPWM1_OSHT_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM4_OSHT_WIDTH_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_PWMA_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM5_PWMA_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM6_PWMA_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM3_CHOPPER_DUTY_NEW.VALUE=50.0
DRIVER.ETPWM.VAR.ETPWM2_CHOPPER_ACTUALPERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM2_OSHT_ACTUAL_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM7_DCBEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_CHOPPER_MODE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_DCBEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_CHOPPER_ACTUALPERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM2_PWMA_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_CBC1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_PWMA_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM5_TB_FREQUENCY.VALUE=110.000
DRIVER.ETPWM.VAR.ETPWM1_SELECT_SOCA.VALUE=DCAEVT1
DRIVER.ETPWM.VAR.ETPWM7_CBC2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM1_SELECT_SOCB.VALUE=DCBEVT1
DRIVER.ETPWM.VAR.ETPWM7_CBC3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_PWMA_PERIOD_REG.VALUE=1000
DRIVER.ETPWM.VAR.ETPWM3_CHOPPER_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM2_HSPCLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_CBC4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM6_CHOPPER_ACTUALPERIOD.VALUE=100.000
DRIVER.ETPWM.VAR.ETPWM7_CBC5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_CBC6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_PWMB_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM5_PWMA_COMPARE.VALUE=50
DRIVER.ETPWM.VAR.ETPWM3_PWMA_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM1_CHOPPER_PERIOD_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM1_PWMB_PERIOD_REG.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM7_PWMA_FALLING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM7_PWMA_RISING_EDGE_DELAY.VALUE=9.091
DRIVER.ETPWM.VAR.ETPWM6_BASE.VALUE=0xFCF79100
DRIVER.ETPWM.VAR.ETPWM3_PWMB_DUTYTIME.VALUE=500.000
DRIVER.ETPWM.VAR.ETPWM6_PWMB_ENA.VALUE=1
DRIVER.ETPWM.VAR.ETPWM5_OSHT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_PWMB_RISING_EDGE_DELAY_REG.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_PWMA_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM5_OSHT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_DEADBAND_INPUT.VALUE=PWMA_RED_FED
DRIVER.ETPWM.VAR.ETPWM5_PWMB_ACTUALPERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM5_OSHT3.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_OSHT4.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM2_SELECT_EVENT.VALUE=NO_EVENT
DRIVER.ETPWM.VAR.ETPWM5_OSHT5.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM5_PWMB_DUTY.VALUE=50
DRIVER.ETPWM.VAR.ETPWM5_OSHT6.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM7_OSHT_ACTUAL_WIDTH.VALUE=100
DRIVER.ETPWM.VAR.ETPWM6_CLKDIV.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_PWMA_DEADBAND_OUT.VALUE=0
DRIVER.ETPWM.VAR.ETPWM7_HSPCLKDIV_REG.VALUE=0
DRIVER.ETPWM.VAR.ETPWM2_CHOPPER_DUTY_NEW.VALUE=50.0
DRIVER.ETPWM.VAR.ETPWM3_PWMA_PERIOD.VALUE=1000.000
DRIVER.ETPWM.VAR.ETPWM2_TB_FREQUENCY.VALUE=110.000
DRIVER.ETPWM.VAR.ETPWM6_DCAEVT1.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM3_PWMA_POLARITY.VALUE=0
DRIVER.ETPWM.VAR.ETPWM6_SOCA_PERIOD.VALUE=1
DRIVER.ETPWM.VAR.ETPWM6_DCAEVT2.VALUE=0x0000
DRIVER.ETPWM.VAR.ETPWM4_FDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM1_RDELAY_SOURCE.VALUE=0
DRIVER.ETPWM.VAR.ETPWM1_PWMA_DUTYTIME.VALUE=500.000
DRIVER.ECAP.VAR.ECAP1_PRESCALE_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP2_ENA_PWM.VALUE=0
DRIVER.ECAP.VAR.ECAP4_PRD.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP6_RESET_COUNTER_CAP1.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP6_RESET_COUNTER_CAP2.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP6_RESET_COUNTER_CAP3.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP6_RESET_COUNTER_CAP4.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP5_PWM_DUTY.VALUE=50
DRIVER.ECAP.VAR.ECAP5_PWM_PERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP4_CAP2_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP5_PRESCALE.VALUE=0
DRIVER.ECAP.VAR.ECAP5_PRD.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP6_PWM_COMPARE.VALUE=50
DRIVER.ECAP.VAR.ECAP5_CAP4_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP5_ENA_LOAD.VALUE=0
DRIVER.ECAP.VAR.ECAP6_PWM_PERIOD_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP6_WRAP_COUNTER.VALUE=CAPTURE_EVENT1
DRIVER.ECAP.VAR.ECAP3_PWM_COMPARE.VALUE=50
DRIVER.ECAP.VAR.ECAP2_CAP1_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP6_PRD.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP4_PWM_DUTYTIME.VALUE=500.000
DRIVER.ECAP.VAR.ECAP3_RESET_COUNTER_CAP1.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP3_CAP3_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP3_RESET_COUNTER_CAP2.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP3_RESET_COUNTER_CAP3.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP3_RESET_COUNTER_CAP4.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP1_ENA_PWM.VALUE=0
DRIVER.ECAP.VAR.ECAP3_WRAP_COUNTER.VALUE=CAPTURE_EVENT1
DRIVER.ECAP.VAR.ECAP2_PWM_PERIOD_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP5_RESET_COUNTER.VALUE=0
DRIVER.ECAP.VAR.ECAP5_CEVT1.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP4_CAPTURE_MODE.VALUE=ONE_SHOT
DRIVER.ECAP.VAR.ECAP5_CEVT2.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP5_CEVT3.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP5_CEVT4.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP1_PWM_DUTY.VALUE=50
DRIVER.ECAP.VAR.ECAP1_CAP2_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP4_PWM_PERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP1_PWM_DUTYTIME.VALUE=500.000
DRIVER.ECAP.VAR.ECAP5_CNTOVF.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP5_PRESCALE_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP2_CAP4_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP1_PRESCALE.VALUE=0
DRIVER.ECAP.VAR.ECAP1_ENA_LOAD.VALUE=0
DRIVER.ECAP.VAR.ECAP6_CAP2_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP1_CAPTURE_MODE.VALUE=ONE_SHOT
DRIVER.ECAP.VAR.ECAP2_PRESCALE_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP4_PWM_DUTY.VALUE=50
DRIVER.ECAP.VAR.ECAP6_PWM_ACTUALPERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP4_CAP1_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP1_CEVT1.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP1_CEVT2.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP1_CEVT3.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP2_RESET_COUNTER.VALUE=0
DRIVER.ECAP.VAR.ECAP1_CEVT4.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP4_PRESCALE.VALUE=0
DRIVER.ECAP.VAR.ECAP5_CAP3_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP4_ENA_LOAD.VALUE=0
DRIVER.ECAP.VAR.ECAP3_CNTOVF.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP3_PWM_PERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP5_RESET_COUNTER_CAP1.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP5_RESET_COUNTER_CAP2.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP5_RESET_COUNTER_CAP3.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP5_RESET_COUNTER_CAP4.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP6_CEVT1.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP3_PWM_PERIOD_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP6_CEVT2.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP6_CEVT3.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP6_CEVT4.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP5_PWM_COMPARE.VALUE=50
DRIVER.ECAP.VAR.ECAP5_PWM_ACTUALPERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP6_ENA_PWM.VALUE=0
DRIVER.ECAP.VAR.ECAP3_CAP2_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP5_PWM_DUTYTIME.VALUE=500.000
DRIVER.ECAP.VAR.ECAP1_BASE.VALUE=0xFCF79300
DRIVER.ECAP.VAR.ECAP4_CAP4_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP2_PWM_COMPARE.VALUE=50
DRIVER.ECAP.VAR.ECAP4_WRAP_COUNTER.VALUE=CAPTURE_EVENT1
DRIVER.ECAP.VAR.ECAP5_CAPTURE_MODE.VALUE=ONE_SHOT
DRIVER.ECAP.VAR.ECAP1_CAP1_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP2_RESET_COUNTER_CAP1.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP4_PWM_ACTUALPERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP2_RESET_COUNTER_CAP2.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP1_CNTOVF.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP2_PWM_DUTYTIME.VALUE=500.000
DRIVER.ECAP.VAR.ECAP2_RESET_COUNTER_CAP3.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP2_RESET_COUNTER_CAP4.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP2_CAP3_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP6_PRESCALE_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP2_BASE.VALUE=0xFCF79400
DRIVER.ECAP.VAR.ECAP2_CEVT1.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP2_CEVT2.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP2_PWM_PERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP2_CEVT3.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP2_CEVT4.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP1_WRAP_COUNTER.VALUE=CAPTURE_EVENT1
DRIVER.ECAP.VAR.ECAP6_CAP1_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP5_ENA_PWM.VALUE=0
DRIVER.ECAP.VAR.ECAP4_RESET_COUNTER.VALUE=0
DRIVER.ECAP.VAR.ECAP2_CAPTURE_MODE.VALUE=ONE_SHOT
DRIVER.ECAP.VAR.ECAP3_PWM_ACTUALPERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP3_PWM_DUTY.VALUE=50
DRIVER.ECAP.VAR.ECAP3_PRESCALE_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP1_CAP4_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP4_PWM_PERIOD_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP3_PRESCALE.VALUE=0
DRIVER.ECAP.VAR.ECAP6_CNTOVF.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP3_BASE.VALUE=0xFCF79500
DRIVER.ECAP.VAR.ECAP5_CAP2_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP3_ENA_LOAD.VALUE=0
DRIVER.ECAP.VAR.ECAP6_CAP4_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP1_CMP.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP2_PWM_ACTUALPERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP4_ENA_PWM.VALUE=0
DRIVER.ECAP.VAR.ECAP3_CAP1_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP1_PWM_PERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP1_RESET_COUNTER.VALUE=0
DRIVER.ECAP.VAR.ECAP6_PWM_DUTY.VALUE=50
DRIVER.ECAP.VAR.ECAP2_CMP.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP6_PWM_DUTYTIME.VALUE=500.000
DRIVER.ECAP.VAR.ECAP4_CAP3_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP4_BASE.VALUE=0xFCF79600
DRIVER.ECAP.VAR.ECAP6_PRESCALE.VALUE=0
DRIVER.ECAP.VAR.ECAP4_PWM_COMPARE.VALUE=50
DRIVER.ECAP.VAR.ECAP4_RESET_COUNTER_CAP1.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP3_CEVT1.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP4_RESET_COUNTER_CAP2.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP3_CEVT2.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP4_RESET_COUNTER_CAP3.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP3_CEVT3.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP4_RESET_COUNTER_CAP4.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP3_CEVT4.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP6_ENA_LOAD.VALUE=0
DRIVER.ECAP.VAR.ECAP5_WRAP_COUNTER.VALUE=CAPTURE_EVENT1
DRIVER.ECAP.VAR.ECAP4_CNTOVF.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP3_CMP.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP1_PWM_ACTUALPERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP6_RESET_COUNTER.VALUE=0
DRIVER.ECAP.VAR.ECAP6_CAPTURE_MODE.VALUE=ONE_SHOT
DRIVER.ECAP.VAR.ECAP1_PWM_COMPARE.VALUE=50
DRIVER.ECAP.VAR.ECAP2_CAP2_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP3_PWM_DUTYTIME.VALUE=500.000
DRIVER.ECAP.VAR.ECAP3_CAP4_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP4_CMP.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP1_PRD.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP5_PWM_PERIOD_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP6_PWM_PERIOD.VALUE=1000.000
DRIVER.ECAP.VAR.ECAP5_BASE.VALUE=0xFCF79700
DRIVER.ECAP.VAR.ECAP3_ENA_PWM.VALUE=0
DRIVER.ECAP.VAR.ECAP2_WRAP_COUNTER.VALUE=CAPTURE_EVENT1
DRIVER.ECAP.VAR.ECAP3_CAPTURE_MODE.VALUE=ONE_SHOT
DRIVER.ECAP.VAR.ECAP1_RESET_COUNTER_CAP1.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP1_RESET_COUNTER_CAP2.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP1_RESET_COUNTER_CAP3.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP1_RESET_COUNTER_CAP4.VALUE=RESET_DISABLE
DRIVER.ECAP.VAR.ECAP5_CMP.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP2_PRD.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP2_PWM_DUTY.VALUE=50
DRIVER.ECAP.VAR.ECAP1_CAP3_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP4_PRESCALE_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP2_PRESCALE.VALUE=0
DRIVER.ECAP.VAR.ECAP2_CNTOVF.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP5_CAP1_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP1_PWM_PERIOD_REG.VALUE=0
DRIVER.ECAP.VAR.ECAP6_CMP.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP2_ENA_LOAD.VALUE=0
DRIVER.ECAP.VAR.ECAP3_PRD.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP3_RESET_COUNTER.VALUE=0
DRIVER.ECAP.VAR.ECAP6_BASE.VALUE=0xFCF79800
DRIVER.ECAP.VAR.ECAP6_CAP3_POLARITY.VALUE=RISING_EDGE
DRIVER.ECAP.VAR.ECAP4_CEVT1.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP4_CEVT2.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP4_CEVT3.VALUE=0x0000
DRIVER.ECAP.VAR.ECAP4_CEVT4.VALUE=0x0000
DRIVER.EQEP.VAR.EQEP2_QUPRD.VALUE=0
DRIVER.EQEP.VAR.EQEP2_INDEX_EVT_INIT_ENABLE.VALUE=0
DRIVER.EQEP.VAR.EQEP2_IGATE.VALUE=0
DRIVER.EQEP.VAR.EQEP1_QPE_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP1_PC_RST_MODE.VALUE=MAX_POSITION
DRIVER.EQEP.VAR.EQEP1_UTO_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP1_SEL_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP1_INDEX_EVT_SELECT.VALUE=RISING_EDGE
DRIVER.EQEP.VAR.EQEP2_PCE_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP1_PCU_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP1_BASE.VALUE=0xFCF79900
DRIVER.EQEP.VAR.EQEP1_INV_QEPS_POL.VALUE=0
DRIVER.EQEP.VAR.EQEP1_INV_QEPA_POL.VALUE=0
DRIVER.EQEP.VAR.EQEP2_PCSHDW.VALUE=0
DRIVER.EQEP.VAR.EQEP2_PC_INIT_VALUE.VALUE=0x00000000
DRIVER.EQEP.VAR.EQEP2_PCR_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_BASE.VALUE=0xFCF79A00
DRIVER.EQEP.VAR.EQEP1_ENABLE_CAPTURE.VALUE=0
DRIVER.EQEP.VAR.EQEP1_INV_QEPB_POL.VALUE=0
DRIVER.EQEP.VAR.EQEP2_MAXPC_VALUE.VALUE=0x00000000
DRIVER.EQEP.VAR.EQEP1_PCM_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP1_PCPOL.VALUE=ACTIVE_HIGH
DRIVER.EQEP.VAR.EQEP2_UNIT_POS_PRESCALER.VALUE=PS_512
DRIVER.EQEP.VAR.EQEP2_CAP_CLK_PRESCALER.VALUE=PS_8
DRIVER.EQEP.VAR.EQEP1_PCSPW.VALUE=0x000
DRIVER.EQEP.VAR.EQEP1_POSCMP.VALUE=0x00000000
DRIVER.EQEP.VAR.EQEP2_PC_MODE.VALUE=DIRECTION_COUNT
DRIVER.EQEP.VAR.EQEP1_PCE_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_INV_QEPS_POL.VALUE=0
DRIVER.EQEP.VAR.EQEP1_SET_INIT_AT_STARTUP.VALUE=0
DRIVER.EQEP.VAR.EQEP2_ENABLE_CAPTURE.VALUE=0
DRIVER.EQEP.VAR.EQEP2_STROBE_EVT_SELECT.VALUE=DIRECTON_DEPENDENT
DRIVER.EQEP.VAR.EQEP2_PCPOL.VALUE=ACTIVE_HIGH
DRIVER.EQEP.VAR.EQEP2_INV_QEPA_POL.VALUE=0
DRIVER.EQEP.VAR.EQEP1_CAP_CLK_PRESCALER.VALUE=PS_8
DRIVER.EQEP.VAR.EQEP2_QDC_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP1_QCLM.VALUE=ON_POSITION_COUNTER_READ
DRIVER.EQEP.VAR.EQEP1_PC_MODE.VALUE=DIRECTION_COUNT
DRIVER.EQEP.VAR.EQEP2_WTO_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_SWI_ENABLE.VALUE=0
DRIVER.EQEP.VAR.EQEP1_PCR_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_INV_QEPB_POL.VALUE=0
DRIVER.EQEP.VAR.EQEP1_IEL.VALUE=RISING_EDGE
DRIVER.EQEP.VAR.EQEP2_PCSPW.VALUE=0
DRIVER.EQEP.VAR.EQEP1_PC_INIT_VALUE.VALUE=0x00000000
DRIVER.EQEP.VAR.EQEP1_PCLOAD.VALUE=QPOSCNT_EQ_QPSCMP
DRIVER.EQEP.VAR.EQEP2_IEL_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_IEL.VALUE=RISING_EDGE
DRIVER.EQEP.VAR.EQEP1_MAXPC_VALUE.VALUE=0x00000000
DRIVER.EQEP.VAR.EQEP1_INV_QEPI_POL.VALUE=0
DRIVER.EQEP.VAR.EQEP2_QCLM.VALUE=ON_POSITION_COUNTER_READ
DRIVER.EQEP.VAR.EQEP1_STROBE_EVT_INIT_ENABLE.VALUE=0
DRIVER.EQEP.VAR.EQEP2_PCO_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_STROBE_EVT_INIT_ENABLE.VALUE=0
DRIVER.EQEP.VAR.EQEP1_EXT_CLK_RATE.VALUE=RESOLUTION_1x
DRIVER.EQEP.VAR.EQEP1_STROBE_EVT_SELECT.VALUE=DIRECTON_DEPENDENT
DRIVER.EQEP.VAR.EQEP1_UNIT_POS_PRESCALER.VALUE=PS_512
DRIVER.EQEP.VAR.EQEP1_WDPRD.VALUE=0x0000
DRIVER.EQEP.VAR.EQEP1_SEL.VALUE=RISING_EDGE
DRIVER.EQEP.VAR.EQEP1_SOEN.VALUE=0
DRIVER.EQEP.VAR.EQEP2_QPE_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_PC_RST_MODE.VALUE=MAX_POSITION
DRIVER.EQEP.VAR.EQEP1_WDE.VALUE=0
DRIVER.EQEP.VAR.EQEP2_SET_INIT_AT_STARTUP.VALUE=0
DRIVER.EQEP.VAR.EQEP2_UTO_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP1_SWI_ENABLE.VALUE=0
DRIVER.EQEP.VAR.EQEP2_POSITIVE_ROTATION.VALUE=CLOCKWISE
DRIVER.EQEP.VAR.EQEP2_SEL_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_SEL.VALUE=RISING_EDGE
DRIVER.EQEP.VAR.EQEP2_PCU_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_WDE.VALUE=0
DRIVER.EQEP.VAR.EQEP1_SPSEL.VALUE=INDEX_PIN
DRIVER.EQEP.VAR.EQEP1_PCSHDW.VALUE=0
DRIVER.EQEP.VAR.EQEP1_SWAP.VALUE=0
DRIVER.EQEP.VAR.EQEP2_SOEN.VALUE=0
DRIVER.EQEP.VAR.EQEP2_POSCMP.VALUE=0
DRIVER.EQEP.VAR.EQEP1_QUPRD.VALUE=0x00000000
DRIVER.EQEP.VAR.EQEP1_IGATE.VALUE=0
DRIVER.EQEP.VAR.EQEP1_QDC_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_SWAP.VALUE=0
DRIVER.EQEP.VAR.EQEP2_WDPRD.VALUE=0
DRIVER.EQEP.VAR.EQEP1_WTO_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP1_POSITIVE_ROTATION.VALUE=CLOCKWISE
DRIVER.EQEP.VAR.EQEP2_INV_QEPI_POL.VALUE=0
DRIVER.EQEP.VAR.EQEP2_PCM_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP1_IEL_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_EXT_CLK_RATE.VALUE=RESOLUTION_1x
DRIVER.EQEP.VAR.EQEP2_SPSEL.VALUE=INDEX_PIN
DRIVER.EQEP.VAR.EQEP1_PCO_INT_ENA.VALUE=0
DRIVER.EQEP.VAR.EQEP2_INDEX_EVT_SELECT.VALUE=RISING_EDGE
DRIVER.EQEP.VAR.EQEP1_INDEX_EVT_INIT_ENABLE.VALUE=0
DRIVER.EQEP.VAR.EQEP2_PCLOAD.VALUE=QPOSCNT_EQ_QPSCMP
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_11_NUMBER.VALUE=11
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_10_END.VALUE=9
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_7_NUMBER.VALUE=7
DRIVER.FEE.VAR.FEE_START_SECTOR.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_3_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_13_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_4_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_21_START.VALUE=20
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_13_START.VALUE=12
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_9_START.VALUE=8
DRIVER.FEE.VAR.FEE_VS29_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_11_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_VS30_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS22_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS14_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_9_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_32_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_24_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_16_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_11_END.VALUE=10
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_11_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_2_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_VS7_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_2_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_READ_CYCLE_COUNT.VALUE=10
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_5_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_3_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_NUMBER_OF_VIRTUAL_SECTORS.VALUE=4
DRIVER.FEE.VAR.FEE_BLOCK_INDEX15_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX4_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_FLASH_CRC_ENABLE.VALUE=STD_ON
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_26_START.VALUE=25
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_18_START.VALUE=17
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_7_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_12_NUMBER.VALUE=12
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_20_END.VALUE=19
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_12_END.VALUE=11
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_10_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_16_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_5_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_3_NUMBER.VALUE=3
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_32_NUMBER.VALUE=32
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_24_NUMBER.VALUE=24
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_16_NUMBER.VALUE=16
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_13_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_16_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_5_NUMBER.VALUE=5
DRIVER.FEE.VAR.FEE_SECTORS_EEP1.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_33_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_25_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_17_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_21_END.VALUE=20
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_13_END.VALUE=12
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_12_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_16_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_14_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_11_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_5_START.VALUE=4
DRIVER.FEE.VAR.FEE_BLOCK_NUMBER.VALUE=1
DRIVER.FEE.VAR.FEE_VS27_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS19_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS20_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS12_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_7_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_DRIVER_INDEX.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_6_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_13_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_9_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_8_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_VS5_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_30_END.VALUE=29
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_22_END.VALUE=21
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_14_END.VALUE=13
DRIVER.FEE.VAR.FEE_BLOCK_INDEX9_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_12_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX13_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX2_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_6_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_30_START.VALUE=29
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_22_START.VALUE=21
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_14_START.VALUE=13
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_3_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_11_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_7_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_10_NUMBER.VALUE=10
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_26_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_18_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_NUMBER_OF_EEPS.VALUE=1
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_8_NUMBER.VALUE=8
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_31_END.VALUE=30
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_29_NUMBER.VALUE=29
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_23_END.VALUE=22
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_15_END.VALUE=14
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_13_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_13_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_1_NUMBER.VALUE=1
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_30_NUMBER.VALUE=30
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_22_NUMBER.VALUE=22
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_14_NUMBER.VALUE=14
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_10_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_6_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_DEVICE_INDEX.VALUE=0
DRIVER.FEE.VAR.FEE_PAGE_OVERHEAD.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_3_NUMBER.VALUE=3
DRIVER.FEE.VAR.FEE_TI_FEE_SW_MAJOR_VERSION.VALUE=1
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_27_START.VALUE=26
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_19_START.VALUE=18
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_11_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_9_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_8_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_14_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_12_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_9_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_32_END.VALUE=31
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_24_END.VALUE=23
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_16_END.VALUE=15
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_1_END.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_1_START.VALUE=0
DRIVER.FEE.VAR.FEE_VS33_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS25_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS17_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_14_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_4_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_SECTOR_NUMBER.VALUE=1
DRIVER.FEE.VAR.FEE_VS10_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUALPAGE_SIZE.VALUE=8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_5_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_7_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VS3_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX7_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_3_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_1_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_2_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_27_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_19_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_33_END.VALUE=32
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_25_END.VALUE=24
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_17_END.VALUE=16
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_2_END.VALUE=1
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_16_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_14_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX11_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_FLASH_WRITECOUNTER_SAVE.VALUE=STD_ON
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_15_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_VS_INDEX.VALUE=2
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_15_NUMBER.VALUE=15
DRIVER.FEE.VAR.FEE_TI_FEE_SW_PATCH_VERSION.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_10_START.VALUE=9
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_6_START.VALUE=5
DRIVER.FEE.VAR.FEE_JOBERROR_NOTIFICATION.VALUE=JobErrorNotification
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_1_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_10_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_6_NUMBER.VALUE=6
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_27_NUMBER.VALUE=27
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_19_NUMBER.VALUE=19
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_1_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_2_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_26_END.VALUE=25
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_20_NUMBER.VALUE=20
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_18_END.VALUE=17
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_12_NUMBER.VALUE=12
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_8_NUMBER.VALUE=8
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_3_END.VALUE=2
DRIVER.FEE.VAR.FEE_BLOCK_SIZE.VALUE=0x10
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_16_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_15_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_TOTAL_BLOCKS_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_1_NUMBER.VALUE=1
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_8_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_31_START.VALUE=30
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_23_START.VALUE=22
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_15_START.VALUE=14
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_1_SIZE.VALUE=8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_12_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX.VALUE=1
DRIVER.FEE.VAR.FEE_VS31_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS23_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS15_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_15_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_3_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_28_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_27_END.VALUE=26
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_19_END.VALUE=18
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_4_END.VALUE=3
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_15_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_6_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_VS8_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_3_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_5_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_MAXIMUM_BLOCKING_TIME.VALUE=600
DRIVER.FEE.VAR.FEE_VS1_ENABLE.VALUE=1
DRIVER.FEE.VAR.FEE_NO_OF_UNCONFIGURED_BLOCKS_TO_COPY.VALUE=0
DRIVER.FEE.VAR.FEE_FLASH_BANK_NUM.VALUE=7
DRIVER.FEE.VAR.FEE_BLOCK_INDEX16_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_14_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX5_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_11_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_28_START.VALUE=27
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_4_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_13_NUMBER.VALUE=13
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_28_END.VALUE=27
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_5_END.VALUE=4
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_2_START.VALUE=1
DRIVER.FEE.VAR.FEE_SECTOR_OVERHEAD.VALUE=16
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_14_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_12_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_8_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_9_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_4_NUMBER.VALUE=4
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_33_NUMBER.VALUE=32
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_25_NUMBER.VALUE=25
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_17_NUMBER.VALUE=17
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_2_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_TI_FEE_SW_MINOR_VERSION.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_10_NUMBER.VALUE=10
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_6_NUMBER.VALUE=6
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_5_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_29_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_29_END.VALUE=28
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_6_END.VALUE=5
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_16_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_11_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_7_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_11_START.VALUE=10
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_7_START.VALUE=6
DRIVER.FEE.VAR.FEE_VS28_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VERSIONINFO_API.VALUE=STD_ON
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_10_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_11_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_8_DATASETS.VALUE=1
DRIVER.FEE.VAR.MAX_BLOCK_TIME.VALUE=600
DRIVER.FEE.VAR.FEE_VS21_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS13_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_8_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_20_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_12_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VS6_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_WRITE_CYCLES.VALUE=10
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_6_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_5_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_1_OFFSET.VALUE=16
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_7_END.VALUE=6
DRIVER.FEE.VAR.FEE_NUMBER_OF_BLOCKS.VALUE=1
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_BANK.VALUE=1
DRIVER.FEE.VAR.FEE_BLOCK_INDEX14_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_4_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_BLOCK_INDEX3_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_NUMBER_OF_EIGHTBYTEWRITES.VALUE=1
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_1_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_32_START.VALUE=31
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_24_START.VALUE=23
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_16_START.VALUE=15
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_4_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_3_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_11_NUMBER.VALUE=11
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_7_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_9_NUMBER.VALUE=9
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_8_END.VALUE=7
DRIVER.FEE.VAR.FEE_END_SECTOR.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_1_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_2_NUMBER.VALUE=2
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_31_NUMBER.VALUE=31
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_23_NUMBER.VALUE=23
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_15_NUMBER.VALUE=15
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_2_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_FLASH_ERROR_CORRECTION_HANDLING.VALUE=TI_Fee_None
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_4_NUMBER.VALUE=4
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_12_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_9_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_DEVERROR_DETECT.VALUE=STD_ON
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_14_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_21_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_13_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_29_START.VALUE=28
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_15_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_8_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_9_END.VALUE=8
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_3_START.VALUE=2
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_1_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_VS26_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS18_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS11_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_6_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_4_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_VS4_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_16_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_4_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_BLOCK_INDEX8_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_MAX_NUMBER_OF_LINKS.VALUE=256
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_9_EEP.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX12_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX1_ENABLE.VALUE=1
DRIVER.FEE.VAR.FEE_FLASH_ERROR_CORRECTION_ENABLE.VALUE=STD_ON
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_2_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_DATASELECT_BITS.VALUE=0
DRIVER.FEE.VAR.FEE_OPERATING_FREQ.VALUE=150.000
DRIVER.FEE.VAR.FEE_TOTAL_SECTORS.VALUE=32
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_16_NUMBER.VALUE=16
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_20_START.VALUE=19
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_12_START.VALUE=11
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_8_START.VALUE=7
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_15_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_2_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_30_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_22_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_14_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_7_NUMBER.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_28_NUMBER.VALUE=28
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_21_NUMBER.VALUE=21
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_13_NUMBER.VALUE=13
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_9_NUMBER.VALUE=9
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_13_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_9_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_2_NUMBER.VALUE=2
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_33_START.VALUE=32
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_25_START.VALUE=24
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_17_START.VALUE=16
DRIVER.FEE.VAR.FEE_JOBEND_NOTIFICATION.VALUE=JobEndNotification
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_5_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_13_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_12_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_10_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_8_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_7_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_VS32_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS24_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_VS16_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_ENABLE_ECC.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_OVERHEAD.VALUE=24
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_10_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_7_DATASETS.VALUE=1
DRIVER.FEE.VAR.FEE_VS9_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_4_OFFSET.VALUE=0
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_3_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VS2_ENABLE.VALUE=1
DRIVER.FEE.VAR.FEE_BLOCK_INDEX6_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_10_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_6_DEVICE_INDEX.VALUE=0x00000000
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_31_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_23_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_15_BANK.VALUE=7
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_10_SIZE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX10_ENABLE.VALUE=0
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_14_NUMBER.VALUE=14
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_4_START.VALUE=3
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_15_IMED_DATA.VALUE=TRUE
DRIVER.FEE.VAR.FEE_CHECK_BANK7_ACCESS.VALUE=STD_OFF
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_5_WRITE_CYCLES.VALUE=0x8
DRIVER.FEE.VAR.FEE_POLLING_MODE.VALUE=STD_ON
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_5_NUMBER.VALUE=5
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_26_NUMBER.VALUE=26
DRIVER.FEE.VAR.FEE_VIRTUAL_SECTOR_18_NUMBER.VALUE=18
DRIVER.FEE.VAR.FEE_BLOCK_INDEX_6_SIZE.VALUE=0
DRIVER.AJSM.VAR.AJSM_NEW_KEY_WORD_2.VALUE=0xFFFDFFFE
DRIVER.AJSM.VAR.AJSM_NEW_KEY_WORD_3.VALUE=0xFFEFFFFF
DRIVER.AJSM.VAR.AJSM_VISIBLE_KEY_WORD_0.VALUE=0xEFFDFFFF
DRIVER.AJSM.VAR.AJSM_VISIBLE_KEY_WORD_1.VALUE=0xFFFFFFFF
DRIVER.AJSM.VAR.AJSM_VISIBLE_KEY_WORD_2.VALUE=0xFFFDFFFE
DRIVER.AJSM.VAR.AJSM_VISIBLE_KEY_WORD_3.VALUE=0xFFEFFFFF
DRIVER.AJSM.VAR.AJSM_SCAN_PATTERN_WORD_0.VALUE=PATTERN_NOT_REQUIRED
DRIVER.AJSM.VAR.AJSM_VISIBLE_KEY_ECC_BYTE_0.VALUE=0xED
DRIVER.AJSM.VAR.AJSM_SCAN_PATTERN_WORD_1.VALUE=PATTERN_NOT_REQUIRED
DRIVER.AJSM.VAR.AJSM_VISIBLE_KEY_ECC_BYTE_1.VALUE=0xED
DRIVER.AJSM.VAR.AJSM_SCAN_PATTERN_WORD_2.VALUE=PATTERN_NOT_REQUIRED
DRIVER.AJSM.VAR.AJSM_SCAN_PATTERN_WORD_3.VALUE=PATTERN_NOT_REQUIRED
DRIVER.AJSM.VAR.AJSM_NEW_KEY_ECC_BYTE_0.VALUE=0xED
DRIVER.AJSM.VAR.AJSM_NEW_KEY_ECC_BYTE_1.VALUE=0xED
DRIVER.AJSM.VAR.AJSM_SCAN_PATTERN.VALUE=PATTERN_NOT_REQUIRED
DRIVER.AJSM.VAR.AJSM_NEW_KEY_WORD_0.VALUE=0xEFFDFFFF
DRIVER.AJSM.VAR.AJSM_NEW_KEY_WORD_1.VALUE=0xFFFFFFFF
