{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Cross Reference Tool","MCU Database","MSP Database","Parametric"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cross Reference Tool","index":0,"n_rows":38,"n_cols":27,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
[null,"Input Competitor Part No:","R5F52105"]
[null,null,"R5F52105BDFP","MSP432P401M","MSP430FR6035","MSP430F5419A","MSP430FR69791","MSP430F6765","MSP430F67651","MSP430F67451A","MSP430F6765A","MSP430F6775","MSP430F6775A","MSP430FR6879","MSP430FR6889","MSP430FR6979","MSP430FR68791","MSP430FR6989","MSP430F6745","MSP430F67451","MSP430FR69891","MSP430F67651A","MSP430F6745A","MSP430F67751A","MSP430F67751","MSP430FR6005","MSP430FR6045"]
[null,"Vendor","Renesas","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI","TI"]
[null,"CPU","RX","ARM CM4F","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430","MSP430"]
[null,"CPU-Freq/MHz",50,48,16,25,16,25,25,25,25,25,25,16,16,16,16,16,25,25,16,25,25,25,25,16,16]
[null,"NVM/kB",128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128]
[null,"EEPROM/kB",8,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"RAM/kB",20,32,8,16,2,16,16,16,16,16,16,2,2,2,2,2,16,16,2,16,16,16,16,8,8]
[null,"ADC Resolution",null,14,12,12,12,24,24,24,24,24,24,12,12,12,12,12,24,24,12,24,24,24,24,12,12]
[null,"ADC Channel #",16,24,16,14,16,6,6,4,6,7,7,16,16,16,16,16,4,4,16,6,4,7,7,16,16]
[null,"DAC",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"COMP",null,16,16,0,16,0,0,0,0,0,0,16,16,16,16,16,0,0,16,0,0,0,0,16,16]
[null,"IO count",85,84,80,87,83,90,90,90,90,90,90,83,83,83,83,83,90,90,83,90,90,90,90,81,80]
[null,"LCD",null,"No","Yes","No","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","No","Yes"]
[null,"I2C",8,4,2,4,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
[null,"SPI",8,8,6,8,4,6,6,6,6,6,6,4,4,4,4,4,6,6,4,6,6,6,6,4,6]
[null,"I2S"]
[null,"USB",null,"No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No"]
[null,"Timer",14,6,6,3,5,4,4,4,4,4,4,5,5,5,5,5,4,4,5,4,4,4,4,6,6]
[null,"Other Timers",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RTC, CRC"]
[null,"Tempmin",-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40,-40]
[null,"Tempmax",85,85,85,85,85,85,85,85,85,85,85,85,85,85,85,85,85,85,85,85,85,85,85,105,85]
[null,"Vmin/V",1.62,1.62,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8,1.8]
[null,"Vmax/V",5.5,3.7,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6,3.6]
[null,"PIN count",100,100,100,113,100,100,100,100,100,100,100,100,100,100,100,100,100,100,100,100,100,100,100,100,100]
[null,"Package","100LFQFP","LQFP|100, NFBGA|80, VQFN|64","LQFP|100","BGA MICROSTAR JUNIOR|113, LQFP|100","LQFP|100, LQFP|80","LQFP|100, LQFP|128","LQFP|100, LQFP|128","LQFP|100, LQFP|128","LQFP|100, LQFP|128","LQFP|100, LQFP|128","LQFP|100, LQFP|128","LQFP|100, LQFP|80","LQFP|100, LQFP|80","LQFP|100, LQFP|80","LQFP|100, LQFP|80","LQFP|100, LQFP|80","LQFP|100, LQFP|128","LQFP|100, LQFP|128","LQFP|100, LQFP|80","LQFP|100, LQFP|128","LQFP|100, LQFP|128","LQFP|100, LQFP|128","LQFP|100, LQFP|128","LQFP|100","LQFP|100"]
[null,"Price",null,null,2.1800000000000002,2.2000000000000002,2.25,2.76,2.76,2.76,2.76,2.76,2.76,2.9,2.9,2.95,3,3.3,3.31,3.4,3.43,3.6,3.63,3.8,3.8,4.5,8.17]
[null,"USART"]
[null,"UART",7,4,4,4,2,4,4,4,4,4,4,2,2,2,2,2,4,4,2,4,4,4,4,4,4]
[null,"Power-sleep/uA",null,80]
[null,"Power-AM/(uA/MHz)",null,0.66]
[null,"Cap Touch",null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Crypto"]
[null,"TRNG"]
[null,"Status","Mass Production",null,"ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE","ACTIVE"]
[null,"Others",""]
[null,"OPA"]
[null,"Special Feaures"]

{"sheet":"MCU Database","index":1,"n_rows":13307,"n_cols":56,"rows_kept":2250,"cut":true,"hidden":true,"merged":[],"bounds":{"rows_first":1000,"rows_last":250,"rows_between":1000,"halvings":1}}
["PN","Vendor&GPN","Vendor","CPU","CPUFreq/MHz","NVM/kB","EEPROM/kB","RAM/kB","ADC Resolution","ADC Channel #","DAC","COMP","IO count","LCD","I2C","SPI","I2S","USB","Timer","Other Timers","Tempmin","Tempmax","Vmin/V","Vmax/V","pin count","Package","Price","USART","UART","Powersleep/uA","PowerAM/(uA/MHz)","Cap Touch Buttons","Crypto","TRNG","Status","Others","Description","OPA","Special Feaures","LCD (Raw)","USB (Raw)","Cap Touch (Y/N)"]
["MKM33Z128ACLH5","NXPMKM33Z128ACLH5","NXP","ARM CM0+",50,128,null,16,16,null,2,null,38,"Yes",2,2,null,"No",1,null,-40,85,1.71,3.6,64,"LQFP64",1.8,null,4,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, Segment LCD, 64LQFP",null,null,null,0]
["MKM33Z128ACLH5R","NXPMKM33Z128ACLH5R","NXP","ARM CM0+",50,128,null,16,16,null,2,null,38,"Yes",2,2,null,"No",1,null,-40,85,1.71,3.6,64,"LQFP64",1.8,null,4,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, Segment LCD, 64LQFP",null,null,null,0]
["MKM33Z128ACLL5","NXPMKM33Z128ACLL5","NXP","ARM CM0+",50,128,null,16,16,null,2,null,68,"Yes",2,2,null,"No",1,null,-40,85,1.71,3.6,100,"LQFP100",1.88,null,4,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, Segment LCD, 100LQFP",null,null,null,0]
["MKM33Z128ACLL5R","NXPMKM33Z128ACLL5R","NXP","ARM CM0+",50,128,null,16,16,null,2,null,68,"Yes",2,2,null,"No",1,null,-40,85,1.71,3.6,100,"LQFP100",1.88,null,4,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, Segment LCD, 100LQFP",null,null,null,0]
["MKM33Z64ACLH5","NXPMKM33Z64ACLH5","NXP","ARM CM0+",50,64,null,16,16,null,2,null,38,"Yes",2,2,null,"No",1,null,-40,85,1.71,3.6,64,"LQFP64",1.57,null,4,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 64KB Flash, 16KB SRAM, Segment LCD, 64LQFP",null,null,null,0]
["MKM33Z64ACLH5R","NXPMKM33Z64ACLH5R","NXP","ARM CM0+",50,64,null,16,16,null,2,null,38,"Yes",2,2,null,"No",1,null,-40,85,1.71,3.6,64,"LQFP64",1.57,null,4,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 64KB Flash, 16KB SRAM, Segment LCD, 64LQFP",null,null,null,0]
["MKM33Z64ACLL5","NXPMKM33Z64ACLL5","NXP","ARM CM0+",50,64,null,16,16,null,2,null,68,"Yes",2,2,null,"No",1,null,-40,85,1.71,3.6,100,"LQFP100",1.67,null,4,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 64KB Flash, 16KB SRAM, Segment LCD, 100LQFP",null,null,null,0]
["MKM33Z64ACLL5R","NXPMKM33Z64ACLL5R","NXP","ARM CM0+",50,64,null,16,16,null,2,null,68,"Yes",2,2,null,"No",1,null,-40,85,1.71,3.6,100,"LQFP100",1.67,null,4,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 64KB Flash, 16KB SRAM, Segment LCD, 100LQFP",null,null,null,0]
["MKM34Z128ACLL5","NXPMKM34Z128ACLL5","NXP","ARM CM0+",50,128,null,16,16,null,2,null,68,"Yes",2,2,null,"No",1,null,-40,85,1.71,3.6,100,"LQFP100",2.02,null,4,null,null,null,null,null,null,null,"Kinetis KM34: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, Segment LCD, 100LQFP,",null,null,null,0]
["MKM34Z128ACLL5R","NXPMKM34Z128ACLL5R","NXP","ARM CM0+",50,128,null,16,16,null,2,null,68,"Yes",2,2,null,"No",1,null,-40,85,1.71,3.6,100,"LQFP100",2.02,null,4,null,null,null,null,null,null,null,"Kinetis KM34: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, Segment LCD, 100LQFP,",null,null,null,0]
["MKV10Z128VFM7","NXPMKV10Z128VFM7","NXP","ARM CM0+",75,128,null,16,16,null,1,null,28,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.18,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 128KB Flash, 16KB SRAM, 32QFN",null,null,null,0]
["MKV10Z128VLF7","NXPMKV10Z128VLF7","NXP","ARM CM0+",75,128,null,16,16,null,1,null,40,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.29,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 128KB Flash, 16KB SRAM, 48LQFP",null,null,null,0]
["MKV10Z128VLH7","NXPMKV10Z128VLH7","NXP","ARM CM0+",75,128,null,16,16,null,1,null,54,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.42,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 128KB Flash, 16KB SRAM, 64LQFP",null,null,null,0]
["MKV10Z16VFM7","NXPMKV10Z16VFM7","NXP","ARM CM0+",75,16,null,8,16,null,1,null,28,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",0.89,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 16KB Flash, 8KB SRAM, 32QFN",null,null,null,0]
["MKV10Z16VLC7","NXPMKV10Z16VLC7","NXP","ARM CM0+",75,16,null,8,16,null,1,null,28,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,null,"LQFP",0.84,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 16KB Flash, 8KB SRAM, 32LQFP",null,null,null,0]
["MKV10Z16VLF7","NXPMKV10Z16VLF7","NXP","ARM CM0+",75,16,null,8,16,null,1,null,40,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.02,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 16KB Flash, 8KB SRAM, 48LQFP",null,null,null,0]
["MKV10Z32VFM7","NXPMKV10Z32VFM7","NXP","ARM CM0+",75,32,null,8,16,null,1,null,28,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",0.97,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 32KB Flash, 8KB SRAM, 32QFN",null,null,null,0]
["MKV10Z32VFM7R","NXPMKV10Z32VFM7R","NXP","ARM CM0+",75,32,null,8,16,null,1,null,28,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",0.97,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 32KB Flash, 8KB SRAM, 32QFN",null,null,null,0]
["MKV10Z32VLC7","NXPMKV10Z32VLC7","NXP","ARM CM0+",75,32,null,8,16,null,1,null,28,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,null,"LQFP",0.94,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 32KB Flash, 8KB SRAM, 32LQFP",null,null,null,0]
["MKV10Z32VLC7R","NXPMKV10Z32VLC7R","NXP","ARM CM0+",75,32,null,8,16,null,1,null,28,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,null,"LQFP",0.94,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 32KB Flash, 8KB SRAM, 32LQFP",null,null,null,0]
["MKV10Z32VLF7","NXPMKV10Z32VLF7","NXP","ARM CM0+",75,32,null,8,16,null,1,null,40,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.1100000000000001,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 32KB Flash, 8KB SRAM, 48LQFP",null,null,null,0]
["MKV10Z64VFM7","NXPMKV10Z64VFM7","NXP","ARM CM0+",75,64,null,16,16,null,1,null,28,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.07,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 64KB Flash, 16KB SRAM, 32QFN",null,null,null,0]
["MKV10Z64VFM7R","NXPMKV10Z64VFM7R","NXP","ARM CM0+",75,64,null,16,16,null,1,null,28,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.07,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 64KB Flash, 16KB SRAM, 32QFN",null,null,null,0]
["MKV10Z64VLF7","NXPMKV10Z64VLF7","NXP","ARM CM0+",75,64,null,16,16,null,1,null,40,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.21,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 64KB Flash, 16KB SRAM, 48LQFP",null,null,null,0]
["MKV10Z64VLF7R","NXPMKV10Z64VLF7R","NXP","ARM CM0+",75,64,null,16,16,null,1,null,40,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.21,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 64KB Flash, 16KB SRAM, 48LQFP",null,null,null,0]
["MKV10Z64VLH7","NXPMKV10Z64VLH7","NXP","ARM CM0+",75,64,null,16,16,null,1,null,54,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.34,null,2,null,null,null,null,null,null,null,"Kinetis KV10: 75MHz CortexM0+ Realtime Control MCU, 64KB Flash, 16KB SRAM, 64LQFP",null,null,null,0]
["MKV11Z128VFM7","NXPMKV11Z128VFM7","NXP","ARM CM0+",75,128,null,16,16,null,1,null,28,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.21,null,2,null,null,null,null,null,null,null,"Kinetis KV11: 75MHz CortexM0+ Realtime Control MCU, 128KB Flash, 16KB SRAM, CAN, 32QFN",null,null,null,0]
["MKV11Z128VLF7","NXPMKV11Z128VLF7","NXP","ARM CM0+",75,128,null,16,16,null,1,null,40,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.33,null,2,null,null,null,null,null,null,null,"Kinetis KV11: 75MHz CortexM0+ Realtime Control MCU, 128KB Flash, 16KB SRAM, CAN, 48LQFP",null,null,null,0]
["MKV11Z128VLH7","NXPMKV11Z128VLH7","NXP","ARM CM0+",75,128,null,16,16,null,1,null,54,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.46,null,2,null,null,null,null,null,null,null,"Kinetis KV11: 75MHz CortexM0+ Realtime Control MCU, 128KB Flash, 16KB SRAM, CAN, 64LQFP",null,null,null,0]
["MKV11Z64VFM7","NXPMKV11Z64VFM7","NXP","ARM CM0+",75,64,null,16,16,null,1,null,28,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.1200000000000001,null,2,null,null,null,null,null,null,null,"Kinetis KV11: 75MHz CortexM0+ Realtime Control MCU, 64KB Flash, 16KB SRAM, CAN, 32QFN",null,null,null,0]
["MKV11Z64VLF7","NXPMKV11Z64VLF7","NXP","ARM CM0+",75,64,null,16,16,null,1,null,40,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.26,null,2,null,null,null,null,null,null,null,"Kinetis KV11: 75MHz CortexM0+ Realtime Control MCU, 64KB Flash, 16KB SRAM, CAN, 48LQFP",null,null,null,0]
["MKV11Z64VLH7","NXPMKV11Z64VLH7","NXP","ARM CM0+",75,64,null,16,16,null,1,null,54,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.38,null,2,null,null,null,null,null,null,null,"Kinetis KV11: 75MHz CortexM0+ Realtime Control MCU, 64KB Flash, 16KB SRAM, CAN, 64LQFP",null,null,null,0]
["MKV30F128VFM10","NXPMKV30F128VFM10","NXP","ARM CM4F",100,128,null,16,16,null,1,null,26,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.33,null,2,null,null,null,null,null,null,null,"Kinetis KV30: 100MHz CortexM4F Realtime Control MCU, 128KB Flash, 16KB SRAM, 32QFN",null,null,null,0]
["MKV30F128VLF10","NXPMKV30F128VLF10","NXP","ARM CM4F",100,128,null,16,16,null,1,null,35,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.46,null,2,null,null,null,null,null,null,null,"Kinetis KV30: 100MHz CortexM4F Realtime Control MCU, 128KB Flash, 16KB SRAM, 48LQFP",null,null,null,0]
["MKV30F128VLH10","NXPMKV30F128VLH10","NXP","ARM CM4F",100,128,null,16,16,null,1,null,46,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.49,null,2,null,null,null,null,null,null,null,"Kinetis KV30: 100MHz CortexM4F Realtime Control MCU, 128KB Flash, 16KB SRAM, 64LQFP",null,null,null,0]
["MKV30F64VFM10","NXPMKV30F64VFM10","NXP","ARM CM4F",100,64,null,16,16,null,1,null,26,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.1399999999999999,null,2,null,null,null,null,null,null,null,"Kinetis KV30: 100MHz CortexM4F Realtime Control MCU, 64KB Flash, 16KB SRAM, 32QFN",null,null,null,0]
["MKV30F64VLF10","NXPMKV30F64VLF10","NXP","ARM CM4F",100,64,null,16,16,null,1,null,35,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.27,null,2,null,null,null,null,null,null,null,"Kinetis KV30: 100MHz CortexM4F Realtime Control MCU, 64KB Flash, 16KB SRAM, 48LQFP",null,null,null,0]
["MKV30F64VLF10R","NXPMKV30F64VLF10R","NXP","ARM CM4F",100,64,null,16,16,null,1,null,35,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.27,null,2,null,null,null,null,null,null,null,"Kinetis KV30: 100MHz CortexM4F Realtime Control MCU, 64KB Flash, 16KB SRAM, 48LQFP",null,null,null,0]
["MKV30F64VLH10","NXPMKV30F64VLH10","NXP","ARM CM4F",100,64,null,16,16,null,1,null,46,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.39,null,2,null,null,null,null,null,null,null,"Kinetis KV30: 100MHz CortexM4F Realtime Control MCU, 64KB Flash, 16KB SRAM, 64LQFP",null,null,null,0]
["MKV31F128VLH10","NXPMKV31F128VLH10","NXP","ARM CM4F",100,128,null,24,16,null,1,null,46,"No",2,2,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.54,null,4,null,null,null,null,null,null,null,"Kinetis KV31: 100MHz CortexM4F Realtime Control MCU, 128KB Flash, 24KB SRAM, 64LQFP",null,null,null,0]
["MKV31F128VLL10","NXPMKV31F128VLL10","NXP","ARM CM4F",100,128,null,24,16,null,1,null,70,"No",2,2,null,"No",1,null,-40,105,1.71,3.6,100,"LQFP100",1.54,null,4,null,null,null,null,null,null,null,"Kinetis KV31: 100MHz CortexM4F Realtime Control MCU, 128KB Flash, 24KB SRAM, 100LQFP",null,null,null,0]
["MKV31F256VLH12","NXPMKV31F256VLH12","NXP","ARM CM4F",120,256,null,48,16,null,1,null,46,"No",2,2,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.74,null,4,null,null,null,null,null,null,null,"Kinetis KV31: 120MHz CortexM4F Realtime Control MCU, 256K Flash, 48K RAM, KMS enabled, 64LQFP,",null,null,null,0]
["MKV31F256VLH12R","NXPMKV31F256VLH12R","NXP","ARM CM4F",120,256,null,48,16,null,1,null,46,"No",2,2,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.74,null,4,null,null,null,null,null,null,null,"Kinetis KV31: 120MHz CortexM4F Realtime Control MCU, 256K Flash, 48K RAM, KMS enabled, 64LQFP,",null,null,null,0]
["MKV31F256VLL12","NXPMKV31F256VLL12","NXP","ARM CM4F",120,256,null,48,16,null,1,null,70,"No",2,2,null,"No",1,null,-40,105,1.71,3.6,100,"LQFP100",1.85,null,4,null,null,null,null,null,null,null,"Kinetis KV31: 120MHz CortexM4F Realtime Control MCU, 256KB Flash, 48KB SRAM, 100LQFP",null,null,null,0]
["MKV31F512VLH12","NXPMKV31F512VLH12","NXP","ARM CM4F",120,512,null,96,16,null,2,null,46,"No",2,2,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",2.2200000000000002,null,4,null,null,null,null,null,null,null,"Kinetis KV31: 120MHz CortexM4F Realtime Control MCU, 512KB Flash, 96KB SRAM, 64LQFP",null,null,null,0]
["MKV31F512VLH12R","NXPMKV31F512VLH12R","NXP","ARM CM4F",120,512,null,96,16,null,2,null,46,"No",2,2,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",2.2200000000000002,null,4,null,null,null,null,null,null,null,"Kinetis KV31: 120MHz CortexM4F Realtime Control MCU, 512KB Flash, 96KB SRAM, 64LQFP",null,null,null,0]
["MKV31F512VLL12","NXPMKV31F512VLL12","NXP","ARM CM4F",120,512,null,96,16,null,2,null,70,"No",2,2,null,"No",1,null,-40,105,1.71,3.6,100,"LQFP100",2.33,null,4,null,null,null,null,null,null,null,"Kinetis KV31: 120MHz CortexM4F Realtime Control MCU, 512KB Flash, 96KB SRAM, 100LQFP",null,null,null,0]
["MKV42F128VLF16","NXPMKV42F128VLF16","NXP","ARM CM4F",168,128,null,24,12,null,4,null,38,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.29,null,2,null,null,null,null,null,null,null,"Kinetis KV42: 168MHz CortexM4F Realtime Control MCU, 128KB Flash, 24KB SRAM, 3xFlexTimer, 48LQFP",null,null,null,0]
["MKV42F128VLH16","NXPMKV42F128VLH16","NXP","ARM CM4F",168,128,null,24,12,null,4,null,48,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.35,null,2,null,null,null,null,null,null,null,"Kinetis KV42: 168MHz CortexM4F Realtime Control MCU, 128KB Flash, 24KB SRAM, 3xFlexTimer, 64LQFP",null,null,null,0]
["MKV42F128VLL16","NXPMKV42F128VLL16","NXP","ARM CM4F",168,128,null,24,12,null,4,null,74,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,100,"LQFP100",1.43,null,2,null,null,null,null,null,null,null,"Kinetis KV42: 168MHz CortexM4F Realtime Control MCU, 128KB Flash, 24KB SRAM, 3xFlexTimer, 100LQFP",null,null,null,0]
["MKV42F256VLH16","NXPMKV42F256VLH16","NXP","ARM CM4F",168,256,null,32,12,null,4,null,48,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.5,null,2,null,null,null,null,null,null,null,"Kinetis KV42: 168MHz CortexM4F Realtime Control MCU, 256KB Flash, 32KB SRAM, 3xFlexTimer, 64LQFP",null,null,null,0]
["MKV42F256VLL16","NXPMKV42F256VLL16","NXP","ARM CM4F",168,256,null,32,12,null,4,null,74,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,100,"LQFP100",2.4,null,2,null,null,null,null,null,null,null,"Kinetis KV42: 168MHz CortexM4F Realtime Control MCU, 256KB Flash, 32KB SRAM, 3xFlexTimer, 100LQFP",null,null,null,0]
["MKV42F64VLF16","NXPMKV42F64VLF16","NXP","ARM CM4F",168,64,null,16,12,null,4,null,38,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.1399999999999999,null,2,null,null,null,null,null,null,null,"Kinetis KV42: 168MHz CortexM4F Realtime Control MCU, 64KB Flash, 16KB SRAM, 3xFlexTimer, 48LQFP",null,null,null,0]
["MKV42F64VLF16R","NXPMKV42F64VLF16R","NXP","ARM CM4F",168,64,null,16,12,null,4,null,38,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.1399999999999999,null,2,null,null,null,null,null,null,null,"Kinetis KV42: 168MHz CortexM4F Realtime Control MCU, 64KB Flash, 16KB SRAM, 3xFlexTimer, 48LQFP",null,null,null,0]
["MKV42F64VLH16","NXPMKV42F64VLH16","NXP","ARM CM4F",168,64,null,16,12,null,4,null,48,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.2,null,2,null,null,null,null,null,null,null,"Kinetis KV42: 168MHz CortexM4F Realtime Control MCU, 64KB Flash, 16KB SRAM, 3xFlexTimer, 64LQFP",null,null,null,0]
["MKV44F128VLF16","NXPMKV44F128VLF16","NXP","ARM CM4F",168,128,null,24,12,null,5,null,38,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.49,null,2,null,null,null,null,null,null,null,"Kinetis KV44: 168MHz CortexM4F Realtime Ctrl MCU, 128KB Flash, 24KB RAM, DAC, PWM NanoEdge, 48LQFP",null,null,null,0]
["MKV44F64VLF16","NXPMKV44F64VLF16","NXP","ARM CM4F",168,64,null,16,12,null,5,null,38,"No",1,1,null,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.34,null,2,null,null,null,null,null,null,null,"Kinetis KV44: 168MHz CortexM4F Realtime Ctrl MCU, 64KB Flash, 16KB RAM, DAC, PWM NanoEdge, 48LQFP",null,null,null,0]
["MKV56F1M0VLL24","NXPMKV56F1M0VLL24","NXP","ARM CM7",240,1024,null,256,16,null,5,null,74,"No",2,3,null,"No",1,null,-40,105,1.71,3.6,100,"LQFP100",null,null,6,null,null,null,null,null,null,null,"Kinetis KV56: 220MHz CortexM7F RealTime Control MCU, 1MB Flash, 256KB SRAM, 100LQFP",null,null,null,0]
["MKV56F1M0VLQ24","NXPMKV56F1M0VLQ24","NXP","ARM CM7",240,1024,null,256,16,null,5,null,111,"No",2,3,null,"No",1,null,-40,105,1.71,3.6,144,"LQFP144",null,null,6,null,null,null,null,null,null,null,"Kinetis KV56: 220MHz CortexM7F RealTime Control MCU, 1MB Flash, 256KB SRAM, 144LQFP",null,null,null,0]
["MKV56F512VLL24","NXPMKV56F512VLL24","NXP","ARM CM7",240,512,null,128,16,null,5,null,74,"No",2,3,null,"No",1,null,-40,105,1.71,3.6,100,"LQFP100",null,null,6,null,null,null,null,null,null,null,"Kinetis KV56: 220MHz CortexM7F RealTime Control MCU, 512KB Flash, 128KB SRAM, 100LQFP",null,null,null,0]
["MKV56F512VLQ24","NXPMKV56F512VLQ24","NXP","ARM CM7",240,512,null,128,16,null,5,null,111,"No",2,3,null,"No",1,null,-40,105,1.71,3.6,144,"LQFP144",null,null,6,null,null,null,null,null,null,null,"Kinetis KV56: 220MHz CortexM7F RealTime Control MCU, 512KB Flash, 128KB SRAM, 144LQFP",null,null,null,0]
["MKV56F512VLQ24R","NXPMKV56F512VLQ24R","NXP","ARM CM7",240,512,null,128,16,null,5,null,111,"No",2,3,null,"No",1,null,-40,105,1.71,3.6,144,"LQFP144",null,null,6,null,null,null,null,null,null,null,"Kinetis KV56: 220MHz CortexM7F RealTime Control MCU, 512KB Flash, 128KB SRAM, 144LQFP",null,null,null,0]
["MKV58F1M0VLL24","NXPMKV58F1M0VLL24","NXP","ARM CM7",240,1024,null,256,16,null,5,null,74,"No",2,3,null,"No",1,null,-40,105,1.71,3.6,100,"LQFP100",null,null,6,null,null,null,null,null,null,null,"Kinetis KV58: 220MHz CortexM7F RealTime Control MCU, 1MB Flash, 256KB SRAM, Ethernet, 100LQFP",null,null,null,0]
["MKV58F512VLL24","NXPMKV58F512VLL24","NXP","ARM CM7",240,512,null,128,16,null,5,null,74,"No",2,3,null,"No",1,null,-40,105,1.71,3.6,100,"LQFP100",null,null,6,null,null,null,null,null,null,null,"Kinetis KV58: 220MHz CortexM7F RealTime Control MCU, 512KB Flash, 128KB SRAM, Ethernet, 100LQFP",null,null,null,0]
["MKV58F512VLQ24","NXPMKV58F512VLQ24","NXP","ARM CM7",240,512,null,128,16,null,5,null,111,"No",2,3,null,"No",1,null,-40,105,1.71,3.6,144,"LQFP144",null,null,6,null,null,null,null,null,null,null,"Kinetis KV58: 220MHz CortexM7F RealTime Control MCU, 512KB Flash, 128KB SRAM, Ethernet, 144LQFP",null,null,null,0]
["MKL43Z128VLH4","NXPMKL43Z128VLH4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,50,"Yes",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.88,null,3,null,null,null,null,null,null,null,"Kinetis KL43: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB SRAM, USB, Segment LCD, 64LQFP",null,null,null,1]
["MKL43Z128VMP4","NXPMKL43Z128VMP4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,50,"Yes",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LFBGA64",1.93,null,3,null,null,null,null,null,null,null,"Kinetis KL43: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB RAM, USB, Segment LCD, 64BGA",null,null,null,1]
["MKL43Z256VLH4","NXPMKL43Z256VLH4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,50,"Yes",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",2.1800000000000002,null,3,null,null,null,null,null,null,null,"Kinetis KL43: 48MHz CortexM0+ UltraLow Power MCU, 256KB Flash, 32KB SRAM, USB, Segment LCD, 64LQFP",null,null,null,1]
["MKL43Z256VMP4","NXPMKL43Z256VMP4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,50,"Yes",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LFBGA64",2.23,null,3,null,null,null,null,null,null,null,"Kinetis KL43: 48MHz CortexM0+ UltraLow Power MCU, 256KB Flash, 32KB RAM, USB, Segment LCD, 64BGA",null,null,null,1]
["MKL46Z128VLH4","NXPMKL46Z128VLH4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,50,"Yes",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",2,null,3,null,null,null,null,null,null,null,"Kinetis KL46: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB SRAM, USB, Segment LCD, 64LQFP",null,null,null,1]
["MKL46Z128VLL4","NXPMKL46Z128VLL4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,84,"Yes",2,2,1,"Yes",null,null,-40,105,1.71,3.6,100,"LQFP100",2.16,null,3,null,null,null,null,null,null,null,"Kinetis KL46: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB RAM, USB, Segment LCD, 100LQFP",null,null,null,1]
["MKL46Z128VMC4","NXPMKL46Z128VMC4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,84,"Yes",2,2,1,"Yes",null,null,-40,105,1.71,3.6,121,"LFBGA121",2.2599999999999998,null,3,null,null,null,null,null,null,null,"Kinetis KL46: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB RAM, USB, Segment LCD, 121BGA",null,null,null,1]
["MKL46Z256VLH4","NXPMKL46Z256VLH4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,50,"Yes",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",2.2999999999999998,null,3,null,null,null,null,null,null,null,"Kinetis KL46: 48MHz CortexM0+ UltraLow Power MCU, 256KB Flash, 32KB SRAM, USB, Segment LCD, 64LQFP",null,null,null,1]
["MKL46Z256VLL4","NXPMKL46Z256VLL4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,84,"Yes",2,2,1,"Yes",null,null,-40,105,1.71,3.6,100,"LQFP100",2.46,null,3,null,null,null,null,null,null,null,"Kinetis KL46: 48MHz CortexM0+ UltraLow Power MCU, 256KB Flash, 32KB RAM, USB, Segment LCD, 100LQFP",null,null,null,1]
["MKL46Z256VMC4","NXPMKL46Z256VMC4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,84,"Yes",2,2,1,"Yes",null,null,-40,105,1.71,3.6,121,"LFBGA121",2.56,null,3,null,null,null,null,null,null,null,"Kinetis KL46: 48MHz CortexM0+ UltraLow Power MCU, 256KB Flash, 32KB RAM, USB, Segment LCD, 121BGA",null,null,null,1]
["MKL46Z256VMP4","NXPMKL46Z256VMP4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,50,"Yes",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LFBGA64",2.35,null,3,null,null,null,null,null,null,null,"Kinetis KL46: 48MHz CortexM0+ UltraLow Power MCU, 256KB Flash, 32KB RAM, USB, Segment LCD, 64BGA",null,null,null,1]
["MKL81Z128VLK7","NXPMKL81Z128VLK7","NXP","ARM CM0+",72,128,null,96,16,null,1,null,56,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,80,"LQFP80",2.99,null,3,null,null,null,null,null,null,null,"Kinetis KL81: 72MHz CortexM0+ Secure LowPower MCU, 128KB Flash, 96KB RAM, USB, Antitamper, 80LQFP",null,null,null,1]
["MKL81Z128VMC7","NXPMKL81Z128VMC7","NXP","ARM CM0+",72,128,null,96,16,null,1,null,85,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,121,"LFBGA121",2.99,null,3,null,null,null,null,null,null,null,"Kinetis KL81: 72MHz CortexM0+ Secure LowPower MCU, 128KB Flash, 96KB RAM, USB, Antitamper, 121BGA",null,null,null,1]
["MKL81Z128VMC7R","NXPMKL81Z128VMC7R","NXP","ARM CM0+",72,128,null,96,16,null,1,null,85,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,121,"LFBGA121",2.99,null,3,null,null,null,null,null,null,null,"Kinetis KL81: 72MHz CortexM0+ Secure LowPower MCU, 128KB Flash, 96KB RAM, USB, Antitamper, 121BGA",null,null,null,1]
["MKL81Z128VMP7","NXPMKL81Z128VMP7","NXP","ARM CM0+",72,128,null,96,16,null,1,null,41,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,64,"LFBGA64",2.89,null,3,null,null,null,null,null,null,null,"Kinetis KL81: 72MHz CortexM0+ Secure LowPower MCU, 128KB Flash, 96KB RAM, USB, Antitamper, 64BGA",null,null,null,1]
["MKL82Z128VLK7","NXPMKL82Z128VLK7","NXP","ARM CM0+",72,128,null,96,16,null,1,null,56,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,80,"LQFP80",2.79,null,3,null,null,null,null,null,null,null,"Kinetis KL82: 72MHz CortexM0+ Secure LowPower MCU, 128KB Flash, 96KB SRAM, USB, 80LQFP",null,null,null,1]
["MKL82Z128VLK7R","NXPMKL82Z128VLK7R","NXP","ARM CM0+",72,128,null,96,16,null,1,null,56,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,80,"LQFP80",2.79,null,3,null,null,null,null,null,null,null,"Kinetis KL82: 72MHz CortexM0+ Secure LowPower MCU, 128KB Flash, 96KB SRAM, USB, 80LQFP",null,null,null,1]
["MKL82Z128VMC7","NXPMKL82Z128VMC7","NXP","ARM CM0+",72,128,null,96,16,null,1,null,85,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,121,"LFBGA121",3.18,null,3,null,null,null,null,null,null,null,"Kinetis KL82: 72MHz CortexM0+ Secure LowPower MCU, 128KB Flash, 96KB RAM, USB, 121MAPBGA",null,null,null,1]
["MKL82Z128VMP7","NXPMKL82Z128VMP7","NXP","ARM CM0+",72,128,null,96,16,null,1,null,41,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,64,"LFBGA64",2.79,null,3,null,null,null,null,null,null,null,"Kinetis KL82: 72MHz CortexM0+ Secure LowPower MCU, 128KB Flash, 96KB SRAM, USB, 64BGA",null,null,null,1]
["LPC1114FN28/102,12","NXPLPC1114FN28/102,12","NXP","ARM CM0",50,32,null,4,10,null,0,null,22,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,28,"DIP28",null,null,1,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores"]
["LPC4072FBD80E","NXPLPC4072FBD80E","NXP","ARM CM4",120,512,null,null,12,null,1,null,null,"Yes",null,null,null,"No",null,null,0,null,null,null,80,"LQFP80",null,null,null,null,null,null,null,null,null,null,"32bit ARM CM4 MCU; up to 512 kB flash, 96 kB SRAM; USB Device/Host/OTG; Ethernet; EMC; SPIFI"]
["LPC810M021FN8FP","NXPLPC810M021FN8FP","NXP","ARM CM0+",30,16,null,null,0,null,0,null,null,"No",null,null,null,"No",null,null,0,null,null,null,8,"DIP8",null,null,null,null,null,null,null,null,null,null,"Low Cost 32bit Microcontroller (MCU) based on ARM CM0+ Core"]
["MK11DN512VLK5","NXPMK11DN512VLK5","NXP","ARM CM4",50,512,null,64,16,null,0,null,60,"No",2,2,1,"No",13,null,-40,105,1.71,3.6,80,"LQFP80",null,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, Antitamper, 80LQFP",null,null,null,0]
["MK11DN512VLK5R","NXPMK11DN512VLK5R","NXP","ARM CM4",50,512,null,64,16,null,0,null,60,"No",2,2,1,"No",13,null,-40,105,1.71,3.6,80,"LQFP80",null,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, Antitamper, 80LQFP",null,null,null,0]
["MK11DN512VMC5","NXPMK11DN512VMC5","NXP","ARM CM4",50,512,null,64,16,null,1,null,64,"No",2,2,1,"No",13,null,-40,105,1.71,3.6,121,"LFBGA121",null,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, Antitamper, 121MAPBGA",null,null,null,0]
["MK11DX128VLK5","NXPMK11DX128VLK5","NXP","ARM CM4",50,192,4,32,16,null,0,null,60,"No",2,2,1,"No",13,null,-40,105,1.71,3.6,80,"LQFP80",null,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 192KB Flash, 32KB SRAM, Antitamper, 80LQFP",null,null,null,0]
["MK11DX128VMC5","NXPMK11DX128VMC5","NXP","ARM CM4",50,192,4,32,16,null,1,null,64,"No",2,2,1,"No",13,null,-40,105,1.71,3.6,121,"LFBGA121",null,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 192KB Flash, 32KB SRAM, Antitamper, 121MAPBGA",null,null,null,0]
["MK11DX256VLK5","NXPMK11DX256VLK5","NXP","ARM CM4",50,320,4,32,16,null,0,null,60,"No",2,2,1,"No",13,null,-40,105,1.71,3.6,80,"LQFP80",null,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 320KB Flash, 32KB SRAM, Antitamper, 80LQFP",null,null,null,0]
["MK11DX256VMC5","NXPMK11DX256VMC5","NXP","ARM CM4",50,320,4,32,16,null,1,null,64,"No",2,2,1,"No",13,null,-40,105,1.71,3.6,121,"LFBGA121",null,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 320KB Flash, 32KB SRAM, Antitamper, 121MAPBGA",null,null,null,0]
["MKL33Z64VLK4","NXPMKL33Z64VLK4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,70,"Yes",2,2,0,"No",null,null,-40,105,1.71,3.6,80,"LQFP80",1.36,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ Core, 64KB Flash, 48MHz, SLCD, LQFP 80",null,null,null,0]
["MKL34Z64VLH4","NXPMKL34Z64VLH4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,54,"Yes",2,2,0,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.41,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 64KB Flash, 48MHz, Segment LCD, QFP 64",null,null,null,0]
["MKL34Z64VLL4","NXPMKL34Z64VLL4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,84,"Yes",2,2,0,"No",null,null,-40,105,1.71,3.6,100,"LQFP100",1.56,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 64KB Flash, 48MHz, Segment LCD, QFP 100",null,null,null,0]
["MKL36Z128VLH4","NXPMKL36Z128VLH4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,54,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.81,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, Segment LCD, QFP 64",null,null,null,0]
["MKL36Z128VLL4","NXPMKL36Z128VLL4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,84,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,100,"LQFP100",1.96,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, Segment LCD, QFP 100",null,null,null,0]
["MKL36Z128VLL4R","NXPMKL36Z128VLL4R","NXP","ARM CM0+",48,128,null,16,16,null,1,null,84,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,100,"LQFP100",1.96,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, Segment LCD, QFP 100",null,null,null,0]
["MKL36Z128VMC4","NXPMKL36Z128VMC4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,84,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,121,"LFBGA121",2.4700000000000002,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, Segment LCD, MAPBGA 121",null,null,null,0]
["MKL36Z256VLH4","NXPMKL36Z256VLH4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,54,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",2.11,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, Segment LCD, QFP 64",null,null,null,0]
["MKL36Z256VLL4","NXPMKL36Z256VLL4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,84,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,100,"LQFP100",2.2599999999999998,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, Segment LCD, QFP 100",null,null,null,0]
["MKL36Z256VLL4R","NXPMKL36Z256VLL4R","NXP","ARM CM0+",48,256,null,32,16,null,1,null,84,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,100,"LQFP100",2.2599999999999998,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, Segment LCD, QFP 100",null,null,null,0]
["MKL36Z256VMC4","NXPMKL36Z256VMC4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,84,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,121,"LFBGA121",2.36,null,3,null,null,null,null,null,null,null,"Kinetis KL36: 48MHz CortexM0+ UltraLow Power MCU, 256KB Flash, 32KB SRAM, Segment LCD, 121MAPBGA",null,null,null,0]
["MKL36Z256VMP4","NXPMKL36Z256VMP4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,54,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,64,"LFBGA64",2.16,null,3,null,null,null,null,null,null,null,"Kinetis KL36: 48MHz CortexM0+ UltraLow Power MCU, 256KB Flash, 32KB SRAM, Segment LCD, 64MAPBGA",null,null,null,0]
["MKL36Z64VLH4","NXPMKL36Z64VLH4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,54,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.5,null,3,null,null,null,null,null,null,null,"Kinetis KL36: 48MHz CortexM0+ UltraLow Power MCU, 64KB Flash, 8KB SRAM, Segment LCD, 64LQFP",null,null,null,0]
["MKL36Z64VLL4","NXPMKL36Z64VLL4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,84,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,100,"LQFP100",1.65,null,3,null,null,null,null,null,null,null,"Kinetis KL36: 48MHz CortexM0+ UltraLow Power MCU, 64KB Flash, 8KB SRAM, Segment LCD, 100LQFP",null,null,null,0]
["MKL81Z128CBH7R","NXPMKL81Z128CBH7R","NXP","ARM CM0",72,128,null,null,0,null,0,null,40,"No",2,2,null,"No",null,null,-40,105,1.71,3.6,64,"WLCSP64",2.99,null,3,null,null,null,null,null,null,null,"Kinetis KL81: 72MHz CortexM0+ Secure LowPower MCU, 128KB Flash, 96KB RAM, USB, Antitamper, 64WLCSP",null,null,null,0]
["MKM14Z128ACHH5","NXPMKM14Z128ACHH5","NXP","ARM CM0+",50,128,null,16,24,null,2,null,20,"No",1,2,null,"No",4,null,-40,85,1.71,3.6,44,"HVQFN44R",1.5,null,2,null,null,null,null,null,null,null,"Kinetis KM14: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, 44LGA",null,null,null,0]
["MKM14Z128ACHH5R","NXPMKM14Z128ACHH5R","NXP","ARM CM0+",50,128,null,16,24,null,2,null,20,"No",1,2,null,"No",4,null,-40,85,1.71,3.6,44,"HVQFN44R",1.5,null,2,null,null,null,null,null,null,null,"Kinetis KM14: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, 44LGA",null,null,null,0]
["MKM14Z128CHH5","NXPMKM14Z128CHH5","NXP","ARM CM0+",50,128,null,16,0,null,0,null,20,"No",null,null,null,"No",null,null,-40,85,1.71,3.6,44,"HVQFN44R",1.5,null,null,null,null,null,null,null,null,null,"Kinetis M 32bit MCU, ARM CM0+ core, 128KB Flash, 50MHz, MAPBGA 44",null,null,null,0]
["MKM14Z128CHH5R","NXPMKM14Z128CHH5R","NXP","ARM CM0+",50,128,null,16,0,null,0,null,20,"No",null,null,null,"No",null,null,-40,85,1.71,3.6,44,"HVQFN44R",1.5,null,null,null,null,null,null,null,null,null,"Kinetis M 32bit MCU, ARM CM0+ core, 128KB Flash, 50MHz, MAPBGA 44",null,null,null,0]
["MKM14Z64ACHH5","NXPMKM14Z64ACHH5","NXP","ARM CM0+",50,64,null,16,24,null,2,null,20,"No",1,2,null,"No",4,null,-40,85,1.71,3.6,44,"HVQFN44R",1.28,null,2,null,null,null,null,null,null,null,"Kinetis KM14: 50MHz CortexM0+ Metrology MCU, 64KB Flash, 16KB SRAM, 44LGA",null,null,null,0]
["MKM14Z64CHH5","NXPMKM14Z64CHH5","NXP","ARM CM0+",50,64,null,16,0,null,0,null,20,"No",null,null,null,"No",null,null,-40,85,1.71,3.6,44,"HVQFN44R",1.28,null,null,null,null,null,null,null,null,null,"Kinetis KM14: 50MHz CortexM0+ Metrology MCU, 64KB Flash, 16KB SRAM, 44LGA",null,null,null,0]
["MKM33Z128CLH5","NXPMKM33Z128CLH5","NXP","ARM CM0+",50,128,null,16,0,null,0,null,38,"Yes",null,null,null,"No",null,null,-40,85,1.71,3.6,64,"LQFP64",1.8,null,null,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, Segment LCD, 64LQFP",null,null,null,0]
["MKM33Z128CLH5R","NXPMKM33Z128CLH5R","NXP","ARM CM0+",50,128,null,16,0,null,0,null,38,"Yes",null,null,null,"No",null,null,-40,85,1.71,3.6,64,"LQFP64",1.8,null,null,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, Segment LCD, 64LQFP",null,null,null,0]
["MKM33Z128CLL5","NXPMKM33Z128CLL5","NXP","ARM CM0+",50,128,null,16,0,null,0,null,68,"Yes",null,null,null,"No",null,null,-40,85,1.71,3.6,100,"LQFP100",1.88,null,null,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, Segment LCD, 100LQFP",null,null,null,0]
["MKM33Z64CLH5","NXPMKM33Z64CLH5","NXP","ARM CM0+",50,64,null,16,0,null,0,null,38,"Yes",null,null,null,"No",null,null,-40,85,1.71,3.6,64,"LQFP64",1.57,null,null,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 64KB Flash, 16KB SRAM, Segment LCD, 64LQFP",null,null,null,0]
["MKM33Z64CLL5","NXPMKM33Z64CLL5","NXP","ARM CM0+",50,64,null,16,0,null,0,null,68,"Yes",null,null,null,"No",null,null,-40,85,1.71,3.6,100,"LQFP100",1.67,null,null,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 64KB Flash, 16KB SRAM, Segment LCD, 100LQFP",null,null,null,0]
["MKM33Z64CLL5R","NXPMKM33Z64CLL5R","NXP","ARM CM0+",50,64,null,16,0,null,0,null,68,"Yes",null,null,null,"No",null,null,-40,85,1.71,3.6,100,"LQFP100",1.67,null,null,null,null,null,null,null,null,null,"Kinetis KM33: 50MHz CortexM0+ Metrology MCU, 64KB Flash, 16KB SRAM, Segment LCD, 100LQFP",null,null,null,0]
["MKM34Z128CLL5","NXPMKM34Z128CLL5","NXP","ARM CM0+",50,128,null,16,0,null,0,null,68,"Yes",null,null,null,"No",null,null,-40,85,1.71,3.6,100,"LQFP100",2.02,null,null,null,null,null,null,null,null,null,"Kinetis KM34: 50MHz CortexM0+ Metrology MCU, 128KB Flash, 16KB SRAM, Segment LCD, 100LQFP",null,null,null,0]
["MKM34Z256VLL7","NXPMKM34Z256VLL7","NXP","ARM CM0+",75,256,null,32,24,null,3,null,72,"Yes",2,2,null,"No",4,null,-40,105,1.71,3.6,100,"LQFP100",2.31,null,5,null,null,null,null,null,null,null,"Kinetis KM34: 75MHz CortexM0+ Metrology MCU, 256KB Flash, 32KB SRAM, Segment LCD, 100LQFP",null,null,null,0]
["MKM34Z256VLL7R","NXPMKM34Z256VLL7R","NXP","ARM CM0+",75,256,null,32,24,null,3,null,72,"Yes",2,2,null,"No",4,null,-40,105,1.71,3.6,100,"LQFP100",2.31,null,5,null,null,null,null,null,null,null,"Kinetis KM34: 75MHz CortexM0+ Metrology MCU, 256KB Flash, 32KB SRAM, Segment LCD, 100LQFP",null,null,null,0]
["MKM34Z256VLQ7","NXPMKM34Z256VLQ7","NXP","ARM CM0+",75,256,null,32,24,null,3,null,99,"Yes",2,2,null,"No",4,null,-40,105,1.71,3.6,144,"LQFP144",2.58,null,5,null,null,null,null,null,null,null,"Kinetis KM34: 75MHz CortexM0+ Metrology MCU, 256KB Flash, 32KB SRAM, Segment LCD, 144LQFP",null,null,null,0]
["MKV44F128VLH16","NXPMKV44F128VLH16","NXP","ARM CM4F",168,128,null,24,12,null,5,null,48,"No",1,1,null,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.55,null,2,null,null,null,null,null,null,null,"Kinetis KV44: 168MHz CortexM4F Realtime Ctrl MCU, 128KB Flash, 24KB RAM, DAC, PWM NanoEdge, 64LQFP",null,null,null,0]
["MKV44F128VLL16","NXPMKV44F128VLL16","NXP","ARM CM4F",168,128,null,24,12,null,5,null,74,"No",1,1,null,"No",null,null,-40,105,1.71,3.6,100,"LQFP100",1.63,null,2,null,null,null,null,null,null,null,"Kinetis KV44: 168MHz CortexM4F Realtime Ctrl MCU, 128KB Flash, 24K RAM, DAC, PWM NanoEdge, 100LQFP",null,null,null,0]
["MKV44F256VLH16","NXPMKV44F256VLH16","NXP","ARM CM4F",168,256,null,32,12,null,5,null,48,"No",1,1,null,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.7,null,2,null,null,null,null,null,null,null,"Kinetis KV44: 168MHz CortexM4F Realtime Ctrl MCU, 256KB Flash, 32KB RAM, DAC, PWM NanoEdge, 64LQFP",null,null,null,0]
["MKV44F256VLL16","NXPMKV44F256VLL16","NXP","ARM CM4F",168,256,null,32,12,null,5,null,74,"No",1,1,null,"No",null,null,-40,105,1.71,3.6,100,"LQFP100",1.78,null,2,null,null,null,null,null,null,null,"Kinetis KV44: 168MHz CortexM4F Realtime Ctrl MCU, 256KB Flash, 32K RAM, DAC, PWM NanoEdge, 100LQFP",null,null,null,0]
["MKV44F64VLH16","NXPMKV44F64VLH16","NXP","ARM CM4F",168,64,null,16,12,null,5,null,48,"No",1,1,null,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.39,null,2,null,null,null,null,null,null,null,"Kinetis KV44: 168MHz CortexM4F Realtime Ctrl MCU, 64KB Flash, 16KB RAM, DAC, PWM NanoEdge, 64LQFP",null,null,null,0]
["MKV46F128VLH16","NXPMKV46F128VLH16","NXP","ARM CM4F",168,128,null,24,12,null,5,null,48,"No",1,1,null,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.58,null,2,null,null,null,null,null,null,null,"Kinetis KV46: 168MHz M4F Realtime Ctrl MCU, 128KB Flash, 24KB RAM, 3xTimer, DAC, PWM nEdge, 64LQFP",null,null,null,0]
["MKV46F128VLL16","NXPMKV46F128VLL16","NXP","ARM CM4F",168,128,null,24,12,null,5,null,74,"No",1,1,null,"No",null,null,-40,105,1.71,3.6,100,"LQFP100",1.65,null,2,null,null,null,null,null,null,null,"Kinetis KV46: 168MHz M4F Realtime Ctrl MCU, 128KB Flash, 24KB RAM, 3xTimer, DAC, PWM nEdge, 100LQFP",null,null,null,0]
["MKV46F256VLH16","NXPMKV46F256VLH16","NXP","ARM CM4F",168,256,null,32,12,null,5,null,48,"No",1,1,null,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.72,null,2,null,null,null,null,null,null,null,"Kinetis KV46: 168MHz M4F Realtime Ctrl MCU, 256KB Flash, 32KB RAM, 3xTimer, DAC, PWM nEdge, 64LQFP",null,null,null,0]
["MKV46F256VLH16R","NXPMKV46F256VLH16R","NXP","ARM CM4F",168,256,null,32,12,null,5,null,48,"No",1,1,null,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.72,null,2,null,null,null,null,null,null,null,"Kinetis KV46: 168MHz M4F Realtime Ctrl MCU, 256KB Flash, 32KB RAM, 3xTimer, DAC, PWM nEdge, 64LQFP",null,null,null,0]
["MKV46F256VLL16","NXPMKV46F256VLL16","NXP","ARM CM4F",168,256,null,32,12,null,5,null,74,"No",1,1,null,"No",null,null,-40,105,1.71,3.6,100,"LQFP100",2.73,null,2,null,null,null,null,null,null,null,"Kinetis KV46: 168MHz M4F Realtime Ctrl MCU, 256KB Flash, 32KB RAM, 3xTimer, DAC, PWM nEdge, 100LQFP",null,null,null,0]
["MKV46F256VLL16Q","NXPMKV46F256VLL16Q","NXP","ARM CM4F",null,256,null,32,0,null,0,null,null,"No",null,null,null,"No",null,null,0,null,null,null,100,"LQFP100",null,null,null,null,null,null,null,null,null,null,"Kinetis KV46: 168MHz M4F Realtime Ctrl MCU, 256KB Flash, 32KB RAM, 3xTimer, DAC, PWM nEdge, 100LQFP",null,null,null,0]
["MKV58F1M0VLQ24","NXPMKV58F1M0VLQ24","NXP","ARM CM7",240,1024,null,256,16,null,5,null,111,"No",2,3,null,"No",null,null,-40,105,1.71,3.6,144,"LQFP144",null,null,6,null,null,null,null,null,null,null,"Kinetis KV58: 220MHz CortexM7F RealTime Control MCU, 1MB Flash, 256KB SRAM, Ethernet, 144LQFP",null,null,null,0]
["LPC802M001JDH16FP","NXPLPC802M001JDH16FP","NXP","ARM CM0+",15,16,null,2,12,null,0,null,13,"No",1,1,0,{"$f":"IF(OR(ISBLANK(AO139), AO139=0), \"No\", \"Yes\")","v":"No"},1,null,-40,105,1.71,3.6,16,"TSSOP16",0.34,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC802M001JDH16J","NXPLPC802M001JDH16J","NXP","ARM CM0+",15,16,null,2,12,null,0,null,13,"No",1,1,0,"No",1,null,-40,105,1.71,3.6,16,"TSSOP16",0.34,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC802M001JDH20FP","NXPLPC802M001JDH20FP","NXP","ARM CM0+",15,16,null,2,12,null,0,null,17,"No",1,1,0,"No",1,null,-40,105,1.71,3.6,20,"TSSOP20",0.36,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC802M001JDH20J","NXPLPC802M001JDH20J","NXP","ARM CM0+",15,16,null,2,12,null,0,null,17,"No",1,1,0,"No",1,null,-40,105,1.71,3.6,20,"TSSOP20",0.36,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC802M001JHI33E","NXPLPC802M001JHI33E","NXP","ARM CM0+",15,16,null,2,12,null,0,null,17,"No",1,1,0,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",0.39,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC802M001JHI33Y","NXPLPC802M001JHI33Y","NXP","ARM CM0+",15,16,null,2,12,null,0,null,17,"No",1,1,0,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",0.39,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC802M011JDH20FP","NXPLPC802M011JDH20FP","NXP","ARM CM0+",15,16,null,2,12,null,0,null,16,"No",1,1,0,"No",1,null,-40,105,1.71,3.6,20,"TSSOP20",0.37,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC804M101JDH20FP","NXPLPC804M101JDH20FP","NXP","ARM CM0+",15,32,null,4,12,null,0,null,17,"No",2,1,0,"No",1,null,-40,105,1.71,3.6,20,"TSSOP20",0.42,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC804M101JDH20J","NXPLPC804M101JDH20J","NXP","ARM CM0+",15,32,null,4,12,null,0,null,17,"No",2,1,0,"No",1,null,-40,105,1.71,3.6,20,"TSSOP20",0.42,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC804M101JDH20Y","NXPLPC804M101JDH20Y","NXP","ARM CM0+",15,32,null,4,12,null,0,null,17,"No",2,1,0,"No",1,null,-40,105,1.71,3.6,20,"TSSOP20",0.42,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC804M101JDH24FP","NXPLPC804M101JDH24FP","NXP","ARM CM0+",15,32,null,4,12,null,0,null,21,"No",2,1,0,"No",1,null,-40,105,1.71,3.6,24,"TSSOP24",0.45,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC804M101JDH24J","NXPLPC804M101JDH24J","NXP","ARM CM0+",15,32,null,4,12,null,0,null,21,"No",2,1,0,"No",1,null,-40,105,1.71,3.6,24,"TSSOP24",0.45,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC804M101JHI33E","NXPLPC804M101JHI33E","NXP","ARM CM0+",15,32,null,4,12,null,0,null,30,"No",2,1,0,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",0.47,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC804M101JHI33Y","NXPLPC804M101JHI33Y","NXP","ARM CM0+",15,32,null,4,12,null,0,null,30,"No",2,1,0,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",0.47,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC804M111JDH24FP","NXPLPC804M111JDH24FP","NXP","ARM CM0+",15,32,null,4,12,null,0,null,20,"No",2,1,0,"No",1,null,-40,105,1.71,3.6,24,"TSSOP24",0.46,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC804M111JDH24J","NXPLPC804M111JDH24J","NXP","ARM CM0+",15,32,null,4,12,null,0,null,20,"No",2,1,0,"No",1,null,-40,105,1.71,3.6,24,"TSSOP24",0.46,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC811M001JDH16FP","NXPLPC811M001JDH16FP","NXP","ARM CM0+",30,8,null,2,12,null,0,null,14,"No",1,1,null,"No",1,null,-40,105,1.8,3.6,16,"TSSOP16",0.38,null,2,null,null,null,null,null,null,null,"Low Cost 32bit Microcontroller based on ARM CM0+",null,null,null,0,"No"]
["LPC811M001JDH16J","NXPLPC811M001JDH16J","NXP","ARM CM0+",30,8,null,2,12,null,0,null,14,"No",1,1,null,"No",1,null,-40,105,1.8,3.6,16,"TSSOP16",0.38,null,2,null,null,null,null,null,null,null,"Low Cost 32bit Microcontroller based on ARM CM0+",null,null,null,0,"No"]
["LPC812M101JD20FP","NXPLPC812M101JD20FP","NXP","ARM CM0+",30,16,null,4,12,null,0,null,18,"No",1,1,null,"No",1,null,-40,105,1.8,3.6,20,"SO20",0.45,null,2,null,null,null,null,null,null,null,"32bit ARM CM0+ microcontroller; 16 kB flash and 4 kB SRAM",null,null,null,0,"No"]
["LPC812M101JD20J","NXPLPC812M101JD20J","NXP","ARM CM0+",30,16,null,4,12,null,0,null,18,"No",1,1,null,"No",1,null,-40,105,1.8,3.6,20,"SO20",0.45,null,2,null,null,null,null,null,null,null,"32bit ARM CM0+ microcontroller; 16 kB flash and 4 kB SRAM",null,null,null,0,"No"]
["LPC812M101JDH16FP","NXPLPC812M101JDH16FP","NXP","ARM CM0+",30,16,null,4,12,null,0,null,14,"No",1,2,null,"No",1,null,-40,105,1.8,3.6,16,"TSSOP16",0.42,null,3,null,null,null,null,null,null,null,"Low Cost 32bit Microcontroller based on ARM CM0+",null,null,null,0,"No"]
["LPC812M101JDH16J","NXPLPC812M101JDH16J","NXP","ARM CM0+",30,16,null,4,12,null,0,null,14,"No",1,2,null,"No",1,null,-40,105,1.8,3.6,16,"TSSOP16",0.42,null,3,null,null,null,null,null,null,null,"Low Cost 32bit Microcontroller based on ARM CM0+",null,null,null,0,"No"]
["LPC812M101JDH20FP","NXPLPC812M101JDH20FP","NXP","ARM CM0+",30,16,null,4,12,null,0,null,18,"No",1,2,null,"No",1,null,-40,105,1.8,3.6,20,"TSSOP20",0.45,null,3,null,null,null,null,null,null,null,"Low Cost 32bit Microcontroller based on ARM CM0+",null,null,null,0,"No"]
["LPC812M101JDH20J","NXPLPC812M101JDH20J","NXP","ARM CM0+",30,16,null,4,12,null,0,null,18,"No",1,2,null,"No",1,null,-40,105,1.8,3.6,20,"TSSOP20",0.45,null,3,null,null,null,null,null,null,null,"Low Cost 32bit Microcontroller based on ARM CM0+",null,null,null,0,"No"]
["LPC812M101JTB16X","NXPLPC812M101JTB16X","NXP","ARM CM0+",30,16,null,4,12,null,0,null,14,"No",1,2,null,"No",1,null,-40,105,1.8,3.6,16,"XSON16",0.55000000000000004,null,3,null,null,null,null,null,null,null,"Low Cost 32bit Microcontroller based on ARM CM0+",null,null,null,0,"No"]
["R5F104EDDNA","RenesasR5F104EDDNA","Renesas","RL78",32,48,4,5.5,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104EDGNA","RenesasR5F104EDGNA","Renesas","RL78",32,48,4,5.5,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104EEANA","RenesasR5F104EEANA","Renesas","RL78",32,64,4,5.5,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104EEDNA","RenesasR5F104EEDNA","Renesas","RL78",32,64,4,5.5,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104EEGNA","RenesasR5F104EEGNA","Renesas","RL78",32,64,4,5.5,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104EFANA","RenesasR5F104EFANA","Renesas","RL78",32,96,8,12,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104EFDNA","RenesasR5F104EFDNA","Renesas","RL78",32,96,8,12,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104EFGNA","RenesasR5F104EFGNA","Renesas","RL78",32,96,8,12,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104EGANA","RenesasR5F104EGANA","Renesas","RL78",32,128,8,16,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104EGDNA","RenesasR5F104EGDNA","Renesas","RL78",32,128,8,16,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104EGGNA","RenesasR5F104EGGNA","Renesas","RL78",32,128,8,16,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104EHANA","RenesasR5F104EHANA","Renesas","RL78",32,192,8,20,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104EHDNA","RenesasR5F104EHDNA","Renesas","RL78",32,192,8,20,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104EHGNA","RenesasR5F104EHGNA","Renesas","RL78",32,192,8,20,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104FAAFP","RenesasR5F104FAAFP","Renesas","RL78",32,16,4,2.5,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104FADFP","RenesasR5F104FADFP","Renesas","RL78",32,16,4,2.5,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104FAGFP","RenesasR5F104FAGFP","Renesas","RL78",32,16,4,2.5,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104FCAFP","RenesasR5F104FCAFP","Renesas","RL78",32,32,4,4,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104FCDFP","RenesasR5F104FCDFP","Renesas","RL78",32,32,4,4,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104FCGFP","RenesasR5F104FCGFP","Renesas","RL78",32,32,4,4,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104FDAFP","RenesasR5F104FDAFP","Renesas","RL78",32,48,4,5.5,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104FDDFP","RenesasR5F104FDDFP","Renesas","RL78",32,48,4,5.5,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104FDGFP","RenesasR5F104FDGFP","Renesas","RL78",32,48,4,5.5,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104FEAFP","RenesasR5F104FEAFP","Renesas","RL78",32,64,4,5.5,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104FEDFP","RenesasR5F104FEDFP","Renesas","RL78",32,64,4,5.5,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104FEGFP","RenesasR5F104FEGFP","Renesas","RL78",32,64,4,5.5,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104FFAFP","RenesasR5F104FFAFP","Renesas","RL78",32,96,8,12,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104FFDFP","RenesasR5F104FFDFP","Renesas","RL78",32,96,8,12,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104FFGFP","RenesasR5F104FFGFP","Renesas","RL78",32,96,8,12,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104FGAFP","RenesasR5F104FGAFP","Renesas","RL78",32,128,8,16,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104FGDFP","RenesasR5F104FGDFP","Renesas","RL78",32,128,8,16,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104FGGFP","RenesasR5F104FGGFP","Renesas","RL78",32,128,8,16,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104FHAFP","RenesasR5F104FHAFP","Renesas","RL78",32,192,8,20,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104FHDFP","RenesasR5F104FHDFP","Renesas","RL78",32,192,8,20,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104FHGFP","RenesasR5F104FHGFP","Renesas","RL78",32,192,8,20,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104FJAFP","RenesasR5F104FJAFP","Renesas","RL78",32,256,8,24,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104FJDFP","RenesasR5F104FJDFP","Renesas","RL78",32,256,8,24,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104FJGFP","RenesasR5F104FJGFP","Renesas","RL78",32,256,8,24,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GAAFB","RenesasR5F104GAAFB","Renesas","RL78",32,16,4,2.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GAANA","RenesasR5F104GAANA","Renesas","RL78",32,16,4,2.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GADFB","RenesasR5F104GADFB","Renesas","RL78",32,16,4,2.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104GADNA","RenesasR5F104GADNA","Renesas","RL78",32,16,4,2.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104GAGFB","RenesasR5F104GAGFB","Renesas","RL78",32,16,4,2.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GAGNA","RenesasR5F104GAGNA","Renesas","RL78",32,16,4,2.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GCAFB","RenesasR5F104GCAFB","Renesas","RL78",32,32,4,4,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GCANA","RenesasR5F104GCANA","Renesas","RL78",32,32,4,4,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GCDFB","RenesasR5F104GCDFB","Renesas","RL78",32,32,4,4,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104GCDNA","RenesasR5F104GCDNA","Renesas","RL78",32,32,4,4,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104GCGFB","RenesasR5F104GCGFB","Renesas","RL78",32,32,4,4,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GCGNA","RenesasR5F104GCGNA","Renesas","RL78",32,32,4,4,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GDAFB","RenesasR5F104GDAFB","Renesas","RL78",32,48,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GDANA","RenesasR5F104GDANA","Renesas","RL78",32,48,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GDDFB","RenesasR5F104GDDFB","Renesas","RL78",32,48,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104GDDNA","RenesasR5F104GDDNA","Renesas","RL78",32,48,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104GDGFB","RenesasR5F104GDGFB","Renesas","RL78",32,48,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GDGNA","RenesasR5F104GDGNA","Renesas","RL78",32,48,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GEAFB","RenesasR5F104GEAFB","Renesas","RL78",32,64,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GEANA","RenesasR5F104GEANA","Renesas","RL78",32,64,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GEDFB","RenesasR5F104GEDFB","Renesas","RL78",32,64,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104GEDNA","RenesasR5F104GEDNA","Renesas","RL78",32,64,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104GEGFB","RenesasR5F104GEGFB","Renesas","RL78",32,64,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GEGNA","RenesasR5F104GEGNA","Renesas","RL78",32,64,4,5.5,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GFAFB","RenesasR5F104GFAFB","Renesas","RL78",32,96,8,12,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GFANA","RenesasR5F104GFANA","Renesas","RL78",32,96,8,12,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GFDFB","RenesasR5F104GFDFB","Renesas","RL78",32,96,8,12,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104GFDNA","RenesasR5F104GFDNA","Renesas","RL78",32,96,8,12,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104GFGFB","RenesasR5F104GFGFB","Renesas","RL78",32,96,8,12,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GFGNA","RenesasR5F104GFGNA","Renesas","RL78",32,96,8,12,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GGAFB","RenesasR5F104GGAFB","Renesas","RL78",32,128,8,16,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GGANA","RenesasR5F104GGANA","Renesas","RL78",32,128,8,16,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GGDFB","RenesasR5F104GGDFB","Renesas","RL78",32,128,8,16,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104GGDNA","RenesasR5F104GGDNA","Renesas","RL78",32,128,8,16,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104GGGFB","RenesasR5F104GGGFB","Renesas","RL78",32,128,8,16,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GGGNA","RenesasR5F104GGGNA","Renesas","RL78",32,128,8,16,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GHAFB","RenesasR5F104GHAFB","Renesas","RL78",32,192,8,20,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GHANA","RenesasR5F104GHANA","Renesas","RL78",32,192,8,20,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GHDFB","RenesasR5F104GHDFB","Renesas","RL78",32,192,8,20,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104GHDNA","RenesasR5F104GHDNA","Renesas","RL78",32,192,8,20,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104GHGFB","RenesasR5F104GHGFB","Renesas","RL78",32,192,8,20,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GHGNA","RenesasR5F104GHGNA","Renesas","RL78",32,192,8,20,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GJAFB","RenesasR5F104GJAFB","Renesas","RL78",32,256,8,24,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GJANA","RenesasR5F104GJANA","Renesas","RL78",32,256,8,24,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GJDFB","RenesasR5F104GJDFB","Renesas","RL78",32,256,8,24,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104GJDNA","RenesasR5F104GJDNA","Renesas","RL78",32,256,8,24,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104GJGFB","RenesasR5F104GJGFB","Renesas","RL78",32,256,8,24,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GJGNA","RenesasR5F104GJGNA","Renesas","RL78",32,256,8,24,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GKAFB","RenesasR5F104GKAFB","Renesas","RL78",32,384,8,32,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GKANA","RenesasR5F104GKANA","Renesas","RL78",32,384,8,32,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GKGFB","RenesasR5F104GKGFB","Renesas","RL78",32,384,8,32,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GKGNA","RenesasR5F104GKGNA","Renesas","RL78",32,384,8,32,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GLAFB","RenesasR5F104GLAFB","Renesas","RL78",32,512,8,48,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104GLANA","RenesasR5F104GLANA","Renesas","RL78",32,512,8,48,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GLGFB","RenesasR5F104GLGFB","Renesas","RL78",32,512,8,48,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104GLGNA","RenesasR5F104GLGNA","Renesas","RL78",32,512,8,48,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104JCAFA","RenesasR5F104JCAFA","Renesas","RL78",32,32,4,4,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JCDFA","RenesasR5F104JCDFA","Renesas","RL78",32,32,4,4,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104JCGFA","RenesasR5F104JCGFA","Renesas","RL78",32,32,4,4,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JDAFA","RenesasR5F104JDAFA","Renesas","RL78",32,48,4,5.5,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JDDFA","RenesasR5F104JDDFA","Renesas","RL78",32,48,4,5.5,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104JDGFA","RenesasR5F104JDGFA","Renesas","RL78",32,48,4,5.5,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JEAFA","RenesasR5F104JEAFA","Renesas","RL78",32,64,4,5.5,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JEDFA","RenesasR5F104JEDFA","Renesas","RL78",32,64,4,5.5,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104JEGFA","RenesasR5F104JEGFA","Renesas","RL78",32,64,4,5.5,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JFAFA","RenesasR5F104JFAFA","Renesas","RL78",32,96,8,12,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JFDFA","RenesasR5F104JFDFA","Renesas","RL78",32,96,8,12,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104JFGFA","RenesasR5F104JFGFA","Renesas","RL78",32,96,8,12,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JGAFA","RenesasR5F104JGAFA","Renesas","RL78",32,128,8,16,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JGDFA","RenesasR5F104JGDFA","Renesas","RL78",32,128,8,16,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104JGGFA","RenesasR5F104JGGFA","Renesas","RL78",32,128,8,16,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JHAFA","RenesasR5F104JHAFA","Renesas","RL78",32,192,8,20,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JHDFA","RenesasR5F104JHDFA","Renesas","RL78",32,192,8,20,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104JHGFA","RenesasR5F104JHGFA","Renesas","RL78",32,192,8,20,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JJAFA","RenesasR5F104JJAFA","Renesas","RL78",32,256,8,24,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104JJDFA","RenesasR5F104JJDFA","Renesas","RL78",32,256,8,24,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104JJGFA","RenesasR5F104JJGFA","Renesas","RL78",32,256,8,24,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LCAFA","RenesasR5F104LCAFA","Renesas","RL78",32,32,4,4,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LCAFB","RenesasR5F104LCAFB","Renesas","RL78",32,32,4,4,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LCAFP","RenesasR5F104LCAFP","Renesas","RL78",32,32,4,4,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LCALA","RenesasR5F104LCALA","Renesas","RL78",32,32,4,4,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64WFLGA",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104LCDFA","RenesasR5F104LCDFA","Renesas","RL78",32,32,4,4,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104LCDFB","RenesasR5F104LCDFB","Renesas","RL78",32,32,4,4,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104LCDFP","RenesasR5F104LCDFP","Renesas","RL78",32,32,4,4,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104LCGFA","RenesasR5F104LCGFA","Renesas","RL78",32,32,4,4,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LCGFB","RenesasR5F104LCGFB","Renesas","RL78",32,32,4,4,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LCGFP","RenesasR5F104LCGFP","Renesas","RL78",32,32,4,4,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LCGLA","RenesasR5F104LCGLA","Renesas","RL78",32,32,4,4,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64WFLGA",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104LDAFA","RenesasR5F104LDAFA","Renesas","RL78",32,48,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LDAFB","RenesasR5F104LDAFB","Renesas","RL78",32,48,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LDAFP","RenesasR5F104LDAFP","Renesas","RL78",32,48,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LDALA","RenesasR5F104LDALA","Renesas","RL78",32,48,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64WFLGA",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104LDDFA","RenesasR5F104LDDFA","Renesas","RL78",32,48,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104LDDFB","RenesasR5F104LDDFB","Renesas","RL78",32,48,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104LDDFP","RenesasR5F104LDDFP","Renesas","RL78",32,48,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104LDGFA","RenesasR5F104LDGFA","Renesas","RL78",32,48,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LDGFB","RenesasR5F104LDGFB","Renesas","RL78",32,48,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LDGFP","RenesasR5F104LDGFP","Renesas","RL78",32,48,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LDGLA","RenesasR5F104LDGLA","Renesas","RL78",32,48,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64WFLGA",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104LEAFA","RenesasR5F104LEAFA","Renesas","RL78",32,64,4,5.5,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["LPC832M101FDH20FP","NXPLPC832M101FDH20FP","NXP","ARM CM0+",30,16,null,4,12,null,0,null,16,"No",1,2,null,{"$f":"IF(OR(ISBLANK(AO302), AO302=0), \"No\", \"Yes\")","v":"No"},2,null,-40,85,1.8,3.6,20,"TSSOP20",0.5,null,1,null,null,null,null,null,null,null,"32bit ARM CM0+ microcontroller; up to 32 KB flash and 4 KB SRAM; 12bit ADC",null,null,null,0,"No"]
["LPC834M101FHI33Y","NXPLPC834M101FHI33Y","NXP","ARM CM0+",30,32,null,4,12,null,0,null,29,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,32,"HVQFN32",0.56000000000000005,null,1,null,null,null,null,null,null,null,"32bit ARM CM0+ microcontroller; up to 32 KB flash and 4 KB SRAM; 12bit ADC",null,null,null,0,"No"]
["LPC844M201JBD48E","NXPLPC844M201JBD48E","NXP","ARM CM0+",30,64,null,8,12,null,0,null,42,"Yes",2,2,0,"No",2,null,-40,105,1.8,3.6,48,"LQFP48",0.75,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC844M201JBD64E","NXPLPC844M201JBD64E","NXP","ARM CM0+",30,64,null,8,12,null,0,null,54,"Yes",2,2,0,"No",2,null,-40,105,1.8,3.6,64,"LQFP64",0.81,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC844M201JHI33E","NXPLPC844M201JHI33E","NXP","ARM CM0+",30,64,null,8,12,null,0,null,29,"Yes",2,2,0,"No",2,null,-40,105,1.8,3.6,32,"HVQFN32",0.68,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC844M201JHI33Y","NXPLPC844M201JHI33Y","NXP","ARM CM0+",30,64,null,8,12,null,0,null,29,"Yes",2,2,0,"No",2,null,-40,105,1.8,3.6,32,"HVQFN32",0.68,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC844M201JHI48E","NXPLPC844M201JHI48E","NXP","ARM CM0+",30,64,null,8,12,null,0,null,42,"Yes",2,2,0,"No",2,null,-40,105,1.8,3.6,48,"HVQFN48",0.76,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC845M301JBD48E","NXPLPC845M301JBD48E","NXP","ARM CM0+",30,64,null,16,12,null,0,null,42,"Yes",4,2,0,"No",2,null,-40,105,1.8,3.6,48,"LQFP48",0.8,null,5,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC845M301JBD64E","NXPLPC845M301JBD64E","NXP","ARM CM0+",30,64,null,16,12,null,0,null,54,"Yes",4,2,0,"No",2,null,-40,105,1.8,3.6,64,"LQFP64",0.86,null,5,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC845M301JHI33E","NXPLPC845M301JHI33E","NXP","ARM CM0+",30,64,null,16,12,null,0,null,29,"Yes",4,2,0,"No",2,null,-40,105,1.8,3.6,32,"HVQFN32",0.73,null,5,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC845M301JHI33Y","NXPLPC845M301JHI33Y","NXP","ARM CM0+",30,64,null,16,12,null,0,null,29,"Yes",4,2,0,"No",2,null,-40,105,1.8,3.6,32,"HVQFN32",0.73,null,5,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC845M301JHI48E","NXPLPC845M301JHI48E","NXP","ARM CM0+",30,64,null,16,12,null,0,null,42,"Yes",4,2,0,"No",2,null,-40,105,1.8,3.6,48,"HVQFN48",0.81,null,5,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC845M301JHI48K","NXPLPC845M301JHI48K","NXP","ARM CM0+",30,64,null,16,12,null,0,null,42,"Yes",4,2,0,"No",2,null,-40,105,1.8,3.6,48,"HVQFN48",0.81,null,5,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC845M301JHI48Y","NXPLPC845M301JHI48Y","NXP","ARM CM0+",30,64,null,16,12,null,0,null,42,"Yes",4,2,0,"No",2,null,-40,105,1.8,3.6,48,"HVQFN48",0.81,null,5,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC8N04FHI24E","NXPLPC8N04FHI24E","NXP","ARM CM0+",8,32,4,8,0,null,0,null,12,"Yes",1,1,0,"No",1,null,-40,85,1.7,3.6,24,"HVQFN24",0.7,null,0,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["LPC8N04FHI24Z","NXPLPC8N04FHI24Z","NXP","ARM CM0+",8,32,4,8,0,null,0,null,12,"Yes",1,1,0,"No",1,null,-40,85,1.7,3.6,24,"HVQFN24",0.7,null,0,null,null,null,null,null,null,null,null,null,null,null,0,"Yes"]
["MK10DN128VFM5","NXPMK10DN128VFM5","NXP","ARM CM4",50,128,null,16,16,null,0,null,24,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.84,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, 32QFN",null,null,null,0,"Yes"]
["MK10DN128VFT5","NXPMK10DN128VFT5","NXP","ARM CM4",50,128,null,16,16,null,0,null,33,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,48,"HVQFN48",1.97,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, 48QFN",null,null,null,0,"Yes"]
["MK10DN128VLF5","NXPMK10DN128VLF5","NXP","ARM CM4",50,128,null,16,16,null,0,null,33,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.94,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, 48LQFP",null,null,null,0,"Yes"]
["MK10DN128VLF5R","NXPMK10DN128VLF5R","NXP","ARM CM4",50,128,null,16,16,null,0,null,33,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.94,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, 48LQFP",null,null,null,0,"Yes"]
["MK10DN128VLH5","NXPMK10DN128VLH5","NXP","ARM CM4",50,128,null,16,16,null,0,null,44,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",2.06,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, 64LQFP",null,null,null,0,"Yes"]
["MK10DN128VLH5R","NXPMK10DN128VLH5R","NXP","ARM CM4",50,128,null,16,16,null,0,null,44,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",2.06,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, 64LQFP",null,null,null,0,"Yes"]
["MK10DN128VMP5","NXPMK10DN128VMP5","NXP","ARM CM4",50,128,null,16,16,null,0,null,44,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,64,"LFBGA64",2.38,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, 64MAPBGA",null,null,null,0,"Yes"]
["MK10DN32VFM5","NXPMK10DN32VFM5","NXP","ARM CM4",50,32,null,8,16,null,0,null,24,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.35,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 32KB Flash, 8KB SRAM, 32QFN",null,null,null,0,"Yes"]
["MK10DN32VFT5","NXPMK10DN32VFT5","NXP","ARM CM4",50,32,null,8,16,null,0,null,33,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,48,"HVQFN48",1.48,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 32KB Flash, 8KB SRAM, 48QFN",null,null,null,0,"Yes"]
["MK10DN32VLF5","NXPMK10DN32VLF5","NXP","ARM CM4",50,32,null,8,16,null,0,null,33,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.45,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 32KB Flash, 8KB SRAM, 48LQFP",null,null,null,0,"Yes"]
["MK10DN32VLH5","NXPMK10DN32VLH5","NXP","ARM CM4",50,32,null,8,16,null,0,null,44,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.55,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 32KB Flash, 8KB SRAM, 64LQFP",null,null,null,0,"Yes"]
["MK10DN32VMP5","NXPMK10DN32VMP5","NXP","ARM CM4",50,32,null,8,16,null,0,null,44,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,64,"LFBGA64",1.89,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 32KB Flash, 8KB SRAM, 64MAPBGA",null,null,null,0,"Yes"]
["MK10DN512VLK10","NXPMK10DN512VLK10","NXP","ARM CM4",100,512,null,128,16,null,1,null,56,"No",2,2,1,"No",1,null,-40,105,1.71,3.6,80,"LQFP80",4.4800000000000004,null,4,null,null,null,null,null,null,null,"Kinetis K10: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, 80LQFP",null,null,null,0,"Yes"]
["MK10DN512VLK10R","NXPMK10DN512VLK10R","NXP","ARM CM4",100,512,null,128,16,null,1,null,56,"No",2,2,1,"No",1,null,-40,105,1.71,3.6,80,"LQFP80",4.4800000000000004,null,4,null,null,null,null,null,null,null,"Kinetis K10: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, 80LQFP",null,null,null,0,"Yes"]
["MK10DN512VLL10","NXPMK10DN512VLL10","NXP","ARM CM4",100,512,null,128,16,null,1,null,70,"No",2,3,1,"No",1,null,-40,105,1.71,3.6,100,"LQFP100",4.5199999999999996,null,5,null,null,null,null,null,null,null,"Kinetis K10: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, 100LQFP",null,null,null,0,"Yes"]
["MK10DN512VLQ10","NXPMK10DN512VLQ10","NXP","ARM CM4",100,512,null,128,16,null,2,null,104,"No",2,3,1,"No",1,null,-40,105,1.71,3.6,144,"LQFP144",4.9400000000000004,null,6,null,null,null,null,null,null,null,"Kinetis K10: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, 144LQFP",null,null,null,0,"Yes"]
["MK10DN512VMC10","NXPMK10DN512VMC10","NXP","ARM CM4",100,512,null,128,16,null,2,null,90,"No",2,3,1,"No",1,null,-40,105,1.71,3.6,121,"LFBGA121",4.7300000000000004,null,6,null,null,null,null,null,null,null,"Kinetis K10: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, 121MAPBGA",null,null,null,0,"Yes"]
["MK10DN512VMC10R","NXPMK10DN512VMC10R","NXP","ARM CM4",100,512,null,128,16,null,2,null,90,"No",2,3,1,"No",1,null,-40,105,1.71,3.6,121,"LFBGA121",4.7300000000000004,null,6,null,null,null,null,null,null,null,"Kinetis K10: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, 121MAPBGA",null,null,null,0,"Yes"]
["MK10DN512VMD10","NXPMK10DN512VMD10","NXP","ARM CM4",100,512,null,128,16,null,2,null,104,"No",2,3,1,"No",1,null,-40,105,1.71,3.6,144,"LBGA144",5,null,6,null,null,null,null,null,null,null,"Kinetis K10: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, 144MAPBGA",null,null,null,0,"Yes"]
["MK10DN64VFM5","NXPMK10DN64VFM5","NXP","ARM CM4",50,64,null,16,16,null,0,null,24,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.53,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 64KB Flash, 16KB SRAM, 32QFN",null,null,null,0,"Yes"]
["MK10DN64VFT5","NXPMK10DN64VFT5","NXP","ARM CM4",50,64,null,16,16,null,0,null,33,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,48,"HVQFN48",1.68,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 64KB Flash, 16KB SRAM, 48QFN",null,null,null,0,"Yes"]
["MK10DN64VLF5","NXPMK10DN64VLF5","NXP","ARM CM4",50,64,null,16,16,null,0,null,33,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.63,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 64KB Flash, 16KB SRAM, 48LQFP",null,null,null,0,"Yes"]
["MK10DN64VLH5","NXPMK10DN64VLH5","NXP","ARM CM4",50,64,null,16,16,null,0,null,44,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",1.75,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 64KB Flash, 16KB SRAM, 64LQFP",null,null,null,0,"Yes"]
["MK10DN64VMP5","NXPMK10DN64VMP5","NXP","ARM CM4",50,64,null,16,16,null,0,null,44,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,64,"LFBGA64",2.0699999999999998,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 64KB Flash, 16KB SRAM, 64MAPBGA",null,null,null,0,"Yes"]
["MK10FN1M0VLQ12","NXPMK10FN1M0VLQ12","NXP","ARM CM4F",120,1024,null,128,16,null,2,null,104,"No",2,3,2,"No",1,null,-40,105,1.71,3.6,144,"LQFP144",6.03,null,6,null,null,null,null,null,null,null,"Kinetis K10: 120MHz CortexM4F Performance MCU, 1MB Flash, 128KB SRAM, 144LQFP",null,null,null,0,"Yes"]
["MK10FN1M0VMD12","NXPMK10FN1M0VMD12","NXP","ARM CM4F",120,1024,null,128,16,null,2,null,104,"No",2,3,2,"No",1,null,-40,105,1.71,3.6,144,"LBGA144",6.1,null,6,null,null,null,null,null,null,null,"Kinetis K10: 120MHz CortexM4F Performance MCU, 1MB Flash, 128KB SRAM, 144MAPBGA",null,null,null,0,"Yes"]
["MK11DN512AVLK5","NXPMK11DN512AVLK5","NXP","ARM CM4",50,512,null,64,16,null,0,null,60,"No",2,2,1,"No",1,null,-40,105,1.71,3.6,80,"LQFP80",3.24,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, Antitamper, 80LQFP",null,null,null,0,"No"]
["MK11DN512AVLK5R","NXPMK11DN512AVLK5R","NXP","ARM CM4",50,512,null,64,16,null,0,null,60,"No",2,2,1,"No",1,null,-40,105,1.71,3.6,80,"LQFP80",3.24,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, Antitamper, 80LQFP",null,null,null,0,"No"]
["MK11DN512AVMC5","NXPMK11DN512AVMC5","NXP","ARM CM4",50,512,null,64,16,null,1,null,64,"No",2,2,1,"No",1,null,-40,105,1.71,3.6,121,"LFBGA121",3.44,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, Antitamper, 121MAPBGA",null,null,null,0,"No"]
["MK11DX128AVLK5","NXPMK11DX128AVLK5","NXP","ARM CM4",50,192,4,32,16,null,0,null,60,"No",2,2,1,"No",1,null,-40,105,1.71,3.6,80,"LQFP80",2.4900000000000002,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 192KB Flash, 32KB SRAM, Antitamper, 80LQFP",null,null,null,0,"No"]
["MK11DX256AVLK5","NXPMK11DX256AVLK5","NXP","ARM CM4",50,320,4,32,16,null,0,null,60,"No",2,2,1,"No",1,null,-40,105,1.71,3.6,80,"LQFP80",2.83,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 320KB Flash, 32KB SRAM, Antitamper, 80LQFP",null,null,null,0,"No"]
["MK12DN512VLH5","NXPMK12DN512VLH5","NXP","ARM CM4",50,512,null,64,16,null,1,null,44,"No",2,1,1,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",2.8,null,3,null,null,null,null,null,null,null,"Kinetis K12: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, 64LQFP",null,null,null,0,"No"]
["MK12DN512VLH5R","NXPMK12DN512VLH5R","NXP","ARM CM4",50,512,null,64,16,null,1,null,44,"No",2,1,1,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",2.8,null,3,null,null,null,null,null,null,null,"Kinetis K12: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, 64LQFP",null,null,null,0,"No"]
["MK12DN512VLK5","NXPMK12DN512VLK5","NXP","ARM CM4",50,512,null,64,16,null,1,null,60,"No",2,2,1,"No",1,null,-40,105,1.71,3.6,80,"LQFP80",2.99,null,4,null,null,null,null,null,null,null,"Kinetis K12: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, 80LQFP",null,null,null,0,"No"]
["MK12DN512VLK5R","NXPMK12DN512VLK5R","NXP","ARM CM4",50,512,null,64,16,null,1,null,60,"No",2,2,1,"No",1,null,-40,105,1.71,3.6,80,"LQFP80",2.99,null,4,null,null,null,null,null,null,null,"Kinetis K12: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, 80LQFP",null,null,null,0,"No"]
["MK12DN512VMC5","NXPMK12DN512VMC5","NXP","ARM CM4",50,512,null,64,16,null,1,null,60,"No",2,2,1,"No",1,null,-40,105,1.71,3.6,121,"LFBGA121",3.18,null,4,null,null,null,null,null,null,null,"Kinetis K12: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, 121MAPBGA",null,null,null,0,"No"]
["MK12DX128VLF5","NXPMK12DX128VLF5","NXP","ARM CM4",50,192,4,32,16,null,0,null,33,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",1.95,null,3,null,null,null,null,null,null,null,"Kinetis K12: 50MHz CortexM4 Performance MCU, 192KB Flash, 32KB SRAM, 48LQFP",null,null,null,0,"No"]
["MK12DX256VLF5","NXPMK12DX256VLF5","NXP","ARM CM4",50,320,4,32,16,null,0,null,33,"No",1,1,1,"No",1,null,-40,105,1.71,3.6,48,"LQFP48",2.29,null,3,null,null,null,null,null,null,null,"Kinetis K12: 50MHz CortexM4 Performance MCU, 320KB Flash, 32KB SRAM, 48LQFP",null,null,null,0,"No"]
["MK30DN512VLL10","NXPMK30DN512VLL10","NXP","ARM CM4",100,512,null,128,16,null,1,null,68,"Yes",2,3,1,"No",1,null,-40,105,1.71,3.6,100,"LQFP100",4.93,null,5,null,null,null,null,null,null,null,"Kinetis K30: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, Segment LCD, 100LQFP",null,null,null,0,"Yes"]
["MK30DN512VLQ10","NXPMK30DN512VLQ10","NXP","ARM CM4",100,512,null,128,16,null,2,null,102,"Yes",2,3,1,"No",1,null,-40,105,1.71,3.6,144,"LQFP144",5.33,null,6,null,null,null,null,null,null,null,"Kinetis K30: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, Segment LCD, 144LQFP",null,null,null,0,"Yes"]
["MKE02Z16VFM4","NXPMKE02Z16VFM4","NXP","ARM CM0+",40,16,0.25600000000000001,2,12,null,2,null,28,"No",1,2,null,"No",1,null,-40,105,2.7,5.5,32,"HVQFN32",0.63,null,2,null,null,null,null,null,null,null,"Kinetis KE02: 40MHz CortexM0+ 5V/Robust MCU, 16KB Flash, 2KB SRAM, 32QFN",null,null,null,0,"No"]
["MKE02Z32VFM4","NXPMKE02Z32VFM4","NXP","ARM CM0+",40,32,0.25600000000000001,4,12,null,2,null,28,"No",1,2,null,"No",1,null,-40,105,2.7,5.5,32,"HVQFN32",0.83,null,2,null,null,null,null,null,null,null,"Kinetis KE02: 40MHz CortexM0+ 5V/Robust MCU, 32KB Flash, 4KB SRAM, 32QFN",null,null,null,0,"No"]
["MKE02Z32VFM4R","NXPMKE02Z32VFM4R","NXP","ARM CM0+",40,32,0.25600000000000001,4,12,null,2,null,28,"No",1,2,null,"No",1,null,-40,105,2.7,5.5,32,"HVQFN32",0.83,null,2,null,null,null,null,null,null,null,"Kinetis KE02: 40MHz CortexM0+ 5V/Robust MCU, 32KB Flash, 4KB SRAM, 32QFN",null,null,null,0,"No"]
["MKE02Z64VFM4","NXPMKE02Z64VFM4","NXP","ARM CM0+",40,64,0.25600000000000001,4,12,null,2,null,28,"No",1,2,null,"No",1,null,-40,105,2.7,5.5,32,"HVQFN32",0.94,null,2,null,null,null,null,null,null,null,"Kinetis KE02: 40MHz CortexM0+ 5V/Robust MCU, 64KB Flash, 4KB SRAM, 32QFN",null,null,null,0,"No"]
["MKE14F256VLH16","NXPMKE14F256VLH16","NXP","ARM CM4F",160,320,4,32,12,null,3,null,58,"No",2,2,null,"No",1,null,-40,105,2.7,5.5,64,"LQFP64",1.99,null,3,null,null,null,null,null,null,null,"Kinetis KE14F: 160MHz CortexM4F 5V/Robust MCU, 256KB Flash + 64KB FlexMem, 32KB RAM, 64LQFP",null,null,null,0,"No"]
["MKE14F256VLL16","NXPMKE14F256VLL16","NXP","ARM CM4F",160,320,4,32,12,null,3,null,89,"No",2,2,null,"No",1,null,-40,105,2.7,5.5,100,"LQFP100",2.13,null,3,null,null,null,null,null,null,null,"Kinetis KE14F: 160MHz CortexM4F 5V/Robust MCU, 256KB Flash + 64KB FlexMem, 32KB RAM, 100LQFP",null,null,null,0,"No"]
["MKE14F512VLH16","NXPMKE14F512VLH16","NXP","ARM CM4F",160,576,4,64,12,null,3,null,58,"No",2,2,null,"No",1,null,-40,105,2.7,5.5,64,"LQFP64",2.62,null,3,null,null,null,null,null,null,null,"Kinetis KE14F: 160MHz CortexM4F 5V/Robust MCU, 512KB Flash + 64KB FlexMem, 64KB RAM, 64LQFP",null,null,null,0,"No"]
["MKE16F256VLH16","NXPMKE16F256VLH16","NXP","ARM CM4F",160,320,4,32,12,null,3,null,58,"No",2,2,null,"No",1,null,-40,105,2.7,5.5,64,"LQFP64",2.21,null,3,null,null,null,null,null,null,null,"Kinetis KE16F: 160MHz CortexM4F 5V/Robust MCU, 256KB Flash + 64KB FlexMem, 32KB RAM, 1xCAN, 64LQFP",null,null,null,0,"No"]
["MKE16F256VLL16","NXPMKE16F256VLL16","NXP","ARM CM4F",160,320,4,32,12,null,3,null,89,"No",2,2,null,{"$f":"IF(OR(ISBLANK(AO366), AO366=0), \"No\", \"Yes\")","v":"No"},1,null,-40,105,2.7,5.5,100,"LQFP100",2.36,null,3,null,null,null,null,null,null,null,"Kinetis KE16F: 160MHz CortexM4F 5V/Robust MCU, 256KB Flash + 64KB FlexMem, 32KB RAM, 1xCAN, 100LQFP",null,null,null,0,"No"]
["MKE16F512VLH16","NXPMKE16F512VLH16","NXP","ARM CM4F",160,576,4,64,12,null,3,null,58,"No",2,2,null,"No",1,null,-40,105,2.7,5.5,64,"LQFP64",2.84,null,3,null,null,null,null,null,null,null,"Kinetis KE16F: 160MHz CortexM4F 5V/Robust MCU, 512KB Flash + 64KB FlexMem, 64KB RAM, 1xCAN, 64LQFP",null,null,null,0,"No"]
["MKE16F512VLL16","NXPMKE16F512VLL16","NXP","ARM CM4F",160,576,4,64,12,null,3,null,89,"No",2,2,null,"No",1,null,-40,105,2.7,5.5,100,"LQFP100",2.99,null,3,null,null,null,null,null,null,null,"Kinetis KE16F: 160MHz CortexM4F 5V/Robust MCU, 512KB Flash + 64KB FlexMem, 64KB RAM, 1xCAN, 100LQFP",null,null,null,0,"No"]
["MKE18F256VLH16","NXPMKE18F256VLH16","NXP","ARM CM4F",160,320,4,32,12,null,3,null,58,"No",2,2,null,"No",1,null,-40,105,2.7,5.5,64,"LQFP64",2.44,null,3,null,null,null,null,null,null,null,"Kinetis KE18F: 160MHz CortexM4F 5V/Robust MCU, 256KB Flash + 64KB FlexMem, 32KB RAM, 2xCAN, 64LQFP",null,null,null,0,"No"]
["MKE18F256VLL16","NXPMKE18F256VLL16","NXP","ARM CM4F",160,320,4,32,12,null,3,null,89,"No",2,2,null,"No",1,null,-40,105,2.7,5.5,100,"LQFP100",2.59,null,3,null,null,null,null,null,null,null,"Kinetis KE18F: 160MHz CortexM4F 5V/Robust MCU, 256KB Flash + 64KB FlexMem, 32KB RAM, 2xCAN, 100LQFP",null,null,null,0,"No"]
["MKE18F512VLH16","NXPMKE18F512VLH16","NXP","ARM CM4F",160,576,4,64,12,null,3,null,58,"No",2,2,null,"No",1,null,-40,105,2.7,5.5,64,"LQFP64",3.07,null,3,null,null,null,null,null,null,null,"Kinetis KE18F: 160MHz CortexM4F 5V/Robust MCU, 512KB Flash + 64KB FlexMem, 64KB RAM, 2xCAN, 64LQFP",null,null,null,0,"No"]
["MKE18F512VLL16","NXPMKE18F512VLL16","NXP","ARM CM4F",160,576,4,64,12,null,3,null,89,"No",2,2,null,"No",1,null,-40,105,2.7,5.5,100,"LQFP100",3.21,null,3,null,null,null,null,null,null,null,"Kinetis KE18F: 160MHz CortexM4F 5V/Robust MCU, 512KB Flash + 64KB FlexMem, 64KB RAM, 2xCAN, 100LQFP",null,null,null,0,"No"]
["PK12DN512VLH5","NXPPK12DN512VLH5","NXP","ARM CM4",50,512,null,64,16,null,1,null,44,"No",2,1,1,"No",1,null,-40,105,1.71,3.6,64,"LQFP64",2.8,null,3,null,null,null,null,null,null,null,"Kinetis K12: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, 64LQFP",null,null,null,0,"No"]
["KK20DN512ZCAB10R","NXPKK20DN512ZCAB10R","NXP","ARM CM0",100,512,null,null,16,null,0,null,79,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,120,"WLCSP120",5.73,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit MCU, ARM CM4 core, 512KB Flash, 100MHz, USB, WLCSP 120",null,null,null,1,"Yes"]
["KK22FN128CAH12R","NXPKK22FN128CAH12R","NXP","ARM CM0",120,128,null,null,16,null,0,null,40,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,64,"WLCSP64",3.69,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit MCU, ARM CM4 core, 128KB Flash, 120MHz, USB, WLCSP 64",null,null,null,1,"No"]
["KK22FN256CAH12R","NXPKK22FN256CAH12R","NXP","ARM CM0",120,128,null,null,16,null,0,null,40,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,64,"WLCSP64",3.15,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit MCU, ARM CM4 core, 256KB Flash, 120MHz, USB, WLCSP 64",null,null,null,1,"No"]
["KK22FN256CAP12R","NXPKK22FN256CAP12R","NXP","ARM CM0",120,256,null,null,16,null,0,null,52,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,80,"WLCSP80",4.34,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit, ARM CM4 core, 256KB Flash, 120MHz, USB, 80WLCSP",null,null,null,1,"No"]
["KK22FN512CBP12R","NXPKK22FN512CBP12R","NXP","ARM CM0",120,512,null,null,16,null,0,null,52,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,80,"WLCSP80",4.34,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit, ARM CM4 core, 512KB Flash, 120MHz, USB, Thin 80WLCSP",null,null,null,1,"No"]
["KK60DN512ZCAB10R","NXPKK60DN512ZCAB10R","NXP","ARM CM0",100,512,null,null,16,null,0,null,79,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,120,"WLCSP120",6.11,null,null,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Ethernet, 120WLCSP,",null,null,null,1,"Yes"]
["LPC11U12FBD48/201,","NXPLPC11U12FBD48/201,","NXP","ARM CM0",50,16,null,6,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.03,null,1,null,null,null,null,null,null,null,"16kB flash, 6kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U12FHN33/201,","NXPLPC11U12FHN33/201,","NXP","ARM CM0",50,16,null,6,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",0.96,null,1,null,null,null,null,null,null,null,"16kB flash, 6kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U13FBD48/201,","NXPLPC11U13FBD48/201,","NXP","ARM CM0",50,24,null,6,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.08,null,1,null,null,null,null,null,null,null,"24kB flash, 6kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U14FBD48/201,","NXPLPC11U14FBD48/201,","NXP","ARM CM0",50,32,null,6,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.1299999999999999,null,1,null,null,null,null,null,null,null,"32kB flash, 6kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U14FBD48/201J","NXPLPC11U14FBD48/201J","NXP","ARM CM0",50,32,null,6,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.1299999999999999,null,1,null,null,null,null,null,null,null,"32kB flash, 6kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U14FET48/201,","NXPLPC11U14FET48/201,","NXP","ARM CM0",50,32,null,6,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"TFBGA48",1.17,null,1,null,null,null,null,null,null,null,"32kB flash, 6kB SRAM, TFBGA48 package",null,null,null,1,"No"]
["LPC11U14FHI33/201,","NXPLPC11U14FHI33/201,","NXP","ARM CM0",50,32,null,6,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.0900000000000001,null,1,null,null,null,null,null,null,null,"32kB flash, 6kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U14FHN33/201,","NXPLPC11U14FHN33/201,","NXP","ARM CM0",50,32,null,6,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.06,null,1,null,null,null,null,null,null,null,"32kB flash, 6kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U22FBD48/30QL","NXPLPC11U22FBD48/30QL","NXP","ARM CM0",50,16,1,8,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.18,null,1,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC11U23FBD48/301,","NXPLPC11U23FBD48/301,","NXP","ARM CM0",50,24,1,8,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.19,null,1,null,null,null,null,null,null,null,"24kB flash, 6kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U24FBD48/301,","NXPLPC11U24FBD48/301,","NXP","ARM CM0",50,32,2,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.36,null,1,null,null,null,null,null,null,null,"32kB flash, 8kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U24FBD48/401,","NXPLPC11U24FBD48/401,","NXP","ARM CM0",50,32,2,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.36,null,1,null,null,null,null,null,null,null,"32kB flash, 8kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U24FBD64/401,","NXPLPC11U24FBD64/401,","NXP","ARM CM0",50,32,4,10,10,null,0,null,54,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,64,"LQFP64",1.44,null,1,null,null,null,null,null,null,null,"32kB flash, 8kB SRAM, LQFP64 package",null,null,null,1,"No"]
["LPC11U24FET48/301,","NXPLPC11U24FET48/301,","NXP","ARM CM0",50,32,2,8,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"TFBGA48",1.32,null,1,null,null,null,null,null,null,null,"32kB flash, 6kB SRAM, TFBGA48 package",null,null,null,1,"No"]
["LPC11U24FHI33/301,","NXPLPC11U24FHI33/301,","NXP","ARM CM0",50,32,2,8,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.23,null,1,null,null,null,null,null,null,null,"32kB flash, 6kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U24FHI33/301Y","NXPLPC11U24FHI33/301Y","NXP","ARM CM0",50,32,2,8,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.23,null,1,null,null,null,null,null,null,null,"32kB flash, 6kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U24FHN33/401,","NXPLPC11U24FHN33/401,","NXP","ARM CM0",50,32,4,10,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.29,null,1,null,null,null,null,null,null,null,"32kB flash, 8kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U34FBD48/311,","NXPLPC11U34FBD48/311,","NXP","ARM CM0",50,40,4,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.46,null,1,null,null,null,null,null,null,null,"40kB flash, 8kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U34FBD48/421,","NXPLPC11U34FBD48/421,","NXP","ARM CM0",50,40,4,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.46,null,1,null,null,null,null,null,null,null,"40kB flash, 8kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U34FHN33/311,","NXPLPC11U34FHN33/311,","NXP","ARM CM0",50,48,4,10,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.39,null,1,null,null,null,null,null,null,null,"40kB flash, 8kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U34FHN33/421,","NXPLPC11U34FHN33/421,","NXP","ARM CM0",50,48,4,10,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.39,null,1,null,null,null,null,null,null,null,"40kB flash, 8kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U35FBD48/401,","NXPLPC11U35FBD48/401,","NXP","ARM CM0",50,64,4,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.58,null,1,null,null,null,null,null,null,null,"64kB flash, 10kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U35FBD48/401K","NXPLPC11U35FBD48/401K","NXP","ARM CM0",50,64,4,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.58,null,1,null,null,null,null,null,null,null,"64kB flash, 10kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U35FBD64/401,","NXPLPC11U35FBD64/401,","NXP","ARM CM0",50,64,4,10,10,null,0,null,54,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,64,"LQFP64",1.66,null,1,null,null,null,null,null,null,null,"64kB flash, 10kB SRAM, LQFP64 package",null,null,null,1,"No"]
["LPC11U35FET48/501,","NXPLPC11U35FET48/501,","NXP","ARM CM0",50,64,4,12,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"TFBGA48",1.66,null,1,null,null,null,null,null,null,null,"64kB flash, 12kB SRAM, TFBGA48 package",null,null,null,1,"No"]
["LPC11U35FHI33/501,","NXPLPC11U35FHI33/501,","NXP","ARM CM0",50,64,4,12,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.57,null,1,null,null,null,null,null,null,null,"64kB flash, 12kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U35FHI33/501Y","NXPLPC11U35FHI33/501Y","NXP","ARM CM0",50,64,4,12,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.57,null,1,null,null,null,null,null,null,null,"64kB flash, 12kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U35FHN33/401,","NXPLPC11U35FHN33/401,","NXP","ARM CM0",50,64,4,10,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.51,null,1,null,null,null,null,null,null,null,"64kB flash, 10kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U35FHN33/501,","NXPLPC11U35FHN33/501,","NXP","ARM CM0",50,64,4,10,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.51,null,1,null,null,null,null,null,null,null,"64kB flash, 10kB SRAM, HVQFN32 package",null,null,null,1,"No"]
["LPC11U36FBD48/401,","NXPLPC11U36FBD48/401,","NXP","ARM CM0",50,96,4,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.76,null,1,null,null,null,null,null,null,null,"96kB flash, 10kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U36FBD64/401,","NXPLPC11U36FBD64/401,","NXP","ARM CM0",50,96,4,10,10,null,0,null,54,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,64,"LQFP64",1.83,null,1,null,null,null,null,null,null,null,"96kB flash, 10kB SRAM, LQFP64 package",null,null,null,1,"No"]
["LPC11U37FBD48/401,","NXPLPC11U37FBD48/401,","NXP","ARM CM0",50,128,4,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.8,null,1,null,null,null,null,null,null,null,"128kB flash, 10kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U37FBD48/401K","NXPLPC11U37FBD48/401K","NXP","ARM CM0",50,128,4,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.8,null,1,null,null,null,null,null,null,null,"128kB flash, 10kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U37FBD48/40EL","NXPLPC11U37FBD48/40EL","NXP","ARM CM0",50,128,4,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.8,null,1,null,null,null,null,null,null,null,"128kB flash, 10kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U37FBD48/501,","NXPLPC11U37FBD48/501,","NXP","ARM CM0",50,128,4,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.8,null,1,null,null,null,null,null,null,null,"128kB flash, 10kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U37FBD48/CPQL","NXPLPC11U37FBD48/CPQL","NXP","ARM CM0",50,128,4,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,48,"LQFP48",1.8,null,1,null,null,null,null,null,null,null,"128kB flash, 10kB SRAM, LQFP48 package",null,null,null,1,"No"]
["LPC11U37FBD64/401,","NXPLPC11U37FBD64/401,","NXP","ARM CM0",50,128,4,12,10,null,0,null,54,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,64,"LQFP64",1.9,null,1,null,null,null,null,null,null,null,"128kB flash, 12kB SRAM, LQFP64 package",null,null,null,1,"No"]
["LPC11U37FBD64/501,","NXPLPC11U37FBD64/501,","NXP","ARM CM0",50,128,4,12,10,null,0,null,54,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,64,"LQFP64",1.9,null,1,null,null,null,null,null,null,null,"128kB flash, 12kB SRAM, LQFP64 package",null,null,null,1,"No"]
["LPC11U37FBD64/501J","NXPLPC11U37FBD64/501J","NXP","ARM CM0",50,128,4,12,10,null,0,null,54,"No",1,2,null,"Yes",2,null,-40,85,1.8,3.6,64,"LQFP64",1.9,null,1,null,null,null,null,null,null,null,"128kB flash, 12kB SRAM, LQFP64 package",null,null,null,1,"No"]
["LPC11U37HFBD64/4QL","NXPLPC11U37HFBD64/4QL","NXP","ARM CM0",50,128,4,12,10,null,0,null,54,"No",2,2,null,"Yes",2,null,-40,85,1.8,3.6,64,"LQFP64",1.95,null,2,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC11U37HFBD64QL","NXPLPC11U37HFBD64QL","NXP","ARM CM0",50,128,4,12,10,null,0,null,54,"No",2,2,null,"Yes",2,null,-40,85,1.8,3.6,64,"LQFP64",1.95,null,2,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC11U66JBD48E","NXPLPC11U66JBD48E","NXP","ARM CM0+",50,64,4,12,12,null,0,null,34,"No",2,2,null,"Yes",2,null,-40,105,2.4,3.6,48,"LQFP48",1.55,null,3,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC11U67JBD100E","NXPLPC11U67JBD100E","NXP","ARM CM0+",50,128,4,20,12,null,0,null,80,"No",2,2,null,"Yes",2,null,-40,105,2.4,3.6,100,"LQFP100",1.99,null,5,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC11U67JBD48E","NXPLPC11U67JBD48E","NXP","ARM CM0+",50,128,4,20,12,null,0,null,34,"No",2,2,null,"Yes",2,null,-40,105,2.4,3.6,48,"LQFP48",1.62,null,3,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC11U67JBD64E","NXPLPC11U67JBD64E","NXP","ARM CM0+",50,128,4,20,12,null,0,null,48,"No",2,2,null,"Yes",2,null,-40,105,2.4,3.6,64,"LQFP64",1.66,null,3,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC11U68JBD100E","NXPLPC11U68JBD100E","NXP","ARM CM0+",50,256,4,36,12,null,0,null,80,"No",2,2,null,"Yes",2,null,-40,105,2.4,3.6,100,"LQFP100",2.1,null,5,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC11U68JBD100K","NXPLPC11U68JBD100K","NXP","ARM CM0+",50,256,4,36,12,null,0,null,80,"No",2,2,null,"Yes",2,null,-40,105,2.4,3.6,100,"LQFP100",2.1,null,5,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC11U68JBD48E","NXPLPC11U68JBD48E","NXP","ARM CM0+",50,256,4,36,12,null,0,null,34,"No",2,2,null,"Yes",2,null,-40,105,2.4,3.6,48,"LQFP48",1.77,null,3,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC11U68JBD64E","NXPLPC11U68JBD64E","NXP","ARM CM0+",50,256,4,36,12,null,0,null,48,"No",2,2,null,"Yes",2,null,-40,105,2.4,3.6,64,"LQFP64",1.81,null,3,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC11U68JBD64K","NXPLPC11U68JBD64K","NXP","ARM CM0+",50,256,4,36,12,null,0,null,48,"No",2,2,null,"Yes",2,null,-40,105,2.4,3.6,64,"LQFP64",1.81,null,3,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,1,"No"]
["LPC1342FBD48,118","NXPLPC1342FBD48,118","NXP","ARM CM3",72,16,null,4,10,null,0,null,40,"No",1,1,null,{"$f":"IF(OR(ISBLANK(AO430), AO430=0), \"No\", \"Yes\")","v":"Yes"},2,null,-40,85,2,3.6,48,"LQFP48",1.42,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1342FBD48,151","NXPLPC1342FBD48,151","NXP","ARM CM3",72,16,null,4,10,null,0,null,40,"No",1,1,null,"Yes",2,null,-40,85,2,3.6,48,"LQFP48",1.42,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1342FHN33,518","NXPLPC1342FHN33,518","NXP","ARM CM3",72,16,null,4,10,null,0,null,28,"No",1,1,null,"Yes",2,null,-40,85,2,3.6,32,"HVQFN32",1.35,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1342FHN33,551","NXPLPC1342FHN33,551","NXP","ARM CM3",72,16,null,4,10,null,0,null,28,"No",1,1,null,"Yes",2,null,-40,85,2,3.6,32,"HVQFN32",1.35,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1343FBD48,151","NXPLPC1343FBD48,151","NXP","ARM CM3",72,32,null,8,10,null,0,null,40,"No",1,1,null,"Yes",2,null,-40,85,2,3.6,48,"LQFP48",1.56,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1343FHN33,118","NXPLPC1343FHN33,118","NXP","ARM CM3",72,32,null,8,10,null,0,null,28,"No",1,1,null,"Yes",2,null,-40,85,2,3.6,32,"HVQFN32",1.49,null,1,null,null,null,null,null,null,null,"32kB Flash, 8kB  SRAM, USB Device",null,null,null,1,"No"]
["LPC1343FHN33,518","NXPLPC1343FHN33,518","NXP","ARM CM3",72,32,null,8,10,null,0,null,28,"No",1,1,null,"Yes",2,null,-40,85,2,3.6,32,"HVQFN32",1.49,null,1,null,null,null,null,null,null,null,"32kB Flash, 8kB  SRAM, USB Device",null,null,null,1,"No"]
["LPC1343FHN33,551","NXPLPC1343FHN33,551","NXP","ARM CM3",72,32,null,8,10,null,0,null,28,"No",1,1,null,"Yes",2,null,-40,85,2,3.6,32,"HVQFN32",1.49,null,1,null,null,null,null,null,null,null,"32kB Flash, 8kB  SRAM, USB Device",null,null,null,1,"No"]
["LPC1345FBD48,151","NXPLPC1345FBD48,151","NXP","ARM CM3",72,32,2,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,2,3.6,48,"LQFP48",1.79,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1345FHN33,551","NXPLPC1345FHN33,551","NXP","ARM CM3",72,32,2,10,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,2,3.6,32,"HVQFN32",1.72,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1346FBD48,151","NXPLPC1346FBD48,151","NXP","ARM CM3",72,48,4,10,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,2,3.6,48,"LQFP48",1.92,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1346FHN33,551","NXPLPC1346FHN33,551","NXP","ARM CM3",72,48,4,10,10,null,0,null,26,"No",1,2,null,"Yes",2,null,-40,85,2,3.6,32,"HVQFN32",1.85,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1347FBD48,151","NXPLPC1347FBD48,151","NXP","ARM CM3",72,64,4,12,10,null,0,null,40,"No",1,2,null,"Yes",2,null,-40,85,2,3.6,48,"LQFP48",2.0499999999999998,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1347FBD64,551","NXPLPC1347FBD64,551","NXP","ARM CM3",72,64,4,12,10,null,0,null,51,"No",1,2,null,"Yes",2,null,-40,85,2,3.6,64,"LQFP64",2.12,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1547JBD48QL","NXPLPC1547JBD48QL","NXP","ARM CM3",72,64,4,12,12,null,0,null,30,"No",1,2,null,"Yes",4,null,-40,105,2.4,3.6,48,"LQFP48",2.2599999999999998,null,3,null,null,null,null,null,null,null,"Motion Control 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1547JBD64QL","NXPLPC1547JBD64QL","NXP","ARM CM3",72,64,4,12,12,null,0,null,44,"No",1,2,null,"Yes",4,null,-40,105,2.4,3.6,64,"LQFP64",2.4300000000000002,null,3,null,null,null,null,null,null,null,"Motion Control 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1548JBD100E","NXPLPC1548JBD100E","NXP","ARM CM3",72,128,4,20,12,null,0,null,76,"No",1,2,null,"Yes",4,null,-40,105,2.4,3.6,100,"LQFP100",2.83,null,3,null,null,null,null,null,null,null,"Motion Control 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1548JBD64QL","NXPLPC1548JBD64QL","NXP","ARM CM3",72,128,4,20,12,null,0,null,44,"No",1,2,null,"Yes",4,null,-40,105,2.4,3.6,64,"LQFP64",2.67,null,3,null,null,null,null,null,null,null,"Motion Control 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1549JBD100E","NXPLPC1549JBD100E","NXP","ARM CM3",72,256,4,36,12,null,0,null,76,"No",1,2,null,"Yes",4,null,-40,105,2.4,3.6,100,"LQFP100",3.15,null,3,null,null,null,null,null,null,null,"Motion Control 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1549JBD48QL","NXPLPC1549JBD48QL","NXP","ARM CM3",72,256,4,36,12,null,0,null,30,"No",1,2,null,"Yes",4,null,-40,105,2.4,3.6,48,"LQFP48",2.83,null,3,null,null,null,null,null,null,null,"Motion Control 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1549JBD64QL","NXPLPC1549JBD64QL","NXP","ARM CM3",72,256,4,36,12,null,0,null,44,"No",1,2,null,"Yes",4,null,-40,105,2.4,3.6,64,"LQFP64",2.99,null,3,null,null,null,null,null,null,null,"Motion Control 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1751FBD80,551","NXPLPC1751FBD80,551","NXP","ARM CM3",100,32,null,8,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",null,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1752FBD80,551","NXPLPC1752FBD80,551","NXP","ARM CM3",100,64,null,16,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",2.77,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1754FBD80,551","NXPLPC1754FBD80,551","NXP","ARM CM3",100,128,null,32,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",3.2,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1754FBD80K","NXPLPC1754FBD80K","NXP","ARM CM3",100,128,null,32,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",3.2,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1756FBD80,551","NXPLPC1756FBD80,551","NXP","ARM CM3",100,256,null,32,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",3.29,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1756FBD80K","NXPLPC1756FBD80K","NXP","ARM CM3",100,256,null,32,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",3.29,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1756FBD80Y","NXPLPC1756FBD80Y","NXP","ARM CM3",100,256,null,32,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",3.29,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1758FBD80,551","NXPLPC1758FBD80,551","NXP","ARM CM3",100,512,null,64,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",4.12,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1758FBD80K","NXPLPC1758FBD80K","NXP","ARM CM3",100,512,null,64,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",4.12,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1758FBD80Y","NXPLPC1758FBD80Y","NXP","ARM CM3",100,512,null,64,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",4.12,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1759FBD80,551","NXPLPC1759FBD80,551","NXP","ARM CM3",100,512,null,64,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",4.12,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1759FBD80Y","NXPLPC1759FBD80Y","NXP","ARM CM3",100,512,null,64,12,null,0,null,52,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,80,"LQFP80",4.12,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1764FBD100,551","NXPLPC1764FBD100,551","NXP","ARM CM3",100,128,null,32,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"LQFP100",3.15,null,4,null,null,null,null,null,null,null,"128kB flash, 32kB SRAM, Ethernet, USB, LQFP100 package",null,null,null,1,"No"]
["LPC1764FBD100K","NXPLPC1764FBD100K","NXP","ARM CM3",100,128,null,32,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"LQFP100",3.15,null,4,null,null,null,null,null,null,null,"128kB flash, 32kB SRAM, Ethernet, USB, LQFP100 package",null,null,null,1,"No"]
["LPC1765FBD100,551","NXPLPC1765FBD100,551","NXP","ARM CM3",100,256,null,64,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"LQFP100",3.64,null,4,null,null,null,null,null,null,null,"256kB flash, 64kB SRAM, USB, LQFP100 package",null,null,null,1,"No"]
["LPC1765FBD100K","NXPLPC1765FBD100K","NXP","ARM CM3",100,256,null,64,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"LQFP100",3.64,null,4,null,null,null,null,null,null,null,"256kB flash, 64kB SRAM, USB, LQFP100 package",null,null,null,1,"No"]
["LPC1765FET100,551","NXPLPC1765FET100,551","NXP","ARM CM3",100,256,null,64,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"TFBGA100",3.64,null,4,null,null,null,null,null,null,null,"256kB flash, 64kB SRAM, USB, TFBGA100 package",null,null,null,1,"No"]
["LPC1766FBD100,551","NXPLPC1766FBD100,551","NXP","ARM CM3",100,256,null,64,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"LQFP100",3.88,null,4,null,null,null,null,null,null,null,"256kB flash, 64kB SRAM, Ethernet, USB, LQFP100 package",null,null,null,1,"No"]
["LPC1766FBD100K","NXPLPC1766FBD100K","NXP","ARM CM3",100,256,null,64,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"LQFP100",3.88,null,4,null,null,null,null,null,null,null,"256kB flash, 64kB SRAM, Ethernet, USB, LQFP100 package",null,null,null,1,"No"]
["LPC1768FBD100,551","NXPLPC1768FBD100,551","NXP","ARM CM3",100,512,null,64,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"LQFP100",4.37,null,4,null,null,null,null,null,null,null,"512kB flash, 64kB SRAM, Ethernet, USB, LQFP100 package",null,null,null,1,"No"]
["LPC1768FBD100K","NXPLPC1768FBD100K","NXP","ARM CM3",100,512,null,64,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"LQFP100",4.37,null,4,null,null,null,null,null,null,null,"512kB flash, 64kB SRAM, Ethernet, USB, LQFP100 package",null,null,null,1,"No"]
["LPC1768FET100,551","NXPLPC1768FET100,551","NXP","ARM CM3",100,512,null,64,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"TFBGA100",4.37,null,4,null,null,null,null,null,null,null,"512kB flash, 64kB SRAM, Ethernet, USB, TFBGA100 package",null,null,null,1,"No"]
["LPC1768FET100Y","NXPLPC1768FET100Y","NXP","ARM CM3",100,512,null,64,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"TFBGA100",4.37,null,4,null,null,null,null,null,null,null,"512kB flash, 64kB SRAM, Ethernet, USB, TFBGA100 package",null,null,null,1,"No"]
["LPC1769FBD100,551","NXPLPC1769FBD100,551","NXP","ARM CM3",120,512,null,64,12,null,0,null,70,"No",3,2,null,"Yes",10,null,-40,85,2.4,3.6,100,"LQFP100",4.5599999999999996,null,4,null,null,null,null,null,null,null,"512kB flash, 64kB SRAM, Ethernet, USB, LQFP100 package",null,null,null,1,"No"]
["LPC1774FBD144,551","NXPLPC1774FBD144,551","NXP","ARM CM3",120,128,2,40,12,null,0,null,109,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,144,"LQFP144",3.9,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1774FBD208,551","NXPLPC1774FBD208,551","NXP","ARM CM3",120,128,2,40,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",4.92,null,4,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1776FBD208,551","NXPLPC1776FBD208,551","NXP","ARM CM3",120,256,4,80,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",4.97,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1776FBD208K","NXPLPC1776FBD208K","NXP","ARM CM3",120,256,4,80,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",4.97,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1776FET180,551","NXPLPC1776FET180,551","NXP","ARM CM3",120,256,4,80,12,null,0,null,141,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,180,"TFBGA180",4.17,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1777FBD208,551","NXPLPC1777FBD208,551","NXP","ARM CM3",120,512,4,96,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",4.9800000000000004,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1778FBD144,551","NXPLPC1778FBD144,551","NXP","ARM CM3",120,512,4,96,12,null,0,null,109,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,144,"LQFP144",4.51,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1778FBD144K","NXPLPC1778FBD144K","NXP","ARM CM3",120,512,4,96,12,null,0,null,109,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,144,"LQFP144",4.51,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1778FBD208,551","NXPLPC1778FBD208,551","NXP","ARM CM3",120,512,4,96,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",4.9800000000000004,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1778FBD208K","NXPLPC1778FBD208K","NXP","ARM CM3",120,512,4,96,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",4.9800000000000004,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1778FET180,551","NXPLPC1778FET180,551","NXP","ARM CM3",120,512,4,96,12,null,0,null,141,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,180,"TFBGA180",4.6100000000000003,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1778FET208,551","NXPLPC1778FET208,551","NXP","ARM CM3",120,512,4,96,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"TFBGA208",4.71,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1785FBD208,551","NXPLPC1785FBD208,551","NXP","ARM CM3",120,256,4,80,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",5,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1785FBD208K","NXPLPC1785FBD208K","NXP","ARM CM3",120,256,4,80,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",5,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1786FBD208,551","NXPLPC1786FBD208,551","NXP","ARM CM3",120,256,4,80,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",5,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1787FBD208,551","NXPLPC1787FBD208,551","NXP","ARM CM3",120,512,4,96,12,null,0,null,165,"Yes",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",5.43,null,5,null,null,null,null,null,null,null,"512kB flash, 96kB SRAM, USB, LCD, LQFP208 package",null,null,null,1,"No"]
["LPC1788FBD144,551","NXPLPC1788FBD144,551","NXP","ARM CM3",120,512,4,96,12,null,0,null,109,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,144,"LQFP144",5.58,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1788FBD208,551","NXPLPC1788FBD208,551","NXP","ARM CM3",120,512,4,96,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",5.77,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1788FBD208K","NXPLPC1788FBD208K","NXP","ARM CM3",120,512,4,96,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",5.77,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1788FET180,551","NXPLPC1788FET180,551","NXP","ARM CM3",120,512,4,96,12,null,0,null,141,"No",3,3,null,{"$f":"IF(OR(ISBLANK(AO494), AO494=0), \"No\", \"Yes\")","v":"Yes"},9,null,-40,85,2.4,3.6,180,"TFBGA180",5.68,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1788FET208,551","NXPLPC1788FET208,551","NXP","ARM CM3",120,512,4,96,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"TFBGA208",5.77,null,5,null,null,null,null,null,null,null,"Scalable Mainstream 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,1,"No"]
["LPC1820FBD144,551","NXPLPC1820FBD144,551","NXP","ARM CM3",180,null,null,168,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,144,"LQFP144",3.25,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1820FBD144/CPAE","NXPLPC1820FBD144/CPAE","NXP","ARM CM3",180,null,null,168,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,144,"LQFP144",3.25,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1820FET100,551","NXPLPC1820FET100,551","NXP","ARM CM3",180,null,null,168,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,100,"TFBGA100",3.01,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1820FET100/CPAE","NXPLPC1820FET100/CPAE","NXP","ARM CM3",180,null,null,168,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,100,"TFBGA100",3.01,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1822JBD144E","NXPLPC1822JBD144E","NXP","ARM CM3",180,512,16,104,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,144,"LQFP144",4.7699999999999996,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1822JET100E","NXPLPC1822JET100E","NXP","ARM CM3",180,512,16,104,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,100,"TFBGA100",4.46,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1823JBD144E","NXPLPC1823JBD144E","NXP","ARM CM3",180,512,16,104,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,144,"LQFP144",4.7699999999999996,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1823JET100E","NXPLPC1823JET100E","NXP","ARM CM3",180,512,16,104,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,100,"TFBGA100",4.6100000000000003,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1825JBD144E","NXPLPC1825JBD144E","NXP","ARM CM3",180,768,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,144,"LQFP144",5.14,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1825JET100/MP1E","NXPLPC1825JET100/MP1E","NXP","ARM CM3",180,768,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,100,"TFBGA100",5,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1825JET100E","NXPLPC1825JET100E","NXP","ARM CM3",180,768,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,100,"TFBGA100",5,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1827JBD144E","NXPLPC1827JBD144E","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,144,"LQFP144",5.34,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC1827JET100E","NXPLPC1827JET100E","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,100,"TFBGA100",5.19,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,1,"No"]
["LPC4072FET80K","NXPLPC4072FET80K","NXP","ARM CM4",120,64,2,24,12,null,0,null,54,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,80,"TFBGA80",2.9,null,4,null,null,null,null,null,null,null,"Midrange 32bit Microcontroller (MCU) based on ARM CM4 Core",null,null,null,1,"No"]
["LPC4074FBD144,551","NXPLPC4074FBD144,551","NXP","ARM CM4",120,128,2,40,12,null,0,null,109,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,144,"LQFP144",3.28,null,4,null,null,null,null,null,null,null,"Midrange 32bit Microcontroller (MCU) based on ARM CM4 Core",null,null,null,1,"No"]
["LPC4074FBD80,551","NXPLPC4074FBD80,551","NXP","ARM CM4",120,128,2,40,12,null,0,null,54,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,80,"LQFP80",3.27,null,4,null,null,null,null,null,null,null,"32bit ARM CM4 MCU; up to 512 kB flash, 96 kB SRAM; USB Device/Host/OTG; Ethernet; EMC; SPIFI",null,null,null,1,"No"]
["LPC4076FBD144E","NXPLPC4076FBD144E","NXP","ARM CM4F",120,256,4,80,12,null,0,null,109,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,144,"LQFP144",4.1399999999999997,null,5,null,null,null,null,null,null,null,"Midrange 32bit Microcontroller (MCU) based on ARM CM4 Core",null,null,null,1,"No"]
["LPC4076FET180,551","NXPLPC4076FET180,551","NXP","ARM CM4F",120,256,4,80,12,null,0,null,142,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,180,"TFBGA180",4.0199999999999996,null,5,null,null,null,null,null,null,null,"Midrange 32bit Microcontroller (MCU) based on ARM CM4 Core",null,null,null,1,"No"]
["LPC4076FET180K","NXPLPC4076FET180K","NXP","ARM CM4F",120,256,4,80,12,null,0,null,142,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,180,"TFBGA180",4.0199999999999996,null,5,null,null,null,null,null,null,null,"Midrange 32bit Microcontroller (MCU) based on ARM CM4 Core",null,null,null,1,"No"]
["LPC4078FBD100E","NXPLPC4078FBD100E","NXP","ARM CM4F",120,512,4,96,12,null,0,null,69,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,100,"LQFP100",4.24,null,5,null,null,null,null,null,null,null,"32bit ARM CM4 MCU; up to 512 kB flash, 96 kB SRAM; USB Device/Host/OTG; Ethernet; EMC; SPIFI",null,null,null,1,"No"]
["LPC4078FBD144,551","NXPLPC4078FBD144,551","NXP","ARM CM4F",120,512,4,96,12,null,0,null,109,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,144,"LQFP144",4.3499999999999996,null,5,null,null,null,null,null,null,null,"32bit ARM CM4 MCU; up to 512 kB flash, 96 kB SRAM; USB Device/Host/OTG; Ethernet; EMC; SPIFI",null,null,null,1,"No"]
["LPC4078FBD208,551","NXPLPC4078FBD208,551","NXP","ARM CM4F",120,512,4,96,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",4.9000000000000004,null,5,null,null,null,null,null,null,null,"32bit ARM CM4 MCU; up to 512 kB flash, 96 kB SRAM; USB Device/Host/OTG; Ethernet; EMC; SPIFI",null,null,null,1,"No"]
["LPC4078FBD80,551","NXPLPC4078FBD80,551","NXP","ARM CM4F",120,512,4,96,12,null,0,null,null,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,80,"LQFP80",4.1399999999999997,null,5,null,null,null,null,null,null,null,"32bit ARM CM4 MCU; up to 512 kB flash, 96 kB SRAM; USB Device/Host/OTG; Ethernet; EMC; SPIFI",null,null,null,1,"No"]
["LPC4078FET180,551","NXPLPC4078FET180,551","NXP","ARM CM4F",120,512,4,96,12,null,0,null,142,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,180,"TFBGA180",4.24,null,5,null,null,null,null,null,null,null,"32bit ARM CM4 MCU; up to 512 kB flash, 96 kB SRAM; USB Device/Host/OTG; Ethernet; EMC; SPIFI",null,null,null,1,"No"]
["LPC4078FET208,551","NXPLPC4078FET208,551","NXP","ARM CM4F",120,512,4,96,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"TFBGA208",4.74,null,5,null,null,null,null,null,null,null,"32bit ARM CM4 MCU; up to 512 kB flash, 96 kB SRAM; USB Device/Host/OTG; Ethernet; EMC; SPIFI",null,null,null,1,"No"]
["LPC4088FBD144,551","NXPLPC4088FBD144,551","NXP","ARM CM4F",120,512,4,96,12,null,0,null,109,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,144,"LQFP144",5.13,null,5,null,null,null,null,null,null,null,"Midrange 32bit Microcontroller (MCU) based on ARM CM4 Core",null,null,null,1,"No"]
["LPC4088FBD208,551","NXPLPC4088FBD208,551","NXP","ARM CM4F",120,512,4,96,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"LQFP208",5.97,null,5,null,null,null,null,null,null,null,"Midrange 32bit Microcontroller (MCU) based on ARM CM4 Core",null,null,null,1,"No"]
["LPC4088FET180,551","NXPLPC4088FET180,551","NXP","ARM CM4F",120,512,4,96,12,null,0,null,142,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,180,"TFBGA180",4.88,null,5,null,null,null,null,null,null,null,"Midrange 32bit Microcontroller (MCU) based on ARM CM4 Core",null,null,null,1,"No"]
["LPC4088FET208,551","NXPLPC4088FET208,551","NXP","ARM CM4F",120,512,4,96,12,null,0,null,165,"No",3,3,null,"Yes",9,null,-40,85,2.4,3.6,208,"TFBGA208",5.31,null,5,null,null,null,null,null,null,null,"Midrange 32bit Microcontroller (MCU) based on ARM CM4 Core",null,null,null,1,"No"]
["LPC4320FBD144,551","NXPLPC4320FBD144,551","NXP","ARM CM4F",204,null,null,200,10,null,0,null,83,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,144,"LQFP144",3.44,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,1,"No"]
["LPC4320FET100,551","NXPLPC4320FET100,551","NXP","ARM CM4F",204,null,null,200,10,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,100,"TFBGA100",3.3,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,1,"No"]
["LPC4322JBD144E","NXPLPC4322JBD144E","NXP","ARM CM4F",204,512,16,104,10,null,0,null,83,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,144,"LQFP144",5.38,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; two Highspeed USB, LCD, EMC",null,null,null,1,"No"]
["LPC4322JET100E","NXPLPC4322JET100E","NXP","ARM CM4F",204,512,16,104,10,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,100,"TFBGA100",5.24,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,1,"No"]
["LPC4323JBD144E","NXPLPC4323JBD144E","NXP","ARM CM4F",204,512,16,104,10,null,0,null,83,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,144,"LQFP144",5.53,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,1,"No"]
["LPC4323JET100E","NXPLPC4323JET100E","NXP","ARM CM4F",204,512,16,104,10,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,100,"TFBGA100",5.38,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,1,"No"]
["LPC4325JBD144E","NXPLPC4325JBD144E","NXP","ARM CM4F",204,768,16,136,10,null,0,null,83,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,144,"LQFP144",5.92,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; two Highspeed USB, LCD, EMC",null,null,null,1,"No"]
["LPC4325JET100E","NXPLPC4325JET100E","NXP","ARM CM4F",204,768,16,136,10,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,100,"TFBGA100",5.77,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,1,"No"]
["LPC4327JBD144E","NXPLPC4327JBD144E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,83,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,144,"LQFP144",6.11,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; two Highspeed USB, LCD, EMC",null,null,null,1,"No"]
["LPC4327JET100E","NXPLPC4327JET100E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,100,"TFBGA100",5.97,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,1,"No"]
["LPC43S20FBD144E","NXPLPC43S20FBD144E","NXP","ARM CM4F",204,null,null,282,10,null,0,null,83,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,144,"LQFP144",3.54,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 flashless MCU with security features; 200 kB SRAM; USB",null,null,null,1,"No"]
["LPC43S20FET180E","NXPLPC43S20FET180E","NXP","ARM CM4F",204,null,null,200,10,null,0,null,118,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,180,"TFBGA180",3.49,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 flashless MCU with security features; 200 kB SRAM; USB",null,null,null,1,"No"]
["LPC43S20FET180K","NXPLPC43S20FET180K","NXP","ARM CM4F",204,null,null,200,10,null,0,null,118,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,180,"TFBGA180",3.49,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 flashless MCU with security features; 200 kB SRAM; USB",null,null,null,1,"No"]
["LPC54113J256BD64QL","NXPLPC54113J256BD64QL","NXP","ARM CM4F",100,256,null,192,12,null,0,null,50,"No",8,8,null,"Yes",5,null,-40,105,1.62,3.6,64,"LQFP64",2.0299999999999998,null,8,null,null,null,null,null,null,null,"Low Power 32bit Microcontroller based on ARM&#174; Cortex&#174;M4",null,null,null,1,"No"]
["LPC54113J256UK49QL","NXPLPC54113J256UK49QL","NXP","ARM CM4F",100,null,null,192,12,null,0,null,37,"No",8,null,null,"Yes",null,null,-40,105,1.62,3.6,0,"NAU000",1.5,null,null,null,null,null,null,null,null,null,"Low Power 32bit Microcontroller based on ARM CM4",null,null,null,1,"No"]
["LPC54113J256UK49Z","NXPLPC54113J256UK49Z","NXP","ARM CM4F",100,null,null,192,12,null,0,null,37,"No",8,null,null,"Yes",null,null,-40,105,1.62,3.6,0,"NAU000",1.5,null,null,null,null,null,null,null,null,null,"Low Power 32bit Microcontroller based on ARM CM4",null,null,null,1,"No"]
["LPC54114J256BD64QL","NXPLPC54114J256BD64QL","NXP","ARM CM4F",100,256,null,192,12,null,0,null,50,"No",8,8,null,"Yes",5,null,-40,105,1.62,3.6,64,"LQFP64",2.13,null,8,null,null,null,null,null,null,null,"Low Power 32bit Microcontroller based on ARM CM4",null,null,null,1,"No"]
["LPC54114J256UK49QL","NXPLPC54114J256UK49QL","NXP","ARM CM4F",100,null,null,192,12,null,0,null,37,"No",8,null,null,"Yes",null,null,-40,105,1.71,3.6,0,"NAU000",1.58,null,null,null,null,null,null,null,null,null,"Low Power 32bit Microcontroller based on ARM CM4",null,null,null,1,"No"]
["LPC54114J256UK49Z","NXPLPC54114J256UK49Z","NXP","ARM CM4F",100,null,null,192,12,null,0,null,37,"No",8,null,null,"Yes",null,null,-40,105,1.71,3.6,0,"NAU000",1.58,null,null,null,null,null,null,null,null,null,"Low Power 32bit Microcontroller based on ARM CM4",null,null,null,1,"No"]
["MK20DN128VFM5","NXPMK20DN128VFM5","NXP","ARM CM4",50,128,null,16,16,null,0,null,20,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,32,"HVQFN32",2.14,null,2,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"Yes"]
["MK20DN128VFT5","NXPMK20DN128VFT5","NXP","ARM CM4",50,128,null,16,16,null,0,null,29,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,48,"HVQFN48",2.27,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"Yes"]
["MK20DN128VLF5","NXPMK20DN128VLF5","NXP","ARM CM4",50,128,null,16,16,null,0,null,29,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,48,"LQFP48",2.2400000000000002,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 48LQFP",null,null,null,1,"Yes"]
["MK20DN128VLH5","NXPMK20DN128VLH5","NXP","ARM CM4",50,128,null,16,16,null,0,null,40,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,64,"LQFP64",2.34,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"Yes"]
["MK20DN128VMP5","NXPMK20DN128VMP5","NXP","ARM CM4",50,128,null,16,16,null,0,null,40,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,64,"LFBGA64",2.68,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 64MAPBGA",null,null,null,1,"Yes"]
["MK20DN32VFM5","NXPMK20DN32VFM5","NXP","ARM CM4",50,32,null,8,16,null,0,null,20,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.64,null,2,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 32KB Flash, 8KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"Yes"]
["MK20DN32VFT5","NXPMK20DN32VFT5","NXP","ARM CM4",50,32,null,8,16,null,0,null,29,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,48,"HVQFN48",1.78,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 32KB Flash, 8KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"Yes"]
["MK20DN32VLF5","NXPMK20DN32VLF5","NXP","ARM CM4",50,32,null,8,16,null,0,null,29,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,48,"LQFP48",1.74,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 32KB Flash, 8KB SRAM, FullSpeed USB, 48LQFP",null,null,null,1,"Yes"]
["MK20DN32VLH5","NXPMK20DN32VLH5","NXP","ARM CM4",50,32,null,8,16,null,0,null,40,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,64,"LQFP64",1.85,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 32KB Flash, 8KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"Yes"]
["MK20DN32VMP5","NXPMK20DN32VMP5","NXP","ARM CM4",50,32,null,8,16,null,0,null,40,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,64,"LFBGA64",2.1800000000000002,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 32KB Flash, 8KB SRAM, FullSpeed USB, 64MAPBGA",null,null,null,1,"Yes"]
["MK20DN512VLK10","NXPMK20DN512VLK10","NXP","ARM CM4",100,512,null,128,16,null,1,null,52,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",4.8,null,4,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"Yes"]
["MK20DN512VLK10R","NXPMK20DN512VLK10R","NXP","ARM CM4",100,512,null,128,16,null,1,null,52,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",4.8,null,4,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"Yes"]
["MK20DN512VLL10","NXPMK20DN512VLL10","NXP","ARM CM4",100,512,null,128,16,null,1,null,66,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",4.8600000000000003,null,5,null,null,null,null,null,null,null,"Kinetis K 32bit MCU, ARM CM4 core, 512KB Flash, 100MHz, USB, QFP 100",null,null,null,1,"Yes"]
["MK20DN512VLQ10","NXPMK20DN512VLQ10","NXP","ARM CM4",100,512,null,128,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.27,null,6,null,null,null,null,null,null,null,"Kinetis K 32bit MCU, ARM CM4 core, 512KB Flash, 100MHz, USB, QFP 144",null,null,null,1,"Yes"]
["MK20DN512VMC10","NXPMK20DN512VMC10","NXP","ARM CM4",100,512,null,128,16,null,2,null,86,"No",2,3,1,{"$f":"IF(OR(ISBLANK(AO558), AO558=0), \"No\", \"Yes\")","v":"Yes"},1,null,-40,105,1.71,3.6,121,"LFBGA121",5.0599999999999996,null,6,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"Yes"]
["MK20DN512VMD10","NXPMK20DN512VMD10","NXP","ARM CM4",100,512,null,128,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",5.33,null,6,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 144MAPBGA",null,null,null,1,"Yes"]
["MK20DN512ZCAB10R","NXPMK20DN512ZCAB10R","NXP","ARM CM0",100,512,null,null,16,null,0,null,79,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,120,"WLCSP120",5.73,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit MCU, ARM CM4 core, 512KB Flash, 100MHz, USB, WLCSP 120",null,null,null,1,"Yes"]
["MK20DN64VFM5","NXPMK20DN64VFM5","NXP","ARM CM4",50,64,null,16,16,null,0,null,20,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.83,null,2,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 64KB Flash, 16KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"Yes"]
["MK20DN64VFT5","NXPMK20DN64VFT5","NXP","ARM CM4",50,64,null,16,16,null,0,null,29,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,48,"HVQFN48",1.97,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 64KB Flash, 16KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"Yes"]
["MK20DN64VLF5","NXPMK20DN64VLF5","NXP","ARM CM4",50,64,null,16,16,null,0,null,29,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,48,"LQFP48",1.92,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 64KB Flash, 16KB SRAM, FullSpeed USB, 48LQFP",null,null,null,1,"Yes"]
["MK20DN64VLH5","NXPMK20DN64VLH5","NXP","ARM CM4",50,64,null,16,16,null,0,null,40,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,64,"LQFP64",2.0499999999999998,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 64KB Flash, 16KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"Yes"]
["MK20DN64VMP5","NXPMK20DN64VMP5","NXP","ARM CM4",50,64,null,16,16,null,0,null,40,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,64,"LFBGA64",2.37,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 64KB Flash, 16KB SRAM, FullSpeed USB, 64MAPBGA",null,null,null,1,"Yes"]
["MK20DX128VFM5","NXPMK20DX128VFM5","NXP","ARM CM4",50,160,2,16,16,null,0,null,20,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,32,"HVQFN32",2.2400000000000002,null,2,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 160KB Flash, 16KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"Yes"]
["MK20DX128VFT5","NXPMK20DX128VFT5","NXP","ARM CM4",50,160,2,16,16,null,0,null,29,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,48,"HVQFN48",2.37,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 160KB Flash, 16KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"Yes"]
["MK20DX128VLF5","NXPMK20DX128VLF5","NXP","ARM CM4",50,160,2,16,16,null,0,null,29,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,48,"LQFP48",2.3199999999999998,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 160KB Flash, 16KB SRAM, FullSpeed USB, 48LQFP",null,null,null,1,"Yes"]
["MK20DX128VLH5","NXPMK20DX128VLH5","NXP","ARM CM4",50,160,2,16,16,null,0,null,40,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,64,"LQFP64",2.44,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 160KB Flash, 16KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"Yes"]
["MK20DX128VLH7","NXPMK20DX128VLH7","NXP","ARM CM4",72,160,2,32,16,null,1,null,40,"No",2,1,1,"Yes",13,null,-40,105,1.71,3.6,64,"LQFP64",3.07,null,3,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"Yes"]
["MK20DX128VLK7","NXPMK20DX128VLK7","NXP","ARM CM4",72,160,2,32,16,null,1,null,52,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,80,"LQFP80",3.29,null,4,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"Yes"]
["MK20DX128VLL7","NXPMK20DX128VLL7","NXP","ARM CM4",72,160,2,32,16,null,1,null,66,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,100,"LQFP100",3.35,null,5,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"Yes"]
["MK20DX128VLQ10","NXPMK20DX128VLQ10","NXP","ARM CM4",100,256,4,32,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",4.1900000000000004,null,6,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 256KB Flash, 32KB SRAM, FullSpeed USB, 144LQFP",null,null,null,1,"Yes"]
["MK20DX128VMC7","NXPMK20DX128VMC7","NXP","ARM CM4",72,160,2,32,16,null,1,null,70,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",3.56,null,5,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"Yes"]
["MK20DX128VMP5","NXPMK20DX128VMP5","NXP","ARM CM4",50,160,2,16,16,null,0,null,40,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,64,"LFBGA64",2.76,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 160KB Flash, 16KB SRAM, FullSpeed USB, 64MAPBGA",null,null,null,1,"Yes"]
["MK20DX256VLH7","NXPMK20DX256VLH7","NXP","ARM CM4",72,288,2,64,16,null,1,null,40,"No",2,1,1,"Yes",13,null,-40,105,1.71,3.6,64,"LQFP64",3.52,null,3,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"Yes"]
["MK20DX256VLK10","NXPMK20DX256VLK10","NXP","ARM CM4",100,512,4,64,16,null,1,null,52,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",3.75,null,4,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"Yes"]
["MK20DX256VLK10R","NXPMK20DX256VLK10R","NXP","ARM CM4",100,512,4,64,16,null,1,null,52,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",3.75,null,4,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"Yes"]
["MK20DX256VLK7","NXPMK20DX256VLK7","NXP","ARM CM4",72,288,2,64,16,null,1,null,52,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,80,"LQFP80",3.74,null,4,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"Yes"]
["MK20DX256VLK7R","NXPMK20DX256VLK7R","NXP","ARM CM4",72,288,2,64,16,null,1,null,52,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,80,"LQFP80",3.74,null,4,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"Yes"]
["MK20DX256VLL10","NXPMK20DX256VLL10","NXP","ARM CM4",100,512,4,64,16,null,1,null,66,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",3.81,null,5,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"Yes"]
["MK20DX256VLL7","NXPMK20DX256VLL7","NXP","ARM CM4",72,288,2,64,16,null,1,null,66,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,100,"LQFP100",3.8,null,5,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"Yes"]
["MK20DX256VLQ10","NXPMK20DX256VLQ10","NXP","ARM CM4",100,512,4,64,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.0599999999999996,null,6,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 144LQFP",null,null,null,1,"Yes"]
["MK20DX256VLQ10R","NXPMK20DX256VLQ10R","NXP","ARM CM4",100,512,4,64,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.0599999999999996,null,6,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 144LQFP",null,null,null,1,"Yes"]
["MK20DX256VMC10","NXPMK20DX256VMC10","NXP","ARM CM4",100,512,4,64,16,null,2,null,86,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",4.87,null,6,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"Yes"]
["MK20DX256VMC7","NXPMK20DX256VMC7","NXP","ARM CM4",72,288,2,64,16,null,1,null,70,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",4.01,null,5,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"Yes"]
["MK20DX256VMC7R","NXPMK20DX256VMC7R","NXP","ARM CM4",72,288,2,64,16,null,1,null,70,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",4.01,null,5,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"Yes"]
["MK20DX256VMD10","NXPMK20DX256VMD10","NXP","ARM CM4",100,512,4,64,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",5.13,null,6,null,null,null,null,null,null,null,"Kinetis K20: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 144MAPBGA",null,null,null,1,"Yes"]
["MK20DX32VFM5","NXPMK20DX32VFM5","NXP","ARM CM4",50,64,2,8,16,null,0,null,20,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.78,null,2,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"Yes"]
["MK20DX32VFT5","NXPMK20DX32VFT5","NXP","ARM CM4",50,64,2,8,16,null,0,null,29,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,48,"HVQFN48",1.92,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"Yes"]
["MK20DX32VLF5","NXPMK20DX32VLF5","NXP","ARM CM4",50,64,2,8,16,null,0,null,29,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,48,"LQFP48",1.88,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 48LQFP",null,null,null,1,"Yes"]
["MK20DX32VLH5","NXPMK20DX32VLH5","NXP","ARM CM4",50,64,2,8,16,null,0,null,40,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,64,"LQFP64",1.98,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"Yes"]
["MK20DX32VMP5","NXPMK20DX32VMP5","NXP","ARM CM4",50,64,2,8,16,null,0,null,40,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,64,"LFBGA64",2.3199999999999998,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 64MAPBGA",null,null,null,1,"Yes"]
["MK20DX64VFM5","NXPMK20DX64VFM5","NXP","ARM CM4",50,96,2,16,16,null,0,null,20,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,32,"HVQFN32",1.95,null,2,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 96KB Flash, 16KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"Yes"]
["MK20DX64VFT5","NXPMK20DX64VFT5","NXP","ARM CM4",50,96,2,16,16,null,0,null,29,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,48,"HVQFN48",2.09,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 96KB Flash, 16KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"Yes"]
["MK20DX64VLF5","NXPMK20DX64VLF5","NXP","ARM CM4",50,96,2,16,16,null,0,null,29,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,48,"LQFP48",2.0499999999999998,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 96KB Flash, 16KB SRAM, FullSpeed USB, 48LQFP",null,null,null,1,"Yes"]
["MK20DX64VLH5","NXPMK20DX64VLH5","NXP","ARM CM4",50,96,2,16,16,null,0,null,40,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,64,"LQFP64",2.16,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 96KB Flash, 16KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"Yes"]
["MK20DX64VLH7","NXPMK20DX64VLH7","NXP","ARM CM4",72,96,2,16,16,null,1,null,40,"No",2,1,1,"Yes",13,null,-40,105,1.71,3.6,64,"LQFP64",2.61,null,3,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 96KB Flash, 16KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"Yes"]
["MK20DX64VLK7","NXPMK20DX64VLK7","NXP","ARM CM4",72,96,2,16,16,null,1,null,52,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,80,"LQFP80",2.84,null,4,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 96KB Flash, 16KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"Yes"]
["MK20DX64VMC7","NXPMK20DX64VMC7","NXP","ARM CM4",72,96,2,16,16,null,1,null,70,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",3.1,null,5,null,null,null,null,null,null,null,"Kinetis K20: 72MHz CortexM4 Performance MCU, 96KB Flash, 16KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"Yes"]
["MK20DX64VMP5","NXPMK20DX64VMP5","NXP","ARM CM4",50,96,2,16,16,null,0,null,40,"No",1,1,1,"Yes",11,null,-40,105,1.71,3.6,64,"LFBGA64",2.48,null,3,null,null,null,null,null,null,null,"Kinetis K20: 50MHz CortexM4 Performance MCU, 96KB Flash, 16KB SRAM, FullSpeed USB, 64MAPBGA",null,null,null,1,"Yes"]
["MK21DN512AVLK5","NXPMK21DN512AVLK5","NXP","ARM CM4",50,512,null,64,16,null,0,null,56,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",3.5,null,4,null,null,null,null,null,null,null,"Kinetis K21: 50MHz CortexM4 MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, Antitamper, 80LQFP",null,null,null,1,"No"]
["MK21DN512AVMC5","NXPMK21DN512AVMC5","NXP","ARM CM4",50,512,null,64,16,null,1,null,64,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",3.69,null,4,null,null,null,null,null,null,null,"Kinetis K21: 50MHz CortexM4 MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, Antitamper, 121MAPBGA",null,null,null,1,"No"]
["MK21DN512AVMC5R","NXPMK21DN512AVMC5R","NXP","ARM CM4",50,512,null,64,16,null,1,null,64,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",3.69,null,4,null,null,null,null,null,null,null,"Kinetis K21: 50MHz CortexM4 MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, Antitamper, 121MAPBGA",null,null,null,1,"No"]
["MK21DX128AVLK5","NXPMK21DX128AVLK5","NXP","ARM CM4",50,192,4,32,16,null,0,null,56,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",2.73,null,4,null,null,null,null,null,null,null,"Kinetis K21: 50MHz CortexM4 MCU, 192KB Flash, 32KB SRAM, FullSpeed USB, Antitamper, 80LQFP",null,null,null,1,"No"]
["MK21DX128AVMC5","NXPMK21DX128AVMC5","NXP","ARM CM4",50,192,4,32,16,null,1,null,64,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",2.93,null,4,null,null,null,null,null,null,null,"Kinetis K21: 50MHz CortexM4 MCU, 192KB Flash, 32KB SRAM, FullSpeed USB, Antitamper, 121MAPBGA",null,null,null,1,"No"]
["MK21DX256AVLK5","NXPMK21DX256AVLK5","NXP","ARM CM4",50,320,4,32,16,null,0,null,56,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",3.08,null,4,null,null,null,null,null,null,null,"Kinetis K21: 50MHz CortexM4 MCU, 320KB Flash, 32KB SRAM, FullSpeed USB, Antitamper, 80LQFP",null,null,null,1,"No"]
["MK21DX256AVMC5","NXPMK21DX256AVMC5","NXP","ARM CM4",50,320,4,32,16,null,1,null,64,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",3.27,null,4,null,null,null,null,null,null,null,"Kinetis K21: 50MHz CortexM4 MCU, 320KB Flash, 32KB SRAM, FullSpeed USB, Antitamper, 121MAPBGA",null,null,null,1,"No"]
["MK21DX256AVMC5R","NXPMK21DX256AVMC5R","NXP","ARM CM4",50,320,4,32,16,null,1,null,64,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",3.27,null,4,null,null,null,null,null,null,null,"Kinetis K21: 50MHz CortexM4 MCU, 320KB Flash, 32KB SRAM, FullSpeed USB, Antitamper, 121MAPBGA",null,null,null,1,"No"]
["MK21FN1M0AVLQ12","NXPMK21FN1M0AVLQ12","NXP","ARM CM4F",120,1024,null,128,16,null,2,null,100,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.26,null,6,null,null,null,null,null,null,null,"Kinetis K21: 120MHz CortexM4F MCU, 1MB Flash, 128KB SRAM, FullSpeed USB, Antitamper, 144LQFP",null,null,null,1,"No"]
["MK21FN1M0AVMC12","NXPMK21FN1M0AVMC12","NXP","ARM CM4F",120,1024,null,128,16,null,2,null,81,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",5.1100000000000003,null,5,null,null,null,null,null,null,null,"Kinetis K21: 120MHz CortexM4F MCU, 1MB Flash, 128KB SRAM, FullSpeed USB, Antitamper, 121MAPBGA",null,null,null,1,"No"]
["MK21FN1M0AVMC12R","NXPMK21FN1M0AVMC12R","NXP","ARM CM4F",120,1024,null,128,16,null,2,null,81,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",5.1100000000000003,null,5,null,null,null,null,null,null,null,"Kinetis K21: 120MHz CortexM4F MCU, 1MB Flash, 128KB SRAM, FullSpeed USB, Antitamper, 121MAPBGA",null,null,null,1,"No"]
["MK21FN1M0AVMD12","NXPMK21FN1M0AVMD12","NXP","ARM CM4F",120,1024,null,128,16,null,2,null,95,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",5.31,null,6,null,null,null,null,null,null,null,"Kinetis K21: 120MHz CortexM4F MCU, 1MB Flash, 128KB SRAM, FullSpeed USB, Antitamper, 144MAPBGA",null,null,null,1,"No"]
["MK21FX512AVLQ12","NXPMK21FX512AVLQ12","NXP","ARM CM4F",120,640,4,128,16,null,2,null,100,"No",3,3,1,"Yes",13,null,-40,105,1.71,3.6,144,"LQFP144",4.68,null,6,null,null,null,null,null,null,null,"Kinetis K21: 120MHz CortexM4F MCU, 512KB Flash +128KB FlexMem, 128KB RAM, USB, Antitamper, 144LQFP",null,null,null,1,"No"]
["MK21FX512AVMC12","NXPMK21FX512AVMC12","NXP","ARM CM4F",120,640,4,128,16,null,2,null,81,"No",3,3,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",4.53,null,5,null,null,null,null,null,null,null,"Kinetis K21: 120MHz CortexM4F MCU, 512KB Flash + 128KB FlexMem, 128KB RAM, USB, Antitamper, 121BGA",null,null,null,1,"No"]
["MK21FX512AVMD12","NXPMK21FX512AVMD12","NXP","ARM CM4F",120,640,4,128,16,null,2,null,95,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",4.7300000000000004,null,6,null,null,null,null,null,null,null,"Kinetis K21: 120MHz CortexM4F MCU, 512KB Flash + 128KB FlexMem, 128KB RAM, USB, Antitamper, 144BGA",null,null,null,1,"No"]
["MK22DN512VLH5","NXPMK22DN512VLH5","NXP","ARM CM4",50,512,null,64,16,null,1,null,40,"No",2,1,1,"Yes",1,null,-40,105,1.71,3.6,64,"LQFP64",3.06,null,3,null,null,null,null,null,null,null,"Kinetis K22: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MK22DN512VLK5","NXPMK22DN512VLK5","NXP","ARM CM4",50,512,null,64,16,null,1,null,56,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",3.24,null,4,null,null,null,null,null,null,null,"Kinetis K22: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"No"]
["MK22DN512VMC5","NXPMK22DN512VMC5","NXP","ARM CM4",50,512,null,64,16,null,1,null,56,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",3.44,null,4,null,null,null,null,null,null,null,"Kinetis K22: 50MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"No"]
["MK22DX128VLF5","NXPMK22DX128VLF5","NXP","ARM CM4",50,192,4,32,16,null,0,null,29,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,48,"LQFP48",2.19,null,3,null,null,null,null,null,null,null,"Kinetis K22: 50MHz CortexM4 Performance MCU, 192KB Flash, 32KB SRAM, FullSpeed USB, 48LQFP",null,null,null,1,"No"]
["MK22DX128VLH5","NXPMK22DX128VLH5","NXP","ARM CM4",50,192,4,32,16,null,1,null,40,"No",2,1,1,"Yes",13,null,-40,105,1.71,3.6,64,"LQFP64",2.2999999999999998,null,3,null,null,null,null,null,null,null,"Kinetis K22: 50MHz CortexM4 Performance MCU, 192KB Flash, 32KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MK22DX128VLK5","NXPMK22DX128VLK5","NXP","ARM CM4",50,192,4,32,16,null,1,null,56,"No",2,2,1,{"$f":"IF(OR(ISBLANK(AO622), AO622=0), \"No\", \"Yes\")","v":"Yes"},13,null,-40,105,1.71,3.6,80,"LQFP80",2.4900000000000002,null,4,null,null,null,null,null,null,null,"Kinetis K22: 50MHz CortexM4 Performance MCU, 192KB Flash, 32KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"No"]
["MK22DX128VMC5","NXPMK22DX128VMC5","NXP","ARM CM4",50,192,4,32,16,null,1,null,56,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",2.68,null,4,null,null,null,null,null,null,null,"Kinetis K22: 50MHz CortexM4 Performance MCU, 192KB Flash, 32KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"No"]
["MK22DX256VLF5","NXPMK22DX256VLF5","NXP","ARM CM4",50,320,4,32,16,null,0,null,29,"No",1,1,1,"Yes",1,null,-40,105,1.71,3.6,48,"LQFP48",2.54,null,3,null,null,null,null,null,null,null,"Kinetis K22: 50MHz CortexM4 Performance MCU, 320KB Flash, 32KB SRAM, FullSpeed USB, 48LQFP",null,null,null,1,"No"]
["MK22DX256VLH5","NXPMK22DX256VLH5","NXP","ARM CM4",50,320,4,32,16,null,1,null,40,"No",2,1,1,"Yes",13,null,-40,105,1.71,3.6,64,"LQFP64",2.64,null,3,null,null,null,null,null,null,null,"Kinetis K22: 50MHz CortexM4 Performance MCU, 320KB Flash, 32KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MK22DX256VLK5","NXPMK22DX256VLK5","NXP","ARM CM4",50,320,4,32,16,null,1,null,56,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,80,"LQFP80",2.83,null,4,null,null,null,null,null,null,null,"Kinetis K22: 50MHz CortexM4 Performance MCU, 320KB Flash, 32KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"No"]
["MK22DX256VMC5","NXPMK22DX256VMC5","NXP","ARM CM4",50,320,4,32,16,null,1,null,56,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",3.03,null,4,null,null,null,null,null,null,null,"Kinetis K22: 50MHz CortexM4 Performance MCU, 320KB Flash, 32KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"No"]
["MK22FN128CAH12R","NXPMK22FN128CAH12R","NXP","ARM CM0",120,128,null,null,16,null,0,null,40,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,64,"WLCSP64",3.69,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit MCU, ARM CM4 core, 128KB Flash, 120MHz, USB, WLCSP 64",null,null,null,1,"No"]
["MK22FN128VDC10","NXPMK22FN128VDC10","NXP","ARM CM4F",100,128,null,24,16,null,1,null,67,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"XFBGA121",1.94,null,4,null,null,null,null,null,null,null,"Kinetis K22: 100MHz CortexM4F Performance MCU, 128KB Flash, 24KB SRAM, FullSpeed USB, 121XFBGA",null,null,null,1,"No"]
["MK22FN128VLH10","NXPMK22FN128VLH10","NXP","ARM CM4F",100,128,null,24,16,null,1,null,40,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,64,"LQFP64",1.65,null,4,null,null,null,null,null,null,null,"Kinetis K22: 100MHz CortexM4F Performance MCU, 128KB Flash, 24KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MK22FN128VLH10R","NXPMK22FN128VLH10R","NXP","ARM CM4F",100,128,null,24,16,null,1,null,40,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,64,"LQFP64",1.65,null,4,null,null,null,null,null,null,null,"Kinetis K22: 100MHz CortexM4F Performance MCU, 128KB Flash, 24KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MK22FN128VLL10","NXPMK22FN128VLL10","NXP","ARM CM4F",100,128,null,24,16,null,1,null,66,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,100,"LQFP100",1.82,null,4,null,null,null,null,null,null,null,"Kinetis K22: 100MHz CortexM4F Performance MCU, 128KB Flash, 24KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"No"]
["MK22FN128VMP10","NXPMK22FN128VMP10","NXP","ARM CM4F",100,128,null,24,16,null,1,null,40,"No",2,2,1,"Yes",13,null,-40,105,1.71,3.6,64,"LFBGA64",1.87,null,4,null,null,null,null,null,null,null,"Kinetis K22: 100MHz CortexM4F Performance MCU, 128KB Flash, 24KB SRAM, FullSpeed USB, 64MAPBGA",null,null,null,1,"No"]
["MK22FN1M0AVLH12","NXPMK22FN1M0AVLH12","NXP","ARM CM4F",120,1024,null,128,16,null,1,null,40,"No",3,1,1,"Yes",1,null,-40,105,1.71,3.6,64,"LQFP64",4.47,null,3,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 1MB Flash, 128KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MK22FN1M0AVLK12","NXPMK22FN1M0AVLK12","NXP","ARM CM4F",120,1024,null,128,16,null,1,null,52,"No",3,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",4.66,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 1MB Flash, 128KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"No"]
["MK22FN1M0AVLK12R","NXPMK22FN1M0AVLK12R","NXP","ARM CM4F",120,1024,null,128,16,null,1,null,52,"No",3,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",4.66,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 1MB Flash, 128KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"No"]
["MK22FN1M0AVLL12","NXPMK22FN1M0AVLL12","NXP","ARM CM4F",120,1024,null,128,16,null,1,null,66,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",4.6900000000000004,null,5,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 1MB Flash, 128KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"No"]
["MK22FN1M0AVLQ12","NXPMK22FN1M0AVLQ12","NXP","ARM CM4F",120,1024,null,128,16,null,2,null,100,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.01,null,6,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 1MB Flash, 128KB SRAM, FullSpeed USB, 144LQFP",null,null,null,1,"No"]
["MK22FN1M0AVMC12","NXPMK22FN1M0AVMC12","NXP","ARM CM4F",120,1024,null,128,16,null,2,null,86,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",4.8499999999999996,null,6,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 1MB Flash, 128KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"No"]
["MK22FN1M0AVMD12","NXPMK22FN1M0AVMD12","NXP","ARM CM4F",120,1024,null,128,16,null,2,null,100,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",5.0599999999999996,null,6,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 1MB Flash, 128KB SRAM, FullSpeed USB, 144MAPBGA",null,null,null,1,"No"]
["MK22FN256CAH12R","NXPMK22FN256CAH12R","NXP","ARM CM0",120,128,null,null,16,null,0,null,40,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,64,"WLCSP64",3.15,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit MCU, ARM CM4 core, 256KB Flash, 120MHz, USB, WLCSP 64",null,null,null,1,"No"]
["MK22FN256CAP12R","NXPMK22FN256CAP12R","NXP","ARM CM0",120,256,null,null,16,null,0,null,52,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,80,"WLCSP80",4.34,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit, ARM CM4 core, 256KB Flash, 120MHz, USB, 80WLCSP",null,null,null,1,"No"]
["MK22FN256VDC12","NXPMK22FN256VDC12","NXP","ARM CM4F",120,256,null,48,16,null,1,null,70,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,121,"XFBGA121",3.06,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 256KB Flash, 48KB SRAM, FullSpeed USB, 121XFBGA",null,null,null,1,"No"]
["MK22FN256VLH12","NXPMK22FN256VLH12","NXP","ARM CM4F",120,256,null,48,16,null,1,null,40,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,64,"LQFP64",2.69,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 256KB Flash, 48KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MK22FN256VLL12","NXPMK22FN256VLL12","NXP","ARM CM4F",120,256,null,48,16,null,1,null,66,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",2.91,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 256KB Flash, 48KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"No"]
["MK22FN256VLL12R","NXPMK22FN256VLL12R","NXP","ARM CM4F",120,256,null,48,16,null,1,null,66,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",2.91,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 256KB Flash, 48KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"No"]
["MK22FN256VMP12","NXPMK22FN256VMP12","NXP","ARM CM4F",120,256,null,48,16,null,1,null,40,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,64,"LFBGA64",2.97,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 256KB Flash, 48KB SRAM, FullSpeed USB, 64MAPBGA",null,null,null,1,"No"]
["MK22FN512CAP12R","NXPMK22FN512CAP12R","NXP","ARM CM0",120,256,null,null,16,null,0,null,52,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,80,"WLCSP80",4.05,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit MCU, ARM CM4 core, 512KB Flash, 120MHz, USB, WLCSP 80",null,null,null,1,"No"]
["MK22FN512CBP12R","NXPMK22FN512CBP12R","NXP","ARM CM0",120,512,null,null,16,null,0,null,52,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,80,"WLCSP80",4.34,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit, ARM CM4 core, 512KB Flash, 120MHz, USB, Thin 80WLCSP",null,null,null,1,"No"]
["MK22FN512VDC12","NXPMK22FN512VDC12","NXP","ARM CM4F",120,512,null,128,16,null,2,null,81,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,121,"XFBGA121",3.19,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 121XFBGA",null,null,null,1,"No"]
["MK22FN512VDC12R","NXPMK22FN512VDC12R","NXP","ARM CM4F",120,512,null,128,16,null,2,null,81,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,121,"XFBGA121",3.19,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 121XFBGA",null,null,null,1,"No"]
["MK22FN512VFX12","NXPMK22FN512VFX12","NXP","ARM CM4F",120,512,null,128,16,null,1,null,60,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,88,"HVQFN88",2.98,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 88QFN",null,null,null,1,"No"]
["MK22FN512VFX12R","NXPMK22FN512VFX12R","NXP","ARM CM4F",120,512,null,128,16,null,1,null,60,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,88,"HVQFN88",2.98,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 88QFN",null,null,null,1,"No"]
["MK22FN512VLH12","NXPMK22FN512VLH12","NXP","ARM CM4F",120,512,null,128,16,null,1,null,40,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,64,"LQFP64",2.9,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MK22FN512VLH12R","NXPMK22FN512VLH12R","NXP","ARM CM4F",120,512,null,128,16,null,1,null,40,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,64,"LQFP64",2.9,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MK22FN512VLL12","NXPMK22FN512VLL12","NXP","ARM CM4F",120,512,null,128,16,null,1,null,66,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",3.06,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"No"]
["MK22FN512VLL12R","NXPMK22FN512VLL12R","NXP","ARM CM4F",120,512,null,128,16,null,1,null,66,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",3.06,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"No"]
["MK22FN512VMP12","NXPMK22FN512VMP12","NXP","ARM CM4F",120,512,null,128,16,null,1,null,40,"No",2,2,1,"Yes",1,null,-40,105,1.71,3.6,64,"LFBGA64",3.11,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 64MAPBGA",null,null,null,1,"No"]
["MK22FX512AVLH12","NXPMK22FX512AVLH12","NXP","ARM CM4F",120,640,4,128,16,null,1,null,40,"No",3,1,1,"Yes",1,null,-40,105,1.71,3.6,64,"LQFP64",3.9,null,3,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash + 128KB FlexMem, 128KB RAM, USB, 64LQFP",null,null,null,1,"No"]
["MK22FX512AVLH12R","NXPMK22FX512AVLH12R","NXP","ARM CM4F",120,640,4,128,16,null,1,null,40,"No",3,1,1,"Yes",1,null,-40,105,1.71,3.6,64,"LQFP64",3.9,null,3,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash + 128KB FlexMem, 128KB RAM, USB, 64LQFP",null,null,null,1,"No"]
["MK22FX512AVLK12","NXPMK22FX512AVLK12","NXP","ARM CM4F",120,640,4,128,16,null,1,null,52,"No",3,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",4.08,null,4,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash + 128KB FlexMem, 128KB RAM, USB, 80LQFP",null,null,null,1,"No"]
["MK22FX512AVLL12","NXPMK22FX512AVLL12","NXP","ARM CM4F",120,640,4,128,16,null,1,null,66,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",4.12,null,5,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash + 128KB FlexMem, 128KB RAM, USB, 100LQFP",null,null,null,1,"No"]
["MK22FX512AVLQ12","NXPMK22FX512AVLQ12","NXP","ARM CM4F",120,640,4,128,16,null,2,null,100,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",4.42,null,6,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash + 128KB FlexMem, 128KB RAM, USB, 144LQFP",null,null,null,1,"No"]
["MK22FX512AVMC12","NXPMK22FX512AVMC12","NXP","ARM CM4F",120,640,4,128,16,null,2,null,86,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",4.2699999999999996,null,6,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F Performance MCU, 512KB Flash + 128KB FlexMem, 128KB RAM, USB, 121BGA",null,null,null,1,"No"]
["MK22FX512AVMD12","NXPMK22FX512AVMD12","NXP","ARM CM4F",120,640,4,128,16,null,2,null,100,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",4.4800000000000004,null,6,null,null,null,null,null,null,null,"Kinetis K22: 120MHz CortexM4F MCU, 512KB Flash + 128KB FlexMem, 128KB RAM, USB, 144MAPBGA",null,null,null,1,"No"]
["MK24FN1M0CAJ12R","NXPMK24FN1M0CAJ12R","NXP","ARM CM0",120,1024,null,null,16,null,0,null,100,"No",3,null,null,"Yes",null,null,-40,85,1.71,3.6,142,"WLCSP142",6.65,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit MCU, ARM CM4 core, 1MB Flash, 120MHz, WLCSP 142",null,null,null,1,"No"]
["MK24FN1M0VDC12","NXPMK24FN1M0VDC12","NXP","ARM CM4F",120,1024,null,256,16,null,2,null,83,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"XFBGA121",5.31,null,6,null,null,null,null,null,null,null,"Kinetis K24: 120MHz CortexM4F Performance MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, 121XFBGA",null,null,null,1,"No"]
["MK24FN1M0VDC12R","NXPMK24FN1M0VDC12R","NXP","ARM CM4F",120,1024,null,256,16,null,2,null,83,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"XFBGA121",5.31,null,6,null,null,null,null,null,null,null,"Kinetis K24: 120MHz CortexM4F Performance MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, 121XFBGA",null,null,null,1,"No"]
["MK24FN1M0VLL12","NXPMK24FN1M0VLL12","NXP","ARM CM4F",120,1024,null,256,16,null,1,null,66,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",5.16,null,5,null,null,null,null,null,null,null,"Kinetis K24: 120MHz CortexM4F Performance MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"No"]
["MK24FN1M0VLL12R","NXPMK24FN1M0VLL12R","NXP","ARM CM4F",120,1024,null,256,16,null,1,null,66,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",5.16,null,5,null,null,null,null,null,null,null,"Kinetis K24: 120MHz CortexM4F Performance MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"No"]
["MK24FN1M0VLQ12","NXPMK24FN1M0VLQ12","NXP","ARM CM4F",120,1024,null,256,16,null,2,null,100,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.48,null,5,null,null,null,null,null,null,null,"Kinetis K24: 120MHz CortexM4F Performance MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, 144LQFP",null,null,null,1,"No"]
["MK24FN1M0VLQ12R","NXPMK24FN1M0VLQ12R","NXP","ARM CM4F",120,1024,null,256,16,null,2,null,100,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.48,null,5,null,null,null,null,null,null,null,"Kinetis K24: 120MHz CortexM4F Performance MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, 144LQFP",null,null,null,1,"No"]
["MK24FN256VDC12","NXPMK24FN256VDC12","NXP","ARM CM4F",120,256,null,256,16,null,1,null,83,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"XFBGA121",3.24,null,6,null,null,null,null,null,null,null,"Kinetis K24: 120MHz CortexM4F Performance MCU, 256KB Flash, 256KB SRAM, FullSpeed USB, 121XFBGA",null,null,null,1,"No"]
["MK40DN512VLK10","NXPMK40DN512VLK10","NXP","ARM CM4",100,512,null,128,16,null,1,null,52,"Yes",2,2,1,"Yes",1,null,-40,105,1.71,3.6,80,"LQFP80",5.2,null,4,null,null,null,null,null,null,null,"Kinetis K40: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Segment LCD, 80LQFP",null,null,null,1,"Yes"]
["MK40DN512VLL10","NXPMK40DN512VLL10","NXP","ARM CM4",100,512,null,128,16,null,1,null,64,"Yes",2,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",5.26,null,5,null,null,null,null,null,null,null,"Kinetis K40: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Segment LCD, 100LQFP",null,null,null,1,"Yes"]
["MK40DN512VLQ10","NXPMK40DN512VLQ10","NXP","ARM CM4",100,512,null,128,16,null,2,null,98,"Yes",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.65,null,6,null,null,null,null,null,null,null,"Kinetis K40: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Segment LCD, 144LQFP",null,null,null,1,"Yes"]
["MK40DN512VMD10","NXPMK40DN512VMD10","NXP","ARM CM4",100,512,null,128,16,null,2,null,98,"Yes",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",5.73,null,6,null,null,null,null,null,null,null,"Kinetis K40: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Segment LCD, 144MAPBGA",null,null,null,1,"Yes"]
["MK40DX128VLH7","NXPMK40DX128VLH7","NXP","ARM CM4",72,160,2,32,16,null,1,null,36,"Yes",2,1,1,"Yes",13,null,-40,105,1.71,3.6,64,"LQFP64",3.45,null,3,null,null,null,null,null,null,null,"Kinetis K40: 72MHz CortexM4 MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, Segment LCD, 64LQFP",null,null,null,1,"Yes"]
["MK40DX128VLK7","NXPMK40DX128VLK7","NXP","ARM CM4",72,160,2,32,16,null,1,null,52,"Yes",2,2,1,"Yes",13,null,-40,105,1.71,3.6,80,"LQFP80",3.67,null,4,null,null,null,null,null,null,null,"Kinetis K40: 72MHz CortexM4 MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, Segment LCD, 80LQFP",null,null,null,1,"Yes"]
["MK40DX128VLL7","NXPMK40DX128VLL7","NXP","ARM CM4",72,160,2,32,16,null,1,null,64,"Yes",2,2,1,"Yes",13,null,-40,105,1.71,3.6,100,"LQFP100",3.73,null,5,null,null,null,null,null,null,null,"Kinetis K40: 72MHz CortexM4 MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, Segment LCD, 100LQFP",null,null,null,1,"Yes"]
["MK40DX128VMC7","NXPMK40DX128VMC7","NXP","ARM CM4",72,160,2,32,16,null,1,null,68,"Yes",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",3.94,null,5,null,null,null,null,null,null,null,"Kinetis K40: 72MHz CortexM4 MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, Segment LCD, 121MAPBGA",null,null,null,1,"Yes"]
["MK40DX128VMD10","NXPMK40DX128VMD10","NXP","ARM CM4",100,256,4,32,16,null,2,null,98,"Yes",2,3,1,"Yes",13,null,-40,105,1.71,3.6,144,"LBGA144",4.6399999999999997,null,6,null,null,null,null,null,null,null,"Kinetis K40: 100MHz CortexM4 MCU, 256KB Flash, 32KB SRAM, FullSpeed USB, Segment LCD, 144MAPBGA",null,null,null,1,"Yes"]
["MK40DX256VLH7","NXPMK40DX256VLH7","NXP","ARM CM4",72,288,2,64,16,null,1,null,36,"Yes",2,1,1,"Yes",13,null,-40,105,1.71,3.6,64,"LQFP64",3.9,null,3,null,null,null,null,null,null,null,"Kinetis K40: 72MHz CortexM4 MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, Segment LCD, 64LQFP",null,null,null,1,"Yes"]
["MK40DX256VLK7","NXPMK40DX256VLK7","NXP","ARM CM4",72,288,2,64,16,null,1,null,52,"Yes",2,2,1,"Yes",13,null,-40,105,1.71,3.6,80,"LQFP80",4.1399999999999997,null,4,null,null,null,null,null,null,null,"Kinetis K40: 72MHz CortexM4 MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, Segment LCD, 80LQFP",null,null,null,1,"Yes"]
["MK40DX256VLL7","NXPMK40DX256VLL7","NXP","ARM CM4",72,288,2,64,16,null,1,null,64,"Yes",2,2,1,"Yes",13,null,-40,105,1.71,3.6,100,"LQFP100",4.1900000000000004,null,5,null,null,null,null,null,null,null,"Kinetis K40: 72MHz CortexM4 MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, Segment LCD, 100LQFP",null,null,null,1,"Yes"]
["MK40DX256VLQ10","NXPMK40DX256VLQ10","NXP","ARM CM4",100,512,4,64,16,null,2,null,98,"Yes",2,3,1,{"$f":"IF(OR(ISBLANK(AO686), AO686=0), \"No\", \"Yes\")","v":"Yes"},13,null,-40,105,1.71,3.6,144,"LQFP144",5.47,null,6,null,null,null,null,null,null,null,"Kinetis K40: 100MHz CortexM4 MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, Segment LCD, 144LQFP",null,null,null,1,"Yes"]
["MK40DX256VMC7","NXPMK40DX256VMC7","NXP","ARM CM4",72,288,2,64,16,null,1,null,68,"Yes",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",4.3899999999999997,null,5,null,null,null,null,null,null,null,"Kinetis K40: 72MHz CortexM4 MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, Segment LCD, 121MAPBGA",null,null,null,1,"Yes"]
["MK40DX256VMD10","NXPMK40DX256VMD10","NXP","ARM CM4",100,512,4,64,16,null,2,null,98,"Yes",2,3,1,"Yes",13,null,-40,105,1.71,3.6,144,"LBGA144",5.53,null,6,null,null,null,null,null,null,null,"Kinetis K40: 100MHz CortexM4 MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, Segment LCD, 144MAPBGA",null,null,null,1,"Yes"]
["MK40DX64VLH7","NXPMK40DX64VLH7","NXP","ARM CM4",72,96,2,16,16,null,1,null,36,"Yes",2,1,1,"Yes",11,null,-40,105,1.71,3.6,64,"LQFP64",3,null,3,null,null,null,null,null,null,null,"Kinetis K40: 72MHz CortexM4 MCU, 96KB Flash, 16KB SRAM, FullSpeed USB, Segment LCD, 64LQFP",null,null,null,1,"Yes"]
["MK40DX64VLK7","NXPMK40DX64VLK7","NXP","ARM CM4",72,96,2,16,16,null,1,null,52,"Yes",2,2,1,"Yes",13,null,-40,105,1.71,3.6,80,"LQFP80",3.22,null,4,null,null,null,null,null,null,null,"Kinetis K40: 72MHz CortexM4 MCU, 96KB Flash, 16KB SRAM, FullSpeed USB, Segment LCD, 80LQFP",null,null,null,1,"Yes"]
["MK40DX64VMC7","NXPMK40DX64VMC7","NXP","ARM CM4",72,96,2,16,16,null,1,null,68,"Yes",2,2,1,"Yes",13,null,-40,105,1.71,3.6,121,"LFBGA121",3.48,null,5,null,null,null,null,null,null,null,"Kinetis K40: 72MHz CortexM4 MCU, 96KB Flash, 16KB SRAM, FullSpeed USB, Segment LCD, 121MAPBGA",null,null,null,1,"Yes"]
["MK50DN512CLL10","NXPMK50DN512CLL10","NXP","ARM CM4",100,512,null,128,16,null,2,null,59,"No",2,3,1,"Yes",1,null,-40,85,1.71,3.6,100,"LQFP100",5.15,null,5,null,null,null,null,null,null,null,"Kinetis K50: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"Yes"]
["MK50DN512CLQ10","NXPMK50DN512CLQ10","NXP","ARM CM4",100,512,null,128,16,null,2,null,96,"No",2,3,1,"Yes",1,null,-40,85,1.71,3.6,144,"LQFP144",5.57,null,6,null,null,null,null,null,null,null,"Kinetis K50: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 144LQFP",null,null,null,1,"Yes"]
["MK50DN512CMC10","NXPMK50DN512CMC10","NXP","ARM CM4",100,512,null,128,16,null,2,null,78,"No",2,3,1,"Yes",1,null,-40,85,1.71,3.6,121,"LFBGA121",5.37,null,6,null,null,null,null,null,null,null,"Kinetis K50: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"Yes"]
["MK50DN512CMD10","NXPMK50DN512CMD10","NXP","ARM CM4",100,512,null,128,16,null,2,null,96,"No",2,3,1,"Yes",1,null,-40,85,1.71,3.6,144,"LBGA144",5.63,null,6,null,null,null,null,null,null,null,"Kinetis K50: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 144MAPBGA",null,null,null,1,"Yes"]
["MK50DN512CMD10R","NXPMK50DN512CMD10R","NXP","ARM CM4",100,512,null,128,16,null,2,null,96,"No",2,3,1,"Yes",1,null,-40,85,1.71,3.6,144,"LBGA144",5.63,null,6,null,null,null,null,null,null,null,"Kinetis K50: 100MHz CortexM4 Performance MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, 144MAPBGA",null,null,null,1,"Yes"]
["MK50DX128CLH7","NXPMK50DX128CLH7","NXP","ARM CM4",72,160,2,32,16,null,1,null,35,"No",2,1,1,"Yes",1,null,-40,85,1.71,3.6,64,"LQFP64",3.65,null,3,null,null,null,null,null,null,null,"Kinetis K50: 72MHz CortexM4 Performance MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"Yes"]
["MK50DX128CLH7R","NXPMK50DX128CLH7R","NXP","ARM CM4",72,160,2,32,16,null,1,null,35,"No",2,1,1,"Yes",1,null,-40,85,1.71,3.6,64,"LQFP64",3.65,null,3,null,null,null,null,null,null,null,"Kinetis K50: 72MHz CortexM4 Performance MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"Yes"]
["MK50DX128CLK7","NXPMK50DX128CLK7","NXP","ARM CM4",72,160,2,32,16,null,1,null,39,"No",2,2,1,"Yes",1,null,-40,85,1.71,3.6,80,"LQFP80",3.89,null,4,null,null,null,null,null,null,null,"Kinetis K50: 72MHz CortexM4 Performance MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"Yes"]
["MK50DX128CMC7","NXPMK50DX128CMC7","NXP","ARM CM4",72,160,2,32,16,null,1,null,63,"No",2,2,1,"Yes",1,null,-40,85,1.71,3.6,121,"LFBGA121",4.1399999999999997,null,5,null,null,null,null,null,null,null,"Kinetis K50: 72MHz CortexM4 Performance MCU, 160KB Flash, 32KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"Yes"]
["MK50DX256CLK10","NXPMK50DX256CLK10","NXP","ARM CM4",100,512,4,64,16,null,2,null,39,"No",2,2,1,"Yes",1,null,-40,85,1.71,3.6,80,"LQFP80",4.91,null,4,null,null,null,null,null,null,null,"Kinetis K50: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"Yes"]
["MK50DX256CLK7","NXPMK50DX256CLK7","NXP","ARM CM4",72,288,2,64,16,null,1,null,39,"No",2,2,1,"Yes",1,null,-40,85,1.71,3.6,80,"LQFP80",4.3499999999999996,null,4,null,null,null,null,null,null,null,"Kinetis K50: 72MHz CortexM4 Performance MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"Yes"]
["MK50DX256CLL10","NXPMK50DX256CLL10","NXP","ARM CM4",100,512,4,64,16,null,2,null,59,"No",2,3,1,"Yes",1,null,-40,85,1.71,3.6,100,"LQFP100",4.95,null,5,null,null,null,null,null,null,null,"Kinetis K50: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"Yes"]
["MK50DX256CLL7","NXPMK50DX256CLL7","NXP","ARM CM4",72,288,2,64,16,null,1,null,59,"No",2,2,1,"Yes",1,null,-40,85,1.71,3.6,100,"LQFP100",4.3899999999999997,null,5,null,null,null,null,null,null,null,"Kinetis K50: 72MHz CortexM4 Performance MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"Yes"]
["MK50DX256CMC10","NXPMK50DX256CMC10","NXP","ARM CM4",100,512,4,64,16,null,2,null,78,"No",2,3,1,"Yes",1,null,-40,85,1.71,3.6,121,"LFBGA121",5.16,null,6,null,null,null,null,null,null,null,"Kinetis K50: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"Yes"]
["MK50DX256CMC7","NXPMK50DX256CMC7","NXP","ARM CM4",72,288,2,64,16,null,1,null,63,"No",2,2,1,"Yes",1,null,-40,85,1.71,3.6,121,"LFBGA121",4.5999999999999996,null,5,null,null,null,null,null,null,null,"Kinetis K50: 72MHz CortexM4 Performance MCU, 288KB Flash, 64KB SRAM, FullSpeed USB, 121MAPBGA",null,null,null,1,"Yes"]
["MK50DX256CMD10","NXPMK50DX256CMD10","NXP","ARM CM4",100,512,4,64,16,null,2,null,96,"No",2,3,1,"Yes",1,null,-40,85,1.71,3.6,144,"LBGA144",5.43,null,6,null,null,null,null,null,null,null,"Kinetis K50: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, 144MAPBGA",null,null,null,1,"Yes"]
["MK51DN256CMD10","NXPMK51DN256CMD10","NXP","ARM CM4",100,256,null,64,16,null,2,null,94,"Yes",2,3,1,"Yes",1,null,-40,85,1.71,3.6,144,"LBGA144",5.08,null,6,null,null,null,null,null,null,null,"Kinetis K51: 100MHz CortexM4 Measurement MCU, 256KB Flash, 64KB SRAM, USB, Segment LCD, 144MAPBGA",null,null,null,1,"Yes"]
["MK51DN512CLL10","NXPMK51DN512CLL10","NXP","ARM CM4",100,512,null,128,16,null,2,null,57,"Yes",2,3,1,"Yes",1,null,-40,85,1.71,3.6,100,"LQFP100",5.56,null,4,null,null,null,null,null,null,null,"Kinetis K51: 100MHz CortexM4 Measurement MCU, 512KB Flash, 128KB SRAM, USB, Segment LCD, 100LQFP",null,null,null,1,"Yes"]
["MK51DN512CLQ10","NXPMK51DN512CLQ10","NXP","ARM CM4",100,512,null,128,16,null,2,null,94,"Yes",2,3,1,"Yes",1,null,-40,85,1.71,3.6,144,"LQFP144",5.96,null,6,null,null,null,null,null,null,null,"Kinetis K51: 100MHz CortexM4 Measurement MCU, 512KB Flash, 128KB SRAM, USB, Segment LCD, 144LQFP",null,null,null,1,"Yes"]
["MK51DN512CMC10","NXPMK51DN512CMC10","NXP","ARM CM4",100,512,null,128,16,null,2,null,78,"Yes",2,3,1,"Yes",1,null,-40,85,1.71,3.6,121,"LFBGA121",5.77,null,6,null,null,null,null,null,null,null,"Kinetis K51: 100MHz CortexM4 Measurement MCU, 512KB Flash, 128KB SRAM, USB, Segment LCD, 121MAPBGA",null,null,null,1,"Yes"]
["MK51DN512CMD10","NXPMK51DN512CMD10","NXP","ARM CM4",100,512,null,128,16,null,2,null,94,"Yes",2,3,1,"Yes",1,null,-40,85,1.71,3.6,144,"LBGA144",6.03,null,6,null,null,null,null,null,null,null,"Kinetis K51: 100MHz CortexM4 Measurement MCU, 512KB Flash, 128KB SRAM, USB, Segment LCD, 144MAPBGA",null,null,null,1,"Yes"]
["MK51DX128CLH7","NXPMK51DX128CLH7","NXP","ARM CM4",72,160,2,32,16,null,2,null,31,"Yes",1,1,1,"Yes",13,null,-40,85,1.71,3.6,64,"LQFP64",4.03,null,3,null,null,null,null,null,null,null,"Kinetis K51: 72MHz CortexM4 Measurement MCU, 160KB Flash, 32KB SRAM, USB, Segment LCD, 64LQFP",null,null,null,1,"Yes"]
["MK51DX128CLK7","NXPMK51DX128CLK7","NXP","ARM CM4",72,160,2,32,16,null,1,null,39,"Yes",2,2,1,"Yes",1,null,-40,85,1.71,3.6,80,"LQFP80",4.26,null,4,null,null,null,null,null,null,null,"Kinetis K51: 72MHz CortexM4 Measurement MCU, 160KB Flash, 32KB SRAM, USB, Segment LCD, 80LQFP",null,null,null,1,"Yes"]
["MK51DX128CMC7","NXPMK51DX128CMC7","NXP","ARM CM4",72,160,2,32,16,null,1,null,61,"Yes",2,2,1,"Yes",1,null,-40,85,1.71,3.6,121,"LFBGA121",4.5199999999999996,null,5,null,null,null,null,null,null,null,"Kinetis K51: 72MHz CortexM4 Measurement MCU, 160KB Flash, 32KB SRAM, USB, Segment LCD, 121MAPBGA",null,null,null,1,"Yes"]
["MK51DX256CLK10","NXPMK51DX256CLK10","NXP","ARM CM4",100,512,4,64,16,null,2,null,39,"Yes",2,2,1,"Yes",13,null,-40,85,1.71,3.6,80,"LQFP80",5.32,null,4,null,null,null,null,null,null,null,"Kinetis K51: 100MHz CortexM4 Measurement MCU, 512KB Flash, 64KB SRAM, USB, Segment LCD, 80LQFP",null,null,null,1,"Yes"]
["MK51DX256CLK7","NXPMK51DX256CLK7","NXP","ARM CM4",72,288,2,64,16,null,1,null,39,"Yes",2,2,1,"Yes",1,null,-40,85,1.71,3.6,80,"LQFP80",4.72,null,4,null,null,null,null,null,null,null,"Kinetis K51: 72MHz CortexM4 Measurement MCU, 288KB Flash, 64KB SRAM, USB, Segment LCD, 80LQFP",null,null,null,1,"Yes"]
["MK51DX256CLL10","NXPMK51DX256CLL10","NXP","ARM CM4",100,512,4,64,16,null,2,null,57,"Yes",2,3,1,"Yes",13,null,-40,85,1.71,3.6,100,"LQFP100",5.36,null,4,null,null,null,null,null,null,null,"Kinetis K51: 100MHz CortexM4 Measurement MCU, 512KB Flash, 64KB SRAM, USB, Segment LCD, 100LQFP",null,null,null,1,"Yes"]
["MK51DX256CLL7","NXPMK51DX256CLL7","NXP","ARM CM4",72,288,2,64,16,null,1,null,57,"Yes",2,2,1,"Yes",1,null,-40,85,1.71,3.6,100,"LQFP100",4.79,null,4,null,null,null,null,null,null,null,"Kinetis K51: 72MHz CortexM4 Measurement MCU, 288KB Flash, 64KB SRAM, USB, Segment LCD, 100LQFP",null,null,null,1,"Yes"]
["MK51DX256CMC10","NXPMK51DX256CMC10","NXP","ARM CM4",100,512,4,64,16,null,2,null,78,"Yes",2,3,1,"Yes",13,null,-40,85,1.71,3.6,121,"LFBGA121",5.57,null,6,null,null,null,null,null,null,null,"Kinetis K51: 100MHz CortexM4 Measurement MCU, 512KB Flash, 64KB SRAM, USB, Segment LCD, 121MAPBGA",null,null,null,1,"Yes"]
["MK51DX256CMC7","NXPMK51DX256CMC7","NXP","ARM CM4",72,288,2,64,16,null,1,null,61,"Yes",2,2,1,"Yes",1,null,-40,85,1.71,3.6,121,"LFBGA121",4.9800000000000004,null,5,null,null,null,null,null,null,null,"Kinetis K51: 72MHz CortexM4 Measurement MCU, 288KB Flash, 64KB SRAM, USB, Segment LCD, 121MAPBGA",null,null,null,1,"Yes"]
["MK52DN512CLQ10","NXPMK52DN512CLQ10","NXP","ARM CM4",100,512,null,128,16,null,2,null,96,"No",2,3,1,"Yes",1,null,-40,85,1.71,3.6,144,"LQFP144",5.96,null,6,null,null,null,null,null,null,null,"Kinetis K52: 100MHz CortexM4 Measurement MCU, 512KB Flash, 128KB SRAM, USB, Ethernet, 144LQFP",null,null,null,1,"Yes"]
["MK52DN512CMD10","NXPMK52DN512CMD10","NXP","ARM CM4",100,512,null,128,16,null,2,null,96,"No",2,3,1,"Yes",1,null,-40,85,1.71,3.6,144,"LBGA144",6.03,null,6,null,null,null,null,null,null,null,"Kinetis K52: 100MHz CortexM4 Measurement MCU, 512KB Flash, 128KB SRAM, USB, Ethernet, 144MAPBGA",null,null,null,1,"Yes"]
["MK53DN512CLQ10","NXPMK53DN512CLQ10","NXP","ARM CM4",100,512,null,128,16,null,2,null,94,"Yes",2,3,1,"Yes",1,null,-40,85,1.71,3.6,144,"LQFP144",6.36,null,6,null,null,null,null,null,null,null,"Kinetis K53: 100MHz CortexM4 Measurement MCU, 512KB Flash, 128K RAM, USB, ETH, Segment LCD, 144LQFP",null,null,null,1,"Yes"]
["MK53DN512CMD10","NXPMK53DN512CMD10","NXP","ARM CM4",100,512,null,128,16,null,2,null,94,"Yes",2,3,1,"Yes",1,null,-40,85,1.71,3.6,144,"LBGA144",6.42,null,6,null,null,null,null,null,null,null,"Kinetis K53: 100MHz CortexM4 Measurement MCU, 512KB Flash, 128K RAM, USB, ETH, Segment LCD, 144BGA",null,null,null,1,"Yes"]
["MK53DX256CLQ10","NXPMK53DX256CLQ10","NXP","ARM CM4",100,512,4,64,16,null,2,null,94,"Yes",2,3,1,"Yes",13,null,-40,85,1.71,3.6,144,"LQFP144",6.17,null,6,null,null,null,null,null,null,null,"Kinetis K53: 100MHz CortexM4 Measurement MCU, 512KB Flash, 64K RAM, USB, ETH, Segment LCD, 144LQFP",null,null,null,1,"Yes"]
["MK53DX256CMD10","NXPMK53DX256CMD10","NXP","ARM CM4",100,512,4,64,16,null,2,null,94,"Yes",2,3,1,"Yes",13,null,-40,85,1.71,3.6,144,"LBGA144",6.22,null,6,null,null,null,null,null,null,null,"Kinetis K53: 100MHz CortexM4 Measurement MCU, 512KB Flash, 64K RAM, USB, ETH, Segment LCD, 144BGA",null,null,null,1,"Yes"]
["MK60DN256VLL10","NXPMK60DN256VLL10","NXP","ARM CM4",100,256,null,64,16,null,1,null,66,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",4.3,null,5,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 256KB Flash, 64KB SRAM, FullSpeed USB, Ethernet, 100LQFP",null,null,null,1,"Yes"]
["MK60DN256VLL10R","NXPMK60DN256VLL10R","NXP","ARM CM4",100,256,null,64,16,null,1,null,66,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",4.3,null,5,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 256KB Flash, 64KB SRAM, FullSpeed USB, Ethernet, 100LQFP",null,null,null,1,"Yes"]
["MK60DN256VLQ10","NXPMK60DN256VLQ10","NXP","ARM CM4",100,256,null,64,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",4.71,null,6,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 256KB Flash, 64KB SRAM, FullSpeed USB, Ethernet, 144LQFP",null,null,null,1,"Yes"]
["MK60DN256VMC10","NXPMK60DN256VMC10","NXP","ARM CM4",100,256,null,64,16,null,2,null,86,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",4.5199999999999996,null,6,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 256KB Flash, 64KB SRAM, FullSpeed USB, Ethernet, 121MAPBGA",null,null,null,1,"Yes"]
["MK60DN256VMD10","NXPMK60DN256VMD10","NXP","ARM CM4",100,256,null,64,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",4.79,null,6,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 256KB Flash, 64KB SRAM, FullSpeed USB, Ethernet, 144MAPBGA",null,null,null,1,"Yes"]
["MK60DN512VLL10","NXPMK60DN512VLL10","NXP","ARM CM4",100,512,null,128,16,null,1,null,66,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",5.26,null,5,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Ethernet, 100LQFP",null,null,null,1,"Yes"]
["MK60DN512VLL10R","NXPMK60DN512VLL10R","NXP","ARM CM4",100,512,null,128,16,null,1,null,66,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",5.26,null,5,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Ethernet, 100LQFP",null,null,null,1,"Yes"]
["MK60DN512VLQ10","NXPMK60DN512VLQ10","NXP","ARM CM4",100,512,null,128,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.65,null,6,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Ethernet, 144LQFP",null,null,null,1,"Yes"]
["MK60DN512VMC10","NXPMK60DN512VMC10","NXP","ARM CM4",100,512,null,128,16,null,2,null,86,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",5.47,null,6,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Ethernet, 121MAPBGA",null,null,null,1,"Yes"]
["MK60DN512VMC10R","NXPMK60DN512VMC10R","NXP","ARM CM4",100,512,null,128,16,null,2,null,86,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",5.47,null,6,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Ethernet, 121MAPBGA",null,null,null,1,"Yes"]
["MK60DN512VMD10","NXPMK60DN512VMD10","NXP","ARM CM4",100,512,null,128,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",5.73,null,6,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Ethernet, 144MAPBGA",null,null,null,1,"Yes"]
["MK60DN512ZCAB10R","NXPMK60DN512ZCAB10R","NXP","ARM CM0",100,512,null,null,16,null,0,null,79,"No",2,null,null,"Yes",null,null,-40,85,1.71,3.6,120,"WLCSP120",6.11,null,null,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 128KB SRAM, FullSpeed USB, Ethernet, 120WLCSP,",null,null,null,1,"Yes"]
["MK60DX256VLL10","NXPMK60DX256VLL10","NXP","ARM CM4",100,512,4,64,16,null,1,null,66,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",5.05,null,5,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, Ethernet, 100LQFP",null,null,null,1,"Yes"]
["MK60DX256VLQ10","NXPMK60DX256VLQ10","NXP","ARM CM4",100,512,4,64,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.47,null,6,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, Ethernet, 144LQFP",null,null,null,1,"Yes"]
["MK60DX256VMC10","NXPMK60DX256VMC10","NXP","ARM CM4",100,512,4,64,16,null,2,null,86,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"LFBGA121",5.27,null,6,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, Ethernet, 121MAPBGA",null,null,null,1,"Yes"]
["MK60DX256VMD10","NXPMK60DX256VMD10","NXP","ARM CM4",100,512,4,64,16,null,2,null,100,"No",2,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",5.53,null,6,null,null,null,null,null,null,null,"Kinetis K60: 100MHz CortexM4 MCU, 512KB Flash, 64KB SRAM, FullSpeed USB, Ethernet, 144MAPBGA",null,null,null,1,"Yes"]
["MK63FN1M0VLQ12","NXPMK63FN1M0VLQ12","NXP","ARM CM4F",120,1024,null,256,16,null,2,null,100,"No",3,3,1,"Yes",21,null,-40,105,1.71,3.6,144,"LQFP144",6.05,null,6,null,null,null,null,null,null,null,"Kinetis K63: 120MHz CortexM4F MCU, 1MB Flash, 256KB SRAM, USB, Ethernet, Antitamper, 144LQFP",null,null,null,1,"No"]
["MK63FN1M0VLQ12R","NXPMK63FN1M0VLQ12R","NXP","ARM CM4F",120,1024,null,256,16,null,2,null,100,"No",3,3,1,"Yes",21,null,-40,105,1.71,3.6,144,"LQFP144",6.05,null,6,null,null,null,null,null,null,null,"Kinetis K63: 120MHz CortexM4F MCU, 1MB Flash, 256KB SRAM, USB, Ethernet, Antitamper, 144LQFP",null,null,null,1,"No"]
["MK63FN1M0VMD12","NXPMK63FN1M0VMD12","NXP","ARM CM4F",120,1024,null,256,16,null,2,null,95,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",6.09,null,6,null,null,null,null,null,null,null,"Kinetis K63: 120MHz CortexM4F MCU, 1MB Flash, 256KB SRAM, USB, Ethernet, Antitamper, 144MAPBGA",null,null,null,1,"No"]
["MK64FN1M0CAJ12R","NXPMK64FN1M0CAJ12R","NXP","ARM CM0",120,1024,null,null,16,null,0,null,100,"No",3,null,null,"Yes",null,null,-40,85,1.71,3.6,142,"WLCSP142",6.97,null,null,null,null,null,null,null,null,null,"Kinetis K64: 120MHz CortexM4F MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, Ethernet, 142WLCSP,",null,null,null,1,"No"]
["MK64FN1M0VDC12","NXPMK64FN1M0VDC12","NXP","ARM CM4F",120,1024,null,256,16,null,2,null,83,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"XFBGA121",5.64,null,6,null,null,null,null,null,null,null,"Kinetis K64: 120MHz CortexM4F MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, Ethernet, 121XFBGA",null,null,null,1,"No"]
["MK64FN1M0VLL12","NXPMK64FN1M0VLL12","NXP","ARM CM4F",120,1024,null,256,16,null,1,null,66,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",5.48,null,5,null,null,null,null,null,null,null,"Kinetis K64: 120MHz CortexM4F MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, Ethernet, 100LQFP",null,null,null,1,"No"]
["MK64FN1M0VLL12R","NXPMK64FN1M0VLL12R","NXP","ARM CM4F",120,1024,null,256,16,null,1,null,66,"No",3,3,1,{"$f":"IF(OR(ISBLANK(AO750), AO750=0), \"No\", \"Yes\")","v":"Yes"},1,null,-40,105,1.71,3.6,100,"LQFP100",5.48,null,5,null,null,null,null,null,null,null,"Kinetis K64: 120MHz CortexM4F MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, Ethernet, 100LQFP",null,null,null,1,"No"]
["MK64FN1M0VLQ12","NXPMK64FN1M0VLQ12","NXP","ARM CM4F",120,1024,null,256,16,null,2,null,100,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.78,null,6,null,null,null,null,null,null,null,"Kinetis K64: 120MHz CortexM4F MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, Ethernet, 144LQFP",null,null,null,1,"No"]
["MK64FN1M0VMD12","NXPMK64FN1M0VMD12","NXP","ARM CM4F",120,1024,null,256,16,null,2,null,100,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",5.83,null,6,null,null,null,null,null,null,null,"Kinetis K64: 120MHz CortexM4F MCU, 1MB Flash, 256KB SRAM, FullSpeed USB, Ethernet, 144MAPBGA",null,null,null,1,"No"]
["MK64FX512VDC12","NXPMK64FX512VDC12","NXP","ARM CM4F",120,640,4,256,16,null,2,null,86,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"XFBGA121",4.95,null,6,null,null,null,null,null,null,null,"Kinetis K64: 120MHz CortexM4F MCU, 512KB Flash + 128KB FlexMem, 256KB RAM, USB, Ethernet, 121XFBGA",null,null,null,1,"No"]
["MK64FX512VLL12","NXPMK64FX512VLL12","NXP","ARM CM4F",120,640,4,256,16,null,1,null,66,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",4.79,null,5,null,null,null,null,null,null,null,"Kinetis K64: 120MHz CortexM4F MCU, 512KB Flash + 128KB FlexMem, 256KB RAM, USB, Ethernet, 100LQFP",null,null,null,1,"No"]
["MK64FX512VLQ12","NXPMK64FX512VLQ12","NXP","ARM CM4F",120,640,4,256,16,null,2,null,100,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",5.0999999999999996,null,6,null,null,null,null,null,null,null,"Kinetis K64: 120MHz CortexM4F MCU, 512KB Flash + 128KB FlexMem, 256KB RAM, USB, Ethernet, 144LQFP",null,null,null,1,"No"]
["MK64FX512VMD12","NXPMK64FX512VMD12","NXP","ARM CM4F",120,640,4,256,16,null,2,null,100,"No",3,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",5.16,null,6,null,null,null,null,null,null,null,"Kinetis K64: 120MHz CortexM4F MCU, 512KB Flash + 128KB FlexMem, 256KB RAM, USB, Ethernet, 144MAPBGA",null,null,null,1,"No"]
["MK80FN256VDC15","NXPMK80FN256VDC15","NXP","ARM CM4F",150,256,null,256,16,null,2,null,87,"No",4,3,1,"Yes",1,null,-40,105,1.71,3.6,121,"XFBGA121",4.5,null,5,null,null,null,null,null,null,null,"Kinetis K80: 150MHz CortexM4F Secure MCU, 256KB Flash, 256KB SRAM, FullSpeed USB, 121XFBGA",null,null,null,1,"No"]
["MK80FN256VLL15","NXPMK80FN256VLL15","NXP","ARM CM4F",150,256,null,256,16,null,2,null,66,"No",4,3,1,"Yes",1,null,-40,105,1.71,3.6,100,"LQFP100",4.34,null,5,null,null,null,null,null,null,null,"Kinetis K80: 150MHz CortexM4F Secure MCU, 256KB Flash, 256KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"No"]
["MK81FN256VDC15","NXPMK81FN256VDC15","NXP","ARM CM4F",150,256,null,256,16,null,3,null,85,"No",4,3,1,"Yes",25,null,-40,105,1.71,3.6,121,"XFBGA121",6.58,null,5,null,null,null,null,null,null,null,"Kinetis K81: 150MHz CortexM4F Secure MCU, 256K Flash, 256K RAM, USB, Antitamper, HW Crypto, 121BGA",null,null,null,1,"No"]
["MK81FN256VDC15R","NXPMK81FN256VDC15R","NXP","ARM CM4F",150,256,null,256,16,null,3,null,85,"No",4,3,1,"Yes",25,null,-40,105,1.71,3.6,121,"XFBGA121",6.58,null,5,null,null,null,null,null,null,null,"Kinetis K81: 150MHz CortexM4F Secure MCU, 256K Flash, 256K RAM, USB, Antitamper, HW Crypto, 121BGA",null,null,null,1,"No"]
["MK81FN256VLL15","NXPMK81FN256VLL15","NXP","ARM CM4F",150,256,null,256,16,null,3,null,66,"No",4,3,1,"Yes",25,null,-40,105,1.71,3.6,100,"LQFP100",6.39,null,5,null,null,null,null,null,null,null,"Kinetis K81: 150MHz CortexM4F Secure MCU, 256K Flash, 256K RAM, USB, Antitamper, HW Crypto,100LQFP",null,null,null,1,"No"]
["MK82FN256VDC15","NXPMK82FN256VDC15","NXP","ARM CM4F",150,256,null,256,16,null,3,null,87,"No",4,3,1,"Yes",25,null,-40,105,1.71,3.6,121,"XFBGA121",5.08,null,5,null,null,null,null,null,null,null,"Kinetis K82: 150MHz CortexM4F Secure MCU, 256KB Flash, 256KB SRAM, FullSpeed USB, 121XFBGA",null,null,null,1,"No"]
["MK82FN256VLL15","NXPMK82FN256VLL15","NXP","ARM CM4F",150,256,null,256,16,null,3,null,66,"No",4,3,1,"Yes",25,null,-40,105,1.71,3.6,100,"LQFP100",4.9400000000000004,null,5,null,null,null,null,null,null,null,"Kinetis K82: 150MHz CortexM4F Secure MCU, 256KB Flash, 256KB SRAM, FullSpeed USB, 100LQFP",null,null,null,1,"No"]
["MKL24Z32VFM4","NXPMKL24Z32VFM4","NXP","ARM CM0+",48,32,null,4,12,null,1,null,23,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,32,"HVQFN32",1.64,null,3,null,null,null,null,null,null,null,"Kinetis KL24: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"No"]
["MKL24Z32VFT4","NXPMKL24Z32VFT4","NXP","ARM CM0+",48,32,null,4,12,null,1,null,36,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,48,"HVQFN48",1.72,null,3,null,null,null,null,null,null,null,"Kinetis KL24: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"No"]
["MKL24Z32VLH4","NXPMKL24Z32VLH4","NXP","ARM CM0+",48,32,null,4,12,null,1,null,50,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.76,null,3,null,null,null,null,null,null,null,"Kinetis KL24: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MKL24Z32VLK4","NXPMKL24Z32VLK4","NXP","ARM CM0+",48,32,null,4,12,null,1,null,66,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,80,"LQFP80",2.36,null,3,null,null,null,null,null,null,null,"Kinetis KL24: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"No"]
["MKL24Z64VFM4","NXPMKL24Z64VFM4","NXP","ARM CM0+",48,64,null,8,12,null,1,null,23,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,32,"HVQFN32",1.73,null,3,null,null,null,null,null,null,null,"Kinetis KL24: 48MHz CortexM0+ UltraLow Power MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"No"]
["MKL24Z64VFT4","NXPMKL24Z64VFT4","NXP","ARM CM0+",48,64,null,8,12,null,1,null,36,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,48,"HVQFN48",1.81,null,3,null,null,null,null,null,null,null,"Kinetis KL24: 48MHz CortexM0+ UltraLow Power MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"No"]
["MKL24Z64VLH4","NXPMKL24Z64VLH4","NXP","ARM CM0+",48,64,null,8,12,null,1,null,50,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.85,null,3,null,null,null,null,null,null,null,"Kinetis KL24: 48MHz CortexM0+ UltraLow Power MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MKL24Z64VLK4","NXPMKL24Z64VLK4","NXP","ARM CM0+",48,64,null,8,12,null,1,null,66,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,80,"LQFP80",2.4500000000000002,null,3,null,null,null,null,null,null,null,"Kinetis KL24: 48MHz CortexM0+ UltraLow Power MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"No"]
["MKL25Z128VFM4","NXPMKL25Z128VFM4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,23,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,32,"HVQFN32",2.09,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"No"]
["MKL25Z128VFT4","NXPMKL25Z128VFT4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,36,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,48,"HVQFN48",2.1800000000000002,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"No"]
["MKL25Z128VLH4","NXPMKL25Z128VLH4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,50,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",2.23,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MKL25Z128VLK4","NXPMKL25Z128VLK4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,66,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,80,"LQFP80",2.83,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"No"]
["MKL25Z32VFM4","NXPMKL25Z32VFM4","NXP","ARM CM0+",48,32,null,4,16,null,1,null,23,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,32,"HVQFN32",1.69,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"No"]
["MKL25Z32VFT4","NXPMKL25Z32VFT4","NXP","ARM CM0+",48,32,null,4,16,null,1,null,36,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,48,"HVQFN48",1.78,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"No"]
["MKL25Z32VLH4","NXPMKL25Z32VLH4","NXP","ARM CM0+",48,32,null,4,16,null,1,null,50,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.83,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MKL25Z32VLK4","NXPMKL25Z32VLK4","NXP","ARM CM0+",48,32,null,4,16,null,1,null,66,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,80,"LQFP80",2.4300000000000002,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"No"]
["MKL25Z64VFM4","NXPMKL25Z64VFM4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,23,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,32,"HVQFN32",1.78,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"No"]
["MKL25Z64VFT4","NXPMKL25Z64VFT4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,36,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,48,"HVQFN48",1.87,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"No"]
["MKL25Z64VLH4","NXPMKL25Z64VLH4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,50,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.92,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 64LQFP",null,null,null,1,"No"]
["MKL25Z64VLK4","NXPMKL25Z64VLK4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,66,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,80,"LQFP80",2.52,null,3,null,null,null,null,null,null,null,"Kinetis KL25: 48MHz CortexM0+ UltraLow Power MCU, 64KB Flash, 8KB SRAM, FullSpeed USB, 80LQFP",null,null,null,1,"No"]
["MKL26Z128CAL4R","NXPMKL26Z128CAL4R","NXP","ARM CM0",48,128,null,null,16,null,0,null,23,"No",2,null,null,"Yes",null,null,-40,105,1.71,3.6,36,"WLCSP36",1.91,null,null,null,null,null,null,null,null,null,"Kinetis KL26: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB SRAM, FS USB, 36WLCSP,",null,null,null,1,"No"]
["MKL26Z128VFM4","NXPMKL26Z128VFM4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,23,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,32,"HVQFN32",1.89,null,3,null,null,null,null,null,null,null,"Kinetis KL26: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 32QFN",null,null,null,1,"No"]
["MKL26Z128VFT4","NXPMKL26Z128VFT4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,36,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,48,"HVQFN48",1.6,null,3,null,null,null,null,null,null,null,"Kinetis KL26: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"No"]
["MKL26Z128VFT4R","NXPMKL26Z128VFT4R","NXP","ARM CM0+",48,128,null,16,16,null,1,null,36,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,48,"HVQFN48",1.6,null,3,null,null,null,null,null,null,null,"Kinetis KL26: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB SRAM, FullSpeed USB, 48QFN",null,null,null,1,"No"]
["MKL26Z128VLH4","NXPMKL26Z128VLH4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,50,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.64,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, USB, QFP 64",null,null,null,1,"No"]
["MKL26Z128VLH4R","NXPMKL26Z128VLH4R","NXP","ARM CM0+",48,128,null,16,16,null,1,null,50,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.64,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, USB, QFP 64",null,null,null,1,"No"]
["MKL26Z128VLL4","NXPMKL26Z128VLL4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,80,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,100,"LQFP100",1.96,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, USB, QFP 100",null,null,null,1,"No"]
["MKL26Z128VMC4","NXPMKL26Z128VMC4","NXP","ARM CM0+",48,128,null,16,16,null,1,null,80,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,121,"LFBGA121",2.27,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, USB, MAPBGA 121",null,null,null,1,"No"]
["MKL26Z256VLH4","NXPMKL26Z256VLH4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,50,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",2.31,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, USB, QFP 64",null,null,null,1,"No"]
["MKL26Z256VLL4","NXPMKL26Z256VLL4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,80,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,100,"LQFP100",2.2599999999999998,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, USB, QFP 100",null,null,null,1,"No"]
["MKL26Z256VMC4","NXPMKL26Z256VMC4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,80,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,121,"LFBGA121",2.36,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, USB, MAPBGA 121",null,null,null,1,"No"]
["MKL26Z256VMC4R","NXPMKL26Z256VMC4R","NXP","ARM CM0+",48,256,null,32,16,null,1,null,80,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,121,"LFBGA121",2.36,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, USB, MAPBGA 121",null,null,null,1,"No"]
["MKL26Z256VMP4","NXPMKL26Z256VMP4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,50,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LFBGA64",2.15,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, USB, MAPBGA 64",null,null,null,1,"No"]
["MKL26Z32VFM4","NXPMKL26Z32VFM4","NXP","ARM CM0+",48,32,null,4,16,null,1,null,23,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,32,"HVQFN32",1.1100000000000001,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 32KB Flash, 48MHz, USB, QFN 32",null,null,null,1,"No"]
["MKL26Z32VFT4","NXPMKL26Z32VFT4","NXP","ARM CM0+",48,32,null,4,16,null,1,null,36,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,48,"HVQFN48",1.2,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 32KB Flash, 48MHz, USB, QFN 48",null,null,null,1,"No"]
["MKL26Z32VLH4","NXPMKL26Z32VLH4","NXP","ARM CM0+",48,32,null,4,16,null,1,null,50,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.24,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 32KB Flash, 48MHz, USB, QFP 64",null,null,null,1,"No"]
["MKL26Z64VFM4","NXPMKL26Z64VFM4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,23,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,32,"HVQFN32",1.2,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 64KB Flash, 48MHz, USB, QFN 32",null,null,null,1,"No"]
["MKL26Z64VFT4","NXPMKL26Z64VFT4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,36,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,48,"HVQFN48",1.29,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 64KB Flash, 48MHz, USB, QFN 48",null,null,null,1,"No"]
["MKL26Z64VFT4R","NXPMKL26Z64VFT4R","NXP","ARM CM0+",48,64,null,8,16,null,1,null,36,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,48,"HVQFN48",1.29,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 64KB Flash, 48MHz, USB, QFN 48",null,null,null,1,"No"]
["MKL26Z64VLH4","NXPMKL26Z64VLH4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,50,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.33,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 64KB Flash, 48MHz, USB, QFP 64",null,null,null,1,"No"]
["MKL27Z128VFM4","NXPMKL27Z128VFM4","NXP","ARM CM0+",48,128,null,32,16,null,1,null,23,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,32,"HUQFN32",1.61,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, USB, QFN 32",null,null,null,1,"No"]
["MKL27Z128VFM4R","NXPMKL27Z128VFM4R","NXP","ARM CM0+",48,128,null,32,16,null,1,null,23,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,32,"HUQFN32",1.61,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, USB, QFN 32",null,null,null,1,"No"]
["MKL27Z128VFT4","NXPMKL27Z128VFT4","NXP","ARM CM0+",48,128,null,32,16,null,1,null,36,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,48,"HUQFN48",1.69,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, USB, QFN 48",null,null,null,1,"No"]
["MKL27Z128VLH4","NXPMKL27Z128VLH4","NXP","ARM CM0+",48,128,null,32,16,null,1,null,50,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.73,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, USB, LQFP 64",null,null,null,1,"No"]
["MKL27Z128VLH4R","NXPMKL27Z128VLH4R","NXP","ARM CM0+",48,128,null,32,16,null,1,null,50,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.73,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, USB, LQFP 64",null,null,null,1,"No"]
["MKL27Z128VMP4","NXPMKL27Z128VMP4","NXP","ARM CM0+",48,128,null,32,16,null,1,null,50,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LFBGA64",1.78,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 128KB Flash, 48MHz, USB, MAPBGA 64",null,null,null,1,"No"]
["MKL27Z256VFM4","NXPMKL27Z256VFM4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,23,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,32,"HUQFN32",1.86,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, USB, QFN 32",null,null,null,1,"No"]
["MKL27Z256VFM4R","NXPMKL27Z256VFM4R","NXP","ARM CM0+",48,256,null,32,16,null,1,null,23,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,32,"HUQFN32",1.86,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, USB, QFN 32",null,null,null,1,"No"]
["MKL27Z256VFT4","NXPMKL27Z256VFT4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,36,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,48,"HUQFN48",1.94,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, USB, QFN 48",null,null,null,1,"No"]
["MKL27Z256VLH4","NXPMKL27Z256VLH4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,50,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.98,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, USB, LQFP 64",null,null,null,1,"No"]
["MKL27Z256VMP4","NXPMKL27Z256VMP4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,50,"No",2,2,1,"Yes",null,null,-40,105,1.71,3.6,64,"LFBGA64",2.0299999999999998,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, USB, MAPBGA 64",null,null,null,1,"No"]
["MKL27Z32VDA4","NXPMKL27Z32VDA4","NXP","ARM CM0+",48,32,null,8,16,null,1,null,30,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,36,"XFBGA36",1.36,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ Core, 32KB Flash, 48MHz, USB, XFBGA 36",null,null,null,1,"No"]
["MKL27Z32VFM4","NXPMKL27Z32VFM4","NXP","ARM CM0+",48,32,null,8,16,null,1,null,24,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,32,"HUQFN32",1.0900000000000001,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ Core, 32KB Flash, 48MHz, USB, QFN 32",null,null,null,1,"No"]
["MKL27Z32VLH4","NXPMKL27Z32VLH4","NXP","ARM CM0+",48,32,null,8,16,null,1,null,51,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.21,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ Core, 32KB Flash, 48MHz, USB, LQFP 64",null,null,null,1,"No"]
["MKL27Z64VDA4","NXPMKL27Z64VDA4","NXP","ARM CM0+",48,64,null,16,16,null,1,null,30,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,36,"XFBGA36",1.47,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ Core, 64KB Flash, 48MHz, USB, XFBGA 36",null,null,null,1,"No"]
["MKL27Z64VDA4R","NXPMKL27Z64VDA4R","NXP","ARM CM0+",48,64,null,16,16,null,1,null,30,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,36,"XFBGA36",1.47,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ Core, 64KB Flash, 48MHz, USB, XFBGA 36",null,null,null,1,"No"]
["MKL27Z64VFM4","NXPMKL27Z64VFM4","NXP","ARM CM0+",48,64,null,16,16,null,1,null,24,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,32,"HUQFN32",1.2,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ Core, 64KB Flash, 48MHz, USB, QFN 32",null,null,null,1,"No"]
["MKL27Z64VFM4R","NXPMKL27Z64VFM4R","NXP","ARM CM0+",48,64,null,16,16,null,1,null,24,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,32,"HUQFN32",1.2,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ Core, 64KB Flash, 48MHz, USB, QFN 32",null,null,null,1,"No"]
["MKL27Z64VLH4","NXPMKL27Z64VLH4","NXP","ARM CM0+",48,64,null,16,16,null,1,null,51,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.32,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ Core, 64KB Flash, 48MHz, USB, LQFP 64",null,null,null,1,"No"]
["MKL27Z64VLH4R","NXPMKL27Z64VLH4R","NXP","ARM CM0+",48,64,null,16,16,null,1,null,51,"No",2,2,null,"Yes",null,null,-40,105,1.71,3.6,64,"LQFP64",1.32,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ Core, 64KB Flash, 48MHz, USB, LQFP 64",null,null,null,1,"No"]
["MKL28Z512VLL7","NXPMKL28Z512VLL7","NXP","ARM CM0+",72,512,null,128,16,null,2,null,82,"No",3,3,1,"Yes",11,null,-40,105,1.71,3.6,100,"LQFP100",3.17,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 512KB Flash, 128KB RAM, 72MHz, USB OTG, 100LQFP",null,null,null,1,"No"]
["MKL28Z512VLL7R","NXPMKL28Z512VLL7R","NXP","ARM CM0+",72,512,null,128,16,null,2,null,82,"No",3,3,1,"Yes",11,null,-40,105,1.71,3.6,100,"LQFP100",3.17,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 512KB Flash, 128KB RAM, 72MHz, USB OTG, 100LQFP",null,null,null,1,"No"]
["KK26FN2M0CAC18R","NXPKK26FN2M0CAC18R","NXP","ARM CM0",180,2048,null,null,16,null,0,null,116,"No",4,null,null,"Yes",null,null,-40,85,1.71,3.6,169,"WLCSP169",8.64,null,null,null,null,null,null,null,null,null,"Kinetis K 32bit MCU, ARM CM4 core, 2M Flash, 180MHz, WLCSP 169",null,null,null,2,"Yes"]
["KK28FN2M0CAU15R","NXPKK28FN2M0CAU15R","NXP","ARM CM4F",150,120,null,1024,0,null,0,null,null,"No",4,4,2,"Yes",25,null,-40,85,1.71,3.6,210,"WLCSP210",7.76,null,5,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["KK60FN1M0VLQ15","NXPKK60FN1M0VLQ15","NXP","ARM CM4F",150,1024,null,128,16,null,2,null,100,"No",2,3,2,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",7.13,null,6,null,null,null,null,null,null,null,"Kinetis K60: 150MHz CortexM4F MCU, 1MB Flash, 128KB SRAM, Dual USBs (FS + HS), Ethernet, 144LQFP",null,null,null,2,"Yes"]
["KK65FN2M0CAC18R","NXPKK65FN2M0CAC18R","NXP","ARM CM0",180,2048,null,null,16,null,0,null,116,"No",4,null,null,"Yes",null,null,-40,85,1.71,3.6,169,"WLCSP169",9.5399999999999991,null,null,null,null,null,null,null,null,null,"Kinetis K65: 180MHz CortexM4F MCU, 2MB Flash, 256K RAM, 2xUSB, Ethernet, Antitamper, 169WLCSP,",null,null,null,2,"Yes"]
["LPC1830FBD144,551","NXPLPC1830FBD144,551","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,144,"LQFP144",3.35,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1830FBD144K","NXPLPC1830FBD144K","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,144,"LQFP144",3.35,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1830FET100,551","NXPLPC1830FET100,551","NXP","ARM CM3",180,null,null,200,10,null,1,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,100,"TFBGA100",3.2,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1830FET100Y","NXPLPC1830FET100Y","NXP","ARM CM3",180,null,null,200,10,null,1,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,100,"TFBGA100",3.2,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1830FET180,551","NXPLPC1830FET180,551","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,180,"TFBGA180",3.3,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1830FET256,551","NXPLPC1830FET256,551","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,256,"LBGA256",4.07,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1830FET256/CPAE","NXPLPC1830FET256/CPAE","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,256,"LBGA256",4.07,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1833FET256,551","NXPLPC1833FET256,551","NXP","ARM CM3",180,512,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,256,"LBGA256",5.13,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1833JBD144E","NXPLPC1833JBD144E","NXP","ARM CM3",180,512,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,144,"LQFP144",4.95,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1833JET100E","NXPLPC1833JET100E","NXP","ARM CM3",180,512,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,100,"TFBGA100",4.8,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1833JET256,551","NXPLPC1833JET256,551","NXP","ARM CM3",180,512,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,256,"LBGA256",5.14,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1837FET256,551","NXPLPC1837FET256,551","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,256,"LBGA256",5.63,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1837JBD144E","NXPLPC1837JBD144E","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,144,"LQFP144",5.53,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1837JET100E","NXPLPC1837JET100E","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,100,"TFBGA100",5.38,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,2,"No"]
["LPC1837JET256,551","NXPLPC1837JET256,551","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,256,"LBGA256",5.68,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1850FET180,551","NXPLPC1850FET180,551","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"Yes",2,3,null,"Yes",10,null,-40,85,2.4,3.6,180,"TFBGA180",3.74,null,4,null,null,null,null,null,null,null,"Quad SPI Flash Interface  (SPIFI), 200 kB SRAM, two Highspeed USB, Ethernet, LCD, TFBGA180 package",null,null,null,2,"No"]
["LPC1850FET256,551","NXPLPC1850FET256,551","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"Yes",2,3,null,"Yes",10,null,-40,85,2.4,3.6,256,"LBGA256",4.51,null,4,null,null,null,null,null,null,null,"Quad SPI Flash Interface (SPIFI), 200 kB SRAM, two Highspeed USB, Ethernet, LCD, LBGA256 package",null,null,null,2,"No"]
["LPC1850FET256/CPAE","NXPLPC1850FET256/CPAE","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"Yes",2,3,null,"Yes",10,null,-40,85,2.4,3.6,256,"LBGA256",4.51,null,4,null,null,null,null,null,null,null,"Quad SPI Flash Interface (SPIFI), 200 kB SRAM, two Highspeed USB, Ethernet, LCD, LBGA256 package",null,null,null,2,"No"]
["LPC1853FET256,551","NXPLPC1853FET256,551","NXP","ARM CM3",180,512,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,256,"LBGA256",5.63,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,2,"No"]
["LPC1853JBD208E","NXPLPC1853JBD208E","NXP","ARM CM3",180,512,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,208,"LQFP208",5.63,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1853JET256,551","NXPLPC1853JET256,551","NXP","ARM CM3",180,512,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,256,"LBGA256",5.68,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,2,"No"]
["LPC1857FET256,551","NXPLPC1857FET256,551","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"Yes",2,3,null,"Yes",10,null,-40,105,2.4,3.6,256,"LBGA256",6.21,null,4,null,null,null,null,null,null,null,"1 MB flash, 136 kB SRAM, two Highspeed USB, Ethernet, LCD, LBGA256 package",null,null,null,2,"No"]
["LPC1857JBD208E","NXPLPC1857JBD208E","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,208,"LQFP208",6.21,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,2,"No"]
["LPC1857JET256,551","NXPLPC1857JET256,551","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,256,"LBGA256",6.26,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,2,"No"]
["LPC18S30FBD144E","NXPLPC18S30FBD144E","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,144,"LQFP144",3.44,null,4,null,null,null,null,null,null,null,"32bit ARM CM3 flashless MCU with security features; 200 kB SRAM; Ethernet, two HS USB, EMC",null,null,null,2,"No"]
["LPC18S30FET100E","NXPLPC18S30FET100E","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,100,"TFBGA100",3.3,null,4,null,null,null,null,null,null,null,"32bit ARM CM3 flashless MCU with security features; 200 kB SRAM; Ethernet, two HS USB, EMC",null,null,null,2,"No"]
["LPC18S30FET256E","NXPLPC18S30FET256E","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,85,2.4,3.6,256,"LBGA256",4.17,null,4,null,null,null,null,null,null,null,"32bit ARM CM3 flashless MCU with security features; 200 kB SRAM; Ethernet, two HS USB, EMC",null,null,null,2,"No"]
["LPC18S37JBD144E","NXPLPC18S37JBD144E","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,144,"LQFP144",5.63,null,4,null,null,null,null,null,null,null,"32bit ARM CM3 MCU; 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, EMC, AES engine",null,null,null,2,"No"]
["LPC18S37JET100E","NXPLPC18S37JET100E","NXP","ARM CM3",180,1024,16,200,10,null,0,null,null,"No",2,3,null,"Yes",10,null,-40,105,2.4,3.6,100,"TFBGA100",5.48,null,4,null,null,null,null,null,null,null,"32bit ARM CM3 MCU; 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, EMC, AES engine",null,null,null,2,"No"]
["LPC18S50FET180E","NXPLPC18S50FET180E","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"Yes",2,3,null,"Yes",10,null,-40,105,2.4,3.6,180,"TFBGA180",3.83,null,4,null,null,null,null,null,null,null,"32bit ARM CM3 flashless MCU with security features; 200 kB SRAM; Ethernet, two HS USB, LCD, EMC",null,null,null,2,"No"]
["LPC18S50FET256,551","NXPLPC18S50FET256,551","NXP","ARM CM3",180,null,null,200,10,null,0,null,null,"Yes",2,3,null,"Yes",10,null,-40,105,2.4,3.6,256,"LBGA256",4.6100000000000003,null,4,null,null,null,null,null,null,null,"32bit ARM CM3 flashless MCU with security features; 200 kB SRAM; Ethernet, two HS USB, LCD, EMC",null,null,null,2,"No"]
["LPC18S57JBD208E","NXPLPC18S57JBD208E","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"Yes",2,3,null,"Yes",10,null,-40,105,2.4,3.6,208,"LQFP208",6.31,null,4,null,null,null,null,null,null,null,"32bit ARM CM3 MCU; 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC, AES engine",null,null,null,2,"No"]
["LPC18S57JET256E","NXPLPC18S57JET256E","NXP","ARM CM3",180,1024,16,136,10,null,0,null,null,"Yes",2,3,null,"Yes",10,null,-40,105,2.4,3.6,256,"LBGA256",6.35,null,4,null,null,null,null,null,null,null,"32bit ARM CM3 MCU; 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC, AES engine",null,null,null,2,"No"]
["LPC4330FBD144,551","NXPLPC4330FBD144,551","NXP","ARM CM4F",204,null,null,264,10,null,0,null,83,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,144,"LQFP144",3.64,null,4,null,null,null,null,null,null,null,"Dualcore CortexM4/M0, 264 kB SRAM, 2 HS USB with onchip PHY, Ethernet, CAN, AES, SPIFI, SGPIO, SCT",null,null,null,2,"No"]
["LPC4330FBD144Y","NXPLPC4330FBD144Y","NXP","ARM CM4F",204,null,null,264,10,null,0,null,83,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,144,"LQFP144",3.64,null,4,null,null,null,null,null,null,null,"Dualcore CortexM4/M0, 264 kB SRAM, 2 HS USB with onchip PHY, Ethernet, CAN, AES, SPIFI, SGPIO, SCT",null,null,null,2,"No"]
["LPC4330FET100,551","NXPLPC4330FET100,551","NXP","ARM CM4F",204,null,null,264,10,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,100,"TFBGA100",3.49,null,4,null,null,null,null,null,null,null,"Dualcore CortexM4/M0, 264 kB SRAM, 2 HS USB with onchip PHY, Ethernet, CAN, AES, SPIFI, SGPIO, SCT",null,null,null,2,"No"]
["LPC4330FET100Y","NXPLPC4330FET100Y","NXP","ARM CM4F",204,null,null,264,10,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,100,"TFBGA100",3.49,null,4,null,null,null,null,null,null,null,"Dualcore CortexM4/M0, 264 kB SRAM, 2 HS USB with onchip PHY, Ethernet, CAN, AES, SPIFI, SGPIO, SCT",null,null,null,2,"No"]
["LPC4330FET180,551","NXPLPC4330FET180,551","NXP","ARM CM4F",204,null,null,264,10,null,0,null,118,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,180,"TFBGA180",3.59,null,4,null,null,null,null,null,null,null,"Dualcore CortexM4/M0, 264 kB SRAM, 2 HS USB with onchip PHY, Ethernet, CAN, AES, SPIFI, SGPIO, SCT",null,null,null,2,"No"]
["LPC4330FET180Y","NXPLPC4330FET180Y","NXP","ARM CM4F",204,null,null,264,10,null,0,null,118,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,180,"TFBGA180",3.59,null,4,null,null,null,null,null,null,null,"Dualcore CortexM4/M0, 264 kB SRAM, 2 HS USB with onchip PHY, Ethernet, CAN, AES, SPIFI, SGPIO, SCT",null,null,null,2,"No"]
["LPC4330FET256,551","NXPLPC4330FET256,551","NXP","ARM CM4F",204,null,null,264,10,null,0,null,146,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,256,"LBGA256",4.37,null,4,null,null,null,null,null,null,null,"Dualcore CortexM4/M0, 264 kB SRAM, 2 HS USB with onchip PHY, Ethernet, CAN, AES, SPIFI, SGPIO, SCT",null,null,null,2,"No"]
["LPC4333FET256,551","NXPLPC4333FET256,551","NXP","ARM CM4F",204,512,16,136,10,null,0,null,164,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",5.82,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,2,"No"]
["LPC4333JBD144E","NXPLPC4333JBD144E","NXP","ARM CM4F",204,512,16,136,10,null,0,null,83,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,144,"LQFP144",5.72,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,2,"No"]
["LPC4333JET100E","NXPLPC4333JET100E","NXP","ARM CM4F",204,512,16,136,10,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,100,"TFBGA100",5.58,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,2,"No"]
["LPC4333JET256,551","NXPLPC4333JET256,551","NXP","ARM CM4F",204,512,16,136,10,null,0,null,164,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",5.87,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC",null,null,null,2,"No"]
["LPC4337FET256,551","NXPLPC4337FET256,551","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,164,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",6.4,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC",null,null,null,2,"No"]
["LPC4337JBD144E","NXPLPC4337JBD144E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,83,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,144,"LQFP144",6.31,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC",null,null,null,2,"No"]
["LPC4337JET100E","NXPLPC4337JET100E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,49,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,100,"TFBGA100",6.16,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC",null,null,null,2,"No"]
["LPC4337JET256,551","NXPLPC4337JET256,551","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,164,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",6.45,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC",null,null,null,2,"No"]
["LPC4337JET256Y","NXPLPC4337JET256Y","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,164,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",6.45,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC",null,null,null,2,"No"]
["LPC4337JET256Z","NXPLPC4337JET256Z","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,164,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",6.45,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC",null,null,null,2,"No"]
["LPC4350FET180,551","NXPLPC4350FET180,551","NXP","ARM CM4F",204,null,null,264,10,null,0,null,118,"Yes",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,180,"TFBGA180",4.03,null,4,null,null,null,null,null,null,null,"Dualcore CortexM4/M0, 264 kB SRAM, 2 HS USB with onchip PHY, Ethernet, LCD, CAN, AES, SPIFI, SGPIO, SCT",null,null,null,2,"No"]
["LPC4350FET256,551","NXPLPC4350FET256,551","NXP","ARM CM4F",204,null,null,264,10,null,0,null,164,"Yes",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,256,"LBGA256",4.8,null,4,null,null,null,null,null,null,null,"Dualcore CortexM4/M0, 264 kB SRAM, 2 HS USB with onchip PHY, Ethernet, LCD, CAN, AES, SPIFI, SGPIO, SCT",null,null,null,2,"No"]
["LPC4353FET256,551","NXPLPC4353FET256,551","NXP","ARM CM4F",204,512,16,136,10,null,0,null,164,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",6.4,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,2,"No"]
["LPC4353JBD208E","NXPLPC4353JBD208E","NXP","ARM CM4F",204,512,16,136,10,null,0,null,142,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,208,"LQFP208",6.4,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,2,"No"]
["LPC4353JET256,551","NXPLPC4353JET256,551","NXP","ARM CM4F",204,512,16,136,10,null,0,null,164,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",6.45,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC",null,null,null,2,"No"]
["LPC4357FET256,551","NXPLPC4357FET256,551","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,164,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",6.98,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,2,"No"]
["LPC4357JBD208E","NXPLPC4357JBD208E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,142,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,208,"LQFP208",6.78,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC",null,null,null,2,"No"]
["LPC4357JBD208K","NXPLPC4357JBD208K","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,142,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,208,"LQFP208",6.78,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; up to 1 MB flash and 136 kB SRAM; Ethernet, two Highspeed USB, LCD, EMC",null,null,null,2,"No"]
["LPC4357JET256,551","NXPLPC4357JET256,551","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,164,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",6.78,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller (MCU) based on ARM CM4/M0 Cores",null,null,null,2,"No"]
["LPC4370FET100E","NXPLPC4370FET100E","NXP","ARM CM4F",204,null,null,282,10,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,100,"TFBGA100",3.84,null,4,null,null,null,null,null,null,null,"32bit ARM CM4 + 2 x M0 MCU; 282 kB SRAM; Ethernet; two HS USBs; 80 Msps 12bit ADC; configurable peripherals",null,null,null,2,"No"]
["LPC4370FET256E","NXPLPC4370FET256E","NXP","ARM CM4F",204,null,null,282,10,null,0,null,164,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,256,"LBGA256",5.28,null,4,null,null,null,null,null,null,null,"32bit ARM CM4 + 2 x M0 MCU; 282 kB SRAM; Ethernet; two HS USBs; 80 Msps 12bit ADC; configurable peripherals",null,null,null,2,"No"]
["LPC43S30FBD144E","NXPLPC43S30FBD144E","NXP","ARM CM4F",204,null,null,264,10,null,0,null,83,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,144,"LQFP144",3.74,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 flashless MCU with security features; 264 kB SRAM; Ethernet; two HS USBs",null,null,null,2,"No"]
["LPC43S30FET100E","NXPLPC43S30FET100E","NXP","ARM CM4F",204,null,null,264,10,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,100,"TFBGA100",3.59,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 flashless MCU with security features; 264 kB SRAM; Ethernet; two HS USBs",null,null,null,2,"No"]
["LPC43S30FET256E","NXPLPC43S30FET256E","NXP","ARM CM4F",204,null,null,136,10,null,0,null,164,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,256,"LBGA256",4.5,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 flashless MCU with security features; 264 kB SRAM; Ethernet; two HS USBs",null,null,null,2,"No"]
["LPC43S37JBD144E","NXPLPC43S37JBD144E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,83,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,144,"LQFP144",6.4,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; 1 MB flash and 136 kB SRAM; Ethernet, 2 x USB, EMC, AES engine",null,null,null,2,"No"]
["LPC43S37JET100E","NXPLPC43S37JET100E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,100,"TFBGA100",6.26,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; 1 MB flash and 136 kB SRAM; Ethernet, 2 x USB, EMC, AES engine",null,null,null,2,"No"]
["LPC43S50FET180E","NXPLPC43S50FET180E","NXP","ARM CM4F",204,null,null,264,10,null,0,null,118,"Yes",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,180,"TFBGA180",4.12,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 flashless MCU with security features; 264 kB SRAM; Ethernet; two HS USBs; LCD",null,null,null,2,"No"]
["LPC43S50FET256,551","NXPLPC43S50FET256,551","NXP","ARM CM4F",204,null,null,264,10,null,0,null,164,"Yes",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,256,"LBGA256",4.95,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 flashless MCU with security features; 264 kB SRAM; Ethernet; two HS USBs; LCD",null,null,null,2,"No"]
["LPC43S57JBD208E","NXPLPC43S57JBD208E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,142,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,208,"LQFP208",6.88,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; 1 MB flash and 136 kB SRAM; Ethernet, 2 x USB, LCD, EMC, AES engine",null,null,null,2,"No"]
["LPC43S57JET256E","NXPLPC43S57JET256E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,164,"Yes",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",6.88,null,4,null,null,null,null,null,null,null,"32bit ARM CM4/M0 MCU; 1 MB flash and 136 kB SRAM; Ethernet, 2 x USB, LCD, EMC, AES engine",null,null,null,2,"No"]
["LPC43S67JBD208E","NXPLPC43S67JBD208E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,142,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,208,"LQFP208",6.88,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM4/M0",null,null,null,2,"No"]
["LPC43S67JET100E","NXPLPC43S67JET100E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,null,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,100,"TFBGA100",6.26,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM4/M0",null,null,null,2,"No"]
["LPC43S67JET256E","NXPLPC43S67JET256E","NXP","ARM CM4F",204,1024,16,136,10,null,0,null,164,"No",2,3,null,"Yes",12,null,-40,105,2.2000000000000002,3.6,256,"LBGA256",6.88,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM4/M0",null,null,null,2,"No"]
["LPC43S70FET100E","NXPLPC43S70FET100E","NXP","ARM CM4F",204,null,null,282,12,null,0,null,49,"No",2,3,null,"Yes",12,null,-40,85,2.2000000000000002,3.6,100,"TFBGA100",3.94,null,4,null,null,null,null,null,null,null,"32bit ARM CM4 + 2 x M0 MCU; 282 kB SRAM; Ethernet; two HS USBs; 80 Msps 12bit ADC; configurable peripherals, AES",null,null,null,2,"No"]
["LPC54005JBD100E","NXPLPC54005JBD100E","NXP","ARM CM4F",180,0,16,360,16,null,0,null,64,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,100,"LQFP100",2.0099999999999998,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["LPC54005JET100E","NXPLPC54005JET100E","NXP","ARM CM4F",180,0,16,360,16,null,0,null,64,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,100,"TFBGA100",2.06,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["LPC54016JBD100E","NXPLPC54016JBD100E","NXP","ARM CM4F",180,0,16,360,16,null,0,null,64,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,100,"LQFP100",2.3199999999999998,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["LPC54016JBD208E","NXPLPC54016JBD208E","NXP","ARM CM4F",180,0,16,360,16,null,0,null,171,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,208,"LQFP208",2.44,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["LPC54016JET180E","NXPLPC54016JET180E","NXP","ARM CM4F",180,0,16,360,16,null,0,null,145,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,180,"TFBGA180",2.39,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["LPC54018J2MET180E","NXPLPC54018J2MET180E","NXP","ARM CM4F",180,2048,null,360,12,null,0,null,137,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,180,"TFBGA180",2.68,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["LPC54018J4MET180E","NXPLPC54018J4MET180E","NXP","ARM CM4F",180,4096,null,360,12,null,0,null,137,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,180,"TFBGA180",2.8,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["LPC54018JBD208E","NXPLPC54018JBD208E","NXP","ARM CM4F",180,0,16,360,16,null,0,null,171,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,208,"LQFP208",2.65,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["LPC54018JET180E","NXPLPC54018JET180E","NXP","ARM CM4F",180,0,16,360,16,null,0,null,145,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,180,"TFBGA180",2.58,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["LPC54605J256BD100E","NXPLPC54605J256BD100E","NXP","ARM CM4F",180,256,16,136,12,null,0,null,64,"Yes",9,9,2,"Yes",5,null,-40,105,1.7,3.6,100,"LQFP100",2.16,null,9,null,null,null,null,null,null,null,null,null,null,null,2,"Yes"]
["LPC54605J256ET100E","NXPLPC54605J256ET100E","NXP","ARM CM4F",180,256,16,136,12,null,0,null,64,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,100,"TFBGA100",2.2200000000000002,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"Yes"]
["LPC54605J256ET180E","NXPLPC54605J256ET180E","NXP","ARM CM4F",180,256,16,136,12,null,0,null,145,"Yes",0,0,2,"Yes",5,null,0,null,1.7,3.6,180,"TFBGA180",2.3199999999999998,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54605J512BD100E","NXPLPC54605J512BD100E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,64,"Yes",9,9,2,"Yes",5,null,-40,105,1.7,3.6,100,"LQFP100",null,null,9,null,null,null,null,null,null,null,null,null,null,null,2,"Yes"]
["LPC54605J512ET100E","NXPLPC54605J512ET100E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,64,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,100,"TFBGA100",null,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"Yes"]
["LPC54605J512ET180E","NXPLPC54605J512ET180E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,145,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,180,"TFBGA180",2.42,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54605J512ET180K","NXPLPC54605J512ET180K","NXP","ARM CM4F",180,512,16,200,12,null,0,null,145,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,180,"TFBGA180",2.42,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54606J256BD100E","NXPLPC54606J256BD100E","NXP","ARM CM4F",180,256,16,136,12,null,0,null,64,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,100,"LQFP100",2.4700000000000002,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"Yes"]
["LPC54606J256ET100E","NXPLPC54606J256ET100E","NXP","ARM CM4F",180,256,16,136,12,null,0,null,64,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,100,"TFBGA100",2.5299999999999998,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"Yes"]
["LPC54606J256ET180E","NXPLPC54606J256ET180E","NXP","ARM CM4F",180,256,16,136,12,null,0,null,145,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,180,"TFBGA180",2.5499999999999998,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54606J512BD100E","NXPLPC54606J512BD100E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,64,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,100,"LQFP100",2.58,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"Yes"]
["LPC54606J512BD208E","NXPLPC54606J512BD208E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,171,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,208,"LQFP208",2.7,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54606J512ET100E","NXPLPC54606J512ET100E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,64,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,100,"TFBGA100",2.63,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"Yes"]
["LPC54607J256BD208E","NXPLPC54607J256BD208E","NXP","ARM CM4F",180,256,16,136,12,null,0,null,171,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,208,"LQFP208",2.83,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54607J256ET180E","NXPLPC54607J256ET180E","NXP","ARM CM4F",180,256,16,136,12,null,0,null,145,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,180,"TFBGA180",2.8,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54607J512ET180E","NXPLPC54607J512ET180E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,145,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,180,"TFBGA180",2.85,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54608J512BD208E","NXPLPC54608J512BD208E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,171,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,208,"LQFP208",2.91,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54608J512ET180E","NXPLPC54608J512ET180E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,145,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,180,"TFBGA180",2.89,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54616J256ET180E","NXPLPC54616J256ET180E","NXP","ARM CM4F",180,256,16,136,12,null,0,null,145,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,180,"TFBGA180",2.6,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54616J512BD100E","NXPLPC54616J512BD100E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,64,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,100,"LQFP100",2.63,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"Yes"]
["LPC54616J512BD208E","NXPLPC54616J512BD208E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,171,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,208,"LQFP208",2.75,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54616J512ET100E","NXPLPC54616J512ET100E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,64,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,100,"TFBGA100",2.69,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"Yes"]
["LPC54618J512BD208E","NXPLPC54618J512BD208E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,171,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,208,"LQFP208",2.97,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54618J512ET180E","NXPLPC54618J512ET180E","NXP","ARM CM4F",180,512,16,200,12,null,0,null,145,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,180,"TFBGA180",2.95,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) With Advanced Peripherals Based on ARM CM4 Core",null,null,null,2,"Yes"]
["LPC54628J512ET180E","NXPLPC54628J512ET180E","NXP","ARM CM4F",220,512,16,200,12,null,0,null,145,"Yes",0,0,2,"Yes",5,null,-40,105,1.7,3.6,180,"TFBGA180",2.94,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"Yes"]
["LPC54S005JBD100E","NXPLPC54S005JBD100E","NXP","ARM CM4F",180,null,16,360,24,null,0,null,64,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,100,"LQFP100",2.17,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) with Advanced Peripherals Based on Arm® Cortex®M4 Core and Security",null,null,null,2,"No"]
["LPC54S005JET100E","NXPLPC54S005JET100E","NXP","ARM CM4F",180,null,16,360,24,null,0,null,64,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,100,"TFBGA100",2.2200000000000002,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) with Advanced Peripherals Based on Arm® Cortex®M4 Core and Security",null,null,null,2,"No"]
["LPC54S016JBD100E","NXPLPC54S016JBD100E","NXP","ARM CM4F",180,null,16,360,24,null,0,null,64,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,100,"LQFP100",2.4700000000000002,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) with Advanced Peripherals Based on Arm® Cortex®M4 Core and Security",null,null,null,2,"No"]
["LPC54S016JBD208E","NXPLPC54S016JBD208E","NXP","ARM CM4F",180,null,16,360,24,null,0,null,171,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,208,"LQFP208",2.6,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) with Advanced Peripherals Based on Arm® Cortex®M4 Core and Security",null,null,null,2,"No"]
["LPC54S016JET100E","NXPLPC54S016JET100E","NXP","ARM CM4F",180,null,16,360,24,null,0,null,64,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,100,"TFBGA100",2.5299999999999998,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) with Advanced Peripherals Based on Arm® Cortex®M4 Core and Security",null,null,null,2,"No"]
["LPC54S016JET180E","NXPLPC54S016JET180E","NXP","ARM CM4F",180,null,16,360,24,null,0,null,145,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,180,"TFBGA180",2.5499999999999998,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) with Advanced Peripherals Based on Arm® Cortex®M4 Core and Security",null,null,null,2,"No"]
["LPC54S018J2MET180E","NXPLPC54S018J2MET180E","NXP","ARM CM4F",180,2048,null,360,12,null,0,null,137,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,180,"TFBGA180",2.84,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["LPC54S018J4MET180E","NXPLPC54S018J4MET180E","NXP","ARM CM4F",180,4096,null,360,12,null,0,null,137,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,180,"TFBGA180",2.96,null,0,null,null,null,null,null,null,null,null,null,null,null,2,"No"]
["LPC54S018JBD208E","NXPLPC54S018JBD208E","NXP","ARM CM4F",180,null,16,360,24,null,0,null,171,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,208,"LQFP208",2.81,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) with Advanced Peripherals Based on Arm® Cortex®M4 Core and Security",null,null,null,2,"No"]
["LPC54S018JET180E","NXPLPC54S018JET180E","NXP","ARM CM4F",180,null,16,360,24,null,0,null,145,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,180,"TFBGA180",2.73,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) with Advanced Peripherals Based on Arm® Cortex®M4 Core and Security",null,null,null,2,"No"]
["LPC54S018JET180Y","NXPLPC54S018JET180Y","NXP","ARM CM4F",180,null,16,360,24,null,0,null,145,"No",0,1,2,"Yes",5,null,-40,105,1.71,3.6,180,"TFBGA180",2.73,null,0,null,null,null,null,null,null,null,"PowerEfficient Microcontrollers (MCUs) with Advanced Peripherals Based on Arm® Cortex®M4 Core and Security",null,null,null,2,"No"]
["LPC5526JBD100K","NXPLPC5526JBD100K","NXP","ARM CM33",150,256,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,100,"HLQFP100",1.85,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC5526JBD64K","NXPLPC5526JBD64K","NXP","ARM CM33",150,256,null,null,16,null,0,null,36,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,64,"HTQFP64",1.64,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC5526JEV98E","NXPLPC5526JEV98E","NXP","ARM CM33",150,256,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,98,"VFBGA98",1.8,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC5526JEV98K","NXPLPC5526JEV98K","NXP","ARM CM33",150,256,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,98,"VFBGA98",1.8,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC5528JBD100K","NXPLPC5528JBD100K","NXP","ARM CM33",150,512,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,100,"HLQFP100",2.09,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC5528JBD64K","NXPLPC5528JBD64K","NXP","ARM CM33",150,512,null,null,16,null,0,null,36,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,64,"HTQFP64",1.85,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC5528JEV98E","NXPLPC5528JEV98E","NXP","ARM CM33",150,512,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,98,"VFBGA98",2.0499999999999998,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC5528JEV98K","NXPLPC5528JEV98K","NXP","ARM CM33",150,512,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,98,"VFBGA98",2.0499999999999998,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S26JBD100K","NXPLPC55S26JBD100K","NXP","ARM CM33",150,256,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,100,"HLQFP100",1.99,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S26JBD64K","NXPLPC55S26JBD64K","NXP","ARM CM33",150,256,null,null,16,null,0,null,36,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,64,"HTQFP64",1.75,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S26JEV98E","NXPLPC55S26JEV98E","NXP","ARM CM33",150,256,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,98,"VFBGA98",1.94,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S26JEV98K","NXPLPC55S26JEV98K","NXP","ARM CM33",150,256,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,98,"VFBGA98",1.94,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S28JBD100K","NXPLPC55S28JBD100K","NXP","ARM CM33",150,512,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,100,"HLQFP100",2.2200000000000002,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S28JBD64K","NXPLPC55S28JBD64K","NXP","ARM CM33",150,512,null,null,16,null,0,null,36,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,64,"HTQFP64",1.99,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S28JEV98E","NXPLPC55S28JEV98E","NXP","ARM CM33",150,512,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,98,"VFBGA98",2.17,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S28JEV98K","NXPLPC55S28JEV98K","NXP","ARM CM33",150,512,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,98,"VFBGA98",2.17,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S66JBD100K","NXPLPC55S66JBD100K","NXP","ARM CM33",100,320,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,100,"HLQFP100",2.21,null,8,null,null,null,null,null,null,null,"High Efficiency Arm® Cortex®M33based Microcontroller",null,null,null,2,"No"]
["LPC55S66JBD64K","NXPLPC55S66JBD64K","NXP","ARM CM33",150,320,null,null,16,null,0,null,36,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,64,"HTQFP64",1.89,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S66JEV98E","NXPLPC55S66JEV98E","NXP","ARM CM33",100,320,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,98,"VFBGA98",2.11,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S66JEV98K","NXPLPC55S66JEV98K","NXP","ARM CM33",100,320,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,98,"VFBGA98",2.11,null,8,null,null,null,null,null,null,null,"High Efficiency Arm<sup>®</sup> Cortex<sup>®</sup>M33based Microcontroller",null,null,null,2,"No"]
["LPC55S69JBD100K","NXPLPC55S69JBD100K","NXP","ARM CM33",100,640,null,null,16,null,0,null,64,"No",8,8,8,"Yes",5,null,-40,105,1.8,3.6,100,"HLQFP100",2.62,null,8,null,null,null,null,null,null,null,"High Efficiency Arm® Cortex®M33based Microcontroller",null,null,null,2,"No"]
["R5F104LEAFB","RenesasR5F104LEAFB","Renesas","RL78",32,64,4,5.5,10,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LEAFP","RenesasR5F104LEAFP","Renesas","RL78",32,64,4,5.5,10,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LEALA","RenesasR5F104LEALA","Renesas","RL78",32,64,4,5.5,10,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64WFLGA",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104LEDFA","RenesasR5F104LEDFA","Renesas","RL78",32,64,4,5.5,10,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104LEDFB","RenesasR5F104LEDFB","Renesas","RL78",32,64,4,5.5,10,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104LEDFP","RenesasR5F104LEDFP","Renesas","RL78",32,64,4,5.5,10,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104LEGFA","RenesasR5F104LEGFA","Renesas","RL78",32,64,4,5.5,10,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LEGFB","RenesasR5F104LEGFB","Renesas","RL78",32,64,4,5.5,10,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LEGFP","RenesasR5F104LEGFP","Renesas","RL78",32,64,4,5.5,10,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LEGLA","RenesasR5F104LEGLA","Renesas","RL78",32,64,4,5.5,10,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,64,"64WFLGA",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["STM32F030C6","STSTM32F030C6","ST","ARM CM0",48,32,null,4,10,10,0,0,39,"No",1,1,null,"No",5,"24bit downcounter,2xWDG,RTC",-40,85,2.4,3.6,48,"LQFP 48 7x7x1.4",null,1,null,2,250,null,null,null,"Active",null,"Mainstream ARM CM0 Value line MCU with 32 Kbytes Flash, 48 MHz CPU",0]
["STM32F030C8","STSTM32F030C8","ST","ARM CM0",48,64,null,8,10,10,0,0,39,"No",2,2,null,"No",7,"24bit downcounter,2xWDG,RTC",-40,85,2.4,3.6,48,"LQFP 48 7x7x1.4",null,2,null,2,250,null,null,null,"Active",null,"Mainstream ARM CM0 Value line MCU with 64 Kbytes Flash, 48 MHz CPU",0]
["STM32F030CC","STSTM32F030CC","ST","ARM CM0",48,256,null,32,10,10,0,0,38,"No",2,2,null,"No",8,"24bit downcounter,2xWDG,RTC",-40,85,2.4,3.6,48,"LQFP 48 7x7x1.4",null,6,null,2,306,null,null,null,"Active",null,"Mainstream ARM CM0 Value line MCU with 256 Kbytes Flash, 48 MHz CPU",0]
["MSP430F5227","TIMSP430F5227","TI","MSP430",25,64,null,8,10,10,0,8,53,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80",null,null,2,null,null,0,null,null,null,null,"UltraLow Power 1.8V SplitRail I/O",0,"N/A","No",0,"No"]
["ATSAM3N00B","MicrochipATSAM3N00B","Microchip","ARM CM3",48,16,0,4,10,10,1,0,47,"No",2,3,0,"No",6,null,-40,85,1.62,3.6,64," 64/LQFP 64/VQFN",1.87,null,4,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,0,null,null,"N/A","No"]
["ATSAM3N0A","MicrochipATSAM3N0A","Microchip","ARM CM3",48,32,0,8,10,8,1,0,34,"No",2,2,0,"No",6,null,-40,85,1.62,3.6,48," 48/LQFP 48/VQFN",1.74,null,3,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,0,null,null,"N/A","No"]
["ATSAM3N0B","MicrochipATSAM3N0B","Microchip","ARM CM3",48,32,0,8,10,10,0,0,47,"No",2,3,0,"No",6,null,-40,85,1.62,3.6,64," 64/LQFP 64/VQFN",1.87,null,4,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,0,null,null,"N/A","No"]
["ATSAM3N0C","MicrochipATSAM3N0C","Microchip","ARM CM3",48,32,0,8,10,16,1,0,79,"No",2,3,0,"No",6,null,-40,85,1.62,3.6,100," 100/LQFP 100/TFBGA",2.1,null,4,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,0,null,null,"N/A","No"]
["ATSAM3N1A","MicrochipATSAM3N1A","Microchip","ARM CM3",48,64,0,8,10,8,0,0,34,"No",2,2,0,"No",6,null,-40,85,1.62,3.6,48," 48/LQFP 48/VQFN",1.74,null,3,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,0,null,null,"N/A","No"]
["ATSAM3N1B","MicrochipATSAM3N1B","Microchip","ARM CM3",48,64,0,8,10,10,1,0,47,"No",2,3,0,"No",6,null,-40,85,1.62,3.6,64," 64/LQFP 64/VQFN",1.87,null,4,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,0,null,null,"N/A",{"$f":"IF(AF989=0, \"No\", \"Yes\")","v":"No"}]
["ATSAM3N1C","MicrochipATSAM3N1C","Microchip","ARM CM3",48,64,0,8,10,16,1,0,79,"No",2,3,0,"No",6,null,-40,85,1.62,3.6,100," 100/LQFP 100/TFBGA",2.1,null,4,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,0,null,null,"N/A","No"]
["ATSAM4N16B","MicrochipATSAM4N16B","Microchip","ARM CM4",100,1024,0,80,10,10,1,0,47,"No",3,3,0,"No",15,null,-40,85,1.62,3.6,64," 64/LQFP 64/VQFN",3.21,null,6,null,null,0,null,null," In Production ","",null,0,null,null,"N/A","No"]
["ATSAM4N16C","MicrochipATSAM4N16C","Microchip","ARM CM4",100,1024,0,80,10,16,1,0,79,"No",3,4,0,"No",15,null,-40,85,1.62,3.6,100," 100/LQFP 100/TFBGA 100/VFBGA",3.42,null,7,null,null,0,null,null," In Production Consider: AT32UC3L0128","",null,2,null,0," Full Speed","No"]
["ATSAM4N8A","MicrochipATSAM4N8A","Microchip","ARM CM4",100,512,0,64,10,8,1,0,34,"No",3,2,0,"No",15,null,-40,85,1.62,3.6,48," 48/LQFP 48/VQFN",2.5099999999999998,null,5,null,null,0,null,null," In Production ","",null,2,null,0," Full Speed","No"]
["ATSAM4N8B","MicrochipATSAM4N8B","Microchip","ARM CM4",100,512,0,64,10,10,1,0,47,"No",3,3,0,"No",15,null,-40,85,1.62,3.6,64," 64/LQFP 64/VQFN",2.64,null,6,null,null,0,null,null," In Production Consider: AT32UC3L0128","",null,2,null,0," Full Speed","No"]
["ATSAM4N8C","MicrochipATSAM4N8C","Microchip","ARM CM4",100,512,0,64,10,16,1,0,79,"No",3,4,0,"No",15,null,-40,85,1.62,3.6,100," 100/LQFP 100/TFBGA 100/VFBGA",2.8,null,7,null,null,0,null,null," In Production Consider: AT32UC3L0128","",null,2,null,0," Full Speed","No"]
["ATSAMD09C13","MicrochipATSAMD09C13","Microchip","ARM CM0+",48,8,0,4,12,5,0,0,12,"No",2,2,0,"No",5,null,-40,85,2.4,3.6,14," 14/SOIC",0.68,null,2,null,null,0,null,null," In Production ","",null,2,null,0," Full Speed","No"]
["ATSAMD09D14","MicrochipATSAMD09D14","Microchip","ARM CM0+",48,16,0,4,12,5,0,0,22,"No",2,2,0,"No",5,null,-40,85,2.4,3.6,24," 24/VQFN",0.76,null,2,null,null,0,null,null," In Production ","",null,2,null,0," Full Speed","No"]
["ATSAMDA1E14B","MicrochipATSAMDA1E14B","Microchip","ARM CM0+",48,16,0.5,4,12,10,1,2,26,"No",4,4,1,"Yes",12,null,-40,105,2.7,3.63,32," 32/TQFP 32/VQFN",1.63,null,4,null,null,0,null,null," In Production ","CAN,",null,2,null,0," Full Speed","No"]
["ATSAMDA1E16B","MicrochipATSAMDA1E16B","Microchip","ARM CM0+",48,64,0.5,8,10,10,1,2,26,"No",4,4,1,"Yes",12,null,-40,105,2.7,3.63,32," 32/TQFP 32/VQFN",1.8,null,4,null,null,0,null,null," In Production ","CAN,",null,2,null,0," Full Speed","No"]
["ATSAMDA1G14B","MicrochipATSAMDA1G14B","Microchip","ARM CM0+",48,16,1,4,10,14,1,2,38,"No",6,6,1,"Yes",12,null,-40,105,2.7,3.63,48," 48/TQFP 48/VQFN",1.9,null,6,null,null,0,null,null," In Production ","EtherNet",null,2,null,0," Full Speed","No"]
["ATtiny104","MicrochipATtiny104","Microchip"," 8bit AVR MCU",12,1,0,3.125E-2,10,8,0,0,12,"No",0,0,0,"No",1,null,-40,125,1.8,5.5,14," 14/SOIC",0.45,null,1,null,null,0,null,null," In Production ","",null,2,null,0," Full Speed","No"]
["ATtiny44","MicrochipATtiny44","Microchip"," 8bit AVR MCU",20,4,0.25,0.25,10,8,0,1,12,"No",1,1,0,"No",2,null,-40,85,1.8,5.5,14," 14/PDIP 14/SOIC 20/WQFN",1.2,null,0,null,null,0,null,null," In Production ","",null,2,null,0," Full Speed","No"]
["ATtiny861A","MicrochipATtiny861A","Microchip"," 8bit AVR MCU",20,8,0.5,0.5,10,11,0,1,16,"No",1,1,0,"No",2,null,-40,85,1.8,5.5,20," 20/PDIP 20/SOIC 20/TSSOP 32/VQFN",0.75,null,0,null,null,0,null,null," In Production ","",null,2,null,0," Full Speed","No"]
["ATxmega128B3","MicrochipATxmega128B3","Microchip"," 8bit AVR MCU",32,128,2,3.90625E-3,12,8,0,2,36,"Yes",1,2,0,"No",0,null,-40,85,1.6,3.6,64," 64/TQFP 64/VQFN",3.54,null,1,null,null,0,null,null," In Production ","",null,2,null,320," Full Speed","No"]
["ATxmega32D4","MicrochipATxmega32D4","Microchip"," 8bit AVR MCU",32,32,1,4,12,12,0,2,34,"No",2,4,0,"No",4,null,-40,85,1.6,3.6,44," 44/TQFP 44/VQFN 49/VFBGA",1.98,null,2,null,null,0,null,null," In Production ","",null,2,null,0," Host, Device","No"]
["ATxmega8E5","MicrochipATxmega8E5","Microchip"," 8bit AVR MCU",32,8,0.5,1,12,16,0,2,26,"No",1,1,0,"No",3,null,-40,85,1.6,3.6,32," 32/TQFP 32/UQFN 32/VQFN",1.75,null,2,null,null,0,null,null," In Production ","ISO7816,",null,2,null,0," None","No"]
["dsPIC33CH256MP208","MicrochipdsPIC33CH256MP208","Microchip"," 16bit dsPIC DSC",100,256,0,32,12,34,4,4,69,"No",3,3,3,"No",20,null,-40,150,3,3.6,80," 80/TQFP",4.03,null,3,null,null,0,null,null," In Production ","",null,4,null,0," None","No"]
["dsPIC33CH64MP502","MicrochipdsPIC33CH64MP502","Microchip"," 16bit dsPIC DSC",200,64,0,20,12,12,4,4,21,"No",3,3,3,"No",25,null,-40,150,3,3.6,28," 28/SSOP 28/UQFN",2.87,null,3,null,null,0,null,null," In Production ","",null,2,null,0," None","No"]
["dsPIC33EP128GM310","MicrochipdsPIC33EP128GM310","Microchip"," 16bit dsPIC DSC",70,128,0,16,12,49,2,5,85,"No",2,3,1,"No",13,null,-40,150,3,3.6,100," 100/TQFP 121/TFBGA",4.24,null,4,null,null,0,null,null," In Production Consider: dsPIC33EV32GM002","",null,2,null,0," None","No"]
["dsPIC33EV256GM104","MicrochipdsPIC33EV256GM104","Microchip"," 16bit dsPIC DSC",70,256,0,16,12,24,1,5,35,"No",1,2,0,"No",7,null,-40,150,4.5,5.5,44," 44/QFN 44/TQFP 48/TQFP",2.8,null,2,null,null,0,null,null," In Production ","",null,3,null,0," None","No"]
["dsPIC33FJ128MC710A","MicrochipdsPIC33FJ128MC710A","Microchip"," 16bit dsPIC DSC",40,128,0,16,12,24,0,0,85,"No",2,2,0,"No",13,null,-40,150,3,3.6,100," 100/TQFP",5.18,null,2,null,null,0,null,null," In Production ","",null,3,null,0," None","No"]
["PIC12F509","MicrochipPIC12F509","Microchip"," 8bit PIC MCU",4,1.5,0,4.00390625E-2,0,0,0,0,6,"No",0,0,0,"No",1,null,-40,125,2,5.5,8," 8/DFN 8/MSOP 8/PDIP 8/SOIC 8/SOIJ",0.45,null,0,null,null,0,null,null," In Production ","",null,"  ",null,"  ",3,"Yes"]
["PIC12F675","MicrochipPIC12F675","Microchip"," 8bit PIC MCU",20,1.75,0.125,6.25E-2,10,4,0,1,6,"No",0,0,0,"No",2,null,-40,125,2,5.5,8," 8/DFN 8/DFNS 8/PDIP 8/SOIC",0.77,null,0,null,null,0,null,null," In Production ","CAN,",null,0,null,0,3,"Yes"]
["PIC16F1513","MicrochipPIC16F1513","Microchip"," 8bit PIC MCU",20,7,0,0.25,10,17,0,0,25,"No",1,1,0,"No",3,null,-40,125,1.8,5.5,28," 28/SOIC 28/SPDIP 28/SSOP 28/UQFN",0.88,null,1,null,null,0,null,null," In Production ","CAN,",null,1,null,0," High Speed","No"]
["PIC16F15354","MicrochipPIC16F15354","Microchip"," 8bit PIC MCU",32,7,0,0.5,10,24,1,2,25,"No",2,2,0,"No",3,null,-40,125,1.8,5.5,28," 28/QFN 28/SOIC 28/SPDIP 28/SSOP 28/UQFN 28/VQFN",0.73,null,2,null,null,0,null,null," In Production ","",null,3,null,0," None","No"]
["PIC16F1578","MicrochipPIC16F1578","Microchip"," 8bit PIC MCU",32,7,0,0.5,10,12,1,2,18,"No",0,0,0,"No",11,null,-40,125,1.8,5.5,20," 20/PDIP 20/SOIC 20/SSOP 20/UQFN",0.7,null,1,null,null,0,null,null," In Production ","",null,2,null,0," None","No"]
["PIC16F1713","MicrochipPIC16F1713","Microchip"," 8bit PIC MCU",32,7,0,0.5,10,17,2,2,25,"No",1,1,0,"No",5,null,-40,125,1.8,5.5,28," 28/QFN 28/SOIC 28/SPDIP 28/SSOP 28/UQFN",0.92,null,1,null,null,0,null,null," In Production ","",null,2,null,248," None","No"]
["PIC16F1825","MicrochipPIC16F1825","Microchip"," 8bit PIC MCU",32,14,0.25,1,10,8,1,2,12,"No",1,1,0,"No",5,null,-40,125,1.8,5.5,14," 14/PDIP 14/SOIC 14/TSSOP 16/QFN 16/UQFN",0.91,null,1,null,null,0,null,null," In Production ","CAN,",null,2,null,0," None","No"]
["PIC16F18346","MicrochipPIC16F18346","Microchip"," 8bit PIC MCU",32,28,0.25,2,10,17,1,2,18,"No",2,2,0,"No",7,null,-40,125,1.8,5.5,20," 20/PDIP 20/QFN 20/SOIC 20/SSOP 20/UQFN",0.84,null,1,null,null,0,null,null," In Production ","",null,2,null,0," None","No"]
["PIC16F18875","MicrochipPIC16F18875","Microchip"," 8bit PIC MCU",32,14,0.25,1,10,35,1,2,36,"No",2,2,0,"No",7,null,-40,125,1.8,5.5,40," 40/PDIP 40/UQFN 44/QFN 44/TQFP",0.97,null,1,null,null,0,null,null," In Production ","",null,2,null,0,0,"Yes"]
["PIC16F19195","MicrochipPIC16F19195","Microchip"," 8bit PIC MCU",32,14,0.25,1,12,45,1,2,59,"Yes",1,1,0,"No",4,null,-40,125,1.8,5.5,64," 64/QFN 64/TQFP",1.61,null,2,null,null,0,null,null," In Production ","",null,2,null,0,0,"Yes"]
["PIC16F685","MicrochipPIC16F685","Microchip"," 8bit PIC MCU",20,7,0.25,0.25,10,12,0,2,18,"No",0,0,0,"No",3,null,-40,125,2,5.5,20," 20/PDIP 20/QFN 20/SOIC 20/SSOP",1.1299999999999999,null,0,null,null,0,null,null," In Production ","",null,0,null,0," Device + OTG","No"]
["PIC16F721","MicrochipPIC16F721","Microchip"," 8bit PIC MCU",16,7,0,0.25,8,12,0,0,18,"No",1,1,0,"No",3,null,-40,125,1.8,5.5,20," 20/PDIP 20/QFN 20/SOIC 20/SSOP",0.74,null,1,null,null,0,null,null," In Production ","",null,0,null,0," Device + OTG","No"]
["PIC16F84A","MicrochipPIC16F84A","Microchip"," 8bit PIC MCU",20,1.75,6.25E-2,6.640625E-2,0,0,0,0,13,"No",0,0,0,"No",1,null,-40,85,2,6,18," 18/PDIP 18/SOIC 20/SSOP",3.11,null,0,null,null,0,null,null," In Production ","",null,0,null,0," Device + OTG","No"]
["PIC18F1220","MicrochipPIC18F1220","Microchip"," 8bit PIC MCU",40,4,0.25,0.25,10,7,0,0,16,"No",0,0,0,"No",4,null,-40,125,2,5.5,18," 18/PDIP 18/SOIC 20/SSOP 28/QFN",1.96,null,1,null,null,0,null,null," In Production Consider: PIC16F15324","",null,2,null,0," Device + OTG","No"]
["PIC18F24K42","MicrochipPIC18F24K42","Microchip"," 8bit PIC MCU",64,16,0.25,1,12,24,1,2,25,"No",2,1,0,"No",7,null,-40,125,1.8,5.5,28," 28/QFN 28/SOIC 28/SPDIP 28/SSOP 28/UQFN 28/VQFN",1.08,null,2,null,null,0,null,null," In Production Consider: PIC16F18344","",null,2,null,0," FS Device","Yes"]
["PIC18F25J10","MicrochipPIC18F25J10","Microchip"," 8bit PIC MCU",40,32,0,1,10,10,0,2,21,"No",1,1,0,"No",3,null,-40,85,2,3.6,28," 28/QFN 28/SOIC 28/SPDIP 28/SSOP",1.27,null,1,null,null,0,null,null," In Production ","",null,2,null,0," FS Device","Yes"]
["PIC18F26J11","MicrochipPIC18F26J11","Microchip"," 8bit PIC MCU",48,64,0,3.7109375,10,10,0,2,21,"No",2,2,0,"No",5,null,-40,85,2,3.6,28," 28/QFN 28/SOIC 28/SPDIP 28/SSOP",2.0699999999999998,null,2,null,null,0,null,null," In Production ","",null,2,null,0," FS Device","Yes"]
["PIC18F26Q84","MicrochipPIC18F26Q84","Microchip"," 8bit PIC MCU",64,64,1,7.8125E-3,12,24,1,2,25,"No",1,2,0,"No",6,null,-40,125,1.8,5.5,null," Please call for package information",null,null,3,null,null,0,null,null," In Production ","",null,2,null,0," FS Device","Yes"]
["PIC18F43K22","MicrochipPIC18F43K22","Microchip"," 8bit PIC MCU",64,8,0.25,0.5,10,28,1,2,36,"No",2,2,0,"No",4,null,-40,125,1.8,5.5,40," 40/PDIP 40/UQFN 44/QFN 44/TQFP",1.67,null,2,null,null,0,null,null," In Production ","",null,3,null,0," FS Device","Yes"]
["PIC18F44K22","MicrochipPIC18F44K22","Microchip"," 8bit PIC MCU",64,16,0.25,0.75,10,28,1,2,36,"No",2,2,0,"No",4,null,-40,125,1.8,5.5,40," 40/PDIP 40/UQFN 44/QFN 44/TQFP",1.74,null,2,null,null,0,null,null," In Production ","",null,3,null,0," FS Device/Host/OTG","Yes"]
["PIC18F45K20","MicrochipPIC18F45K20","Microchip"," 8bit PIC MCU",64,32,0.25,1.5,10,13,0,2,36,"No",1,1,0,"No",4,null,-40,125,1.8,3.6,40," 40/PDIP 40/UQFN 44/QFN 44/TQFP",1.6,null,1,null,null,0,null,null," In Production ","",null,3,null,0," FS Device/Host/OTG","No"]
["PIC18F46K20","MicrochipPIC18F46K20","Microchip"," 8bit PIC MCU",64,64,1,3.84375,10,13,0,2,36,"No",1,1,0,"No",4,null,-40,125,1.8,3.6,40," 40/PDIP 40/UQFN 44/QFN 44/TQFP",1.82,null,1,null,null,0,null,null," In Production ","",null,3,null,0," FS Device/Host/OTG","No"]
["PIC18F6390","MicrochipPIC18F6390","Microchip"," 8bit PIC MCU",40,8,0,0.75,10,12,0,2,50,"Yes",1,1,0,"No",4,null,-40,125,2,5.5,64," 64/TQFP",2.66,null,2,null,null,0,null,null," In Production ","CAN,",null,3,null,0," FS Device/Host/OTG","No"]
["PIC18F6520","MicrochipPIC18F6520","Microchip"," 8bit PIC MCU",40,32,1,2,10,12,0,2,52,"No",1,1,0,"No",5,null,-40,125,2,5.5,64," 64/TQFP",5.93,null,2,null,null,0,null,null," In Production ","",null,3,null,0," FS Device/Host/OTG","No"]
["PIC18F65K40","MicrochipPIC18F65K40","Microchip"," 8bit PIC MCU",64,32,1,2,10,47,1,3,53,"No",2,2,0,"No",9,null,-40,125,1.8,5.5,64," 64/QFN 64/TQFP",1.48,null,5,null,null,0,null,null," In Production ","CAN,",null,3,null,0," FS Device/Host/OTG","No"]
["PIC18F67J10","MicrochipPIC18F67J10","Microchip"," 8bit PIC MCU",40,128,0,3.84375,10,11,0,2,50,"No",2,2,0,"No",5,null,-40,85,2,3.6,64," 64/TQFP",2.31,null,2,null,null,0,null,null," In Production ","",null,3,null,0," FS Device/Host/OTG","No"]
["PIC18F8490","MicrochipPIC18F8490","Microchip"," 8bit PIC MCU",40,16,0,0.75,10,12,0,2,66,"Yes",1,1,0,"No",4,null,-40,125,2,5.5,80," 80/TQFP",3.5,null,2,null,null,0,null,null," In Production ","",null,2,null,0," FS Device/Host/OTG","No"]
["PIC18F85J90","MicrochipPIC18F85J90","Microchip"," 8bit PIC MCU",40,32,0,2,10,12,0,2,66,"Yes",1,1,0,"No",4,null,-40,85,2,3.6,80," 80/TQFP 128/LQFP",2.44,null,2,null,null,0,null,null," In Production ","",null,2,null,0," FS Device/Host/OTG","No"]
["PIC18F86J16","MicrochipPIC18F86J16","Microchip"," 8bit PIC MCU",48,96,0,3.8125,10,12,0,2,66,"No",2,2,0,"No",5,null,-40,85,2,3.6,80," 80/TQFP",2.7,null,2,null,null,0,null,null," In Production ","",null,2,null,0," FS Device/Host/OTG","No"]
["PIC18F87J90","MicrochipPIC18F87J90","Microchip"," 8bit PIC MCU",48,128,0,3.80859375,10,12,0,2,67,"Yes",1,1,0,"No",4,null,-40,85,2,3.6,80," 80/TQFP",2.98,null,2,null,null,0,null,null," In Production ","",null,2,null,0," FS Device/Host/OTG","Yes"]
["PIC24EP32GP204","MicrochipPIC24EP32GP204","Microchip"," 16bit PIC MCU",70,32,0,4,12,9,1,4,35,"No",2,2,0,"No",7,null,-40,125,3,3.6,44," 44/QFN 44/TQFP 44/VTLA 48/UQFN",1.61,null,2,null,null,0,null,null," In Production ","",null,1,null,0," Full Speed","No"]
["PIC24EP64GP204","MicrochipPIC24EP64GP204","Microchip"," 16bit PIC MCU",70,64,0,8,12,9,1,4,35,"No",2,2,0,"No",7,null,-40,125,3,3.6,44," 44/QFN 44/TQFP 48/UQFN",1.89,null,2,null,null,0,null,null," In Production ","",null,1,null,0," Full Speed","No"]
["PIC24F08KL401","MicrochipPIC24F08KL401","Microchip"," 16bit PIC MCU",32,8,0.5,1,10,12,0,2,18,"No",2,2,0,"No",5,null,-40,85,1.8,3.6,20," 20/PDIP 20/QFN 20/SOIC 20/SSOP",1.36,null,2,null,null,0,null,null," In Production ","",null,1,null,13," Full Speed","No"]
["PIC24F32KA301","MicrochipPIC24F32KA301","Microchip"," 16bit PIC MCU",32,32,0.5,2,12,12,0,3,18,"No",2,2,0,"No",16,null,-40,125,1.8,5.5,20," 20/PDIP 20/SOIC 20/SSOP",2,null,2,null,null,0,null,null," In Production ","",null,1,null,0," Full Speed","No"]
["PIC24FJ128GA610","MicrochipPIC24FJ128GA610","Microchip"," 16bit PIC MCU",32,128,0,32,12,24,0,3,85,"No",3,3,3,"No",7,null,-40,125,2,3.6,100," 100/TQFP 121/TFBGA",2.97,null,6,null,null,0,null,null," In Production ","",null,1,null,0," Full Speed","No"]
["PIC24FJ192GA106","MicrochipPIC24FJ192GA106","Microchip"," 16bit PIC MCU",32,192,0,16,10,16,0,3,53,"No",3,3,0,"No",34,null,-40,125,2,3.6,64," 64/QFN 64/TQFP",3.56,null,4,null,null,0,null,null," In Production ","",null,1,null,0," Full Speed","No"]
["PIC24FJ256GA412","MicrochipPIC24FJ256GA412","Microchip"," 16bit PIC MCU",32,256,0,16,12,24,1,3,102,"Yes",3,4,3,"No",46,null,-40,85,2,3.6,121," 121/TFBGA",4.0999999999999996,null,6,null,null,0,null,null," In Production ","",null,2,null,0," Full Speed","No"]
["PIC24FJ32MC101","MicrochipPIC24FJ32MC101","Microchip"," 16bit PIC MCU",32,32,0,2,10,4,1,3,15,"No",1,1,0,"No",7,null,-40,125,3,3.6,20," 20/PDIP 20/SOIC 20/SSOP",1.68,null,1,null,null,0,null,null," In Production ","",null,5,null,0," Full Speed","No"]
["PIC24FJ64GB106","MicrochipPIC24FJ64GB106","Microchip"," 16bit PIC MCU",32,64,0,16,16,16,0,3,52,"No",3,3,0,"Yes",34,null,-40,85,2,3.6,64," 64/QFN 64/TQFP",3.29,null,4,null,null,0,null,null," In Production ","",null,1,null,0," High Speed","No"]
["PIC24HJ256GP210A","MicrochipPIC24HJ256GP210A","Microchip"," 16bit PIC MCU",80,256,0,16,12,32,0,0,85,"No",2,2,0,"No",13,null,-40,125,3,3.6,100," 100/TQFP",4.63,null,2,null,null,0,null,null," In Production ","",null,1,null,0," High Speed","No"]
["PIC24HJ64GP210A","MicrochipPIC24HJ64GP210A","Microchip"," 16bit PIC MCU",80,64,0,8,12,32,0,0,85,"No",2,2,0,"No",13,null,-40,125,3,3.6,100," 100/TQFP",3.88,null,2,null,null,0,null,null," In Production ","",null,2,null,0," High Speed","No"]
["PIC32MM0032GPL020","MicrochipPIC32MM0032GPL020","Microchip"," 32bit MIPS MCU",25,32,0,8,12,11,1,2,16,"No",0,2,2,"No",10,null,-40,125,2,3.6,20," 20/QFN 20/SSOP",0.87,null,2,null,null,0,null,null," In Production ","",null,2,null,0," High Speed","No"]
["PIC32MX130F064B","MicrochipPIC32MX130F064B","Microchip"," 32bit MIPS MCU",40,64,0,16,10,10,0,3,21,"No",2,2,2,"No",7,null,-40,105,2.2999999999999998,3.6,28," 28/QFN 28/SOIC 28/SPDIP 28/SSOP",1.81,null,2,null,null,0,null,null," In Production ","",null,2,null,0," High Speed","No"]
["PIC32MX150F128D","MicrochipPIC32MX150F128D","Microchip"," 32bit MIPS MCU",50,128,0,64,10,13,0,3,34,"No",2,2,2,"No",7,null,-40,105,2.2999999999999998,3.6,44," 44/QFN 44/TQFP 44/VTLA",2.52,null,2,null,null,0,null,null," In Production ","",null,2,null,0," High Speed","No"]
["PIC32MX340F128H","MicrochipPIC32MX340F128H","Microchip"," 32bit MIPS MCU",80,128,0,32,10,16,0,2,53,"No",2,2,0,"No",6,null,-40,105,2.2999999999999998,3.6,64," 64/QFN 64/TQFP",3.77,null,2,null,null,0,null,null," In Production ","",null,0,null,0," None","Yes"]
["PIC32MX360F512L","MicrochipPIC32MX360F512L","Microchip"," 32bit MIPS MCU",80,512,0,128,10,16,0,2,85,"No",2,2,0,"No",6,null,-40,105,2.2999999999999998,3.6,100," 100/TQFP 121/TFBGA",4.47,null,2,null,null,0,null,null," In Production ","",null,0,null,0," None","Yes"]
["PIC32MZ0512EFF144","MicrochipPIC32MZ0512EFF144","Microchip"," 32bit MIPS MCU",200,512,0,128,12,48,0,2,120,"No",5,6,6,"No",13,null,-40,125,2.2000000000000002,3.6,144," 144/LQFP 144/TFBGA 144/TQFP",6.86,null,6,null,null,0,null,null," In Production ","",null,0,null,0," None","Yes"]
["PIC32MZ1024EFG064","MicrochipPIC32MZ1024EFG064","Microchip"," 32bit MIPS MCU",200,1024,0,512,12,24,0,2,53,"No",4,4,4,"No",13,null,-40,125,2.2000000000000002,3.6,64," 64/QFN 64/TQFP",6.83,null,6,null,null,0,null,null," In Production ","",null,3,null,0," None","Yes"]
["PIC32MZ1025DAK176","MicrochipPIC32MZ1025DAK176","Microchip"," 32bit MIPS MCU",200,1024,0,256,10,45,0,2,120,"No",5,6,6,"Yes",13,null,-40,85,2.2000000000000002,3.6,176," 176/LQFP",8.9,null,6,null,null,0,null,null," In Production ","",null,0,null,0," None","No"]
["PIC32MZ1064DAK169","MicrochipPIC32MZ1064DAK169","Microchip"," 32bit MIPS MCU",200,1024,0,640,10,45,0,2,120,"No",5,6,6,"Yes",13,null,-40,85,2.2000000000000002,3.6,169," 169/LFBGA",8.98,null,6,null,null,0,null,null," In Production ","",null,1,null,0," None","Yes"]
["PIC32MZ2025DAL176","MicrochipPIC32MZ2025DAL176","Microchip"," 32bit MIPS MCU",200,2048,0,256,10,45,0,2,120,"No",5,6,6,"Yes",13,null,-40,85,2.2000000000000002,3.6,176," 176/LQFP",10.33,null,6,null,null,0,null,null," In Production ","",null,1,null,0," None","Yes"]
["PIC32MZ2064DAL169","MicrochipPIC32MZ2064DAL169","Microchip"," 32bit MIPS MCU",200,2048,0,640,10,45,0,2,120,"No",5,6,6,"Yes",13,null,-40,85,2.2000000000000002,3.6,169," 169/LFBGA",10.59,null,6,null,null,0,null,null," In Production ","CAN,",null,1,null,0," None","No"]
["AVR128DA32","MicrochipAVR128DA32","Microchip"," 8bit AVR MCU",24,128,0.5,1.5625E-2,12,14,4,3,26,"No",2,2,0,"No",4,null,-40,125,1.8,5.5,null," Please call for package information",null,null,3,null,null,22,null,null," In Production ","ISO7816,",null,1,null,0," None","No"]
["ATSAML11E16A","MicrochipATSAML11E16A","Microchip","ARM CM23",32,64,2,16,12,10,1,2,25,"No",2,3,0,"No",8,null,-40,125,1.62,3.63,32," 32/TQFP 32/VQFN 32/WLCSP",1.47,null,3,null,null,20,null,null," In Production ","",null,1,null,160," None","No"]
["ATSAML10D14A","MicrochipATSAML10D14A","Microchip","ARM CM23",32,16,2,4,12,5,1,1,17,"No",2,2,0,"No",7,null,-40,125,1.62,3.63,24," 24/SSOP 24/VQFN",1.1399999999999999,null,2,null,null,16,null,null," In Production ","",null,1,null,0," None","No"]
["ATSAMA5D225C-D1M","MicrochipATSAMA5D225C-D1M","Microchip"," Cortex-A5",500,0,"  ",null,12,5,0,"  ",90,"Yes",7,7,2,"Yes",9,null,-40,"105,85",3.1,3.4,196," 196/TFBGA",7,null,9,null,null,12," No",null," In Production ",null,null,1,null,100," None","No"]
["AT32UC3A0512","MicrochipAT32UC3A0512","Microchip"," 32bit AVR MCU",66,512,0,64,10,8,1,0,109,"No",1,6,1,"Yes",3,null,-40,85,0,0,144," 144/LQFP 144/TFBGA",7.79,null,4,null,null,0,null,null," In Production ","",null,1,null,0," None","No"]
["AT32UC3A3256","MicrochipAT32UC3A3256","Microchip"," 32bit AVR MCU",84,256,0,128,10,8,1,0,110,"No",2,6,1,"Yes",6,null,-40,85,3,3.6,144," 144/LQFP 144/TFBGA",8.51,null,4,null,null,0,null,null," In Production ","SD/MMC,",null,0,null,0," None","No"]
["AT32UC3B0256","MicrochipAT32UC3B0256","Microchip"," 32bit AVR MCU",60,256,0,32,12,8,1,0,44,"No",1,4,0,"Yes",3,null,-40,85,0,0,64," 64/TQFP 64/VQFN",4.83,null,3,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,4,null,0," None","No"]
["AT32UC3B1512","MicrochipAT32UC3B1512","Microchip"," 32bit AVR MCU",60,512,0,96,12,6,1,0,28,"No",1,3,1,"Yes",3,null,-40,85,0,0,48," 48/VQFN",5.62,null,2,null,null,0,null,null," In Production ","",null,0,null,0," None","Yes"]
["AT32UC3C2512C","MicrochipAT32UC3C2512C","Microchip"," 32bit AVR MCU",66,512,0,68,12,11,1,2,45,"No",2,5,1,"Yes",6,null,-40,85,0,0,64," 64/TQFP 64/VQFN",6.46,null,4,null,null,0,null,null," In Production ","",null,1,null,0," None","No"]
["MSP430F2013-EP","TIMSP430F2013EP","TI","MSP430",16,2,null,0.125,16,4,0,0,10,"No",1,1,null,"No",1,null,-40,125,1.8,3.6,16,"QFN|16",3.08,null,0,null,null,0,null,null,"ACTIVE",null,"Enhanced Product 16bit UltraLowPower Microcontroller, 2kB Flash, 128B RAM, 16Bit SigmaDelta A/D",1,"N/A",0," None","No"]
["MSP430AFE252","TIMSP430AFE252","TI","MSP430",16,16,null,0.5,24,2,0,0,11,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,24,"TSSOP|24",1.8,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 16KB Flash, 512B RAM, 2x SD24",1,"N/A",0," None","No"]
["MSP430F133","TIMSP430F133","TI","MSP430",16,8,null,0.25,12,8,0,2,48,"No",0,1,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TQFP|64, VQFN|64",2.1,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 8kB Flash, 256B RAM, 12 bit ADC, USART",1,"N/A",0," None","No"]
["MSP430F156","TIMSP430F156","TI","MSP430",16,24,null,1,12,8,1,2,48,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",4.8,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower MCU, 24kB Flash, 1024B RAM, 12Bit ADC, Dual 12Bit DAC, USART, I2C, DMA",2,"N/A",0," None","No"]
["MSP430F2013","TIMSP430F2013","TI","MSP430",16,2,null,0.125,16,4,0,0,10,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.97,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 2kB Flash, 128B RAM, 16Bit SigmaDelta A/D, USI for SPI/I2C",2,"N/A",0," None","No"]
["MSP430F2252","TIMSP430F2252","TI","MSP430",16,16,null,0.5,10,12,0,0,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,49,"DSBGA|49, TSSOP|38, VQFN|40",1.53,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 16KB Flash, 512B RAM",4,"N/A",0," None","No"]
["MSP430F2417","TIMSP430F2417","TI","MSP430",16,92,null,8,12,8,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|64, LQFP|80",3.78,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 92KB Flash, 8KB RAM, 12 Bit ADC, 2 USCIs, HW Multiplier",2,"N/A",0," None","No"]
["MSP430F5131","TIMSP430F5131","TI","MSP430",25,8,null,1,"Slope",0,0,16,31,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,40,"DSBGA|40, TSSOP|38, WQFN|40",0.8,null,1,null,null,0,null,null,"ACTIVE",null,"25MHz MCU with Two 16bit High Res Timers, 8KB flash, 1KB RAM, 16channel Comparator",0,"N/A",0," None","No"]
["MSP430F5219","TIMSP430F5219","TI","MSP430",25,128,null,8,"Slope",0,0,8,53,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, DSBGA|64",2.54,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F522x, MSP430F521x Mixed Signal Microcontroller",0,"N/A",0," None","No"]
["MSP430F5308","TIMSP430F5308","TI","MSP430",25,16,null,6,10,10,0,8,47,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"LQFP|48, VQFN|48, VQFN|64",1.1599999999999999,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F530x Mixed Signal Microcontroller",4,"N/A",0," None","No"]
["MSP430F5340","TIMSP430F5340","TI","MSP430",25,64,null,6,12,7,0,5,38,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.72,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F534x Mixed Signal Microcontroller",4,"N/A",0," None","No"]
["MSP430F5437A","TIMSP430F5437A","TI","MSP430",25,256,null,16,12,14,0,0,67,"No",2,4,null,"No",3,null,-40,85,1.8,3.6,80,"LQFP|80",2.82,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 256KB Flash, 16KB RAM, 12 Bit ADC, 2 USCIs, 32bit HW Multi",3,"N/A",0," None","No"]
["MSP430FR5721","TIMSP430FR5721","TI","MSP430",16,4,null,1,10,12,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",0.84,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5721 8 MHz ULP microcontroller with 4 KB FRAM, 1 KB SRAM,  32 IO, 10bit ADC and comparator",3,"N/A",0," None","No"]
["MSP430FR5730","TIMSP430FR5730","TI","MSP430",16,4,null,1,10,8,0,12,21,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,28,"TSSOP|28, VQFN|24",0.68,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430FR5730 24 MHz ULP microcontroller with 4 KB FRAM, 1 KB SRAM,  21 IO, 10bit ADC and comparator",3,"N/A",0," None","No"]
["MSP430FR5739","TIMSP430FR5739","TI","MSP430",16,16,null,1,10,12,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.1100000000000001,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5739 24 MHz ULP microcontroller with 16 KB FRAM, 1 KB SRAM,  32 IO, 10bit ADC & comparator",3,"N/A",0," None","No"]
["MSP430FR58671","TIMSP430FR58671","TI","MSP430",16,32,null,1,12,16,0,16,40,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,48,"VQFN|48",1.24,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR58xx MixedSignal Microcontrollers",5,"N/A",0," None","No"]
["MSP430FR5958","TIMSP430FR5958","TI","MSP430",16,48,null,2,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.47,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5958 16 MHz UltraLowPower Microcontroller featuring 48 KB FRAM, 2 KB SRAM, 33 IO",4,"N/A",0," None","No"]
["MSP430G2111","TIMSP430G2111","TI","MSP430",16,1,null,0.125,"Slope",0,0,8,10,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.35,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x01, MSP430G2x11 Mixed Signal Microcontroller",3,"N/A",0," None","No"]
["MSP430G2213","TIMSP430G2213","TI","MSP430",16,2,null,0.25,"Slope",0,0,8,24,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.39,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 2 KB Flash, 256 Byte RAM, 24 IO, 2 16bit Timers and comparator",4,"N/A",0," None","No"]
["MSP430G2303","TIMSP430G2303","TI","MSP430",16,4,null,0.25,"N/A",0,0,0,24,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,20,"TSSOP|20, TSSOP|28, VQFN|32",0.4,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x33, MSP430G2x03 Mixed Signal Microcontroller",5,"N/A",0," None","No"]
["MSP430G2444","TIMSP430G2444","TI","MSP430",16,8,null,0.5,10,12,0,0,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,49,"DSBGA|49, TSSOP|38, VQFN|40",1.03,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x44 Mixed Signal Microcontroller",4,"N/A",0," None","No"]
["MSP430G2855","TIMSP430G2855","TI","MSP430",16,48,null,4,10,12,0,8,32,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.19,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x55 Mixed Signal Microcontroller",4,"N/A",0," None","No"]
["CC430F6127","TICC430F6127","TI","MSP430",16,32,null,4,"Slope"," ",0," "," ","Yes",1,1,null,"No",2,null,-40,85,null,null,64,"VQFN|64",1.83,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 32KB Flash, 4KB RAM, CC1101 Radio, AES128, USCI, LCD Driver",4,"N/A",0," None","No"]
["MSP430F4270","TIMSP430F4270","TI","MSP430",16,32,null,0.25,16,5,1,0,32,"Yes",0,0,null,"No",1,null,-40,85,1.8,3.6,48,"SSOP|48, VQFN|48",2.4500000000000002,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 32kB Flash, 256B RAM, 16bit sigma Delta A/D, 12bit D/A, LCD Driver",4,"N/A",0," None","No"]
["MSP430F439","TIMSP430F439","TI","MSP430",16,60,null,2,12,12,0,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,80,"LQFP|80",3.76,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430F43x Mixed Signal Microcontroller",4,"N/A",0," None","No"]
["MSP430F46191","TIMSP430F46191","TI","MSP430",16,120,null,4,"Slope",0,0,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.9800000000000004,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 120KB Flash, 4KB RAM, Comparator, DMA, 160 Seg LCD",5,"N/A",0," None","No"]
["MSP430F4794","TIMSP430F4794","TI","MSP430",16,60,null,2.5,16,4,0,2,72,"Yes",2,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",3.22,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 60KB Flash, 2KB RAM, 4 SigmaDelta ADCs, LCD Driver",2,"N/A",0," None","No"]
["MSP430F6721","TIMSP430F6721","TI","MSP430",25,32,null,2,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",1.85,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 32KB Flash, 2KB RAM",0,"N/A",0," None","No"]
["MSP430F6731A","TIMSP430F6731A","TI","MSP430",25,32,null,2,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,80,"LQFP|80",2.0499999999999998,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 32KB Flash, 2KB RAM",0,"N/A",0," None","No"]
["MSP430F6745","TIMSP430F6745","TI","MSP430",25,128,null,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.31,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, AES, 128KB Flash, 16KB RAM",0,"N/A",0," None","No"]
["MSP430F67471","TIMSP430F67471","TI","MSP430",25,256,null,32,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 32KB RAM",3,"N/A",0," None","No"]
["MSP430F67641","TIMSP430F67641","TI","MSP430",25,128,null,8,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.37,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F676x1 Low cost 3phase metering SOC",2,"N/A",0," None","No"]
["MSP430F6766A","TIMSP430F6766A","TI","MSP430",25,256,null,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 16KB RAM",0,"N/A",0," None","No"]
["MSP430F67761","TIMSP430F67761","TI","MSP430",25,256,null,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.86,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 16KB RAM",1,"N/A",0," None","Yes"]
["MSP430FE423A","TIMSP430FE423A","TI","MSP430",25,8,null,0.25,16,3,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",1.62,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller for Energy Meters, 8KB Flash, 256B RAM",1,"N/A",0," None","Yes"]
["MSP430FR4132","TIMSP430FR4132","TI","MSP430",16,8,null,1,10,10,0,0,60,"Yes",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|48, TSSOP|56",0.6,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller with 8 KB FRAM, 1 KB SRAM, 60 IO, 10bit ADC, LCD, IR Logic",0,"N/A",0," None","No"]
["MSP430FR6047","TIMSP430FR6047","TI","MSP430",16,256,null,8,12,16,0,16,80,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,100,"LQFP|100",6.5,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic MCUs With 256KB FRAM, 12Bit 8 MSPS Sigma Delta ADC, Low Energy Accelerator, AES",2,"Low-energy Accelerator, Ultrasonic Sensing",0," None","No"]
["MSP430FR6879","TIMSP430FR6879","TI","MSP430",16,128,null,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.25,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6879 16 MHz ULP Microcontroller featuring 128 KB FRAM, 2 KB SRAM, 83 IO, 16 ch ADC12, LCD",2,"N/A",0," None","No"]
["MSP430FR69791","TIMSP430FR69791","TI","MSP430",16,128,null,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.25,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR69791 16 MHz UPLP Microcontroller featuring 128 KB FRAM, 2 KB SRAM, 83 IO, ADC12, LCD, AES",2,"N/A",0," None","No"]
["MSP430F5500","TIMSP430F5500","TI","MSP430",25,8,null,4,"Slope",0,0,4,31,"No",1,2,null,"Yes",4,null,-40,85,1.8,3.6,48,"VQFN|48",0.88,null,1,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",3,"N/A",0," None","No"]
["MSP430F5509","TIMSP430F5509","TI","MSP430",25,24,null,4,10,10,0,8,47,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, LQFP|48, VQFN|48, VQFN|64",1.28,null,2,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",2,"N/A",0," None","No"]
["MSP430F5528","TIMSP430F5528","TI","MSP430",25,128,null,8,12,10,0,8,47,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, DSBGA|64, VQFN|64",2.95,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 128KB Flash, 8KB RAM, 12Bit/10 Channel ADC, 32BIT HW Multiplier",2,"N/A",0," None","No"]
["MSP430F6638","TIMSP430F6638","TI","MSP430",25,256,null,16,12,12,1,12,74,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.4000000000000004,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F6638 Mixed Signal Microcontroller",2,"N/A",0," None","No"]
["AT32UC3L016","MicrochipAT32UC3L016","Microchip"," 32bit AVR MCU",50,16,0,8,10,8,0,8,36,"No",2,5,1,"No",6,null,-40,85,1.62,3.6,null," Please call for package information",null,null,4,null,null,0,null,null," In Production ","EtherNet",null,2,null,0," None","No"]
["AT89C51AC2","MicrochipAT89C51AC2","Microchip"," 8bit 8051 MCU",40,32,2,9.765625E-4,12,8,0,0,34,"No",0,0,0,"No",0,null,0,0,3,5.5,44," 44/LQFP 44/PLCC",4.72,null,1,null,null,0,null,null," In Production ","CAN,EtherNet",null,0,null,0," None","No"]
["AT89C51RC","MicrochipAT89C51RC","Microchip"," 8bit 8051 MCU",24,32,0,0,12,0,0,0,32,"No",0,0,0,"No",0,null,0,0,4,6,40," 40/PDIP 44/PLCC 44/TQFP",1.39,null,1,null,null,0,null,null," In Production ","",null,0,null,0," None","Yes"]
["AT89LP51ED2","MicrochipAT89LP51ED2","Microchip"," 8bit 8051 MCU",20,64,4,1.953125E-3,12,7,0,0,42,"No",1,1,0,"No",0,null,0,0,2.4,5.5,40," 40/PDIP 44/LQFP 44/PLCC 44/TQFP 44/VQFN",2.83,null,1,null,null,0,null,null," In Production ","SD/MMC,",null,2,null,0," None","Yes"]
["AT89LS51","MicrochipAT89LS51","Microchip"," 8bit 8051 MCU",16,4,0,0,16,0,0,0,32,"No",0,0,0,"No",0,null,0,0,2.7,4,40," 40/PDIP 44/PLCC 44/TQFP",1.03,null,1,null,null,0,null,null," In Production ","ISO7816,",null,0,null,72," None","No"]
["AT90CAN64","MicrochipAT90CAN64","Microchip"," 8bit AVR MCU",16,64,2,3.90625E-3,16,8,0,1,53,"No",1,1,0,"No",0,null,-40,85,2.7,5.5,64," 64/TQFP 64/VQFN",4.21,null,2,null,null,0,null,null," In Production ","ISO7816,",null,2,null,0," None","No"]
["AT90USB82","MicrochipAT90USB82","Microchip"," 8bit AVR MCU",16,8,0.5,0,0,0,0,1,22,"No",0,2,0,"No",0,null,-40,85,2.7,5.5,32," 32/VQFN",1.82,null,1,null,null,0,null,null," In Production ","SD/MMC,ISO7816,",null,0,null,0," None","No"]
["AT91SAM9G35","MicrochipAT91SAM9G35","Microchip"," ARM926",400,0," 0 / False",null,10,12,0,0,105,"No",3,5,0,"Yes",6,null,-40,85,0.9,1.1000000000000001,217," 217/LFBGA",5.74,null,5,null,null,0," No",null," In Production ",null,null,0,null,0," None","Yes"]
["MSP430FR2355","TIMSP430FR2355","TI","MSP430",16,32,null,4,12,12,1,2,44,"No",2,4,null,"No",4,null,-40,105,1.8,3.6,48,"LQFP|48, TSSOP|38, VQFN|32, VQFN|40",1.03,null,2,null,null,1,null,null,"ACTIVE",null,"24MHz 105C ULP Microcontroller With 32 KB FRAM, 4 KB SRAM, 44 IO, 12bit ADC, 12bit DACs, OpAmp/PGA",2,"N/A",0," None","No"]
["MSP430FG6625","TIMSP430FG6625","TI","MSP430",25,64,null,8,16,10,1,12,73,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",2.42,null,2,null,null,2,null,null,"ACTIVE",null,"25MHz MCU with integrated dual Op Amps, 12bit DACs, 16bit SigmaDelta ADC, USB, LCD, 64KB flash",2,"N/A",0," None","No"]
["MSP430FR2512","TIMSP430FR2512","TI","MSP430",16,8,null,2,10,8,0,0,15,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,16,"TSSOP|16, VQFN|20",0.53,null,1,null,null,4,null,null,"ACTIVE",null,"Capacitive Touch MCU with 4 touch IO (4 sensors), 8KB FRAM, 2KB SRAM, 15 IO, 10bit ADC",2,"N/A",0," None","No"]
["ATmega1284P","MicrochipATmega1284P","Microchip"," 8bit AVR MCU",20,128,4,16,10,8,0,1,32,"No",1,3,0,"No",4,null,-40,85,1.8,5.5,40," 40/PDIP 44/TQFP 44/VQFN",3.84,null,2,null,null,0,null,null," In Production ","SD/MMC,EtherNet",null,2,null,0," None","No"]
["ATMEGA1608","MicrochipATMEGA1608","Microchip"," 8bit AVR MCU",20,16,0.25,2,10,12,0,1,27,"No",1,1,0,"No",4,null,-40,125,1.8,5.5,28," 28/SSOP 32/TQFP 32/VQFN",0.62,null,3,null,null,0,null,null," In Production ","ISO7816,",null,2,null,128," None","No"]
["ATmega168A","MicrochipATmega168A","Microchip"," 8bit AVR MCU",20,16,0.5,1,10,8,0,1,23,"No",1,2,0,"No",3,null,-40,85,1.8,5.5,28," 28/SPDIP 28/VQFN 32/TQFP 32/VQFN",1.1499999999999999,null,1,null,null,0,null,null," In Production ","SD/MMC,CAN,",null,2,null,0," None","No"]
["ATmega32","MicrochipATmega32","Microchip"," 8bit AVR MCU",16,32,1,2,10,8,0,1,32,"No",1,1,0,"No",3,null,-40,85,2.7,5.5,40," 40/PDIP 44/TQFP 44/VQFN",3.91,null,1,null,null,0,null,null," In Production ","",null,2,null,0," None","No"]
["ATmega3290P","MicrochipATmega3290P","Microchip"," 8bit AVR MCU",20,32,1,2,10,8,0,1,69,"Yes",1,2,0,"No",3,null,-40,85,1.8,5.5,100," 100/TQFP",4.1399999999999997,null,1,null,null,0,null,null," In Production ","SD/MMC,ISO7816,",null,2,null,0," None","No"]
["ATMEGA3290PA","MicrochipATMEGA3290PA","Microchip"," 8bit AVR MCU",20,32,1,2,10,8,0,1,32,"Yes",1,3,0,"No",3,null,-40,85,2.7,5.5,100," 100/TQFP",3.65,null,2,null,null,0,null,null," In Production ","SD/MMC,ISO7816,",null,2,null,192," None","No"]
["ATmega644P","MicrochipATmega644P","Microchip"," 8bit AVR MCU",20,64,2,4,10,8,0,1,32,"No",1,3,0,"No",3,null,-40,85,1.8,5.5,40," 40/PDIP 44/TQFP 44/VQFN",3.87,null,2,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,2,null,0," None","No"]
["ATmega6490","MicrochipATmega6490","Microchip"," 8bit AVR MCU",16,64,2,4,10,8,0,1,69,"Yes",1,2,0,"No",3,null,-40,85,1.8,5.5,100," 100/TQFP",6.03,null,1,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,2,null,0," None","No"]
["ATmega88","MicrochipATmega88","Microchip"," 8bit AVR MCU",20,8,0.5,1,10,8,0,1,23,"No",1,2,0,"No",3,null,-40,150,1.8,5.5,28," 28/SPDIP 32/TQFP 32/VQFN",1.84,null,1,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,4,null,0," None","No"]
["ATSAM3N00A","MicrochipATSAM3N00A","Microchip","ARM CM3",48,16,0,4,10,8,0,0,34,"No",2,2,0,"No",6,null,-40,85,1.62,3.6,48," 48/LQFP 48/VQFN",1.74,null,3,null,null,0,null,null," In Production ","SD/MMC,CAN,EtherNet",null,4,null,0," None","No"]
["ATSAM3S4C","MicrochipATSAM3S4C","Microchip","ARM CM3",64,256,0,48,16,15,1,1,79,"No",2,3,1,"Yes",6,null,-40,85,1.62,3.6,100," 100/LQFP 100/TFBGA",3.68,null,4,null,null,0,null,null," In Production ","SD/MMC,",null,4,null,0," None","No"]
["ATSAM3X8C","MicrochipATSAM3X8C","Microchip","ARM CM3",84,512,0,96,0,16,1,0,63,"No",2,4,1,"Yes",9,null,-40,85,1.62,3.6,100," 100/LQFP 100/TFBGA",5.98,null,4,null,null,0,null,null," In Production ","",null,2,null,0," None","No"]
["ATSAM4LS8A","MicrochipATSAM4LS8A","Microchip","ARM CM4",48,512,0,32,16,3,2,1,32,"No",2,1,1,"Yes",3,null,-40,85,1.68,3.6,48," 48/VQFN",4.53,null,3,null,null,0,null,null," In Production ","CAN,EtherNet",null,2,null,0," None","No"]
["ATSAM4LS8B","MicrochipATSAM4LS8B","Microchip","ARM CM4",48,512,0,64,16,7,2,2,48,"No",4,1,1,"Yes",3,null,-40,85,1.68,3.6,64," 64/TQFP 64/VQFN 64/WLCSP",4.7,null,4,null,null,0,null,null," In Production ","CAN,EtherNet",null,2,null,0," None","No"]
["ATSAM4SD32C","MicrochipATSAM4SD32C","Microchip","ARM CM4",120,2048,0,160,16,15,1,1,79,"No",2,3,1,"Yes",6,null,-40,85,1.62,3.6,100," 100/LQFP 100/TFBGA 100/VFBGA",6.27,null,4,null,null,0,null,null," In Production ","",null,3,null,240," None","No"]
["ATSAMC20E16A","MicrochipATSAMC20E16A","Microchip","ARM CM0+",48,64,0,8,12,10,0,2,26,"No",4,4,0,"No",12,null,-40,125,2.7,5.5,32," 32/TQFP 32/VQFN",1.42,null,4,null,null,0,null,null," In Production ","",null,3,null,0," None","No"]
["ATSAMC21E15A","MicrochipATSAMC21E15A","Microchip","ARM CM0+",48,32,0,4,12,10,0,3,26,"No",4,4,0,"No",12,null,-40,125,2.7,5.5,32," 32/TQFP 32/VQFN",1.35,null,4,null,null,0,null,null," In Production ","",null,3,null,0," None","No"]
["ATSAMC21J16A","MicrochipATSAMC21J16A","Microchip","ARM CM0+",48,64,0,8,12,12,0,4,52,"No",6,6,0,"No",12,null,-40,125,2.7,5.5,64," 64/TQFP 64/VQFN",1.72,null,6,null,null,0,null,null," In Production ","",null,2,null,0," None","No"]
["ATSAMD20E16","MicrochipATSAMD20E16","Microchip","ARM CM0+",48,64,0,8,12,10,1,2,26,"No",4,4,0,"No",12,null,-40,85,1.62,3.63,32," 32/TQFP 32/VQFN",1.29,null,4,null,null,0,null,null," In Production ","",null,3,null,0," None","No"]
["ATSAMD20J15","MicrochipATSAMD20J15","Microchip","ARM CM0+",48,32,0,4,12,20,1,2,52,"No",6,6,0,"No",12,null,-40,85,1.62,3.63,64," 64/TQFP 64/UFBGA 64/VQFN",1.29,null,6,null,null,0,null,null," In Production ","",null,3,null,0," None","No"]
["ATSAMD51G18A","MicrochipATSAMD51G18A","Microchip","ARM CM4F",120,256,0,128,16,20,1,2,37,"No",4,6,1,"Yes",16,null,-40,125,1.71,3.6,48," 48/VQFN",2.5499999999999998,null,6,null,null,0,null,null," In Production ","",null,0,null,0," None","No"]
["ATSAMD51G19A","MicrochipATSAMD51G19A","Microchip","ARM CM4F",120,512,0,192,16,20,1,2,37,"No",4,6,1,"Yes",16,null,-40,125,1.71,3.6,48," 48/VQFN",2.83,null,6,null,null,0,null,null," In Production ","",null,0,null,0," None","No"]
["ATSAME54N19A","MicrochipATSAME54N19A","Microchip","ARM CM4F",120,512,0,192,12,28,1,2,81,"No",8,8,1,"Yes",31,null,-40,125,1.71,3.6,100," 100/TQFP",4,null,8,null,null,0,null,null," In Production ","",null,3,null,0," None","No"]
["ATSAME70N21","MicrochipATSAME70N21","Microchip","ARM CM7",300,2048,0,384,10,10,1,1,75,"No",3,4,1,"Yes",12,null,-40,105,1.7,3.6,100," 100/LQFP 100/TFBGA",8.73,null,8,null,null,0,null,null," In Production ","",null,3,null,0," None","No"]
["ATSAML21G16B","MicrochipATSAML21G16B","Microchip","ARM CM0+",48,64,2,12,16,14,2,2,37,"No",6,6,0,"Yes",12,null,-40,105,1.62,3.63,48," 48/TQFP 48/VQFN",2.23,null,6,null,null,0,null,null," In Production ","",null,3,null,0," None","No"]
["ATSAML22J16A","MicrochipATSAML22J16A","Microchip","ARM CM0+",32,64,2,8,16,16,0,2,50,"Yes",4,4,0,"Yes",10,null,-40,85,1.62,3.63,64," 64/TQFP 64/VQFN",2.23,null,4,null,null,0,null,null," In Production ","CAN,",null,2,null,0," None","No"]
["ATSAMS70N19","MicrochipATSAMS70N19","Microchip","ARM CM7",300,512,0,256,10,5,1,1,44,"No",2,1,1,"Yes",12,null,-40,105,1.7,3.6,100," 100/LQFP 100/TFBGA 100/VFBGA",5.86,null,5,null,null,0,null,null," In Production ","",null,2,null,0," None","No"]
["ATSAMV70N20","MicrochipATSAMV70N20","Microchip","ARM CM7",300,1024,0,384,10,10,1,1,75,"No",3,4,2,"Yes",12,null,-40,105,1.7,3.6,100," 100/LQFP 100/TFBGA",6.73,null,8,null,null,0,null,null," In Production ","",null,2,null,0," None","No"]
["R5F104LGAFA","RenesasR5F104LGAFA","Renesas","RL78",32,128,8,16,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LGAFB","RenesasR5F104LGAFB","Renesas","RL78",32,128,8,16,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LJAFA","RenesasR5F104LJAFA","Renesas","RL78",32,256,8,24,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104LKAFB","RenesasR5F104LKAFB","Renesas","RL78",32,384,8,32,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104MFAFA","RenesasR5F104MFAFA","Renesas","RL78",32,96,8,12,null,0,0,null,74,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,80,"80LQFP",null,null,4,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104MGDFB","RenesasR5F104MGDFB","Renesas","RL78",32,128,8,16,null,0,0,null,74,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,80,"80LFQFP",null,null,4,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104MJGFA","RenesasR5F104MJGFA","Renesas","RL78",32,256,8,24,null,0,0,null,74,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,80,"80LQFP",null,null,4,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104MLGFB","RenesasR5F104MLGFB","Renesas","RL78",32,512,8,48,null,0,0,null,74,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,80,"80LFQFP",null,null,4,null,null,null,null,null,"Mass Production","LIN,"]
["R5F104PJDFA","RenesasR5F104PJDFA","Renesas","RL78",32,256,8,24,null,0,0,null,92,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,100,"100LQFP",null,null,4,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F104PJDFB","RenesasR5F104PJDFB","Renesas","RL78",32,256,8,24,null,0,0,null,92,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,100,"100LFQFP",null,null,4,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F10EBCANA","RenesasR5F10EBCANA","Renesas","RL78",32,32,4,2,null,18,0,null,26,null,4,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,3.6,32,"32HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["ATTINY1626","MicrochipATTINY1626","Microchip"," 8bit AVR MCU",20,16,0.25,2,12,15,0,1,18,"No",1,1,0,"No",3,null,-40,125,1.8,5.5,null," Please call for package information",null,null,2,null,null,0,null,null," In Production ","",null,0,null,null," --- ","Yes"]
["ATTINY261","MicrochipATTINY261","Microchip"," 8bit AVR MCU",16,2,0.125,0.125,10,11,0,1,16,"No",1,1,0,"No",2,null,-40,150,2.7,5.5,32," 32/VQFN",1.34,null,0,null,null,0,null,null," In Production Consider: ATMEGA325A","",null,0,null,null," --- ","No"]
["ATTINY412","MicrochipATTINY412","Microchip"," 8bit AVR MCU",20,4,0.125,0.25,10,6,1,1,6,"No",1,1,0,"No",3,null,-40,125,1.8,5.5,8," 8/SOIC",0.32,null,1,null,null,0,null,null," In Production Consider: ATMEGA3290A","",null,0,null,null,"No","No"]
["ATtiny85","MicrochipATtiny85","Microchip"," 8bit AVR MCU",20,8,0.5,0.5,10,4,0,1,6,"No",1,1,0,"No",2,null,-40,85,1.8,5.5,8," 8/PDIP 8/SOIJ 20/WQFN",0.69,null,0,null,null,0,null,null," In Production Consider: ATMEGA645A","",null,0,null,null,"No","No"]
["ATxmega128C3","MicrochipATxmega128C3","Microchip"," 8bit AVR MCU",32,128,2,7.8125E-3,12,16,0,2,50,"No",2,5,0,"No",0,null,-40,85,1.6,3.6,64," 64/TQFP 64/VQFN",3.27,null,3,null,null,0,null,null," In Production ","SD/MMC,",null,0,null,null,"No","No"]
["AVR128DB32","MicrochipAVR128DB32","Microchip"," 8-bit AVR MCU",24,128," 512 / False",null,12,14,1,3,27,"No",2,2,0,"No",4,null,-40,125,1.8,5.5,32," Please call for package information","Call for pricing",null,3,null,null,0,null,null," In Production ","EtherNet",null,0,null,null,"No","No"]
["AVR128DB48","MicrochipAVR128DB48","Microchip"," 8-bit AVR MCU",24,128," 512 / False",null,12,18,1,3,41,"No",2,2,0,"No",6,null,-40,"125,85",1.8,5.5,48," Please call for package information","Call for pricing",null,5,null,null,0,null,null," In Production ","EtherNet",null,0,null,null,"No","No"]
["dsPIC33CH128MP208","MicrochipdsPIC33CH128MP208","Microchip"," 16bit dsPIC DSC",200,128,0,20,12,23,4,4,69,"No",3,3,3,"No",25,null,-40,150,3,3.6,80," 80/TQFP",3.58,null,3,null,null,0,null,null," In Production ","",null,2,null,null,"No","No"]
["dsPIC33CH64MP503","MicrochipdsPIC33CH64MP503","Microchip"," 16bit dsPIC DSC",200,64,0,20,12,17,4,4,27,"No",3,3,3,"No",25,null,-40,150,3,3.6,36," 36/UQFN",2.98,null,3,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33CK128MP508","MicrochipdsPIC33CK128MP508","Microchip"," 16bit dsPIC DSC",100,128,0,16,12,24,3,3,69,"No",3,3,3,"No",14,null,-40,150,3,3.6,80," 80/TQFP",3.15,null,3,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33CK256MP508","MicrochipdsPIC33CK256MP508","Microchip"," 16bit dsPIC DSC",100,256,0,24,12,24,3,3,69,"No",3,3,3,"No",14,null,-40,150,3,3.6,80," 80/TQFP",3.36,null,3,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33CK64MP208","MicrochipdsPIC33CK64MP208","Microchip"," 16bit dsPIC DSC",100,64,0,8,12,24,3,3,69,"No",3,3,3,"No",14,null,-40,150,3,3.6,80," 80/TQFP",2.73,null,3,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33EP128MC506","MicrochipdsPIC33EP128MC506","Microchip"," 16bit dsPIC DSC",70,128,0,16,12,16,1,4,53,"No",2,2,0,"No",7,null,-40,150,3,3.6,64," 64/QFN 64/TQFP",2.52,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33EP32GP502","MicrochipdsPIC33EP32GP502","Microchip"," 16bit dsPIC DSC",70,32,0,4,12,6,1,3,21,"No",2,2,0,"No",7,null,-40,125,3,3.6,28," 28/QFNS 28/SOIC 28/SPDIP 28/SSOP",1.58,null,2,null,null,0,null,null," In Production ","CAN,",null,0,null,null,"No","No"]
["dsPIC33EP32GP503","MicrochipdsPIC33EP32GP503","Microchip"," 16bit dsPIC DSC",70,32,0,4,12,8,1,4,25,"No",2,2,0,"No",7,null,-40,150,3,3.6,36," 36/UQFN 36/VTLA",1.61,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33EP512GP506","MicrochipdsPIC33EP512GP506","Microchip"," 16bit dsPIC DSC",70,512,0,48,12,16,1,4,53,"No",2,2,0,"No",7,null,-40,150,3,3.6,64," 64/QFN 64/TQFP",3.36,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33EP64GS502","MicrochipdsPIC33EP64GS502","Microchip"," 16bit dsPIC DSC",70,64,0,8,12,12,4,4,21,"No",2,2,0,"No",7,null,-40,125,3,3.6,28," 28/QFNS 28/SOIC 28/UQFN",3.05,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33EP64MC202","MicrochipdsPIC33EP64MC202","Microchip"," 16bit dsPIC DSC",70,64,0,8,12,6,1,3,21,"No",2,2,0,"No",7,null,-40,150,3,3.6,28," 28/QFNS 28/SOIC 28/SPDIP 28/SSOP",1.65,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33EV128GM003","MicrochipdsPIC33EV128GM003","Microchip"," 16bit dsPIC DSC",70,128,0,8,12,13,1,5,25,"No",1,2,0,"No",7,null,-40,150,4.5,5.5,36," 36/UQFN",2.21,null,2,null,null,0,null,null," In Production ","CAN,",null,0,null,null,"No","No"]
["dsPIC33EV32GM106","MicrochipdsPIC33EV32GM106","Microchip"," 16bit dsPIC DSC",70,32,0,4,12,36,1,5,53,"No",1,2,0,"No",7,null,-40,150,4.5,5.5,64," 64/QFN 64/TQFP",2.4500000000000002,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33FJ06GS001","MicrochipdsPIC33FJ06GS001","Microchip"," 16bit dsPIC DSC",40,6,0,0.25,10,6,2,2,13,"No",1,1,0,"No",2,null,-40,125,3,3.6,18," 18/PDIP 18/SOIC 20/SSOP",1.61,null,1,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33FJ128GP710A","MicrochipdsPIC33FJ128GP710A","Microchip"," 16bit dsPIC DSC",40,128,0,16,12,32,0,0,85,"No",2,2,1,"No",13,null,-40,150,3,3.6,100," 100/TQFP",4.8600000000000003,null,2,null,null,0,null,null," In Production ","CAN,",null,0,null,null,"No","No"]
["dsPIC33FJ128MC802","MicrochipdsPIC33FJ128MC802","Microchip"," 16bit dsPIC DSC",40,128,0,16,12,6,1,2,21,"No",1,2,0,"No",7,null,-40,150,3,3.6,28," 28/QFNS 28/SOIC 28/SPDIP",3.82,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33FJ32GP202","MicrochipdsPIC33FJ32GP202","Microchip"," 16bit dsPIC DSC",40,32,0,2,12,10,0,0,21,"No",1,1,0,"No",4,null,-40,125,3,3.6,28," 28/QFNS 28/SOIC 28/SPDIP 28/SSOP",2.5299999999999998,null,1,null,null,0,null,null," In Production ","CAN,",null,0,null,null,"No","No"]
["dsPIC33FJ64GP306A","MicrochipdsPIC33FJ64GP306A","Microchip"," 16bit dsPIC DSC",40,64,0,16,12,18,0,0,53,"No",2,2,1,"No",13,null,-40,125,3,3.6,64," 64/QFN 64/TQFP",3.53,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33FJ64GS608","MicrochipdsPIC33FJ64GS608","Microchip"," 16bit dsPIC DSC",40,64,0,9,10,18,4,4,69,"No",2,2,0,"No",7,null,-40,125,3,3.6,80," 80/TQFP",4.34,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["dsPIC33FJ64MC802","MicrochipdsPIC33FJ64MC802","Microchip"," 16bit dsPIC DSC",40,64,0,16,12,6,1,2,21,"No",1,2,0,"No",7,null,-40,150,3,3.6,28," 28/QFNS 28/SOIC 28/SPDIP",3.5,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["PIC12F1501","MicrochipPIC12F1501","Microchip"," 8bit PIC MCU",20,1.75,0,6.25E-2,10,4,1,1,6,"No",0,0,0,"No",3,null,-40,125,1.8,5.5,8," 8/DFN 8/MSOP 8/PDIP 8/SOIC 8/UDFN",0.36,null,0,null,null,0,null,null," In Production ","CAN,",null,0,null,null,"No","No"]
["PIC16F15225","MicrochipPIC16F15225","Microchip"," 8-bit PIC MCU",32,14," 0 / False",null,10,9,0,0,12,"No",1,1,0,"No",3,null,-40,"125,85",1.8,5.5,14," Please call for package information","Call for pricing",null,1,null,null,0,null,null," In Production ","CAN,EtherNet",null,0,null,null,"No","No"]
["PIC16F1823","MicrochipPIC16F1823","Microchip"," 8bit PIC MCU",32,3.5,0.25,0.125,10,8,1,2,12,"No",1,1,0,"No",3,null,-40,125,1.8,5.5,14," 14/PDIP 14/SOIC 14/TSSOP 16/QFN 16/UQFN",0.77,null,1,null,null,0,null,null," In Production ","CAN,",null,0,null,null,"No","No"]
["PIC16F527","MicrochipPIC16F527","Microchip"," 8bit PIC MCU",20,1.5,6.25E-2,6.640625E-2,8,8,0,2,18,"No",0,0,0,"No",1,null,-40,125,2,5.5,20," 20/PDIP 20/QFN 20/SOIC 20/SSOP 20/UQFN 28/SPDIP",0.46,null,0,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["PIC16F753","MicrochipPIC16F753","Microchip"," 8bit PIC MCU",20,3.5,0,0.125,10,8,1,2,11,"No",0,0,0,"No",4,null,-40,125,2,5.5,14," 14/PDIP 14/SOIC 14/TSSOP 16/QFN",0.63,null,0,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["PIC18F04Q40","MicrochipPIC18F04Q40","Microchip"," 8-bit PIC MCU",64,16," 512 / False",null,12,11,2,2,12,"No",1,2,0,"No",5,null,-40,"85",1.8,5.5,14," Please call for package information","Call for pricing",null,3,null,null,0," No",null," In Production ",null,null,0,null,null,"No","No"]
["PIC18F14Q41","MicrochipPIC18F14Q41","Microchip"," 8-bit PIC MCU",64,16," 512 / False",null,12,11,2,2,18,"No",1,2,0,"No",5,null,-40,"85",1.8,5.5,20," Please call for package information","Call for pricing",null,3,null,null,0,"  ",null," Future Product ",null,null,0,null,null,"No","No"]
["PIC18F2553","MicrochipPIC18F2553","Microchip"," 8bit PIC MCU",48,32,0.25,2,10,10,0,2,24,"No",1,1,0,"Yes",4,null,-40,85,2,5.5,28," 28/SOIC 28/SPDIP",4.12,null,1,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["PIC18F4450","MicrochipPIC18F4450","Microchip"," 8bit PIC MCU",48,16,0,0.75,10,13,0,0,34,"No",0,0,0,"Yes",3,null,-40,85,2,5.5,40," 40/PDIP 44/QFN 44/TQFP",2.39,null,1,null,null,0,null,null," In Production ","CAN,",null,0,null,null,"No","No"]
["PIC18F46J11","MicrochipPIC18F46J11","Microchip"," 8bit PIC MCU",48,64,0,3.7109375,10,13,0,2,34,"No",2,2,0,"No",5,null,-40,85,2,3.6,44," 44/QFN 44/TQFP",2.37,null,2,null,null,0,null,null," In Production ","CAN,",null,0,null,null,"No","No"]
["PIC18F66K22","MicrochipPIC18F66K22","Microchip"," 8bit PIC MCU",64,64,1,3.771484375,12,16,0,3,53,"No",2,2,0,"No",11,null,-40,125,1.8,5.5,64," 64/QFN 64/TQFP",2.7,null,2,null,null,0,null,null," Future Product ","SD/MMC,CAN,",null,0,null,null,"No","No"]
["PIC18F86J72","MicrochipPIC18F86J72","Microchip"," 8bit PIC MCU",48,64,0,3.8310546875,16,2,0,2,51,"Yes",1,1,0,"No",4,null,-40,85,2,3.6,80," 80/TQFP",4.12,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["PIC24F16KM104","MicrochipPIC24F16KM104","Microchip"," 16bit PIC MCU",32,16,0.5,1,12,22,0,1,38,"No",1,1,0,"No",7,null,-40,125,1.8,5.5,44," 44/TQFP",2.06,null,1,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["PIC24FJ128GA306","MicrochipPIC24FJ128GA306","Microchip"," 16bit PIC MCU",32,128,0,8,12,16,0,3,53,"Yes",2,2,0,"No",28,null,-40,85,2,3.6,64," 64/QFN 64/TQFP",2.4500000000000002,null,4,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["PIC24FJ128GL406","MicrochipPIC24FJ128GL406","Microchip"," 16-bit PIC MCU",32,128," 0 / True",null,12,16,1,3,54,"Yes",3,4,4,"No",31,null,-40,85,2,3.6,64," 64/QFN, 64/TQFP",2.1,null,6,null,null,0,null,null," In Production ","EtherNet",null,0,null,null,"No","No"]
["PIC24FJ256GA406","MicrochipPIC24FJ256GA406","Microchip"," 16bit PIC MCU",32,256,0,16,12,16,1,3,53,"Yes",3,4,3,"No",46,null,-40,85,2,3.6,64," 64/QFN 64/TQFP",3.44,null,6,null,null,0,null,null," In Production ","",null,0,null,null,"No","No"]
["R5F10EGCAFB","RenesasR5F10EGCAFB","Renesas","RL78",32,32,4,2,null,24,0,null,42,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,3.6,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10EGEANA","RenesasR5F10EGEANA","Renesas","RL78",32,64,4,4,null,24,0,null,42,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,3.6,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F11AGJDNB","RenesasR5F11AGJDNB","Renesas","RL78",32,256,8,20,null,0,0,null,32,null,3,0,null,null,16,"12bit Interval Timer x 1 ch",-40,85,1.6,3.6,48,"48HWQFN",null,null,2,null,null,null,null,null,"Mass Production",""]
["R5F11B7CGNA","RenesasR5F11B7CGNA","Renesas","RL78",32,32,4,5.5,null,0,0,null,20,null,4,null,null,null,13,"12bit interval timer",-40,105,1.6,5.5,24,"24HWQFN",null,"IrDA x 1ch",3,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,"]
["R5F11EB8AFP","RenesasR5F11EB8AFP","Renesas","RL78",24,8,0,1.5,null,0,0,null,28,null,1,0,null,null,11,"12bit Interval Timer x 1 ch",-40,85,2.7,5.5,32,"32LQFP",null,null,2,null,null,null,null,null,"Mass Production",""]
["R5F11NLGAFB","RenesasR5F11NLGAFB","Renesas","RL78",24,128,4,5.5,null,0,1,null,36,null,1,1,null,null,11,"12bit Interval Timer x 1 ch",-40,85,2.4,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F107ACGSP","RenesasR5F107ACGSP","Renesas","RL78",32,32,4,2,null,0,0,null,26,null,1,0,null,null,12,"Interval Timer x 1 ch",-40,105,2.7,5.5,30,"30LSSOP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10NMGDFB","RenesasR5F10NMGDFB","Renesas","RL78",24,128,2,8,null,0,0,null,52,null,3,0,null,null,12,"12bit Interval Timer, Highaccuracy RTC",-40,85,1.7,5.5,80,"80LFQFP",null,"IrDA 1ch",3,null,null,null,null,null,"Mass Production","LIN,",null,null,null,"34 seg X 4 com/32 seg X 6 com/30 seg x 8 com"]
["R5F1177AGNA","RenesasR5F1177AGNA","Renesas","RL78",24,16,2,2,null,6,0,null,18,null,2,0,null,null,4,"12bit Interval Timer x 1 ch<br>8bit Interval Timer x 4 ch<br>TAU x 4ch",-40,105,1.6,3.6,24,"24HWQFN",null,null,1,null,null,null,null,null,"Mass Production",""]
["R5F117GCGFB","RenesasR5F117GCGFB","Renesas","RL78",24,32,2,3,null,17,0,null,42,null,2,1,null,null,4,"12bit Interval Timer x 1 ch<br>8bit Interval Timer x 4 ch<br>TAU x 4ch",-40,105,1.6,3.6,48,"48LFQFP",null,null,1,null,null,null,null,null,"Mass Production",""]
["R5F10RFAAFP","RenesasR5F10RFAAFP","Renesas","RL78",24,16,2,1,null,0,0,null,29,null,1,0,null,null,12,"Remote Control Output<br>12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,1,null,null,null,null,null,"Mass Production(*)","LIN,",null,null,null,"22 seg. X 4 com./18 seg. X 8 com."]
["R5F10RGCGFB","RenesasR5F10RGCGFB","Renesas","RL78",24,32,2,1.5,null,0,0,null,33,null,1,0,null,null,12,"Remote Control Output<br>12bit Interval Timer x 1 ch",-40,105,1.6,5.5,48,"48LFQFP",null,null,1,null,null,null,null,null,"Mass Production(*)","LIN,",null,null,null,"26 seg. X 4 com./22 seg. X 8 com."]
["R5F10RLCAFA","RenesasR5F10RLCAFA","Renesas","RL78",24,32,2,1.5,null,0,0,null,47,null,1,0,null,null,12,"Remote Control Output<br>12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,1,null,null,null,null,null,"Mass Production(*)","LIN,",null,null,null,"39 seg. X 4 com./35 seg. X 8 com."]
["R5F10WLGAFA","RenesasR5F10WLGAFA","Renesas","RL78",24,128,4,8,null,0,0,null,49,null,2,2,null,null,8,"Remote Control Output",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,",null,null,null,"36 seg. X 4 com./32 seg. X 8 com."]
["R5F10WMDAFA","RenesasR5F10WMDAFA","Renesas","RL78",24,48,4,2,null,0,0,null,65,null,2,2,null,null,8,"Remote Control Output",-40,85,1.6,5.5,80,"80LQFP",null,null,4,null,null,null,null,null,"Mass Production","LIN,",null,null,null,"51 seg. X 4 com./47 seg. X 8 com."]
["R5F11MMEAFB","RenesasR5F11MMEAFB","Renesas","RL78",24,64,8,5.5,null,10,2,null,59,null,5,1,null,null,10,0,-40,85,1.8,3.6,80,"80LFQFP",null,null,4,null,null,null,null,null,"Mass Production","LIN,",null,null,null,"32 seg. X 4 com./28 seg. X 8 com."]
["R5F110MGAFB","RenesasR5F110MGAFB","Renesas","RL78",24,128,8,12,null,7,0,null,59,null,5,4,null,null,8,"Remote Control Output",-40,85,1.6,3.6,80,"80LFQFP",null,null,4,null,null,null,null,null,"Mass Production","LIN,",null,null,null,"40seg x 8com./44seg x 4com."]
["R5F110NFGLA","RenesasR5F110NFGLA","Renesas","RL78",24,96,8,10,null,9,0,null,59,null,5,4,null,null,8,"Remote Control Output",-40,105,1.6,3.6,85,"85VFLGA",null,null,4,null,null,null,null,null,"Mass Production","LIN,",null,null,null,"40seg x 8com./44seg x 4com."]
["R5F110PHAFB","RenesasR5F110PHAFB","Renesas","RL78",24,192,8,16,null,11,0,null,77,null,5,4,null,null,8,"Remote Control Output",-40,85,1.6,3.6,100,"100LFQFP",null,null,4,null,null,null,null,null,"Mass Production","LIN,",null,null,null,"52seg x 8com/56seg x 4com"]
["R5F111MGGFB","RenesasR5F111MGGFB","Renesas","RL78",24,128,8,12,null,9,0,null,59,null,5,4,null,null,8,"Remote Control Output",-40,105,1.6,3.6,80,"80LFQFP",null,null,4,null,null,null,null,null,"Mass Production","LIN,",null,null,null,"40seg x 8com./44seg x 4com."]
["R5F111PEGFB","RenesasR5F111PEGFB","Renesas","RL78",24,64,8,8,null,13,0,null,77,null,5,4,null,null,8,"Remote Control Output",-40,105,1.6,3.6,100,"100LFQFP",null,null,4,null,null,null,null,null,"Mass Production","LIN,",null,null,null,"52seg x 8com/56seg x 4com"]
["R5F51101AGNE","RenesasR5F51101AGNE","Renesas","RX",32,32,0,10,null,10,0,null,36,null,4,4,null,null,6,null,-40,105,1.8,3.6,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F51103AGFK","RenesasR5F51103AGFK","Renesas","RX",32,64,0,10,null,14,0,null,52,null,4,4,null,null,6,null,-40,105,1.8,3.6,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F51104AGNE","RenesasR5F51104AGNE","Renesas","RX",32,96,0,16,null,10,0,null,36,null,4,4,null,null,6,null,-40,105,1.8,3.6,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F51105AGNE","RenesasR5F51105AGNE","Renesas","RX",32,128,0,16,null,10,0,null,36,null,4,4,null,null,6,null,-40,105,1.8,3.6,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F5110JADNE","RenesasR5F5110JADNE","Renesas","RX",32,16,0,8,null,10,0,null,36,null,4,4,null,null,6,null,-40,85,1.8,3.6,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F51303AGFL","RenesasR5F51303AGFL","Renesas","RX",32,64,8,10,null,10,0,null,39,null,5,5,null,null,12,"16bit Timers is included Low Power Timer x 1ch",-40,105,1.8,5.5,48,"48LFQFP",null,null,4,null,null,null,null,null,"Mass Production","IEBus,"]
["STM32F031F6","STSTM32F031F6","ST","ARM CM0",48,32,null,4,0,9,0,0,15,"No",1,1,1,"No",5,"24bit downcounter,2xWDG,RTC",-40,"105,85",2,3.6,20,"TSSOP 20",null,1,null,1.4,250,null,null,null,"Active",null,"Mainstream ARM CM0 Access line MCU with 32 Kbytes Flash, 48 MHz CPU, motor control",0]
["STM32F042F6","STSTM32F042F6","ST","ARM CM0",48,32,null,6,12,9,0,0,16,"No",1,1,1,"Yes",5,"24bit downcounter,2xWDG,RTC",-40,"105,85",2,3.6,20,"TSSOP 20",null,2,null,1.4,250,null,null,null,"Active",null,"Mainstream ARM CM0 USB line MCU with 32 Kbytes Flash, 48 MHz CPU, USB, CAN and CEC functions",0,null,null,"USB Device"]
["STM32F058T8","STSTM32F058T8","ST","ARM CM0",48,64,null,8,12,10,0,2,28,"No",1,1,1,"No",7,"24bit downcounter,2xWDG,RTC",-40,85,1.65,1.95,36,"WLCSP 36L P 0.4 MM DIE 440",null,2,null,1.4,250,null,null,null,"Active",null,"Mainstream ARM CM0 Lowvoltage line 1,8V MCU with 64 Kbytes Flash, 48 MHz CPU and CEC functions",0]
["STM32F071VB","STSTM32F071VB","ST","ARM CM0",48,128,null,16,12,16,2,2,87,"No",2,2,2,"No",8,"24bit downcounter,2xWDG,RTC",-40,85,2,3.6,100,"LQFP 100 14x14x1.4,UFBGA 100 7x7x0.6",null,4,null,1.5,260,null,null,null,"Active",null,"Mainstream ARM CM0 Access line MCU with 128 Kbytes Flash, 48 MHz CPU and CEC functions",0]
["STM32F091RC","STSTM32F091RC","ST","ARM CM0",48,256,null,32,12,16,2,2,52,"No",2,2,2,"No",8,"24bit downcounter,2xWDG,RTC",-40,"105,85",2,3.6,64,"LQFP 64 10x10x1.4,UFBGA 5X5X0.6 64L P 0.5 MM,WLCSP 64L DIE 442 P 0.4 MM",null,8,null,1.3,306,null,null,null,"Active",null,"Mainstream ARM CM0 Access line MCU with 256 Kbytes Flash, 48 MHz CPU, CAN and CEC functions",0]
["STM32F100CB","STSTM32F100CB","ST","ARM CM3",24,128,null,8,12,10,2,0,37,"No",2,2,null,"No",7,"24bit down counter,2xWDG,RTC",-40,"105,85",2,3.6,48,"LQFP 48 7x7x1.4",null,3,null,3.1,358,null,null,null,"Active",null,"Mainstream Value line, ARM CM3 MCU with 128 Kbytes Flash, 24 MHz CPU, motor control and CEC functions",0]
["STM32F100ZC","STSTM32F100ZC","ST","ARM CM3",24,256,null,24,12,16,2,0,112,"No",2,3,null,"No",11,"24bit down counter,2xWDG,RTC",-40,85,2,3.6,144,"LQFP 144 20x20x1.4",null,5,null,3.1,396,null,null,null,"Active",null,"Mainstream Value line, ARM CM3 MCU with 256 Kbytes Flash, 24 MHz CPU, motor control and CEC functions",0]
["STM32F101R8","STSTM32F101R8","ST","ARM CM3",36,64,null,10,12,16,0,0,51,"No",2,2,null,"No",3,"24bit down counter,2xWDG,RTC",-40,85,2,3.6,64,"LQFP 64 10x10x1.4",null,3,null,3.2,391,null,null,null,"Active",null,"Mainstream Access line, ARM CM3 MCU with 64 Kbytes Flash, 36 MHz CPU",0]
["STM32F101T8","STSTM32F101T8","ST","ARM CM3",36,64,null,10,12,10,0,0,26,"No",1,1,null,"No",3,"24bit down counter,2xWDG,RTC",-40,85,2,3.6,36,"VFQFPN 36 6x6x10",null,2,null,3.2,391,null,null,null,"Active",null,"Mainstream Access line, ARM CM3 MCU with 64 Kbytes Flash, 36 MHz CPU",0]
["STM32F101ZG","STSTM32F101ZG","ST","ARM CM3",36,1024,null,80,12,16,2,0,112,"No",2,3,null,"No",12,"24bit down counter,2xWDG,RTC",-40,85,2,3.6,144,"LQFP 144 20x20x1.4",null,3,2,3.2,433,null,null,null,"Active",null,"Mainstream Access line, ARM CM3 MCU with 1 Mbyte Flash, 36 MHz CPU",0]
["STM32F103RE","STSTM32F103RE","ST","ARM CM3",72,512,null,64,12,16,2,0,51,"No",2,3,2,"Yes",8,"24bit down counter,2xWDG,RTC",-40,"105,85",2,3.6,64,"LQFP 64 10x10x1.4,WLCSP 64",null,3,2,3.2,421,null,null,null,"Active",null,"Mainstream Performance line, ARM CM3 MCU with 512 Kbytes Flash, 72 MHz CPU, motor control, USB and CAN",0,null,null,"USB Device"]
["STM32F103VF","STSTM32F103VF","ST","ARM CM3",72,768,null,96,12,16,2,0,80,"No",2,3,2,"Yes",14,"24bit down counter,2xWDG,RTC",-40,"105,85",2,3.6,100,"LQFP 100 14x14x1.4",null,3,2,3.2,421,null,null,null,"Active",null,"Mainstream Performance line, ARM CM3 MCU with 768 Kbytes Flash, 72MHz CPU, motor control, USB and CAN",0,null,null,"USB Device"]
["STM32F107RB","STSTM32F107RB","ST","ARM CM3",72,128,null,64,12,16,2,0,51,"No",1,3,2,"Yes",7,"24bit down counter,2xWDG,RTC",-40,"105,85",2,3.6,64,"LQFP 64 10x10x1.4",null,3,2,3.6,393,null,null,null,"Active",null,"Mainstream Connectivity line, ARM CM3 MCU with 128 Kbytes Flash, 72 MHz CPU, Ethernet MAC, CAN and USB 2.0 OTG",0,null,null,"USB OTG FS"]
["STM32F205VB","STSTM32F205VB","ST","ARM CM3",120,128,null,64,12,16,2,0,82,"No",3,3,2,"Yes",12,"24bit down counter,2xWDG,RTC",-40,85,1.8,3.6,100,"LQFP 100 14x14x1.4",null,4,2,3.3,188,null,null,null,"Active",null,"Highperformance ARM CM3 MCU with 128 Kbytes Flash, 120 MHz CPU, ART Accelerator",0,null,null,"USB OTG FS + USB OTG FS/HS"]
["STM32F207VC","STSTM32F207VC","ST","ARM CM3",120,256,null,128,12,16,2,0,82,"No",2,3,2,"Yes",12,"24bit down counter,2xWDG,RTC",-40,"105,85",1.8,3.6,100,"LQFP 100 14x14x1.4",null,4,2,3.3,188,null,null,null,"Active",null,"Highperformance ARM CM3 MCU with 256 Kbytes Flash, 120 MHz CPU, ART Accelerator, Ethernet",0,null,null,"USB OTG FS + USB OTG FS/HS"]
["STM32F215RG","STSTM32F215RG","ST","ARM CM3",120,1024,null,128,12,16,2,0,51,"No",3,3,2,"Yes",12,"24bit down counter,2xWDG,RTC",-40,85,1.8,3.6,64,"LQFP 64 10x10x1.4",null,4,2,3.3,188,null,"AES,DES/TDES,MD5,SHA","true","Active",null,"Highperformance ARM CM3 MCU with 1 Mbyte Flash, 120 MHz CPU, ART Accelerator, HW crypto",0,null,null,"USB OTG FS + USB OTG FS/HS"]
["STM32F217ZE","STSTM32F217ZE","ST","ARM CM3",120,512,null,128,12,24,2,0,114,"No",2,3,2,"Yes",12,"24bit down counter,2xWDG,RTC",-40,"105,85",1.8,3.6,144,"LQFP 144 20x20x1.4",null,4,2,3.3,188,null,"AES,DES/TDES,MD5,SHA","true","Active",null,"Highperformance ARM CM3 MCU with 512 Kbytes Flash, 120 MHz CPU, ART Accelerator, Ethernet, HW crypto",0,null,null,"USB OTG FS + USB OTG FS/HS"]
["STM32F302K8","STSTM32F302K8","ST","ARM CM4F",72,64,null,16,12,8,1,2,24,"No",3,2,2,"Yes",5,"2xWDG,RTC,SysTick",-40,"105,85",2,3.6,32,"UFQFPN 32 5x5x0.55",null,2,null,1.3,349,null,null,null,"Active",null,"Mainstream Mixed signals MCUs ARM CM4 core with DSP and FPU, 64 Kbytes Flash, 72 MHz CPU, 12bit ADC 5 MSPS, Comparator, OpAmp","1",null,null,"USB Device"]
["STM32F303RB","STSTM32F303RB","ST","ARM CM4F",72,128,null,40,12,22,2,7,52,"No",2,3,2,"Yes",9,"2xWDG,RTC,SysTick",-40,"105,85",2,3.6,64,"LQFP 64 10x10x1.4",null,3,2,1.3,392,null,null,null,"Active",null,"Mainstream Mixed signals MCUs ARM CM4 core with DSP and FPU, 128 Kbytes Flash, 72 MHz CPU, MPU, CCM, 12bit ADC 5 MSPS, PGA, comparators","4",null,null,"USB Device"]
["STM32F334C4","STSTM32F334C4","ST","ARM CM4F",72,16,null,16,12,15,3,3,37,"No",1,1,null,"No",7,"2xWDG,RTC,SysTick",-40,85,2,3.6,48,"LQFP 48 7x7x1.4",null,3,null,1.3,420,null,null,null,"Active",null,"Mainstream Mixed signals MCUs ARM CM4 core with DSP and FPU, 16 Kbytes Flash, 72 MHz CPU, CCM, 12bit ADC 5 MSPS, comparators, opamp, hr timer","1"]
["STM32F358RC","STSTM32F358RC","ST","ARM CM4F",72,256,null,48,12,21,2,7,51,"No",2,3,2,"No",9,"2xWDG,RTC,SysTick",-40,85,1.65,1.95,64,"LQFP 64 10x10x1.4",null,3,2,0.87,368,null,null,null,"Active",null,"Mainstream Mixed signals MCUs ARM CM4 core with DSP and FPU, 256 Kbytes Flash, 72 MHz CPU, MPU, CCM, 12bit ADC 5Msps, PGA, comparators","4"]
["STM32F373VB","STSTM32F373VB","ST","ARM CM4F",72,128,null,24,16,16,3,2,84,"No",2,3,3,"Yes",12,"2xWDG,RTC,SysTick",-40,"105,85",2,3.6,100,"LQFP 100 14x14x1.4,UFBGA 100 7x7x0.6",null,3,null,1.3,417,null,null,null,"Active",null,"Mainstream Mixed signals MCUs ARM CM4 core with DSP and FPU, 128 KBytes Flash, 72 MHz CPU, MPU, 16bit ADC comparators",0,null,null,"USB Device"]
["STM32F401RE","STSTM32F401RE","ST","ARM CM4F",84,512,null,96,12,16,0,0,50,"No",3,3,2,"Yes",6,"24bit downcounter,2xWDG,RTC",-40,"105,85",1.7,3.6,64,"LQFP 64 10x10x1.4",null,3,null,2.8,137,null,null,null,"Active",null,"STM32 Dynamic Efficiency MCU, ARM CM4 core with DSP and FPU, up to 512 Kbytes Flash, 84 MHz CPU, Art Accelerator",0,null,null,"USB OTG FS"]
["STM32F405ZG","STSTM32F405ZG","ST","ARM CM4F",168,1024,null,192,12,24,2,0,114,"No",3,3,2,"Yes",12,"24bit down counter,2xWDG,RTC",-40,"105,85",1.8,3.6,144,"LQFP 144 20x20x1.4",null,4,2,3.3,215,null,null,"true","Active",null,"Highperformance foundation line, ARM CM4 core with DSP and FPU, 1 Mbyte Flash, 168 MHz CPU, ART Accelerator, FSMC",0,null,null,"USB OTG FS + USB OTG FS/HS"]
["STM32F410R8","STSTM32F410R8","ST","ARM CM4F",100,64,null,32,12,16,1,0,50,"No",3,3,3,"No",5,"24bit downcounter,2xWDG,RTC",-40,85,1.7,3.6,64,"LQFP 64 10x10x1.4",null,3,null,3.4,89,null,null,null,"Active",null,"STM32 Dynamic Efficiency MCU with BAM, Highperformance and DSP with FPU, ARM CM4 MCU with 64 Kbytes Flash, 100 MHz CPU, Art Accelerator",0]
["STM32F412RG","STSTM32F412RG","ST","ARM CM4F",100,1024,null,256,12,16,0,0,50,"No",4,5,5,"Yes",12,"2xWDG,RTC,SysTick",-40,85,1.7,3.6,64,"LQFP 64 10x10x1.4,WLCSP 64L DIE 441 P 0.4 MM",null,4,null,3.7,112,null,null,null,"Active",null,"STM32 Dynamic Efficiency MCU with BAM, Highperformance and DSP with FPU, ARM CM4 MCU with 1 Mbyte Flash, 100 MHz CPU, Art Accelerator, DFSDM",0,null,null,"USB OTG FS"]
["STM32F417VE","STSTM32F417VE","ST","ARM CM4F",168,512,null,192,12,16,2,0,82,"No",3,3,2,"Yes",12,"24bit down counter,2xWDG,RTC",-40,85,1.8,3.6,100,"LQFP 100 14x14x1.4",null,4,2,3.3,215,null,"AES,DES/TDES,HMAC,MD5,SHA","true","Active",null,"Highperformance foundation line, ARM CM4 core with DSP and FPU, 512 Kbytes Flash, 168 MHz CPU, ART Accelerator, Ethernet, FSMC, HW crypto",0,null,null,"USB OTG FS + USB OTG FS/HS"]
["STM32F427VG","STSTM32F427VG","ST","ARM CM4F",180,1024,null,256,12,16,2,0,82,"No",3,4,2,"Yes",12,"24bit down counter,2xWDG,RTC",-40,85,1.8,3.6,100,"LQFP 100 14x14x1.4",null,4,4,3.1,208,null,null,"true","Active",null,"Highperformance advanced line, ARM CM4 core with DSP and FPU, 1 Mbyte Flash, 180 MHz CPU, ART Accelerator, ChromART Accelerator, FSMC",0,null,null,"USB OTG FS + USB OTG FS/HS"]
["STM32F427ZI","STSTM32F427ZI","ST","ARM CM4F",180,2048,null,256,12,24,2,0,114,"No",3,6,2,"Yes",12,"24bit down counter,2xWDG,RTC",-40,"105,85",1.7,3.6,144,"LQFP 144 20x20x1.4",null,4,4,3.1,208,null,null,"true","Active",null,"Highperformance advanced line, ARM CM4 core with DSP and FPU, 2 Mbytes Flash, 180 MHz CPU, ART Accelerator, ChromART Accelerator, FMC with SDRAM",0,null,null,"USB OTG FS + USB OTG FS/HS"]
["R5F51305ADFL","RenesasR5F51305ADFL","Renesas","RX",32,128,8,16,null,10,0,null,39,null,5,5,null,null,12,"16bit Timers is included Low Power Timer x 1ch",-40,85,1.8,5.5,48,"48LFQFP",null,null,4,null,null,null,null,null,"Mass Production","IEBus,"]
["STM32F429VI","STSTM32F429VI","ST","ARM CM4F",180,2048,null,256,12,16,2,0,82,"Yes",3,4,2,"Yes",12,"24bit down counter,2xWDG,RTC",-40,85,1.8,3.6,100,"LQFP 100 14x14x1.4",null,4,4,3.1,208,null,null,null,"Active",null,"Highperformance advanced line, ARM CM4 core with DSP and FPU, 2 Mbytes Flash, 180 MHz CPU, ART Accelerator, ChromART Accelerator, FSMC, TFT",0,null,"LCD TFT Controller up to 1024x728","USB OTG FS + USB OTG FS/HS"]
["STM32F437ZG","STSTM32F437ZG","ST","ARM CM4F",180,1024,null,256,12,24,2,0,114,"No",3,6,2,"Yes",12,"24bit down counter,2xWDG,RTC",-40,85,1.7,3.6,144,"LQFP 144 20x20x1.4",null,4,4,3.1,208,null,"AES,DES/TDES,HMAC,MD5,SHA","true","Active",null,"Highperformance advanced line, ARM CM4 core with DSP and FPU, 1 Mbyte Flash, 180 MHz CPU, ART Accelerator, ChromART Accelerator, FMC with SDRAM, HW crypto",0,null,null,"USB OTG FS + USB OTG FS/HS"]
["STM32F439VG","STSTM32F439VG","ST","ARM CM4F",180,1024,null,256,12,16,2,0,82,"Yes",3,4,2,"Yes",12,"24bit down counter,2xWDG,RTC",-40,85,1.7,3.6,100,"LQFP 100 14x14x1.4",null,4,4,3.1,208,null,"AES,DES/TDES,HMAC,MD5,SHA","true","Active",null,"Highperformance advanced line, ARM CM4 core with DSP and FPU, 1 Mbyte Flash, 180 MHz CPU, ART Accelerator, ChromART Accelerator, FSMC, TFT, HW crypto",0,null,"LCD TFT Controller up to 1024x728","USB OTG FS + USB OTG FS/HS"]
["STM32F469AG","STSTM32F469AG","ST","ARM CM4F",180,1024,null,384,12,24,2,0,114,"Yes",3,6,2,"Yes",12,"24bit downcounter,2xWDG,RTC",-40,85,1.7,3.6,169,"UFBGA 7X7X0.6 169L P 0.5 MM,WLCSP 168L DIE 434 12X14 P 0.4MM",null,4,4,3.2,282,null,null,null,"Active",null,"Highperformance advanced line, ARM CM4 core with DSP and FPU, 1 Mbyte Flash, 180 MHz CPU, ART Accelerator, ChromART Accelerator, FMC with SDRAM, Dual QSPI, TFT, MIPIDSI",0,null,"LCD TFT Controller up to 1024x728,MIPI DSI","USB OTG FS + USB OTG FS/HS"]
["STM32F479IG","STSTM32F479IG","ST","ARM CM4F",180,1024,null,384,12,24,2,0,131,"Yes",3,6,2,"Yes",12,"24bit downcounter,2xWDG,RTC",-40,85,1.7,3.6,176,"BGA 176",null,4,4,3.2,282,null,"AES,DES/TDES,HMAC,MD5,SHA","true","Active",null,"Highperformance advanced line, ARM CM4 core with DSP and FPU, 1 Mbyte Flash, 180 MHz CPU, ART Accelerator, ChromART Accelerator, FMC with SDRAM, Dual QSPI, TFT, MIPIDSI, HW crypto",0,null,"LCD TFT Controller up to 1024x728,MIPI DSI","USB OTG FS + USB OTG FS/HS"]
["STM32F722VE","STSTM32F722VE","ST","ARM CM7",216,512,null,256,12,16,2,0,82,"No",4,4,3,"Yes",12,"24bit downcounter,2xWDG,RTC",-40,"105,85",1.7,3.6,100,"LQFP 100 14x14x1.4",null,4,4,2.5,435,null,null,"true","Active",null,"Highperformance and DSP with FPU, ARM CM7 MCU with 512 Kbytes Flash, 216 MHz CPU, Art Accelerator, L1 cache, SDRAM",0,null,null,"USB OTG FS + USB OTG FS/HS"]
["STM32F730R8","STSTM32F730R8","ST","ARM CM7",216,64,null,256,12,16,2,0,50,"No",4,4,3,"Yes",12,"24bit downcounter,2xWDG,RTC",-40,"105,85",1.7,3.6,64,"LQFP 64 10x10x1.4",null,4,4,2.5,472,null,"AES","true","Active",null,"Highperformance and DSP with FPU, ARM CM7 MCU with 64 Kbytes of Flash memory, 216 MHz CPU, Art Accelerator, L1 cache,  HW crypto,SDRAM",0,null,null,"USB OTG FS,USB OTG FS + USB OTG FS/HS"]
["STM32F733ZE","STSTM32F733ZE","ST","ARM CM7",216,512,null,256,12,16,2,0,112,"No",4,5,3,"Yes",12,"24bit downcounter,2xWDG,RTC",-40,"105,85",1.7,3.6,144,"LQFP 144 20x20x1.4,UFBGA 144 7x7x0.6",null,4,4,2.5,435,null,"AES","true","Active",null,"Highperformance and DSP with FPU, ARM CM7 MCU with 512 Kbytes Flash, 216 MHz CPU, Art Accelerator, L1 cache, SDRAM",0,null,null,"USB OTG FS + USB OTG FS/HS"]
["STM32F746VE","STSTM32F746VE","ST","ARM CM7",216,512,null,320,12,16,2,0,82,"Yes",4,4,3,"Yes",12,"24bit downcounter,2xWDG,RTC",-40,85,1.7,3.6,100,"LQFP 100 14x14x1.4,TFBGA 8X8 100L F10X10 0.8 MM PIT",null,4,4,2.9,472,null,null,"true","Active",null,"Highperformance and DSP with FPU, ARM CM7 MCU with 512 Kbytes Flash, 216 MHz CPU, Art Accelerator, L1 cache, TFT",0,null,"LCD TFT Controller up to 1024x728","USB OTG FS + USB OTG FS/HS"]
["STM32F756NG","STSTM32F756NG","ST","ARM CM7",216,1024,null,320,12,24,2,0,168,"Yes",4,6,3,"Yes",12,"24bit downcounter,2xWDG,RTC",-40,85,1.7,3.6,216,"TFBGA 13X13X1.2 216L P 0.8 MM",null,4,4,2.9,472,null,"AES,DES/TDES,HMAC,MD5,SHA","true","Active",null,"Highperformance and DSP with FPU, ARM CM7 MCU with 1 Mbyte Flash, 216 MHz CPU, Art Accelerator, L1 cache, HW crypto, SDRAM, TFT",0,null,"LCD TFT Controller up to 1024x728","USB OTG FS + USB OTG FS/HS"]
["STM32F767BG","STSTM32F767BG","ST","ARM CM7",216,1024,null,512,12,24,2,0,168,"Yes",4,6,3,"Yes",12,"24bit downcounter,2xWDG,RTC",-40,85,1.7,3.6,208,"LQFP 208 28x28x1.4",null,4,4,3.5,420,null,null,"true","Active",null,"Highperformance and DSP with FPU, ARM CM7 MCU with 1 Mbyte Flash, 216 MHz CPU, Art Accelerator, L1 cache, SDRAM, TFT, JPEG codec, DFSDM",0,null,"LCD TFT Controller up to 1024x728","USB OTG FS + USB OTG FS/HS"]
["STM32F767ZI","STSTM32F767ZI","ST","ARM CM7",216,2048,null,512,12,24,2,0,114,"Yes",4,6,3,"Yes",12,"24bit downcounter,2xWDG,RTC",-40,85,1.7,3.6,144,"LQFP 144 20x20x1.4",null,4,4,3.5,420,null,null,"true","Active",null,"Highperformance and DSP with FPU, ARM CM7 MCU with 2 Mbytes Flash, 216 MHz CPU, Art Accelerator, L1 cache, SDRAM, TFT, JPEG codec, DFSDM",0,null,"LCD TFT Controller up to 1024x728","USB OTG FS + USB OTG FS/HS"]
["STM32G030J6","STSTM32G030J6","ST","ARM CM0+",64,32,null,8,12,6,0,0,6,"No",2,2,1,"No",8,"32bit timer",-40,85,2,3.6,8,"SO8",0.36919999999999997,2,1,1.8,100,null,null,null,"Active",null,"Mainstream Value Line ARM CM0+ MCU with 32 Kbytes of Flash memory, 8 Kbytes RAM, 64 MHz CPU, 2x USART, timers, ADC, comm. I/F, 23.6V",0]
["STM32G031G8","STSTM32G031G8","ST","ARM CM0+",64,64,null,8,12,12,0,0,26,"No",2,2,1,"No",8,"32bit timer",-40,85,1.7,3.6,28,"UFQFPN 28 4x4x0.55",0.82420000000000004,2,1,1.8,100,null,null,null,"Active",null,"Mainstream ARM CM0+ MCU with 64 Kbytes of Flash memory, 8 Kbytes RAM, 64 MHz CPU, 2x USART, timers, ADC, comm. I/F, 1.73.6V",0]
["STM32G041C6","STSTM32G041C6","ST","ARM CM0+",64,64,null,8,12,16,0,0,44,"No",2,2,1,"No",8,"32bit timer",-40,85,1.7,3.6,48,"LQFP 48 7x7x1.4",1.0417000000000001,2,1,1.8,100,null,"AES",true,"Active",null,"Mainstream ARM CM0+ MCU with 64 Kbytes of Flash memory, 8 Kbytes RAM, 64 MHz CPU, 2x USART, timers, ADC, comm. I/F, AES256, 1.73.6V",0]
["STM32G070CB","STSTM32G070CB","ST","ARM CM0+",64,128,null,36,12,14,0,0,44,"No",2,2,1,"No",8,null,-40,85,2,3.6,48,"LQFP 48 7x7x1.4",0.75419999999999998,4,1,1.8,100,null,null,null,"Active",null,"Mainstream Value line, ARM CM0+ MCU with 128 Kbytes of Flash memory, 36 Kbytes RAM, 64 MHz CPU, 4x USART, timers, ADC, comm. I/F, 23.6V",0]
["STM32G071KB","STSTM32G071KB","ST","ARM CM0+",64,128,null,36,12,11,2,2,30,"No",2,2,1,"No",10,"32bit timer",-40,125,1.7,3.6,32,"LQFP 32 7x7x1.4,UFQFPN 32 5x5x0.55",1.4077999999999999,4,1,1.8,100,"HDMI CEC",null,null,"Active",null,"Mainstream ARM CM0+ MCU with 128 Kbytes of Flash memory, 36 Kbytes RAM, 64 MHz CPU, 4x USART, timers, ADC, DAC, comm. I/F including USB TypeC and Power Delivery Interface, 1.73.6V",0]
["STM32G431C8","STSTM32G431C8","ST","ARM CM4F",170,64,null,32,12,13,4,4,42,"No",3,3,2,"Yes",11,"2xWDG,PWM,RTC,SysTick",-40,"125,85",1.71,3.6,48,"LQFP 48 7x7x1.4,UFQFPN 48 7x7x0.55",null,3,null,0.8,138,null,null,null,"Active",null,"Mainstream ARM CM4 core with DSP and FPU, 170MHz with 64Kbytes of Flash memory, Math Accelerator, Medium Analog level integration","3",null,null,"USB Device,USB TypeC"]
["STM32G441RB","STSTM32G441RB","ST","ARM CM4F",170,128,null,32,12,18,4,4,86,"No",3,3,2,"Yes",11,"2xWDG,HR Timer,PWM,RTC,SysTick",-40,"125,85",1.71,3.6,64,"LQFP 64 10x10x1.4",null,3,1,0.8,138,null,null,null,"Active",null,"Mainstream ARM CM4 core with DSP and FPU, 170MHz with 128Kbytes of Flash memory, Math Accelerator, Medium Analog level integration","3",null,null,"USB Device,USB TypeC"]
["STM32G473RC","STSTM32G473RC","ST","ARM CM4F",170,256,null,128,12,26,7,7,52,"No",4,3,2,"Yes",11,"2xWDG,PWM,RTC,SysTick",-40,85,1.71,3.6,64,"LQFP 64 10x10x1.4",null,3,3,0.9,162,null,null,null,"Active",null,"Mainstream ARM CM4 core with DSP and FPU, 170MHz with 256Kbytes of Flash memory, Math Accelerator, High Analog level integration","6",null,null,"USB Device,USB TypeC"]
["STM32G484CE","STSTM32G484CE","ST","ARM CM4F",170,512,null,128,12,21,7,7,42,"No",4,3,2,"Yes",12,"2xWDG,PWM,RTC,SysTick",-40,"125,85",1.71,3.6,48,"LQFP 48 7x7x1.4,UFQFPN 48 7x7x0.55",null,3,1,0.9,162,null,"AES",null,"Active",null,"Mainstream ARM CM4 core with DSP and FPU, 170MHz with 512Kbytes of Flash memory, Math Accelerator, HR Timer, High Analog level integration, Crypto AES256","6",null,null,"USB Device,USB TypeC"]
["STM32H742XI","STSTM32H742XI","ST","ARM CM7",480,2048,null,692,0,null,2,2,168,"No",4,6,3,"Yes",18,"24bit downcounter,2xWDG,HR Timer,LP timer,RTC",-40,85,1.62,3.6,240,"TFBGA 14X14X1.2 P 0.8 240+25L",null,4,5,4,270,null,null,"true","Active",null,"Highperformance and DSP with DPFPU, ARM CM7 MCU with 2MBytes of Flash memory, 692KB RAM, 480 MHz CPU, L1 cache, external memory interface, subset of peripherals","2",null,null,"USB OTG FS,USB OTG FS + USB OTG FS/HS"]
["STM32H743VG","STSTM32H743VG","ST","ARM CM7",480,1024,null,1024,0,null,2,2,82,"No",4,6,3,"Yes",18,"24bit downcounter,2xWDG,HR Timer,RTC",-40,85,"1.62,1.71",3.6,100,"LQFP 100 14x14x1.4,TFBGA 8X8 100L F10X10 0.8 MM PIT",null,4,5,4,270,null,null,"true","Active",null,"Highperformance and DSP with DPFPU, ARM CM7 MCU with 1MBytes of Flash memory, 1MB RAM, 480 MHz CPU, L1 cache, external memory interface, JPEG codec, large set of peripherals","2",null,null,"USB OTG FS,USB OTG FS + USB OTG FS/HS"]
["STM32H745ZI","STSTM32H745ZI","ST","ARM CM7+M4 Dual",480,2048,null,1024,0,null,2,2,null,"No",4,6,3,"Yes",18,"24bit downcounter,2xWDG,HR Timer,RTC",-40,"125,85",1.62,3.6,144,"LQFP 144 20x20x1.4",null,4,5,4,270,null,null,"true","Active",null,"Highperformance and DSP with DPFPU, Dual core ARM CM7+ CortexM4 MCU with 2MBytes of Flash memory, 1MB RAM, 480 MHz CPU, Art Accelerator, L1 cache, external memory interface, large set of peripherals, SMPS","2",null,null,"USB OTG FS,USB OTG FS + USB OTG FS/HS"]
["STM32H747ZI","STSTM32H747ZI","ST","ARM CM7+M4 Dual",480,2048,null,1024,0,null,2,2,null,"No",4,6,3,"Yes",18,"24bit downcounter,2xWDG,HR Timer,RTC",-40,85,1.62,3.6,150,"WLCSP 150L DIE 450 PITCH 0.35",null,4,5,4,270,null,null,"true","Evaluation",null,"Highperformance and DSP with DPFPU, ARM CM7 + CortexM4 MCU with 2MBytes of Flash memory, 1MB RAM, 480 MHz CPU, Art Accelerator, L1 cache, external memory interface, large set of peripherals, SMPS, MIPIDSI","2",null,null,"USB OTG FS,USB OTG FS + USB OTG FS/HS"]
["STM32H753XI","STSTM32H753XI","ST","ARM CM7",480,2048,null,1024,0,null,2,2,168,"Yes",4,6,3,"Yes",18,"24bit downcounter,2xWDG,HR Timer,RTC",-40,85,1.62,3.6,240,"TFBGA 14X14X1.2 P 0.8 240+25L",null,4,5,4,270,null,"AES,DES/TDES,HMAC,MD5,SHA","true","Active",null,"Highperformance and DSP with DPFPU, ARM CM7 MCU with 2MBytes of Flash memory, 1MB RAM, 480 MHz CPU, Art Accelerator, L1 cache, external memory interface, large set of peripherals including a Crypto accelerator, with security services support","2",null,"LCD TFT Controller up to 1024x728","USB OTG FS,USB OTG FS + USB OTG FS/HS"]
["STM32L010K4","STSTM32L010K4","ST","ARM CM0+",32,16,0.125,2,12,10,0,0,26,"No",1,1,null,"No",3,"2xWDG,RTC,SysTick",-40,85,1.8,3.6,32,"LQFP 32 7x7x1.4",0.495,1,1,0.8,87,null,null,null,"Active",null,"Ultralowpower value line ARM CM0+ MCU with 16Kbyte of Flash memory and 32 MHz CPU",0]
["STM32L011F3","STSTM32L011F3","ST","ARM CM0+",32,8,0.5,2,0,9,0,2,16,"No",1,1,null,"No",3,"2xWDG,RTC,SysTick",-40,85,1.65,3.6,20,"TSSOP 20,UFQFPN 20 3x3x0.6",0.63370000000000004,1,1,0.8,87,null,null,null,"Active",null,"Ultralowpower ARM CM0+ MCU with 8Kbytes Flash, 32 MHz CPU",0]
["STM32L031F6","STSTM32L031F6","ST","ARM CM0+",32,32,1,8,0,10,0,2,15,"No",1,1,null,"No",4,"2xWDG,RTC,SysTick",-40,85,1.65,3.6,20,"TSSOP 20",0.84199999999999997,1,1,0.8,87,null,null,null,"Active",null,"Ultralowpower ARM CM0+ MCU with 32Kbytes Flash, 32 MHz CPU",0]
["STM32L041F6","STSTM32L041F6","ST","ARM CM0+",32,32,1,8,0,10,0,2,15,"No",1,1,null,"No",4,"2xWDG,RTC,SysTick",-40,105,1.65,3.6,20,"TSSOP 20",0.97509999999999997,1,1,0.8,87,null,"AES",null,"Active",null,"Ultralowpower ARM CM0+ MCU with 32Kbytes Flash, 32 MHz CPU, AES",0]
["STM32L051K6","STSTM32L051K6","ST","ARM CM0+",32,32,2,8,0,10,0,2,27,"No",1,1,null,"No",5,"2xWDG,RTC,SysTick",-40,85,1.65,3.6,32,"LQFP 32 7x7x1.4,UFQFPN 32 5x5x0.55",1.1519999999999999,2,null,0.8,87,null,null,null,"Active",null,"Ultralowpower ARM CM0+ MCU with 32 Kbytes Flash, 32 MHz CPU",0]
["STM32L052K6","STSTM32L052K6","ST","ARM CM0+",32,32,2,8,0,10,1,2,27,"No",1,1,1,"Yes",5,"2xWDG,RTC,SysTick",-40,105,1.65,3.6,32,"LQFP 32 7x7x1.4,UFQFPN 32 5x5x0.55",1.4059999999999999,2,null,0.8,87,null,null,true,"Active",null,"Ultralowpower ARM CM0+ MCU with 32 Kbytes Flash, 32 MHz CPU, USB",0,null,null,"USB Device"]
["STM32L052T8","STSTM32L052T8","ST","ARM CM0+",32,64,2,8,0,10,1,2,29,"No",2,1,1,"Yes",5,"2xWDG,RTC,SysTick",-40,85,1.65,3.6,36,"THIN WLCSP 36L DIE 417 P 0.4 MM,WLCSP 36L DIE 417 P 0.4 MM",1.5338000000000001,2,1,0.8,87,null,null,true,"Active",null,"Ultralowpower ARM CM0+ MCU with 64 Kbytes Flash, 32 MHz CPU, USB",0,null,null,"USB Device"]
["STM32L053R6","STSTM32L053R6","ST","ARM CM0+",32,32,2,8,0,16,1,2,51,"Yes",2,2,1,"Yes",5,"2xWDG,RTC,SysTick",-40,85,1.65,3.6,64,"LQFP 64 10x10x1.4,TFBGA 64 5x5x1.2",1.5916999999999999,2,1,0.8,87,null,null,true,"Active",null,"Ultralowpower ARM CM0+ MCU with 32 Kbytes Flash, 32 MHz CPU, USB, LCD",0,null,"LCD 4x31/8x28","USB Device"]
["R5F51307ADFK","RenesasR5F51307ADFK","Renesas","RX",32,384,8,48,null,14,0,null,53,null,5,5,null,null,12,"16bit Timers is included Low Power Timer x 1ch",-40,85,1.8,5.5,64,"64LQFP",null,null,4,null,null,null,null,null,"Mass Production","IEBus,"]
["R5F51307AGFP","RenesasR5F51307AGFP","Renesas","RX",32,384,8,48,null,24,0,null,89,null,8,8,null,null,12,"16bit Timers is included Low Power Timer x 1ch",-40,105,1.8,5.5,100,"100LFQFP",null,null,7,null,null,null,null,null,"Mass Production","IEBus,"]
["R5F52104BGFL","RenesasR5F52104BGFL","Renesas","RX",50,96,8,16,null,8,0,null,35,null,6,6,null,null,14,null,-40,105,1.62,5.5,48,"48LFQFP",null,null,5,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F52105BGFF","RenesasR5F52105BGFF","Renesas","RX",50,128,8,20,null,14,0,null,65,null,8,8,null,null,14,null,-40,105,1.62,5.5,80,"80LQFP",null,null,7,null,null,null,null,null,"Product Inquiry","",null,null,null,0]
["R5F52106BDFM","RenesasR5F52106BDFM","Renesas","RX",50,256,8,32,null,12,0,null,49,null,7,7,null,null,14,null,-40,85,1.62,5.5,64,"64LFQFP",null,null,6,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F52107BGFB","RenesasR5F52107BGFB","Renesas","RX",50,384,8,64,null,16,0,null,123,null,14,14,null,null,20,null,-40,105,1.62,5.5,144,"144LFQFP",null,null,13,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F52107CGFP","RenesasR5F52107CGFP","Renesas","RX",50,384,8,64,null,16,0,null,85,null,8,8,null,null,14,null,-40,105,1.62,5.5,100,"100LFQFP",null,null,7,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F52108CGFF","RenesasR5F52108CGFF","Renesas","RX",50,512,8,64,null,14,0,null,65,null,8,8,null,null,14,null,-40,105,1.62,5.5,80,"80LQFP",null,null,7,null,null,null,null,null,"Product Inquiry","",null,null,null,0]
["R5F5210BBDLK","RenesasR5F5210BBDLK","Renesas","RX",50,1024,8,96,null,16,0,null,123,null,14,14,null,null,20,null,-40,85,1.62,5.5,145,"145TFLGA",null,null,13,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F521A6BGFP","RenesasR5F521A6BGFP","Renesas","RX",50,256,8,32,null,0,0,null,66,null,7,7,null,null,14,null,-40,105,1.8,3.6,100,"100LFQFP",null,null,5,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F521A8BGFN","RenesasR5F521A8BGFN","Renesas","RX",50,512,8,64,null,0,0,null,51,null,7,7,null,null,14,null,-40,105,1.8,3.6,80,"80LFQFP",null,null,5,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F52205BGFL","RenesasR5F52205BGFL","Renesas","RX",32,128,8,8,null,8,0,null,35,null,5,5,null,null,14,null,-40,105,1.62,5.5,48,"48LFQFP",null,null,4,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F52206BGFM","RenesasR5F52206BGFM","Renesas","RX",32,256,8,16,null,12,0,null,49,null,6,6,null,null,14,null,-40,105,1.62,5.5,64,"64LFQFP",null,null,5,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F52305AGNE","RenesasR5F52305AGNE","Renesas","RXv2",54,128,8,32,null,8,0,null,35,null,6,6,null,null,21,null,-40,105,1.8,5.5,48,"48HWQFN",null,null,5,null,null,null,null,null,"Mass Production",""]
["R5F52306AGFM","RenesasR5F52306AGFM","Renesas","RXv2",54,256,8,32,null,12,2,null,48,null,7,7,null,null,21,null,-40,105,1.8,5.5,64,"64LFQFP",null,null,6,null,null,null,null,null,"Mass Production",""]
["R5F523E6ADNF","RenesasR5F523E6ADNF","Renesas","RXv2 coer",32,256,8,32,null,4,0,null,17,null,1,1,null,null,13,null,-40,85,1.8,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","CAN,"]
["R5F523T5ADFD","RenesasR5F523T5ADFD","Renesas","RX",40,128,0,12,null,10,0,null,40,null,3,3,null,null,14,null,-40,85,2.7,5.5,52,"52LQFP",null,null,2,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F524T8AGFN","RenesasR5F524T8AGFN","Renesas","RX",80,128,8,16,null,17,0,null,58,null,4,4,null,null,21,"3phase PWM Output: 2",-40,105,2.7,5.5,80,"80LFQFP",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F524TBAGFP","RenesasR5F524TBAGFP","Renesas","RX",80,256,8,32,null,22,0,null,80,null,4,4,null,null,25,"3phase PWM Output: 3",-40,105,2.7,5.5,100,"100LFQFP",null,null,3,null,null,null,null,null,"Mass Production","CAN,",null,null,null,0]
["R5F56106VDFP","RenesasR5F56106VDFP","Renesas","RX",100,1024,32,128,null,0,0,null,117,null,2,0,null,null,20,null,-40,85,3,3.6,144,"144LFQFP",null,null,7,null,null,null,null,null,"Nonpromotion","",null,null,null,0]
["R5F56108VNFP","RenesasR5F56108VNFP","Renesas","RX",100,2048,32,128,null,0,0,null,117,null,2,0,null,null,20,null,-20,85,3,3.6,144,"144LFQFP",null,null,7,null,null,null,null,null,"Nonpromotion","",null,null,null,0]
["R5F562GADDFH","RenesasR5F562GADDFH","Renesas","RX",100,256,32,16,null,8,0,null,82,null,1,1,null,null,16,null,-40,85,4,5.5,112,"112LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,",null,null,null,0]
["R5F562T6BDFK","RenesasR5F562T6BDFK","Renesas","RX",100,64,8,8,null,8,0,null,46,null,1,1,null,null,16,null,-40,85,2.7,3.6,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,",null,null,null,0]
["R5F562T6EDFK","RenesasR5F562T6EDFK","Renesas","RX",100,64,8,8,null,8,0,null,46,null,1,1,null,null,16,null,-40,85,2.7,3.6,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,",null,null,null,0]
["R5F562T7BDFH","RenesasR5F562T7BDFH","Renesas","RX",100,128,8,8,null,8,0,null,82,null,1,1,null,null,16,null,-40,85,2.7,3.6,112,"112LQFP",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,",null,null,null,0]
["R5F562T7DDFF","RenesasR5F562T7DDFF","Renesas","RX",100,128,8,8,null,8,0,null,57,null,1,1,null,null,16,null,-40,85,4,5.5,80,"80LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,",null,null,null,0]
["R5F562TAADFH","RenesasR5F562TAADFH","Renesas","RX",100,256,32,16,null,8,0,null,82,null,1,1,null,null,16,null,-40,85,4,5.5,112,"112LQFP",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,",null,null,null,0]
["R5F562TADDFK","RenesasR5F562TADDFK","Renesas","RX",100,256,32,16,null,8,0,null,46,null,1,1,null,null,16,null,-40,85,4,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,",null,null,null,0]
["R5F562TAGGFF","RenesasR5F562TAGGFF","Renesas","RX",100,256,32,16,null,8,0,null,57,null,1,1,null,null,16,null,-40,105,4,5.5,80,"80LQFP",null,null,3,null,null,null,null,null,"Product Inquiry","CAN,LIN,",null,null,null,0]
["R5F563T5EGFL","RenesasR5F563T5EGFL","Renesas","RX",100,48,8,8,null,6,0,null,34,null,1,4,null,null,16,null,-40,105,2.7,3.6,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F563TBAGFP","RenesasR5F563TBAGFP","Renesas","RX",100,256,32,24,null,8,0,null,78,null,5,6,null,null,19,null,-40,105,4,5.5,100,"100LFQFP",null,null,4,null,null,null,null,null,"Mass Production","CAN,",null,null,null,0]
["R5F563TCBDFH","RenesasR5F563TCBDFH","Renesas","RX",100,384,32,32,null,8,0,null,90,null,6,7,null,null,20,null,-40,85,2.7,3.6,112,"112LQFP",null,null,5,null,null,null,null,null,"Mass Production","CAN,",null,null,null,0]
["R5F563TEADFP","RenesasR5F563TEADFP","Renesas","RX",100,512,32,48,null,8,0,null,78,null,5,6,null,null,19,null,-40,85,4,5.5,100,"100LFQFP",null,null,4,null,null,null,null,null,"Mass Production","CAN,",null,null,null,0]
["R5F563TEEDFH","RenesasR5F563TEEDFH","Renesas","RX",100,512,32,48,null,8,0,null,90,null,6,7,null,null,20,null,-40,85,2.7,3.6,112,"112LQFP",null,null,5,null,null,null,null,null,"Mass Production","",null,null,null,0]
["R5F566TAEDFP","RenesasR5F566TAEDFP","Renesas","RXv3 core",160,256,32,64,null,22,2,null,81,null,8,8,null,null,31,"3phase PWM Output: 3",-40,85,2.7,5.5,100,"100LFQFP",null,null,7,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F566TEAGFP","RenesasR5F566TEAGFP","Renesas","RXv3 core",160,512,32,64,null,22,2,null,81,null,8,8,null,null,31,"3phase PWM Output: 3",-40,105,2.7,5.5,100,"100LFQFP",null,null,7,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F566TEEGFH","RenesasR5F566TEEGFH","Renesas","RXv3 core",160,512,32,64,null,22,2,null,93,null,8,8,null,null,31,"3phase PWM Output: 4",-40,105,2.7,5.5,112,"112LQFP",null,null,7,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F566TFFGFP","RenesasR5F566TFFGFP","Renesas","RXv3 core",160,512,32,128,null,22,2,null,80,null,8,8,null,null,31,"3phase PWM Output: 3",-40,105,2.7,5.5,100,"100LFQFP",null,null,7,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F572TFADFP","RenesasR5F572TFADFP","Renesas","RXv3 core",200,512,32,128,null,22,2,null,81,null,8,8,null,null,31,"3phase PWM Output: 3",-40,85,2.7,5.5,100,"100LFQFP",null,null,7,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F572TKEGFP","RenesasR5F572TKEGFP","Renesas","RXv3 core",200,1024,32,128,null,22,2,null,81,null,8,8,null,null,31,"3phase PWM Output: 3",-40,105,2.7,5.5,100,"100LFQFP",null,null,7,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F71242N50FP","RenesasR5F71242N50FP","Renesas","SH2",50,64,0,8,null,0,0,null,31,null,0,0,null,null,8,null,-20,85,4,5.5,48,"48LQFP",null,"SCI (CSI:2ch/UART:3ch)",3,null,null,null,null,null,"Nonpromotion",""]
["R5F71250AN50FP","RenesasR5F71250AN50FP","Renesas","SH2",50,16,0,4,null,0,0,null,45,null,0,0,null,null,8,null,-20,85,4,5.5,64,"64LFQFP",null,"SCI (CSI:3ch/UART:3ch)",3,null,null,null,null,null,"Nonpromotion",""]
["R5F71253D50FP","RenesasR5F71253D50FP","Renesas","SH2",50,128,0,8,null,0,0,null,45,null,0,0,null,null,8,null,-40,85,4,5.5,64,"64LFQFP",null,"SCI (CSI:3ch/UART:3ch)",3,null,null,null,null,null,"Nonpromotion",""]
["HD6437041AXXXF","RenesasHD6437041AXXXF","Renesas","SH2",28.7,64,0,4,null,0,0,null,106,null,0,0,null,null,7,null,-20,75,3,5.5,144,144,null,"SCI (CSI:2ch/UART:2ch)",2,null,null,null,null,null,"Product Inquiry",""]
["HD6437041AXXXFI","RenesasHD6437041AXXXFI","Renesas","SH2",28.7,64,0,4,null,0,0,null,106,null,0,0,null,null,7,null,-40,85,3,5.5,144,144,null,"SCI (CSI:2ch/UART:2ch)",2,null,null,null,null,null,"Product Inquiry",""]
["HD64F7047F50V","RenesasHD64F7047F50V","Renesas","SH2",50,256,0,12,null,0,0,null,69,null,0,0,null,null,7,null,-20,75,4.5,5.5,100,"100FQFP",null,"SCI (CSI:3ch/UART:3ch)",3,null,null,null,null,null,"Nonpromotion","CAN,"]
["HD64F7065AF60V","RenesasHD64F7065AF60V","Renesas","SH2DSP",60,256,0,8,null,0,0,null,118,null,0,0,null,null,9,null,-20,75,3,3.6,176,"176LFQFP",null,"SCI (CSI:3ch/UART:3ch)",3,null,null,null,null,null,"Nonpromotion",""]
["R5F70844AD80FPV","RenesasR5F70844AD80FPV","Renesas","SH2",80,256,0,16,null,0,0,null,84,null,1,1,null,null,11,null,-40,85,3,5.5,112,"112LQFP",null,"SCI (CSI:3ch/UART:3ch), SCIF (CSI:1ch/UART:1ch), SSU (SPI), I2C",4,null,null,null,null,null,"Nonpromotion",""]
["R5F70865AN80FPV","RenesasR5F70865AN80FPV","Renesas","SH2",80,512,0,32,null,0,0,null,134,null,1,1,null,null,11,null,-20,85,3,5.5,176,"176LFQFP",null,"SCI (CSI:3ch/UART:3ch), SCIF (CSI:1ch/UART:1ch), SSU (SPI), I2C",4,null,null,null,null,null,"Nonpromotion",""]
["HD6437144WXXXF","RenesasHD6437144WXXXF","Renesas","SH2",50,256,0,8,null,0,0,null,82,null,1,0,null,null,7,null,-20,75,3,3.6,112,112,null,"SCI (CSI:4ch/UART:4ch), I2C",4,null,null,null,null,null,"Product Inquiry",""]
["R5F71464AN80FPV","RenesasR5F71464AN80FPV","Renesas","SH2",80,256,0,8,null,0,0,null,57,null,0,0,null,null,11,null,-20,85,4,5.5,80,"80LQFP",null,"SCI (CSI:3ch/UART:3ch)",3,null,null,null,null,null,"Nonpromotion",""]
["R5F72115D160FPV","RenesasR5F72115D160FPV","Renesas","SH2A",160,512,0,32,null,8,0,null,75,null,1,0,null,null,11,null,-40,85,3,3.6,144,"144LFQFP",null,"SCIF (CSI:4ch/UART:4ch), I2C",4,null,null,null,null,null,"Mass Production",""]
["R5F72145ADFA","RenesasR5F72145ADFA","Renesas","SH2A",200,512,32,64,null,8,0,null,112,null,1,4,null,null,11,null,-40,85,3,3.6,176,"176LFQFP",null,"SCI (CSI:4ch/UART:4ch), SCIF (CSI:1ch/UART:1ch), RSPI, I2C",5,null,null,null,null,null,"Mass Production","CAN,EtherNet,"]
["R5F72146HDFA","RenesasR5F72146HDFA","Renesas","SH2A",100,768,32,96,null,8,0,null,112,null,1,4,null,null,11,null,-40,85,3,3.6,176,"176LFQFP",null,"SCI (CSI:4ch/UART:4ch), SCIF (CSI:1ch/UART:1ch), RSPI, I2C",5,null,null,null,null,null,"Mass Production","CAN,"]
["R5F72147GDFA","RenesasR5F72147GDFA","Renesas","SH2A",100,1024,32,128,null,8,0,null,112,null,1,4,null,null,11,null,-40,85,3,3.6,176,"176LFQFP",null,"SCI (CSI:4ch/UART:4ch), SCIF (CSI:1ch/UART:1ch), RSPI, I2C",5,null,null,null,null,null,"Mass Production","CAN,EtherNet,"]
["R5F72165GDFP","RenesasR5F72165GDFP","Renesas","SH2AFPU",100,512,32,64,null,8,0,null,112,null,1,4,null,null,11,null,-40,85,3,3.6,176,"176LFQFP",null,"SCI (CSI:4ch/UART:4ch), SCIF (CSI:1ch/UART:1ch), RSPI, I2C",5,null,null,null,null,null,"Mass Production","CAN,EtherNet,"]
["R5F72166BDFP","RenesasR5F72166BDFP","Renesas","SH2AFPU",200,768,32,96,null,8,0,null,112,null,1,4,null,null,11,null,-40,85,3,3.6,176,"176LFQFP",null,"SCI (CSI:4ch/UART:4ch), SCIF (CSI:1ch/UART:1ch), RSPI, I2C",5,null,null,null,null,null,"Mass Production","CAN,"]
["R5F72167ADFP","RenesasR5F72167ADFP","Renesas","SH2AFPU",200,1024,32,128,null,8,0,null,112,null,1,4,null,null,11,null,-40,85,3,3.6,176,"176LFQFP",null,"SCI (CSI:4ch/UART:4ch), SCIF (CSI:1ch/UART:1ch), RSPI, I2C",5,null,null,null,null,null,"Mass Production","CAN,EtherNet,"]
["R5F72315ADBA","RenesasR5F72315ADBA","Renesas","SH2AFPU",100,1024,32,32,null,0,0,null,184,null,1,4,null,null,15,null,-40,85,3,3.6,272,"272FBGA",null,"SCI (CSI:4ch/UART:4ch), SCIF (CSI:4ch/UART:4ch), RSPI, I2C",8,null,null,null,null,null,"Nonpromotion","CAN,"]
["R5F72533KFPU","RenesasR5F72533KFPU","Renesas","SH2AFPU",160,2048,32,96,null,32,0,null,112,null,0,2,null,null,35,"24bit timer x 73",-40,125,4.5,5.5,176,176,null,"SCI (CSI:3ch/UART:3ch), RSPI (SPI:2ch)",3,null,null,null,null,null,"Product Inquiry","CAN,"]
["R5F72543RKBGV","RenesasR5F72543RKBGV","Renesas","SH2AFPU",200,2048,128,128,null,37,0,null,144,null,0,3,null,null,41,"24bit timer x 73",-40,125,3,5.5,272,272,null,"SCI (CSI:5ch/UART:5ch), RSPI (SPI:3ch)",5,null,null,null,null,null,"Product Inquiry","CAN,"]
["R5F72A06K2CFM","RenesasR5F72A06K2CFM","Renesas","SH2AFPU",80,256,0,32,null,6,0,null,46,null,0,0,null,null,30,null,-40,125,3.3,5.5,64,64,null,"SCI (CSI:4ch/UART:4ch), SBI ( SBI:4ch/CSI:4ch), LIN",4,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["R5F72A28KACFP","RenesasR5F72A28KACFP","Renesas","SH2AFPU",80,512,32,64,null,6,0,null,80,null,0,0,null,null,30,null,-40,125,3.3,5.5,100,100,null,"SCI (CSI:4ch/UART:4ch), SBI ( SBI:4ch/CSI:4ch), LIN:2ch",4,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["UPD70F3422GJ(A)GAEAX","RenesasUPD70F3422GJ(A)GAEAX","Renesas","V850E1",32,384,0,16,null,0,0,null,98,null,2,3,null,null,13,null,-40,85,3.5,5.5,144,"144LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion","CAN,LIN,",null,null,null,"seg=40, com=4"]
["UPD70F3454F1DA9A","RenesasUPD70F3454F1DA9A","Renesas","V850E1",64,256,0,12,null,10,0,null,64,null,1,0,null,null,13,"Timer for Moter Control (TAB2ch&#43;TMQOP2ch&#43;TAA2ch)",-40,85,3.5,5.5,161,"161LFBGA",null,null,4,null,null,null,null,null,"Nonpromotion",""]
["UPD703111GM15UEUA","RenesasUPD703111GM15UEUA","Renesas",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,0,null,null,null,176,"176LFQFP",null,null,null,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["UPD70F3478AGJAGAEG","RenesasUPD70F3478AGJAGAEG","Renesas","V850E1",48,1536,0,92,null,0,0,null,128,null,6,0,null,null,13,null,-40,85,2.85,3.6,144,"144LFQFP",null,null,8,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,"]
["UPD70F3936BGJAGAEG","RenesasUPD70F3936BGJAGAEG","Renesas","V850E1",48,768,0,76,null,0,0,null,128,null,6,0,null,null,13,null,-40,85,2.85,3.6,144,144,null,null,8,null,null,null,null,null,"Product Inquiry","CAN,LIN,IEBus,"]
["UPD70F3937BGJAGAEG","RenesasUPD70F3937BGJAGAEG","Renesas","V850E1",48,1024,0,76,null,0,0,null,128,null,6,0,null,null,13,null,-40,85,2.85,3.6,144,144,null,null,8,null,null,null,null,null,"Product Inquiry","LIN,IEBus,"]
["UPD70F3526GJAGBGG","RenesasUPD70F3526GJAGBGG","Renesas","V850E2M",120,3072,32,256,null,16,0,null,105,null,2,1,null,null,92,"Timer for OS x 1 ch",-40,85,2.7,5.5,144,144,null,"I2S 1ch",2,null,null,null,null,null,"Product Inquiry","CAN,LIN,",null,null,null,"69seg x 6com"]
["UPD70F4154GCA2UEUAX","RenesasUPD70F4154GCA2UEUAX","Renesas","V850E2M",80,384,16,24,null,18,0,null,46,null,0,0,null,null,26,"Timer for OS x 2 ch",-40,125,3,5.5,100,100,null,null,2,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["UPD70F4015M2GJAGAEG","RenesasUPD70F4015M2GJAGAEG","Renesas","V850E2M",160,1024,32,160,null,0,0,null,100,null,4,0,null,null,20,"Timer for OS x 1 ch",-40,85,3,3.6,144,144,null,"I2S/PCM/MLB Support",5,null,null,null,null,null,"Product Inquiry","LIN,IEBus,"]
["UPD70F4018M1GMA9GARG","RenesasUPD70F4018M1GMA9GARG","Renesas","V850E2M",160,2048,32,256,null,0,0,null,127,null,4,0,null,null,36,"Timer for OS x 1 ch, Encoder Timer x 2 ch",-40,105,3,3.6,176,176,null,"I2S/PCM/MLB Support",5,null,null,null,null,null,"Product Inquiry","CAN,EtherNet,LIN,IEBus,"]
["UPD70F3371M1GBA2GAHAX","RenesasUPD70F3371M1GBA2GAHAX","Renesas","V850ES",24,256,32,16,null,0,0,null,51,null,1,0,null,null,7,"Watch Timer x 1 ch",-40,125,3.3,5.5,64,"64LFQFP",null,null,2,null,null,null,null,null,"Nonpromotion","CAN,LIN,"]
["UPD70F3376AM1GCA1UEUAX","RenesasUPD70F3376AM1GCA1UEUAX","Renesas","V850ES",48,384,32,24,null,0,0,null,84,null,1,0,null,null,8,"Watch Timer x 1 ch",-40,110,3.3,5.5,100,"100LFQFP",null,null,5,null,null,null,null,null,"Nonpromotion","CAN,LIN,"]
["UPD70F3381M2GJA1GAEAX","RenesasUPD70F3381M2GJA1GAEAX","Renesas","V850ES",48,768,32,40,null,0,0,null,128,null,1,0,null,null,9,"Watch Timer x 1 ch",-40,110,3.3,5.5,144,"144LFQFP",null,null,6,null,null,null,null,null,"Nonpromotion","CAN,LIN,"]
["UPD70F3381M2GJAGAEAX","RenesasUPD70F3381M2GJAGAEAX","Renesas","V850ES",48,768,32,40,null,0,0,null,128,null,1,0,null,null,9,"Watch Timer x 1 ch",-40,85,3.3,5.5,144,"144LFQFP",null,null,6,null,null,null,null,null,"Nonpromotion","CAN,LIN,"]
["UPD70F3622M2GCA1UEUAX","RenesasUPD70F3622M2GCA1UEUAX","Renesas","V850ES",20,256,0,16,null,0,0,null,84,null,1,0,null,null,6,null,-40,110,3.3,5.5,100,"100LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion","CAN,LIN,"]
["UPD70F3744GJGAEAX","RenesasUPD70F3744GJGAEAX","Renesas","V850ES",32,512,0,40,null,0,0,null,128,null,3,0,null,null,11,"Watch Timer x 1 ch",-40,85,2.85,3.6,144,"144LFQFP",null,null,4,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD70F3792GCUEUAX","RenesasUPD70F3792GCUEUAX","Renesas","V850ES",20,384,0,32,null,0,0,null,83,null,3,0,null,null,8,"Watch Timer x 1 ch",-40,85,2,3.6,100,"100LFQFP",null,null,7,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD70F3334GC(A)UEUAX","RenesasUPD70F3334GC(A)UEUAX","Renesas","V850ES",32,384,0,32,null,0,0,null,84,null,3,0,null,null,8,"Watch Timer x 1 ch",-40,85,2.85,3.6,100,"100LFQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,IEBus,"]
["UPD70F3348GJ(A)GAEAX","RenesasUPD70F3348GJ(A)GAEAX","Renesas","V850ES",32,1024,0,60,null,0,0,null,128,null,3,0,null,null,11,"Watch Timer x 1 ch",-40,85,2.85,3.6,144,"144LFQFP",null,null,4,null,null,null,null,null,"Mass Production","LIN,IEBus,"]
["UPD70F3356GJ(A)UENA","RenesasUPD70F3356GJ(A)UENA","Renesas","V850ES",32,640,0,48,null,0,0,null,128,null,3,0,null,null,11,"Watch Timer x 1 ch",-40,85,2.85,3.6,144,"144LFQFP",null,null,4,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,"]
["R5F2L36ACNFA","RenesasR5F2L36ACNFA","Renesas","R8C",20,96,4,10,null,0,0,null,52,null,2,1,null,"No",7,null,-40,85,1.8,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,",null,null,null,"32 seg.(max)<br> 8 com.(max)",0]
["R5F2L36CCDFA","RenesasR5F2L36CCDFA","Renesas","R8C",20,128,4,10,null,0,0,null,52,null,2,1,null,"No",7,null,-40,85,1.8,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,",null,null,null,"32 seg.(max)<br> 8 com.(max)",0]
["R7F701311EAFP","RenesasR7F701311EAFP","Renesas","G3M",160,1024,32,128,null,24,0,null,86,null,0,0,null,"No",60,"TSG3 x2unit, ENCA x2unit, OSTM x7unit, TPBA x2unit",-40,150,3,5.5,144,"144LFQFP",null,null,3,null,null,null,null,null,"Product Inquiry","CAN,LIN,",null,null,null,null,0]
["R7F701321EAFP","RenesasR7F701321EAFP","Renesas","G3M",160,2048,64,128,null,19,0,null,52,null,0,0,null,"No",60,"TSG3 x2unit, ENCA x2unit, OSTM x7unit, TPBA x2unit",-40,150,3,5.5,100,"100LFQFP",null,null,3,null,null,null,null,null,"Product Inquiry","CAN,LIN,",null,null,null,null,0]
["R7F701385EAFP","RenesasR7F701385EAFP","Renesas","G3M",160,1024,32,192,null,24,0,null,86,null,0,0,null,"No",60,"TSG3 x2unit, ENCA x2unit, OSTM x7unit, TPBA x2unit",-40,150,3,5.5,144,"144LFQFP",null,null,3,null,null,null,null,null,"Product Inquiry","CAN,LIN,",null,null,null,null,0]
["NANO120SD2BN","NuvotonNANO120SD2BN","Nuvoton","ARM CM0",42,64,null,8,null,7,2,null,48,null,2,3,null,"Yes",4,null,-40,85,1.8,3.6,64,"LQFP64(7x7mm)",null,null,5,null,null,null,null,null,null,null,null,null,null,null,1]
["NUC029LGE","NuvotonNUC029LGE","Nuvoton","ARM CM0",72,256,null,20,null,9,null,2,35,null,2,2,null,"Yes",4,null,-40,105,2.5,5.5,48,"LQFP48",null,null,3,null,null,null,null,null,null,null,null,null,null,null,1]
["NUC120VE3DN","NuvotonNUC120VE3DN","Nuvoton","ARM CM0",72,128,null,16,null,8,null,2,81,null,2,4,null,"Yes",4,null,-40,85,2.5,5.5,100,"LQFP100",null,null,3,null,null,null,null,null,null,null,null,null,null,null,1]
["NUC220LE3AN","NuvotonNUC220LE3AN","Nuvoton","ARM CM0",72,128,null,16,null,7,null,1,31,null,2,1,null,"Yes",4,null,-40,85,2.5,5.5,48,"LQFP48",null,null,2,null,null,null,null,null,null,null,null,null,null,null,1]
["NUC220SC2AN","NuvotonNUC220SC2AN","Nuvoton","ARM CM0",72,32,null,8,null,7,null,2,45,null,2,2,null,"Yes",4,null,-40,85,2.5,5.5,64,"LQFP64(7x7mm)",null,null,2,null,null,null,null,null,null,null,null,null,null,null,1]
["NUC140RE3CN","NuvotonNUC140RE3CN","Nuvoton","ARM CM0",72,128,null,16,null,8,null,2,45,null,2,2,null,"Yes",4,null,-40,85,2.5,5.5,64,"LQFP64",null,null,3,null,null,null,null,null,null,"CAN",null,null,null,null,1]
["M481SGCAE","NuvotonM481SGCAE","Nuvoton","ARM CM4F",192,256,null,128,null,16,1,2,52,null,3,5,4,"No",4,null,-40,105,1.8,3.6,64,"LFQP64",null,null,8,null,null,null,null,null,null,null,null,null,null,null,""]
["M453LC3AE","NuvotonM453LC3AE","Nuvoton","ARM CM4F",72,40,null,16,null,10,1,2,35,null,2,2,1,"Yes",4,null,-40,105,2.5,5.5,48,"LQFP48",null,null,5,null,null,null,null,null,null,"CAN",null,null,null,null,"DEVICE"]
["GD32F103R6T6","GigaDeviceGD32F103R6T6","GigaDevice","ARM CM3",108,32,null,10,2,16,null,null,51,null,1,1,null,"Yes",3,"SysTick, WDT, RTC",-40,85,2.6,3.6,64,"LQFP64",null,null,2,null,null,null,null,null,null,null,null,null,null,null,"FS"]
["GD32F103TBU6","GigaDeviceGD32F103TBU6","GigaDevice","ARM CM3",108,128,null,20,2,10,null,null,26,null,1,1,null,"Yes",4,"SysTick, WDT, RTC",-40,85,2.6,3.6,36,"QFN36",null,null,2,null,null,null,null,null,null,null,null,null,null,null,"FS"]
["GD32F103VKT6","GigaDeviceGD32F103VKT6","GigaDevice","ARM CM3",108,3072,null,96,3,16,2,null,80,null,2,3,2,"Yes",14,"SysTick, WDT, RTC",-40,85,2.6,3.6,100,"LQFP100",null,null,5,null,null,null,null,null,null,null,null,null,null,null,"FS"]
["GD32F150G8U6","GigaDeviceGD32F150G8U6","GigaDevice","ARM CM3",72,64,null,8,null,10,1,null,24,null,2,2,1,"Yes",9,"SysTick, WDT, RTC",-40,85,2.6,3.6,28,"QFN28",null,null,2,null,null,null,null,null,null,null,null,null,null,null,"FS"]
["GD32F303CGT6","GigaDeviceGD32F303CGT6","GigaDevice","ARM CM4",120,1024,null,96,3,10,2,null,37,null,2,3,2,"Yes",13,"SysTick, WDT, RTC",-40,85,2.6,3.6,48,"LQFP48",null,null,3,null,null,null,null,null,null,null,null,null,null,null,"FS"]
["GD32VF103R6U6","GigaDeviceGD32VF103R6U6","GigaDevice","RISCV",108,32,null,10,2,16,2,null,51,null,1,1,null,"Yes",5,"SysTick, WDT, RTC",-40,85,2.6,3.6,64,"LQFP64",null,null,2,null,null,null,null,null,null,null,null,null,null,null,"FS"]
["PIC24FJ256GB210","MicrochipPIC24FJ256GB210","Microchip"," 16bit PIC MCU",32,256,0,96,16,24,0,3,84,"No",3,3,0,"Yes",34,null,-40,85,2.2000000000000002,3.6,100," 100/TQFP 121/TFBGA",5.14,null,4,null,null,0,null,null," In Production ","ISO7816,CAN,EtherNet",null,0,null,null,"No","No"]
["PIC24FJ256GL410","MicrochipPIC24FJ256GL410","Microchip"," 16-bit PIC MCU",32,256," 0 / True",null,12,24,1,3,86,"Yes",3,4,4,"No",31,null,-40,"105,85",2,3.6,100," 100/TQFP",2.39,null,6,null,null,0,null,null," In Production ","CAN,EtherNet",null,0,null,null,"Yes","No"]
["PIC24FJ48GA004","MicrochipPIC24FJ48GA004","Microchip"," 16bit PIC MCU",32,48,0,8,10,13,0,2,35,"No",2,2,0,"No",7,null,-40,125,2,3.6,44," 44/QFN 44/TQFP",2.16,null,2,null,null,0,null,null," In Production ","",null,0,null,null,"Yes","No"]
["PIC24FJ64GA410","MicrochipPIC24FJ64GA410","Microchip"," 16bit PIC MCU",32,64,0,8,12,24,1,3,85,"Yes",3,4,3,"No",46,null,-40,85,2,3.6,100," 100/TQFP",3.51,null,6,null,null,0,null,null," In Production ","",null,0,null,null,"Yes","No"]
["PIC24FJ64GC006","MicrochipPIC24FJ64GC006","Microchip"," 16bit PIC MCU",32,64,0,8,16,2,2,3,48,"Yes",2,2,0,"Yes",18,null,-40,85,2,3.6,64," 64/QFN 64/TQFP",3.36,null,4,null,null,0,null,null," In Production ","SD/MMC,",null,0,null,null,"Yes","No"]
["GD32F407IGH6","GigaDeviceGD32F407IGH6","GigaDevice","ARM CM4F",168,1024,null,192,3,24,2,null,140,null,3,3,2,"Yes",16,"WDT, RTC",-40,85,2.6,3.6,176,"BGA176",null,4,2,null,null,null,null,null,null,null,null,null,null,null,"FS+HS"]
["GD32F407VKH6","GigaDeviceGD32F407VKH6","GigaDevice","ARM CM4F",168,3072,null,192,3,16,2,null,82,null,3,3,2,"Yes",16,"WDT, RTC",-40,85,2.6,3.6,100,"BGA100",null,4,2,null,null,null,null,null,null,null,null,null,null,null,"FS+HS"]
["NUC505DSA","NuvotonNUC505DSA","Nuvoton","ARM CM4F",100,512,null,128,null,5,null,null,34,null,2,2,1,"Yes",4,null,-40,85,3,3.6,64,"LQFP64",null,null,3,null,null,null,null,null,null,null,null,null,null,null,"HOST+DEVICE"]
["GD32E103T8U6","GigaDeviceGD32E103T8U6","GigaDevice","ARM CM4F",120,64,null,20,2,10,2,null,26,null,1,1,null,"Yes",7,"SysTick, WDT, RTC",-40,85,1.71,3.6,36,"QFN36",null,2,0,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["GD32F105RFT6","GigaDeviceGD32F105RFT6","GigaDevice","ARM CM3",108,768,null,96,2,16,2,null,51,null,2,3,2,"Yes",14,"SysTick, WDT, RTC",-40,85,2.6,3.6,64,"LQFP64",null,null,5,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["GD32F105ZCT6","GigaDeviceGD32F105ZCT6","GigaDevice","ARM CM3",108,256,null,96,2,16,2,null,112,null,2,3,2,"Yes",8,"SysTick, WDT, RTC",-40,85,2.6,3.6,144,"LQFP144",null,null,5,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["GD32F107VDT6","GigaDeviceGD32F107VDT6","GigaDevice","ARM CM3",108,384,null,96,2,16,2,null,80,null,2,3,2,"Yes",8,"SysTick, WDT, RTC",-40,85,2.6,3.6,100,"LQFP100",null,null,5,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["GD32F205RCT6","GigaDeviceGD32F205RCT6","GigaDevice","ARM CM3",120,256,null,128,3,16,2,null,51,null,3,3,2,"Yes",14,"SysTick, WDT, RTC",-40,85,2.6,3.6,64,"LQFP64",null,4,2,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["GD32F207IGT6","GigaDeviceGD32F207IGT6","GigaDevice","ARM CM3",120,1024,null,256,3,24,2,null,140,null,3,3,2,"Yes",14,"SysTick, WDT, RTC",-40,85,2.6,3.6,176,"LQFP176",null,4,4,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["GD32F207VKT6","GigaDeviceGD32F207VKT6","GigaDevice","ARM CM3",120,3072,null,256,3,16,2,null,82,null,3,3,2,"Yes",14,"SysTick, WDT, RTC",-40,85,2.6,3.6,100,"LQFP100",null,4,4,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["GD32F307ZCT6","GigaDeviceGD32F307ZCT6","GigaDevice","ARM CM4",120,256,null,96,2,16,2,null,112,null,2,3,2,"Yes",8,"SysTick, WDT, RTC",-40,85,2.6,3.6,144,"LQFP144",null,null,5,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["GD32F350R4T6","GigaDeviceGD32F350R4T6","GigaDevice","ARM CM4",108,16,null,4,null,16,1,2,55,null,1,1,1,"Yes",9,"SysTick, WDT, RTC",-40,85,2.6,3.6,64,"LQFP64",null,null,1,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["GD32F403VCH6","GigaDeviceGD32F403VCH6","GigaDevice","ARM CM4F",168,256,null,64,3,16,2,null,80,null,2,3,2,"Yes",12,"WDT, RTC",-40,85,2.6,3.6,100,"BGA100",null,3,2,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["GD32F403ZIT6","GigaDeviceGD32F403ZIT6","GigaDevice","ARM CM4F",168,2048,null,128,3,21,2,null,112,null,2,3,2,"Yes",12,"WDT, RTC",-40,85,2.6,3.6,144,"LQFP144",null,3,2,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["M453LG6AE","NuvotonM453LG6AE","Nuvoton","ARM CM4F",72,256,null,32,null,8,1,2,34,null,2,3,2,"Yes",4,null,-40,105,2.5,5.5,48,"LQFP48",null,null,4,null,null,null,null,null,null,"CAN",null,null,null,null,"OTG"]
["M485ZIDAE","NuvotonM485ZIDAE","Nuvoton","ARM CM4F",192,512,null,160,null,10,2,2,26,null,5,4,4,"Yes",4,null,-40,105,1.8,3.6,33,"QFN33",null,null,6,null,null,null,null,null,null,null,null,null,null,null,"OTG"]
["M4TKRE6AE","NuvotonM4TKRE6AE","Nuvoton","ARM CM4F",72,128,null,32,null,12,1,2,48,null,2,3,2,"Yes",4,null,-40,105,2.5,5.5,64,"LQFP64",null,null,5,null,null,11,null,null,null,null,null,null,null,null,"OTG"]
["NUC442RI8AE","NuvotonNUC442RI8AE","Nuvoton","ARM CM4F",84,512,null,64,2,8,null,2,45,null,2,3,1,"Yes",4,null,-40,105,2.5,5.5,64,"LQFP64",null,null,7,null,null,null,null,null,"NRND",null,null,null,null,null,"OTG+DEVICE"]
["M483SGCAE","NuvotonM483SGCAE","Nuvoton","ARM CM4F",192,256,null,128,null,16,1,2,52,null,3,5,4,"Yes",4,null,-40,105,1.8,3.6,64,"LFQP64",null,null,8,null,null,null,null,null,null,"CAN",null,null,null,null,"OTG+HOST+DEVICE"]
["UPD70F3817GAGAMAX","RenesasUPD70F3817GAGAMAX","Renesas","V850ES",48,128,0,24,null,0,0,null,32,null,2,0,null,"Yes",10,"Encoder Timer x 1 ch, 32bit timer can be constructed by cascade connection.",-40,85,2.85,3.6,48,"48LFQFP",null,null,4,null,null,null,null,null,"Nonpromotion(*)","LIN,",null,null,null,null,"Provides free sample code for USB CDC, HID, Mass Storage & Printer class."]
["UPD70F3779GFGATAX","RenesasUPD70F3779GFGATAX","Renesas","V850ES",50,384,0,76,null,0,0,null,84,null,4,0,null,"Yes",13,"Timer for Motor Control x 1 ch, Encoder Timer x 1 ch, 32bit timer can be constructed by cascade connection.",-40,85,2.85,3.6,128,"128LFQFP",null,null,8,null,null,null,null,null,"Nonpromotion(*)","EtherNet,LIN,",null,null,null,null,"Provides free sample code for USB CDC, HID, Mass Storage class."]
["HC32F460JEUAQFN48TR","HUADAHC32F460JEUAQFN48TR","HUADA","ARM CM4F",168,512,null,192,2,10,null,3,38,null,3,4,null,"Yes",14,null,-40,85,1.8,3.6,48,"QFN48（5*5）",null,null,4,null,null,null,null,null,null,null,null,null,null,null,"USB 2.0 OTG_FS"]
["R5F52315AGFP","RenesasR5F52315AGFP","Renesas","RXv2",54,128,8,32,null,24,2,null,80,null,8,8,null,"Yes",21,null,-40,105,1.8,5.5,100,"100LFQFP",null,null,7,null,null,null,null,null,"Mass Production","CAN,",null,null,null,null,"USB Battery Charging Specification Rev 1.2 support"]
["R5F52315CDNE","RenesasR5F52315CDNE","Renesas","RXv2",54,128,8,32,null,8,0,null,31,null,6,6,null,"Yes",21,null,-40,85,1.8,5.5,48,"48HWQFN",null,null,5,null,null,null,null,null,"Mass Production","",null,null,null,null,"USB Battery Charging Specification Rev 1.2 support"]
["R5F52316AGFM","RenesasR5F52316AGFM","Renesas","RXv2",54,256,8,32,null,12,2,null,44,null,7,7,null,"Yes",21,null,-40,105,1.8,5.5,64,"64LFQFP",null,null,6,null,null,null,null,null,"Mass Production","CAN,",null,null,null,null,"USB Battery Charging Specification Rev 1.2 support"]
["R5F52316CDND","RenesasR5F52316CDND","Renesas","RXv2",54,256,8,32,null,12,2,null,44,null,7,7,null,"Yes",21,null,-40,85,1.8,5.5,64,"64HWQFN",null,null,6,null,null,null,null,null,"Mass Production","",null,null,null,null,"USB Battery Charging Specification Rev 1.2 support"]
["R5F52317AGFL","RenesasR5F52317AGFL","Renesas","RXv2",54,384,8,64,null,8,0,null,31,null,6,6,null,"Yes",21,null,-40,105,1.8,5.5,48,"48LFQFP",null,null,5,null,null,null,null,null,"Mass Production","CAN,",null,null,null,null,"USB Battery Charging Specification Rev 1.2 support"]
["R5F52318ADNE","RenesasR5F52318ADNE","Renesas","RXv2",54,512,8,64,null,8,0,null,31,null,6,6,null,"Yes",21,null,-40,85,1.8,5.5,48,"48HWQFN",null,null,5,null,null,null,null,null,"Mass Production","CAN,",null,null,null,null,"USB Battery Charging Specification Rev 1.2 support"]
["R5F52318BDLA","RenesasR5F52318BDLA","Renesas","RXv2",54,512,8,64,null,24,2,null,80,null,8,8,null,"Yes",21,null,-40,85,1.8,5.5,100,"100TFLGA",null,null,7,null,null,null,null,null,"Mass Production","CAN,",null,null,null,null,"USB Battery Charging Specification Rev 1.2 support"]
["R5F523W8ADNG","RenesasR5F523W8ADNG","Renesas","RXv2",54,512,8,64,null,8,1,null,30,null,4,4,null,"Yes",20,null,-40,85,1.8,3.6,56,"56QFN",null,null,3,null,null,9,null,null,"Mass Production","CAN,",null,null,null,null,"USB Battery Charging Specification Rev 1.2 support"]
["UPD78F1025F1AN9A","RenesasUPD78F1025F1AN9A","Renesas","78K0R",20,96,0,8,null,0,0,null,53,null,3,0,null,"Yes",8,null,-40,85,1.8,3.6,64,"64LFBGA",null,null,4,null,null,null,null,null,"Nonpromotion","LIN,",null,null,null,null,"USB full speed support"]
["R5F21346UDFP","RenesasR5F21346UDFP","Renesas","R8C",20,32,4,4,null,0,0,null,36,null,1,0,null,"Yes",4,null,-40,85,1.8,5.5,48,"48LFQFP",null,null,4,null,null,null,null,null,"Nonpromotion","LIN,",null,null,null,null,"USB2.0 Full Speed"]
["R7FA6M2AF3CFP","RenesasR7FA6M2AF3CFP","Renesas","ARM CM4F",120,1024,32,384,null,19,2,null,76,null,2,2,null,"Yes",13,"16bit Asynchronous Timer x 2",-40,105,2.7,3.6,100,"100LFQFP",null,null,10,null,null,12,null,null,"New","CAN,EtherNet,LIN,SD/MMC",null,null,null,null,"USB2.0 Full Speed  & USB  OTG (OnTheGO) Support & USB Battery Charhing 1.2 Support"]
["R7FA6M3AF3CFP","RenesasR7FA6M3AF3CFP","Renesas","ARM CM4F",120,1024,64,640,null,19,2,null,76,null,2,2,null,"Yes",13,"16bit Asynchronous Timer x 2",-40,105,2.7,3.6,100,"100LFQFP",null,null,10,null,null,12,null,null,"New","CAN,EtherNet,LIN,SD/MMC",null,null,null,null,"USB2.0 Full Speed  & USB  OTG (OnTheGO) Support & USB Battery Charhing 1.2 Support"]
["R7FA6M1AD3CNB","RenesasR7FA6M1AD3CNB","Renesas","ARM CM4F",120,512,8,256,null,10,2,null,40,null,2,2,null,"Yes",11,"16bit Asynchronous Timer x 2",-40,105,2.7,3.6,64,"64HWQFN",null,null,7,null,null,10,null,null,"New","CAN,LIN,SD/MMC",null,null,null,null,"USB2.0 Full Speed & USB  OTG (OnTheGO) Support"]
["MK20FN1M0VLQ12","NXPMK20FN1M0VLQ12","NXP","ARM CM4F",120,1024,null,128,16,null,2,null,100,"No",2,3,2,"Yes",1,null,-40,105,1.71,3.6,144,"LQFP144",6.48,null,6,null,null,null,null,null,null,null,"Kinetis K20: 120MHz CortexM4F Performance MCU, 1MB Flash, 128KB SRAM, Dual USBs (FS + HS), 144LQFP",null,null,null,2,"Yes"]
["MK27FN2M0AVMI15","NXPMK27FN2M0AVMI15","NXP","ARM CM4F",150,2048,null,1024,16,null,2,null,120,"No",4,4,2,"Yes",25,null,-40,105,1.71,3.6,169,"LFBGA169",8.18,null,5,null,null,null,null,null,null,null,"Kinetis K27: 150MHz CortexM4 Performance MCU, 2MB Flash, 1MB RAM, 2x USB (FS + HS), 169 MAPBGA",null,null,null,2,"No"]
["MK60FX512VMD12","NXPMK60FX512VMD12","NXP","ARM CM4F",120,1024,16,128,16,null,2,null,100,"No",2,3,2,"Yes",21,null,-40,105,1.71,3.6,144,"LBGA144",6.94,null,6,null,null,null,null,null,null,null,"Kinetis K60: 120MHz CortexM4F MCU, 512KB Flash + 512KB FlexMem, 128KB RAM, 2xUSB, Ethernet, 144BGA",null,null,null,2,"Yes"]
["MK61FX512VMJ12","NXPMK61FX512VMJ12","NXP","ARM CM4F",120,1024,16,128,16,null,2,null,128,"No",2,3,2,"Yes",21,null,-40,105,1.71,3.6,256,"LBGA256",7.76,null,6,null,null,null,null,null,null,null,"Kinetis K61: 120MHz M4F MCU, 512KB Flash + 512KB FlexMem, 128KB RAM, 2xUSB, ETH, Antitamper, 256BGA",null,null,null,2,"Yes"]
["MK66FN2M0VMD18","NXPMK66FN2M0VMD18","NXP","ARM CM4F",180,2048,null,256,16,null,2,null,100,"No",4,3,1,"Yes",1,null,-40,105,1.71,3.6,144,"LBGA144",7.8,null,6,null,null,null,null,null,null,null,"Kinetis K66: 180MHz CortexM4F MCU, 2MB Flash, 256KB SRAM, Dual USBs (FS + HS), Ethernet, 144MAPBGA",null,null,null,2,"Yes"]
["K32L2B21VFM0A","NXPK32L2B21VFM0A","NXP","ARM CM0+",48,128,null,32,16,null,2,null,23,"No",0,0,null,"No",1,null,-40,105,1.71,3.6,null,null,1.01,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"No"]
["KKL03Z32CAF4R","NXPKKL03Z32CAF4R","NXP","ARM CM0",48,32,null,2,12,null,0,null,18,"No",1,null,null,"No",null,null,-40,85,1.71,3.6,20,"WLCSP20",0.99,null,null,null,null,null,null,null,null,null,"Kinetis KL03: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 2KB SRAM, 20WLCSP",null,null,null,0,"No"]
["LPC1111FHN33,551","NXPLPC1111FHN33,551","NXP","ARM CM0",50,8,null,2,10,null,0,null,28,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,32,"HVQFN32",0.75,null,1,null,null,null,null,null,null,null,null,null,null,null,0,"No"]
["LPC1112FHN33,551","NXPLPC1112FHN33,551","NXP","ARM CM0",50,16,null,2,10,null,0,null,28,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,32,"HVQFN32",0.85,null,1,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,0,"No"]
["LPC1112JHI33/203E","NXPLPC1112JHI33/203E","NXP","ARM CM0",50,16,null,2,10,null,0,null,28,"No",1,2,null,"No",2,null,-40,105,1.8,3.6,32,"HVQFN32",0.84,null,1,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,0,"No"]
["LPC1113FHN33/203,5","NXPLPC1113FHN33/203,5","NXP","ARM CM0",50,24,null,8,10,null,0,null,28,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,32,"HVQFN32",0.96,null,1,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,0,"No"]
["LPC1114FBD48/301,1","NXPLPC1114FBD48/301,1","NXP","ARM CM0",50,32,null,8,10,null,0,null,42,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,48,"LQFP48",1.22,null,1,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,0,"No"]
["LPC1114FHN33/201,5","NXPLPC1114FHN33/201,5","NXP","ARM CM0",50,32,null,4,10,null,0,null,28,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.1499999999999999,null,1,null,null,null,null,null,null,null,"32kB flash, 8kB SRAM, HVQFN32 package",null,null,null,0,"No"]
["LPC1114FHN33/333,5","NXPLPC1114FHN33/333,5","NXP","ARM CM0",50,32,null,4,10,null,0,null,28,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,32,"HVQFN32",1.1499999999999999,null,1,null,null,null,null,null,null,null,"32kB flash, 8kB SRAM, HVQFN32 package",null,null,null,0,"No"]
["LPC1114LVFHI33/303","NXPLPC1114LVFHI33/303","NXP","ARM CM0",50,32,null,8,10,null,0,null,27,"No",1,1,null,"No",2,null,-40,85,1.65,1.95,32,"HVQFN32",1.02,null,1,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,0,"No"]
["LPC11A11FHN33/101,","NXPLPC11A11FHN33/101,","NXP","ARM CM0",50,8,1,2,10,null,1,null,28,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,32,"HVQFN32",0.95,null,1,null,null,null,null,null,null,null,"8kB flash, 2kB SRAM, HVQFN32 package",null,null,null,0,"No"]
["LPC11E14FBD48/401,","NXPLPC11E14FBD48/401,","NXP","ARM CM0",50,32,4,10,10,null,0,null,40,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,48,"LQFP48",1.1499999999999999,null,1,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,0,"No"]
["LPC11E37HFBD64QL","NXPLPC11E37HFBD64QL","NXP","ARM CM0",50,128,4,10,10,null,0,null,54,"No",2,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP64",1.85,null,2,null,null,null,null,null,null,null,"Scalable Entry Level 32bit Microcontroller (MCU) based on ARM CM0+/M0 Cores",null,null,null,0,"No"]
["LPC1224FBD64,151","NXPLPC1224FBD64,151","NXP","ARM CM0",45,4,null,4,10,null,0,null,55,"No",1,1,null,"No",2,null,-40,85,3.2,3.6,64,"LQFP64",1.71,null,2,null,null,null,null,null,null,null,"32kB flash, 4kB SRAM, LQFP64 package",null,null,null,0,"No"]
["LPC1225FBD64,151","NXPLPC1225FBD64,151","NXP","ARM CM0",45,80,null,8,10,null,0,null,55,"No",1,1,null,"No",2,null,-40,85,3.2,3.6,64,"LQFP64",1.52,null,2,null,null,null,null,null,null,null,"80kB flash, 8kB SRAM, LQFP64 package",null,null,null,0,"No"]
["LPC12D27FBD100/301","NXPLPC12D27FBD100/301","NXP","ARM CM0",45,128,null,8,10,null,0,null,40,"No",1,1,null,"No",2,null,-40,85,2,3.6,100,"LQFP100",2.12,null,2,null,null,null,null,null,null,null,"Robust and Reliable 32bit Microcontroller (MCU) based on ARM CM0 Core",null,null,null,0,"No"]
["LPC1315FHN33,551","NXPLPC1315FHN33,551","NXP","ARM CM3",72,32,2,8,12,null,0,null,28,"No",1,2,null,"No",2,null,-40,85,2,3.6,32,"HVQFN32",1.38,null,1,null,null,null,null,null,null,null,"Entrylevel 32bit Microcontroller (MCU) based on ARM CM3 Core",null,null,null,0,"No"]
["LPC1518JBD100E","NXPLPC1518JBD100E","NXP","ARM CM3",72,128,4,20,12,null,0,null,78,"No",1,2,null,"No",4,null,-40,105,2.4,3.6,100,"LQFP100",2.2599999999999998,null,3,null,null,null,null,null,null,null,"Motion Control 32bit Microcontroller based on ARM CM3",null,null,null,0,"No"]
["LPC1812JBD144E","NXPLPC1812JBD144E","NXP","ARM CM3",180,512,16,104,10,null,0,null,null,"No",2,3,null,"No",10,null,-40,105,2.4,3.6,144,"LQFP144",4.7699999999999996,null,4,null,null,null,null,null,null,null,"High Performance 32bit Microcontroller based on ARM CM3",null,null,null,0,"No"]
["LPC54101J256UK49Z","NXPLPC54101J256UK49Z","NXP","ARM CM4F",100,null,null,104,12,null,0,null,37,"No",3,null,null,"No",null,null,-40,105,1.62,3.6,null,"WLCSP",1.93,null,null,null,null,null,null,null,null,null,"Low Power 32bit Microcontroller (MCU) based on ARM CM4 Core",null,null,null,0,"No"]
["LPC804UKZ","NXPLPC804UKZ","NXP",null,15,32,null,null,0,null,0,null,17,"No",2,1,null,"No",null,null,0,null,1.71,3.6,20,"WLCSP20",0.44,null,2,null,null,null,null,null,null,null,null,null,null,null,0,"No"]
["MK02FN64VLH10","NXPMK02FN64VLH10","NXP","ARM CM4F",100,64,null,16,16,null,1,null,46,"No",1,1,null,"No",11,null,-40,105,1.71,3.6,64,"LQFP64",1.27,null,2,null,null,null,null,null,null,null,"Kinetis K02: 100MHz CortexM4F Performance MCU, 64KB Flash, 16KB SRAM, 64LQFP",null,null,null,0,"No"]
["MK10DX128VLL7","NXPMK10DX128VLL7","NXP","ARM CM4",72,160,2,32,16,null,1,null,70,"No",2,2,1,"No",13,null,-40,105,1.71,3.6,100,"LQFP100",3.03,null,5,null,null,null,null,null,null,null,"Kinetis K10: 72MHz CortexM4 Performance MCU, 160KB Flash, 32KB SRAM, 100LQFP",null,null,null,0,"Yes"]
["MK10DX256VMD10","NXPMK10DX256VMD10","NXP","ARM CM4",100,512,4,64,16,null,2,null,104,"No",2,3,1,"No",null,null,-40,105,1.71,3.6,144,"LBGA144",4.8,null,6,null,null,null,null,null,null,null,"Kinetis K10: 100MHz CortexM4 Performance MCU, 512KB Flash, 64KB SRAM, 144MAPBGA",null,null,null,0,"Yes"]
["MK10DX64VLH5","NXPMK10DX64VLH5","NXP","ARM CM4",50,96,2,16,16,null,0,null,44,"No",1,1,1,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.87,null,3,null,null,null,null,null,null,null,"Kinetis K10: 50MHz CortexM4 Performance MCU, 96KB Flash, 16KB SRAM, 64LQFP",null,null,null,0,"Yes"]
["MK11DX256AVMC5","NXPMK11DX256AVMC5","NXP","ARM CM4",50,320,4,32,16,null,1,null,64,"No",2,2,1,"No",13,null,-40,105,1.71,3.6,121,"LFBGA121",3.03,null,4,null,null,null,null,null,null,null,"Kinetis K11: 50MHz CortexM4 Performance MCU, 320KB Flash, 32KB SRAM, Antitamper, 121MAPBGA",null,null,null,0,"No"]
["MK30DX256VLL7","NXPMK30DX256VLL7","NXP","ARM CM4",72,288,2,64,16,null,1,null,68,"Yes",2,2,1,"No",13,null,-40,105,1.71,3.6,100,"LQFP100",3.87,null,5,null,null,null,null,null,null,null,"Kinetis K30: 72MHz CortexM4 Performance MCU, 288KB Flash, 64KB SRAM, Segment LCD, 100LQFP",null,null,null,0,"Yes"]
["MKE02Z32VLD4","NXPMKE02Z32VLD4","NXP","ARM CM0+",40,32,0.25600000000000001,4,12,null,2,null,37,"No",1,2,null,"No",10,null,-40,105,2.7,5.5,44,"LQFP44",0.93,null,3,null,null,null,null,null,null,null,"Kinetis KE02: 40MHz CortexM0+ 5V/Robust MCU, 32KB Flash, 4KB SRAM, 44LQFP",null,null,null,0,"No"]
["MKE04Z128VLD4","NXPMKE04Z128VLD4","NXP","ARM CM0+",48,128,null,16,12,null,2,null,38,"No",2,2,null,"No",10,null,-40,105,2.7,5.5,44,"LQFP44",1.38,null,3,null,null,null,null,null,null,null,"Kinetis KE04: 48MHz CortexM0+ 5V/Robust MCU, 128KB Flash, 16KB SRAM, 44LQFP",null,null,null,0,"No"]
["MKE04Z64VLK4","NXPMKE04Z64VLK4","NXP","ARM CM0+",48,64,null,8,12,null,2,null,71,"No",2,2,null,"No",10,null,-40,105,2.7,5.5,null,"LQFP",1.33,null,3,null,null,null,null,null,null,null,"Kinetis KE04: 48MHz CortexM0+ 5V/Robust MCU, 64KB Flash, 8KB SRAM, 80LQFP",null,null,null,0,"No"]
["MKE06Z128VLD4","NXPMKE06Z128VLD4","NXP","ARM CM0+",48,128,null,16,12,null,2,null,38,"No",2,2,null,"No",10,null,-40,105,2.7,5.5,44,"LQFP44",1.6,null,3,null,null,null,null,null,null,null,"Kinetis KE06: 48MHz CortexM0+ 5V/Robust MCU, 128KB Flash, 16KB SRAM, 44LQFP",null,null,null,0,"No"]
["MKE14Z256VLH7R","NXPMKE14Z256VLH7R","NXP","ARM CM0+",72,288,2,32,12,null,2,null,58,"No",2,2,null,"No",19,null,-40,105,2.7,5.5,64,"LQFP64",1.82,null,3,null,null,null,null,null,null,null,"Kinetis KE14Z: 72MHz CortexM0+ 5V/Robust MCU, 256KB Flash + 32KB FlexMem, 32KB RAM, 64LQFP",null,null,null,0,"No"]
["MKE15Z256VLH7","NXPMKE15Z256VLH7","NXP","ARM CM0+",72,288,2,32,12,null,2,null,58,"No",2,2,null,"No",19,null,-40,105,2.7,5.5,64,"LQFP64",1.9,null,3,null,null,null,null,null,null,null,"Kinetis KE15Z: 72MHz CortexM0+ 5V MCU, 256KB Flash+32KB FlexMem, 32KB RAM, Touch Interface, 64LQFP",null,null,null,0,"No"]
["MKE16Z64VLD4","NXPMKE16Z64VLD4","NXP","ARM CM0+",48,64,null,8,12,null,1,null,38,"No",1,1,null,"No",null,null,-40,105,2.7,5.5,44,"LQFP44",1.03,null,3,null,null,null,null,null,null,null,null,null,null,null,0,"No"]
["MKL02Z8VFG4","NXPMKL02Z8VFG4","NXP","ARM CM0+",48,8,null,1,12,null,0,null,14,"No",2,1,0,"No",null,null,-40,105,1.71,3.6,16,"HUQFN16",0.65,null,1,null,null,null,null,null,null,null,"Kinetis KL02: 48MHz CortexM0+ UltraLow Power MCU, 8KB Flash, 1KB SRAM, 16QFN",null,null,null,0,"No"]
["MKL04Z32VFK4R","NXPMKL04Z32VFK4R","NXP","ARM CM0+",48,32,null,4,12,null,0,null,22,"No",1,1,0,"No",null,null,-40,105,1.71,3.6,24,"HVQFN24",1.01,null,1,null,null,null,null,null,null,null,"Kinetis KL04: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, 24QFN",null,null,null,0,"No"]
["MKL05Z16VLC4","NXPMKL05Z16VLC4","NXP","ARM CM0+",48,16,null,2,12,null,1,null,28,"No",1,1,0,"No",null,null,-40,105,1.71,3.6,null,"LQFP",1.08,null,1,null,null,null,null,null,null,null,"Kinetis KL05: 48MHz CortexM0+ UltraLow Power MCU, 16KB Flash, 2KB SRAM, 32LQFP",null,null,null,0,"No"]
["MKL05Z32VLF4R","NXPMKL05Z32VLF4R","NXP","ARM CM0+",48,32,null,4,12,null,1,null,41,"No",1,1,0,"No",null,null,-40,105,1.71,3.6,48,"LQFP48",1.19,null,1,null,null,null,null,null,null,null,"Kinetis KL05: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, 48LQFP",null,null,null,0,"No"]
["MKL14Z32VFM4R","NXPMKL14Z32VFM4R","NXP","ARM CM0+",48,32,null,4,12,null,1,null,28,"No",2,2,0,"No",null,null,-40,105,1.71,3.6,32,"HVQFN32",1.45,null,3,null,null,null,null,null,null,null,"Kinetis KL14: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, 32QFN",null,null,null,0,"No"]
["MKL15Z128VFM4R","NXPMKL15Z128VFM4R","NXP","ARM CM0+",48,128,null,16,16,null,1,null,28,"No",2,2,0,"No",null,null,-40,105,1.71,3.6,32,"HVQFN32",1.9,null,3,null,null,null,null,null,null,null,"Kinetis KL15: 48MHz CortexM0+ UltraLow Power MCU, 128KB Flash, 16KB SRAM, 32QFN",null,null,null,0,"No"]
["MKL15Z32VLK4","NXPMKL15Z32VLK4","NXP","ARM CM0+",48,32,null,4,16,null,1,null,70,"Yes",2,2,0,"No",null,null,-40,105,1.71,3.6,80,"LQFP80",2.2400000000000002,null,3,null,null,null,null,null,null,null,"Kinetis KL15: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 4KB SRAM, 80LQFP",null,null,null,0,"No"]
["MKL16Z256VLH4R","NXPMKL16Z256VLH4R","NXP","ARM CM0+",48,256,null,32,16,null,1,null,54,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.91,null,3,null,null,null,null,null,null,null,"Kinetis KL16: 48MHz CortexM0+ UltraLow Power MCU, 256KB Flash, 32KB SRAM, 64LQFP",null,null,null,0,"No"]
["MKL16Z64VFT4","NXPMKL16Z64VFT4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,40,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,48,"HVQFN48",1.1000000000000001,null,3,null,null,null,null,null,null,null,"Kinetis KL16: 48MHz CortexM0+ UltraLow Power MCU, 64KB Flash, 8KB SRAM, 48QFN",null,null,null,0,"Yes"]
["MKL17Z32VFM4","NXPMKL17Z32VFM4","NXP","ARM CM0+",48,32,null,8,16,null,1,null,28,"Yes",2,2,0,"No",null,null,-40,105,1.71,3.6,32,"HUQFN32",0.87,null,3,null,null,null,null,null,null,null,"Kinetis KL17: 48MHz CortexM0+ UltraLow Power MCU, 32KB Flash, 8KB SRAM, 32QFN",null,null,null,0,"Yes"]
["MKL33Z256VMP4","NXPMKL33Z256VMP4","NXP","ARM CM0+",48,256,null,32,16,null,1,null,54,"Yes",2,2,1,"No",null,null,-40,105,1.71,3.6,64,"LFBGA64",2.04,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ core, 256KB Flash, 48MHz, Segment LCD, MAPBGA 64",null,null,null,0,"Yes"]
["MKL33Z64VLH4","NXPMKL33Z64VLH4","NXP","ARM CM0+",48,64,null,8,16,null,1,null,54,"Yes",2,2,0,"No",null,null,-40,105,1.71,3.6,64,"LQFP64",1.26,null,3,null,null,null,null,null,null,null,"Kinetis L 32bit MCU, ARM CM0+ Core, 64KB Flash, 48MHz, SLCD, LQFP 64",null,null,null,0,"Yes"]
["R5F562N7BDLE","RenesasR5F562N7BDLE","Renesas","RX",100,384,32,64,null,8,0,null,105,null,2,2,null,"Yes",20,null,-40,85,2.7,3.6,145,"145TFLGA",null,null,6,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,0,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56316CDLC","RenesasR5F56316CDLC","Renesas","RX",100,256,32,128,null,21,0,null,134,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,177,"177TFLGA",null,null,13,null,null,null,null,null,"Mass Production","IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56316DDLK","RenesasR5F56316DDLK","Renesas","RX",100,256,32,128,null,21,0,null,112,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,145,"145TFLGA",null,null,13,null,null,null,null,null,"Mass Production","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56317CDFC","RenesasR5F56317CDFC","Renesas","RX",100,384,32,128,null,21,0,null,134,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,176,"176LFQFP",null,null,13,null,null,null,null,null,"Mass Production","IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56317DDLC","RenesasR5F56317DDLC","Renesas","RX",100,384,32,128,null,21,0,null,134,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,177,"177TFLGA",null,null,13,null,null,null,null,null,"Mass Production","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56318DDFB","RenesasR5F56318DDFB","Renesas","RX",100,512,32,128,null,21,0,null,112,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,144,"144LFQFP",null,null,13,null,null,null,null,null,"Mass Production","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56318SDLK","RenesasR5F56318SDLK","Renesas","RX",100,512,32,128,null,21,0,null,112,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,145,"145TFLGA",null,null,13,null,null,null,null,null,"Mass Production","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5631ACDLK","RenesasR5F5631ACDLK","Renesas","RX",100,768,32,128,null,21,0,null,112,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,145,"145TFLGA",null,null,13,null,null,null,null,null,"Mass Production","IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5631ADGFC","RenesasR5F5631ADGFC","Renesas","RX",100,768,32,128,null,21,0,null,134,null,17,16,null,"Yes",26,null,-40,105,2.7,3.6,176,"176LFQFP",null,null,13,null,null,null,null,null,"Product Inquiry","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5631BDDLC","RenesasR5F5631BDDLC","Renesas","RX",100,1024,32,128,null,21,0,null,134,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,177,"177TFLGA",null,null,13,null,null,null,null,null,"Mass Production","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5631DCDFP","RenesasR5F5631DCDFP","Renesas","RX",100,1536,32,128,null,14,0,null,79,null,11,11,null,"Yes",20,null,-40,85,2.7,3.6,100,"100LFQFP",null,null,9,null,null,null,null,null,"Mass Production","IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5631DDGFP","RenesasR5F5631DDGFP","Renesas","RX",100,1536,32,128,null,14,0,null,79,null,11,11,null,"Yes",20,null,-40,105,2.7,3.6,100,"100LFQFP",null,null,9,null,null,null,null,null,"Product Inquiry","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5631EDDFB","RenesasR5F5631EDDFB","Renesas","RX",100,2048,32,128,null,21,0,null,112,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,144,"144LFQFP",null,null,13,null,null,null,null,null,"Mass Production","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5631GDGFP","RenesasR5F5631GDGFP","Renesas","RX",100,1536,32,192,null,14,0,null,79,null,11,11,null,"Yes",20,null,-40,105,2.7,3.6,100,"100LFQFP",null,null,9,null,null,null,null,null,"Product Inquiry","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5631MDDFL","RenesasR5F5631MDDFL","Renesas","RX",100,256,32,64,null,8,0,null,30,null,6,7,null,"Yes",20,null,-40,85,2.7,3.6,48,"48LFQFP",null,null,5,null,null,null,null,null,"Mass Production","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5631NDGFL","RenesasR5F5631NDGFL","Renesas","RX",100,384,32,64,null,8,0,null,30,null,6,7,null,"Yes",20,null,-40,105,2.7,3.6,48,"48LFQFP",null,null,5,null,null,null,null,null,"Product Inquiry","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5631PDGFL","RenesasR5F5631PDGFL","Renesas","RX",100,512,32,64,null,8,0,null,30,null,6,7,null,"Yes",20,null,-40,105,2.7,3.6,48,"48LFQFP",null,null,5,null,null,null,null,null,"Product Inquiry","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5631YDGFP","RenesasR5F5631YDGFP","Renesas","RX",100,1024,32,256,null,14,0,null,79,null,11,11,null,"Yes",20,null,-40,105,2.7,3.6,100,"100LFQFP",null,null,9,null,null,null,null,null,"Product Inquiry","CAN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563NACDLJ","RenesasR5F563NACDLJ","Renesas","RX",100,768,32,128,null,14,0,null,79,null,11,11,null,"Yes",20,null,-40,85,2.7,3.6,100,"100TFLGA",null,null,9,null,null,null,null,null,"Mass Production","EtherNet,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563NBCDFB","RenesasR5F563NBCDFB","Renesas","RX",100,1024,32,128,null,21,0,null,112,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,144,"144LFQFP",null,null,13,null,null,null,null,null,"Mass Production","EtherNet,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563NBDDFP","RenesasR5F563NBDDFP","Renesas","RX",100,1024,32,128,null,14,0,null,79,null,11,11,null,"Yes",20,null,-40,85,2.7,3.6,100,"100LFQFP",null,null,9,null,null,null,null,null,"Mass Production","CAN,EtherNet,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563NDDGFB","RenesasR5F563NDDGFB","Renesas","RX",100,1536,32,128,null,21,0,null,112,null,17,16,null,"Yes",26,null,-40,105,2.7,3.6,144,"144LFQFP",null,null,13,null,null,null,null,null,"Product Inquiry","CAN,EtherNet,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563NEDDFP","RenesasR5F563NEDDFP","Renesas","RX",100,2048,32,128,null,14,0,null,79,null,11,11,null,"Yes",20,null,-40,85,2.7,3.6,100,"100LFQFP",null,null,9,null,null,null,null,null,"Mass Production","CAN,EtherNet,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563NFDDFP","RenesasR5F563NFDDFP","Renesas","RX",100,2048,32,256,null,14,0,null,79,null,11,11,null,"Yes",20,null,-40,85,2.7,3.6,100,"100LFQFP",null,null,9,null,null,null,null,null,"Mass Production","CAN,EtherNet,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563NKDGFB","RenesasR5F563NKDGFB","Renesas","RX",100,2048,32,192,null,21,0,null,112,null,17,16,null,"Yes",26,null,-40,105,2.7,3.6,144,"144LFQFP",null,null,13,null,null,null,null,null,"Product Inquiry","CAN,EtherNet,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563NWHDFB","RenesasR5F563NWHDFB","Renesas","RX",100,1024,32,192,null,21,0,null,112,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,144,"144LFQFP",null,null,13,null,null,null,null,null,"Mass Production","CAN,EtherNet,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563NYDGFB","RenesasR5F563NYDGFB","Renesas","RX",100,1024,32,256,null,21,0,null,112,null,17,16,null,"Yes",26,null,-40,105,2.7,3.6,144,"144LFQFP",null,null,13,null,null,null,null,null,"Product Inquiry","CAN,EtherNet,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563TBBDFA","RenesasR5F563TBBDFA","Renesas","RX",100,256,32,24,null,8,0,null,93,null,7,7,null,"Yes",20,null,-40,85,2.7,3.6,120,"120LFQFP",null,null,5,null,null,null,null,null,"Mass Production","CAN,",null,null,null,0,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563TCADFB","RenesasR5F563TCADFB","Renesas","RX",100,384,32,32,null,8,0,null,110,null,7,7,null,"Yes",20,null,-40,85,4,5.5,144,"144LFQFP",null,null,5,null,null,null,null,null,"Mass Production","CAN,",null,null,null,0,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F563TEAGFA","RenesasR5F563TEAGFA","Renesas","RX",100,512,32,48,null,8,0,null,93,null,7,7,null,"Yes",20,null,-40,105,4,5.5,120,"120LFQFP",null,null,5,null,null,null,null,null,"Mass Production","CAN,",null,null,null,0,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56514BGFP","RenesasR5F56514BGFP","Renesas","RXv2",120,512,0,256,null,22,1,null,79,null,2,14,null,"Yes",26,"Independent Watch Dog Timer",-40,105,2.7,3.6,100,"100LFQFP",null,"QSPI, FIFO(2ch)",11,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56514FDLJ","RenesasR5F56514FDLJ","Renesas","RXv2",120,512,0,256,null,22,1,null,79,null,13,14,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,100,"100TFLGA",null,"QSPI, FIFO(2ch)",11,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56517BDLK","RenesasR5F56517BDLK","Renesas","RXv2",120,768,0,256,null,29,2,null,112,null,15,16,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,145,"145TFLGA",null,"QSPI, FIFO(2ch)",13,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56517FDFB","RenesasR5F56517FDFB","Renesas","RXv2",120,768,0,256,null,29,2,null,112,null,15,16,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,144,"144LFQFP",null,"QSPI, FIFO(2ch)",13,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56519ADFB","RenesasR5F56519ADFB","Renesas","RXv2",120,1024,0,256,null,29,2,null,112,null,15,16,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,144,"144LFQFP",null,"QSPI, FIFO(2ch)",13,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56519EGFP","RenesasR5F56519EGFP","Renesas","RXv2",120,1024,0,256,null,22,1,null,79,null,2,14,null,"Yes",26,"Independent Watch Dog Timer",-40,105,2.7,3.6,100,"100LFQFP",null,"QSPI, FIFO(2ch)",11,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5651CDDFC","RenesasR5F5651CDDFC","Renesas","RXv2",120,1536,32,640,null,29,2,null,137,null,3,16,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,176,"176LFQFP",null,"QSPI, FIFO(2ch)",13,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5651CHDLJ","RenesasR5F5651CHDLJ","Renesas","RXv2",120,1536,32,640,null,22,1,null,79,null,2,14,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,100,"100TFLGA",null,"QSPI, FIFO(2ch)",11,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F5651EHDLK","RenesasR5F5651EHDLK","Renesas","RXv2",120,2048,32,640,null,29,2,null,112,null,3,16,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,145,"145TFLGA",null,"QSPI, FIFO(2ch)",13,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F565N4AGFP","RenesasR5F565N4AGFP","Renesas","RXv2",120,512,0,256,null,22,1,null,79,null,2,14,null,"Yes",26,"Independent Watch Dog Timer",-40,105,2.7,3.6,100,"100LFQFP",null,"QSPI, FIFO(2ch)",11,null,null,null,null,null,"Mass Production","CAN,EtherNet,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F565N4FDFB","RenesasR5F565N4FDFB","Renesas","RXv2",120,512,0,256,null,29,2,null,112,null,15,16,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,144,"144LFQFP",null,"QSPI, FIFO(2ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F565N7ADLK","RenesasR5F565N7ADLK","Renesas","RXv2",120,768,0,256,null,29,2,null,112,null,15,16,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,145,"145TFLGA",null,"QSPI, FIFO(2ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F565N7EDFB","RenesasR5F565N7EDFB","Renesas","RXv2",120,768,0,256,null,29,2,null,112,null,15,16,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,144,"144LFQFP",null,"QSPI, FIFO(2ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F565N9ADFP","RenesasR5F565N9ADFP","Renesas","RXv2",120,1024,0,256,null,22,1,null,79,null,13,14,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,100,"100LFQFP",null,"QSPI, FIFO(2ch)",11,null,null,null,null,null,"Mass Production","CAN,EtherNet,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F565N9BGFB","RenesasR5F565N9BGFB","Renesas","RXv2",120,1024,0,256,null,29,2,null,112,null,2,16,null,"Yes",26,"Independent Watch Dog Timer",-40,105,2.7,3.6,144,"144LFQFP",null,"QSPI, FIFO(2ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F565N9FGFP","RenesasR5F565N9FGFP","Renesas","RXv2",120,1024,0,256,null,22,1,null,79,null,2,14,null,"Yes",26,"Independent Watch Dog Timer",-40,105,2.7,3.6,100,"100LFQFP",null,"QSPI, FIFO(2ch)",11,null,null,null,null,null,"Mass Production","CAN,EtherNet,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F565NEDDBG","RenesasR5F565NEDDBG","Renesas","RXv2",120,2048,32,640,null,29,2,null,137,null,3,16,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,176,"176LFBGA",null,"QSPI, FIFO(2ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F565NEDGFP","RenesasR5F565NEDGFP","Renesas","RXv2",120,2048,32,640,null,22,1,null,79,null,2,14,null,"Yes",26,"Independent Watch Dog Timer",-40,105,2.7,3.6,100,"100LFQFP",null,"QSPI, FIFO(2ch)",11,null,null,null,null,null,"Mass Production","CAN,EtherNet,LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F566TFCGFB","RenesasR5F566TFCGFB","Renesas","RXv3 core",160,512,32,128,null,30,2,null,119,null,8,8,null,"Yes",31,"3phase PWM Output: 4",-40,105,2.7,5.5,144,"144LFQFP",null,null,7,null,null,null,null,null,"Mass Production","CAN,LIN,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F566TKCGFP","RenesasR5F566TKCGFP","Renesas","RXv3 core",160,1024,32,128,null,22,2,null,78,null,8,8,null,"Yes",31,"3phase PWM Output: 3",-40,105,2.7,5.5,100,"100LFQFP",null,null,7,null,null,null,null,null,"New","CAN,LIN,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F572TKCDFB","RenesasR5F572TKCDFB","Renesas","RXv3 core",200,1024,32,128,null,30,2,null,119,null,8,8,null,"Yes",31,"3phase PWM Output: 4",-40,85,2.7,5.5,144,"144LFQFP",null,null,7,null,null,null,null,null,"Mass Production","CAN,LIN,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F572TKGDFP","RenesasR5F572TKGDFP","Renesas","RXv3 core",200,1024,32,128,null,22,2,null,78,null,8,8,null,"Yes",31,"3phase PWM Output: 3",-40,85,2.7,5.5,100,"100LFQFP",null,null,7,null,null,null,null,null,"New","CAN,LIN,",null,null,null,null,"USB2.0 Full Speed & USB OTG (OnTheGo) Support"]
["R5F56308DGFP","RenesasR5F56308DGFP","Renesas","RX",100,512,32,64,null,14,0,null,79,null,11,11,null,"Yes",20,null,-40,105,2.7,3.6,100,"100LFQFP",null,null,9,null,null,null,null,null,"Product Inquiry","CAN,IEBus,",null,null,null,0,"USB2.0 Full Speed Support"]
["R5F5630ADGFB","RenesasR5F5630ADGFB","Renesas","RX",100,768,32,96,null,21,0,null,118,null,17,16,null,"Yes",26,null,-40,105,2.7,3.6,144,"144LFQFP",null,null,13,null,null,null,null,null,"Product Inquiry","CAN,IEBus,",null,null,null,0,"USB2.0 Full Speed Support"]
["R5F5630DCDLK","RenesasR5F5630DCDLK","Renesas","RX",100,1536,32,128,null,21,0,null,118,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,145,"145TFLGA",null,null,13,null,null,null,null,null,"Mass Production","IEBus,",null,null,null,0,"USB2.0 Full Speed Support"]
["R5F5630ECDFC","RenesasR5F5630ECDFC","Renesas","RX",100,2048,32,128,null,21,0,null,149,null,17,16,null,"Yes",26,null,-40,85,2.7,3.6,176,"176LFQFP",null,null,13,null,null,null,null,null,"Mass Production","IEBus,",null,null,null,0,"USB2.0 Full Speed Support"]
["R5F564MFCDFP","RenesasR5F564MFCDFP","Renesas","RXv2",120,2048,64,512,null,22,1,null,79,null,9,8,null,"Yes",29,null,-40,85,2.7,3.6,100,"100LFQFP",null,"FIFO (2ch)",9,null,null,null,null,null,"Mass Production(*)","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MFDDFC","RenesasR5F564MFDDFC","Renesas","RXv2",120,2048,64,512,null,29,2,null,128,null,11,10,null,"Yes",29,null,-40,85,2.7,3.6,176,"176LFQFP",null,"FIFO (4ch)",13,null,null,null,null,null,"Mass Production(*)","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MFGDLJ","RenesasR5F564MFGDLJ","Renesas","RXv2",120,2048,64,512,null,22,1,null,79,null,9,8,null,"Yes",29,null,-40,85,2.7,3.6,100,"100TFLGA",null,"FIFO (2ch)",9,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MFHDLC","RenesasR5F564MFHDLC","Renesas","RXv2",120,2048,64,512,null,29,2,null,128,null,11,10,null,"Yes",29,null,-40,85,2.7,3.6,177,"177TFLGA",null,"FIFO (4ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MGCDFP","RenesasR5F564MGCDFP","Renesas","RXv2",120,2560,64,512,null,22,1,null,79,null,9,8,null,"Yes",29,null,-40,85,2.7,3.6,100,"100LFQFP",null,"FIFO (2ch)",9,null,null,null,null,null,"Mass Production(*)","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MGDDLK","RenesasR5F564MGDDLK","Renesas","RXv2",120,2560,64,512,null,29,2,null,112,null,11,10,null,"Yes",29,null,-40,85,2.7,3.6,145,"145TFLGA",null,"FIFO (4ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MGHGFB","RenesasR5F564MGHGFB","Renesas","RXv2",120,2560,64,512,null,29,2,null,112,null,11,10,null,"Yes",29,null,-40,105,2.7,3.6,144,"144LFQFP",null,"FIFO (4ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MJCDLK","RenesasR5F564MJCDLK","Renesas","RXv2",120,3072,64,512,null,29,2,null,112,null,11,10,null,"Yes",29,null,-40,85,2.7,3.6,145,"145TFLGA",null,"FIFO (4ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MJDGFP","RenesasR5F564MJDGFP","Renesas","RXv2",120,3072,64,512,null,22,1,null,79,null,9,8,null,"Yes",29,null,-40,105,2.7,3.6,100,"100LFQFP",null,"FIFO (2ch)",9,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MJGGFC","RenesasR5F564MJGGFC","Renesas","RXv2",120,3072,64,512,null,29,2,null,128,null,11,10,null,"Yes",29,null,-40,105,2.7,3.6,176,"176LFQFP",null,"FIFO (4ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MLCDFB","RenesasR5F564MLCDFB","Renesas","RXv2",120,4096,64,512,null,29,2,null,112,null,11,10,null,"Yes",29,null,-40,85,2.7,3.6,144,"144LFQFP",null,"FIFO (4ch)",13,null,null,null,null,null,"Mass Production(*)","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MLDDBG","RenesasR5F564MLDDBG","Renesas","RXv2",120,4096,64,512,null,29,2,null,128,null,11,10,null,"Yes",29,null,-40,85,2.7,3.6,176,"176LFBGA",null,"FIFO (4ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MLDGFP","RenesasR5F564MLDGFP","Renesas","RXv2",120,4096,64,512,null,22,1,null,79,null,9,8,null,"Yes",29,null,-40,105,2.7,3.6,100,"100LFQFP",null,"FIFO (2ch)",9,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F564MLHGFB","RenesasR5F564MLHGFB","Renesas","RXv2",120,4096,64,512,null,29,2,null,112,null,11,10,null,"Yes",29,null,-40,105,2.7,3.6,144,"144LFQFP",null,"FIFO (4ch)",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F56519BGFM","RenesasR5F56519BGFM","Renesas","RXv2",120,1024,0,256,null,10,1,null,43,null,2,11,null,"Yes",26,"Independent Watch Dog Timer",-40,105,2.7,3.6,64,"64LFQFP",null,"QSPI, FIFO(2ch)",9,null,null,null,null,null,"New","LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F56519FDBP","RenesasR5F56519FDBP","Renesas","RXv2",120,1024,0,256,null,10,0,null,43,null,2,11,null,"Yes",26,"Independent Watch Dog Timer",-40,85,2.7,3.6,64,"64LFBGA",null,"QSPI, FIFO(2ch)",9,null,null,null,null,null,"New","LIN,IEBus,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F571MFDDFB","RenesasR5F571MFDDFB","Renesas","RXv2",240,2048,64,512,null,29,2,null,112,null,11,11,null,"Yes",29,null,-40,85,2.7,3.6,144,"144LFQFP",null,"FIFO(4ch), QSPI",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F571MFGDLK","RenesasR5F571MFGDLK","Renesas","RXv2",240,2048,64,512,null,29,2,null,112,null,11,11,null,"Yes",29,null,-40,85,2.7,3.6,145,"145TFLGA",null,"FIFO(4ch), QSPI",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F571MGCGFB","RenesasR5F571MGCGFB","Renesas","RXv2",240,2560,64,512,null,29,2,null,112,null,11,11,null,"Yes",29,null,-40,105,2.7,3.6,144,"144LFQFP",null,"FIFO(4ch), QSPI",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F571MGGDFP","RenesasR5F571MGGDFP","Renesas","RXv2",240,2560,64,512,null,22,1,null,79,null,9,9,null,"Yes",29,null,-40,85,2.7,3.6,100,"100LFQFP",null,"FIFO(2ch), QSPI",9,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F571MGHGFB","RenesasR5F571MGHGFB","Renesas","RXv2",240,2560,64,512,null,29,2,null,112,null,11,11,null,"Yes",29,null,-40,105,2.7,3.6,144,"144LFQFP",null,"FIFO(4ch), QSPI",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F571MJDGFP","RenesasR5F571MJDGFP","Renesas","RXv2",240,3072,64,512,null,22,1,null,79,null,9,9,null,"Yes",29,null,-40,105,2.7,3.6,100,"100LFQFP",null,"FIFO(2ch), QSPI",9,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F571MLDDLJ","RenesasR5F571MLDDLJ","Renesas","RXv2",240,4096,64,512,null,22,1,null,79,null,9,9,null,"Yes",29,null,-40,85,2.7,3.6,100,"100TFLGA",null,"FIFO(2ch), QSPI",9,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F571MLDDLK","RenesasR5F571MLDDLK","Renesas","RXv2",240,4096,64,512,null,29,2,null,112,null,11,11,null,"Yes",29,null,-40,85,2.7,3.6,145,"145TFLGA",null,"FIFO(4ch), QSPI",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 Full Speed Support"]
["R5F51111AGNF","RenesasR5F51111AGNF","Renesas","RX",32,32,8,10,null,7,0,null,25,null,4,4,null,"Yes",8,null,-40,105,1.8,3.6,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0,"USB2.0 Full Speed/Low Speed & Battery Charging Support"]
["R5F51114ADNE","RenesasR5F51114ADNE","Renesas","RX",32,96,8,16,null,10,0,null,32,null,4,4,null,"Yes",8,null,-40,85,1.8,3.6,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0,"USB2.0 Full Speed/Low Speed & Battery Charging Support"]
["R5F51117AGFL","RenesasR5F51117AGFL","Renesas","RX",32,384,8,64,null,10,0,null,32,null,4,4,null,"Yes",8,null,-40,105,1.8,3.6,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0,"USB2.0 Full Speed/Low Speed & Battery Charging Support"]
["R5F5111JADNF","RenesasR5F5111JADNF","Renesas","RX",32,16,8,8,null,7,0,null,25,null,4,4,null,"Yes",8,null,-40,85,1.8,3.6,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0,"USB2.0 Full Speed/Low Speed & Battery Charging Support"]
["R5F51113AGFM","RenesasR5F51113AGFM","Renesas","RX",32,64,8,10,null,14,0,null,48,null,4,4,null,"Yes",8,null,-40,105,1.8,3.6,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0,"USB2.0 Full Speed/Low Speed & USB OTG (OnTheGo) & Battery Charging Support"]
["R5F51115AGFK","RenesasR5F51115AGFK","Renesas","RX",32,128,8,16,null,14,0,null,48,null,4,4,null,"Yes",8,null,-40,105,1.8,3.6,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0,"USB2.0 Full Speed/Low Speed & USB OTG (OnTheGo) & Battery Charging Support"]
["R5F5111JAGFM","RenesasR5F5111JAGFM","Renesas","RX",32,16,8,8,null,14,0,null,48,null,4,4,null,"Yes",8,null,-40,105,1.8,3.6,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production","",null,null,null,0,"USB2.0 Full Speed/Low Speed & USB OTG (OnTheGo) & Battery Charging Support"]
["R5F51135ADFP","RenesasR5F51135ADFP","Renesas","RX",32,128,8,32,null,17,2,null,84,null,9,9,null,"Yes",15,null,-40,85,1.8,3.6,100,"100LFQFP",null,null,8,null,null,null,null,null,"Mass Production","",null,null,null,"36segx8com(40segx4com)","USB2.0 Full Speed/Low Speed/USB2.0 low Speed & USB OTG (OnTheGo) & Battery Charging Support"]
["R5F10JBCGFP","RenesasR5F10JBCGFP","Renesas","RL78",24,32,2,5.5,null,0,0,null,22,null,3,0,null,"Yes",8,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,32,"32LQFP",null,null,1,null,null,null,null,null,"Mass Production","",null,null,null,null,"USB2.0 Full/Low Speed & Battery Charging Support"]
["R5F10KBCGNA","RenesasR5F10KBCGNA","Renesas","RL78",24,32,2,5.5,null,0,0,null,22,null,3,0,null,"Yes",8,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,32,"32HWQFN",null,null,1,null,null,null,null,null,"Mass Production","",null,null,null,null,"USB2.0 Full/Low Speed & Battery Charging Support"]
["R5F572MNDDBD","RenesasR5F572MNDDBD","Renesas","RXv3 core",240,4096,32,1024,null,29,2,null,183,null,16,16,null,"Yes",29,null,-40,85,2.7,3.6,224,"224LFBGA",null,"FIFO(5ch), QSPI",13,null,null,null,null,null,"New","CAN,EtherNet,",null,null,null,null,"USB2.0 Full/Low Speed Support"]
["R7FA6M3AF3CFC","RenesasR7FA6M3AF3CFC","Renesas","ARM CM4F",120,1024,64,640,null,24,2,null,133,null,3,2,null,"Yes",14,"16bit Asynchronous Timer x 2",-40,105,2.7,3.6,176,"176LFQFP",null,null,10,null,null,13,null,null,"New","CAN,EtherNet,LIN,SD/MMC",null,null,null,null,"USB2.0 High & Full Speed  & USB  OTG (OnTheGO) Support & USB Battery Charhing 1.2 Support"]
["R5F571MFGDLC","RenesasR5F571MFGDLC","Renesas","RXv2",240,2048,64,512,null,29,2,null,128,null,11,11,null,"Yes",29,null,-40,85,2.7,3.6,177,"177TFLGA",null,"FIFO(4ch), QSPI",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 High Speed Support"]
["R5F571MGCGFC","RenesasR5F571MGCGFC","Renesas","RXv2",240,2560,64,512,null,29,2,null,128,null,11,11,null,"Yes",29,null,-40,105,2.7,3.6,176,"176LFQFP",null,"FIFO(4ch), QSPI",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 High Speed Support"]
["R5F571MJGDBG","RenesasR5F571MJGDBG","Renesas","RXv2",240,3072,64,512,null,29,2,null,128,null,11,11,null,"Yes",29,null,-40,85,2.7,3.6,176,"176LFBGA",null,"FIFO(4ch), QSPI",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 High Speed Support"]
["R5F571MJGDFC","RenesasR5F571MJGDFC","Renesas","RXv2",240,3072,64,512,null,29,2,null,128,null,11,11,null,"Yes",29,null,-40,85,2.7,3.6,176,"176LFQFP",null,"FIFO(4ch), QSPI",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 High Speed Support"]
["R5F571MLHDLC","RenesasR5F571MLHDLC","Renesas","RXv2",240,4096,64,512,null,29,2,null,128,null,11,11,null,"Yes",29,null,-40,85,2.7,3.6,177,"177TFLGA",null,"FIFO(4ch), QSPI",13,null,null,null,null,null,"Mass Production","CAN,EtherNet,",null,null,null,null,"USB2.0 High Speed Support"]
["M262SIAAE","NuvotonM262SIAAE","Nuvoton","ARM CM23",64,512,null,96,null,16,2,2,51,null,3,4,4,"Yes",4,null,-40,105,1.8,3.6,64,"LQFP64",null,null,6,2.8,45,null,null,null,null,null,null,null,null,null,"Y"]
["GD32E230F8V6","GigaDeviceGD32E230F8V6","GigaDevice","ARM CM23",72,64,null,8,null,9,null,1,15,null,2,2,1,null,6,"SysTick, WDT, RTC",-40,85,1.8,3.6,20,"LGA20",null,2]
["GD32E230K8U6","GigaDeviceGD32E230K8U6","GigaDevice","ARM CM23",72,64,null,8,null,10,null,1,27,null,2,2,1,null,7,"SysTick, WDT, RTC",-40,85,1.8,3.6,32,"QFN32",null,2]
["GD32F101RDT6","GigaDeviceGD32F101RDT6","GigaDevice","ARM CM3",56,384,null,48,1,16,2,null,51,null,2,3,null,null,6,"SysTick, WDT, RTC",-40,85,2.6,3.6,64,"LQFP64",null,null,5]
["GD32F101TBU6","GigaDeviceGD32F101TBU6","GigaDevice","ARM CM3",56,128,null,16,1,10,null,null,26,null,1,1,null,null,3,"SysTick, WDT, RTC",-40,85,2.6,3.6,36,"QFN36",null,null,2]
["GD32F130F6P6","GigaDeviceGD32F130F6P6","GigaDevice","ARM CM3",48,32,null,4,null,9,null,null,15,null,1,1,null,null,7,"SysTick, WDT, RTC",-40,85,2.6,3.6,20,"TSSOP20",null,null,2]
["GD32F130F8P6","GigaDeviceGD32F130F8P6","GigaDevice","ARM CM3",48,64,null,8,null,9,null,null,15,null,2,2,null,null,7,"SysTick, WDT, RTC",-40,85,2.6,3.6,20,"TSSOP20",null,null,2]
["GD32F170T8U6","GigaDeviceGD32F170T8U6","GigaDevice","ARM CM3",48,64,null,8,null,10,null,null,null,null,3,3,null,null,8,"SysTick, WDT, RTC",-40,85,2.5,5.5,36,"QFN36",null,null,2]
["GD32F330G6U6","GigaDeviceGD32F330G6U6","GigaDevice","ARM CM4",84,32,null,4,null,10,null,null,23,null,1,1,null,null,7,"SysTick, WDT, RTC",-40,85,2.6,3.6,28,"QFN28",null,null,2]
["HC16LC16J6UAQN48","HUADAHC16LC16J6UAQN48","HUADA","8bit 8051 MCU",16,32,null,4,null,7,null,1,34,null,1,1,null,null,8,null,-40,85,1.8,3.8,48,"QFN48（6*6）",null,null,2]
["HC32F005C6PASOP20","HUADAHC32F005C6PASOP20","HUADA","ARM CM0+",32,32,null,4,null,9,null,2,"16+1",null,1,1,null,null,6,null,-40,85,1.8,5.5,20,"SOP20",null,null,2]
["HC32F072JATALQ48","HUADAHC32F072JATALQ48","HUADA","ARM CM0+",48,128,null,16,null,17,2,3,36,null,2,2,null,null,7,null,-40,85,1.8,5.5,48,"LQFP48（7*7）",null,null,2]
["HC32F176KATALQ64","HUADAHC32F176KATALQ64","HUADA","ARM CM0+",48,128,null,16,null,23,1,3,56,null,2,2,null,null,7,null,-40,85,1.8,5.5,64,"LQFP64（7*7）",null,null,4]
["HC32L110B4PATSSOP16TR","HUADAHC32L110B4PATSSOP16TR","HUADA","ARM CM0+",32,16,null,2,null,6,null,2,"12+1",null,1,1,null,null,6,null,-40,85,1.8,5.5,16,"TSSOP16",null,null,2]
["HC32L110B6PATSSOP16","HUADAHC32L110B6PATSSOP16","HUADA","ARM CM0+",32,32,null,4,null,6,null,2,"12+1",null,1,1,null,null,6,null,-40,85,1.8,5.5,16,"TSSOP16",null,null,2]
["HC32L176KATALQ64","HUADAHC32L176KATALQ64","HUADA","ARM CM0+",48,128,null,16,null,23,1,3,56,null,2,2,null,null,7,null,-40,85,1.8,5.5,64,"LQFP64（7*7）",null,null,4]
["HC32M140J8UAQFN48","HUADAHC32M140J8UAQFN48","HUADA","ARM CM0+",48,64,null,8,null,16,null,1,41,null,4,4,null,null,5,null,-40,85,2.7,5.5,48,"QFN48（7*7）",null,null,4]
["MS51XB9AE","NuvotonMS51XB9AE","Nuvoton","8bit 8051 MCU",24,16,null,1,null,8,null,null,18,null,1,1,null,null,4,null,-40,105,2.4,5.5,20,"QFN20",null,null,2,null,null,null,null,null,null,null,"1T 8051， 24 MHz internal RC， KBI， onchip debugger"]
["N79E825","NuvotonN79E825","Nuvoton","8bit 8051 MCU",20,16,null,0.25,null,4,null,2,18,null,1,null,null,null,2,null,-40,85,2.4,5.5,20,"SOP20/PDIP20",null,null,1,null,null,null,null,null,null,null,"internal 6 MHz RC， KBI， BOR"]
["ML51EC0AE","NuvotonML51EC0AE","Nuvoton","8bit 8051 MCU",24,32,null,2,null,8,null,2,24,null,2,2,null,null,4,null,-40,105,1.8,5.5,28,"TSSOP28",null,null,2,null,null,null,null,null,null,null,"1T 8051， 24 MHz internal RC， KBI， onchip debugger"]
["ML51XB9AE","NuvotonML51XB9AE","Nuvoton","8bit 8051 MCU",24,16,null,1,null,6,null,null,17,null,2,1,null,null,4,null,-40,105,1.8,5.5,20,"QFN20",null,null,2,null,null,null,null,null,null,null,"1T 8051， 24 MHz internal RC， KBI， onchip debugger"]
["M052ZDN","NuvotonM052ZDN","Nuvoton","ARM CM0",50,8,null,4,null,5,null,4,24,null,2,1,null,null,4,null,-40,85,2.5,5.5,33,"QFN33",null,null,2]
["M054LDE","NuvotonM054LDE","Nuvoton","ARM CM0",50,16,null,4,null,8,null,4,40,null,2,2,null,null,4,null,-40,105,2.5,5.5,48,"LQFP48",null,null,2]
["M0564LE4AE","NuvotonM0564LE4AE","Nuvoton","ARM CM0",72,128,null,20,null,10,null,2,41,null,2,2,null,null,4,null,-40,105,2.5,5.5,48,"LQFP48",null,null,3]
["M451RD3AE","NuvotonM451RD3AE","Nuvoton","ARM CM4F",72,72,null,16,null,16,1,2,53,null,2,2,1,null,4,null,-40,105,2.5,5.5,64,"LQFP64",null,null,5]
["MINI51ZDE","NuvotonMINI51ZDE","Nuvoton","ARM CM0",50,4,null,2,null,8,null,2,29,null,1,1,null,null,2,null,-40,105,2.1,5.5,33,"QFN33",null,null,1]
["MINI54FDE","NuvotonMINI54FDE","Nuvoton","ARM CM0",50,16,null,2,null,4,null,null,17,null,1,1,null,null,2,null,-40,105,2.1,5.5,20,"TSSOP20",null,null,1]
["NANO100KD3BN","NuvotonNANO100KD3BN","Nuvoton","ARM CM0",42,64,null,16,null,12,2,null,86,null,2,3,null,null,4,null,-40,85,1.8,3.6,128,"LQFP128",null,null,5]
["NANO100NE3BN","NuvotonNANO100NE3BN","Nuvoton","ARM CM0",42,128,null,16,null,7,2,null,38,null,2,3,null,null,4,null,-40,85,1.8,3.6,48,"QFN48",null,null,4]
["NANO110KC2BN","NuvotonNANO110KC2BN","Nuvoton","ARM CM0",42,32,null,8,null,12,2,null,86,null,2,3,null,null,4,null,-40,85,1.8,3.6,128,"LQFP128",null,null,5,null,null,null,null,null,null,null,null,null,null,"4x40， 6x38"]
["NANO110SD2BN","NuvotonNANO110SD2BN","Nuvoton","ARM CM0",42,64,null,8,null,7,2,null,51,null,2,3,null,null,4,null,-40,85,1.8,3.6,64,"LQFP64(7x7mm)",null,null,5,null,null,null,null,null,null,null,null,null,null,"4x31， 6x29"]
["NUC100RD1DN","NuvotonNUC100RD1DN","Nuvoton","ARM CM0",72,64,null,4,null,8,null,2,51,null,2,2,null,null,4,null,-40,85,2.5,5.5,64,"LQFP64",null,null,3]
["NUC130LE3CN","NuvotonNUC130LE3CN","Nuvoton","ARM CM0",72,128,null,16,null,8,null,1,35,null,2,1,null,null,4,null,-40,85,2.5,5.5,48,"LQFP48",null,null,3,null,null,null,null,null,null,"CAN"]
["NUC230SD2AE","NuvotonNUC230SD2AE","Nuvoton","ARM CM0",72,64,null,8,null,7,null,2,49,null,2,2,null,null,4,null,-40,105,2.5,5.5,64,"LQFP64(7x7mm)",null,null,5,null,null,null,null,null,null,"CAN"]
["N78E366A","NuvotonN78E366A","Nuvoton","8bit 8051 MCU",40,64,null,1.25,null,null,null,null,40,null,null,1,null,null,3,null,-40,85,2.4,5.5,40,"PDIP40/PLCC44/PQFP44/LQFP48",null,null,1,null,null,null,null,null,null,null,"6T/12T option， Extra I/O port， internal 22 MHz RC， 4 level BOR"]
["W78E052D","NuvotonW78E052D","Nuvoton","8bit 8051 MCU",40,8,null,0.25,null,null,null,null,36,null,null,null,null,null,3,null,-40,85,2.4,5.5,40,"PDIP40/PLCC44/PQFP44/LQFP48/TQFP44",null,null,1,null,null,null,null,null,null,null,"6T/12T option， Extra I/O port"]
["W79E658A","NuvotonW79E658A","Nuvoton","8bit 8051 MCU",40,128,null,1.25,null,8,null,null,60,null,2,null,null,null,3,null,-40,85,2.4,5.5,100,"PQFP100",null,null,1,null,null,null,null,null,null,null,"JTAG interface， Extra I/O port"]
["UPD78F0842GKA2GAKG","RenesasUPD78F0842GKA2GAKG","Renesas","78K0",20,24,0,2,null,0,0,null,63,null,1,0,null,null,7,null,-40,105,2.7,5.5,80,"80LFQFP",null,null,2,null,null,null,null,null,"Mass Production","LIN,",null,null,null,"seg=28, com=4"]
["UPD78F0881AGBAGAFG","RenesasUPD78F0881AGBAGAFG","Renesas","78K0",20,32,0,2,null,0,0,null,37,null,0,0,null,null,6,null,-40,85,1.8,5.5,44,"44LQFP",null,null,2,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["UPD78F0895AGAAGAMG","RenesasUPD78F0895AGAAGAMG","Renesas","78K0",20,128,0,7,null,0,0,null,41,null,0,0,null,null,6,null,-40,85,1.8,5.5,48,"48LFQFP",null,null,2,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["UPD78F0750MAFAAAX","RenesasUPD78F0750MAFAAAX","Renesas","78K0",10,4,0,0.375,null,0,0,null,12,null,0,0,null,null,5,null,-40,105,2.7,5.5,16,"16SSOP",null,null,0,null,null,null,null,null,"Nonpromotion",""]
["UPD78F0756K83B4AX","RenesasUPD78F0756K83B4AX","Renesas","78K0",10,16,0,0.75,null,0,0,null,23,null,1,0,null,null,5,null,-40,105,2.7,5.5,32,"32HWQFN",null,null,1,null,null,null,null,null,"Nonpromotion",""]
["UPD78F0133HGK9ETA","RenesasUPD78F0133HGK9ETA","Renesas","78K0",16,24,null,1,null,null,null,null,null,null,null,null,null,null,6,null,-40,85,null,null,64,"64TQFP",null,null,null,null,null,null,null,null,"Mass Production","LIN,IEBus,"]
["UPD78F0501AFCAA3A","RenesasUPD78F0501AFCAA3A","Renesas","78K0",20,16,0,0.75,null,0,0,null,23,null,1,0,null,null,5,null,-40,85,1.8,5.5,36,"36VFLGA",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0503DAMCCABAX","RenesasUPD78F0503DAMCCABAX","Renesas","78K0",20,32,0,1,null,0,0,null,23,null,1,0,null,null,5,null,-40,85,1.8,5.5,30,"30LSSOP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0511AMCA2GAAG","RenesasUPD78F0511AMCA2GAAG","Renesas","78K0",20,16,0,0.75,null,0,0,null,31,null,1,0,null,null,5,null,-40,125,2.7,5.5,38,38,null,null,2,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F0512AMCGAAAX","RenesasUPD78F0512AMCGAAAX","Renesas","78K0",20,24,0,1,null,0,0,null,31,null,1,0,null,null,5,null,-40,85,1.8,5.5,38,"38SSOP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0517DAGAGAMAX","RenesasUPD78F0517DAGAGAMAX","Renesas","78K0",20,128,0,7,null,0,0,null,41,null,1,0,null,null,5,null,-40,85,1.8,5.5,48,"48LFQFP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0525AGBAGAGG","RenesasUPD78F0525AGBAGAGG","Renesas","78K0",20,60,0,3,null,0,0,null,45,null,1,0,null,null,5,null,-40,85,1.8,5.5,52,52,null,null,2,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F0531AFCAA1A","RenesasUPD78F0531AFCAA1A","Renesas","78K0",20,16,0,0.75,null,0,0,null,55,null,1,0,null,null,5,null,-40,85,1.8,5.5,64,"64VFLGA",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0532AGBA2GAHG","RenesasUPD78F0532AGBA2GAHG","Renesas","78K0",20,24,0,1,null,0,0,null,55,null,1,0,null,null,5,null,-40,125,2.7,5.5,64,64,null,null,2,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F0533AFCAA1A","RenesasUPD78F0533AFCAA1A","Renesas","78K0",20,32,0,1,null,0,0,null,55,null,1,0,null,null,5,null,-40,85,1.8,5.5,64,"64VFLGA",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0533AGKAGAJG","RenesasUPD78F0533AGKAGAJG","Renesas","78K0",20,32,0,1,null,0,0,null,55,null,1,0,null,null,5,null,-40,85,1.8,5.5,64,64,null,null,2,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F0535AFCAA1A","RenesasUPD78F0535AFCAA1A","Renesas","78K0",20,60,0,3,null,0,0,null,55,null,1,0,null,null,6,null,-40,85,1.8,5.5,64,"64VFLGA",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0536AFCAA1A","RenesasUPD78F0536AFCAA1A","Renesas","78K0",20,96,0,5,null,0,0,null,55,null,1,0,null,null,6,null,-40,85,1.8,5.5,64,"64VFLGA",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0537DAF1AA2A","RenesasUPD78F0537DAF1AA2A","Renesas","78K0",20,128,0,7,null,0,0,null,55,null,1,0,null,null,6,null,-40,85,1.8,5.5,64,64,null,null,2,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F0545AGCA2GADG","RenesasUPD78F0545AGCA2GADG","Renesas","78K0",20,60,0,3,null,0,0,null,71,null,1,0,null,null,6,null,-40,125,2.7,5.5,80,80,null,null,2,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F0546AGKA2GAKG","RenesasUPD78F0546AGKA2GAKG","Renesas","78K0",20,96,0,5,null,0,0,null,71,null,1,0,null,null,6,null,-40,125,2.7,5.5,80,80,null,null,2,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F0592GAGAMAX","RenesasUPD78F0592GAGAMAX","Renesas","78K0",20,16,0,1,null,12,0,null,40,null,1,0,null,null,5,null,-40,85,1.8,5.5,48,"48LFQFP",null,null,1,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0550MAFAAAX","RenesasUPD78F0550MAFAAAX","Renesas","78K0",10,4,0,0.375,null,0,0,null,12,null,1,0,null,null,3,null,-40,85,1.8,5.5,16,"16SSOP",null,null,1,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0565MCCAAAX","RenesasUPD78F0565MCCAAAX","Renesas","78K0",10,4,0,0.375,null,0,0,null,16,null,1,0,null,null,3,null,-40,85,1.8,5.5,20,"20LSSOP",null,null,1,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0567MCCAAAX","RenesasUPD78F0567MCCAAAX","Renesas","78K0",10,16,0,0.75,null,0,0,null,16,null,1,0,null,null,3,null,-40,85,1.8,5.5,20,"20LSSOP",null,null,1,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0581K84B4AX","RenesasUPD78F0581K84B4AX","Renesas","78K0",10,8,0,0.5,null,0,0,null,34,null,1,0,null,null,5,null,-40,85,1.8,5.5,40,"40HWQFN",null,null,1,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F0588GAGAMAX","RenesasUPD78F0588GAGAMAX","Renesas","78K0",10,32,0,1,null,0,0,null,42,null,1,0,null,null,5,null,-40,85,1.8,5.5,48,"48LFQFP",null,null,1,null,null,null,null,null,"Mass Production","LIN,"]
["UPD78F0441GKGAJAX","RenesasUPD78F0441GKGAJAX","Renesas","78K0",10,16,0,0.75,null,0,0,null,46,null,0,0,null,null,7,null,-40,85,1.8,5.5,64,"64LQFP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,",null,null,null,"seg=28, com=8 or seg=32, com=4"]
["UPD78F0444GKGAJAX","RenesasUPD78F0444GKGAJAX","Renesas","78K0",10,48,0,2,null,0,0,null,46,null,0,0,null,null,7,null,-40,85,1.8,5.5,64,"64LQFP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,",null,null,null,"seg=28, com=8 or seg=32, com=4"]
["UPD78F0454GAHABAX","RenesasUPD78F0454GAHABAX","Renesas","78K0",10,48,0,2,null,0,0,null,46,null,0,0,null,null,7,null,-40,85,1.8,5.5,64,"64TFQFP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,",null,null,null,"seg=28, com=8 or seg=32, com=4"]
["UPD78F0462GKGAJAX","RenesasUPD78F0462GKGAJAX","Renesas","78K0",10,24,0,1,null,0,0,null,46,null,0,0,null,null,7,null,-40,85,1.8,5.5,64,"64LQFP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,",null,null,null,"seg=20, com=8 or seg=24, com=4"]
["UPD78F0472GCGADAX","RenesasUPD78F0472GCGADAX","Renesas","78K0",10,24,0,1,null,0,0,null,62,null,0,0,null,null,7,null,-40,85,1.8,5.5,80,"80LQFP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,",null,null,null,"seg=36, com=8 or seg=40, com=4"]
["UPD78F0483GKGAKAX","RenesasUPD78F0483GKGAKAX","Renesas","78K0",10,32,0,1,null,0,0,null,62,null,0,0,null,null,7,null,-40,85,1.8,5.5,80,"80LFQFP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,",null,null,null,"seg=36, com=8 or seg=40, com=4"]
["UPD78F0493GCGADAX","RenesasUPD78F0493GCGADAX","Renesas","78K0",10,32,0,1,null,0,0,null,62,null,0,0,null,null,7,null,-40,85,1.8,5.5,80,"80LQFP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,",null,null,null,"seg=28, com=8 or seg=32, com=4"]
["UPD78F1036AGBGAHAX","RenesasUPD78F1036AGBGAHAX","Renesas","78K0R",20,64,0,4,null,0,0,null,55,null,2,0,null,null,21,"16bit wakeup timer:1 channel",-40,85,2.7,5.5,64,64,null,0,4,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["UPD78F1213MCGAAAX","RenesasUPD78F1213MCGAAAX","Renesas","78K0R",20,32,0,1.5,null,0,0,null,31,null,2,0,null,null,12,null,-40,85,2.7,5.5,38,"38SSOP",null,0,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F1234GKGAJAX","RenesasUPD78F1234GKGAJAX","Renesas","78K0R",20,48,0,2,null,0,0,null,55,null,2,0,null,null,12,null,-40,85,2.7,5.5,64,"64LQFP",null,0,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F1143AGB(A)GAHAX","RenesasUPD78F1143AGB(A)GAHAX","Renesas","78K0R",20,96,0,6,null,0,0,null,55,null,2,0,null,null,8,null,-40,85,1.8,5.5,64,64,null,0,3,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F1144AGK(A)GAJAX","RenesasUPD78F1144AGK(A)GAJAX","Renesas","78K0R",20,128,0,8,null,0,0,null,55,null,2,0,null,null,8,null,-40,85,1.8,5.5,64,64,null,0,3,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F1146AGB(A)GAHAX","RenesasUPD78F1146AGB(A)GAHAX","Renesas","78K0R",20,256,0,12,null,0,0,null,55,null,2,0,null,null,8,null,-40,85,1.8,5.5,64,64,null,0,3,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F1154AGKGAKAX","RenesasUPD78F1154AGKGAKAX","Renesas","78K0R",20,128,0,8,null,0,0,null,70,null,3,0,null,null,8,null,-40,85,1.8,5.5,80,"80LFQFP",null,0,4,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F1155AGK(A)GAKAX","RenesasUPD78F1155AGK(A)GAKAX","Renesas","78K0R",20,192,0,10,null,0,0,null,70,null,3,0,null,null,8,null,-40,85,1.8,5.5,80,80,null,0,4,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F1163AGCUEUAX","RenesasUPD78F1163AGCUEUAX","Renesas","78K0R",20,96,0,6,null,0,0,null,88,null,3,0,null,null,8,null,-40,85,1.8,5.5,100,"100LFQFP",null,0,1,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F1167AGFGASAX","RenesasUPD78F1167AGFGASAX","Renesas","78K0R",20,384,0,24,null,0,0,null,88,null,3,0,null,null,8,null,-40,85,1.8,5.5,100,"100LQFP",null,0,1,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F1175AGFGATAX","RenesasUPD78F1175AGFGATAX","Renesas","78K0R",20,192,0,10,null,0,0,null,116,null,5,0,null,null,12,null,-40,85,1.8,5.5,128,"128LFQFP",null,0,4,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F1187AGJGAEAX","RenesasUPD78F1187AGJGAEAX","Renesas","78K0R",20,384,0,24,null,0,0,null,132,null,5,0,null,null,12,null,-40,85,1.8,5.5,144,"144LFQFP",null,0,4,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F1000GBGAFAX","RenesasUPD78F1000GBGAFAX","Renesas","78K0R",20,16,0,1,null,0,0,null,37,null,1,0,null,null,8,null,-40,85,1.8,5.5,44,"44LQFP",null,0,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F1007GBGAHAX","RenesasUPD78F1007GBGAHAX","Renesas","78K0R",20,32,0,1.5,null,0,0,null,55,null,2,0,null,null,8,null,-40,85,1.8,5.5,64,"64LFQFP",null,0,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F1009GAHABAX","RenesasUPD78F1009GAHABAX","Renesas","78K0R",20,64,0,3,null,0,0,null,55,null,2,0,null,null,8,null,-40,85,1.8,5.5,64,"64TFQFP",null,0,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F1013F1BAKA","RenesasUPD78F1013F1BAKA","Renesas","78K0R",20,96,0,6,null,0,0,null,89,null,3,0,null,null,12,null,-40,85,1.8,5.5,100,"100TFBGA",null,0,4,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F1030GFGASAX","RenesasUPD78F1030GFGASAX","Renesas","78K0R",20,256,0,12,null,0,0,null,89,null,3,0,null,null,12,null,-40,85,1.8,5.5,100,"100LQFP",null,0,4,null,null,null,null,null,"Nonpromotion","LIN,"]
["UPD78F8070GCUEUAX","RenesasUPD78F8070GCUEUAX","Renesas","78K0R",20,128,0,7,null,null,0,null,45,null,2,0,null,null,12,null,-40,85,1.8,3.6,100,100,null,null,3,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD78F9221MC(A2)CAAAX","RenesasUPD78F9221MC(A2)CAAAX","Renesas","78K0S",10,2,0,0.125,null,0,0,null,17,null,0,0,null,null,3,null,-40,125,2,5.5,20,"20LSSOP",null,null,1,null,null,null,null,null,"Mass Production","LIN,"]
["UPD780023AF1CN3A","RenesasUPD780023AF1CN3A","Renesas","78K0",12,24,0,1,null,0,0,null,51,null,0,0,null,null,3,null,-40,85,1.8,5.5,73,"73LFBGA",null,null,1,null,null,null,null,null,"Mass Production",""]
["UPD780024ASGB(A)8ETA","RenesasUPD780024ASGB(A)8ETA","Renesas","78K0",12,32,0,1,null,0,0,null,39,null,0,0,null,null,3,null,-40,85,1.8,5.5,52,"52LQFP",null,null,1,null,null,null,null,null,"Mass Production",""]
["UPD780033AGC(A)8BSA","RenesasUPD780033AGC(A)8BSA","Renesas","78K0",12,24,0,1,null,0,0,null,51,null,0,0,null,null,3,null,-40,85,1.8,5.5,64,"64LQFP",null,null,1,null,null,null,null,null,"Mass Production",""]
["UPD78F0034AYCWA","RenesasUPD78F0034AYCWA","Renesas","78K0",8,32,0,1,null,0,0,null,51,null,1,0,null,null,3,null,-40,85,1.8,5.5,64,"64SDIP",null,null,1,null,null,null,null,null,"Mass Production",""]
["UPD780055YGC(A)8BTA","RenesasUPD780055YGC(A)8BTA","Renesas","78K0",5,40,0,1,null,0,0,null,68,null,1,0,null,null,3,null,-40,85,1.8,5.5,80,"80LQFP",null,null,1,null,null,null,null,null,"Mass Production",""]
["UPD78F0862MC(A)5A4A","RenesasUPD78F0862MC(A)5A4A","Renesas","78K0",10,16,0,0.75,null,0,0,null,14,null,0,0,null,null,4,null,-40,85,2.7,5.5,20,20,null,null,1,null,null,null,null,null,"Product Inquiry","LIN,"]
["UPD789134AMC5A4A","RenesasUPD789134AMC5A4A","Renesas","78K0S",4,8,0,0.25,null,0,0,null,20,null,0,0,null,null,2,null,-40,85,1.8,5.5,30,30,null,null,1,null,null,null,null,null,"Product Inquiry",""]
["UPD78F9436GK9ETA","RenesasUPD78F9436GK9ETA","Renesas","78K0S",5,16,0,0.5,null,0,0,null,40,null,0,0,null,null,3,null,-40,85,1.8,5.5,64,"64TQFP",null,null,1,null,null,null,null,null,"Mass Production","",null,null,null,"seg=5, com=4"]
["UPD78F8024GKGAJAX","RenesasUPD78F8024GKGAJAX","Renesas","78K0",20,8,0,0.5,null,0,0,null,23,null,1,0,null,null,5,null,-40,85,1.8,5.5,64,64,null,null,2,null,null,null,null,null,"Product Inquiry","LIN,"]
["R5F21184SP","RenesasR5F21184SP","Renesas","R8C",20,16,0,1,null,0,0,null,13,null,0,0,null,null,3,null,-20,85,2.7,5.5,20,"20LSSOP",null,null,2,null,null,null,null,null,"Nonpromotion",""]
["R5F211A2SP","RenesasR5F211A2SP","Renesas","R8C",20,8,0,0.5,null,0,0,null,13,null,1,0,null,null,3,null,-20,85,2.7,5.5,20,"20LSSOP",null,null,2,null,null,null,null,null,"Nonpromotion",""]
["R5F211B2SP","RenesasR5F211B2SP","Renesas","R8C",20,8,2,0.5,null,0,0,null,13,null,1,0,null,null,3,null,-20,85,2.7,5.5,20,"20LSSOP",null,null,2,null,null,null,null,null,"Nonpromotion",""]
["R5F21245SNFP","RenesasR5F21245SNFP","Renesas","R8C",20,24,0,2,null,0,0,null,41,null,1,0,null,null,5,null,-20,85,2.2000000000000002,5.5,52,"52LQFP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F21257SDFP","RenesasR5F21257SDFP","Renesas","R8C",20,48,2,2.5,null,0,0,null,41,null,1,0,null,null,5,null,-40,85,2.2000000000000002,5.5,52,"52LQFP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F21282SNSP","RenesasR5F21282SNSP","Renesas","R8C",20,8,0,0.5,null,0,0,null,13,null,1,0,null,null,4,null,-20,85,2.2000000000000002,5.5,20,"20LSSOP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F212L4SDFP","RenesasR5F212L4SDFP","Renesas","R8C",20,16,2,1.5,null,0,0,null,25,null,0,0,null,null,5,null,-40,85,2.2000000000000002,5.5,32,"32LQFP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F21321DNSP","RenesasR5F21321DNSP","Renesas","R8C",20,4,0,1,null,0,0,null,15,null,1,0,null,null,4,null,-20,85,1.8,5.5,20,"20LSSOP",null,null,2,null,null,null,null,null,"Nonpromotion",""]
["R5F21324HJSP","RenesasR5F21324HJSP","Renesas","R8C",20,16,0,1.5,null,0,0,null,15,null,1,0,null,null,5,null,-40,85,2.7,5.5,20,20,null,null,2,null,null,null,null,null,"Nonpromotion","LIN,IEBus,"]
["R5F21332CNFP","RenesasR5F21332CNFP","Renesas","R8C",20,8,4,1,null,0,0,null,27,null,2,0,null,null,4,null,-20,85,1.8,5.5,32,"32LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F21332DDFP","RenesasR5F21332DDFP","Renesas","R8C",20,8,0,1,null,0,0,null,27,null,1,0,null,null,4,null,-40,85,1.8,5.5,32,"32LQFP",null,null,2,null,null,null,null,null,"Nonpromotion(*)",""]
["R5F21334GKFP","RenesasR5F21334GKFP","Renesas","R8C",20,16,4,1.5,null,0,0,null,27,null,1,0,null,null,5,null,-40,125,2.7,5.5,32,32,null,null,2,null,null,null,null,null,"Nonpromotion","LIN,IEBus,"]
["R5F21335MDFP","RenesasR5F21335MDFP","Renesas","R8C",20,24,4,2,null,0,0,null,27,null,2,0,null,null,4,null,-40,85,1.8,5.5,32,"32LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F21347EKFP","RenesasR5F21347EKFP","Renesas",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,0,null,null,null,48,48,null,null,null,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F2134CFKFP","RenesasR5F2134CFKFP","Renesas",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,0,null,null,null,48,48,null,null,null,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F2134CGJFP","RenesasR5F2134CGJFP","Renesas",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,0,null,null,null,48,48,null,null,null,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F2134AHKFP","RenesasR5F2134AHKFP","Renesas",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,0,null,null,null,48,48,null,null,null,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F21344RJFP","RenesasR5F21344RJFP","Renesas","R8C",20,16,0,1.5,null,0,0,null,43,null,1,0,null,null,5,null,-40,85,2.7,5.5,48,48,null,null,2,null,null,null,null,null,"Nonpromotion","LIN,IEBus,"]
["R5F21348WKFP","RenesasR5F21348WKFP","Renesas","R8C",20,64,4,6,null,0,0,null,43,null,1,0,null,null,6,null,-40,125,2.7,5.5,48,48,null,null,2,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F2134CXJFP","RenesasR5F2134CXJFP","Renesas","R8C",20,128,0,10,null,0,0,null,43,null,1,0,null,null,6,null,-40,85,2.7,5.5,48,48,null,null,2,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F2134AYKFP","RenesasR5F2134AYKFP","Renesas","R8C",20,96,4,8,null,0,0,null,43,null,1,0,null,null,6,null,-40,125,2.7,5.5,48,48,null,null,2,null,null,null,null,null,"Nonpromotion","LIN,IEBus,"]
["R5F21358CDFP","RenesasR5F21358CDFP","Renesas","R8C",20,64,4,6,null,0,0,null,47,null,2,0,null,null,6,null,-40,85,1.8,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F21354MNFP","RenesasR5F21354MNFP","Renesas","R8C",20,16,4,1.5,null,0,0,null,47,null,1,0,null,null,6,null,-20,85,1.8,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F2135AMDFP","RenesasR5F2135AMDFP","Renesas","R8C",20,96,4,8,null,0,0,null,47,null,1,0,null,null,6,null,-40,85,1.8,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F21364CNFP","RenesasR5F21364CNFP","Renesas","R8C",20,16,4,1.5,null,0,0,null,59,null,2,0,null,null,8,null,-20,85,1.8,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)",""]
["R5F21367CDFA","RenesasR5F21367CDFA","Renesas","R8C",20,48,4,4,null,0,0,null,59,null,2,0,null,null,8,null,-40,85,1.8,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)",""]
["R5F21368CNFA","RenesasR5F21368CNFA","Renesas","R8C",20,64,4,6,null,0,0,null,59,null,2,0,null,null,8,null,-20,85,1.8,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)",""]
["R5F2136CCNFB","RenesasR5F2136CCNFB","Renesas","R8C",20,128,4,10,null,0,0,null,59,null,2,0,null,null,8,null,-20,85,1.8,5.5,64,"64TFQFP",null,null,3,null,null,null,null,null,"Nonpromotion",""]
["R5F21368FKFP","RenesasR5F21368FKFP","Renesas","R8C",20,64,0,6,null,0,0,null,null,null,null,null,null,null,9,null,-40,125,null,null,64,64,null,null,null,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F21365MDFA","RenesasR5F21365MDFA","Renesas","R8C",20,24,4,2,null,0,0,null,59,null,2,0,null,null,8,null,-40,85,1.8,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)",""]
["R5F21368MDFP","RenesasR5F21368MDFP","Renesas","R8C",20,64,4,6,null,0,0,null,59,null,2,0,null,null,8,null,-40,85,1.8,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)",""]
["R5F2136AMDFA","RenesasR5F2136AMDFA","Renesas","R8C",20,96,4,8,null,0,0,null,59,null,2,0,null,null,8,null,-40,85,1.8,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)",""]
["R5F21368WJFP","RenesasR5F21368WJFP","Renesas","R8C",20,64,4,6,null,0,0,null,59,null,1,0,null,null,9,null,-40,85,2.7,5.5,64,64,null,null,3,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F2136AXKFP","RenesasR5F2136AXKFP","Renesas","R8C",20,96,0,8,null,0,0,null,59,null,1,0,null,null,9,null,-40,125,2.7,5.5,64,64,null,null,3,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F21368ZJFP","RenesasR5F21368ZJFP","Renesas","R8C",20,64,0,6,null,0,0,null,59,null,1,0,null,null,9,null,-40,85,2.7,5.5,64,64,null,null,3,null,null,null,null,null,"Nonpromotion","LIN,IEBus,"]
["R5F2138ACNFP","RenesasR5F2138ACNFP","Renesas","R8C",20,96,4,8,null,0,0,null,75,null,1,0,null,null,8,null,-20,85,1.8,5.5,80,"80LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F21388FKFP","RenesasR5F21388FKFP","Renesas","R8C",20,64,0,6,null,0,0,null,null,null,null,null,null,null,9,null,-40,125,null,null,80,80,null,null,null,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F2138AMDFP","RenesasR5F2138AMDFP","Renesas","R8C",20,96,4,8,null,0,0,null,75,null,1,0,null,null,8,null,-40,85,1.8,5.5,80,"80LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F2138AWKFP","RenesasR5F2138AWKFP","Renesas","R8C",20,96,4,8,null,0,0,null,75,null,0,0,null,null,9,null,-40,125,2.7,5.5,80,80,null,null,3,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F21388YJFP","RenesasR5F21388YJFP","Renesas","R8C",20,64,4,6,null,0,0,null,75,null,0,0,null,null,9,null,-40,85,2.7,5.5,80,80,null,null,3,null,null,null,null,null,"Nonpromotion","CAN,LIN,IEBus,"]
["R5F213G1CNSP","RenesasR5F213G1CNSP","Renesas","R8C",20,4,4,0.5,null,0,0,null,19,null,2,0,null,null,4,null,-20,85,1.8,5.5,24,"24LSSOP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F213G5CNSP","RenesasR5F213G5CNSP","Renesas","R8C",20,24,4,2,null,0,0,null,19,null,2,0,null,null,4,null,-20,85,1.8,5.5,24,"24LSSOP",null,null,2,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F213G4DNSP","RenesasR5F213G4DNSP","Renesas","R8C",20,16,0,1,null,0,0,null,19,null,1,0,null,null,4,null,-20,85,1.8,5.5,24,"24LSSOP",null,null,2,null,null,null,null,null,"Nonpromotion",""]
["R5F213J2MNNP","RenesasR5F213J2MNNP","Renesas","R8C",20,8,4,1,null,0,0,null,31,null,2,0,null,null,6,null,-20,85,1.8,5.5,36,"36HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F21546EJFP","RenesasR5F21546EJFP","Renesas","R8C",32,32,4,2.5,null,0,0,null,43,null,2,0,null,null,7,null,-40,85,2.7,5.5,48,48,null,null,3,null,null,null,null,null,"Nonpromotion","CAN,LIN,"]
["R5F21546GKFP","RenesasR5F21546GKFP","Renesas","R8C",32,32,4,2.5,null,0,0,null,43,null,2,0,null,null,7,null,-40,125,2.7,5.5,48,48,null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F21548HJFP","RenesasR5F21548HJFP","Renesas","R8C",32,64,0,6,null,0,0,null,43,null,2,0,null,null,7,null,-40,85,2.7,5.5,48,48,null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F21567EKFP","RenesasR5F21567EKFP","Renesas","R8C",32,48,4,4,null,0,0,null,59,null,2,0,null,null,10,null,-40,125,2.7,5.5,64,64,null,null,3,null,null,null,null,null,"Nonpromotion","CAN,LIN,"]
["R5F2156CEKFP","RenesasR5F2156CEKFP","Renesas","R8C",32,128,4,10,null,0,0,null,59,null,2,0,null,null,10,null,-40,125,2.7,5.5,64,64,null,null,3,null,null,null,null,null,"Nonpromotion","CAN,LIN,"]
["R5F2156AGJFP","RenesasR5F2156AGJFP","Renesas","R8C",32,96,4,8,null,0,0,null,59,null,2,0,null,null,10,null,-40,85,2.7,5.5,64,64,null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F21568HKFP","RenesasR5F21568HKFP","Renesas","R8C",32,64,0,6,null,0,0,null,59,null,2,0,null,null,10,null,-40,125,2.7,5.5,64,64,null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F2L357MDFP","RenesasR5F2L357MDFP","Renesas","R8C",20,48,4,6,null,0,0,null,41,null,2,1,null,null,7,null,-40,85,1.8,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,",null,null,null,"24 seg.(max)<br> 4 com.(max)"]
["R5F2L367CNFP","RenesasR5F2L367CNFP","Renesas","R8C",20,48,4,6,null,0,0,null,52,null,2,1,null,null,7,null,-20,85,1.8,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,",null,null,null,"32 seg.(max)<br> 8 com.(max)"]
["R5F2L368MNFA","RenesasR5F2L368MNFA","Renesas","R8C",20,64,4,8,null,0,0,null,52,null,2,1,null,null,7,null,-20,85,1.8,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,",null,null,null,"32 seg.(max)<br> 8 com.(max)"]
["R5F2L387MNFP","RenesasR5F2L387MNFP","Renesas","R8C",20,48,4,6,null,0,0,null,68,null,2,1,null,null,7,null,-20,85,1.8,5.5,80,"80LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,",null,null,null,"48 seg.(max)<br> 8 com.(max)"]
["R5F2L38CMDFA","RenesasR5F2L38CMDFA","Renesas","R8C",20,128,4,10,null,0,0,null,68,null,2,1,null,null,7,null,-40,85,1.8,5.5,80,"80LQFP",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,",null,null,null,"48 seg.(max)<br> 8 com.(max)"]
["R5F2L3A7MNFP","RenesasR5F2L3A7MNFP","Renesas","R8C",20,48,4,6,null,0,0,null,88,null,2,1,null,null,7,null,-20,85,1.8,5.5,100,"100LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,",null,null,null,"56 seg.(max)<br> 8 com.(max)"]
["R5F2LA34ADFP","RenesasR5F2LA34ADFP","Renesas","R8C",20,16,2,2,null,0,0,null,26,null,1,1,null,null,6,null,-40,85,1.8,5.5,32,"32LQFP",null,null,1,null,null,null,null,null,"Nonpromotion(*)","",null,null,null,"11 seg.(max)<br> 4 com.(max)"]
["R5F2LA54ANFP","RenesasR5F2LA54ANFP","Renesas","R8C",20,16,4,2,null,0,0,null,44,null,1,1,null,null,6,null,-20,85,1.8,5.5,52,"52LQFP",null,null,1,null,null,null,null,null,"Nonpromotion(*)","",null,null,null,"27 seg.(max)<br> 4 com.(max)"]
["R5F2LA67ADFA","RenesasR5F2LA67ADFA","Renesas","R8C",20,48,2,3.5,null,0,0,null,56,null,2,1,null,null,6,null,-40,85,1.8,5.5,64,"64LQFP",null,null,2,null,null,null,null,null,"Nonpromotion(*)","",null,null,null,"32 seg.(max)<br> 4 com.(max)"]
["R5F2LA6AADFP","RenesasR5F2LA6AADFP","Renesas","R8C",20,96,4,5.5,null,0,0,null,56,null,2,1,null,null,6,null,-40,85,1.8,5.5,64,"64LFQFP",null,null,2,null,null,null,null,null,"Nonpromotion(*)","",null,null,null,"32 seg.(max)<br> 4 com.(max)"]
["R5F2LA87ANFP","RenesasR5F2LA87ANFP","Renesas","R8C",20,48,2,3.5,null,0,0,null,72,null,2,1,null,null,7,null,-20,85,1.8,5.5,80,"80LFQFP",null,null,2,null,null,null,null,null,"Nonpromotion(*)","",null,null,null,"40 seg.(max)<br> 4 com.(max)"]
["R5F2M122ADSP","RenesasR5F2M122ADSP","Renesas","R8C",20,8,2,0.5,null,0,0,null,17,null,0,0,null,null,4,null,-40,85,1.8,5.5,20,"20LSSOP",null,null,1,null,null,null,null,null,"Nonpromotion",""]
["R7F701402EAFB","RenesasR7F701402EAFB","Renesas","G3M",120,4096,64,512,null,16,0,null,103,null,2,6,null,null,55,null,-40,150,2.7,5.5,144,"144LFQFP",null,null,4,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["R7F701428EABG","RenesasR7F701428EABG","Renesas","G3M",240,3840,64,512,null,20,0,null,159,null,2,6,null,null,55,null,-40,150,2.7,5.5,376,"376BGA",null,null,4,null,null,null,null,null,"Product Inquiry","CAN,EtherNet,LIN,"]
["R7F7010024AFP","RenesasR7F7010024AFP","Renesas","RH850G3K",80,512,32,64,null,16,0,null,81,null,1,4,null,null,40,"Timer for OS x 1ch",-40,125,null,5.5,100,"100LFQFP",null,"UART: RLIN3, LIN: RLIN3＋RLIN2",4,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["R7F7010123AFP","RenesasR7F7010123AFP","Renesas","RH850G3K",80,384,32,48,null,10,0,null,49,null,1,1,null,null,20,"Timer for OS x 1ch",-40,105,null,5.5,64,"64LFQFP",null,"UART: RLIN3, LIN: RLIN3＋RLIN2",2,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["R7F7010163AFP","RenesasR7F7010163AFP","Renesas","RH850G3K",80,256,32,32,null,11,0,null,65,null,1,3,null,null,20,"Timer for OS x 1ch",-40,105,null,5.5,80,"80LFQFP",null,"UART: RLIN3, LIN: RLIN3＋RLIN2",3,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["R7F7010204AFP","RenesasR7F7010204AFP","Renesas","RH850G3K",80,1024,32,128,null,11,0,null,65,null,1,3,null,null,20,"Timer for OS x 1ch",-40,125,null,5.5,80,"80LFQFP",null,"UART: RLIN3, LIN: RLIN3＋RLIN2",3,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["R7F7010293AFP","RenesasR7F7010293AFP","Renesas","RH850G3K",80,1024,32,128,null,24,0,null,120,null,1,4,null,null,40,"Timer for OS x 1ch",-40,105,null,5.5,144,"144LFQFP",null,"UART: RLIN3, LIN: RLIN3＋RLIN2",6,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["R7F7010454AFP","RenesasR7F7010454AFP","Renesas","RH850G3K",96,1024,32,128,null,16,0,null,81,null,1,4,null,null,40,"Timer for OS x 1ch",-40,125,null,5.5,100,"100LFQFP",null,"UART: RLIN3, LIN: RLIN3＋RLIN2",4,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["R7F7010503AFP","RenesasR7F7010503AFP","Renesas","RH850G3K",96,768,32,96,null,32,0,null,150,null,1,4,null,null,56,"Timer for OS x 1ch",-40,105,null,5.5,176,"176LFQFP",null,"UART: RLIN3, LIN: RLIN3＋RLIN2",6,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["R7F7010564AFP","RenesasR7F7010564AFP","Renesas","RH850G3K",96,1536,64,160,null,32,0,null,150,null,1,4,null,null,56,"Timer for OS x 1ch",-40,125,null,5.5,176,"176LFQFP",null,"UART: RLIN3, LIN: RLIN3＋RLIN2",6,null,null,null,null,null,"Product Inquiry","CAN,LIN,"]
["R5F10CLDJFB","RenesasR5F10CLDJFB","Renesas","RL78",32,48,8,3,null,0,0,null,54,null,1,0,null,null,24,"Interval Timer x 1 ch, Wakeup Timer x 1ch",-40,85,2.7,5.5,64,"64LFQFP",null,null,2,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10DLDLFB","RenesasR5F10DLDLFB","Renesas","RL78",24,48,8,3,null,0,0,null,54,null,1,0,null,null,24,"Interval Timer x 1 ch, Wakeup Timer x 1ch",-40,105,2.7,5.5,64,"64LFQFP",null,null,2,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10DMGJFB","RenesasR5F10DMGJFB","Renesas","RL78",32,128,8,8,null,0,0,null,68,null,1,0,null,null,24,"Interval Timer x 1 ch, Wakeup Timer x 1ch",-40,85,2.7,5.5,80,"80LFQFP",null,null,2,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10DPGLFB","RenesasR5F10DPGLFB","Renesas","RL78",24,128,8,8,null,0,0,null,84,null,1,0,null,null,24,"Interval Timer x 1 ch, Wakeup Timer x 1ch",-40,105,2.7,5.5,100,"100LFQFP",null,null,2,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10TPJJFB","RenesasR5F10TPJJFB","Renesas","RL78",32,256,8,16,null,0,0,null,84,null,1,0,null,null,24,"Interval Timer x 1 ch, Wakeup Timer x 1ch",-40,85,2.7,5.5,100,"100LFQFP",null,null,2,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F109ADKSP","RenesasR5F109ADKSP","Renesas","RL78",32,48,4,3,null,0,0,null,26,null,3,0,null,null,8,"Interval Timer x 1 ch, Wakeup Timer x 1ch",-40,125,2.7,5.5,30,"30LSSOP",null,null,5,null,null,null,null,null,"Mass Production","LIN,"]
["R5F109BDJNA","RenesasR5F109BDJNA","Renesas","RL78",32,48,4,3,null,0,0,null,28,null,3,0,null,null,8,"Interval Timer x 1 ch, Wakeup Timer x 1ch",-40,85,1.8,5.5,32,"32HWQFN",null,null,5,null,null,null,null,null,"Mass Production","LIN,"]
["R5F109GEKFB","RenesasR5F109GEKFB","Renesas","RL78",32,64,4,4,null,0,0,null,44,null,5,0,null,null,8,"Interval Timer x 1 ch, Wakeup Timer x 1ch",-40,125,2.7,5.5,48,"48LFQFP",null,null,5,null,null,null,null,null,"Mass Production","LIN,"]
["R5F109LEJFB","RenesasR5F109LEJFB","Renesas","RL78",32,64,4,4,null,0,0,null,58,null,6,0,null,null,8,"Interval Timer x 1 ch, Wakeup Timer x 1ch",-40,85,1.8,5.5,64,"64LFQFP",null,null,5,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10A6EYSP","RenesasR5F10A6EYSP","Renesas","RL78",24,64,4,4,null,0,0,null,13,null,2,2,null,null,11,null,0,150,2.7,5.5,20,"20LSSOP",null,null,2,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10AACLSP","RenesasR5F10AACLSP","Renesas","RL78",32,32,4,2,null,0,0,null,23,null,2,2,null,null,11,null,-40,105,2.7,5.5,30,"30LSSOP",null,null,2,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10ABDKNA","RenesasR5F10ABDKNA","Renesas","RL78",24,48,4,3,null,0,0,null,25,null,2,2,null,null,11,null,-40,125,2.7,5.5,32,"32HVQFN",null,null,2,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10AGCKNA","RenesasR5F10AGCKNA","Renesas","RL78",24,32,4,2,null,0,0,null,38,null,2,2,null,null,11,null,-40,125,2.7,5.5,48,"48HVQFN",null,null,2,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10AGFYFB","RenesasR5F10AGFYFB","Renesas","RL78",24,96,4,6,null,0,0,null,38,null,5,4,null,null,15,null,0,150,2.7,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10AGFYNA","RenesasR5F10AGFYNA","Renesas","RL78",24,96,4,6,null,0,0,null,38,null,5,4,null,null,15,null,0,150,2.7,5.5,48,"48HVQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10ALGYFB","RenesasR5F10ALGYFB","Renesas","RL78",24,128,4,8,null,0,0,null,52,null,5,4,null,null,15,null,0,150,2.7,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10AMGYFB","RenesasR5F10AMGYFB","Renesas","RL78",24,128,4,8,null,0,0,null,68,null,5,4,null,null,15,null,0,150,2.7,5.5,80,"80LFQFP",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10BAGKSP","RenesasR5F10BAGKSP","Renesas","RL78",24,128,4,8,null,0,0,null,23,null,3,2,null,null,15,null,-40,125,2.7,5.5,30,"30LSSOP",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10BBEKNA","RenesasR5F10BBEKNA","Renesas","RL78",24,64,4,4,null,0,0,null,25,null,4,2,null,null,15,null,-40,125,2.7,5.5,32,"32HVQFN",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10BGCKFB","RenesasR5F10BGCKFB","Renesas","RL78",24,32,4,2,null,0,0,null,38,null,5,3,null,null,15,null,-40,125,2.7,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10BGEKNA","RenesasR5F10BGEKNA","Renesas","RL78",24,64,4,4,null,0,0,null,38,null,5,3,null,null,15,null,-40,125,2.7,5.5,48,"48HVQFN",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10BLDLFB","RenesasR5F10BLDLFB","Renesas","RL78",32,48,4,3,null,0,0,null,52,null,5,4,null,null,15,null,-40,105,2.7,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10BLDYFB","RenesasR5F10BLDYFB","Renesas","RL78",24,48,4,3,null,0,0,null,52,null,5,4,null,null,15,null,0,150,2.7,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10PADYSP","RenesasR5F10PADYSP","Renesas","RL78",24,48,4,4,null,0,0,null,23,null,3,2,null,null,15,null,0,150,2.7,5.5,30,"30LSSOP",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10PBEYNA","RenesasR5F10PBEYNA","Renesas","RL78",24,64,4,6,null,0,0,null,25,null,4,2,null,null,15,null,0,150,2.7,5.5,32,"32HVQFN",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10PGFKFB","RenesasR5F10PGFKFB","Renesas","RL78",24,96,4,8,null,0,0,null,38,null,5,3,null,null,15,null,-40,125,2.7,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10PGGLNA","RenesasR5F10PGGLNA","Renesas","RL78",32,128,8,10,null,0,0,null,38,null,5,3,null,null,19,null,-40,105,2.7,5.5,48,"48HVQFN",null,null,4,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10PGJKFB","RenesasR5F10PGJKFB","Renesas","RL78",24,256,8,20,null,0,0,null,38,null,5,3,null,null,19,null,-40,125,2.7,5.5,48,"48LFQFP",null,null,4,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10PLJKFB","RenesasR5F10PLJKFB","Renesas","RL78",24,256,8,20,null,0,0,null,52,null,5,4,null,null,19,null,-40,125,2.7,5.5,64,"64LFQFP",null,null,4,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10PMJYFB","RenesasR5F10PMJYFB","Renesas","RL78",24,256,8,20,null,0,0,null,68,null,5,4,null,null,19,null,0,150,2.7,5.5,80,"80LFQFP",null,null,4,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F10PPEKFB","RenesasR5F10PPEKFB","Renesas","RL78",24,64,4,6,null,0,0,null,86,null,5,4,null,null,19,null,-40,125,2.7,5.5,100,"100LFQFP",null,null,4,null,null,null,null,null,"Mass Production","CAN,LIN,"]
["R5F113GLLFB","RenesasR5F113GLLFB","Renesas","RL78",32,512,16,32,null,0,0,null,38,null,5,3,null,null,19,null,-40,105,2.7,5.5,48,"48LFQFP",null,null,2,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,"]
["R5F113MLLFB","RenesasR5F113MLLFB","Renesas","RL78",32,512,16,32,null,0,0,null,68,null,5,4,null,null,19,null,-40,105,2.7,5.5,80,"80LFQFP",null,null,2,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,"]
["R5F113THKFB","RenesasR5F113THKFB","Renesas","RL78",24,192,8,16,null,0,0,null,130,null,5,4,null,null,27,null,-40,125,2.7,5.5,144,"144LFQFP",null,null,3,null,null,null,null,null,"Mass Production","CAN,LIN,IEBus,"]
["R5F10Y14DSP","RenesasR5F10Y14DSP","Renesas","RL78",20,1,0,0.125,null,0,0,null,8,null,1,0,null,null,4,0,-40,85,2,5.5,10,"10LSSOP",null,"1ch simplified IIC",1,null,null,null,null,null,"Mass Production",""]
["R5F1054AASP","RenesasR5F1054AASP","Renesas","RL78",24,16,2,1.5,null,0,0,null,13,null,2,0,null,null,7,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,16,"16SSOP",null,null,2,null,null,null,null,null,"Mass Production","LIN,"]
["R5F10266DSP","RenesasR5F10266DSP","Renesas","RL78",24,2,2,0.25,null,0,0,null,18,null,3,0,null,null,8,"12bit Interval Timer x 1 ch",-40,85,1.8,5.5,20,"20LSSOP",null,null,1,null,null,null,null,null,"Nonpromotion(*)",""]
["R5F10279DNA","RenesasR5F10279DNA","Renesas","RL78",24,12,2,1,null,0,0,null,22,null,3,0,null,null,8,"12bit Interval Timer x 1 ch",-40,85,1.8,5.5,24,"24HWQFN",null,null,1,null,null,null,null,null,"Nonpromotion",""]
["R5F10279GNA","RenesasR5F10279GNA","Renesas","RL78",24,12,2,1,null,0,0,null,22,null,3,0,null,null,8,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,24,"24HWQFN",null,null,1,null,null,null,null,null,"Mass Production(*)",""]
["R5F10368DSP","RenesasR5F10368DSP","Renesas","RL78",24,8,0,0.75,null,0,0,null,18,null,1,0,null,null,8,"12bit Interval Timer x 1 ch",-40,85,1.8,5.5,20,"20LSSOP",null,null,1,null,null,null,null,null,"Nonpromotion(*)",""]
["R5F10379ANA","RenesasR5F10379ANA","Renesas","RL78",24,12,0,1,null,0,0,null,22,null,1,0,null,null,8,"12bit Interval Timer x 1 ch",-40,85,1.8,5.5,24,"24HWQFN",null,null,1,null,null,null,null,null,"Mass Production(*)",""]
["R5F1006ADSP","RenesasR5F1006ADSP","Renesas","RL78",32,16,4,2,null,0,0,null,16,null,2,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,20,"20LSSOP",null,null,2,null,null,null,null,null,"Nonpromotion(*)",""]
["R5F1006EDSP","RenesasR5F1006EDSP","Renesas","RL78",32,64,4,4,null,0,0,null,16,null,2,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,20,"20LSSOP",null,null,2,null,null,null,null,null,"Nonpromotion(*)",""]
["R5F1007EGNA","RenesasR5F1007EGNA","Renesas","RL78",32,64,4,4,null,0,0,null,20,null,3,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,24,"24HWQFN",null,null,2,null,null,null,null,null,"Mass Production",""]
["R5F100AAASP","RenesasR5F100AAASP","Renesas","RL78",32,16,4,2,null,0,0,null,26,null,4,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,30,"30LSSOP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100BCANA","RenesasR5F100BCANA","Renesas","RL78",32,32,4,2,null,0,0,null,28,null,4,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,32,"32HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F100BCGNA","RenesasR5F100BCGNA","Renesas","RL78",32,32,4,2,null,0,0,null,28,null,4,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,32,"32HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F100CFALA","RenesasR5F100CFALA","Renesas","RL78",32,96,8,8,null,0,0,null,32,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,36,"36WFLGA",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F100EEANA","RenesasR5F100EEANA","Renesas","RL78",32,64,4,4,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F100EHANA","RenesasR5F100EHANA","Renesas","RL78",32,192,8,16,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F100FDAFP","RenesasR5F100FDAFP","Renesas","RL78",32,48,4,3,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100FHDFP","RenesasR5F100FHDFP","Renesas","RL78",32,192,8,16,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F100GAAFB","RenesasR5F100GAAFB","Renesas","RL78",32,16,4,2,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100GEDNA","RenesasR5F100GEDNA","Renesas","RL78",32,64,4,4,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F100GEGFB","RenesasR5F100GEGFB","Renesas","RL78",32,64,4,4,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100GJANA","RenesasR5F100GJANA","Renesas","RL78",32,256,8,20,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F100JCAFA","RenesasR5F100JCAFA","Renesas","RL78",32,32,4,2,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100JFAFA","RenesasR5F100JFAFA","Renesas","RL78",32,96,8,8,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100JJAFA","RenesasR5F100JJAFA","Renesas","RL78",32,256,8,20,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100LCGFA","RenesasR5F100LCGFA","Renesas","RL78",32,32,4,2,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100LDGFB","RenesasR5F100LDGFB","Renesas","RL78",32,48,4,3,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100LGDFB","RenesasR5F100LGDFB","Renesas","RL78",32,128,8,12,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F100LGGBG","RenesasR5F100LGGBG","Renesas","RL78",32,128,8,12,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,64,"64VFBGA",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F100LJGFA","RenesasR5F100LJGFA","Renesas","RL78",32,256,8,20,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100MGDFA","RenesasR5F100MGDFA","Renesas","RL78",32,128,8,12,null,0,0,null,74,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,80,"80LQFP",null,null,4,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F100MHGFB","RenesasR5F100MHGFB","Renesas","RL78",32,192,8,16,null,0,0,null,74,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,80,"80LFQFP",null,null,4,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100MKDFA","RenesasR5F100MKDFA","Renesas","RL78",32,384,8,24,null,0,0,null,74,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,80,"80LQFP",null,null,4,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100PGAFB","RenesasR5F100PGAFB","Renesas","RL78",32,128,8,12,null,0,0,null,92,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,100,"100LFQFP",null,null,4,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100PHGFA","RenesasR5F100PHGFA","Renesas","RL78",32,192,8,16,null,0,0,null,92,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,100,"100LQFP",null,null,4,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100PLAFB","RenesasR5F100PLAFB","Renesas","RL78",32,512,8,32,null,0,0,null,92,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,100,"100LFQFP",null,null,4,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F100SLAFB","RenesasR5F100SLAFB","Renesas","RL78",32,512,8,32,null,0,0,null,120,null,10,0,null,null,24,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,128,"128LFQFP",null,null,4,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F1018EALA","RenesasR5F1018EALA","Renesas","RL78",32,64,0,4,null,0,0,null,21,null,3,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,25,"25WFLGA",null,null,2,null,null,null,null,null,"Mass Production",""]
["R5F101BAANA","RenesasR5F101BAANA","Renesas","RL78",32,16,0,2,null,0,0,null,28,null,4,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,32,"32HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F101BFDNA","RenesasR5F101BFDNA","Renesas","RL78",32,96,0,8,null,0,0,null,28,null,4,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,32,"32HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F101EAANA","RenesasR5F101EAANA","Renesas","RL78",32,16,0,2,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F101EHDNA","RenesasR5F101EHDNA","Renesas","RL78",32,192,0,16,null,0,0,null,36,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,40,"40HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F101FFAFP","RenesasR5F101FFAFP","Renesas","RL78",32,96,0,8,null,0,0,null,40,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,44,"44LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F101GAANA","RenesasR5F101GAANA","Renesas","RL78",32,16,0,2,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F101GDDFB","RenesasR5F101GDDFB","Renesas","RL78",32,48,0,3,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F101GJDNA","RenesasR5F101GJDNA","Renesas","RL78",32,256,0,20,null,0,0,null,44,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F101JEAFA","RenesasR5F101JEAFA","Renesas","RL78",32,64,0,4,null,0,0,null,48,null,6,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,52,"52LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F101LCABG","RenesasR5F101LCABG","Renesas","RL78",32,32,0,2,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64VFBGA",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F101LDABG","RenesasR5F101LDABG","Renesas","RL78",32,48,0,3,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64VFBGA",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F101LFDFA","RenesasR5F101LFDFA","Renesas","RL78",32,96,0,8,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LQFP",null,null,3,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F101LHAFB","RenesasR5F101LHAFB","Renesas","RL78",32,192,0,16,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F101LLAFB","RenesasR5F101LLAFB","Renesas","RL78",32,512,0,32,null,0,0,null,58,null,7,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,64,"64LFQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F101MGDFA","RenesasR5F101MGDFA","Renesas","RL78",32,128,0,12,null,0,0,null,74,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,80,"80LQFP",null,null,4,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F101PFDFB","RenesasR5F101PFDFB","Renesas","RL78",32,96,0,8,null,0,0,null,92,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,100,"100LFQFP",null,null,4,null,null,null,null,null,"Nonpromotion(*)","LIN,"]
["R5F101PKAFA","RenesasR5F101PKAFA","Renesas","RL78",32,384,0,24,null,0,0,null,92,null,10,0,null,null,20,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,100,"100LQFP",null,null,4,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F101SHDFB","RenesasR5F101SHDFB","Renesas","RL78",32,192,0,16,null,0,0,null,120,null,10,0,null,null,24,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,128,"128LFQFP",null,null,4,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F140GLAFB","RenesasR5F140GLAFB","Renesas","RL78",32,512,8,32,null,0,0,null,44,null,1,0,null,null,8,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,48,"48LFQFP",null,null,3,null,null,null,null,null,"Under Development","LIN,"]
["R5F140PLGFB","RenesasR5F140PLGFB","Renesas","RL78",32,512,8,32,null,0,0,null,92,null,2,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,2.4,5.5,100,"100LFQFP",null,null,4,null,null,null,null,null,"Under Development","LIN,"]
["R5F104ADGSP","RenesasR5F104ADGSP","Renesas","RL78",32,48,4,5.5,null,0,0,null,26,null,4,0,null,null,12,"12bit Interval Timer x 1 ch",-40,105,1.6,5.5,30,"30LSSOP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104BADNA","RenesasR5F104BADNA","Renesas","RL78",32,16,4,2.5,null,0,0,null,28,null,4,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,32,"32HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104BDAFP","RenesasR5F104BDAFP","Renesas","RL78",32,48,4,5.5,null,0,0,null,28,null,4,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,32,"32LQFP",null,null,3,null,null,null,null,null,"Mass Production(*)","LIN,"]
["R5F104BGDNA","RenesasR5F104BGDNA","Renesas","RL78",32,128,8,16,null,0,0,null,28,null,4,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,32,"32HWQFN",null,null,3,null,null,null,null,null,"Nonpromotion","LIN,"]
["R5F104CGALA","RenesasR5F104CGALA","Renesas","RL78",32,128,8,16,null,0,0,null,32,null,5,0,null,null,12,"12bit Interval Timer x 1 ch",-40,85,1.6,5.5,36,"36WFLGA",null,null,3,null,null,null,null,null,"Mass Production","LIN,"]
["R5F70854AN80FPV","RenesasR5F70854AN80FPV","Renesas","SH2",80,256,0,16,null,0,0,null,108,null,1,1,null,null,11,null,-20,85,3,5.5,144,"144LFQFP",null,"SCI (CSI:3ch/UART:3ch), SCIF (CSI:1ch/UART:1ch), SSU (SPI), I2C",4,null,null,null,null,null,"Nonpromotion",""]
["STM32L071RB","STSTM32L071RB","ST","ARM CM0+",32,128,6,20,0,16,0,2,51,"No",2,2,1,"No",7,"2xWDG,RTC,SysTick",-40,105,1.65,3.6,64,"LQFP 64 10x10x1.4,TFBGA 64 5x5x1.2",1.827,4,1,0.8,87,null,null,null,"Active",null,"Ultralowpower ARM CM0+ MCU with 128Kbytes Flash, 32 MHz CPU",0]
["STM32L072CZ","STSTM32L072CZ","ST","ARM CM0+",32,192,6,20,0,13,2,2,40,"No",3,2,1,"Yes",7,"2xWDG,RTC,SysTick",-40,85,1.65,3.6,49,"EWLCSP 49L DIE 447 P 0.4 MM,LQFP 48 7x7x1.4,UFQFPN 48 7x7x0.55,WLCSP 49L DIE 447 P 0.4 MM",1.8694,4,1,0.8,87,null,null,true,"Active",null,"Ultralowpower ARM CM0+ MCU with 192Kbytes Flash, 32 MHz CPU, USB",0,null,null,"USB Device"]
["STM32L072RB","STSTM32L072RB","ST","ARM CM0+",32,128,6,20,0,16,2,2,51,"No",3,2,1,"Yes",7,"2xWDG,RTC,SysTick",-40,125,1.65,3.6,64,"LQFP 64 10x10x1.4,TFBGA 64 5x5x1.2,UFBGA 5X5X0.6 64L P 0.5 MM",1.8,4,1,0.8,87,null,null,true,"Active",null,"Ultralowpower ARM CM0+ MCU with 128Kbytes Flash, 32 MHz CPU, USB",0,null,null,"USB Device"]
["STM32L073VB","STSTM32L073VB","ST","ARM CM0+",32,128,6,20,0,16,2,2,84,"Yes",3,2,1,"Yes",7,"2xWDG,RTC,SysTick",-40,105,1.65,3.6,100,"LQFP 100 14x14x1.4",2.3717999999999999,4,1,0.8,87,null,null,true,"Active",null,"Ultralowpower ARM CM0+ MCU with 128Kbytes Flash, 32 MHz CPU, USB, LCD",0,null,"LCD 4x52/8x48","USB Device"]
["STM32L083CB","STSTM32L083CB","ST","ARM CM0+",32,128,6,20,0,10,2,2,40,"Yes",3,2,1,"Yes",7,"2xWDG,RTC,SysTick",-40,85,1.65,3.6,48,"LQFP 48 7x7x1.4",1.9388000000000001,4,1,0.8,87,null,"AES",true,"Active",null,"Ultralowpower ARM CM0+ MCU with 128Kbytes Flash, 32 MHz CPU, USB, LCD, AES",0,null,"LCD 4x18","USB Device"]
["STM32L100RC","STSTM32L100RC","ST","ARM CM3",32,256,4,16,0,20,2,2,51,"Yes",2,3,null,"Yes",6,"24bit down counter,2xWDG,RTC",-40,85,1.8,3.6,64,"LQFP 64 10x10x1.4",null,3,null,1.1000000000000001,185,null,null,null,"Active",null,"Ultralowpower 32bit Value Line ARM CM3 MCU with 256 Kbytes Flash, 32 MHz CPU, LCD, USB",0,null,"LCD 4x32/8x28","USB Device"]
["STM32L151UC","STSTM32L151UC","ST","ARM CM3",32,256,8,32,0,21,2,2,51,"No",2,3,2,"Yes",8,"2xWDG,RTC,SysTick",-40,"105,85",1.65,3.6,63,"WLCSP 63L (7X9) DIE 427 P 0.4 MM",null,3,null,1.1000000000000001,185,null,null,null,"Active",null,"Ultralowpower ARM CM3 MCU with 256 Kbytes Flash, 32 MHz CPU, USB, 2xOpamp",0,null,null,"USB Device"]
["STM32L151VE","STSTM32L151VE","ST","ARM CM3",32,512,16,80,0,25,2,2,83,"No",2,3,2,"Yes",8,"2xWDG,RTC,SysTick",-40,"105,85",1.65,3.6,100,"LQFP 100 14x14x1.4,WLCSP 104L DIE 437 P 0.4MM",null,5,null,1.1000000000000001,195,null,null,null,"Active",null,"Ultralowpower ARM CM3 MCU with 512 Kbytes Flash, 32 MHz CPU, MCD, USB, 2xOpamp","2",null,null,"USB Device"]
["STM32L152QE","STSTM32L152QE","ST","ARM CM3",32,512,16,80,0,40,2,2,109,"Yes",2,3,2,"Yes",8,"2xWDG,RTC,SysTick",-40,85,1.65,3.6,169,"UFBGA 7X7X0.6 132L P 0.5 R 12X12",null,5,null,1.1000000000000001,195,null,null,null,"Active",null,"Ultralowpower ARM CM3 MCU with 512 Kbytes Flash, 32 MHz CPU, USB, 2xOpamp","2",null,"LCD 4x44/8x40","USB Device"]
["STM32L152RD","STSTM32L152RD","ST","ARM CM3",32,384,12,48,0,21,2,2,51,"Yes",2,3,2,"Yes",8,"2xWDG,RTC,SysTick",-40,85,1.65,3.6,64,"LQFP 64 10x10x1.4,WLCSP 64 BALLS DIE 436 P 0.4 MM",null,5,null,1.1000000000000001,230,null,null,null,"Active",null,"Ultralowpower ARM CM3 MCU with 384 Kbytes Flash, 32 MHz CPU, LCD, USB, 3xOpamp","3",null,"LCD 4x32/8x28","USB Device"]
["STM32L152VD","STSTM32L152VD","ST","ARM CM3",32,384,12,48,0,25,2,2,83,"Yes",2,3,2,"Yes",8,"2xWDG,RTC,SysTick",-40,85,1.65,3.6,100,"LQFP 100 14x14x1.4",null,5,null,1.1000000000000001,230,null,null,null,"Active",null,"Ultralowpower CortexM3 MCU with 384 Kbytes Flash, 32 MHz CPU, LCD, USB, 3xOpamp","3",null,"LCD 4x44/8x40","USB Device"]
["STM32L162VC-A","STSTM32L162VCA","ST","ARM CM3",32,256,8,32,0,25,2,2,83,"Yes",2,3,2,"Yes",8,"2xWDG,RTC,SysTick",-40,85,1.65,3.6,100,"LQFP 100 14x14x1.4",null,3,null,1.1000000000000001,185,null,"AES",null,"NRND",null,"Ultralowpower ARM CM3 MCU with 256 Kbytes Flash, 32 MHz CPU, LCD, USB, 2xOpamp, AES","2",null,"LCD 4x44/8x40","USB Device"]
["STM32L412K8","STSTM32L412K8","ST","ARM CM4F",80,64,null,40,12,10,0,1,26,"No",2,1,null,"Yes",5,"2xWDG,RTC,SysTick",-40,85,1.71,3.6,32,"LQFP 32 7x7x1.4,UFQFPN 32 5x5x0.55",null,3,null,0.77500000000000002,70,null,null,"true","Active",null,"Ultralowpower with FPU ARM CM4 MCU 80 MHz with 64Kbyte of Flash memory, USB","1",null,null,"USB Device"]
["STM32L431KC","STSTM32L431KC","ST","ARM CM4F",80,256,null,64,0,10,2,2,26,"No",2,2,null,"No",7,"2xWDG,RTC,SysTick",-40,85,1.71,3.6,32,"UFQFPN 32 5x5x0.55",null,2,1,0.77500000000000002,80,null,null,"true","Active",null,"Ultralowpower with FPU ARM CM4 MCU 80 MHz with 256 Kbytes Flash","1"]
["STM32L452CC","STSTM32L452CC","ST","ARM CM4F",80,256,null,160,12,10,1,2,38,"No",4,3,null,"Yes",7,"2xWDG,RTC,SysTick",-40,85,1.71,3.6,48,"UFQFPN 48 7x7x0.55",null,5,1,0.51,100,null,null,null,"Active",null,"Ultralowpower with FPU ARM CM4 MCU 80 MHz with 256 Kbytes Flash, USB Device, DFSDM","1",null,null,"USB Device"]
["STM32L471QE","STSTM32L471QE","ST","ARM CM4F",80,512,null,128,0,19,2,2,109,"No",3,3,null,"No",11,"2xWDG,RTC,SysTick",-40,"105,85",1.71,3.6,132,"UFBGA 7X7X0.6 132L P 0.5 R 12X12",null,5,1,0.51,100,null,null,"true","Active",null,"Ultralowpower with FPU ARM CM4 MCU 80 MHz with 512 Kbytes Flash, DFSDM","2"]
["STM32L475VG","STSTM32L475VG","ST","ARM CM4F",80,1024,null,128,0,16,2,2,82,"No",3,3,null,"Yes",11,"2xWDG,RTC,SysTick",-40,85,1.71,3.6,100,"LQFP 100 14x14x1.4",null,5,1,0.51,100,null,null,"true","Active",null,"Ultralowpower with FPU ARM CM4 MCU 80 MHz with 1 Mbyte Flash, USB OTG, DFSDM","2",null,null,"USB OTG FS"]
["STM32L476RG","STSTM32L476RG","ST","ARM CM4F",80,1024,null,128,0,16,2,2,51,"Yes",3,3,null,"Yes",11,"2xWDG,RTC,SysTick",-40,"125,85",1.71,3.6,64,"LQFP 64 10x10x1.4",null,5,1,0.51,100,null,null,"true","Active",null,"Ultralowpower with FPU ARM CM4 MCU 80 MHz with 1 Mbyte Flash, LCD, USB OTG, DFSDM","2",null,"LCD 4x32/8x28","USB OTG FS"]
["STM32L496VE","STSTM32L496VE","ST","ARM CM4F",80,512,null,320,0,16,2,2,83,"Yes",4,3,null,"Yes",11,"2xWDG,RTC,SysTick",-40,85,1.71,3.6,100,"LQFP 100 14x14x1.4",null,5,1,0.51,90,null,null,null,"Active",null,"Ultralowpower with FPU ARM CM4 MCU 80 MHz with 512 Kbytes Flash, USB OTG, LCD, DFSDM","2",null,"LCD 4x44/8x40","USB OTG FS"]
["STM32L4A6RG","STSTM32L4A6RG","ST","ARM CM4F",80,1024,null,320,0,16,2,2,52,"Yes",3,3,null,"Yes",11,"2xWDG,RTC,SysTick",-40,85,1.71,3.6,64,"LQFP 64 10x10x1.4",null,5,1,0.51,90,null,"AES,SHA",null,"Active",null,"Ultralowpower with FPU ARM CM4 MCU 80 MHz with 1 Mbyte Flash, USB OTG, LCD, AES256, DFSDM","2",null,"LCD 4x44/8x40","USB OTG FS"]
["STM32L4R5ZG","STSTM32L4R5ZG","ST","ARM CM4F",120,1024,null,640,0,16,2,2,115,"No",4,3,null,"Yes",11,"2xWDG,RTC,SysTick",-40,85,1.71,3.6,144,"LQFP 144 20x20x1.4,WLCSP 144L DIE 470 PITCH 0.4",null,6,null,0.64500000000000002,112,null,null,"true","Active",null,"Ultralowpower with FPU ARM CM4 MCU 120 MHz with 1024 kbytes Flash, USB OTG, DFSDM, CHROMART","2",null,null,"USB OTG FS"]
["STM32L4S5VI","STSTM32L4S5VI","ST","ARM CM4F",120,2048,null,640,0,16,2,2,83,"No",4,3,null,"Yes",11,"2xWDG,RTC,SysTick",-40,85,1.71,3.6,100,"LQFP 100 14x14x1.4",null,6,null,0.64500000000000002,112,null,null,"true","Active",null,"Ultralowpower with FPU ARM CM4 MCU 120 MHz with 2048 kbytes Flash, USB OTG, DFSDM, CHROMART, AES256, HASH","2",null,null,"USB OTG FS"]
["STM32L562QE","STSTM32L562QE","ST","ARM CM33",110,512,null,256,12,16,2,2,106109,"No",4,3,null,"Yes",12,"2xWDG,RTC,SysTick","40,85","40,85",1.71,3.6,132,"UFBGA 7X7X0.6 132L P 0.5 R 12X12",null,6,null,0.64500000000000002,96,null,"HMAC,MD5,SHA","true","Active",null,"Ultralowpower with FPU ARM CM33 with Trust Zone, MCU 110 MHz with 512 kbytes of Flash memory","2",null,null,"USB Device,USB FS,USB TypeC"]
["STM8AF528A","STSTM8AF528A","ST","STM8",24,64,2,6,10,16,0,0,70,"No",1,1,null,"No",4,"AWU,Beeper,IWDG,WWDG",-40,"125,85",3,5.5,80,"LQFP 80 14x14x1.4",null,1,1,5,500,null,null,null,"Active",null,"Automotive 8bit MCU with 64 Kbytes Flash, LIN, CAN, 24 MHz CPU, integrated EEPROM",0]
["STM8AF6268","STSTM8AF6268","ST","STM8",16,32,1,2,10,10,0,0,38,"No",1,1,null,"No",4,"AWU,Beeper,IWDG,WWDG",-40,"125,150,85",3,5.5,48,"LQFP 48 7x7x1.4",null,null,1,5,430,null,null,null,"Active",null,"Automotive 8bit MCU with 32 Kbytes Flash, LIN, 16 MHz CPU, integrated EEPROM",0]
["STM8AF62AA","STSTM8AF62AA","ST","STM8",24,128,2,6,10,16,0,0,70,"No",1,1,null,"No",4,"AWU,Beeper,IWDG,WWDG",-40,"125,85",3,5.5,80,"LQFP 80 14x14x1.4",null,null,1,5,500,null,null,null,"Active",null,"Automotive 8bit MCU with 128 Kbytes Flash, LIN, 24 MHz CPU, integrated EEPROM",0]
["STM8AL31E89","STSTM8AL31E89","ST","STM8",16,64,1.953125,4,12,28,2,2,54,"No",1,1,null,"No",5,"AWU,Beeper,IWDG,RTC,WWDG",-40,125,1.8,3.6,64,"LQFP 64 10x10x1.4",null,3,null,0.4,200,null,"AES",null,"Active",null,"Automotive 8bit ultralowpower MCU with 64 Kbytes Flash, LIN, RTC, data EEPROM, timers, USARTs, I2C, SPIs, ADC, DAC, COMPs, AES",0]
["STM8AL3LE88","STSTM8AL3LE88","ST","STM8",16,64,1.953125,4,12,25,2,2,41,"Yes",1,1,null,"No",5,"AWU,Beeper,IWDG,RTC,WWDG",-40,"125,85",1.8,3.6,48,"LQFP 48 7x7x1.4",null,3,null,0.4,200,null,"AES",null,"Active",null,"Automotive 8bit ultralowpower MCU with 64 Kbytes Flash, LIN, RTC, LCD, data EEPROM, timers, USARTs, I2C, SPIs, ADC, DAC, COMPs, AES",0,null,"LCD 4x32/8x28"]
["STM8L101F2","STSTM8L101F2","ST","STM8",16,4,null,1.5,0,0,0,2,18,"No",1,1,null,"No",3,"AWU,Beeper,IWDG",-40,"125,85",1.65,3.6,20,"TSSOP 20,UFQFPN 20 3x3x0.6",0.95,1,null,0.3,150,null,null,null,"Active",null,"Ultralowpower 8bit MCU with 4 Kbytes Flash, 16 MHz CPU, integrated EEPROM",0]
["STM8L151G3","STSTM8L151G3","ST","STM8",16,8,0.25,1,12,18,0,2,26,"No",1,1,null,"No",3,"Beeper,IWDG,RTC,WWDG",-40,"125,85",1.65,3.6,28,"UFQFPN 28 4x4x0.55",0.47199999999999998,1,null,0.35,180,null,null,null,"Active",null,"Ultralowpower 8bit MCU with 8 Kbytes Flash, 16 MHz CPU, integrated EEPROM",0]
["STM8S001J3","STSTM8S001J3","ST","STM8",16,8,0.125,1,12,4,0,0,5,"No",1,1,null,"No",3,"IWDG,WWDG",-40,125,2.95,5.5,8,"SO8",0.66,0,1,5,230,null,null,null,"Active",null,"Mainstream Value line 8bit MCU with 8 Kbytes Flash, 16 MHz CPU",0]
["STM8S105C4","STSTM8S105C4","ST","STM8",16,16,1,2,10,10,0,0,38,"No",1,1,null,"No",4,"Beeper,IWDG,WWDG",-40,"125,85",2.95,5.5,48,"LQFP 48 7x7x1.4",1.88,null,1,5,430,null,null,null,"Active",null,"Mainstream Access line 8bit MCU with 16 Kbytes Flash, 16 MHz CPU, integrated EEPROM",0]
["STM8S207R6","STSTM8S207R6","ST","STM8",24,32,1,6,10,16,0,0,52,"No",1,1,null,"No",4,"Beeper,IWDG,WWDG",-40,85,2.95,5.5,64,"LQFP 64 10x10x1.4",2.65,null,2,5,500,null,null,null,"Active",null,"Mainstream Performance line 8bit MCU with 32 Kbytes Flash, 24 MHz CPU, integrated EEPROM",0]
["STM8S208MB","STSTM8S208MB","ST","STM8",24,128,2,6,10,16,0,0,68,"No",1,1,null,"No",4,"Beeper,IWDG,WWDG",-40,85,2.95,5.5,80,"LQFP 80 14x14x1.4",1.6081000000000001,null,2,5,500,null,null,null,"Active",null,"Mainstream Performance line 8bit MCU with 128 Kbytes Flash, 24 MHz CPU, integrated EEPROM",0]
["STM8TL53F4","STSTM8TL53F4","ST","STM8",16,16,2,null,0,0,0,0,12,"No",1,1,null,"No",3,null,-40,85,1.65,3.6,20,"TSSOP 20",null,1,null,12,250,null,null,null,"NRND",null,"8bit, ultralowpower, touchsensing MCUs with 16Kbyte Flash and proximity detection",0]
["PIC32MM0064GPM064","MicrochipPIC32MM0064GPM064","Microchip"," 32bit MIPS MCU",25,64,0,16,16,20,1,3,52,"No",3,3,3,"Yes",31,null,-40,125,2,3.6,64," 64/QFN 64/TQFP",1.47,null,3,null,null,0,null,null," In Production ","",null,2,null,0," None","No"]
["PIC32MM0128GPM048","MicrochipPIC32MM0128GPM048","Microchip"," 32bit MIPS MCU",25,128,0,16,16,17,1,3,38,"No",3,3,3,"Yes",31,null,-40,125,2,3.6,48," 48/TQFP 48/UQFN",1.42,null,3,null,null,0,null,null," In Production ","",null,2,null,0," None","No"]
["PIC32MX230F064B","MicrochipPIC32MX230F064B","Microchip"," 32bit MIPS MCU",40,64,0,16,16,9,0,3,19,"No",2,2,2,"Yes",7,null,-40,105,2.2999999999999998,3.6,28," 28/QFN 28/SOIC 28/SPDIP 28/SSOP",2.02,null,2,null,null,0,null,null," In Production ","",null,2,null,0," None","Yes"]
["PIC32MX440F128H","MicrochipPIC32MX440F128H","Microchip"," 32bit MIPS MCU",80,128,0,32,16,16,0,2,51,"No",2,1,0,"Yes",6,null,-40,105,2.2999999999999998,3.6,64," 64/QFN 64/TQFP",4.0199999999999996,null,2,null,null,0,null,null," In Production ","",null,0,null,0,0,"No"]
["PIC32MX530F128L","MicrochipPIC32MX530F128L","Microchip"," 32bit MIPS MCU",50,128,0,16,16,48,0,3,81,"No",2,4,4,"Yes",7,null,-40,105,2.2999999999999998,3.6,100," 100/TQFP",2.93,null,5,null,null,0,null,null," Future Product ","SD/MMC,",null,0,null,0,0,"No"]
["PIC32MX570F512H","MicrochipPIC32MX570F512H","Microchip"," 32bit MIPS MCU",50,512,0,64,16,28,0,3,49,"No",2,3,3,"Yes",7,null,-40,105,2.2999999999999998,3.6,64," 64/QFN 64/TQFP",3.79,null,4,null,null,0,null,null," In Production ","",null,3,null,360,1,"No"]
["PIC32MX664F128L","MicrochipPIC32MX664F128L","Microchip"," 32bit MIPS MCU",80,128,0,32,16,16,0,2,85,"No",5,4,0,"Yes",7,null,-40,105,2.2999999999999998,3.6,100," 100/TQFP 121/TFBGA",3.86,null,6,null,null,0,null,null," Future Product ","SD/MMC,",null,3,null,464,1,"No"]
["PIC32MZ1024EFM144","MicrochipPIC32MZ1024EFM144","Microchip"," 32bit MIPS MCU",200,1024,0,512,12,48,0,2,120,"No",5,6,6,"No",13,null,-40,125,2.2000000000000002,3.6,144," 144/LQFP 144/TFBGA 144/TQFP",8.1199999999999992,null,6,null,null,0,null,null," In Production ","CAN,EtherNet",null,"  ",null,"  ",3,"No"]
["PIC32MZ2048EFH144","MicrochipPIC32MZ2048EFH144","Microchip"," 32bit MIPS MCU",252,2048,0,512,12,48,0,2,120,"No",5,6,6,"No",13,null,-40,125,2.2000000000000002,3.6,144," 144/LQFP 144/TFBGA 144/TQFP",8.82,null,6,null,null,0,null,null," In Production ","CAN,EtherNet",null,0,null,0,3,"No"]
["MSP432P4011","TIMSP432P4011","TI","ARM CM4F",48,2048,null,256,14,12,0,2,48,"No",3,6,null,"No",5,null,-40,85,1.62,3.7,64,"VQFN|64",null,null,3,100,0.82,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 2MB Flash and 256KB RAM",0,"N/A",0,3,"No"]
["MSP432P411YT","TIMSP432P411YT","TI","ARM CM4F",24,1025,null,256,14,24,0,2,84,"Yes",4,8,null,"No",6,null,-40,105,1.62,3.7,100,"LQFP|100",null,null,4,100,14.4,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 1MB Flash and 256KB RAM",null,"N/A",0," Full Speed","No"]
["LPC11E35FHI33/501E","NXPLPC11E35FHI33/501E","NXP","Arm Cortex-M0",50,256,4,null,10,null,0,null,null,"No",1,2,"","No","2 x 16",null,-40,85,null,null,null,"HVQFN32",1.52,null,1,null,null,null,"","","Active",null,null,null,null,"",0,"No"]
["LPC2210FBD144/01,5","NXPLPC2210FBD144/01,5","NXP","Arm7",60,"","",null,10,null,0,null,null,"No",1,1,"","No","",null,null,null,3,3.6,null,"LQFP144",3.79,null,2,null,null,null,"","","Not Recommended for New Designs",null,null,null,null,"",0,"No",null,null,null,null,null,null,null,null,null,"MSP430FR2100","MSP430FR2110","MSP430FR2000","MSP430G2001","MSP430FR2111"]
["LPC5512JBD100Y","NXPLPC5512JBD100Y","NXP","Arm Cortex-M33",150,64,"",null,16,null,0,null,null,"No",0,0,8,"No","",null,-40,105,1.8,3.6,null,"HLQFP100",1.21,null,0,null,null,null,"","AES-D, CRC, RNG, SD, UUID","Active",null,null,null,null,"AES-D, CRC, RNG, SD, UUID",0,"No"]
["LPC5514JBD64Y","NXPLPC5514JBD64Y","NXP","Arm Cortex-M33",150,128,"",null,16,null,0,null,null,"No",0,0,8,"No","",null,-40,105,1.8,3.6,null,"HTQFP64",1.21,null,0,null,null,null,"","AES-D, CRC, RNG, SD, UUID","Active",null,null,null,null,"AES-D, CRC, RNG, SD, UUID",0,"No"]
["LPC55S14JBD64E","NXPLPC55S14JBD64E","NXP","Arm Cortex-M33",150,128,"",null,16,null,0,null,null,"No",0,0,8,"No","",null,-40,105,1.8,3.6,null,"HTQFP64",1.31,null,0,null,null,null,"","AES-D, CRC, RNG, SD, UUID","Active",null,null,null,null,"AES-D, CRC, RNG, SD, UUID",0,"No"]
["LPC55S16JEV98E","NXPLPC55S16JEV98E","NXP","Arm Cortex-M33",150,256,"",null,16,null,0,null,null,"No",0,0,8,"No","",null,-40,105,1.8,3.6,null,"VFBGA98",1.75,null,0,null,null,null,"","AES-D, CRC, RNG, SD, TZ, UUID","Active",null,null,null,null,"AES-D, CRC, RNG, SD, TZ, UUID",0,"No"]
["LPC11U14FBD48/20EL","NXPLPC11U14FBD48/20EL","NXP","Arm Cortex-M0",50,32,"",null,10,null,0,null,null,"No",1,2,"","Yes","2 x 16",null,-40,85,1.8,3.6,null,"LQFP48",1.1299999999999999,null,1,null,null,null,"","","Qualification",null,null,null,null,"",1,"No"]
["LPC1820FET100/3DK","NXPLPC1820FET100/3DK","NXP","Arm Cortex-M3",180,"","",null,10,null,0,null,null,"No",2,3,"","Yes","",null,-40,85,2.4,3.6,null,"TFBGA100",3.01,null,4,null,null,null,"","","Qualification",null,null,null,null,"",1,"No",null,null,null,null,null,null,null,null,null,"MSP430FR2100","MSP430FR2110","MSP430FR2000","MSP430G2001","MSP430FR2111"]
["LPC51U68JBD64QL","NXPLPC51U68JBD64QL","NXP","Arm Cortex-M0+",100,256,"",null,12,null,0,null,null,"No",8,8,8,"Yes","",null,-40,105,1.62,3.6,null,"LQFP64",1.37,null,8,null,null,null,"","","Active",null,null,null,null,"",1,"No"]
["LPC54608J512BD208K","NXPLPC54608J512BD208K","NXP","Arm Cortex-M4",180,512,16,null,12,null,0,null,null,"Yes",10,10,2,"Yes","",null,-40,105,1.71,3.6,null,"LQFP208",2.91,null,10,null,null,null,"","CRC, LTC, RNG","Qualification",null,null,null,null,"CRC, LTC, RNG",2,"Yes"]
["LPC5528JBD64E","NXPLPC5528JBD64E","NXP","Arm Cortex-M33",150,512,"",null,16,null,0,null,null,"No",8,8,8,"Yes","",null,-40,105,1.8,3.6,null,"HTQFP64",1.85,null,8,null,null,null,"","CRC, RNG","Active",null,null,null,null,"CRC, RNG",2,"No"]
["LPC55S28JBD100Y","NXPLPC55S28JBD100Y","NXP","Arm Cortex-M33",150,512,"",null,16,null,0,null,null,"No",8,8,8,"Yes","",null,-40,105,1.8,3.6,null,"HLQFP100",2.2200000000000002,null,8,null,null,null,"","CRC, RNG","Active",null,null,null,null,"CRC, RNG",2,"No"]
["ST10F276Z5","STST10F276Z5","ST","ST10",null,832,64,68,10,24,0,0,11,"No",1,null,null,"No",null,"RTC,WDG",-40,125,1.8,5,144,"LQFP 144 20x20x1.4",null,null,null,null,null,null,null,null,"NRND",null,null,0]
["ST72324BJ4","STST72324BJ4","ST","ST7",null,null,null,null,10,12,0,0,32,"No",null,null,null,"No",null,"RTC,WDG",-40,85,null,null,null,"LQFP 44 10x10x1.4",null,null,null,null,null,null,null,null,"NRND",null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,"MSP430FR5731","MSP430FR5733","MSP430FR5735","MSP430FR5723","MSP430F5131"]
["ST7232AK2","STST7232AK2","ST","ST7",null,null,null,null,10,8,0,0,24,"No",null,null,null,"No",null,"RTC,WDG",-40,85,null,null,null,"LQFP 32 7x7x1.4",null,null,null,null,null,null,null,null,"NRND",null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,"MSP430G2233","MSP430G2203","MSP430G2153","MSP430G2213","MSP430G2253"]
["ST7LITE09Y0","STST7LITE09Y0","ST","ST7",null,null,null,null,8,5,0,0,13,"No",null,null,null,"No",null,"RTC,WDG",-40,85,null,null,null,"PDIP 16,SO-16",null,null,null,null,null,null,null,null,"NRND",null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,"MSP430FR2100","MSP430FR2110","MSP430FR2000","MSP430G2001","MSP430FR2111"]
["STM32WB55RE","STSTM32WB55RE","ST","Arm Cortex-M4",64,512,null,256,12,19,0,2,49,"Yes",2,2,"-","Yes",6,"Dual Watchdog,LP timer,RTC,SysTick",-40,"105,85",1.71,3.6,null,"VFQFPN 8X8X1.0 68L PITCH 0.4",null,1,1,0.04,90,null,"AES","true","Active",null,null,0,null,"Segment LCD","USB FS",null,null,null,null,null,null,null,null,null,null,"MSP432P401V","MSP432P401VT"]
["STR711FR1","STSTR711FR1","ST","ARM7TDMI",null,null,null,null,12,4,0,0,30,"No",null,null,null,"No",null,"RTC,WDG",-40,85,null,null,null,"LQFP 64 10x10x1.4",null,null,null,null,null,null,null,null,"NRND",null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,"MSP430FR5731","MSP430FR5733","MSP430FR5735","MSP430FR5723","MSP430F5131"]
["STR735FZ1","STSTR735FZ1","ST","ARM7TDMI",null,null,null,null,10,16,0,0,112,"No",null,null,null,"No",null,"RTC,WDG",-40,"105,85",null,null,null,"LQFP 144 20x20x1.4",null,null,null,null,null,null,null,null,"NRND",null,null,0]
["STR755FV1","STSTR755FV1","ST","ARM7TDMI",null,null,null,null,10,16,0,0,72,"No",null,null,null,"No",null,"RTC,WDG",-40,85,null,null,null,"LQFP 100 14x14x1.4",null,null,null,null,null,null,null,null,"NRND",null,null,0]
["EFM8BB10F8I-QSOP24","SiliconLabsEFM8BB10F8I-QSOP24","SiliconLabs","8051","25","8",null,"0.5","12","16",0,"2","18","No","1","1","0","No","4",null,null,null,"2.2","3.6",null,"QSOP24",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2433","MSP430FR2512","MSP430G2412","MSP430G2402"]
["EFM8BB22F16I-QFN28","SiliconLabsEFM8BB22F16I-QFN28","SiliconLabs","8051","50","16",null,"2.25","12","20",0,"2","22","No","1","1","0","No","5",null,null,null,"2.2","3.6",null,"QFN28",null,0,"2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430G2533","MSP430G2513","MSP430G2553","MSP430G2544"]
["EFM8BB31F32A-4QFN24","SiliconLabsEFM8BB31F32A-4QFN24","SiliconLabs","8051","50","32",null,"2.25","12","12",2,"2","20","No","1","1","0","No","6",null,null,null,"2.2","3.6",null,"QFN24",null,0,"2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430I2021","MSP430I2031","MSP430I2041"]
["EFM8BB31F32I-QFN32","SiliconLabsEFM8BB31F32I-QFN32","SiliconLabs","8051","50","32",null,"2.25","12","20",2,"2","29","No","1","1","0","No","6",null,null,null,"2.2","3.6",null,"QFN32",null,0,"2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2744","MSP430G2755","MSP430F5171","MSP430F5172","MSP430FR5857"]
["EFM8LB11F16E-QFN24","SiliconLabsEFM8LB11F16E-QFN24","SiliconLabs","8051","72","16",null,"1.25","14","12",2,"2","20","No","1","1","0","No","6",null,null,null,"2.2","3.6",null,"QFN24",null,0,"2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430I2020","MSP430G2553","MSP430G2533","MSP430G2513"]
["EFM8SB10F2G-QFN20","SiliconLabsEFM8SB10F2G-QFN20","SiliconLabs","8051","25","2",null,"0.25","12","9",0,"1","16","No","1","1","0","No","4",null,null,null,"1.8","3.6",null,"QFN20",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2110","MSP430FR2111","MSP430FR2422","MSP430FR2310","MSP430FR2311"]
["EFM8SB20F32G-QFN24","SiliconLabsEFM8SB20F32G-QFN24","SiliconLabs","8051","25","32",null,"4","10","15",0,"2","16","No","1","2","0","No","4",null,null,null,"1.8","3.6",null,"QFN24",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430I2021","MSP430I2031","MSP430I2041","MSP430F427A","MSP430FE4272"]
["EFM8UB11F16G-QSOP24","SiliconLabsEFM8UB11F16G-QSOP24","SiliconLabs","8051","48","16",null,"2","12","15",0,"2","17","No","2","1",0,"Yes","5",null,null,null,"2.2","5.25",null,"QSOP24",null,0,"2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430I2020","MSP430G2553","MSP430G2533","MSP430G2513"]
["C8051F005","SiliconLabsC8051F005","SiliconLabs","8051","25","32",null,"2.25","12","8",2,"2","32","No","1","1","0","No","4",null,null,null,"2.7","3.6",null,"QFP64",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2744","MSP430G2755","MSP430F5171","MSP430FR58671","MSP430F5172"]
["C8051F018","SiliconLabsC8051F018","SiliconLabs","8051","25","16",null,"1.25","10","8",2,"2","32","No","1","1","0","No","4",null,null,null,"2.7","3.6",null,"QFP64",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2544","MSP430FR5729","MSP430FR5727","MSP430F5151","MSP430F5152"]
["C8051F040","SiliconLabsC8051F040","SiliconLabs","8051","25","64",null,"4.25","12","13",2,"3","64","No","1","1","0","No","5",null,null,null,"2.7","3.6",null,"QFP100",null,0,"2",null,null,null,"No",null,null,"CAN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5515","MSP430F5325","MSP430F6723","MSP430FG6425","MSP430F67621"]
["C8051F061","SiliconLabsC8051F061","SiliconLabs","8051","25","64",null,"4.25","16","1",2,"3","24","No","1","1","0","No","5",null,null,null,"2.7","3.6",null,"QFP64",null,0,"2",null,null,null,"No",null,null,"CAN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5849","MSP430FR5859","MSP430FR5949","MSP430FR5959"]
["C8051F301-GM","SiliconLabsC8051F301-GM","SiliconLabs","8051","25","8",null,"0.25",null,null,0,"1","8","No","1","0","0","No","3",null,null,null,"2.7","3.6",null,"QFN11",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2512","MSP430G2412","MSP430G2402","MSP430G2452"]
["C8051F313","SiliconLabsC8051F313","SiliconLabs","8051","25","8",null,"1.25","10","17",0,"2","25","No","1","1","0","No","4",null,null,null,"2.7","3.6",null,"QFN28",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2433","MSP430G2413","MSP430G2403","MSP430G2453","MSP430FR5734"]
["C8051F340-GQ","SiliconLabsC8051F340-GQ","SiliconLabs","8051","50","64",null,"4.25","10","20",0,"2","40","No","1","1","0","Yes","4",null,null,null,"2.7","5.25",null,"QFP48",null,0,"2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR59691","MSP430FR2476","MSP430FR2676","MSP430F5232","MSP430F5242"]
["C8051F349-GM","SiliconLabsC8051F349-GM","SiliconLabs","8051","25","32",null,"2.25",null,null,0,"2","25","No","1","1","0","Yes","4",null,null,null,"2.7","5.25",null,"QFN32",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2744","MSP430G2755","MSP430F5171","MSP430F5172","MSP430FR5857"]
["C8051F331","SiliconLabsC8051F331","SiliconLabs","8051","25","8",null,"0.75",null,null,0,"1","17","No","1","1","0","No","4",null,null,null,"2.7","3.6",null,"QFN20",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2433","MSP430FR2512","MSP430G2412","MSP430G2402"]
["C8051F350","SiliconLabsC8051F350","SiliconLabs","8051","50","8",null,"0.75","24","8",2,"1","17","No","1","1","0","No","4",null,null,null,"2.7","3.6",null,"QFP32",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2433","MSP430FR2512","MSP430G2412","MSP430G2402"]
["C8051F369","SiliconLabsC8051F369","SiliconLabs","8051","50","16",null,"1.25","10","17",1,"2","25","No","1","1","0","No","4",null,null,null,"2.7","3.6",null,"QFN28",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2553","MSP430G2533","MSP430G2513","MSP430G2544","MSP430FR5728"]
["C8051F385-GQ","SiliconLabsC8051F385-GQ","SiliconLabs","8051","50","64",null,"4.25",null,null,0,"2","25","No","2","1","0","Yes","6",null,null,null,"2.7","5.25",null,"QFP32",null,0,"2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5849","MSP430FR5859","MSP430FR5949","MSP430FR5959"]
["C8051F399-A-GM","SiliconLabsC8051F399-A-GM","SiliconLabs","8051","50","4",null,"1",null,null,0,"1","17","No","2","1","0","No","6",null,null,null,"1.8","3.6",null,"QFN20",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2111","MSP430FR2422","MSP430FR2311","MSP430G2302","MSP430FR2512"]
["C8051F502-AM","SiliconLabsC8051F502-AM","SiliconLabs","8051","50","64",null,"4.25","12","25",0,"2","25","No","1","1","0","No","4",null,null,null,"1.8","5.25",null,"QFN32",null,0,"1",null,null,null,"No",null,null,"CAN LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5849","MSP430FR5859","MSP430FR5949","MSP430FR5959"]
["C8051F502-IQ","SiliconLabsC8051F502-IQ","SiliconLabs","8051","50","64",null,"4.25","12","25",0,"2","25","No","1","1","0","No","4",null,null,null,"1.8","5.25",null,"QFP32",null,0,"1",null,null,null,"No",null,null,"CAN LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5849","MSP430FR5859","MSP430FR5949","MSP430FR5959"]
["C8051F507-IQ","SiliconLabsC8051F507-IQ","SiliconLabs","8051","50","32",null,"4.25","12","25",0,"2","25","No","1","1","0","No","4",null,null,null,"1.8","5.25",null,"QFP32",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2744","MSP430G2755","MSP430F5171","MSP430F5172","MSP430FR5857"]
["C8051F520-C-AM","SiliconLabsC8051F520-C-AM","SiliconLabs","8051","25","8",null,"0.25","12","6",0,"1","6","No","0","1","0","No","3",null,null,null,"2","5.25",null,"DFN10",null,0,"1",null,null,null,"No",null,null,"LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2512","MSP430G2412","MSP430G2402","MSP430G2452"]
["C8051F526-C-IM","SiliconLabsC8051F526-C-IM","SiliconLabs","8051","25","2",null,"0.25","12","6",0,"1","6","No","0","1","0","No","3",null,null,null,"2","5.25",null,"DFN10",null,0,"1",null,null,null,"No",null,null,"LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2110","MSP430FR2111","MSP430G2210","MSP430FR2422","MSP430G2230"]
["C8051F533-C-IM","SiliconLabsC8051F533-C-IM","SiliconLabs","8051","25","4",null,"0.25","12","16",0,"1","16","No","0","1","0","No","3",null,null,null,"2","5.25",null,"QFN20",null,0,"1",null,null,null,"No",null,null,"LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2111","MSP430FR2422","MSP430FR2311","MSP430G2302","MSP430FR2512"]
["C8051F536-C-IT","SiliconLabsC8051F536-C-IT","SiliconLabs","8051","25","2",null,"0.25","12","16",0,"1","16","No","0","1","0","No","3",null,null,null,"2","5.25",null,"TSSOP20",null,0,"1",null,null,null,"No",null,null,"LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2110","MSP430FR2111","MSP430FR2422","MSP430FR2310","MSP430FR2311"]
["C8051F542-AM","SiliconLabsC8051F542-AM","SiliconLabs","8051","50","16",null,"1.25","12","18",0,"2","18","No","0","1","0","No","4",null,null,null,"1.8","5.25",null,"QFN24",null,0,"1",null,null,null,"No",null,null,"LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430I2020","MSP430G2553","MSP430G2533","MSP430G2513"]
["C8051F552-IM","SiliconLabsC8051F552-IM","SiliconLabs","8051","50","32",null,"2.25","12","18",0,"2","18","No","1","1","0","No","4",null,null,null,"1.8","5.25",null,"QFN24",null,0,"1",null,null,null,"No",null,null,"LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430I2021","MSP430I2031","MSP430I2041","MSP430F427A","MSP430FE4272"]
["C8051F557-AM","SiliconLabsC8051F557-AM","SiliconLabs","8051","50","16",null,"2.25","12","18",0,"2","18","No","1","1","0","No","4",null,null,null,"1.8","5.25",null,"QFN24",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430I2020","MSP430G2553","MSP430G2533","MSP430G2513"]
["C8051F562-IQ","SiliconLabsC8051F562-IQ","SiliconLabs","8051","50","32",null,"2.25","12","25",0,"2","25","No","1","1","0","No","4",null,null,null,"1.8","5.25",null,"QFP32",null,0,"1",null,null,null,"No",null,null,"LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2744","MSP430G2755","MSP430F5171","MSP430F5172","MSP430FR5857"]
["C8051F565-AM","SiliconLabsC8051F565-AM","SiliconLabs","8051","50","16",null,"2.25","12","25",0,"2","25","No","1","1","0","No","4",null,null,null,"1.8","5.25",null,"QFN32",null,0,"1",null,null,null,"No",null,null,"CAN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2553","MSP430G2533","MSP430G2513","MSP430G2544","MSP430FR5728"]
["C8051F567-AQ","SiliconLabsC8051F567-AQ","SiliconLabs","8051","50","16",null,"2.25","12","25",0,"2","25","No","1","1","0","No","4",null,null,null,"1.8","5.25",null,"QFP32",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2553","MSP430G2533","MSP430G2513","MSP430G2544","MSP430FR5728"]
["C8051F573-AM","SiliconLabsC8051F573-AM","SiliconLabs","8051","50","16",null,"2.25","12","32",0,"2","33","No","1","1","0","No","4",null,null,null,"1.8","5.25",null,"QFN40",null,0,"1",null,null,null,"No",null,null,"CAN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2544","MSP430FR5729","MSP430FR5727","MSP430F5151","MSP430F5152"]
["C8051F580-IQ","SiliconLabsC8051F580-IQ","SiliconLabs","8051","50","128",null,"8","12","32",0,"3","40","No","1","1","0","No","6",null,null,null,"1.8","5.25",null,"QFP48",null,0,"2",null,null,null,"No",null,null,"CAN LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5234","MSP430F5244","MSP430FR59891","MSP430F5214","MSP430F5224"]
["C8051F584-AM","SiliconLabsC8051F584-AM","SiliconLabs","8051","50","96",null,"8","12","32",0,"3","40","No","1","1","0","No","6",null,null,null,"1.8","5.25",null,"QFN48",null,0,"2",null,null,null,"No",null,null,"CAN LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5326","MSP430F5341","MSP430F5526","MSP430FR5888","MSP430FR5988"]
["C8051F590-IM","SiliconLabsC8051F590-IM","SiliconLabs","8051","50","96",null,"8","12","32",0,"3","33","No","1","1","0","No","6",null,null,null,"1.8","5.25",null,"QFN40",null,0,"2",null,null,null,"No",null,null,"CAN LIN ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5341"]
["C8051F803-GS","SiliconLabsC8051F803-GS","SiliconLabs","8051","25","16",null,"0.5","10","12",0,"1","13","No","1","1","0","No","3",null,null,null,"1.8","3.6",null,"SOIC16",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430I2020","MSP430I2030","MSP430I2040","MSP430FR5728"]
["C8051F807-GU","SiliconLabsC8051F807-GU","SiliconLabs","8051","25","16",null,"0.5",null,null,0,"1","17","No","1","1","0","No","3",null,null,null,"1.8","3.6",null,"QSOP24",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430I2020","MSP430G2553","MSP430G2533","MSP430G2513"]
["C8051F819-GM","SiliconLabsC8051F819-GM","SiliconLabs","8051","25","8",null,"0.5",null,null,0,"1","17","No","1","1","0","No","3",null,null,null,"1.8","3.6",null,"QFN20",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2433","MSP430FR2512","MSP430G2412","MSP430G2402"]
["C8051F826-GS","SiliconLabsC8051F826-GS","SiliconLabs","8051","25","8",null,"0.25","10","12",0,"1","13","No","1","1","0","No","3",null,null,null,"1.8","3.6",null,"SOIC16",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2433","MSP430FR2512","MSP430G2412","MSP430G2402"]
["C8051F851-C-GU","SiliconLabsC8051F851-C-GU","SiliconLabs","8051","25","4",null,"0.5",null,null,0,"2","18","No","1","1","0","No","4",null,null,null,"2.2","3.6",null,"QSOP24",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2311","MSP430G2302","MSP430FR2512","MSP430G2312"]
["C8051F860-C-GS","SiliconLabsC8051F860-C-GS","SiliconLabs","8051","25","8",null,"0.5","12","12",0,"2","13","No","1","1","0","No","4",null,null,null,"2.2","3.6",null,"SOIC16",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2433","MSP430FR2512","MSP430G2412","MSP430G2402"]
["C8051F912-GU","SiliconLabsC8051F912-GU","SiliconLabs","8051","25","16",null,"0.75","12","15",0,"2","16","No","1","2","0","No","4",null,null,null,"0.9","3.6",null,"QSOP24",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430I2020","MSP430G2533","MSP430G2513","MSP430G2553"]
["C8051F969-B-GM","SiliconLabsC8051F969-B-GM","SiliconLabs","8051","25","16",null,"4.25","12","16",0,"2","34","No","1","1","0","No","4",null,null,null,"1.8","3.8",null,"QFN40",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2353","MSP430FR2153","MSP430G2544","MSP430FR5729","MSP430F5151"]
["C8051F982-GM","SiliconLabsC8051F982-GM","SiliconLabs","8051","25","4",null,"0.5","10","9",0,"1","16","No","1","1","0","No","4",null,null,null,"1.8","3.6",null,"QFN20",null,0,"1","10","tiv",null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2111","MSP430FR2422","MSP430FR2311","MSP430G2302","MSP430FR2512"]
["C8051F996-GM","SiliconLabsC8051F996-GM","SiliconLabs","8051","25","8",null,"0.5","12","10",0,"1","17","No","1","1","0","No","4",null,null,null,"1.8","3.6",null,"QFN24",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2433","MSP430FR2512","MSP430G2412","MSP430G2402"]
["C8051T602-GS","SiliconLabsC8051T602-GS","SiliconLabs","8051","25","4",null,"0.25","10","8",0,"1","8","No","1","0","0","No","3",null,null,null,"1.8","3.6",null,"SOIC14",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2111","MSP430FR2422","MSP430FR2311","MSP430G2302","MSP430FR2512"]
["C8051T616-GM","SiliconLabsC8051T616-GM","SiliconLabs","8051","25","16",null,"1.25","10","13",0,"2","21","No","1","1","0","No","4",null,null,null,"1.8","3.6",null,"QFN24",null,0,"1",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430I2020","MSP430G2533","MSP430G2513","MSP430G2553"]
["C8051T623-GM","SiliconLabsC8051T623-GM","SiliconLabs","8051","48","8",null,"1.25",null,null,0,"0","16","No","1","1","0","Yes","4",null,null,null,"1.8","5.25",null,"QFN24",null,0,"2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2433","MSP430FR2512","MSP430G2412","MSP430G2402"]
["EFM32TG11B120F128GM64","SiliconLabsEFM32TG11B120F128GM64","SiliconLabs",null,"48","128",null,"32","12","36",2,"2","56","No","2","4","4","No","2","RTC ",null,null,"1.8","3.8",null,"QFN64",null,"4","1",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430F5229","MSP430F5256"]
["EFM32TG11B140F64IQ48","SiliconLabsEFM32TG11B140F64IQ48","SiliconLabs",null,"48","64",null,"32","12","22",2,"2","37","No","2","4","4","No","2","RTC ",null,null,"1.8","3.8",null,"QFP48",null,"4","1",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR59691","MSP430FR2476","MSP430FR2676","MSP430F5232","MSP430FR5849"]
["EFM32TG11B520F128IM64","SiliconLabsEFM32TG11B520F128IM64","SiliconLabs",null,"48","128",null,"32","12","43",2,"2","53","Yes","2","4","4","No","2","RTC ",null,null,"1.8","3.8",null,"QFN64",null,"4","1",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["EFM32TG11B540F64GQ64","SiliconLabsEFM32TG11B540F64GQ64","SiliconLabs",null,"48","64",null,"32","12","40",2,"2","50","Yes","2","4","4","No","2","RTC ",null,null,"1.8","3.8",null,"QFP64",null,"4","1",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32GG11B120F2048GQ64","SiliconLabsEFM32GG11B120F2048GQ64","SiliconLabs",null,"72","2048",null,"512","12","ksps",1,"4","53","No","3","6","3","No","7","RTC ",null,null,"1.8","3.8",null,"QFP64",null,"6","2",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P4011","MSP432P4011T"]
["EFM32GG11B420F2048GM64","SiliconLabsEFM32GG11B420F2048GM64","SiliconLabs",null,"72","2048",null,"512","12","ksps",1,"4","53","Yes","3","6","3","Yes","7","RTC ",null,null,"1.8","3.8",null,"QFN64",null,"6","2",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P4011","MSP432P4011T"]
["EFM32GG11B510F2048IQ64","SiliconLabsEFM32GG11B510F2048IQ64","SiliconLabs",null,"72","2048",null,"384","12","ksps",1,"4","50","Yes","3","6","3","No","7","RTC ",null,null,"1.8","3.8",null,"QFP64",null,"6","2",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P4011","MSP432P4011T"]
["EFM32GG11B520F2048IQ64","SiliconLabsEFM32GG11B520F2048IQ64","SiliconLabs",null,"72","2048",null,"512","12","ksps",1,"4","50","Yes","3","6","3","No","7","RTC ",null,null,"1.8","3.8",null,"QFP64",null,"6","2",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P4011","MSP432P4011T"]
["EFM32GG11B820F2048IM64","SiliconLabsEFM32GG11B820F2048IM64","SiliconLabs",null,"72","2048",null,"512","12","ksps",1,"4","50","Yes","3","6","3","Yes","7","RTC ",null,null,"1.8","3.8",null,"QFN64",null,"6","2",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P4011","MSP432P4011T"]
["EFM32GG11B840F1024IQ64","SiliconLabsEFM32GG11B840F1024IQ64","SiliconLabs",null,"72","1024",null,"512","12","ksps",1,"4","47","Yes","3","6","3","Yes","7","RTC ",null,null,"1.8","3.8",null,"QFP64",null,"6","2",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401Y","MSP432P401YT"]
["EFM32GG12B410F1024IQ100","SiliconLabsEFM32GG12B410F1024IQ100","SiliconLabs",null,"72","1024",null,"192","12","ksps",1,"3","83","Yes","2","5","2","Yes","4","RTC ",null,null,"1.8","3.8",null,"QFP100",null,"5","2",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y","MSP432P411Y","MSP432P411YT"]
["EFM32GG12B410F1024IQ64","SiliconLabsEFM32GG12B410F1024IQ64","SiliconLabs",null,"72","1024",null,"192","12","ksps",1,"3","50","Yes","2","5","2","Yes","4","RTC ",null,null,"1.8","3.8",null,"QFP64",null,"5","2",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401Y","MSP432P401YT"]
["EFM32GG12B530F512GL112","SiliconLabsEFM32GG12B530F512GL112","SiliconLabs",null,"72","512",null,"192","12","ksps",1,"3","92","Yes","2","5","2","No","4","RTC ",null,null,"1.8","3.8",null,"BGA112",null,"5","2",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6778A","MSP430F67781A","MSP430F67481A","MSP430F6769A","MSP430F67691A"]
["EFM32GG12B530F512IQ64","SiliconLabsEFM32GG12B530F512IQ64","SiliconLabs",null,"72","512",null,"192","12","ksps",1,"3","51","Yes","2","5","2","No","4","RTC ",null,null,"1.8","3.8",null,"QFP64",null,"5","2",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401V","MSP432P401VT"]
["EFM32GG12B830F512GM64","SiliconLabsEFM32GG12B830F512GM64","SiliconLabs",null,"72","512",null,"192","12","ksps",1,"3","51","Yes","2","5","2","Yes","4","RTC ",null,null,"1.8","3.8",null,"QFN64",null,"5","2",null,null,null,"ECC SHA-1 SHA-2 AES-1AES-256 ",null,null,"CAN Ethernet ","0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401V","MSP432P401VT"]
["EFM32JG12B500F1024GM48","SiliconLabsEFM32JG12B500F1024GM48","SiliconLabs",null,"40","1024",null,"256","12","33",2,"2","33","No","2","4","2","No","2","CryoTimer LeTimer",null,null,"1.8","3.8",null,"QFN48",null,"4","0",null,null,null,"AES-128AES-256 ECC SHA-1 SHA-2 TRNG SMU ",null,null,null,"3",null,null,null,"Yes"]
["EFM32JG1B200F256GM48","SiliconLabsEFM32JG1B200F256GM48","SiliconLabs",null,"40","256",null,"32","12","24",0,"2","32","No","1","2","1","No","2","CryoTimer LeTimer",null,null,"1.85","3.8",null,"QFN48",null,"2","0",null,null,null,"AES-128AES-256 ECC SHA-1 SHA-2 ",null,null,null,"0",null,null,null,"Yes"]
["EFM32PG1B200F256GM48","SiliconLabsEFM32PG1B200F256GM48","SiliconLabs",null,"40","256",null,"32","12","24",0,"2","32","No","1","2","1","No","2","CryoTimer LeTimer",null,null,"1.85","3.8",null,"QFN48",null,"2","0",null,null,null,"AES-128AES-256 ECC SHA-1 SHA-2 ",null,null,null,"0",null,null,null,"Yes"]
["EFM32HG108F64G-QFN24","SiliconLabsEFM32HG108F64G-QFN24","SiliconLabs",null,"25","64",null,"8",null,null,0,2,"17","No","1","1","0","No","3","RTC ",null,null,"3.8","QFN24",null,"5x5",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No"]
["EFM32HG108F64N-QFN24","SiliconLabsEFM32HG108F64N-QFN24","SiliconLabs",null,"25","64",null,"8",null,null,0,2,"17","No","1","1","0","No","3","RTC ",null,null,"3.8","QFN24",null,"5x5",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No"]
["EFM32HG310F32G-QFN32","SiliconLabsEFM32HG310F32G-QFN32","SiliconLabs",null,"25","32",null,"8","12","4",0,2,"22","No","1","1","0","Yes","3","RTC ",null,null,"3.8","QFN32",null,"6x6",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2744","MSP430G2755","MSP430F5171","MSP430F5172","MSP430F5503"]
["EFM32HG322F32N-QFP48","SiliconLabsEFM32HG322F32N-QFP48","SiliconLabs",null,"25","32",null,"8","12","4",0,2,"35","No","1","1","0","Yes","3","RTC ",null,null,"3.8","QFP48",null,"7x7",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2155","MSP430FR2355","MSP430G2744","MSP430G2755","MSP430FR2475"]
["EFM32WG280F64-QFP100","SiliconLabsEFM32WG280F64-QFP100","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","86","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32WG295F256-BGA120","SiliconLabsEFM32WG295F256-BGA120","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","93","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6767A","MSP430F6777A","MSP430F67771A","MSP430F6746A","MSP430F6747"]
["EFM32WG380F64-QFP100","SiliconLabsEFM32WG380F64-QFP100","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","83","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32WG390F128-BGA112","SiliconLabsEFM32WG390F128-BGA112","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","87","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430F5419A","MSP430FR69791","MSP430F67451A","MSP430F6765"]
["EFM32WG390F256-BGA112","SiliconLabsEFM32WG390F256-BGA112","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","87","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401R","MSP430F5438A","MSP430F6767A","MSP430F6746A","MSP430F6747"]
["EFM32WG390F64-BGA112","SiliconLabsEFM32WG390F64-BGA112","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","87","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32WG395F128-BGA120","SiliconLabsEFM32WG395F128-BGA120","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","93","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6775A","MSP430F6775","MSP430F67451A","MSP430F6765A","MSP430F6765"]
["EFM32WG395F256-BGA120","SiliconLabsEFM32WG395F256-BGA120","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","93","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6767A","MSP430F6777A","MSP430F67771A","MSP430F6746A","MSP430F6747"]
["EFM32WG395F64-BGA120","SiliconLabsEFM32WG395F64-BGA120","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","93","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32WG840F128-QFN64","SiliconLabsEFM32WG840F128-QFN64","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","56","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430F5229","MSP430F5256"]
["EFM32WG840F256-QFN64","SiliconLabsEFM32WG840F256-QFN64","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","56","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32WG840F64-QFN64","SiliconLabsEFM32WG840F64-QFN64","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","56","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32WG842F128-QFP64","SiliconLabsEFM32WG842F128-QFP64","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","53","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["EFM32WG842F256-QFP64","SiliconLabsEFM32WG842F256-QFP64","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","53","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32WG842F64-QFP64","SiliconLabsEFM32WG842F64-QFP64","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","53","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32WG880F128-QFP100","SiliconLabsEFM32WG880F128-QFP100","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","86","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430F5419A","MSP430FR69791","MSP430F67451A","MSP430F6765"]
["EFM32WG880F256-QFP100","SiliconLabsEFM32WG880F256-QFP100","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","86","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401R","MSP430F5438A","MSP430F6767A","MSP430F6746A","MSP430F6747"]
["EFM32WG880F64-QFP100","SiliconLabsEFM32WG880F64-QFP100","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","86","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32WG890F128-BGA112","SiliconLabsEFM32WG890F128-BGA112","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","90","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5419A","MSP430F6775A","MSP430F67451A","MSP430F6775","MSP430F6765"]
["EFM32WG890F256-BGA112","SiliconLabsEFM32WG890F256-BGA112","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","90","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5438A","MSP430F6767A","MSP430F6777A","MSP430F6746A","MSP430F6747"]
["EFM32WG890F64-BGA112","SiliconLabsEFM32WG890F64-BGA112","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","90","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32WG895F128-BGA120","SiliconLabsEFM32WG895F128-BGA120","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","93","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6775A","MSP430F6775","MSP430F67451A","MSP430F6765A","MSP430F6765"]
["EFM32WG895F256-BGA120","SiliconLabsEFM32WG895F256-BGA120","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","93","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6767A","MSP430F6777A","MSP430F67771A","MSP430F6746A","MSP430F6747"]
["EFM32WG895F64-BGA120","SiliconLabsEFM32WG895F64-BGA120","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","93","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32WG940F128-QFN64","SiliconLabsEFM32WG940F128-QFN64","SiliconLabs",null,"48","128",null,"32","12","8",2,"1","53","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["EFM32WG940F256-QFN64","SiliconLabsEFM32WG940F256-QFN64","SiliconLabs",null,"48","256",null,"32","12","8",2,"1","53","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32WG940F64-QFN64","SiliconLabsEFM32WG940F64-QFN64","SiliconLabs",null,"48","64",null,"32","12","8",2,"1","53","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32WG942F128-QFP64","SiliconLabsEFM32WG942F128-QFP64","SiliconLabs",null,"48","128",null,"32","12","8",2,"1","50","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["EFM32WG942F256-QFP64","SiliconLabsEFM32WG942F256-QFP64","SiliconLabs",null,"48","256",null,"32","12","8",2,"1","50","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32WG942F64-QFP64","SiliconLabsEFM32WG942F64-QFP64","SiliconLabs",null,"48","64",null,"32","12","8",2,"1","50","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32WG980F128-QFP100","SiliconLabsEFM32WG980F128-QFP100","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","83","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430FR6035","MSP430F5419A","MSP430FR69791","MSP430F6765"]
["EFM32WG980F64-QFP100","SiliconLabsEFM32WG980F64-QFP100","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","83","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32WG990F128-BGA112","SiliconLabsEFM32WG990F128-BGA112","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","87","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430F5419A","MSP430FR69791","MSP430F67451A","MSP430F6765"]
["EFM32WG990F256-BGA112","SiliconLabsEFM32WG990F256-BGA112","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","87","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401R","MSP430F5438A","MSP430F6767A","MSP430F6746A","MSP430F6747"]
["EFM32WG990F64-BGA112","SiliconLabsEFM32WG990F64-BGA112","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","87","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32WG995F128-BGA120","SiliconLabsEFM32WG995F128-BGA120","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","93","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6775A","MSP430F6775","MSP430F67451A","MSP430F6765A","MSP430F6765"]
["EFM32WG995F256-BGA120","SiliconLabsEFM32WG995F256-BGA120","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","93","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6767A","MSP430F6777A","MSP430F67771A","MSP430F6746A","MSP430F6747"]
["EFM32WG995F64-BGA120","SiliconLabsEFM32WG995F64-BGA120","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","93","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG230F128G-QFN64","SiliconLabsEFM32LG230F128G-QFN64","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","56","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430F5229","MSP430F5256"]
["EFM32LG230F256G-QFN64","SiliconLabsEFM32LG230F256G-QFN64","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","56","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG230F64G-QFN64","SiliconLabsEFM32LG230F64G-QFN64","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","56","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32LG232F128G-QFP64","SiliconLabsEFM32LG232F128G-QFP64","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","53","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["EFM32LG232F256G-QFP64","SiliconLabsEFM32LG232F256G-QFP64","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","53","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG232F64G-QFP64","SiliconLabsEFM32LG232F64G-QFP64","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","53","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32LG280F128G-QFP100","SiliconLabsEFM32LG280F128G-QFP100","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","86","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430F5419A","MSP430FR69791","MSP430F67451A","MSP430F6765"]
["EFM32LG280F256G-QFP100","SiliconLabsEFM32LG280F256G-QFP100","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","86","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401R","MSP430F5438A","MSP430F6767A","MSP430F6746A","MSP430F6747"]
["EFM32LG280F64G-QFP100","SiliconLabsEFM32LG280F64G-QFP100","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","86","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32LG290F128G-BGA112","SiliconLabsEFM32LG290F128G-BGA112","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","90","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5419A","MSP430F6775A","MSP430F67451A","MSP430F6775","MSP430F6765"]
["EFM32LG290F256G-BGA112","SiliconLabsEFM32LG290F256G-BGA112","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","90","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5438A","MSP430F6767A","MSP430F6777A","MSP430F6746A","MSP430F6747"]
["EFM32LG290F64G-BGA112","SiliconLabsEFM32LG290F64G-BGA112","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","90","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG295F128G-BGA120","SiliconLabsEFM32LG295F128G-BGA120","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","93","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6775A","MSP430F6775","MSP430F67451A","MSP430F6765A","MSP430F6765"]
["EFM32LG295F256G-BGA120","SiliconLabsEFM32LG295F256G-BGA120","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","93","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6767A","MSP430F6777A","MSP430F67771A","MSP430F6746A","MSP430F6747"]
["EFM32LG295F64G-BGA120","SiliconLabsEFM32LG295F64G-BGA120","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","93","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG330F256G-QFN64","SiliconLabsEFM32LG330F256G-QFN64","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","53","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG330F64G-QFN64","SiliconLabsEFM32LG330F64G-QFN64","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","53","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32LG332F128G-QFP64","SiliconLabsEFM32LG332F128G-QFP64","SiliconLabs",null,"48","128",null,"32","12","8",2,"1","50","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["EFM32LG332F256G-QFP64","SiliconLabsEFM32LG332F256G-QFP64","SiliconLabs",null,"48","256",null,"32","12","8",2,"1","50","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG332F64G-QFP64","SiliconLabsEFM32LG332F64G-QFP64","SiliconLabs",null,"48","64",null,"32","12","8",2,"1","50","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32LG360F128G-CSP81","SiliconLabsEFM32LG360F128G-CSP81","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","65","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"CSP81",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5962","MSP430F5418A","MSP430F5329","MSP430F6636","MSP430F6735A"]
["EFM32LG360F256G-CSP81","SiliconLabsEFM32LG360F256G-CSP81","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","65","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"CSP81",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5964","MSP430F5437A","MSP430F5335","MSP430F5338","MSP430FR59941"]
["EFM32LG360F64G-CSP81","SiliconLabsEFM32LG360F64G-CSP81","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","65","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"CSP81",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5515","MSP430F5325","MSP430F6723","MSP430FG6425","MSP430F67621"]
["EFM32LG380F128G-QFP100","SiliconLabsEFM32LG380F128G-QFP100","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","83","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430FR6035","MSP430F5419A","MSP430FR69791","MSP430F6765"]
["EFM32LG380F256G-QFP100","SiliconLabsEFM32LG380F256G-QFP100","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","83","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401R","MSP430FR60371","MSP430F5438A","MSP430F6746A","MSP430F6747"]
["EFM32LG380F64G-QFP100","SiliconLabsEFM32LG380F64G-QFP100","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","83","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32LG390F128G-BGA112","SiliconLabsEFM32LG390F128G-BGA112","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","87","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430F5419A","MSP430FR69791","MSP430F67451A","MSP430F6765"]
["EFM32LG390F256G-BGA112","SiliconLabsEFM32LG390F256G-BGA112","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","87","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401R","MSP430F5438A","MSP430F6767A","MSP430F6746A","MSP430F6747"]
["EFM32LG390F64G-BGA112","SiliconLabsEFM32LG390F64G-BGA112","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","87","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32LG395F128G-BGA120","SiliconLabsEFM32LG395F128G-BGA120","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","93","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6775A","MSP430F6775","MSP430F67451A","MSP430F6765A","MSP430F6765"]
["EFM32LG395F256G-BGA120","SiliconLabsEFM32LG395F256G-BGA120","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","93","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6767A","MSP430F6777A","MSP430F67771A","MSP430F6746A","MSP430F6747"]
["EFM32LG395F64G-BGA120","SiliconLabsEFM32LG395F64G-BGA120","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","93","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG840F128G-QFN64","SiliconLabsEFM32LG840F128G-QFN64","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","56","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430F5229","MSP430F5256"]
["EFM32LG840F256G-QFN64","SiliconLabsEFM32LG840F256G-QFN64","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","56","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG840F64G-QFN64","SiliconLabsEFM32LG840F64G-QFN64","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","56","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32LG842F128G-QFP64","SiliconLabsEFM32LG842F128G-QFP64","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","53","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["EFM32LG842F256G-QFP64","SiliconLabsEFM32LG842F256G-QFP64","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","53","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG842F64G-QFP64","SiliconLabsEFM32LG842F64G-QFP64","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","53","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32LG880F128G-QFP100","SiliconLabsEFM32LG880F128G-QFP100","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","86","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430F5419A","MSP430FR69791","MSP430F67451A","MSP430F6765"]
["EFM32LG880F256G-QFP100","SiliconLabsEFM32LG880F256G-QFP100","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","86","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401R","MSP430F5438A","MSP430F6767A","MSP430F6746A","MSP430F6747"]
["EFM32LG880F64G-QFP100","SiliconLabsEFM32LG880F64G-QFP100","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","86","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32LG890F128G-BGA112","SiliconLabsEFM32LG890F128G-BGA112","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","90","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5419A","MSP430F6775A","MSP430F67451A","MSP430F6775","MSP430F6765"]
["EFM32LG890F256G-BGA112","SiliconLabsEFM32LG890F256G-BGA112","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","90","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5438A","MSP430F6767A","MSP430F6777A","MSP430F6746A","MSP430F6747"]
["EFM32LG890F64G-BGA112","SiliconLabsEFM32LG890F64G-BGA112","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","90","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG895F128G-BGA120","SiliconLabsEFM32LG895F128G-BGA120","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","93","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6775A","MSP430F6775","MSP430F67451A","MSP430F6765A","MSP430F6765"]
["EFM32LG895F256G-BGA120","SiliconLabsEFM32LG895F256G-BGA120","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","93","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6767A","MSP430F6777A","MSP430F67771A","MSP430F6746A","MSP430F6747"]
["EFM32LG895F64G-BGA120","SiliconLabsEFM32LG895F64G-BGA120","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","93","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG940F128G-QFN64","SiliconLabsEFM32LG940F128G-QFN64","SiliconLabs",null,"48","128",null,"32","12","8",2,"1","53","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["EFM32LG940F256G-QFN64","SiliconLabsEFM32LG940F256G-QFN64","SiliconLabs",null,"48","256",null,"32","12","8",2,"1","53","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG940F64G-QFN64","SiliconLabsEFM32LG940F64G-QFN64","SiliconLabs",null,"48","64",null,"32","12","8",2,"1","53","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32LG942F128G-QFP64","SiliconLabsEFM32LG942F128G-QFP64","SiliconLabs",null,"48","128",null,"32","12","8",2,"1","50","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["EFM32LG942F256G-QFP64","SiliconLabsEFM32LG942F256G-QFP64","SiliconLabs",null,"48","256",null,"32","12","8",2,"1","50","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32LG942F64G-QFP64","SiliconLabsEFM32LG942F64G-QFP64","SiliconLabs",null,"48","64",null,"32","12","8",2,"1","50","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32LG980F128G-QFP100","SiliconLabsEFM32LG980F128G-QFP100","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","83","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430FR6035","MSP430F5419A","MSP430FR69791","MSP430F6765"]
["EFM32LG980F256G-QFP100","SiliconLabsEFM32LG980F256G-QFP100","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","83","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401R","MSP430FR60371","MSP430F5438A","MSP430F6746A","MSP430F6747"]
["EFM32LG980F64G-QFP100","SiliconLabsEFM32LG980F64G-QFP100","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","83","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32LG990F128G-BGA112","SiliconLabsEFM32LG990F128G-BGA112","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","87","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430F5419A","MSP430FR69791","MSP430F67451A","MSP430F6765"]
["EFM32LG990F256G-BGA112","SiliconLabsEFM32LG990F256G-BGA112","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","87","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401R","MSP430F5438A","MSP430F6767A","MSP430F6746A","MSP430F6747"]
["EFM32LG990F64G-BGA112","SiliconLabsEFM32LG990F64G-BGA112","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","87","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32LG995F128G-BGA120","SiliconLabsEFM32LG995F128G-BGA120","SiliconLabs",null,"48","128",null,"32","12","8",2,"2","93","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6775A","MSP430F6775","MSP430F67451A","MSP430F6765A","MSP430F6765"]
["EFM32LG995F256G-BGA120","SiliconLabsEFM32LG995F256G-BGA120","SiliconLabs",null,"48","256",null,"32","12","8",2,"2","93","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6767A","MSP430F6777A","MSP430F67771A","MSP430F6746A","MSP430F6747"]
["EFM32LG995F64G-BGA120","SiliconLabsEFM32LG995F64G-BGA120","SiliconLabs",null,"48","64",null,"32","12","8",2,"2","93","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32GG230F1024-QFN64","SiliconLabsEFM32GG230F1024-QFN64","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","56","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32GG230F512-QFN64","SiliconLabsEFM32GG230F512-QFN64","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","56","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32GG232F1024-QFP64","SiliconLabsEFM32GG232F1024-QFP64","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","53","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401Y","MSP432P401YT"]
["EFM32GG232F512-QFP64","SiliconLabsEFM32GG232F512-QFP64","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","53","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401V","MSP432P401VT"]
["EFM32GG280F1024-QFP100","SiliconLabsEFM32GG280F1024-QFP100","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","86","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y","MSP432P411Y","MSP432P411YT"]
["EFM32GG280F512-QFP100","SiliconLabsEFM32GG280F512-QFP100","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","86","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P411VT","MSP432P411V","MSP430F67481A","MSP430F6778A","MSP430F67781A"]
["EFM32GG290F1024-BGA112","SiliconLabsEFM32GG290F1024-BGA112","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","90","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y"]
["EFM32GG290F512-BGA112","SiliconLabsEFM32GG290F512-BGA112","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","90","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6778A","MSP430F67781A","MSP430F67481A","MSP430F6769A","MSP430F67691A"]
["EFM32GG295F1024-BGA120","SiliconLabsEFM32GG295F1024-BGA120","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","93","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y"]
["EFM32GG295F512-BGA120","SiliconLabsEFM32GG295F512-BGA120","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","93","No","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6778A","MSP430F67781A","MSP430F67481A","MSP430F6769A","MSP430F67691A"]
["EFM32GG330F1024-QFN64","SiliconLabsEFM32GG330F1024-QFN64","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","53","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401Y","MSP432P401YT"]
["EFM32GG330F512-QFN64","SiliconLabsEFM32GG330F512-QFN64","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","53","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401V","MSP432P401VT"]
["EFM32GG332F1024-QFP64","SiliconLabsEFM32GG332F1024-QFP64","SiliconLabs",null,"48","1024",null,"128","12","8",2,"1","50","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401Y","MSP432P401YT"]
["EFM32GG332F512-QFP64","SiliconLabsEFM32GG332F512-QFP64","SiliconLabs",null,"48","512",null,"128","12","8",2,"1","50","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401V","MSP432P401VT"]
["EFM32GG380F1024-QFP100","SiliconLabsEFM32GG380F1024-QFP100","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","83","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y","MSP432P411Y","MSP432P411YT"]
["EFM32GG380F512-QFP100","SiliconLabsEFM32GG380F512-QFP100","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","83","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P411VT","MSP432P411V","MSP430F67481A","MSP430F6778A","MSP430F67781A"]
["EFM32GG390F1024-BGA112","SiliconLabsEFM32GG390F1024-BGA112","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","87","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y","MSP432P411Y","MSP432P411YT"]
["EFM32GG390F512-BGA112","SiliconLabsEFM32GG390F512-BGA112","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","87","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P411VT","MSP432P411V","MSP430F67481A","MSP430F6778A","MSP430F67781A"]
["EFM32GG395F1024-BGA120","SiliconLabsEFM32GG395F1024-BGA120","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","93","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y"]
["EFM32GG395F512-BGA120","SiliconLabsEFM32GG395F512-BGA120","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","93","No","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6778A","MSP430F67781A","MSP430F67481A","MSP430F6769A","MSP430F67691A"]
["EFM32GG840F1024-QFN64","SiliconLabsEFM32GG840F1024-QFN64","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","56","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32GG840F512-QFN64","SiliconLabsEFM32GG840F512-QFN64","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","56","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32GG842F1024-QFP64","SiliconLabsEFM32GG842F1024-QFP64","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","53","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401Y","MSP432P401YT"]
["EFM32GG842F512-QFP64","SiliconLabsEFM32GG842F512-QFP64","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","53","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401V","MSP432P401VT"]
["EFM32GG880F1024-QFP100","SiliconLabsEFM32GG880F1024-QFP100","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","86","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y","MSP432P411Y","MSP432P411YT"]
["EFM32GG880F512-QFP100","SiliconLabsEFM32GG880F512-QFP100","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","86","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P411VT","MSP432P411V","MSP430F67481A","MSP430F6778A","MSP430F67781A"]
["EFM32GG890F1024-BGA112","SiliconLabsEFM32GG890F1024-BGA112","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","90","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y"]
["EFM32GG890F512-BGA112","SiliconLabsEFM32GG890F512-BGA112","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","90","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6778A","MSP430F67781A","MSP430F67481A","MSP430F6769A","MSP430F67691A"]
["EFM32GG895F1024-BGA120","SiliconLabsEFM32GG895F1024-BGA120","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","93","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y"]
["EFM32GG895F512-BGA120","SiliconLabsEFM32GG895F512-BGA120","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","93","Yes","2","3","1","No","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6778A","MSP430F67781A","MSP430F67481A","MSP430F6769A","MSP430F67691A"]
["EFM32GG940F1024-QFN64","SiliconLabsEFM32GG940F1024-QFN64","SiliconLabs",null,"48","1024",null,"128","12","8",2,"1","53","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401Y","MSP432P401YT"]
["EFM32GG940F512-QFN64","SiliconLabsEFM32GG940F512-QFN64","SiliconLabs",null,"48","512",null,"128","12","8",2,"1","53","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401V","MSP432P401VT"]
["EFM32GG942F1024-QFP64","SiliconLabsEFM32GG942F1024-QFP64","SiliconLabs",null,"48","1024",null,"128","12","8",2,"1","50","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401Y","MSP432P401YT"]
["EFM32GG942F512-QFP64","SiliconLabsEFM32GG942F512-QFP64","SiliconLabs",null,"48","512",null,"128","12","8",2,"1","50","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","5",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401V","MSP432P401VT"]
["EFM32GG980F1024-QFP100","SiliconLabsEFM32GG980F1024-QFP100","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","83","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y","MSP432P411Y","MSP432P411YT"]
["EFM32GG980F512-QFP100","SiliconLabsEFM32GG980F512-QFP100","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","83","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P411VT","MSP432P411V","MSP430F67481A","MSP430F6778A","MSP430F67781A"]
["EFM32GG990F1024-BGA112","SiliconLabsEFM32GG990F1024-BGA112","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","87","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y","MSP432P411Y","MSP432P411YT"]
["EFM32GG990F512-BGA112","SiliconLabsEFM32GG990F512-BGA112","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","87","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P411VT","MSP432P411V","MSP430F67481A","MSP430F6778A","MSP430F67781A"]
["EFM32GG995F1024-BGA120","SiliconLabsEFM32GG995F1024-BGA120","SiliconLabs",null,"48","1024",null,"128","12","8",2,"2","93","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432E401Y"]
["EFM32GG995F512-BGA120","SiliconLabsEFM32GG995F512-BGA120","SiliconLabs",null,"48","512",null,"128","12","8",2,"2","93","Yes","2","3","1","Yes","4","RTC ",null,null,"1.98","3.8",null,"BGA120",null,"3","7",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F6778A","MSP430F67781A","MSP430F67481A","MSP430F6769A","MSP430F67691A"]
["EFM32TG108F16-QFN24","SiliconLabsEFM32TG108F16-QFN24","SiliconLabs",null,"32","16",null,"4",12,8,1,"2","17","No","1","1","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN24",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430I2020","MSP430G2553","MSP430G2533","MSP430G2513"]
["EFM32TG108F32-QFN24","SiliconLabsEFM32TG108F32-QFN24","SiliconLabs",null,"32","32",null,"4",12,8,1,"2","17","No","1","1","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN24",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430I2021","MSP430I2031","MSP430I2041","MSP430F427A","MSP430FE4272"]
["EFM32TG108F4-QFN24","SiliconLabsEFM32TG108F4-QFN24","SiliconLabs",null,"32","4",null,"2",12,8,1,"2","17","No","1","1","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN24",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2111","MSP430FR2422","MSP430FR2311","MSP430G2302","MSP430FR2512"]
["EFM32TG108F8-QFN24","SiliconLabsEFM32TG108F8-QFN24","SiliconLabs",null,"32","8",null,"2",12,8,1,"2","17","No","1","1","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN24",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2433","MSP430FR2512","MSP430G2412","MSP430G2402"]
["EFM32TG110F16-QFN24","SiliconLabsEFM32TG110F16-QFN24","SiliconLabs",null,"32","16",null,"4","12","2",2,"2","17","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN24",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430I2020","MSP430G2553","MSP430G2533","MSP430G2513"]
["EFM32TG110F32-QFN24","SiliconLabsEFM32TG110F32-QFN24","SiliconLabs",null,"32","32",null,"4","12","2",2,"2","17","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN24",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430I2021","MSP430I2031","MSP430I2041","MSP430F427A","MSP430FE4272"]
["EFM32TG110F4-QFN24","SiliconLabsEFM32TG110F4-QFN24","SiliconLabs",null,"32","4",null,"2","12","2",2,"2","17","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN24",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2111","MSP430FR2422","MSP430FR2311","MSP430G2302","MSP430FR2512"]
["EFM32TG110F8-QFN24","SiliconLabsEFM32TG110F8-QFN24","SiliconLabs",null,"32","8",null,"2","12","2",2,"2","17","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN24",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2422","MSP430FR2433","MSP430FR2512","MSP430G2412","MSP430G2402"]
["EFM32TG210F16-QFN32","SiliconLabsEFM32TG210F16-QFN32","SiliconLabs",null,"32","16",null,"4","12","4",2,"2","24","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN32",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430G2533","MSP430G2513","MSP430G2553","MSP430G2544"]
["EFM32TG210F32-QFN32","SiliconLabsEFM32TG210F32-QFN32","SiliconLabs",null,"32","32",null,"4","12","4",2,"2","24","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN32",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2744","MSP430G2755","MSP430F5171","MSP430F5172","MSP430FR5857"]
["EFM32TG210F8-QFN32","SiliconLabsEFM32TG210F8-QFN32","SiliconLabs",null,"32","8",null,"2","12","4",2,"2","24","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN32",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430G2433","MSP430G2413","MSP430G2403","MSP430G2453"]
["EFM32TG222F16-QFP48","SiliconLabsEFM32TG222F16-QFP48","SiliconLabs",null,"32","16",null,"4","12","4",2,"2","37","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2353","MSP430FR2153","MSP430G2544","MSP430FR5729","MSP430FR5727"]
["EFM32TG222F32-QFP48","SiliconLabsEFM32TG222F32-QFP48","SiliconLabs",null,"32","32",null,"4","12","4",2,"2","37","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2155","MSP430FR2355","MSP430G2744","MSP430G2755","MSP430FR2475"]
["EFM32TG222F8-QFP48","SiliconLabsEFM32TG222F8-QFP48","SiliconLabs",null,"32","8",null,"2","12","4",2,"2","37","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2353","MSP430FR2153","MSP430FR5733","MSP430FR5735","MSP430FR5723"]
["EFM32TG225F16-BGA48","SiliconLabsEFM32TG225F16-BGA48","SiliconLabs",null,"32","16",null,"4","12","4",2,"2","37","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"BGA48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2353","MSP430FR2153","MSP430G2544","MSP430FR5729","MSP430FR5727"]
["EFM32TG225F32-BGA48","SiliconLabsEFM32TG225F32-BGA48","SiliconLabs",null,"32","32",null,"4","12","4",2,"2","37","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"BGA48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2155","MSP430FR2355","MSP430G2744","MSP430G2755","MSP430FR2475"]
["EFM32TG225F8-BGA48","SiliconLabsEFM32TG225F8-BGA48","SiliconLabs",null,"32","8",null,"2","12","4",2,"2","37","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"BGA48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2353","MSP430FR2153","MSP430FR5733","MSP430FR5735","MSP430FR5723"]
["EFM32TG230F16-QFN64","SiliconLabsEFM32TG230F16-QFN64","SiliconLabs",null,"32","16",null,"4","12","8",2,"2","56","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2033","MSP430FR4133","MSP430F4152"]
["EFM32TG230F32-QFN64","SiliconLabsEFM32TG230F32-QFN64","SiliconLabs",null,"32","32",null,"4","12","8",2,"2","56","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6870","MSP430FR6970","MSP430FR5870"]
["EFM32TG230F8-QFN64","SiliconLabsEFM32TG230F8-QFN64","SiliconLabs",null,"32","8",null,"2","12","8",2,"2","56","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2032","MSP430FR4132","MSP430FR2033","MSP430FR4133","MSP430F4132"]
["EFM32TG232F16-QFP64","SiliconLabsEFM32TG232F16-QFP64","SiliconLabs",null,"32","16",null,"4","12","8",2,"2","53","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2033","MSP430FR4133","MSP430F415","MSP430F4152","MSP430F235"]
["EFM32TG232F32-QFP64","SiliconLabsEFM32TG232F32-QFP64","SiliconLabs",null,"32","32",null,"4","12","8",2,"2","53","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6970","MSP430FR6870","MSP430FR5870"]
["EFM32TG232F8-QFP64","SiliconLabsEFM32TG232F8-QFP64","SiliconLabs",null,"32","8",null,"2","12","8",2,"2","53","No","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2032","MSP430FR4132","MSP430FR2033","MSP430FR4133","MSP430F413"]
["EFM32TG822F16-QFP48","SiliconLabsEFM32TG822F16-QFP48","SiliconLabs",null,"32","16",null,"4","12","4",2,"2","37","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2353","MSP430FR2153","MSP430G2544","MSP430FR5729","MSP430FR5727"]
["EFM32TG822F32-QFP48","SiliconLabsEFM32TG822F32-QFP48","SiliconLabs",null,"32","32",null,"4","12","4",2,"2","37","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2155","MSP430FR2355","MSP430G2744","MSP430G2755","MSP430FR2475"]
["EFM32TG822F8-QFP48","SiliconLabsEFM32TG822F8-QFP48","SiliconLabs",null,"32","8",null,"2","12","4",2,"2","37","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2353","MSP430FR2153","MSP430FR5733","MSP430FR5735","MSP430FR5723"]
["EFM32TG825F16-BGA48","SiliconLabsEFM32TG825F16-BGA48","SiliconLabs",null,"32","16",null,"4","12","4",2,"2","37","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"BGA48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2353","MSP430FR2153","MSP430G2544","MSP430FR5729","MSP430FR5727"]
["EFM32TG825F32-BGA48","SiliconLabsEFM32TG825F32-BGA48","SiliconLabs",null,"32","32",null,"4","12","4",2,"2","37","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"BGA48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2155","MSP430FR2355","MSP430G2744","MSP430G2755","MSP430FR2475"]
["EFM32TG825F8-BGA48","SiliconLabsEFM32TG825F8-BGA48","SiliconLabs",null,"32","8",null,"2","12","4",2,"2","37","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"BGA48",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2353","MSP430FR2153","MSP430FR5733","MSP430FR5735","MSP430FR5723"]
["EFM32TG840F16-QFN64","SiliconLabsEFM32TG840F16-QFN64","SiliconLabs",null,"32","16",null,"4","12","8",2,"2","56","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2033","MSP430FR4133","MSP430F4152"]
["EFM32TG840F32-QFN64","SiliconLabsEFM32TG840F32-QFN64","SiliconLabs",null,"32","32",null,"4","12","8",2,"2","56","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6870","MSP430FR6970","MSP430FR5870"]
["EFM32TG840F8-QFN64","SiliconLabsEFM32TG840F8-QFN64","SiliconLabs",null,"32","8",null,"2","12","8",2,"2","56","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2032","MSP430FR4132","MSP430FR2033","MSP430FR4133","MSP430F4132"]
["EFM32TG842F16-QFP64","SiliconLabsEFM32TG842F16-QFP64","SiliconLabs",null,"32","16",null,"4","12","8",2,"2","53","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2033","MSP430FR4133","MSP430F415","MSP430F4152","MSP430F235"]
["EFM32TG842F32-QFP64","SiliconLabsEFM32TG842F32-QFP64","SiliconLabs",null,"32","32",null,"4","12","8",2,"2","53","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6970","MSP430FR6870","MSP430FR5870"]
["EFM32TG842F8-QFP64","SiliconLabsEFM32TG842F8-QFP64","SiliconLabs",null,"32","8",null,"2","12","8",2,"2","53","Yes","1","2","1","No","2","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"2","3",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2032","MSP430FR4132","MSP430FR2033","MSP430FR4133","MSP430F413"]
["EFM32G200F16-QFN32","SiliconLabsEFM32G200F16-QFN32","SiliconLabs",null,"32","16",null,"8","12","4",1,"2","24","No","1","2","0","No","2","RTC ",null,null,"1.98","3.8",null,"QFN32",null,"2","0",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2433","MSP430G2533","MSP430G2513","MSP430G2553","MSP430G2544"]
["EFM32G200F32-QFN32","SiliconLabsEFM32G200F32-QFN32","SiliconLabs",null,"32","32",null,"8","12","4",1,"2","24","No","1","2","0","No","2","RTC ",null,null,"1.98","3.8",null,"QFN32",null,"2","0",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2744","MSP430G2755","MSP430F5171","MSP430F5172","MSP430FR5857"]
["EFM32G200F64-QFN32","SiliconLabsEFM32G200F64-QFN32","SiliconLabs",null,"32","64",null,"16","12","4",1,"2","24","No","1","2","0","No","2","RTC ",null,null,"1.98","3.8",null,"QFN32",null,"2","0",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5849","MSP430FR5859","MSP430FR5949","MSP430FR5959"]
["EFM32G210F128-QFN32","SiliconLabsEFM32G210F128-QFN32","SiliconLabs",null,"32","128",null,"16","12","4",1,"2","24","No","1","2","0","No","2","RTC ",null,null,"1.98","3.8",null,"QFN32",null,"2","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32G222F128-QFP48","SiliconLabsEFM32G222F128-QFP48","SiliconLabs",null,"32","128",null,"16","12","4",1,"2","37","No","1","2","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP48",null,"2","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5234","MSP430F5244","MSP430F5214","MSP430F5224","MSP430F5328"]
["EFM32G222F32-QFP48","SiliconLabsEFM32G222F32-QFP48","SiliconLabs",null,"32","32",null,"8","12","4",1,"2","37","No","1","2","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP48",null,"2","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR2155","MSP430FR2355","MSP430G2744","MSP430G2755","MSP430FR2475"]
["EFM32G222F64-QFP48","SiliconLabsEFM32G222F64-QFP48","SiliconLabs",null,"32","64",null,"16","12","4",1,"2","37","No","1","2","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP48",null,"2","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR59691","MSP430FR2476","MSP430FR2676","MSP430F5232","MSP430FR5849"]
["EFM32G230F128-QFN64","SiliconLabsEFM32G230F128-QFN64","SiliconLabs",null,"32","128",null,"16","12","8",2,"2","56","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430F5229","MSP430F5256"]
["EFM32G230F32-QFN64","SiliconLabsEFM32G230F32-QFN64","SiliconLabs",null,"32","32",null,"8","12","8",2,"2","56","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6870","MSP430FR6970","MSP430FR5870"]
["EFM32G230F64-QFN64","SiliconLabsEFM32G230F64-QFN64","SiliconLabs",null,"32","64",null,"16","12","8",2,"2","56","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32G232F128-QFP64","SiliconLabsEFM32G232F128-QFP64","SiliconLabs",null,"32","128",null,"16","12","8",1,"2","53","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["EFM32G232F32-QFP64","SiliconLabsEFM32G232F32-QFP64","SiliconLabs",null,"32","32",null,"8","12","8",1,"2","53","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6970","MSP430FR6870","MSP430FR5870"]
["EFM32G232F64-QFP64","SiliconLabsEFM32G232F64-QFP64","SiliconLabs",null,"32","64",null,"16","12","8",1,"2","53","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32G280F128-QFP100","SiliconLabsEFM32G280F128-QFP100","SiliconLabs",null,"32","128",null,"16","12","8",2,"2","86","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430F5419A","MSP430FR69791","MSP430F67451A","MSP430F6765"]
["EFM32G280F32-QFP100","SiliconLabsEFM32G280F32-QFP100","SiliconLabs",null,"32","32",null,"8","12","8",2,"2","86","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32G280F64-QFP100","SiliconLabsEFM32G280F64-QFP100","SiliconLabs",null,"32","64",null,"16","12","8",2,"2","86","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32G290F128-BGA112","SiliconLabsEFM32G290F128-BGA112","SiliconLabs",null,"32","128",null,"16","12","8",2,"2","90","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5419A","MSP430F6775A","MSP430F67451A","MSP430F6775","MSP430F6765"]
["EFM32G290F32-BGA112","SiliconLabsEFM32G290F32-BGA112","SiliconLabs",null,"32","32",null,"8","12","8",2,"2","90","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32G290F64-BGA112","SiliconLabsEFM32G290F64-BGA112","SiliconLabs",null,"32","64",null,"16","12","8",2,"2","90","No","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32G840F128-QFN64","SiliconLabsEFM32G840F128-QFN64","SiliconLabs",null,"32","128",null,"16","12","8",2,"2","56","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430F5229","MSP430F5256"]
["EFM32G840F32-QFN64","SiliconLabsEFM32G840F32-QFN64","SiliconLabs",null,"32","32",null,"8","12","8",2,"2","56","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6870","MSP430FR6970","MSP430FR5870"]
["EFM32G840F64-QFN64","SiliconLabsEFM32G840F64-QFN64","SiliconLabs",null,"32","64",null,"16","12","8",2,"2","56","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFN64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32G842F128-QFP64","SiliconLabsEFM32G842F128-QFP64","SiliconLabs",null,"32","128",null,"16","12","8",1,"2","53","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["EFM32G842F32-QFP64","SiliconLabsEFM32G842F32-QFP64","SiliconLabs",null,"32","32",null,"8","12","8",1,"2","53","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6970","MSP430FR6870","MSP430FR5870"]
["EFM32G842F64-QFP64","SiliconLabsEFM32G842F64-QFP64","SiliconLabs",null,"32","64",null,"16","12","8",1,"2","53","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP64",null,"3","0",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["EFM32G880F128-QFP100","SiliconLabsEFM32G880F128-QFP100","SiliconLabs",null,"32","128",null,"16","12","8",2,"2","86","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP432P401M","MSP430F5419A","MSP430FR69791","MSP430F67451A","MSP430F6765"]
["EFM32G880F32-QFP100","SiliconLabsEFM32G880F32-QFP100","SiliconLabs",null,"32","32",null,"8","12","8",2,"2","86","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32G880F64-QFP100","SiliconLabsEFM32G880F64-QFP100","SiliconLabs",null,"32","64",null,"16","12","8",2,"2","86","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"QFP100",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR6977","MSP430FR6887","MSP430FR6987","MSP430FR6877"]
["EFM32G890F128-BGA112","SiliconLabsEFM32G890F128-BGA112","SiliconLabs",null,"32","128",null,"16","12","8",2,"2","90","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5419A","MSP430F6775A","MSP430F67451A","MSP430F6775","MSP430F6765"]
["EFM32G890F32-BGA112","SiliconLabsEFM32G890F32-BGA112","SiliconLabs",null,"32","32",null,"8","12","8",2,"2","90","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["EFM32G890F64-BGA112","SiliconLabsEFM32G890F64-BGA112","SiliconLabs",null,"32","64",null,"16","12","8",2,"2","90","Yes","1","3","0","No","3","RTC ",null,null,"1.98","3.8",null,"BGA112",null,"3","1",null,null,null,"AES-128AES-256 ",null,null,null,"0",null,null,null,"No"]
["SiM3C134-B-GM","SiliconLabsSiM3C134-B-GM","SiliconLabs",null,"80","32",null,"8","12","7",2,"2","28","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"QFN40",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2744","MSP430G2755","MSP430F5171","MSP430F5172","MSP430FR5857"]
["SiM3C136-B-GM","SiliconLabsSiM3C136-B-GM","SiliconLabs",null,"80","32",null,"8","12","13",2,"2","50","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"QFN64",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6970","MSP430F5310","MSP430FR6870"]
["SiM3C136-B-GQ","SiliconLabsSiM3C136-B-GQ","SiliconLabs",null,"80","32",null,"8","12","16",2,"2","50","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"TQFP64",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6970","MSP430F5310","MSP430FR6870"]
["SiM3C144-B-GM","SiliconLabsSiM3C144-B-GM","SiliconLabs",null,"80","64",null,"16","12","13",2,"2","28","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"QFN40",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5232","MSP430FR5849","MSP430FR5859","MSP430F5242","MSP430FR5959"]
["SiM3C146-B-GM","SiliconLabsSiM3C146-B-GM","SiliconLabs",null,"80","64",null,"16","12","7",2,"2","50","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"QFN64",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["SiM3C146-B-GQ","SiliconLabsSiM3C146-B-GQ","SiliconLabs",null,"80","64",null,"16","12","7",2,"2","50","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"TQFP64",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["SiM3C154-B-GM","SiliconLabsSiM3C154-B-GM","SiliconLabs",null,"80","128",null,"32","12","13",2,"2","28","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"QFN40",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5234","MSP430F5244","MSP430F5224","MSP430F5214","MSP430F5342"]
["SiM3C156-B-GM","SiliconLabsSiM3C156-B-GM","SiliconLabs",null,"80","128",null,"32","12","13",2,"2","50","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"QFN64",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["SiM3C156-B-GQ","SiliconLabsSiM3C156-B-GQ","SiliconLabs",null,"80","128",null,"32","12","13",2,"2","50","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"TQFP64",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["SiM3C157-B-GM","SiliconLabsSiM3C157-B-GM","SiliconLabs",null,"80","128",null,"32","12","7",2,"2","65","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"LGA92",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5962","MSP430F5418A","MSP430F5329","MSP430F6636","MSP430F6735A"]
["SiM3C157-B-GQ","SiliconLabsSiM3C157-B-GQ","SiliconLabs",null,"80","128",null,"32","12","13",2,"2","65","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"TQFP80",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5962","MSP430F5418A","MSP430F5329","MSP430F6636","MSP430F6735A"]
["SiM3C164-B-GM","SiliconLabsSiM3C164-B-GM","SiliconLabs",null,"80","256",null,"32","12","13",2,"2","28","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"QFN40",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No"]
["SiM3C166-B-GM","SiliconLabsSiM3C166-B-GM","SiliconLabs",null,"80","256",null,"32","12","13",2,"2","50","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"QFN64",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No"]
["SiM3C166-B-GQ","SiliconLabsSiM3C166-B-GQ","SiliconLabs",null,"80","256",null,"32","12","16",2,"2","50","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"TQFP64",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No"]
["SiM3C167-B-GM","SiliconLabsSiM3C167-B-GM","SiliconLabs",null,"80","256",null,"32","12","16",2,"2","65","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"LGA92",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5964","MSP430F5437A","MSP430F5335","MSP430F5338","MSP430FR59941"]
["SiM3C167-B-GQ","SiliconLabsSiM3C167-B-GQ","SiliconLabs",null,"80","256",null,"32","12","16",2,"2","65","No","2","3","1","No","5","RTC ",null,null,"1.8","5.5",null,"TQFP80",null,"0","4",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5964","MSP430F5437A","MSP430F5335","MSP430F5338","MSP430FR59941"]
["SiM3L134-C-GM","SiliconLabsSiM3L134-C-GM","SiliconLabs",null,"50","32",null,"8","12","20",0,"2","28","No","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"QFN40",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2744","MSP430G2755","MSP430F5171","MSP430F5172","MSP430FR5857"]
["SiM3L136-C-GM","SiliconLabsSiM3L136-C-GM","SiliconLabs",null,"50","32",null,"8","12","23",0,"2","51","Yes","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"QFN64",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6970","MSP430F5310","MSP430FR6870"]
["SiM3L136-C-GQ","SiliconLabsSiM3L136-C-GQ","SiliconLabs",null,"50","32",null,"8","12","23",0,"2","51","Yes","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"TQFP64",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6970","MSP430F5310","MSP430FR6870"]
["SiM3L144-C-GM","SiliconLabsSiM3L144-C-GM","SiliconLabs",null,"50","64",null,"16","12","20",0,"2","28","No","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"QFN40",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5232","MSP430FR5849","MSP430FR5859","MSP430F5242","MSP430FR5959"]
["SiM3L146-C-GM","SiliconLabsSiM3L146-C-GM","SiliconLabs",null,"50","64",null,"16","12","23",0,"2","51","Yes","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"QFN64",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["SiM3L146-C-GQ","SiliconLabsSiM3L146-C-GQ","SiliconLabs",null,"50","64",null,"16","12","23",0,"2","51","Yes","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"TQFP64",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["SiM3L154-C-GM","SiliconLabsSiM3L154-C-GM","SiliconLabs",null,"50","128",null,"32","12","20",0,"2","28","No","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"QFN40",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5234","MSP430F5244","MSP430F5224","MSP430F5214","MSP430F5342"]
["SiM3L156-C-GM","SiliconLabsSiM3L156-C-GM","SiliconLabs",null,"50","128",null,"32","12","23",0,"2","51","Yes","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"QFN64",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["SiM3L156-C-GQ","SiliconLabsSiM3L156-C-GQ","SiliconLabs",null,"50","128",null,"32","12","23",0,"2","51","Yes","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"TQFP64",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["SiM3L157-C-GQ","SiliconLabsSiM3L157-C-GQ","SiliconLabs",null,"50","128",null,"32","12","24",0,"2","62","Yes","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"TQFP80",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5962","MSP430F5418A","MSP430F5329","MSP430F6725A","MSP430F6725"]
["SiM3L164-C-GM","SiliconLabsSiM3L164-C-GM","SiliconLabs",null,"50","256",null,"32","12","20",0,"2","28","No","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"QFN40",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No"]
["SiM3L166-C-GM","SiliconLabsSiM3L166-C-GM","SiliconLabs",null,"50","256",null,"32","12","23",0,"2","51","Yes","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"QFN64",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No"]
["SiM3L166-C-GQ","SiliconLabsSiM3L166-C-GQ","SiliconLabs",null,"50","256",null,"32","12","23",0,"2","51","Yes","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"TQFP64",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No"]
["SiM3L167-C-GQ","SiliconLabsSiM3L167-C-GQ","SiliconLabs",null,"50","256",null,"32","12","24",0,"2","62","Yes","1","2","0","No","3","RTC ",null,null,"1.8","3.8",null,"TQFP80",null,"1","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5964","MSP430F5437A","MSP430FR5994","MSP430FR59941"]
["SiM3U134-B-GM","SiliconLabsSiM3U134-B-GM","SiliconLabs",null,"80","32",null,"8","12","7",2,"2","28","No","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"QFN40",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430G2744","MSP430G2755","MSP430F5171","MSP430F5172","MSP430FR5857"]
["SiM3U136-B-GM","SiliconLabsSiM3U136-B-GM","SiliconLabs",null,"80","32",null,"8","12","13",2,"2","50","No","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"QFN64",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6970","MSP430F5310","MSP430FR6870"]
["SiM3U136-B-GQ","SiliconLabsSiM3U136-B-GQ","SiliconLabs",null,"80","32",null,"8","12","13",2,"2","50","Yes","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"TQFP64",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5970","MSP430FR6920","MSP430FR6970","MSP430F5310","MSP430FR6870"]
["SiM3U144-B-GM","SiliconLabsSiM3U144-B-GM","SiliconLabs",null,"80","64",null,"16","12","7",2,"2","28","No","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"QFN40",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5232","MSP430FR5849","MSP430FR5859","MSP430F5242","MSP430FR5959"]
["SiM3U146-B-GM","SiliconLabsSiM3U146-B-GM","SiliconLabs",null,"80","64",null,"16","12","13",2,"2","50","No","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"QFN64",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["SiM3U146-B-GQ","SiliconLabsSiM3U146-B-GQ","SiliconLabs",null,"80","64",null,"16","12","13",2,"2","50","Yes","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"TQFP64",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5227","MSP430FR59221","MSP430FR5922","MSP430F5247","MSP430FR59721"]
["SiM3U154-B-GM","SiliconLabsSiM3U154-B-GM","SiliconLabs",null,"80","128",null,"32","12","7",2,"2","28","No","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"QFN40",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5234","MSP430F5244","MSP430F5224","MSP430F5214","MSP430F5342"]
["SiM3U156-B-GM","SiliconLabsSiM3U156-B-GM","SiliconLabs",null,"80","128",null,"32","12","13",2,"2","50","No","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"QFN64",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["SiM3U156-B-GQ","SiliconLabsSiM3U156-B-GQ","SiliconLabs",null,"80","128",null,"32","12","13",2,"2","50","Yes","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"TQFP64",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430F5239","MSP430F5257","MSP430F5249","MSP430FR59891","MSP430F5229"]
["SiM3U157-B-GM","SiliconLabsSiM3U157-B-GM","SiliconLabs",null,"80","128",null,"32","12","16",2,"2","65","No","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"LGA92",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5962","MSP430F5418A","MSP430F5329","MSP430F6636","MSP430F6735A"]
["SiM3U157-B-GQ","SiliconLabsSiM3U157-B-GQ","SiliconLabs",null,"80","128",null,"32","12","16",2,"2","65","Yes","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"TQFP80",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5962","MSP430F5418A","MSP430F5329","MSP430F6636","MSP430F6735A"]
["SiM3U164-B-GM","SiliconLabsSiM3U164-B-GM","SiliconLabs",null,"80","256",null,"32","12","7",2,"2","28","No","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"QFN40",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No"]
["SiM3U166-B-GM","SiliconLabsSiM3U166-B-GM","SiliconLabs",null,"80","256",null,"32","12","13",2,"2","50","No","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"QFN64",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No"]
["SiM3U166-B-GQ","SiliconLabsSiM3U166-B-GQ","SiliconLabs",null,"80","256",null,"32","12","13",2,"2","50","Yes","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"TQFP64",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No"]
["SiM3U167-B-GM","SiliconLabsSiM3U167-B-GM","SiliconLabs",null,"80","256",null,"32","12","16",2,"2","65","No","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"LGA92",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5964","MSP430F5437A","MSP430F5335","MSP430F5338","MSP430FR59941"]
["SiM3U167-B-GQ","SiliconLabsSiM3U167-B-GQ","SiliconLabs",null,"80","256",null,"32","12","16",2,"2","65","Yes","2","3","1","Yes","1","RTC ",null,null,"1.8","5.5",null,"TQFP80",null,"2","2",null,null,null,"No",null,null,null,"0",null,null,null,"No",null,null,null,null,null,null,null,null,null,null,"MSP430FR5964","MSP430F5437A","MSP430F5335","MSP430F5338","MSP430FR59941"]

{"sheet":"MSP Database","index":2,"n_rows":582,"n_cols":39,"rows_kept":582,"cut":false,"hidden":true,"merged":[]}
["PN","Vendor&GPN","Vendor","CPU","CPUFreq/MHz","NVM/kB","EEPROM/kB","RAM/kB","ADC Resolution","ADC Channel #","DAC","COMP","IO count","LCD","I2C","SPI","I2S","USB","Timer","Other Timers","Tempmin","Tempmax","Vmin/V","Vmax/V","PIN count","Package","Price","USART","UART","Powersleep/uA","PowerAM/(uA/MHz)","Cap Touch","Crypto","TRNG","Status","Others","Description","OPA","Special Features"]
["MSP430F5659","TIMSP430F5659","TI","MSP430",25,512,0,64,12,12,2,12,74,"No",3,6,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.05,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F56xx Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6659","TIMSP430F6659","TI","MSP430",25,512,0,64,12,12,2,12,74,"Yes",3,6,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",5.68,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F66xx Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5658","TIMSP430F5658","TI","MSP430",25,384,0,32,12,12,2,12,74,"No",3,6,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.2699999999999996,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F56xx Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6658","TIMSP430F6658","TI","MSP430",25,384,0,32,12,12,2,12,74,"Yes",3,6,null,"Yes",4,null,-40,85,1.8,3.6,100,"LQFP|100",4.72,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F66x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5638","TIMSP430F5638","TI","MSP430",25,256,0,16,12,12,1,12,74,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",3.34,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F563x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6638","TIMSP430F6638","TI","MSP430",25,256,0,16,12,12,1,12,74,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.4000000000000004,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F6638 Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5632","TIMSP430F5632","TI","MSP430",25,256,0,16,"Slope",0,0,12,74,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",3.17,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F563x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5635","TIMSP430F5635","TI","MSP430",25,256,0,16,12,12,0,12,74,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",3.26,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F563x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6632","TIMSP430F6632","TI","MSP430",25,256,0,16,"Slope",0,0,12,74,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,100,"LQFP|100",4.1500000000000004,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F663x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6635","TIMSP430F6635","TI","MSP430",25,256,0,16,12,12,0,12,74,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.22,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F663x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5637","TIMSP430F5637","TI","MSP430",25,192,0,16,12,12,1,12,74,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,100,"LQFP|100",4.1500000000000004,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F563x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6637","TIMSP430F6637","TI","MSP430",25,192,0,16,12,12,1,12,74,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,100,"LQFP|100",3.48,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F663x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5631","TIMSP430F5631","TI","MSP430",25,192,0,16,"Slope",0,0,12,74,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,100,"LQFP|100",3.62,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F563x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5634","TIMSP430F5634","TI","MSP430",25,192,0,16,12,12,0,12,74,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,100,"LQFP|100",3.64,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F563x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6631","TIMSP430F6631","TI","MSP430",25,192,0,16,"Slope",0,0,12,74,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,100,"LQFP|100",3.75,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F663x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6634","TIMSP430F6634","TI","MSP430",25,192,0,16,12,12,0,12,74,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.0199999999999996,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F663x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5636","TIMSP430F5636","TI","MSP430",25,128,0,16,12,12,1,12,74,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,100,"LQFP|100",2.99,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F563x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6636","TIMSP430F6636","TI","MSP430",25,128,0,16,12,12,1,12,74,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",2.3199999999999998,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F663x Mixed Signal Microcontroller",0,"N/A"]
["MSP430FG6626","TIMSP430FG6626","TI","MSP430",25,128,0,8,16,10,1,12,73,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.41,null,2,null,null,0,null,null,"ACTIVE",null,"25MHz MCU with integrated dual Op Amps, 12bit DACs, 16bit SigmaDelta ADC, USB, LCD, 128KB flash",2,"N/A"]
["MSP430F5519","TIMSP430F5519","TI","MSP430",25,128,0,8,"Slope",0,0,12,63,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"LQFP|80",2.82,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 128KB Flash, 8KB RAM, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5528","TIMSP430F5528","TI","MSP430",25,128,0,8,12,10,0,8,47,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, DSBGA|64, VQFN|64",2.95,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 128KB Flash, 8KB RAM, 12Bit/10 Channel ADC, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5529","TIMSP430F5529","TI","MSP430",25,128,0,8,12,14,0,12,63,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"LQFP|80",2.99,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 128KB Flash, 8KB RAM, 12Bit/14 Channel ADC, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5630","TIMSP430F5630","TI","MSP430",25,128,0,16,"Slope",0,0,12,74,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",2.71,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F563x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5633","TIMSP430F5633","TI","MSP430",25,128,0,16,12,12,0,12,74,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",2.5299999999999998,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F563x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6630","TIMSP430F6630","TI","MSP430",25,128,0,16,"Slope",0,0,12,74,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,100,"LQFP|100",3.17,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F663x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6633","TIMSP430F6633","TI","MSP430",25,128,0,16,12,12,0,12,74,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",3.8,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F663x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5517","TIMSP430F5517","TI","MSP430",25,96,0,6,"Slope",0,0,12,63,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"LQFP|80",2.97,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 96KB Flash, 6KB RAM, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5526","TIMSP430F5526","TI","MSP430",25,96,0,6,12,10,0,8,47,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",2.82,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 96KB Flash, 6KB RAM, 12Bit/10 Channel ADC, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5527","TIMSP430F5527","TI","MSP430",25,96,0,6,12,14,0,12,63,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"LQFP|80",2.86,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 96KB Flash, 6KB RAM, 12Bit/14 Channel ADC, 32BIT HW Multiplier",0,"N/A"]
["MSP430FG6625","TIMSP430FG6625","TI","MSP430",25,64,0,8,16,10,1,12,73,"Yes",2,4,null,"Yes",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",2.42,null,2,null,null,0,null,null,"ACTIVE",null,"25MHz MCU with integrated dual Op Amps, 12bit DACs, 16bit SigmaDelta ADC, USB, LCD, 64KB flash",2,"N/A"]
["MSP430F5514","TIMSP430F5514","TI","MSP430",25,64,0,4,"Slope",0,0,8,47,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",2.5499999999999998,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 64KB Flash, 4KB RAM, 12Bit/14 Channel ADC, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5515","TIMSP430F5515","TI","MSP430",25,64,0,4,"Slope",0,0,12,63,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"LQFP|80",1.7,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 64KB Flash, 4KB RAM, 12Bit/14 Channel ADC, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5524","TIMSP430F5524","TI","MSP430",25,64,0,4,12,10,0,8,47,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",2.68,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 64KB Flash, 4KB RAM, 12Bit/10 Channel ADC, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5525","TIMSP430F5525","TI","MSP430",25,64,0,4,12,14,0,12,63,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"LQFP|80",2.73,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 64KB Flash, 4KB RAM, 12Bit/14 Channel ADC, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5503","TIMSP430F5503","TI","MSP430",25,32,0,4,"Slope",0,0,4,31,"No",1,2,null,"Yes",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.42,null,1,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5507","TIMSP430F5507","TI","MSP430",25,32,0,4,10,6,0,0,31,"No",1,2,null,"Yes",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.46,null,1,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5510","TIMSP430F5510","TI","MSP430",25,32,0,4,10,10,0,8,47,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,48,"LQFP|48, VQFN|48, VQFN|64",1.5,null,2,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5513","TIMSP430F5513","TI","MSP430",25,32,0,4,"Slope",0,0,8,47,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",1.3,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 32KB Flash, 4KB RAM, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5521","TIMSP430F5521","TI","MSP430",25,32,0,6,12,14,0,12,63,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"LQFP|80",2.46,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 32KB Flash, 6KB RAM, 12Bit/14 Channel ADC, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5522","TIMSP430F5522","TI","MSP430",25,32,0,8,12,10,0,8,47,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",2.5099999999999998,null,2,null,null,0,null,null,"ACTIVE",null,"25 MHz MCU with Integrated USB Phy, 32KB Flash, 8KB RAM, 12Bit/10 Channel ADC, 32BIT HW Multiplier",0,"N/A"]
["MSP430F5502","TIMSP430F5502","TI","MSP430",25,24,0,4,"Slope",0,0,4,31,"No",1,2,null,"Yes",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.33,null,1,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5506","TIMSP430F5506","TI","MSP430",25,24,0,4,10,6,0,0,31,"No",1,2,null,"Yes",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.37,null,1,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5509","TIMSP430F5509","TI","MSP430",25,24,0,4,10,10,0,8,47,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, LQFP|48, VQFN|48, VQFN|64",1.42,null,2,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5501","TIMSP430F5501","TI","MSP430",25,16,0,4,"Slope",0,0,4,31,"No",1,2,null,"Yes",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.24,null,1,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5505","TIMSP430F5505","TI","MSP430",25,16,0,4,10,6,0,0,31,"No",1,2,null,"Yes",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.2,null,1,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5508","TIMSP430F5508","TI","MSP430",25,16,0,4,10,10,0,8,47,"No",2,4,null,"Yes",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, LQFP|48, VQFN|48, VQFN|64",1.28,null,2,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5500","TIMSP430F5500","TI","MSP430",25,8,0,4,"Slope",0,0,4,31,"No",1,2,null,"Yes",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.1499999999999999,null,1,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5504","TIMSP430F5504","TI","MSP430",25,8,0,4,10,6,0,0,31,"No",1,2,null,"Yes",4,null,-40,85,1.8,3.6,48,"LQFP|48, VQFN|48",1.5,null,1,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller",0,"N/A"]
["MSP432E401Y","TIMSP432E401Y","TI","ARM CM4F",120,1024,0,256,12,20,0,3,90,"No",10,4,null,"Yes",8,null,-40,105,2.97,3.63,128,"TQFP|128",null,null,8,642,454,null,null,null,null,null,"SimpleLink™ ethernet microcontroller",0,{"$error":"#N/A"}]
["MSP432E411Y","TIMSP432E411Y","TI","ARM CM4F",120,1024,0,256,12,24,0,3,140,"Yes",10,4,null,"Yes",8,null,-40,105,2.97,3.63,212,"NFBGA|212",null,null,8,642,454,null,null,null,null,null,"SimpleLink Ethernet Microcontroller",0,{"$error":"#N/A"}]
["MSP430L092","TIMSP430F5358","TI","MSP430",25,384,0,34,12,12,2,12,74,"No",3,6,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.62,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F53xx Mixed Signal Microcontroller",0,"N/A"]
["MSP430FR2310","TIMSP430F5359","TI","MSP430",25,512,0,66,12,12,2,12,74,"No",3,6,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.4000000000000004,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F53xx Mixed Signal Microcontroller",0,"N/A"]
["MSP430FR2311","TIMSP430F6458","TI","MSP430",25,384,0,34,12,12,2,12,74,"Yes",3,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100",5.3,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F64xx Mixed Signal Microcontroller",0,"N/A"]
["MSP430F412","TIMSP430F6459","TI","MSP430",25,512,0,66,12,12,2,12,74,"Yes",3,6,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.75,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F64xx Mixed Signal Microcontroller",0,"N/A"]
["MSP430FR4131","TIMSP430F4250","TI","MSP430",16,16,0,0.25,16,5,1,0,32,"Yes",0,0,null,"No",1,null,-40,85,1.8,3.6,48,"SSOP|48, VQFN|48",2.68,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 16kB Flash, 256B RAM, 16bit SigmaDelta A/D, 12bit D/A, LCD Driver",0,"N/A"]
["MSP430F4260","TIMSP430F4260","TI","MSP430",16,24,0,0.25,16,5,1,0,32,"Yes",0,0,null,"No",1,null,-40,85,1.8,3.6,48,"SSOP|48, VQFN|48",2.99,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 24kB Flash, 256B RAM, 16bit SigmaDelta A/D, 12bit D/A, LCD Driver",0,"N/A"]
["MSP430F4270","TIMSP430F4270","TI","MSP430",16,32,0,0.25,16,5,1,0,32,"Yes",0,0,null,"No",1,null,-40,85,1.8,3.6,48,"SSOP|48, VQFN|48",3.21,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 32kB Flash, 256B RAM, 16bit sigma Delta A/D, 12bit D/A, LCD Driver",0,"N/A"]
["MSP430F477","TIMSP430F477","TI","MSP430",16,32,0,2,16,5,1,2,48,"Yes",1,2,null,"No",2,null,-40,85,1.8,3.6,80,"LQFP|80",4.05,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 32KB Flash, 2KB RAM, 16bit SigmaDelta A/D, 12bit D/A, 128Seg LCD",0,"N/A"]
["MSP430F478","TIMSP430F478","TI","MSP430",16,48,0,2,16,5,1,2,48,"Yes",1,2,null,"No",2,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|80",4.4000000000000004,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 48KB Flash, 2KB RAM, 16bit SigmaDelta A/D, 12bit D/A, 128Seg LCD",0,"N/A"]
["MSP430F479","TIMSP430F479","TI","MSP430",16,60,0,2,16,5,1,2,48,"Yes",1,2,null,"No",2,null,-40,85,1.8,3.6,80,"LQFP|80",4.71,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 32KB Flash, 2KB RAM, 16bit SigmaDelta ADC, 12bit DAC, 128Seg LCD",0,"N/A"]
["MSP430F2619S-HT","TIMSP430F2619SHT","TI","MSP430",16,120,0,4,12,8,1,8,48,"No",2,4,null,"No",2,null,-55,150,1.8,3.6,64,"LQFP|64",70.900000000000006,null,2,null,null,0,null,null,"ACTIVE",null,"High Temp 16Bit UltraLowPower MCU, 120KB Flash, 4KB RAM, 12Bit ADC, Dual DAC, 2 USCI,HW Mult,DMA",0,"N/A"]
["MSP430L092","TIMSP430L092","TI","MSP430",16,0,0,2,8,4,1,2,11,"No",0,0,null,"No",2,null,0,50,null,null,14,"TSSOP|14",0.75,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430L092 Mixed Signal Microcontroller",0,"N/A"]
["MSP430F155","TIMSP430F155","TI","MSP430",16,16,0,0.5,12,8,1,2,48,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",4.83,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower MCU, 16kB Flash, 512B RAM, 12Bit ADC, Dual 12Bit DAC, USART, I2C, DMA",0,"N/A"]
["MSP430F156","TIMSP430F156","TI","MSP430",16,24,0,1,12,8,1,2,48,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",5.04,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower MCU, 24kB Flash, 1024B RAM, 12Bit ADC, Dual 12Bit DAC, USART, I2C, DMA",0,"N/A"]
["MSP430F157","TIMSP430F157","TI","MSP430",16,32,0,1,12,8,1,2,48,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",5.34,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower MCU, 32kB Flash, 1024B RAM, 12Bit ADC, Dual 12Bit DAC, USART, I2C, DMA",0,"N/A"]
["MSP430F1610","TIMSP430F1610","TI","MSP430",16,32,0,5,12,8,1,2,48,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",7.83,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower MCU, 32kB Flash, 5124B RAM, 12Bit ADC, Dual DAC, 2 USART, I2C, HW Mult, DMA",0,"N/A"]
["MSP430F167","TIMSP430F167","TI","MSP430",16,32,0,1,12,8,1,2,48,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",6.18,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower MCU, 32kB Flash, 1024B RAM, 12Bit ADC, Dual DAC, 2 USART, I2C, HW Mult, DMA",0,"N/A"]
["MSP430F1611","TIMSP430F1611","TI","MSP430",16,48,0,10,12,8,1,2,48,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",8.2200000000000006,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower MCU, 48kB Flash, 10240B RAM, 12Bit ADC, Dual DAC, 2 USART, I2C, HW Mult, DMA",0,"N/A"]
["MSP430F168","TIMSP430F168","TI","MSP430",16,48,0,2,12,8,1,2,48,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",6.83,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower MCU, 48kB Flash, 2048B RAM, 12Bit ADC, Dual DAC, 2 USART, I2C, HW Mult, DMA",0,"N/A"]
["MSP430F1612","TIMSP430F1612","TI","MSP430",16,55,0,5,12,8,1,2,48,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",8.5299999999999994,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower MCU, 55kB Flash, 5120B RAM, 12Bit ADC, Dual DAC, 2 USART, I2C, HW Mult, DMA",0,"N/A"]
["MSP430F169","TIMSP430F169","TI","MSP430",16,60,0,2,12,8,1,2,48,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",7.32,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower MCU, 60kB Flash, 2048B RAM, 12Bit ADC, Dual DAC, 2 USART, I2C, HW Mult, DMA",0,"N/A"]
["MSP430F2616","TIMSP430F2616","TI","MSP430",16,92,0,4,12,8,1,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|64, LQFP|80",5.15,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 92KB Flash, 4KB RAM, 12Bit ADC, Dual DAC, 2 USCI, HW Mult, DMA",0,"N/A"]
["MSP430F2617","TIMSP430F2617","TI","MSP430",16,92,0,8,12,8,1,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|64, LQFP|80",5.32,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 92KB Flash, 8KB RAM, 12Bit ADC, Dual DAC, 2 USCI, HW Mult, DMA",0,"N/A"]
["MSP430F2618","TIMSP430F2618","TI","MSP430",16,116,0,8,12,8,1,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|64, LQFP|80",5.59,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 116kB Flash, 8KB RAM, 12Bit ADC, Dual DAC, 2 USCI, HW Mult, DMA",0,"N/A"]
["MSP430F2619","TIMSP430F2619","TI","MSP430",16,120,0,4,12,8,1,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|64, LQFP|80",5.85,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 120KB Flash, 4KB RAM, 12Bit ADC, Dual DAC, 2 USCI, HW Mult, DMA",0,"N/A"]
["MSP430F5336","TIMSP430F5336","TI","MSP430",25,128,0,18,12,12,1,12,74,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",3.04,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F533x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5338","TIMSP430F5338","TI","MSP430",25,256,0,18,12,12,1,12,74,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",3.04,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F533x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6436","TIMSP430F6436","TI","MSP430",25,128,0,18,12,12,1,12,74,"Yes",2,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100",3.7,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F643x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6438","TIMSP430F6438","TI","MSP430",25,256,0,18,12,12,1,12,74,"Yes",2,4,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.1399999999999997,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F643x Mixed Signal Microcontroller",0,"N/A"]
["MSP430FG437","TIMSP430FG437","TI","MSP430",25,32,0,1,12,12,1,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,80,"LQFP|80, NFBGA|113",3.4,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 32KB Flash, 1KB RAM, 12Bit ADC, Dual DAC, DMA, 3 OPAMP, 128 Seg LCD",3,"N/A"]
["MSP430FG438","TIMSP430FG438","TI","MSP430",25,48,0,2,12,12,1,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,80,"LQFP|80, NFBGA|113",3.96,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 48KB Flash, 2KB RAM, 12Bit ADC, Dual DAC, DMA, 3 OPAMP, 128 Seg LCD",3,"N/A"]
["MSP430FG439","TIMSP430FG439","TI","MSP430",25,60,0,2,12,12,1,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,80,"LQFP|80, NFBGA|113",4.62,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 60KB Flash, 2KB RAM, 12Bit ADC, Dual DAC, DMA, 3 OPAMP, 128 Seg LCD",3,"N/A"]
["MSP430FG4616","TIMSP430FG4616","TI","MSP430",25,92,0,4,12,12,1,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",6.56,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 92KB Flash, 4KB RAM, 12Bit ADC, Dual DAC, DMA, 3 OPAMP, 160 Seg LCD",3,"N/A"]
["MSP430FG4617","TIMSP430FG4617","TI","MSP430",25,92,0,8,12,12,1,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",7,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 92KB Flash, 8KB RAM, 12Bit ADC, Dual DAC, DMA, 3 OPAMP, 160 Seg LCD",3,"N/A"]
["MSP430FG4618","TIMSP430FG4618","TI","MSP430",25,116,0,8,12,12,1,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",7.35,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 116KB Flash, 8KB RAM, 12Bit ADC, Dual DAC, DMA, 3 OPAMP, 160 Seg LCD",3,"N/A"]
["MSP430FG4619","TIMSP430FG4619","TI","MSP430",25,120,0,4,12,12,1,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",7,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 120KB Flash, 4KB RAM, 12Bit ADC, Dual DAC, DMA, 3 OPAMP, 160 Seg LCD",3,"N/A"]
["MSP430FG4250","TIMSP430FG4250","TI","MSP430",25,16,0,0.25,16,5,1,0,32,"Yes",0,0,null,"No",1,null,-40,85,1.8,3.6,48,"SSOP|48, VQFN|48",2.9,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 16kB Flash, 256B RAM, 16bit SigmaDelta A/D, 12bit D/A, 2 OPAMP, LCD",2,"N/A"]
["MSP430FG4260","TIMSP430FG4260","TI","MSP430",25,24,0,0.25,16,5,1,0,32,"Yes",0,0,null,"No",1,null,-40,85,1.8,3.6,48,"SSOP|48, VQFN|48",3.17,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 24kB Flash, 256B RAM, 16bit SigmaDelta A/D, 12bit D/A, 2 OPAMP, LCD",2,"N/A"]
["MSP430FG4270","TIMSP430FG4270","TI","MSP430",25,32,0,0.25,16,5,1,0,32,"Yes",0,0,null,"No",1,null,-40,85,1.8,3.6,48,"SSOP|48, VQFN|48",3.52,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 32kB Flash, 256B RAM, 16bit sigma Delta A/D, 12bit D/A, 2 OPAMP, LCD",2,"N/A"]
["MSP430FG477","TIMSP430FG477","TI","MSP430",25,32,0,2,16,1,1,2,48,"Yes",1,2,null,"No",2,null,-40,85,1.8,3.6,80,"LQFP|80",4.18,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 32KB Flash, 2KB RAM, 16bit SigmaDelta ADC, 12bit DAC, OpAmp, 128Seg LCD",2,"N/A"]
["MSP430FG478","TIMSP430FG478","TI","MSP430",25,48,0,2,16,1,1,2,48,"Yes",1,2,null,"No",2,null,-40,85,1.8,3.6,80,"LQFP|80",4.88,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 48KB Flash, 2KB RAM, 16bit SigmaDelta ADC, 12bit DAC, OpAmp, 128Seg LCD",2,"N/A"]
["MSP430FG479","TIMSP430FG479","TI","MSP430",25,60,0,2,16,1,1,2,48,"Yes",1,2,null,"No",2,null,-40,85,1.8,3.6,80,"LQFP|80",5.46,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 60KB Flash, 2KB RAM, 16bit SigmaDelta ADC, 12bit DAC, OpAmp, 128Seg LCD",2,"N/A"]
["MSP430FG6425","TIMSP430FG6425","TI","MSP430",25,64,0,10,16,10,1,12,73,"Yes",2,4,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",2.2799999999999998,null,2,null,null,0,null,null,"ACTIVE",null,"25MHz MCU with integrated dual Op Amps, 12bit DACs, 16bit SigmaDelta ADC,  LCD, 64KB flash",2,"N/A"]
["MSP430FG6426","TIMSP430FG6426","TI","MSP430",25,128,0,10,16,10,1,12,73,"Yes",2,4,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.13,null,2,null,null,0,null,null,"ACTIVE",null,"25MHz MCU with integrated dual Op Amps, 12bit DACs, 16bit SigmaDelta ADC,  LCD, 128KB flash",2,"N/A"]
["MSP430FR2310","TIMSP430FR2310","TI","MSP430",16,2,0,1,10,8,1,2,16,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,16,"TSSOP|16, TSSOP|20, VQFN|16",0.39,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller  2 KB FRAM, 1 KB SRAM, 16 IO, 8ch 10bit ADC, OpAmp, TIA",1,"N/A"]
["MSP430FR2311","TIMSP430FR2311","TI","MSP430",16,4,0,1,10,8,1,2,16,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,16,"TSSOP|16, TSSOP|20, VQFN|16",0.41,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller  4 KB FRAM, 1 KB SRAM, 16 IO, 8ch 10bit ADC, OpAmp, TIA",1,"N/A"]
["MSP430FR2353","TIMSP430FR2353","TI","MSP430",16,16,0,2,12,12,1,2,44,"No",2,4,null,"No",4,null,-40,105,1.8,3.6,48,"LQFP|48, TSSOP|38, VQFN|32, VQFN|40",0.77,null,2,null,null,0,null,null,"ACTIVE",null,"24MHz 105C ULP Microcontroller With 16 KB FRAM, 2 KB SRAM, 44 IO, 12bit ADC, 12bit DACs, OpAmp/PGA",1,"N/A"]
["MSP430FR2355","TIMSP430FR2355","TI","MSP430",16,32,0,4,12,12,1,2,44,"No",2,4,null,"No",4,null,-40,105,1.8,3.6,48,"LQFP|48, TSSOP|38, VQFN|32, VQFN|40",0.85,null,2,null,null,0,null,null,"ACTIVE",null,"24MHz 105C ULP Microcontroller With 32 KB FRAM, 4 KB SRAM, 44 IO, 12bit ADC, 12bit DACs, OpAmp/PGA",1,"N/A"]
["MSP430FR6888","TIMSP430FR6888","TI","MSP430",16,96,0,2,12,16,0,16,83,"No",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",3.07,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6888 16 MHz ULP Microcontroller featuring 96 KB FRAM, 2 KB SRAM, 83 IO, ADC, LCD, Scan IF",0,"Scan Interface"]
["MSP430FR6928","TIMSP430FR6928","TI","MSP430",16,96,0,2,12,8,0,12,52,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64",2.54,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6928 16 MHz ULP Microcontroller featuring 96 KB FRAM, 2 KB SRAM, 52 IO, 8 ch ADC12, LCD, AES",0,"N/A"]
["MSP430FR6988","TIMSP430FR6988","TI","MSP430",16,96,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.56,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6988 16 MHz UltraLowPower Microcontroller featuring 96 KB FRAM, ULP ADC12, LCD, AES, ESI",0,"Scan Interface"]
["MSP430F412","TIMSP430F412","TI","MSP430",16,4,0,0.25,"Slope",0,0,2,48,"Yes",0,0,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.1399999999999999,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 4kB Flash, 256B RAM, Comparator, 96 segment LCD",0,"N/A"]
["MSP430FR4131","TIMSP430FR4131","TI","MSP430",16,4,0,0.5,10,10,0,0,60,"Yes",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|48, TSSOP|56",0.6,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller with 4 KB FRAM, .5 KB SRAM, 60 IO, 10bit ADC, LCD, IR Logic",0,"N/A"]
["MSP430F413","TIMSP430F413","TI","MSP430",16,8,0,0.25,"Slope",0,0,2,48,"Yes",0,0,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.19,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 8kB Flash, 256B RAM, Comparator, 96 segment LCD",0,"N/A"]
["MSP430F4132","TIMSP430F4132","TI","MSP430",16,8,0,0.5,10,8,0,2,56,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|48",1.32,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 8KB Flash, 512B RAM, 10bit ADC, USCI, Analog Comp, 56 I/Os, LCD Driv",0,"N/A"]
["MSP430F423A","TIMSP430F423A","TI","MSP430",16,8,0,0.25,16,3,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",1.8,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 8KB Flash, 256B RAM, SigmaDelta ADC, 128 Seg LCD",0,"N/A"]
["MSP430FR4132","TIMSP430FR4132","TI","MSP430",16,8,0,1,10,10,0,0,60,"Yes",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|48, TSSOP|56",0.66,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller with 8 KB FRAM, 1 KB SRAM, 60 IO, 10bit ADC, LCD, IR Logic",0,"N/A"]
["CC430F6135","TICC430F6135","TI","MSP430",16,16,0,2,"ADC12","  ",0,"  ","  ","Yes",1,1,null,"No",2,null,-40,85,null,null,64,"VQFN|64",1.56,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 16KB Flash, 2KB RAM, CC1101 Radio, AES128, 12Bit ADC, USCI, LCD driver",0,"N/A"]
["MSP430F415","TIMSP430F415","TI","MSP430",16,16,0,0.5,"Slope",0,0,2,48,"Yes",0,0,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.32,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 16kB Flash, 512B RAM, Comparator, 96 Segment LCD",0,"N/A"]
["MSP430F4152","TIMSP430F4152","TI","MSP430",16,16,0,0.5,10,8,0,2,56,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|48",1.5,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 16KB Flash, 512B RAM, 10bit ADC, USCI, Analog Comp, 56 I/Os, LCD Driver",0,"N/A"]
["MSP430F425A","TIMSP430F425A","TI","MSP430",16,16,0,0.5,16,3,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",2.02,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 16KB Flash, 512B RAM, SigmaDelta ADC, 128 Seg LCD",0,"N/A"]
["MSP430F435","TIMSP430F435","TI","MSP430",16,16,0,0.5,12,8,0,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.99,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 16kB Flash, 512B RAM, 12Bit ADC, USART, 160 Segment LCD",0,"N/A"]
["MSP430F4351","TIMSP430F4351","TI","MSP430",16,16,0,0.5,"Slope",0,0,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.76,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 16kB Flash, 512B RAM, USART, 160 Segment LCD",0,"N/A"]
["MSP430F6720","TIMSP430F6720","TI","MSP430",25,16,0,1,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",1.79,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 16KB Flash, 1KB RAM",0,"N/A"]
["MSP430F6720A","TIMSP430F6720A","TI","MSP430",25,16,0,1,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",1.79,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 16KB Flash, 1KB RAM",0,"N/A"]
["MSP430F6730","TIMSP430F6730","TI","MSP430",25,16,0,1,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",1.87,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 16KB Flash, 1KB RAM",0,"N/A"]
["MSP430F6730A","TIMSP430F6730A","TI","MSP430",25,16,0,1,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",1.79,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 16KB Flash, 1KB RAM",0,"N/A"]
["MSP430FR4133","TIMSP430FR4133","TI","MSP430",16,16,0,2,10,10,0,0,60,"Yes",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|48, TSSOP|56",0.79,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller with 16 KB FRAM, 2 KB SRAM, 60 IO, 10bit ADC, LCD, IR Logic",0,"N/A"]
["MSP430F436","TIMSP430F436","TI","MSP430",16,24,0,1,12,8,0,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",3.26,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 24kB Flash, 1024B RAM, 12Bit ADC, USART, 160 Segment LCD",0,"N/A"]
["MSP430F4361","TIMSP430F4361","TI","MSP430",16,24,0,1,"Slope",0,0,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",3.01,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 24kB Flash, 1024B RAM, USART, 160 Segment LCD",0,"N/A"]
["CC430F6127","TICC430F6127","TI","MSP430",16,32,0,4,"Slope","  ",0,"  ","  ","Yes",1,1,null,"No",2,null,-40,85,null,null,64,"VQFN|64",1.83,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 32KB Flash, 4KB RAM, CC1101 Radio, AES128, USCI, LCD Driver",0,"N/A"]
["MSP430F417","TIMSP430F417","TI","MSP430",16,32,0,1,"Slope",0,0,2,48,"Yes",0,0,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.73,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 32kB Flash, 1kB RAM, Comparator, 96 Segment LCD",0,"N/A"]
["MSP430F427A","TIMSP430F427A","TI","MSP430",16,32,0,1,16,3,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",2.2000000000000002,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 32KB Flash, 1KB RAM, SigmaDelta ADC, 128 Seg LCD",0,"N/A"]
["MSP430F437","TIMSP430F437","TI","MSP430",16,32,0,1,12,8,0,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",3.43,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 32kB Flash, 1024B RAM, 12Bit ADC, USART, 160 Segment LCD",0,"N/A"]
["MSP430F4371","TIMSP430F4371","TI","MSP430",16,32,0,1,"Slope",0,0,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",3.17,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 32kB Flash, 1024B RAM, USART, 160 Segment LCD",0,"N/A"]
["MSP430F447","TIMSP430F447","TI","MSP430",16,32,0,1,12,8,0,2,48,"Yes",0,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",3.82,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 32kB Flash, 1024B RAM, 12Bit ADC, 2 USARTs, HW Multiplier, 160 Seg LCD",0,"N/A"]
["MSP430F6721","TIMSP430F6721","TI","MSP430",25,32,0,2,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",1.85,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 32KB Flash, 2KB RAM",0,"N/A"]
["MSP430F6721A","TIMSP430F6721A","TI","MSP430",25,32,0,2,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.0499999999999998,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 32KB Flash, 2KB RAM",0,"N/A"]
["MSP430F6731","TIMSP430F6731","TI","MSP430",25,32,0,2,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,80,"LQFP|80",2.0499999999999998,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 32KB Flash, 2KB RAM",0,"N/A"]
["MSP430F6731A","TIMSP430F6731A","TI","MSP430",25,32,0,2,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,80,"LQFP|80",2.0499999999999998,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 32KB Flash, 2KB RAM",0,"N/A"]
["MSP430FR6820","TIMSP430FR6820","TI","MSP430",16,32,0,2,12,8,0,8,52,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|56, VQFN|64",1.78,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6820 16 MHz UltraLowPower MCU featuring 32 KB FRAM, 2 KB SRAM, 51 IO, ADC12, LCD",0,"N/A"]
["MSP430FR6870","TIMSP430FR6870","TI","MSP430",16,32,0,2,12,8,0,8,51,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.28,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6870 16 MHz UltraLowPower MCU featuring 32 KB FRAM, 2 KB SRAM, 51 IO, ADC12, LCD",0,"N/A"]
["MSP430FR6920","TIMSP430FR6920","TI","MSP430",16,32,0,2,12,8,0,8,52,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|56, VQFN|64",1.26,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6920 16 MHz UltraLowPower MCU featuring 32 KB FRAM, 2 KB SRAM, 52 IO, ADC12, LCD",0,"N/A"]
["MSP430FR6970","TIMSP430FR6970","TI","MSP430",16,32,0,2,12,8,0,8,51,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.28,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6970 16 MHz UltraLowPower MCU featuring 32 KB FRAM, 2 KB SRAM, 51 IO, ADC12, LCD",0,"N/A"]
["MSP430F448","TIMSP430F448","TI","MSP430",16,48,0,2,12,8,0,2,48,"Yes",0,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",3.83,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 48kB Flash, 2048B RAM, 12Bit ADC, 2 USARTs, HW Multiplier, 160 Seg LCD",0,"N/A"]
["MSP430F4481","TIMSP430F4481","TI","MSP430",16,48,0,2,"Slope",0,0,2,48,"Yes",0,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",3.56,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 48kB Flash, 2048B RAM, Comparator, 2 USARTs, HW Multiplier, 160 Seg LCD",0,"N/A"]
["MSP430F4783","TIMSP430F4783","TI","MSP430",16,48,0,2,16,3,0,2,72,"Yes",2,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",3.52,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 48KB Flash, 2KB RAM, 3 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F4784","TIMSP430F4784","TI","MSP430",16,48,0,2,16,4,0,2,72,"Yes",2,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",3.52,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 48KB Flash, 2KB RAM, 4 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F47126","TIMSP430F47126","TI","MSP430",16,56,0,4,16,6,0,2,72,"Yes",2,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.1900000000000004,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 56KB Flash, 4KB RAM, 6 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F47127","TIMSP430F47127","TI","MSP430",16,56,0,4,16,7,0,2,72,"Yes",2,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.4800000000000004,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 56KB Flash, 4KB RAM, 7 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F449","TIMSP430F449","TI","MSP430",16,60,0,2,12,8,0,2,48,"Yes",0,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.09,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 60kB Flash, 2048B RAM, 12Bit ADC, 2 USARTs HW Multiplier, 160 Seg LCD",0,"N/A"]
["MSP430F4491","TIMSP430F4491","TI","MSP430",16,60,0,2,"Slope",0,0,2,48,"Yes",0,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.0599999999999996,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 60kB Flash, 2048B RAM, Comparator, 2 USARTs, HW Multiplier, 160 Seg LCD",0,"N/A"]
["MSP430F4793","TIMSP430F4793","TI","MSP430",16,60,0,2.5,16,3,0,2,72,"Yes",2,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",3.78,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 60KB Flash, 2.5KB RAM, 3 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F4794","TIMSP430F4794","TI","MSP430",16,60,0,2.5,16,4,0,2,72,"Yes",2,2,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",3.78,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 60KB Flash, 2KB RAM, 4 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F6723","TIMSP430F6723","TI","MSP430",25,64,0,4,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.02,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 64KB Flash, 4KB RAM",0,"N/A"]
["MSP430F6723A","TIMSP430F6723A","TI","MSP430",25,64,0,4,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.35,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 64KB Flash, 4KB RAM",0,"N/A"]
["MSP430F6733","TIMSP430F6733","TI","MSP430",25,64,0,4,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.42,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 64KB Flash, 4KB RAM",0,"N/A"]
["MSP430F6733A","TIMSP430F6733A","TI","MSP430",25,64,0,4,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.42,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 64KB Flash, 4KB RAM",0,"N/A"]
["MSP430FR6822","TIMSP430FR6822","TI","MSP430",16,64,0,2,12,8,0,8,52,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|56, VQFN|64",1.64,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6822 16 MHz UltraLowPower MCU featuring 64 KB FRAM, 2 KB SRAM, 51 IO, ADC12, LCD",0,"N/A"]
["MSP430FR68221","TIMSP430FR68221","TI","MSP430",16,64,0,2,12,8,0,8,52,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|56, VQFN|64",1.64,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR68221 16 MHz UltraLowPower MCU featuring 64 KB FRAM, 2 KB SRAM, 51 IO, ADC12, LCD",0,"N/A"]
["MSP430FR6872","TIMSP430FR6872","TI","MSP430",16,64,0,2,12,8,0,8,51,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.66,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6872 16 MHz UltraLowPower MCU featuring 64 KB FRAM, 2 KB SRAM, 51 IO, ADC12, LCD",0,"N/A"]
["MSP430FR68721","TIMSP430FR68721","TI","MSP430",16,64,0,2,12,8,0,8,51,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.66,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR68721 16 MHz UltraLowPower MCU featuring 64 KB FRAM, 2 KB SRAM, 51 IO, ADC12, LCD",0,"N/A"]
["MSP430FR6877","TIMSP430FR6877","TI","MSP430",16,64,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.77,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6877 16 MHz ULP Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 83 IO, 16 ch ADC12, LCD",0,"N/A"]
["MSP430FR6887","TIMSP430FR6887","TI","MSP430",16,64,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.02,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6887 16 MHz ULP Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 83 IO, ADC12, LCD, Scan IF",0,"Scan Interface"]
["MSP430FR6922","TIMSP430FR6922","TI","MSP430",16,64,0,2,12,8,0,8,52,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|56, VQFN|64",1.95,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6922 16 MHz UltraLowPower MCU featuring 64 KB FRAM, 2 KB SRAM, 52 IO, ADC12, LCD, AES",0,"N/A"]
["MSP430FR69221","TIMSP430FR69221","TI","MSP430",16,64,0,2,12,8,0,8,52,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|56, VQFN|64",1.64,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR69221 16 MHz UltraLowPower MCU featuring 64 KB FRAM, 2 KB SRAM, 52 IO, ADC12, LCD, AES",0,"N/A"]
["MSP430FR6927","TIMSP430FR6927","TI","MSP430",16,64,0,2,12,8,0,12,52,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",2.57,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6927 16 MHz ULP Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 52 IO, 8 ch ADC12, LCD, AES",0,"N/A"]
["MSP430FR6972","TIMSP430FR6972","TI","MSP430",16,64,0,2,12,8,0,8,51,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.66,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6972 16 MHz UltraLowPower MCU featuring 64 KB FRAM, 2 KB SRAM, 51 IO, ADC12, LCD, AES",0,"N/A"]
["MSP430FR69721","TIMSP430FR69721","TI","MSP430",16,64,0,2,12,8,0,8,51,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",2.0499999999999998,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR69721 16 MHz UltraLowPower MCU featuring 64KB FRAM, 2KB SRAM, 51 IO, ADC12, LCD, AES",0,"N/A"]
["MSP430FR6977","TIMSP430FR6977","TI","MSP430",16,64,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.02,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6977 16 MHz ULP Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 83 IO, ADC12, LCD, AES",0,"N/A"]
["MSP430FR6987","TIMSP430FR6987","TI","MSP430",16,64,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.56,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6987 16 MHz ULP Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 83 IO, ADC12, LCD, AES, ESI",0,"Scan Interface"]
["MSP430F4616","TIMSP430F4616","TI","MSP430",16,92,0,4,12,12,0,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",5.54,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 92KB Flash, 4KB RAM, 12Bit ADC, DMA, 160 Seg LCD",0,"N/A"]
["MSP430F46161","TIMSP430F46161","TI","MSP430",16,92,0,4,"Slope",0,0,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.75,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 92KB Flash, 4KB RAM, Comparator, DMA, 160 Seg LCD",0,"N/A"]
["MSP430F4617","TIMSP430F4617","TI","MSP430",16,92,0,8,12,12,0,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",5.9,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 92KB Flash, 8KB RAM, 12Bit ADC, DMA, 160 Seg LCD",0,"N/A"]
["MSP430F46171","TIMSP430F46171","TI","MSP430",16,92,0,8,"Slope",0,0,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.7699999999999996,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 92KB Flash, 8KB RAM, Comparator, DMA, 160 Seg LCD",0,"N/A"]
["MSP430F47163","TIMSP430F47163","TI","MSP430",16,92,0,4,16,3,0,2,72,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.4800000000000004,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 92KB Flash, 4KB RAM, 3 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F47166","TIMSP430F47166","TI","MSP430",16,92,0,4,16,6,0,2,68,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.4800000000000004,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller,  92KB Flash, 4KB RAM, 6 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F47167","TIMSP430F47167","TI","MSP430",16,92,0,4,16,7,0,2,68,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.78,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller,  92KB Flash, 4KB RAM, 7 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F47173","TIMSP430F47173","TI","MSP430",16,92,0,8,16,3,0,2,72,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.93,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 92KB Flash, 8KB RAM, 3 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F47176","TIMSP430F47176","TI","MSP430",16,92,0,8,16,6,0,2,68,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.93,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller,  92KB Flash, 8KB RAM, 6 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F47177","TIMSP430F47177","TI","MSP430",16,92,0,8,16,7,0,2,68,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",5.25,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller,  92KB Flash, 8KB RAM, 7 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F6724","TIMSP430F6724","TI","MSP430",25,96,0,4,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.37,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 96KB Flash, 4KB RAM",0,"N/A"]
["MSP430F6724A","TIMSP430F6724A","TI","MSP430",25,96,0,4,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.37,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 96KB Flash, 4KB RAM",0,"N/A"]
["MSP430F6734","TIMSP430F6734","TI","MSP430",25,96,0,4,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.64,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 96KB Flash, 4KB RAM",0,"N/A"]
["MSP430F6734A","TIMSP430F6734A","TI","MSP430",25,96,0,4,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.37,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 96KB Flash, 4KB RAM",0,"N/A"]
["MSP430F4618","TIMSP430F4618","TI","MSP430",16,116,0,8,12,12,0,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",6.25,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 116KB Flash, 8KB RAM, 12Bit ADC, DMA, 160 Seg LCD",0,"N/A"]
["MSP430F46181","TIMSP430F46181","TI","MSP430",16,116,0,8,"Slope",0,0,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",5.46,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 116KB Flash, 8KB RAM, Comparator, DMA, 160 Seg LCD",0,"N/A"]
["MSP430F47183","TIMSP430F47183","TI","MSP430",16,116,0,8,16,3,0,2,72,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",5.23,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 116KB Flash, 8KB RAM, 3 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F47186","TIMSP430F47186","TI","MSP430",16,116,0,8,16,6,0,2,68,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",5.23,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller,  116KB Flash, 8KB RAM, 6 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F47187","TIMSP430F47187","TI","MSP430",16,116,0,8,16,7,0,2,68,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",5.57,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller,  116KB Flash, 8KB RAM, 7 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F4619","TIMSP430F4619","TI","MSP430",16,120,0,4,12,12,0,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",5.9,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 120KB Flash, 4KB RAM, 12Bit ADC, DMA, 160 Seg LCD",0,"N/A"]
["MSP430F46191","TIMSP430F46191","TI","MSP430",16,120,0,4,"Slope",0,0,2,80,"Yes",1,1,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",4.9800000000000004,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower MCU, 120KB Flash, 4KB RAM, Comparator, DMA, 160 Seg LCD",0,"N/A"]
["MSP430F47193","TIMSP430F47193","TI","MSP430",16,120,0,4,16,3,0,2,72,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",5.19,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 120KB Flash, 4KB RAM, 3 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F47196","TIMSP430F47196","TI","MSP430",16,120,0,4,16,6,0,2,68,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",3.36,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller,  120KB Flash, 4KB RAM, 6 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F47197","TIMSP430F47197","TI","MSP430",16,120,0,4,16,7,0,2,68,"Yes",2,4,null,"No",2,null,-40,85,1.8,3.6,100,"LQFP|100",5.53,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller,  120KB Flash, 4KB RAM, 7 SigmaDelta ADCs, LCD Driver",0,"N/A"]
["MSP430F6725","TIMSP430F6725","TI","MSP430",25,128,0,4,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.37,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 4KB RAM",0,"N/A"]
["MSP430F6725A","TIMSP430F6725A","TI","MSP430",25,128,0,4,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.37,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 4KB RAM",0,"N/A"]
["MSP430F6726","TIMSP430F6726","TI","MSP430",25,128,0,8,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.38,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 8KB RAM",0,"N/A"]
["MSP430F6726A","TIMSP430F6726A","TI","MSP430",25,128,0,8,24,2,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.38,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 2 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 8KB RAM",0,"N/A"]
["MSP430F6735","TIMSP430F6735","TI","MSP430",25,128,0,4,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.84,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 4KB RAM",0,"N/A"]
["MSP430F6735A","TIMSP430F6735A","TI","MSP430",25,128,0,4,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.37,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 4KB RAM",0,"N/A"]
["MSP430F6736","TIMSP430F6736","TI","MSP430",25,128,0,8,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.86,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 8KB RAM",0,"N/A"]
["MSP430F6736A","TIMSP430F6736A","TI","MSP430",25,128,0,8,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.9,null,3,null,null,0,null,null,"ACTIVE",null,"Singlephase Metering SoC with 3 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 8KB RAM",0,"N/A"]
["MSP430F6745","TIMSP430F6745","TI","MSP430",25,128,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.31,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, AES, 128KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67451","TIMSP430F67451","TI","MSP430",25,128,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.4,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67451A","TIMSP430F67451A","TI","MSP430",25,128,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",2.76,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6745A","TIMSP430F6745A","TI","MSP430",25,128,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.63,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, AES, 128KB Flash, 1KB RAM",0,"N/A"]
["MSP430F6765","TIMSP430F6765","TI","MSP430",25,128,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",2.76,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, AES, 128KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67651","TIMSP430F67651","TI","MSP430",25,128,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",2.76,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67651A","TIMSP430F67651A","TI","MSP430",25,128,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.6,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6765A","TIMSP430F6765A","TI","MSP430",25,128,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",2.76,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, AES, 128KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6775","TIMSP430F6775","TI","MSP430",25,128,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",2.76,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, AES, 128KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67751","TIMSP430F67751","TI","MSP430",25,128,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.8,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67751A","TIMSP430F67751A","TI","MSP430",25,128,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.8,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, 128KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6775A","TIMSP430F6775A","TI","MSP430",25,128,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",2.76,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, AES, 128KB Flash, 16KB RAM",0,"N/A"]
["MSP430FR6879","TIMSP430FR6879","TI","MSP430",16,128,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.9,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6879 16 MHz ULP Microcontroller featuring 128 KB FRAM, 2 KB SRAM, 83 IO, 16 ch ADC12, LCD",0,"N/A"]
["MSP430FR68791","TIMSP430FR68791","TI","MSP430",16,128,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",3,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR68791 16 MHz ULP Microcontroller featuring 128 KB FRAM, 2 KB SRAM, 83 IO, 16 ch ADC12, LCD",0,"N/A"]
["MSP430FR6889","TIMSP430FR6889","TI","MSP430",16,128,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.9,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6889 16 MHz ULP Microcontroller featuring 128 KB FRAM, 2 KB SRAM, 83 IO, ADC12, LCD, Scan IF",0,"Scan Interface"]
["MSP430FR6979","TIMSP430FR6979","TI","MSP430",16,128,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.95,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6979 16 MHz ULP Microcontroller featuring 128 KB FRAM, 2 KB SRAM, 83 IO, ADC12, LCD, AES",0,"N/A"]
["MSP430FR69791","TIMSP430FR69791","TI","MSP430",16,128,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.25,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR69791 16 MHz UPLP Microcontroller featuring 128 KB FRAM, 2 KB SRAM, 83 IO, ADC12, LCD, AES",0,"N/A"]
["MSP430FR6989","TIMSP430FR6989","TI","MSP430",16,128,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",3.3,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR6989 16 MHz ULP Microcontroller  128 KB FRAM, 2KB SRAM, 83 IO, ADC12, LCD, AES, Scan IF",0,"Scan Interface"]
["MSP430FR69891","TIMSP430FR69891","TI","MSP430",16,128,0,2,12,16,0,16,83,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",3.43,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR69891 16 MHz ULP Microcontroller featuring 128 KB FRAM, 2 KB SRAM, 83 IO, ADC12, LCD, AES",0,"Scan Interface"]
["MSP430F6746","TIMSP430F6746","TI","MSP430",25,256,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.86,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67461","TIMSP430F67461","TI","MSP430",25,256,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.86,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67461A","TIMSP430F67461A","TI","MSP430",25,256,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.1100000000000003,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6746A","TIMSP430F6746A","TI","MSP430",25,256,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6747","TIMSP430F6747","TI","MSP430",25,256,0,32,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67471","TIMSP430F67471","TI","MSP430",25,256,0,32,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67471A","TIMSP430F67471A","TI","MSP430",25,256,0,32,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 32KB RAM",0,"N/A"]
["MSP430F6747A","TIMSP430F6747A","TI","MSP430",25,256,0,32,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 32KB RAM",0,"N/A"]
["MSP430F6766","TIMSP430F6766","TI","MSP430",25,256,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.86,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67661","TIMSP430F67661","TI","MSP430",25,256,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.86,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67661A","TIMSP430F67661A","TI","MSP430",25,256,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6766A","TIMSP430F6766A","TI","MSP430",25,256,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6767","TIMSP430F6767","TI","MSP430",25,256,0,32,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.86,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67671","TIMSP430F67671","TI","MSP430",25,256,0,32,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.86,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67671A","TIMSP430F67671A","TI","MSP430",25,256,0,32,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 32KB RAM",0,"N/A"]
["MSP430F6776","TIMSP430F6776","TI","MSP430",25,256,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.63,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67761","TIMSP430F67761","TI","MSP430",25,256,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.86,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67761A","TIMSP430F67761A","TI","MSP430",25,256,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6776A","TIMSP430F6776A","TI","MSP430",25,256,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.76,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6777","TIMSP430F6777","TI","MSP430",25,256,0,32,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67771","TIMSP430F67771","TI","MSP430",25,256,0,32,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.63,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67771A","TIMSP430F67771A","TI","MSP430",25,256,0,32,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, 256KB Flash, 32KB RAM",0,"N/A"]
["MSP430F6777A","TIMSP430F6777A","TI","MSP430",25,256,0,32,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, AES, 256KB Flash, 32KB RAM",0,"N/A"]
["MSP430F6748","TIMSP430F6748","TI","MSP430",25,512,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.77,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67481","TIMSP430F67481","TI","MSP430",25,512,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.77,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67481A","TIMSP430F67481A","TI","MSP430",25,512,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.8099999999999996,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6748A","TIMSP430F6748A","TI","MSP430",25,512,0,16,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.37,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6749","TIMSP430F6749","TI","MSP430",25,512,0,32,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.77,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67491","TIMSP430F67491","TI","MSP430",25,512,0,32,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.77,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67491A","TIMSP430F67491A","TI","MSP430",25,512,0,32,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.8099999999999996,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F6749A","TIMSP430F6749A","TI","MSP430",25,512,0,32,24,4,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.8099999999999996,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 4 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F6768","TIMSP430F6768","TI","MSP430",25,512,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.77,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67681","TIMSP430F67681","TI","MSP430",25,512,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.4,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67681A","TIMSP430F67681A","TI","MSP430",25,512,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.8099999999999996,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6768A","TIMSP430F6768A","TI","MSP430",25,512,0,16,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.8099999999999996,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6769","TIMSP430F6769","TI","MSP430",25,512,0,32,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.77,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67691","TIMSP430F67691","TI","MSP430",25,512,0,32,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.51,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67691A","TIMSP430F67691A","TI","MSP430",25,512,0,32,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.8099999999999996,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F6769A","TIMSP430F6769A","TI","MSP430",25,512,0,32,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.8099999999999996,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 6 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F6778","TIMSP430F6778","TI","MSP430",25,512,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.84,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67781","TIMSP430F67781","TI","MSP430",25,512,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.77,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F67781A","TIMSP430F67781A","TI","MSP430",25,512,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.8099999999999996,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6778A","TIMSP430F6778A","TI","MSP430",25,512,0,16,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",4.8099999999999996,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 16KB RAM",0,"N/A"]
["MSP430F6779","TIMSP430F6779","TI","MSP430",25,512,0,32,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.95,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67791","TIMSP430F67791","TI","MSP430",25,512,0,32,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.71,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F67791A","TIMSP430F67791A","TI","MSP430",25,512,0,32,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.71,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F6779A","TIMSP430F6779A","TI","MSP430",25,512,0,32,24,7,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",5.95,null,4,null,null,0,null,null,"ACTIVE",null,"Polyphase Metering SoC with 7 SigmaDelta ADCs, LCD, RealTime Clock, AES, 512KB Flash, 32KB RAM",0,"N/A"]
["MSP430F2013-EP","TIMSP430F2013EP","TI","MSP430",16,2,0,0.125,16,4,0,0,10,"No",1,1,null,"No",1,null,-40,125,1.8,3.6,16,"QFN|16",3.08,null,0,null,null,0,null,null,"ACTIVE",null,"Enhanced Product 16bit UltraLowPower Microcontroller, 2kB Flash, 128B RAM, 16Bit SigmaDelta A/D",0,"N/A"]
["MSP430G2230-EP","TIMSP430G2230EP","TI","MSP430",16,2,0,0.125,10,4,0,0,4,"No",1,1,null,"No",1,null,-40,125,1.8,3.6,8,"SOIC|8",1.27,null,0,null,null,0,null,null,"ACTIVE",null,"Enhanced Product 16bit UltraLowPower Mixed Signal Microcontroller, 2kB Flash, 128B RAM",0,"N/A"]
["MSP430G2231-EP","TIMSP430G2231EP","TI","MSP430",16,2,0,0.125,10,8,0,0,10,"No",1,1,null,"No",1,null,-40,125,1.8,3.6,14,"TSSOP|14",1.58,null,0,null,null,0,null,null,"ACTIVE",null,"Enhanced Product 16bit UltraLowPower Mixed Signal Microcontroller, 2kB Flash, 128B RAM",0,"N/A"]
["MSP430G2302-EP","TIMSP430G2302EP","TI","MSP430",16,4,0,0.25,"N/A",0,0,0,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,14,"TSSOP|14",1.58,null,0,null,null,0,null,null,"ACTIVE",null,"Enhanced Product Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2332-EP","TIMSP430G2332EP","TI","MSP430",16,4,0,0.25,10,8,0,0,16,"No",1,1,null,"No",1,null,-40,125,1.8,3.6,20,"TSSOP|20",1.78,null,0,null,null,0,null,null,"ACTIVE",null,"Enhanced Product Mixed Signal Microcontroller",0,"N/A"]
["MSP430F2132-EP","TIMSP430F2132EP","TI","MSP430",16,8,0,0.5,10,8,0,8,24,"No",1,2,null,"No",2,null,-40,125,1.8,3.6,32,"VQFN|32",3.7,null,1,null,null,0,null,null,"ACTIVE",null,"Enhanced Product 16bit UltraLowPower Microcontroller, 8kB Flash, 512B RAM, 10 bit ADC, 1 USCI",0,"N/A"]
["MSP430FR5739-EP","TIMSP430FR5739EP","TI","MSP430",16,16,0,1,10,12,0,"  ",32,"No",1,3,null,"No",5,null,-55,85,1.8,3.6,40,"VQFN|40",3.4,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5739 24 MHz ULP microcontroller with 16 KB FRAM, 1 KB SRAM,  32 IO, 10bit ADC & comparator",0,"N/A"]
["MSP430F249-EP","TIMSP430F249EP","TI","MSP430",16,60,0,2,12,8,0,8,48,"No",4,2,null,"No",2,null,-55,125,1.8,3.6,64,"LQFP|64",8.36,null,2,null,null,0,null,null,"ACTIVE",null,"Enhanced Product 16bit UltraLowPower Microcontroller, 60KB Flash, 2KB RAM, 12Bit ADC, 2 USCIs,",0,"N/A"]
["MSP430FR5969-SP","TIMSP430FR5969SP","TI","MSP430",16,64,0,2,12,16,0,16,40,"No",1,3,null,"No",5,null,-55,105,1.8,3.6,48,"HTQFP|48, VQFN|48",1.76,null,2,null,null,0,null,null,"ACTIVE",null,"Radiation Hardened MixedSignal Microcontroller",0,"N/A"]
["MSP430F5328-EP","TIMSP430F5328EP","TI","MSP430",25,128,0,10,12,10,0,8,47,"No",2,2,null,"No",4,null,-40,105,1.8,3.6,64,"VQFN|64",5.7,null,2,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller, MSP430F5328EP",0,"N/A"]
["MSP430FR5989-EP","TIMSP430FR5989EP","TI","MSP430",16,128,0,2,12,12,0,"  ",48,"No",2,4,null,"No",5,null,-55,95,1.8,3.6,64,"VQFN|64",3.04,null,2,null,null,0,null,null,"ACTIVE",null,"16 MHz ULP Microcontroller Featuring 128 KB FRAM, 2 KB SRAM, 48 IO, ADC12, Scan IF, AES",0,"Scan Interface"]
["MSP430F5438A-EP","TIMSP430F5438AEP","TI","MSP430",25,256,0,16,12,14,0,0,87,"No",4,8,null,"No",3,null,-55,125,1.8,3.6,100,"LQFP|100",6.4,null,4,null,null,0,null,null,"ACTIVE",null,"Mixed Signal Microcontroller, MSP430F5438AEP",0,"N/A"]
["MSP430F6459-HIREL","TIMSP430F6459HIREL","TI","MSP430",25,512,0,66,12,12,0,12,74,"Yes",3,6,null,"No",4,null,-40,105,1.8,3.6,100,"LQFP|100",9.35,null,3,null,null,0,null,null,"ACTIVE",null,"HiRel Mixed Signal Microcontroller",0,"N/A"]
["MSP430FR2000","TIMSP430FR2000","TI","MSP430",16,0.5,0,0.5,"Slope",0,0,4,12,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,16,"TSSOP|16, VQFN|24",0.25,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller With 0.5 KB FRAM, 0.5 KB SRAM, 12 IO",0,"N/A"]
["MSP430G2001","TIMSP430G2001","TI","MSP430",16,0.5,0,0.125,"N/A",0,0,0,10,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.3,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x01, MSP430G2x11 Mixed Signal Microcontroller",0,"N/A"]
["MSP430F1101A","TIMSP430F1101A","TI","MSP430",16,1,0,0.125,"Slope",0,0,2,14,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,20,"SOIC|20, TSSOP|20, TVSOP|20, VQFN|24",0.95,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 1kB Flash, 128B RAM, Comparator",0,"N/A"]
["MSP430F2001","TIMSP430F2001","TI","MSP430",16,1,0,0.125,"Slope",0,0,6,10,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.41,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 1kB Flash, 128B RAM, Comparator",0,"N/A"]
["MSP430F2002","TIMSP430F2002","TI","MSP430",16,1,0,0.125,10,8,0,0,10,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.56999999999999995,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 1kB Flash, 128B RAM, 10Bit SAR A/D, USI for SPI/I2C",0,"N/A"]
["MSP430F2003","TIMSP430F2003","TI","MSP430",16,1,0,0.125,16,4,0,0,10,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.87,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 1kB Flash, 128B RAM, 16Bit SigmaDelta A/D, USI for SPI/I2C",0,"N/A"]
["MSP430F2101","TIMSP430F2101","TI","MSP430",16,1,0,0.125,"Slope",0,0,6,16,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,20,"SOIC|20, TSSOP|20, TVSOP|20, VQFN|24",0.53,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 1kB Flash, 128B RAM, Comparator",0,"N/A"]
["MSP430FR2100","TIMSP430FR2100","TI","MSP430",16,1,0,0.5,10,8,0,4,12,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,16,"TSSOP|16, VQFN|24",0.23,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller With 1 KB FRAM, 0.5 KB SRAM, 12 IO, 8 ch 10bit ADC",0,"N/A"]
["MSP430G2101","TIMSP430G2101","TI","MSP430",16,1,0,0.125,"N/A",0,0,0,10,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.39,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x01, MSP430G2x11 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2102","TIMSP430G2102","TI","MSP430",16,1,0,0.125,"N/A",0,0,0,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.42,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x32, MSP430G2x02 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2111","TIMSP430G2111","TI","MSP430",16,1,0,0.125,"Slope",0,0,8,10,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.41,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x01, MSP430G2x11 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2112","TIMSP430G2112","TI","MSP430",16,1,0,0.125,"Slope",0,0,8,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.4,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x52, MSP430G2x12 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2121","TIMSP430G2121","TI","MSP430",16,1,0,0.125,"N/A",0,0,0,10,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.4,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x21, MSP430G2x31 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2131","TIMSP430G2131","TI","MSP430",16,1,0,0.125,10,8,0,0,10,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.44,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x21, MSP430G2x31 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2132","TIMSP430G2132","TI","MSP430",16,1,0,0.125,10,8,0,0,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.48,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x32, MSP430G2x02 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2152","TIMSP430G2152","TI","MSP430",16,1,0,0.125,10,8,0,8,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.48,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x52, MSP430G2x12 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2153","TIMSP430G2153","TI","MSP430",16,1,0,0.25,10,8,0,8,24,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.53,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 1 KB Flash, 256 Byte RAM, 24 IO, 2 16bit Timers and comparator",0,"N/A"]
["MSP430F1111A","TIMSP430F1111A","TI","MSP430",16,2,0,0.125,"Slope",0,0,2,14,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,20,"SOIC|20, TSSOP|20, TVSOP|20, VQFN|24",1.1000000000000001,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 2kB Flash, 128B RAM, Comparator",0,"N/A"]
["MSP430F2011","TIMSP430F2011","TI","MSP430",16,2,0,0.125,"Slope",0,0,6,10,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.48,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 2kB Flash, 128B RAM, Comparator",0,"N/A"]
["MSP430F2012","TIMSP430F2012","TI","MSP430",16,2,0,0.125,10,8,0,0,10,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.75,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 2kB Flash, 128B RAM, 10Bit SAR A/D, USI for SPI/I2C",0,"N/A"]
["MSP430F2013","TIMSP430F2013","TI","MSP430",16,2,0,0.125,16,4,0,0,10,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.97,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 2kB Flash, 128B RAM, 16Bit SigmaDelta A/D, USI for SPI/I2C",0,"N/A"]
["MSP430F2111","TIMSP430F2111","TI","MSP430",16,2,0,0.125,"Slope",0,0,6,16,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,20,"SOIC|20, TSSOP|20, TVSOP|20, VQFN|24",0.62,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 2kB Flash, 128B RAM, Comparator",0,"N/A"]
["MSP430F2112","TIMSP430F2112","TI","MSP430",16,2,0,0.25,10,8,0,8,24,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,28,"TSSOP|28, VQFN|32",0.97,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 2kB Flash, 256B RAM, 10 bit ADC, 1 USCI",0,"N/A"]
["MSP430FR2110","TIMSP430FR2110","TI","MSP430",16,2,0,1,10,8,0,4,12,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,16,"TSSOP|16, VQFN|24",0.24,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller With 2 KB FRAM, 1 KB SRAM, 12 IO, 8 ch 10bit ADC",0,"N/A"]
["MSP430G2201","TIMSP430G2201","TI","MSP430",16,2,0,0.125,"N/A",0,0,0,10,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.41,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x01, MSP430G2x11 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2202","TIMSP430G2202","TI","MSP430",16,2,0,0.25,"N/A",0,0,0,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.44,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x32, MSP430G2x02 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2203","TIMSP430G2203","TI","MSP430",16,2,0,0.25,"N/A",0,0,0,24,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.53,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x33, MSP430G2x03 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2210","TIMSP430G2210","TI","MSP430",16,2,0,0.125,"Slope",0,0,4,4,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,8,"SOIC|8",0.31,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G22x0 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2211","TIMSP430G2211","TI","MSP430",16,2,0,0.125,"Slope",0,0,8,10,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.43,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x01, MSP430G2x11 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2212","TIMSP430G2212","TI","MSP430",16,2,0,0.25,"Slope",0,0,8,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.48,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x52, MSP430G2x12 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2213","TIMSP430G2213","TI","MSP430",16,2,0,0.25,"Slope",0,0,8,24,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.56000000000000005,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 2 KB Flash, 256 Byte RAM, 24 IO, 2 16bit Timers and comparator",0,"N/A"]
["MSP430G2221","TIMSP430G2221","TI","MSP430",16,2,0,0.125,"N/A",0,0,0,10,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.43,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x21, MSP430G2x31 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2230","TIMSP430G2230","TI","MSP430",16,2,0,0.125,10,4,0,0,4,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,8,"SOIC|8",0.35,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G22x0 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2231","TIMSP430G2231","TI","MSP430",16,2,0,0.125,10,8,0,0,10,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,14,"PDIP|14, QFN|16, TSSOP|14",0.48,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x21, MSP430G2x31 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2232","TIMSP430G2232","TI","MSP430",16,2,0,0.25,10,8,0,0,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.48,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x32, MSP430G2x02 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2233","TIMSP430G2233","TI","MSP430",16,2,0,0.25,10,8,0,0,24,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.53,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x33, MSP430G2x03 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2252","TIMSP430G2252","TI","MSP430",16,2,0,0.25,10,8,0,8,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.53,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x52, MSP430G2x12 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2253","TIMSP430G2253","TI","MSP430",16,2,0,0.25,10,8,0,8,24,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.56999999999999995,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 2 KB Flash, 256 Byte RAM, 10bit ADC, 24 IO, 2 16bit Timers and comparator",0,"N/A"]
["MSP430AFE221","TIMSP430AFE221","TI","MSP430",16,4,0,0.25,16,1,0,0,11,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,24,"TSSOP|24",1.58,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 4KB Flash, 256B RAM, 1x SD24",0,"N/A"]
["MSP430AFE222","TIMSP430AFE222","TI","MSP430",16,4,0,0.25,24,2,0,0,11,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,24,"TSSOP|24",1.72,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 4KB Flash, 256B RAM, 2x SD24",0,"N/A"]
["MSP430AFE223","TIMSP430AFE223","TI","MSP430",16,4,0,0.25,24,3,0,0,11,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,24,"TSSOP|24",1.85,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 4KB Flash, 256B RAM, 3x SD24",0,"N/A"]
["MSP430F112","TIMSP430F112","TI","MSP430",16,4,0,0.25,"N/A",0,0,0,14,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,20,"TSSOP|20",1.38,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit  UltraLowPower Microcontroller, 4kB Flash, 256B RAM",0,"N/A"]
["MSP430F1121A","TIMSP430F1121A","TI","MSP430",16,4,0,0.25,"Slope",0,0,2,14,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,20,"SOIC|20, TSSOP|20, TVSOP|20, VQFN|24",1.4,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 4kB Flash, 256B RAM, Comparator",0,"N/A"]
["MSP430F1122","TIMSP430F1122","TI","MSP430",16,4,0,0.25,10,5,0,0,14,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,20,"SOIC|20, TSSOP|20, VQFN|32",1.5,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 4kB Flash, 256B RAM, 10 bit ADC",0,"N/A"]
["MSP430F122","TIMSP430F122","TI","MSP430",16,4,0,0.25,"Slope",0,0,2,22,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,28,"SOIC|28, TSSOP|28, VQFN|32",1.5,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 4kB Flash, 256B RAM, USART, Comparator",0,"N/A"]
["MSP430F1222","TIMSP430F1222","TI","MSP430",16,4,0,0.25,10,8,0,0,22,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,28,"SOIC|28, TSSOP|28, VQFN|32",1.55,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 4kB Flash, 256B RAM, 10 bit ADC, 1 USART",0,"N/A"]
["MSP430F2121","TIMSP430F2121","TI","MSP430",16,4,0,0.25,"Slope",0,0,6,16,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,20,"SOIC|20, TSSOP|20, TVSOP|20, VQFN|24",0.79,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 4kB Flash, 256B RAM, Comparator",0,"N/A"]
["MSP430F2122","TIMSP430F2122","TI","MSP430",16,4,0,0.5,10,8,0,8,24,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,28,"TSSOP|28, VQFN|32, WQFN|32",1.23,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 4kB Flash, 512B RAM, 10 bit ADC, 1 USCI",0,"N/A"]
["MSP430FR2111","TIMSP430FR2111","TI","MSP430",16,4,0,1,10,8,0,4,12,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,16,"TSSOP|16, VQFN|24",0.3,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller With 4 KB FRAM, 1 KB SRAM, 12 IO, 8 ch 10bit ADC",0,"N/A"]
["MSP430FR5720","TIMSP430FR5720","TI","MSP430",16,4,0,1,10,8,0,12,21,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,28,"TSSOP|28, VQFN|24",0.96,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430FR5720 8 MHz ULP microcontroller with 4 KB FRAM, 1 KB SRAM,  21 IO, 10bit ADC and comparator",0,"N/A"]
["MSP430FR5721","TIMSP430FR5721","TI","MSP430",16,4,0,1,10,12,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.01,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5721 8 MHz ULP microcontroller with 4 KB FRAM, 1 KB SRAM,  32 IO, 10bit ADC and comparator",0,"N/A"]
["MSP430FR5730","TIMSP430FR5730","TI","MSP430",16,4,0,1,10,8,0,12,21,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,28,"TSSOP|28, VQFN|24",1,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430FR5730 24 MHz ULP microcontroller with 4 KB FRAM, 1 KB SRAM,  21 IO, 10bit ADC and comparator",0,"N/A"]
["MSP430FR5731","TIMSP430FR5731","TI","MSP430",16,4,0,1,10,12,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,40,"VQFN|40",0.68,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5731 24 MHz ULP microcontroller with 4 KB FRAM, 1 KB SRAM,  32 IO, 10bit ADC and comparator",0,"N/A"]
["MSP430G2302","TIMSP430G2302","TI","MSP430",16,4,0,0.25,"N/A",0,0,0,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.48,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x32, MSP430G2x02 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2303","TIMSP430G2303","TI","MSP430",16,4,0,0.25,"N/A",0,0,0,24,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,20,"TSSOP|20, TSSOP|28, VQFN|32",0.56999999999999995,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x33, MSP430G2x03 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2312","TIMSP430G2312","TI","MSP430",16,4,0,0.25,"Slope",0,0,8,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.53,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x52, MSP430G2x12 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2313","TIMSP430G2313","TI","MSP430",16,4,0,0.25,"Slope",0,0,8,24,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.56999999999999995,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 4 KB Flash, 256 Byte RAM, 24 IO, 2 16bit Timers and comparator",0,"N/A"]
["MSP430G2332","TIMSP430G2332","TI","MSP430",16,4,0,0.25,10,8,0,0,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.53,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x32, MSP430G2x02 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2333","TIMSP430G2333","TI","MSP430",16,4,0,0.25,10,8,0,0,24,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.56999999999999995,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x33, MSP430G2x03 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2352","TIMSP430G2352","TI","MSP430",16,4,0,0.25,10,8,0,8,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.54,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x52, MSP430G2x12 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2353","TIMSP430G2353","TI","MSP430",16,4,0,0.25,10,8,0,8,24,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.62,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 4 KB Flash, 256 Byte RAM, 10bit ADC, 24 IO, 2 16bit Timers and comparator",0,"N/A"]
["MSP430AFE231","TIMSP430AFE231","TI","MSP430",16,8,0,0.5,24,1,0,0,11,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,24,"TSSOP|24",1.63,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 8KB Flash, 512B RAM, 1x SD24",0,"N/A"]
["MSP430AFE232","TIMSP430AFE232","TI","MSP430",16,8,0,0.5,24,2,0,0,11,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,24,"TSSOP|24",1.76,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 8KB Flash, 512B RAM, 2x SD24",0,"N/A"]
["MSP430AFE233","TIMSP430AFE233","TI","MSP430",16,8,0,0.5,24,3,0,0,11,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,24,"TSSOP|24",1.85,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 8KB Flash, 512B RAM, 3x SD24",0,"N/A"]
["MSP430F1132","TIMSP430F1132","TI","MSP430",16,8,0,0.25,10,5,0,0,14,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,20,"SOIC|20, TSSOP|20, VQFN|32",1.6,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 8kB Flash, 256B RAM, 10 bit ADC",0,"N/A"]
["MSP430F123","TIMSP430F123","TI","MSP430",16,8,0,0.25,"Slope",0,0,2,22,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,28,"SOIC|28, TSSOP|28, VQFN|32",1.54,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 8kB Flash, 256B RAM, USART, Comparator",0,"N/A"]
["MSP430F1232","TIMSP430F1232","TI","MSP430",16,8,0,0.25,10,8,0,0,22,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,28,"SOIC|28, TSSOP|28, VQFN|32",1.64,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 8kB Flash, 256B RAM, 10 bit ADC, 1 USART",0,"N/A"]
["MSP430F133","TIMSP430F133","TI","MSP430",16,8,0,0.25,12,8,0,2,48,"No",0,1,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TQFP|64, VQFN|64",2.64,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 8kB Flash, 256B RAM, 12 bit ADC, USART",0,"N/A"]
["MSP430F2131","TIMSP430F2131","TI","MSP430",16,8,0,0.25,"Slope",0,0,6,16,"No",0,0,null,"No",1,null,-40,85,1.8,3.6,20,"SOIC|20, TSSOP|20, TVSOP|20, VQFN|24",1.06,null,0,null,null,0,null,null,"ACTIVE",null,"16Bit  UltraLowPower Microcontroller, 8kB Flash, 256B RAM, Comparator",0,"N/A"]
["MSP430F2132","TIMSP430F2132","TI","MSP430",16,8,0,0.5,10,8,0,8,24,"No",1,2,null,"No",2,null,-40,105,1.8,3.6,28,"TSSOP|28, VQFN|32, WQFN|32",1.32,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 8kB Flash, 512B RAM, 10 bit ADC, 1 USCI",0,"N/A"]
["MSP430F2232","TIMSP430F2232","TI","MSP430",16,8,0,0.5,10,12,0,0,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.45,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 8KB Flash, 512B RAM",0,"N/A"]
["MSP430F233","TIMSP430F233","TI","MSP430",16,8,0,1,12,8,0,8,48,"No",1,1,null,"No",2,null,-40,105,1.8,3.6,64,"LQFP|64, VQFN|64",1.9,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 8KB Flash, 1KB RAM, 12Bit ADC, USCI, HW Multiplier",0,"N/A"]
["MSP430F2330","TIMSP430F2330","TI","MSP430",16,8,0,1,"Slope",0,0,8,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,40,"VQFN|40",2.04,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 8KB Flash, 1024B RAM, Comparator",0,"N/A"]
["MSP430F5131","TIMSP430F5131","TI","MSP430",25,8,0,1,"Slope",0,0,16,31,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,40,"DSBGA|40, TSSOP|38, WQFN|40",0.97,null,1,null,null,0,null,null,"ACTIVE",null,"25MHz MCU with Two 16bit High Res Timers, 8KB flash, 1KB RAM, 16channel Comparator",0,"N/A"]
["MSP430F5132","TIMSP430F5132","TI","MSP430",25,8,0,1,10,9,0,16,31,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,40,"DSBGA|40, TSSOP|38, WQFN|40",1.01,null,1,null,null,0,null,null,"ACTIVE",null,"25MHz MCU with Two 16bit High Res Timers, 8KB flash, 1KB RAM, 10bit ADC, 16channel Comparator",0,"N/A"]
["MSP430F5304","TIMSP430F5304","TI","MSP430",25,8,0,6,10,6,0,0,31,"No",1,2,null,"No",4,null,-40,85,1.8,3.6,48,"LQFP|48, VQFN|48",1.36,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430F530x Mixed Signal Microcontroller",0,"N/A"]
["MSP430FR2032","TIMSP430FR2032","TI","MSP430",16,8,0,1,10,10,0,0,60,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|48, TSSOP|56",0.56999999999999995,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller With 8 KB FRAM, 1 KB SRAM, 60 IO, 10bit ADC, IR Logic",0,"N/A"]
["MSP430FR2422","TIMSP430FR2422","TI","MSP430",16,8,0,2,10,8,0,0,15,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,16,"TSSOP|16, VQFN|20",0.32,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller With 8 KB FRAM, 2 KB RAM, 10bit ADC, 15 IO, 2 16bit Timers",0,"N/A"]
["MSP430FR2512","TIMSP430FR2512","TI","MSP430",16,8,0,2,10,8,0,0,15,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,16,"TSSOP|16, VQFN|20",0.52,null,1,null,null,4,null,null,"ACTIVE",null,"Capacitive Touch MCU with 4 touch IO (4 sensors), 8KB FRAM, 2KB SRAM, 15 IO, 10bit ADC",0,"N/A"]
["MSP430FR2522","TIMSP430FR2522","TI","MSP430",16,8,0,2,10,8,0,0,15,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,16,"TSSOP|16, VQFN|20",0.63,null,1,null,null,8,null,null,"ACTIVE",null,"Capacitive Touch MCU with 8 touch IO (16 sensors), 8KB FRAM, 2KB SRAM, 15 IO, 10bit ADC",0,"N/A"]
["MSP430FR2632","TIMSP430FR2632","TI","MSP430",16,8,0,2,10,8,0,0,15,"No",1,2,null,"No",4,null,-40,85,1.8,3.6,24,"DSBGA|24, VQFN|24",1.1100000000000001,null,2,null,null,8,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller With 8 KB FRAM, CapTIvate touch technology",0,"N/A"]
["MSP430FR5722","TIMSP430FR5722","TI","MSP430",16,8,0,1,"Slope",0,0,12,21,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,28,"TSSOP|28, VQFN|24",0.95,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430FR5722 8 MHz ULP microcontroller with 8 KB FRAM, 1 KB SRAM,  21 IO and comparator",0,"N/A"]
["MSP430FR5723","TIMSP430FR5723","TI","MSP430",16,8,0,1,"Slope",0,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,40,"VQFN|40",0.9,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5723 8 MHz ULP microcontroller with 8 KB FRAM, 1 KB SRAM,  32 IO and comparator",0,"N/A"]
["MSP430FR5724","TIMSP430FR5724","TI","MSP430",16,8,0,1,10,8,0,12,21,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,28,"TSSOP|28, VQFN|24",1.01,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430FR5724 8 MHz ULP microcontroller with 8 KB FRAM, 1 KB SRAM,  21 IO, 10bit ADC and comparator",0,"N/A"]
["MSP430FR5725","TIMSP430FR5725","TI","MSP430",16,8,0,1,10,12,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.06,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5725 8 MHz ULP microcontroller with 8 KB FRAM, 1 KB SRAM,  32 IO, 10bit ADC and comparator",0,"N/A"]
["MSP430FR5732","TIMSP430FR5732","TI","MSP430",16,8,0,1,"Slope",0,0,12,21,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,28,"TSSOP|28, VQFN|24",1.1000000000000001,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430FR5732 24 MHz ULP microcontroller with 8 KB FRAM, 1 KB SRAM,  21 IO and comparator",0,"N/A"]
["MSP430FR5733","TIMSP430FR5733","TI","MSP430",16,8,0,1,"Slope",0,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,40,"VQFN|40",0.8,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5733 24 MHz ULP microcontroller with 8 KB FRAM, 1 KB SRAM,  32 IO and comparator",0,"N/A"]
["MSP430FR5734","TIMSP430FR5734","TI","MSP430",16,8,0,1,10,8,0,12,21,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,28,"TSSOP|28",0.78,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430FR5734 24 MHz ULP microcontroller with 8 KB FRAM, 1 KB SRAM,  21 IO, 10bit ADC and comparator",0,"N/A"]
["MSP430FR5735","TIMSP430FR5735","TI","MSP430",16,8,0,1,10,12,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",0.8,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5735 24 MHz ULP microcontroller with 8 KB FRAM, 1 KB SRAM,  32 IO, 10bit ADC and comparator",0,"N/A"]
["MSP430G2402","TIMSP430G2402","TI","MSP430",16,8,0,0.25,"N/A",0,0,0,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.56999999999999995,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x32, MSP430G2x02 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2403","TIMSP430G2403","TI","MSP430",16,8,0,0.5,"N/A",0,0,0,24,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.66,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x33, MSP430G2x03 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2412","TIMSP430G2412","TI","MSP430",16,8,0,0.25,"Slope",0,0,8,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.56000000000000005,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x52, MSP430G2x12 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2413","TIMSP430G2413","TI","MSP430",16,8,0,0.5,"Slope",0,0,8,24,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.66,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 8 KB Flash, 512 Byte RAM, 24 IO, 2 16bit Timers and comparator",0,"N/A"]
["MSP430G2432","TIMSP430G2432","TI","MSP430",16,8,0,0.25,10,8,0,0,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.62,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x32, MSP430G2x02 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2433","TIMSP430G2433","TI","MSP430",16,8,0,0.5,10,8,0,0,24,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.66,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x33, MSP430G2x03 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2444","TIMSP430G2444","TI","MSP430",16,8,0,0.5,10,12,0,0,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,49,"DSBGA|49, TSSOP|38, VQFN|40",1.03,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x44 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2452","TIMSP430G2452","TI","MSP430",16,8,0,0.25,10,8,0,8,16,"No",1,1,null,"No",1,null,-40,85,1.8,3.6,20,"PDIP|20, QFN|16, TSSOP|14, TSSOP|20",0.62,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430G2x52, MSP430G2x12 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2453","TIMSP430G2453","TI","MSP430",16,8,0,0.5,10,8,0,8,24,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.7,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 8 KB Flash, 512 Byte RAM, 10bit ADC, 24 IO, 2 16bit Timers and comparator",0,"N/A"]
["MSP430AFE251","TIMSP430AFE251","TI","MSP430",16,16,0,0.5,24,1,0,0,11,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,24,"TSSOP|24",1.97,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 16KB Flash, 512B RAM, 1x SD24",0,"N/A"]
["MSP430AFE252","TIMSP430AFE252","TI","MSP430",16,16,0,0.5,24,2,0,0,11,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,24,"TSSOP|24",1.8,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 16KB Flash, 512B RAM, 2x SD24",0,"N/A"]
["MSP430AFE253","TIMSP430AFE253","TI","MSP430",16,16,0,0.5,24,3,0,0,11,"No",0,1,null,"No",1,null,-40,85,1.8,3.6,24,"TSSOP|24",1.94,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 16KB Flash, 512B RAM, 3x SD24",0,"N/A"]
["MSP430F135","TIMSP430F135","TI","MSP430",16,16,0,0.5,12,8,0,2,48,"No",0,1,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TQFP|64, VQFN|64",2.94,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 16kB Flash, 512B RAM, 12 bit ADC, USART",0,"N/A"]
["MSP430F2252","TIMSP430F2252","TI","MSP430",16,16,0,0.5,10,12,0,0,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,49,"DSBGA|49, TSSOP|38, VQFN|40",1.72,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 16KB Flash, 512B RAM",0,"N/A"]
["MSP430F235","TIMSP430F235","TI","MSP430",16,16,0,2,12,8,0,8,48,"No",1,1,null,"No",2,null,-40,105,1.8,3.6,64,"LQFP|64, VQFN|64",2.29,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 16KB Flash, 2KB RAM, 12Bit ADC, USCI, HW Multiplier",0,"N/A"]
["MSP430F2350","TIMSP430F2350","TI","MSP430",16,16,0,2,"Slope",0,0,8,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,49,"DSBGA|49, VQFN|40",2.08,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 16KB Flash, 2048B RAM, Comparator",0,"N/A"]
["MSP430F5151","TIMSP430F5151","TI","MSP430",25,16,0,2,"Slope",0,0,16,31,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,40,"DSBGA|40, TSSOP|38, WQFN|40",1.1100000000000001,null,1,null,null,0,null,null,"ACTIVE",null,"25MHz MCU with Two 16bit High Res Timers, 16KB flash, 2KB RAM, 16channel Comparator",0,"N/A"]
["MSP430F5152","TIMSP430F5152","TI","MSP430",25,16,0,2,10,9,0,16,31,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,40,"DSBGA|40, TSSOP|38, WQFN|40",1.1399999999999999,null,1,null,null,0,null,null,"ACTIVE",null,"25MHz MCU with Two 16bit High Res Timers, 16KB flash, 2KB RAM, 10bit ADC, 16channel Comparator",0,"N/A"]
["MSP430F5308","TIMSP430F5308","TI","MSP430",25,16,0,6,10,10,0,8,47,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"LQFP|48, VQFN|48, VQFN|64",1.19,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F530x Mixed Signal Microcontroller",0,"N/A"]
["MSP430FR2033","TIMSP430FR2033","TI","MSP430",16,16,0,2,10,10,0,0,60,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|48, TSSOP|56",0.7,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller with 16 KB FRAM, 2 KB SRAM, 60 IO, 10bit ADC, IR Logic",0,"N/A"]
["MSP430FR2153","TIMSP430FR2153","TI","MSP430",16,16,0,2,12,12,0,2,44,"No",2,4,null,"No",4,null,-40,105,1.8,3.6,48,"LQFP|48, TSSOP|38, VQFN|32, VQFN|40",0.79,null,2,null,null,0,null,null,"ACTIVE",null,"24MHz 105C ULP Microcontroller With 16 KB FRAM, 2 KB SRAM, 44 IO, 12bit ADC",0,"N/A"]
["MSP430FR2433","TIMSP430FR2433","TI","MSP430",16,16,0,4,10,8,0,0,19,"No",1,2,null,"No",4,null,-40,85,1.8,3.6,24,"DSBGA|24, VQFN|24",0.5,null,2,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller with 16 KB FRAM, 4 KB RAM, 10bit ADC, 19 IO, 4 16bit Timers",0,"N/A"]
["MSP430FR2533","TIMSP430FR2533","TI","MSP430",16,16,0,2,10,8,0,0,19,"No",1,2,null,"No",4,null,-40,85,1.8,3.6,32,"TSSOP|32, VQFN|32",1.31,null,2,null,null,16,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller with 16 KB FRAM, CapTIvate touch technology",0,"N/A"]
["MSP430FR2633","TIMSP430FR2633","TI","MSP430",16,16,0,4,10,8,0,0,19,"No",1,2,null,"No",4,null,-40,85,1.8,3.6,24,"DSBGA|24, TSSOP|32, VQFN|32",1.45,null,2,null,null,16,null,null,"ACTIVE",null,"MSP430 MCU with CapTIvate technology  the lowest power, most noiseimmune capacitive touch",0,"N/A"]
["MSP430FR5726","TIMSP430FR5726","TI","MSP430",16,16,0,1,"Slope",0,0,12,21,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,28,"TSSOP|28, VQFN|24",1.05,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430FR5726 8 MHz ULP microcontroller with 16 KB FRAM, 1 KB SRAM,  21 IO and comparator",0,"N/A"]
["MSP430FR5727","TIMSP430FR5727","TI","MSP430",16,16,0,1,"Slope",0,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.1100000000000001,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5727 8 MHz ULP microcontroller with 16 KB FRAM, 1 KB SRAM,  32 IO and comparator",0,"N/A"]
["MSP430FR5728","TIMSP430FR5728","TI","MSP430",16,16,0,1,10,8,0,12,21,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,28,"TSSOP|28, VQFN|24",1.04,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430FR5728 8 MHz ULP microcontroller with 16 KB FRAM, 1 KB SRAM,  21 IO, 10bit ADC and comparator",0,"N/A"]
["MSP430FR5729","TIMSP430FR5729","TI","MSP430",16,16,0,1,10,12,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.0900000000000001,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5729 8 MHz ULP microcontroller with 16 KB FRAM, 1 KB SRAM,  32 IO, 10bit ADC and comparator",0,"N/A"]
["MSP430FR5736","TIMSP430FR5736","TI","MSP430",16,16,0,1,"Slope",0,0,12,21,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,28,"TSSOP|28, VQFN|24",1.07,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430FR5736 24 MHz ULP microcontroller with 16 KB FRAM, 1 KB SRAM,  21 IO, and comparator",0,"N/A"]
["MSP430FR5737","TIMSP430FR5737","TI","MSP430",16,16,0,1,"Slope",0,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,40,"VQFN|40",1.28,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5737 24 MHz ULP microcontroller with 16 KB FRAM, 1 KB SRAM,  32 IO and comparator",0,"N/A"]
["MSP430FR5738","TIMSP430FR5738","TI","MSP430",16,16,0,1,10,8,0,12,21,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,24,"DSBGA|24, TSSOP|28, VQFN|24",1.08,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430FR5738 24 MHz ULP microcontroller with 16 KB FRAM, 1 KB SRAM, 21 IO, 10bit ADC and comparator",0,"N/A"]
["MSP430FR5739","TIMSP430FR5739","TI","MSP430",16,16,0,1,10,12,0,16,32,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.21,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5739 24 MHz ULP microcontroller with 16 KB FRAM, 1 KB SRAM,  32 IO, 10bit ADC & comparator",0,"N/A"]
["MSP430G2513","TIMSP430G2513","TI","MSP430",16,16,0,0.5,10,8,0,8,24,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.79,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 16 KB Flash, 512 Byte RAM, 24 IO, 2 16bit Timers and comparator",0,"N/A"]
["MSP430G2533","TIMSP430G2533","TI","MSP430",16,16,0,0.5,10,8,0,0,24,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.79,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x33, MSP430G2x03 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2544","TIMSP430G2544","TI","MSP430",16,16,0,0.5,10,12,0,0,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",0.97,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x44 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2553","TIMSP430G2553","TI","MSP430",16,16,0,0.5,10,8,0,8,24,"No",1,2,null,"No",2,null,-40,85,1.8,3.6,20,"PDIP|20, TSSOP|20, TSSOP|28, VQFN|32",0.79,null,1,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 16 KB Flash, 512 Byte RAM, 10bit ADC, 24 IO, 2 16bit Timers and comparator",0,"N/A"]
["MSP430I2020","TIMSP430I2020","TI","MSP430",16,16,0,1,24,2,0,0,16,"No",1,2,null,"No",2,null,-40,105,1.8,3.6,28,"TSSOP|28, VQFN|32",0.78,null,1,null,null,0,null,null,"ACTIVE",null,"16MHz MCU with two 24bit SigmaDelta ADCs, two 16bit High Res Timers, 16KB flash, 1KB RAM",0,"N/A"]
["MSP430I2030","TIMSP430I2030","TI","MSP430",16,16,0,1,24,3,0,0,16,"No",1,2,null,"No",2,null,-40,105,1.8,3.6,28,"TSSOP|28, VQFN|32",0.92,null,1,null,null,0,null,null,"ACTIVE",null,"16MHz MCU with three 24bit SigmaDelta ADCs, two 16bit High Res Timers, 16KB flash, 1KB RAM",0,"N/A"]
["MSP430I2040","TIMSP430I2040","TI","MSP430",16,16,0,1,24,4,0,0,16,"No",1,2,null,"No",2,null,-40,105,1.8,3.6,28,"TSSOP|28, VQFN|32",0.96,null,1,null,null,0,null,null,"ACTIVE",null,"16MHz MCU with four 24bit SigmaDelta ADCs, two 16bit High Res Timers, 16KB flash, 1KB RAM",0,"N/A"]
["MSP430F5309","TIMSP430F5309","TI","MSP430",25,24,0,6,10,10,0,8,47,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"LQFP|48, VQFN|48, VQFN|64",1.29,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F530x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F147","TIMSP430F147","TI","MSP430",16,32,0,1,12,8,0,2,48,"No",0,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TQFP|64, VQFN|64",3.59,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 32 kB Flash, 1KB RAM, 12 bit ADC, 2 USARTs, HW multiplier",0,"N/A"]
["MSP430F1471","TIMSP430F1471","TI","MSP430",16,32,0,1,"Slope",0,0,2,48,"No",0,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",4.08,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 32 kB Flash, 1KB RAM,  2 USARTs, HW multiplier",0,"N/A"]
["MSP430F2272","TIMSP430F2272","TI","MSP430",16,32,0,1,10,12,0,0,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,49,"DSBGA|49, TSSOP|38, VQFN|40",1.76,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 32KB Flash, 512B RAM​",0,"N/A"]
["MSP430F2370","TIMSP430F2370","TI","MSP430",16,32,0,2,"Slope",0,0,8,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,49,"DSBGA|49, VQFN|40",1.72,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 32KB Flash, 2048B RAM, Comparator",0,"N/A"]
["MSP430F247","TIMSP430F247","TI","MSP430",16,32,0,4,12,8,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,64,"LQFP|64, VQFN|64",2.42,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 32KB Flash, 4KB RAM, 12Bit ADC,up to 4 USCIs, HW Multiplier",0,"N/A"]
["MSP430F2471","TIMSP430F2471","TI","MSP430",16,32,0,4,"Slope",0,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,64,"LQFP|64, VQFN|64",2.77,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 32KB Flash, 4KB RAM, 2 USCIs, HW Multiplier",0,"N/A"]
["MSP430F5171","TIMSP430F5171","TI","MSP430",25,32,0,2,"Slope",0,0,16,31,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,40,"DSBGA|40, TSSOP|38, WQFN|40",1.23,null,1,null,null,0,null,null,"ACTIVE",null,"25MHz MCU with Two 16bit High Res Timers, 32KB flash, 2KB RAM, 16channel Comparator",0,"N/A"]
["MSP430F5172","TIMSP430F5172","TI","MSP430",25,32,0,2,10,9,0,16,31,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,40,"DSBGA|40, TSSOP|38, WQFN|40",1.36,null,1,null,null,0,null,null,"ACTIVE",null,"25MHz MCU with Two 16bit High Res Timers, 32KB flash, 2KB RAM, 10bit ADC, 16channel Comparator",0,"N/A"]
["MSP430F5310","TIMSP430F5310","TI","MSP430",25,32,0,6,10,10,0,8,47,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"LQFP|48, VQFN|48, VQFN|64",1.28,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F530x Mixed Signal Microcontroller",0,"N/A"]
["MSP430FR2155","TIMSP430FR2155","TI","MSP430",16,32,0,4,12,12,0,2,44,"No",2,4,null,"No",4,null,-40,105,1.8,3.6,48,"LQFP|48, TSSOP|38, VQFN|32, VQFN|40",0.62,null,2,null,null,0,null,null,"ACTIVE",null,"24MHz 105C ULP Microcontroller With 32 KB FRAM, 4 KB SRAM, 44 IO, 12bit ADC",0,"N/A"]
["MSP430FR5847","TIMSP430FR5847","TI","MSP430",16,32,0,1,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.38,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5847 16 MHz UltraLowPower Microcontroller featuring 32 KB FRAM, 1 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR58471","TIMSP430FR58471","TI","MSP430",16,32,0,1,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,40,"VQFN|40",1.45,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR58471 16 MHz UltraLowPower Microcontroller featuring 32 KB FRAM, 1 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5857","TIMSP430FR5857","TI","MSP430",16,32,0,1,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.38,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5857 16 MHz UltraLowPower Microcontroller featuring 32 KB FRAM, 1 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5867","TIMSP430FR5867","TI","MSP430",16,32,0,1,12,16,0,16,40,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,48,"VQFN|48",1.52,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5867 16 MHz UltraLowPower Microcontroller featuring 32 KB FRAM, 1 KB SRAM, 40 IO",0,"N/A"]
["MSP430FR58671","TIMSP430FR58671","TI","MSP430",16,32,0,1,12,16,0,16,40,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,48,"VQFN|48",1.24,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR58xx MixedSignal Microcontrollers",0,"N/A"]
["MSP430FR5870","TIMSP430FR5870","TI","MSP430",16,32,0,2,12,8,0,8,51,"No",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.59,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5870 16 MHz UltraLowPower Microcontroller featuring 32 KB FRAM, 2 KB SRAM, 51 IO, ADC12",0,"N/A"]
["MSP430FR5947","TIMSP430FR5947","TI","MSP430",16,32,0,1,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.47,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5947 16 MHz UltraLowPower Microcontroller featuring 32 KB FRAM, 1 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR59471","TIMSP430FR59471","TI","MSP430",16,32,0,1,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,40,"VQFN|40",1.54,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR59471 16 MHz UltraLowPower Microcontroller featuring 32 KB FRAM, 1 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5957","TIMSP430FR5957","TI","MSP430",16,32,0,1,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.47,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5957 16 MHz UltraLowPower Microcontroller featuring 32 KB FRAM, 1 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5967","TIMSP430FR5967","TI","MSP430",16,32,0,1,12,16,0,16,40,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,48,"VQFN|48",1.57,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5967 16 MHz UltraLowPower Microcontroller featuring 32 KB FRAM, 1 KB SRAM, 40 IO",0,"N/A"]
["MSP430FR5970","TIMSP430FR5970","TI","MSP430",16,32,0,2,12,8,0,8,51,"No",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.26,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5970 16 MHz UltraLowPower Microcontroller featuring 32KB FRAM, 2KB SRAM, 51 IO, ADC12, AES",0,"N/A"]
["MSP430G2744","TIMSP430G2744","TI","MSP430",16,32,0,1,10,12,0,0,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,49,"DSBGA|49, TSSOP|38, VQFN|40",1,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x44 Mixed Signal Microcontroller",0,"N/A"]
["MSP430G2755","TIMSP430G2755","TI","MSP430",16,32,0,4,10,12,0,8,32,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.06,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x55 Mixed Signal Microcontroller",0,"N/A"]
["MSP430I2021","TIMSP430I2021","TI","MSP430",16,32,0,2,24,2,0,0,16,"No",1,2,null,"No",2,null,-40,105,1.8,3.6,28,"TSSOP|28, VQFN|32",0.88,null,1,null,null,0,null,null,"ACTIVE",null,"16MHz MCU with two 24bit SigmaDelta ADCs, two 16bit High Res Timers, 32KB flash, 2KB RAM",0,"N/A"]
["MSP430I2031","TIMSP430I2031","TI","MSP430",16,32,0,2,24,3,0,0,16,"No",1,2,null,"No",2,null,-40,105,1.8,3.6,28,"TSSOP|28, VQFN|32",1.01,null,1,null,null,0,null,null,"ACTIVE",null,"16MHz MCU with three 24bit SigmaDelta ADCs, two 16bit High Res Timers, 32KB flash, 2KB RAM",0,"N/A"]
["MSP430I2041","TIMSP430I2041","TI","MSP430",16,32,0,2,24,4,0,0,16,"No",1,2,null,"No",2,null,-40,105,1.8,3.6,28,"TSSOP|28, VQFN|32",1.06,null,1,null,null,0,null,null,"ACTIVE",null,"16MHz MCU with four 24bit SigmaDelta ADCs, two 16bit High Res Timers, 32KBKB flash, 2KB RAM",0,"N/A"]
["MSP430F148","TIMSP430F148","TI","MSP430",16,48,0,2,12,8,0,2,48,"No",0,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TQFP|64, VQFN|64",3.89,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 48 kB Flash, 2KB RAM, 12 bit ADC, 2 USARTs, HW multiplier",0,"N/A"]
["MSP430F1481","TIMSP430F1481","TI","MSP430",16,48,0,2,"Slope",0,0,2,48,"No",0,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",4.59,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 48 kB Flash, 2KB RAM,  2 USARTs, HW multiplier",0,"N/A"]
["MSP430F248","TIMSP430F248","TI","MSP430",16,48,0,4,12,8,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,64,"LQFP|64, VQFN|64",3,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 48KB Flash, 4KB RAM, 12Bit ADC, 2 USCIs, HW Multiplier",0,"N/A"]
["MSP430F2481","TIMSP430F2481","TI","MSP430",16,48,0,4,"Slope",0,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,64,"LQFP|64, VQFN|64",2.64,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 48KB Flash, 4KB RAM, 2 USCIs, HW Multiplier",0,"N/A"]
["MSP430FR5848","TIMSP430FR5848","TI","MSP430",16,48,0,2,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.47,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5848 16 MHz UltraLowPower Microcontroller featuring 48 KB FRAM, 2 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5858","TIMSP430FR5858","TI","MSP430",16,48,0,2,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.38,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5858 16 MHz UltraLowPower Microcontroller featuring 48 KB FRAM, 2 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5868","TIMSP430FR5868","TI","MSP430",16,48,0,2,12,16,0,16,40,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,48,"VQFN|48",1.51,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5868 16 MHz UltraLowPower Microcontroller featuring 48 KB FRAM, 2 KB SRAM, 40 IO",0,"N/A"]
["MSP430FR5948","TIMSP430FR5948","TI","MSP430",16,48,0,2,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.47,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5948 16 MHz UltraLowPower Microcontroller featuring 48 KB FRAM, 2 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5958","TIMSP430FR5958","TI","MSP430",16,48,0,2,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.47,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5958 16 MHz UltraLowPower Microcontroller featuring 48 KB FRAM, 2 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5968","TIMSP430FR5968","TI","MSP430",16,48,0,2,12,16,0,16,40,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,48,"VQFN|48",1.51,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5968 16 MHz UltraLowPower Microcontroller featuring 48 KB FRAM, 2 KB SRAM, 40 IO",0,"N/A"]
["MSP430G2855","TIMSP430G2855","TI","MSP430",16,48,0,4,10,12,0,8,32,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.19,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x55 Mixed Signal Microcontroller",0,"N/A"]
["MSP430F2410","TIMSP430F2410","TI","MSP430",16,56,0,4,12,8,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,64,"LQFP|64, VQFN|64",4.05,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 56KB Flash, 4KB RAM, 12Bit ADC, 2 USCIs, HW Multiplier",0,"N/A"]
["MSP430G2955","TIMSP430G2955","TI","MSP430",16,56,0,4,10,12,0,8,32,"No",1,2,null,"No",3,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.1399999999999999,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430G2x55 Mixed Signal Microcontroller",0,"N/A"]
["MSP430F149","TIMSP430F149","TI","MSP430",16,60,0,2,12,8,0,2,48,"No",0,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, TQFP|64, VQFN|64",4.18,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 60 kB Flash, 2KB RAM, 12 bit ADC, 2 USARTs, HW multiplier",0,"N/A"]
["MSP430F1491","TIMSP430F1491","TI","MSP430",16,60,0,2,"Slope",0,0,2,48,"No",0,2,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",4.8,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 60 kB Flash, 2KB RAM,  2 USARTs, HW multiplier",0,"N/A"]
["MSP430F249","TIMSP430F249","TI","MSP430",16,60,0,2,12,8,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,64,"LQFP|64, VQFN|64",3.28,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 60KB Flash, 2KB RAM, 12Bit ADC, 2 USCIs, HW Multiplier",0,"N/A"]
["MSP430F2491","TIMSP430F2491","TI","MSP430",16,60,0,2,"Slope",0,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,64,"LQFP|64, VQFN|64",3.45,null,2,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 60KB Flash, 2KB RAM, 2 USCIs, HW Multiplier",0,"N/A"]
["MSP430F5212","TIMSP430F5212","TI","MSP430",25,64,0,8,"Slope",0,0,6,37,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.86,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F522x, MSP430F521x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5217","TIMSP430F5217","TI","MSP430",25,64,0,8,"Slope",0,0,8,53,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,64,"DSBGA|64, VQFN|64",1.64,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F522x, MSP430F521x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5222","TIMSP430F5222","TI","MSP430",25,64,0,8,10,8,0,6,37,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.94,null,2,null,null,0,null,null,"ACTIVE",null,"UltraLow Power 1.8V SplitRail I/O",0,"N/A"]
["MSP430F5232","TIMSP430F5232","TI","MSP430",25,64,0,8,"Slope",0,0,6,37,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.45,null,2,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 with 64 KB Flash",0,"N/A"]
["MSP430F5237","TIMSP430F5237","TI","MSP430",25,64,0,8,"Slope",0,0,8,53,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",1.64,null,2,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 with 64 KB Flash",0,"N/A"]
["MSP430F5242","TIMSP430F5242","TI","MSP430",25,64,0,8,10,8,0,6,37,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.58,null,2,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 with 64 KB Flash",0,"N/A"]
["MSP430F5247","TIMSP430F5247","TI","MSP430",25,64,0,8,10,10,0,8,53,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,64,"VQFN|64",1.63,null,2,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 with 64 KB Flash",0,"N/A"]
["MSP430F5324","TIMSP430F5324","TI","MSP430",25,64,0,6,12,10,0,8,47,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",1.88,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F532x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5325","TIMSP430F5325","TI","MSP430",25,64,0,6,12,14,0,12,63,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"LQFP|80",1.94,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F532x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5340","TIMSP430F5340","TI","MSP430",25,64,0,6,12,7,0,5,38,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.89,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F534x Mixed Signal Microcontroller",0,"N/A"]
["MSP430FR5849","TIMSP430FR5849","TI","MSP430",16,64,0,2,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.51,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5849 16 MHz UltraLowPower Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5859","TIMSP430FR5859","TI","MSP430",16,64,0,2,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.51,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5859 16 MHz UltraLowPower Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5869","TIMSP430FR5869","TI","MSP430",16,64,0,2,12,16,0,16,40,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,48,"VQFN|48",1.67,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5869 16 MHz UltraLowPower Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 40 IO",0,"N/A"]
["MSP430FR5872","TIMSP430FR5872","TI","MSP430",16,64,0,2,12,8,0,8,51,"No",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.72,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5872 16 MHz UltraLowPower Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 51 IO, ADC12",0,"N/A"]
["MSP430FR58721","TIMSP430FR58721","TI","MSP430",16,64,0,2,12,8,0,8,51,"No",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.64,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR58721 16 MHz UltraLowPower Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 51 IO, ADC12",0,"N/A"]
["MSP430FR5922","TIMSP430FR5922","TI","MSP430",16,64,0,2,12,8,0,8,51,"No",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|56, VQFN|64",1.62,null,2,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller featuring 64KB FRAM, 2KB SRAM, 51 IO, ADC12, AES",0,"N/A"]
["MSP430FR59221","TIMSP430FR59221","TI","MSP430",16,64,0,2,12,8,0,8,51,"No",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, TSSOP|56, VQFN|64",1.62,null,2,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower MCU featuring 64KB FRAM, 2KB SRAM, 51 IO, ADC12, AES",0,"N/A"]
["MSP430FR5949","TIMSP430FR5949","TI","MSP430",16,64,0,2,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.6,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5949 16 MHz UltraLowPower Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5959","TIMSP430FR5959","TI","MSP430",16,64,0,2,12,14,0,16,33,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.6,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5959 16 MHz UltraLowPower Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 33 IO",0,"N/A"]
["MSP430FR5969","TIMSP430FR5969","TI","MSP430",16,64,0,2,12,16,0,16,40,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,48,"VQFN|48",1.76,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5969 16 MHz UltraLowPower Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 40 IO",0,"N/A"]
["MSP430FR59691","TIMSP430FR59691","TI","MSP430",16,64,0,2,12,16,0,16,40,"No",1,3,null,"No",5,null,-40,85,1.8,3.6,48,"VQFN|48"," ",null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR59691 16 MHz UltraLowPower Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 40 IO",0,"N/A"]
["MSP430FR5972","TIMSP430FR5972","TI","MSP430",16,64,0,2,12,8,0,8,51,"No",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.81,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5972 16 MHz UltraLowPower MCU featuring 64 KB FRAM, 2 KB SRAM, 51 IO, ADC12, AES",0,"N/A"]
["MSP430FR59721","TIMSP430FR59721","TI","MSP430",16,64,0,2,12,8,0,8,51,"No",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",1.64,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR59721 16 MHz UltraLowPower MCUfeaturing 64KB FRAM, 2KB SRAM, 51IO, ADC12, AES",0,"N/A"]
["MSP430F2416","TIMSP430F2416","TI","MSP430",16,92,0,4,12,8,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|64, LQFP|80",4.1399999999999997,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 92KB Flash, 4KB RAM, 12 Bit ADC, 2 USCIs, HW Multiplier",0,"N/A"]
["MSP430F2417","TIMSP430F2417","TI","MSP430",16,92,0,8,12,8,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|64, LQFP|80",4.22,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 92KB Flash, 8KB RAM, 12 Bit ADC, 2 USCIs, HW Multiplier",0,"N/A"]
["MSP430F5326","TIMSP430F5326","TI","MSP430",25,96,0,8,12,10,0,8,47,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",2.16,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F532x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5327","TIMSP430F5327","TI","MSP430",25,96,0,8,12,14,0,12,63,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"LQFP|80",2.2000000000000002,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F532x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5341","TIMSP430F5341","TI","MSP430",25,96,0,8,12,7,0,5,38,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",2.1800000000000002,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F534x Mixed Signal Microcontroller",0,"N/A"]
["MSP430FR5888","TIMSP430FR5888","TI","MSP430",16,96,0,2,12,12,0,12,48,"No",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",2.92,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5888 16 MHz ULP Microcontroller featuring 96 KB FRAM, 2 KB SRAM, 40 IO, ADC12, Scan IF",0,"Scan Interface"]
["MSP430FR5988","TIMSP430FR5988","TI","MSP430",16,96,0,2,12,12,0,12,48,"No",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",2.92,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5988 16 MHz UPLMicrocontroller featuring 96 KB FRAM, 2 KB SRAM, 48 IO, ADC12, Scan IF, AES",0,"Scan Interface"]
["MSP430F2418","TIMSP430F2418","TI","MSP430",16,116,0,8,12,8,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|64, LQFP|80",4.4000000000000004,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 116KB Flash, 8KB RAM, 12 Bit ADC, 2 USCIs, HW Multiplier",0,"N/A"]
["MSP430F2419","TIMSP430F2419","TI","MSP430",16,120,0,4,12,8,0,8,48,"No",2,2,null,"No",2,null,-40,105,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|64, LQFP|80",4.66,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 120KB Flash, 4KB RAM, 12 Bit ADC, 2 USCIs, HW Multiplier",0,"N/A"]
["MSP430F5214","TIMSP430F5214","TI","MSP430",25,128,0,8,"Slope",0,0,6,37,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",2.1800000000000002,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F522x, MSP430F521x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5219","TIMSP430F5219","TI","MSP430",25,128,0,8,"Slope",0,0,8,53,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, DSBGA|64",2.54,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F522x, MSP430F521x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5224","TIMSP430F5224","TI","MSP430",25,128,0,8,10,8,0,6,37,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",2.1800000000000002,null,2,null,null,0,null,null,"ACTIVE",null,"UltraLow Power 1.8V SplitRail I/O",0,"N/A"]
["MSP430F5229","TIMSP430F5229","TI","MSP430",25,128,0,8,10,10,0,8,53,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,64,"DSBGA|64, VQFN|64",2.21,null,2,null,null,0,null,null,"ACTIVE",null,"UltraLow Power 1.8V SplitRail I/O",0,"N/A"]
["MSP430F5234","TIMSP430F5234","TI","MSP430",25,128,0,8,"Slope",0,0,6,37,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.8,null,2,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 with 128 KB Flash",0,"N/A"]
["MSP430F5239","TIMSP430F5239","TI","MSP430",25,128,0,8,"Slope",0,0,8,53,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",1.85,null,2,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 with 128 KB Flash",0,"N/A"]
["MSP430F5244","TIMSP430F5244","TI","MSP430",25,128,0,8,10,8,0,6,37,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",1.94,null,2,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 with 128 KB Flash",0,"N/A"]
["MSP430F5249","TIMSP430F5249","TI","MSP430",25,128,0,8,10,10,0,8,53,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,64,"VQFN|64",1.98,null,2,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 with 128 KB Flash",0,"N/A"]
["MSP430F5252","TIMSP430F5252","TI","MSP430",25,128,0,16,"Slope",0,0,8,53,"No",4,8,null,"No",4,null,-40,85,1.8,3.6,64,"VQFN|64",2.21,null,4,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 1.8V SplitRail I/O",0,"N/A"]
["MSP430F5253","TIMSP430F5253","TI","MSP430",25,128,0,16,10,10,0,8,53,"No",4,8,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",2.21,null,4,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 1.8V SplitRail I/O",0,"N/A"]
["MSP430F5254","TIMSP430F5254","TI","MSP430",25,128,0,32,"Slope",0,0,8,53,"No",4,8,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",2.21,null,4,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 1.8V SplitRail I/O",0,"N/A"]
["MSP430F5255","TIMSP430F5255","TI","MSP430",25,128,0,32,10,10,0,8,53,"No",4,8,null,"No",4,null,-40,85,1.8,3.6,64,"VQFN|64",2.33,null,4,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 1.8V SplitRail I/O",0,"N/A"]
["MSP430F5256","TIMSP430F5256","TI","MSP430",25,128,0,16,"Slope",0,0,8,53,"No",4,8,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",2.21,null,4,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 1.8V SplitRail I/O",0,"N/A"]
["MSP430F5257","TIMSP430F5257","TI","MSP430",25,128,0,16,10,10,0,8,53,"No",4,8,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",1.89,null,4,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 1.8V SplitRail I/O",0,"N/A"]
["MSP430F5258","TIMSP430F5258","TI","MSP430",25,128,0,32,"Slope",0,0,8,53,"No",4,8,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",2.21,null,4,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 1.8V SplitRail I/O",0,"N/A"]
["MSP430F5259","TIMSP430F5259","TI","MSP430",25,128,0,32,10,10,0,8,53,"No",4,8,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",2.33,null,4,null,null,0,null,null,"ACTIVE",null,"UltraLow Power MSP430 1.8V SplitRail I/O",0,"N/A"]
["MSP430F5328","TIMSP430F5328","TI","MSP430",25,128,0,10,12,10,0,8,47,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80, VQFN|64",2.2400000000000002,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F532x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5329","TIMSP430F5329","TI","MSP430",25,128,0,10,12,14,0,12,63,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"LQFP|80",2.29,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F532x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5333","TIMSP430F5333","TI","MSP430",25,128,0,10,12,12,0,12,74,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",2.48,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F533x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5342","TIMSP430F5342","TI","MSP430",25,128,0,10,12,7,0,5,38,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,48,"VQFN|48",2.29,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F534x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5418A","TIMSP430F5418A","TI","MSP430",25,128,0,16,12,14,0,0,67,"No",2,4,null,"No",3,null,-40,85,1.8,3.6,80,"LQFP|80",2.11,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 128KB Flash, 16KB RAM, 12 Bit ADC, 2 USCIs, 32bit HW Multi",0,"N/A"]
["MSP430F5419A","TIMSP430F5419A","TI","MSP430",25,128,0,16,12,14,0,0,87,"No",4,8,null,"No",3,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",2.2000000000000002,null,4,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 128KB Flash, 16KB RAM, 12 Bit ADC, 4 USCIs, 32bit HW Multi",0,"N/A"]
["MSP430FR5962","TIMSP430FR5962","TI","MSP430",16,128,0,8,12,20,0,16,68,"No",4,8,null,"No",6,null,-40,85,1.8,3.6,64,"LQFP|64, LQFP|80, NFBGA|87, VQFN|48",1.93,null,4,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower MCU with 128 KB FRAM, 8 KB SRAM, AES, 12bit ADC",0,"N/A"]
["MSP430FR5992","TIMSP430FR5992","TI","MSP430",16,128,0,8,12,20,0,16,68,"No",4,8,null,"No",6,null,-40,85,1.8,3.6,64,"LQFP|64, LQFP|80, NFBGA|87, VQFN|48",2.68,null,4,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower MCU With 128 KB FRAM, 8 KB SRAM, LowEnergy Vector Math Accelerator",0,"Low-energy Accelerator"]
["MSP430F5435A","TIMSP430F5435A","TI","MSP430",25,192,0,16,12,14,0,0,67,"No",2,4,null,"No",3,null,-40,85,1.8,3.6,80,"LQFP|80",3.17,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 192KB Flash, 16KB RAM, 12 Bit ADC, 2 USCIs, 32bit HW Multi",0,"N/A"]
["MSP430F5436A","TIMSP430F5436A","TI","MSP430",25,192,0,16,12,14,0,0,87,"No",4,8,null,"No",3,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",2.5099999999999998,null,4,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 192KB Flash, 16KB RAM, 12 Bit ADC, 4 USCIs, 32bit HW Multi",0,"N/A"]
["MSP430BT5190","TIMSP430BT5190","TI","MSP430",16,256,0,16,12,14,0,0,87,"No",4,4,null,"No",3,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",4.3600000000000003,null,0,null,null,0,null,null,"ACTIVE",null,"16bit Microcontroller designed for use with CC2560 TI Bluetooth® Based Solutions",0,"N/A"]
["MSP430F5335","TIMSP430F5335","TI","MSP430",25,256,0,18,12,12,0,12,74,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",2.95,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F533x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F5437A","TIMSP430F5437A","TI","MSP430",25,256,0,16,12,14,0,0,67,"No",2,4,null,"No",3,null,-40,85,1.8,3.6,80,"LQFP|80",2.82,null,2,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 256KB Flash, 16KB RAM, 12 Bit ADC, 2 USCIs, 32bit HW Multi",0,"N/A"]
["MSP430F5438A","TIMSP430F5438A","TI","MSP430",25,256,0,16,12,14,0,0,87,"No",4,8,null,"No",3,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",2.86,null,4,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller, 256KB Flash, 16KB RAM, 12 Bit ADC, 4 USCIs, 32bit HW Multi",0,"N/A"]
["MSP430FR5964","TIMSP430FR5964","TI","MSP430",16,256,0,8,12,20,0,16,68,"No",4,8,null,"No",6,null,-40,85,1.8,3.6,64,"LQFP|64, LQFP|80, NFBGA|87, VQFN|48",2.13,null,4,null,null,0,null,null,"ACTIVE",null,"16 MHz UltraLowPower MCU With 256 KB FRAM, 8 KB SRAM, AES, 12bit ADC​",0,"N/A"]
["MSP430FR5994","TIMSP430FR5994","TI","MSP430",16,256,0,8,12,20,0,16,68,"No",4,8,null,"No",6,null,-40,85,1.8,3.6,64,"LQFP|64, LQFP|80, NFBGA|87, VQFN|48",3.12,null,4,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 256KB FRAM, 8KB SRAM, LEA, AES, 12bit ADC , Comparator, DMA, UART/SPI/I2C, Timer",0,"Low-energy Accelerator"]
["MSP430FR59941","TIMSP430FR59941","TI","MSP430",16,256,0,8,12,20,0,16,68,"No",4,8,null,"No",6,null,-40,85,1.8,3.6,64,"LQFP|64, LQFP|80, NFBGA|87, VQFN|48",3.12,null,4,null,null,0,null,null,"ACTIVE",null,"16 MHz MCU with 256KB FRAM, 8KB SRAM, LEA, AES, 12bit ADC , Comparator, DMA, 68 IO, eUSCI",0,"Low-energy Accelerator"]
["MSP430FE423","TIMSP430FE423","TI","MSP430",25,8,0,0.25,16,3,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",1.62,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller for Energy Meters, 8KB Flash, 256B RAM",0,"N/A"]
["MSP430FE4232","TIMSP430FE4232","TI","MSP430",25,8,0,0.25,16,2,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",1.62,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller for Energy Meters, 8KB Flash, 256B RAM",0,"N/A"]
["MSP430FE423A","TIMSP430FE423A","TI","MSP430",25,8,0,0.25,16,3,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",3.33,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller for Energy Meters, 8KB Flash, 256B RAM",0,"N/A"]
["MSP430FW423","TIMSP430FW423","TI","MSP430",16,8,0,0.125,"Slope",0,0,2,48,"Yes",0,0,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64",1.99,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller for Electronic Flow Meters",0,"Scan Interface"]
["MSP430FE4242","TIMSP430FE4242","TI","MSP430",25,12,0,0.5,16,2,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",2.17,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller for Energy Meters, 12KB Flash, 512B RAM",0,"N/A"]
["MSP430FE425","TIMSP430FE425","TI","MSP430",25,16,0,0.5,16,3,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",4.51,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller for Energy Meters, 16KB Flash, 512B RAM",0,"N/A"]
["MSP430FE4252","TIMSP430FE4252","TI","MSP430",25,16,0,0.5,16,2,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",2.17,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller for Energy Meters, 16KB Flash, 512B RAM",0,"N/A"]
["MSP430FE425A","TIMSP430FE425A","TI","MSP430",25,16,0,0.5,16,3,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",2.17,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller for Energy Meters, 16KB Flash, 512B RAM",0,"N/A"]
["MSP430FW425","TIMSP430FW425","TI","MSP430",16,16,0,0.5,"Slope",0,0,2,48,"Yes",0,0,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64",2.4900000000000002,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller for Electronic Flow Meters",0,"Scan Interface"]
["CC430F6147","TICC430F6147","TI","MSP430",16,32,0,4,10,"  ",0,"  ","  ","Yes",1,1,null,"No",2,null,-40,85,null,null,64,"VQFN|64",2.82,null,1,null,null,0,null,null,"ACTIVE",null,"CC430F614x, CC430F514x, CC430F512x SoC With RF Core",0,"N/A"]
["MSP430FE427","TIMSP430FE427","TI","MSP430",25,32,0,1,16,3,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",4.8,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller for Energy Meters, 32KB Flash, 1024B RAM",0,"N/A"]
["MSP430FE4272","TIMSP430FE4272","TI","MSP430",25,32,0,1,16,2,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",2.21,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller for Energy Meters, 32KB Flash, 1024B RAM",0,"N/A"]
["MSP430FE427A","TIMSP430FE427A","TI","MSP430",25,32,0,1,16,3,0,0,14,"Yes",0,1,null,"No",1,null,-40,85,1.8,3.6,64,"LQFP|64",3.86,null,1,null,null,0,null,null,"ACTIVE",null,"16Bit UltraLowPower Microcontroller for Energy Meters, 32KB Flash, 1024B RAM",0,"N/A"]
["MSP430FW427","TIMSP430FW427","TI","MSP430",16,32,0,1,"Slope",0,0,2,48,"Yes",0,0,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64",2.84,null,0,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller for Electronic Flow Meters",0,"Scan Interface"]
["MSP430F438","TIMSP430F438","TI","MSP430",16,48,0,2,12,12,0,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,80,"LQFP|80",3.62,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430F43x Mixed Signal Microcontroller",0,"N/A"]
["MSP430FR5986","TIMSP430FR5986","TI","MSP430",16,48,0,2,12,12,0,12,48,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64",2.7,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5986 16 MHz ULP Microcontroller featuring 48 KB FRAM, 2 KB SRAM, 48 IO, ADC12, Scan IF, AES",0,"Scan Interface"]
["MSP430FW428","TIMSP430FW428","TI","MSP430",16,48,0,2,"Slope",0,0,2,48,"Yes",0,0,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64",2.62,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430FW42x Mixed Signal Microcontroller",0,"Scan Interface"]
["MSP430F439","TIMSP430F439","TI","MSP430",16,60,0,2,12,12,0,2,48,"Yes",0,1,null,"No",2,null,-40,85,1.8,3.6,80,"LQFP|80",3.76,null,1,null,null,0,null,null,"ACTIVE",null,"MSP430F43x Mixed Signal Microcontroller",0,"N/A"]
["MSP430FW429","TIMSP430FW429","TI","MSP430",16,60,0,2,"Slope",0,0,2,48,"Yes",0,0,null,"No",2,null,-40,85,1.8,3.6,64,"LQFP|64",2.95,null,0,null,null,0,null,null,"ACTIVE",null,"MSP430FW42x Mixed Signal Microcontroller",0,"Scan Interface"]
["MSP430F67621","TIMSP430F67621","TI","MSP430",25,64,0,4,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.35,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F676x1  Low cost 3phase metering SOC",0,"N/A"]
["MSP430F67621A","TIMSP430F67621A","TI","MSP430",25,64,0,4,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",2.35,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F676x1A Polyphase Metering SoCs",0,"N/A"]
["MSP430FR5887","TIMSP430FR5887","TI","MSP430",16,64,0,2,12,12,0,12,48,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",2.54,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5888 16 MHz ULP Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 40 IO, ADC12, Scan IF",0,"Scan Interface"]
["MSP430FR5987","TIMSP430FR5987","TI","MSP430",16,64,0,2,12,12,0,12,48,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",2.54,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5987 16 MHz ULP Microcontroller featuring 64 KB FRAM, 2 KB SRAM, 48 IO, ADC12, Scan IF, AES",0,"Scan Interface"]
["MSP430F6433","TIMSP430F6433","TI","MSP430",25,128,0,10,12,12,0,12,74,"Yes",2,4,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",3.21,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F643x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F67641","TIMSP430F67641","TI","MSP430",25,128,0,8,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",3.08,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F676x1  Low cost 3phase metering SOC",0,"N/A"]
["MSP430F67641A","TIMSP430F67641A","TI","MSP430",25,128,0,8,24,3,0,0,72,"Yes",1,4,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|80",3.08,null,3,null,null,0,null,null,"ACTIVE",null,"MSP430F676x1A Polyphase Metering SoCs",0,"N/A"]
["MSP430FR5889","TIMSP430FR5889","TI","MSP430",16,128,0,2,12,12,0,12,48,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",2.88,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5889 16 MHz ULP Microcontroller featuring 128 KB FRAM, 2 KB SRAM, 40 IO, ADC12, Scan IF",0,"Scan Interface"]
["MSP430FR58891","TIMSP430FR58891","TI","MSP430",16,128,0,2,12,12,0,12,48,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64",3.07,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR58891 Mixed Signal Microcontroller",0,"Scan Interface"]
["MSP430FR5989","TIMSP430FR5989","TI","MSP430",16,128,0,2,12,12,0,12,48,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",2.92,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR5989 16 MHz ULP Microcontroller featuring 128 KB FRAM, 2 KB SRAM, 48 IO, ADC12, Scan IF, AES",0,"Scan Interface"]
["MSP430FR59891","TIMSP430FR59891","TI","MSP430",16,128,0,2,12,12,0,12,48,"Yes",2,4,null,"No",5,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",11.4,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430FR59891 16 MHz ULP Microcontroller featuring 128 KB FRAM, 2 KB SRAM, 48 IO, ADC12, ScanIF, AE",0,"Scan Interface"]
["MSP430FR6035","TIMSP430FR6035","TI","MSP430",16,128,0,8,12,16,0,16,80,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,100,"LQFP|100",2.1800000000000002,null,4,null,null,0,null,null,"ACTIVE",null,"Ultra Low Power MCUs With 128KB FRAM, 12Bit  8 MSPS Sigma Delta ADC, Low Energy Accelerator, AES",0,"Low-energy Accelerator"]
["MSP430FR6045","TIMSP430FR6045","TI","MSP430",16,128,0,8,12,16,0,16,80,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,100,"LQFP|100",8.17,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic MCUs With 128KB FRAM, 12Bit  8 MSPS Sigma Delta ADC, Low Energy Accelerator, AES",0,"Low-energy Accelerator, Ultrasonic Sensing"]
["MSP430F6435","TIMSP430F6435","TI","MSP430",25,256,0,18,12,12,0,12,74,"Yes",2,4,null,"No",4,null,-40,85,1.8,3.6,113,"BGA MICROSTAR JUNIOR|113, LQFP|100",3.54,null,2,null,null,0,null,null,"ACTIVE",null,"MSP430F643x Mixed Signal Microcontroller",0,"N/A"]
["MSP430F6767A","TIMSP430F6767A","TI","MSP430",25,256,0,32,24,6,0,0,90,"Yes",2,6,null,"No",4,null,-40,85,1.8,3.6,100,"LQFP|100, LQFP|128",3.22,null,4,null,null,0,null,null,"ACTIVE",null,"MSP430F6767A Mixed Signal Microcontroller",0,"N/A"]
["MSP430FR6037","TIMSP430FR6037","TI","MSP430",16,256,0,8,12,16,0,16,80,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,100,"LQFP|100",6.26,null,4,null,null,0,null,null,"ACTIVE",null,"Ultra Low Power  MCUs With 256KB FRAM, 12Bit  8 MSPS Sigma Delta ADC, Low Energy Accelerator, AES",0,"Low-energy Accelerator"]
["MSP430FR60371","TIMSP430FR60371","TI","MSP430",16,256,0,8,12,16,0,16,80,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,100,"LQFP|100",2.6,null,4,null,null,0,null,null,"ACTIVE",null,"Ultra Low Power MCUs With 256KB FRAM, 12Bit  8 MSPS Sigma Delta ADC, LEA, AES & IIC Boot Loader",0,"Low-energy Accelerator"]
["MSP430FR6047","TIMSP430FR6047","TI","MSP430",16,256,0,8,12,16,0,16,80,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,100,"LQFP|100",8.7899999999999991,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic MCUs With 256KB FRAM, 12Bit  8 MSPS Sigma Delta ADC, Low Energy Accelerator, AES",0,"Low-energy Accelerator, Ultrasonic Sensing"]
["MSP430FR60471","TIMSP430FR60471","TI","MSP430",16,256,0,8,12,16,0,16,80,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,100,"LQFP|100",8.7899999999999991,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic MCUs With 256KB FRAM, 12Bit  8 MSPS Sigma Delta ADC, LEA, AES & IIC Boot Loader",0,"Low-energy Accelerator, Ultrasonic Sensing"]
["MSP430FR6005","TIMSP430FR6005","TI","MSP430",16,128,0,8,12,16,0,16,81,"No",2,4,null,"No",6,"RTC, CRC",-40,105,1.8,3.6,100,"LQFP|100",4.5,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic Sensing MCU with 128KB FRAM, 8KB RAM, LCD  for water meters",0,"Ultrasonic Sensing"]
["MSP430F2274-EP","TIMSP430F2274EP","TI","MSP430",16,32,0,1,10,12,0,0,32,"No",1,1,null,"No",2,null,-55,125,1.8,3.6,38,"TSSOP|38, VQFN|40",5.99,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Micro controller, 32kB Flash, 1K RAM",2,"N/A"]
["MSP430F2234","TIMSP430F2234","TI","MSP430",16,8,0,0.5,10,12,0,0,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.63,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 8KB Flash, 512B RAM",2,"N/A"]
["MSP430F2254","TIMSP430F2254","TI","MSP430",16,16,0,0.5,10,12,0,0,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,38,"TSSOP|38, VQFN|40",1.89,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 16KB Flash, 512B RAM",2,"N/A"]
["MSP430F2274","TIMSP430F2274","TI","MSP430",16,32,0,1,10,12,0,0,32,"No",1,1,null,"No",2,null,-40,85,1.8,3.6,49,"DSBGA|49, TSSOP|38, VQFN|40",2.2000000000000002,null,1,null,null,0,null,null,"ACTIVE",null,"16bit UltraLowPower Microcontroller, 32KB Flash, 1K RAM",2,"N/A"]
["MSP432P401M","TIMSP432P401M","TI","ARM CM4F",48,128,0,32,14,24,0,16,84,"No",4,8,null,"No",6,null,-40,85,1.62,3.7,100,"LQFP|100, NFBGA|80, VQFN|64",null,null,4,80,0.66,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU With Precision ADC, 128KB Flash and 32KB RAM",0,"N/A"]
["MSP432P401R","TIMSP432P401R","TI","ARM CM4F",48,256,0,64,14,24,0,2,84,"No",4,8,null,"No",6,null,-40,85,1.62,3.7,100,"LQFP|100, NFBGA|80, VQFN|64",null,null,4,80,0.66,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU With Precision ADC, 256KB Flash and 64KB RAM",0,"N/A"]
["MSP432P401V","TIMSP432P401V","TI","ARM CM4F",48,512,0,128,14,12,0,2,48,"No",3,6,null,"No",5,null,-40,85,1.62,3.7,64,"VQFN|64",null,null,3,100,0.82,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 512KB Flash and 128KB RAM",0,"N/A"]
["MSP432P401VT","TIMSP432P401VT","TI","ARM CM4F",24,512,0,128,14,12,0,2,48,"No",3,6,null,"No",5,null,-40,105,1.62,3.7,64,"VQFN|64",null,null,3,100,14.4,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 512KB Flash and 128KB RAM",0,"N/A"]
["MSP432P401Y","TIMSP432P401Y","TI","ARM CM4F",48,1024,0,256,14,12,0,2,48,"No",3,6,null,"No",5,null,-40,85,1.62,3.7,64,"VQFN|64",null,null,3,100,0.82,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 1MB Flash and 256KB RAM",0,"N/A"]
["MSP432P401YT","TIMSP432P401YT","TI","ARM CM4F",24,1024,0,256,14,12,0,2,48,"No",3,6,null,"No",5,null,-40,105,1.62,3.7,64,"VQFN|64",null,null,3,100,14.4,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 1MB Flash and 256KB RAM",0,"N/A"]
["MSP432P4011","TIMSP432P4011","TI","ARM CM4F",48,2048,0,256,14,12,0,2,48,"No",3,6,null,"No",5,null,-40,85,1.62,3.7,64,"VQFN|64",null,null,3,100,0.82,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 2MB Flash and 256KB RAM",0,"N/A"]
["MSP432P4011T","TIMSP432P4011T","TI","ARM CM4F",24,2048,0,256,14,12,0,2,48,"No",3,6,null,"No",5,null,-40,105,1.62,3.7,64,"VQFN|64",null,null,3,100,14.4,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 2MB Flash and 256KB RAM",0,"N/A"]
["MSP432P411V","TIMSP432P411V","TI","ARM CM4F",48,512,0,128,14,24,0,2,84,"Yes",4,8,null,"No",6,null,-40,85,1.62,3.7,100,"LQFP|100",null,null,4,100,0.82,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 512KB Flash and 128KB RAM",0,"N/A"]
["MSP432P411VT","TIMSP432P411VT","TI","ARM CM4F",24,512,0,128,14,24,0,2,84,"Yes",4,8,null,"No",6,null,-40,105,1.62,3.7,100,"LQFP|100",null,null,4,100,14.4,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 512KB Flash and 128KB RAM",0,"N/A"]
["MSP432P411Y","TIMSP432P411Y","TI","ARM CM4F",48,1024,0,256,14,24,0,2,84,"Yes",4,8,null,"No",6,null,-40,85,1.62,3.7,100,"LQFP|100",null,null,4,100,0.82,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 1MB Flash and 256KB RAM",0,"N/A"]
["MSP432P411YT","TIMSP432P411YT","TI","ARM CM4F",24,1025,0,256,14,24,0,2,84,"Yes",4,8,null,"No",6,null,-40,105,1.62,3.7,100,"LQFP|100",null,null,4,100,14.4,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 1MB Flash and 256KB RAM",0,"N/A"]
["MSP432P4111","TIMSP432P4111","TI","ARM CM4F",48,2048,0,256,14,24,0,2,84,"Yes",4,8,null,"No",6,null,-40,85,1.62,3.7,100,"LQFP|100",null,null,4,100,0.82,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 2MB Flash and 256KB RAM",0,"N/A"]
["MSP432P4111T","TIMSP432P4111T","TI","ARM CM4F",24,2048,0,256,14,24,0,2,84,"Yes",4,8,null,"No",6,null,-40,105,1.62,3.7,100,"LQFP|100",null,null,4,100,14.4,null,null,null,null,null,"SimpleLink UltraLowPower 32Bit ARM CM4F MCU with Precision ADC, 2MB Flash and 256KB RAM",0,"N/A"]
["MSP430FR6041","TIMSP430FR6041","TI","MSP430",16,32,0,12,12,8,0,12,57,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,80,"LQFP|80",4.68,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic Sensing MCU with 32KB FRAM, 12KB RAM, LCD  for gas and water metering applications",0,"Low-energy Accelerator, Ultrasonic Sensing"]
["MSP430FR6043","TIMSP430FR6043","TI","MSP430",16,64,0,12,12,8,0,12,57,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,80,"LQFP|80",6.34,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic Sensing MCU with 64KB FRAM, 12KB RAM, LCD  for gas and water metering applications",0,"Low-energy Accelerator, Ultrasonic Sensing"]
["MSP430FR60431","TIMSP430FR60431","TI","MSP430",16,64,0,12,12,8,0,12,57,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,80,"LQFP|80",6.34,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic Sensing MCU with 64KB FRAM, 12KB RAM, LCD, I2C Bootloader  for flow meters",0,"Low-energy Accelerator, Ultrasonic Sensing"]
["MSP430FR2532","TIMSP430FR2532","TI","MSP430",16,8,0,1,10,8,0,"  ",15,"No",1,1,null,"No",4,null,-40,85,1.8,3.6,24,"VQFN|24",1.01,null,2,null,null,8,null,null,"ACTIVE",null,"16 MHz UltraLowPower Microcontroller With 8 KB FRAM, CapTIvate Touch Technology",0,"N/A"]
["MSP430FR2475","TIMSP430FR2475","TI","MSP430",16,32,0,4,12,12,0,4,43,"No",2,4,null,"No",5,null,-40,105,1.8,3.6,48,"LQFP|48, VQFN|32, VQFN|40",1.19,null,2,null,null,0,null,null,"ACTIVE",null,"16 MHz ultralowpower microcontroller with 32 KB FRAM, 4 KB RAM, 12bit ADC, 43 IO, 5 16bit timers",0,"N/A"]
["MSP430FR2675","TIMSP430FR2675","TI","MSP430",16,32,0,6,12,12,0,4,43,"No",2,4,null,"No",5,null,-40,105,1.8,3.6,48,"LQFP|48, VQFN|32, VQFN|40",1.28,null,2,null,null,16,null,null,"ACTIVE",null,"CapTIvate™ capacitive touch sensing microcontroller with 32KB FRAM, 6KB SRAM, 43 IO, 12bit ADC",0,"N/A"]
["MSP430FR2476","TIMSP430FR2476","TI","MSP430",16,64,0,8,12,12,0,4,43,"No",2,4,null,"No",5,null,-40,105,1.8,3.6,48,"LQFP|48, VQFN|32, VQFN|40",0.83,null,2,null,null,0,null,null,"ACTIVE",null,"16 MHz ultralowpower microcontroller with 64 KB FRAM, 8 KB RAM, 12bit ADC, 43 IO, 5 16bit timers",0,"N/A"]
["MSP430FR2676","TIMSP430FR2676","TI","MSP430",16,64,0,8,12,12,0,4,43,"No",2,4,null,"No",5,null,-40,105,1.8,3.6,48,"LQFP|48, VQFN|32, VQFN|40",1.4,null,2,null,null,16,null,null,"ACTIVE",null,"CapTIvate™ capacitive touch sensing microcontroller with 64KB FRAM, 8KB SRAM, 43 IO, 12bit ADC",0,"N/A"]
["MSP430FR5041","TIMSP430FR5041","TI","MSP430",16,32,0,12,12,8,0,12,44,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",4.66,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic Sensing MCU with 32KB FRAM, 12KB RAM for gas and water metering applications",0,"Low-energy Accelerator, Ultrasonic Sensing"]
["MSP430FR5043","TIMSP430FR5043","TI","MSP430",16,64,0,12,12,8,0,12,44,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",5.94,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic Sensing MCU with 64KB FRAM, 12KB RAM for gas and water metering applications",0,"Low-energy Accelerator, Ultrasonic Sensing"]
["MSP430FR50431","TIMSP430FR50431","TI","MSP430",16,64,0,12,12,8,0,12,44,"Yes",2,6,null,"No",6,null,-40,85,1.8,3.6,64,"LQFP|64, VQFN|64",5.94,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic Sensing MCU with 64KB FRAM, 12KB RAM, I2C Boot Loader for flow meters",0,"Low-energy Accelerator, Ultrasonic Sensing"]
["MSP430FR6007","TIMSP430FR6007","TI","MSP430",16,256,0,1,12,16,0,16,81,"No",2,4,null,"No",6,"RTC, CRC",-40,105,1.8,3.6,100,"LQFP|100",5,null,4,null,null,0,null,null,"ACTIVE",null,"Ultrasonic Sensing MCU with 256KB FRAM, 8KB RAM, LCD  for water meters",0,"Ultrasonic Sensing"]
["MSP430FR2673","TIMSP430FR2673","TI","MSP430",16,16,0,4,12,8,0,4,27,"No",2,4,null,"No",5,"RTC, CRC",-40,105,1.8,3.6,32,"VQFN|32",1.1499999999999999,null,2,null,16,16,null,null,"ACTIVE",null,"Capacitive-touch MCU with 16 I/O (64 sensors), 16-KB FRAM, 4-KB SRAM, 27 I/O and 12-bit ADC",0,"N/A"]
["MSP430FR2672","TIMSP430FR2672","TI","MSP430",16,8,0,2,12,8,0,4,27,"No",2,4,null,"No",5,"RTC, CRC",-40,105,1.8,3.6,32,"VQFN|32",1.05,null,2,null,16,16,null,null,"ACTIVE",null,"Capacitive-touch MCU with 16 I/O (16 sensors), 8-KB FRAM, 2-KB SRAM, 27 I/O and 12-bit ADC",0,"N/A"]
["MSP430F5227","TIMSP430F5227","TI","MSP430",25,64,0,8,10,12,0,8,53,"No",2,4,null,"No",4,null,-40,85,1.8,3.6,80,"BGA MICROSTAR JUNIOR|80",null,null,2,null,null,null,null,null,null,null,"UltraLow Power 1.8V SplitRail I/O",0,"N/A"]

{"sheet":"Parametric","index":3,"n_rows":25,"n_cols":4,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["Filter Priority","Filter Enable","RangeMinus","RangePlus"]
["NVM/kB",true,0,8]
["PIN count",false,10,4]
["LCD",false,0,0]
["USB",false,0,0]
["Cap Touch",false,0,8]
["ADC Resolution",false,0,2]
["ADC Channel #",false,2,8]
["DAC",false,0,4]
["OPA",false,1,4]
["UART",false,2,4]
["SPI",false,2,4]
["I2C",false,2,4]
["I2S",false,2,2]
["CAN",false,2,2]
["Timer",false,1,4]
["Price",false,0.5,3]
["IO count",true,5,10]
["RAM/kB",false,4,16]
["Package",false,0,0]
["Vmin/V",false,1,1]
["Vmax/V",false,1,1]
["Tempmin",false,0,0]
["Tempmax",false,0,0]
["COMP",false,0,2]