
RM44 – Only 5A5A5A5A location @ 0xF0404F44:



RM46 after CAN Update: