Hi Sunil,

Yes, I have undergone the example of hetPWM.c

I have a doubt in HALCoGen configuration in HET1 Tab,



This Pin 8 is refers to HET1[8] or HET1[0] because it says PWM 0 and Pin 8.



And also Dir should be selected for output is it correct



How to configure the particular frequency and its formula ?

Thank you in advance.