|  | # # Hercules Safety Microcontrollers

| ##
### ### Key benefits | ### Key benefits | ### Key applications
--- | --- | ---
Up to 160 MHz, ARM Cortex-R4F CPU Lock-Step CPUs with fail safe detection logic Up to 2 MB of Embedded Flash Memory with ECC Dual 12-bit ADC, 8 redundant channels FlexRay, CAN, LIN, Multi-Buffered SPIs, and DMA Timer Co-Processer for PWM and input capture Package options: 144 QFP and 337 BGA | Architected for safety critical transportation applications ARM Cortex-R4F with Floating Point (single and double precision) Automotive qualified across full temperature range Flexible real-time control peripherals Robust communication interfaces Development network and support | Braking systems (ABS and ESC) Electric power steering (EPS) HEV/EV inverter systems Battery management systems Active driver assistance systems Aerospace and avionics Railway communications Off road vehicles

#  | ### Copyright © 2013 Texas Instruments Incorporated. All rights reserved.