- Errata: Synchronization loss ???
- Transmits large file in 1024 Byte chunks over socket
- sometimes occur 0 length IQR between the blocks which are cleared
- one interrupt occurs during DMA transfer and cannot served
- chip hangs afterwards, not responding to any commands
