

# How are you sending data from the CC3200 AP to the PC? Is it a TCP socket?


Tcp socket


# Step 1 Set PIN55/57 for Uart,and set PIN62 for NWP logs according to the Application document



# Step 2 set Terminal Property








# Step 3 Capture the running log

The UART 0 , print the log When the system transmission is abnormal can be as listed the figure



The NWP log is in the file teraterm0617.log