/*
 * Copyright (C) 2012 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
/dts-v1/;

#include "am33xx.dtsi"
#include "am335x-bone-common.dtsi"
#include <dt-bindings/display/tda998x.h>

/ {
	model = "TI AM335x BeagleBone Black";
	compatible = "ti,am335x-bone-black", "ti,am335x-bone", "ti,am33xx";
};

&ldo3_reg {
	regulator-min-microvolt = <1800000>;
	regulator-max-microvolt = <1800000>;
	regulator-always-on;
};

&mmc1 {
	vmmc-supply = <&vmmcsd_fixed>;
};

/*&mmc2 {
	vmmc-supply = <&vmmcsd_fixed>;
	pinctrl-names = "default";
	pinctrl-0 = <&emmc_pins>;
	bus-width = <8>;
	status = "okay";
};*/

&cpu0_opp_table {
	/*
	 * All PG 2.0 silicon may not support 1GHz but some of the early
	 * BeagleBone Blacks have PG 2.0 silicon which is guaranteed
	 * to support 1GHz OPP so enable it for PG 2.0 on this board.
	 */
	oppnitro@1000000000 {
		opp-supported-hw = <0x06 0x0100>;
	};
};

&am33xx_pinmux {
	nxp_hdmi_bonelt_pins: nxp_hdmi_bonelt_pins {
		pinctrl-single,pins = <
			AM33XX_IOPAD(0x9b0, PIN_OUTPUT_PULLDOWN | MUX_MODE3)	/* xdma_event_intr0 */
			AM33XX_IOPAD(0x8a0, PIN_OUTPUT | MUX_MODE0)		/* lcd_data0.lcd_data0 */
			AM33XX_IOPAD(0x8a4, PIN_OUTPUT | MUX_MODE0)		/* lcd_data1.lcd_data1 */
			AM33XX_IOPAD(0x8a8, PIN_OUTPUT | MUX_MODE0)		/* lcd_data2.lcd_data2 */
			AM33XX_IOPAD(0x8ac, PIN_OUTPUT | MUX_MODE0)		/* lcd_data3.lcd_data3 */
			AM33XX_IOPAD(0x8b0, PIN_OUTPUT | MUX_MODE0)		/* lcd_data4.lcd_data4 */
			AM33XX_IOPAD(0x8b4, PIN_OUTPUT | MUX_MODE0)		/* lcd_data5.lcd_data5 */
			AM33XX_IOPAD(0x8b8, PIN_OUTPUT | MUX_MODE0)		/* lcd_data6.lcd_data6 */
			AM33XX_IOPAD(0x8bc, PIN_OUTPUT | MUX_MODE0)		/* lcd_data7.lcd_data7 */
			AM33XX_IOPAD(0x8c0, PIN_OUTPUT | MUX_MODE0)		/* lcd_data8.lcd_data8 */
			AM33XX_IOPAD(0x8c4, PIN_OUTPUT | MUX_MODE0)		/* lcd_data9.lcd_data9 */
			AM33XX_IOPAD(0x8c8, PIN_OUTPUT | MUX_MODE0)		/* lcd_data10.lcd_data10 */
			AM33XX_IOPAD(0x8cc, PIN_OUTPUT | MUX_MODE0)		/* lcd_data11.lcd_data11 */
			AM33XX_IOPAD(0x8d0, PIN_OUTPUT | MUX_MODE0)		/* lcd_data12.lcd_data12 */
			AM33XX_IOPAD(0x8d4, PIN_OUTPUT | MUX_MODE0)		/* lcd_data13.lcd_data13 */
			AM33XX_IOPAD(0x8d8, PIN_OUTPUT | MUX_MODE0)		/* lcd_data14.lcd_data14 */
			AM33XX_IOPAD(0x8dc, PIN_OUTPUT | MUX_MODE0)		/* lcd_data15.lcd_data15 */
			AM33XX_IOPAD(0x8e0, PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* lcd_vsync.lcd_vsync */
			AM33XX_IOPAD(0x8e4, PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* lcd_hsync.lcd_hsync */
			AM33XX_IOPAD(0x8e8, PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* lcd_pclk.lcd_pclk */
			AM33XX_IOPAD(0x8ec, PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* lcd_ac_bias_en.lcd_ac_bias_en */
		>;
	};
	nxp_hdmi_bonelt_off_pins: nxp_hdmi_bonelt_off_pins {
		pinctrl-single,pins = <
			AM33XX_IOPAD(0x9b0, PIN_OUTPUT_PULLDOWN | MUX_MODE3)	/* xdma_event_intr0 */
		>;
	};

	mcasp0_pins: mcasp0_pins {
		pinctrl-single,pins = <
			AM33XX_IOPAD(0x9ac, PIN_INPUT_PULLUP | MUX_MODE0) /* mcasp0_ahcklx.mcasp0_ahclkx */
			AM33XX_IOPAD(0x99c, PIN_OUTPUT_PULLDOWN | MUX_MODE2) /* mcasp0_ahclkr.mcasp0_axr2*/
			AM33XX_IOPAD(0x994, PIN_OUTPUT_PULLUP | MUX_MODE0) /* mcasp0_fsx.mcasp0_fsx */
			AM33XX_IOPAD(0x990, PIN_OUTPUT_PULLDOWN | MUX_MODE0) /* mcasp0_aclkx.mcasp0_aclkx */
			AM33XX_IOPAD(0x86c, PIN_OUTPUT_PULLDOWN | MUX_MODE7) /* gpmc_a11.GPIO1_27 */
		>;
	};
};

&lcdc {
	status = "okay";

	/* If you want to get 24 bit RGB and 16 BGR mode instead of
	 * current 16 bit RGB and 24 BGR modes, set the propety
	 * below to "crossed" and uncomment the video-ports -property
	 * in tda19988 node.
	 */
	blue-and-red-wiring = "straight";

	port {
		lcdc_0: endpoint@0 {
			remote-endpoint = <&hdmi_0>;
		};
	};
};

&i2c0 {
	tda19988: tda19988 {
		compatible = "nxp,tda998x";
		reg = <0x70>;

		pinctrl-names = "default", "off";
		pinctrl-0 = <&nxp_hdmi_bonelt_pins>;
		pinctrl-1 = <&nxp_hdmi_bonelt_off_pins>;

		/* Convert 24bit BGR to RGB, e.g. cross red and blue wiring */
		/* video-ports = <0x234501>; */

		#sound-dai-cells = <0>;
		audio-ports = <	TDA998x_I2S	0x03>;

		ports {
			port@0 {
				hdmi_0: endpoint@0 {
					remote-endpoint = <&lcdc_0>;
				};
			};
		};
	};
};

&rtc {
	system-power-controller;
};

&mcasp0	{
	#sound-dai-cells = <0>;
	pinctrl-names = "default";
	pinctrl-0 = <&mcasp0_pins>;
	status = "okay";
	op-mode = <0>;	/* MCASP_IIS_MODE */
	tdm-slots = <2>;
	serial-dir = <	/* 0: INACTIVE, 1: TX, 2: RX */
			0 0 1 0
		>;
	tx-num-evt = <32>;
	rx-num-evt = <32>;
};

&sgx {
	status = "okay";
};

/ {
	clk_mcasp0_fixed: clk_mcasp0_fixed {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <24576000>;
	};

	clk_mcasp0: clk_mcasp0 {
		#clock-cells = <0>;
		compatible = "gpio-gate-clock";
		clocks = <&clk_mcasp0_fixed>;
		enable-gpios = <&gpio1 27 0>; /* BeagleBone Black Clk enable on GPIO1_27 */
	};

	sound {
		compatible = "simple-audio-card";
		simple-audio-card,name = "TI BeagleBone Black";
		simple-audio-card,format = "i2s";
		simple-audio-card,bitclock-master = <&dailink0_master>;
		simple-audio-card,frame-master = <&dailink0_master>;

		dailink0_master: simple-audio-card,cpu {
			sound-dai = <&mcasp0>;
			clocks = <&clk_mcasp0>;
		};

		simple-audio-card,codec {
			sound-dai = <&tda19988>;
		};
	};

};

/* Overlay the wilink8 based cape support */
#include "am335x-bone-e14-wl1837.dtsi"
