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Wlan_start initial sequence:
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Wlan_start initial sequence - HOST_SYNC_PATTERN   0x5C5C5C5C observed after some time – Does this part of ctrlCmdFw_WLSendCommand?
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