# QuickTrack Test Tool Report

## DUT Information

DUT Type | Station
DUT Vendor Name |
DUT Vendor ID |

## Test Result

Test ID | TestCaseName | Test Result
--- | --- | ---
376 | CT_Security_PMF_STA_CCMP-ProtectedUnicastMgmtFrames-CorrectProtDisassoc_10084_1 | PASS

## Test Measurements

TestCaseName: CT_Security_PMF_STA_CCMP-ProtectedUnicastMgmtFrames-CorrectProtDisassoc_10084_1
TestResult:PASS
Band:2.4GHz

Measurements Name | Description | Value | Validation Result
--- | --- | --- | ---
IS_CONNECTED | STAUT connection status with the AP | true | PASS
DATA_PACKET_RECEIVED | The percentage of Data packets received from the STAUT | 0.0 | PASS