[11:50:45.072838]	Beacon Request	03-08-95-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 1
	Protocol: ZigBee
	Timestamp: 11:50:45.072838
	Time Delta: 4.516568
	Channel: 13
	Length: 10
	Link Quality: -29 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF950803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 149
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.075086]	Beacon	00-80-E5-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 2
	Protocol: ZigBee
	Timestamp: 11:50:45.075086
	Time Delta: 0.002248
	Channel: 13
	Length: 28
	Link Quality: -28 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFE58000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 229
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.076510]	Beacon	00-80-67-43-7F-7B-64-FF-0F-00-00-00-22-9C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 3
	Protocol: ZigBee
	Timestamp: 11:50:45.076510
	Time Delta: 0.001424
	Channel: 13
	Length: 28
	Link Quality: -45 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x647B7F43678000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 103
	Source PAN ID: 0x7F43
	Source Address: 0x647B
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.078758]	Beacon	00-80-3E-43-7F-0A-F0-FF-0F-00-00-00-22-A4-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 4
	Protocol: ZigBee
	Timestamp: 11:50:45.078758
	Time Delta: 0.002248
	Channel: 13
	Length: 28
	Link Quality: -43 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xF00A7F433E8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 62
	Source PAN ID: 0x7F43
	Source Address: 0xF00A
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0xA422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·010 0··· ···· ···· = Device Depth: 0x4
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.080286]	Beacon	00-80-64-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 5
	Protocol: ZigBee
	Timestamp: 11:50:45.080286
	Time Delta: 0.001528
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F43648000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 100
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.445742]	Link Status	41-88-4A-43-7F-FF-FF-7B-64-09-10-FC-FF-7B-64-01-3D-F9-AA-C6-01-00-4B-12-00-08-63-68-33-11-9C-D9-11-0A-F0-11-FF-FF
Frame Information: (38 bytes)
	Packet Number: 6
	Protocol: ZigBee
	Timestamp: 11:50:45.445742
	Time Delta: 0.365456
	Channel: 13
	Length: 38
	Link Quality: -44 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 74
	Destination PAN ID: 0x7F43
	Destination Address: 0xFFFF
	Source Address: 0x647B
MAC Payload: (27 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x647B
		Radius: 0x01
		Sequence Number: 61
		Source IEEE Address: 00:12:4B:00:01:C6:AA:F9
	NWK Payload: (11 bytes)
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x63
			···0 0011 = Entry Count: 0x3
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: (9 bytes)
			Entry 0: 0x113368
				Neighbor Network Address: 0x3368
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11D99C
				Neighbor Network Address: 0xD99C
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 2: 0x11F00A
				Neighbor Network Address: 0xF00A
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.479062]	Rejoin Request	61-88-9A-17-F8-E0-7A-4D-A4-09-10-E0-7A-4D-A4-01-AE-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 7
	Protocol: ZigBee
	Timestamp: 11:50:45.479062
	Time Delta: 0.033320
	Channel: 13
	Length: 29
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 154
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x7AE0
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 174
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.482366]	Rejoin Request	61-88-9A-17-F8-E0-7A-4D-A4-09-10-E0-7A-4D-A4-01-AE-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 8
	Protocol: ZigBee
	Timestamp: 11:50:45.482366
	Time Delta: 0.003304
	Channel: 13
	Length: 29
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 154
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x7AE0
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 174
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.486350]	Rejoin Request	61-88-9A-17-F8-E0-7A-4D-A4-09-10-E0-7A-4D-A4-01-AE-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 9
	Protocol: ZigBee
	Timestamp: 11:50:45.486350
	Time Delta: 0.003984
	Channel: 13
	Length: 29
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 154
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x7AE0
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 174
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.490310]	Rejoin Request	61-88-9A-17-F8-E0-7A-4D-A4-09-10-E0-7A-4D-A4-01-AE-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 10
	Protocol: ZigBee
	Timestamp: 11:50:45.490310
	Time Delta: 0.003960
	Channel: 13
	Length: 29
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 154
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x7AE0
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 174
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.496766]	Rejoin Request	61-88-9B-17-F8-E0-7A-4D-A4-09-10-E0-7A-4D-A4-01-AE-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 11
	Protocol: ZigBee
	Timestamp: 11:50:45.496766
	Time Delta: 0.006456
	Channel: 13
	Length: 29
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 155
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x7AE0
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 174
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.500094]	Rejoin Request	61-88-9B-17-F8-E0-7A-4D-A4-09-10-E0-7A-4D-A4-01-AE-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 12
	Protocol: ZigBee
	Timestamp: 11:50:45.500094
	Time Delta: 0.003328
	Channel: 13
	Length: 29
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 155
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x7AE0
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 174
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.504046]	Rejoin Request	61-88-9B-17-F8-E0-7A-4D-A4-09-10-E0-7A-4D-A4-01-AE-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 13
	Protocol: ZigBee
	Timestamp: 11:50:45.504046
	Time Delta: 0.003952
	Channel: 13
	Length: 29
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 155
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x7AE0
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 174
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.507998]	Rejoin Request	61-88-9B-17-F8-E0-7A-4D-A4-09-10-E0-7A-4D-A4-01-AE-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 14
	Protocol: ZigBee
	Timestamp: 11:50:45.507998
	Time Delta: 0.003952
	Channel: 13
	Length: 29
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 155
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x7AE0
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 174
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.914102]	Data Request	63-88-9C-17-F8-E0-7A-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 15
	Protocol: ZigBee
	Timestamp: 11:50:45.914102
	Time Delta: 0.406104
	Channel: 13
	Length: 12
	Link Quality: -27 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 156
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.916566]	Data Request	63-88-9C-17-F8-E0-7A-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 16
	Protocol: ZigBee
	Timestamp: 11:50:45.916566
	Time Delta: 0.002464
	Channel: 13
	Length: 12
	Link Quality: -27 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 156
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.920654]	Data Request	63-88-9C-17-F8-E0-7A-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 17
	Protocol: ZigBee
	Timestamp: 11:50:45.920654
	Time Delta: 0.004088
	Channel: 13
	Length: 12
	Link Quality: -27 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 156
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.924382]	Data Request	63-88-9C-17-F8-E0-7A-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 18
	Protocol: ZigBee
	Timestamp: 11:50:45.924382
	Time Delta: 0.003728
	Channel: 13
	Length: 12
	Link Quality: -27 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 156
	Destination PAN ID: 0xF817
	Destination Address: 0x7AE0
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.933062]	Orphan Notification	43-C8-9D-FF-FF-FF-FF-F0-BC-8D-01-00-4B-12-00-06-FF-FF
Frame Information: (18 bytes)
	Packet Number: 19
	Protocol: ZigBee
	Timestamp: 11:50:45.933062
	Time Delta: 0.008680
	Channel: 13
	Length: 18
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (15 bytes)
	Frame Control: 0xC843
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		11·· ···· ···· ···· = Source Addr Mode: [0x3] 64-bit Extended Address
	Sequence Number: 157
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
	Source Address: 00:12:4B:00:01:8D:BC:F0
MAC Payload: 0x06
	Command Frame ID: [0x06] Orphan Notification
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.941262]	Coordinator Realignment	23-CC-94-FF-FF-F0-BC-8D-01-00-4B-12-00-43-7F-E1-2A-70-02-00-4B-12-00-08-43-7F-68-33-0D-35-64-FF-FF
Frame Information: (33 bytes)
	Packet Number: 20
	Protocol: ZigBee
	Timestamp: 11:50:45.941262
	Time Delta: 0.008200
	Channel: 13
	Length: 33
	Link Quality: -58 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (23 bytes)
	Frame Control: 0xCC23
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 11·· ···· ···· = Destination Addr Mode: [0x3] 64-bit Extended Address
		··00 ···· ···· ···· = Reserved: 0x0
		11·· ···· ···· ···· = Source Addr Mode: [0x3] 64-bit Extended Address
	Sequence Number: 148
	Destination PAN ID: 0xFFFF
	Destination Address: 00:12:4B:00:01:8D:BC:F0
	Source PAN ID: 0x7F43
	Source Address: 00:12:4B:00:02:70:2A:E1
MAC Payload: 0x64350D33687F4308
	Command Frame ID: [0x08] Coordinator Realignment
	Command Payload: 0x64350D33687F43
		Re-PAN ID: 0x7F43
		Re-Coordinator Short Address: 0x3368
		Re-Logical Channel: 0x0D
		Re-Short Address: 0x6435
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:45.942702]	Acknowledgement	02-00-94-FF-FF
Frame Information: (5 bytes)
	Packet Number: 21
	Protocol: ZigBee
	Timestamp: 11:50:45.942702
	Time Delta: 0.001440
	Channel: 13
	Length: 5
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0x940002
	Frame Control: 0x0002
		···· ···· ···· ·010 = Frame Type: [0x2] Acknowledgement
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 148
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.124822]	Beacon Request	03-08-9E-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 22
	Protocol: ZigBee
	Timestamp: 11:50:46.124822
	Time Delta: 0.182120
	Channel: 13
	Length: 10
	Link Quality: -27 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF9E0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 158
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.127214]	Beacon	00-80-E6-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 23
	Protocol: ZigBee
	Timestamp: 11:50:46.127214
	Time Delta: 0.002392
	Channel: 13
	Length: 28
	Link Quality: -28 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFE68000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 230
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.128574]	Beacon	00-80-65-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 24
	Protocol: ZigBee
	Timestamp: 11:50:46.128574
	Time Delta: 0.001360
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F43658000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 101
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.131358]	Beacon	00-80-68-43-7F-7B-64-FF-0F-00-00-00-22-9C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 25
	Protocol: ZigBee
	Timestamp: 11:50:46.131358
	Time Delta: 0.002784
	Channel: 13
	Length: 28
	Link Quality: -44 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x647B7F43688000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 104
	Source PAN ID: 0x7F43
	Source Address: 0x647B
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.133214]	Beacon	00-80-6D-43-7F-68-33-FF-0F-00-00-00-22-8C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 26
	Protocol: ZigBee
	Timestamp: 11:50:46.133214
	Time Delta: 0.001856
	Channel: 13
	Length: 28
	Link Quality: -56 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x33687F436D8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 109
	Source PAN ID: 0x7F43
	Source Address: 0x3368
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 1··· ···· ···· = Device Depth: 0x1
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.140822]	Beacon	00-80-3F-43-7F-0A-F0-FF-0F-00-00-00-22-A4-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 27
	Protocol: ZigBee
	Timestamp: 11:50:46.140822
	Time Delta: 0.007608
	Channel: 13
	Length: 28
	Link Quality: -42 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xF00A7F433F8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 63
	Source PAN ID: 0x7F43
	Source Address: 0xF00A
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0xA422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·010 0··· ···· ···· = Device Depth: 0x4
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.768454]	Beacon Request	03-08-A3-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 28
	Protocol: ZigBee
	Timestamp: 11:50:46.768454
	Time Delta: 0.627632
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFA30803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 163
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.770622]	Beacon	00-80-6E-43-7F-68-33-FF-0F-00-00-00-22-8C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 29
	Protocol: ZigBee
	Timestamp: 11:50:46.770622
	Time Delta: 0.002168
	Channel: 13
	Length: 28
	Link Quality: -55 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x33687F436E8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 110
	Source PAN ID: 0x7F43
	Source Address: 0x3368
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 1··· ···· ···· = Device Depth: 0x1
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.772190]	Beacon	00-80-66-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 30
	Protocol: ZigBee
	Timestamp: 11:50:46.772190
	Time Delta: 0.001568
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F43668000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 102
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.776022]	Beacon	00-80-E7-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 31
	Protocol: ZigBee
	Timestamp: 11:50:46.776022
	Time Delta: 0.003832
	Channel: 13
	Length: 28
	Link Quality: -28 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFE78000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 231
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.777622]	Beacon	00-80-40-43-7F-0A-F0-FF-0F-00-00-00-22-A4-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 32
	Protocol: ZigBee
	Timestamp: 11:50:46.777622
	Time Delta: 0.001600
	Channel: 13
	Length: 28
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xF00A7F43408000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 64
	Source PAN ID: 0x7F43
	Source Address: 0xF00A
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0xA422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·010 0··· ···· ···· = Device Depth: 0x4
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:46.786278]	Beacon	00-80-69-43-7F-7B-64-FF-0F-00-00-00-22-9C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 33
	Protocol: ZigBee
	Timestamp: 11:50:46.786278
	Time Delta: 0.008656
	Channel: 13
	Length: 28
	Link Quality: -45 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x647B7F43698000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 105
	Source PAN ID: 0x7F43
	Source Address: 0x647B
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.322838]	Beacon Request	03-08-A8-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 34
	Protocol: ZigBee
	Timestamp: 11:50:47.322838
	Time Delta: 0.536560
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFA80803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 168
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.325318]	Beacon	00-80-6A-43-7F-7B-64-FF-0F-00-00-00-22-9C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 35
	Protocol: ZigBee
	Timestamp: 11:50:47.325318
	Time Delta: 0.002480
	Channel: 13
	Length: 28
	Link Quality: -45 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x647B7F436A8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 106
	Source PAN ID: 0x7F43
	Source Address: 0x647B
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.327150]	Beacon	00-80-67-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 36
	Protocol: ZigBee
	Timestamp: 11:50:47.327150
	Time Delta: 0.001832
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F43678000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 103
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.329998]	Beacon	00-80-E8-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 37
	Protocol: ZigBee
	Timestamp: 11:50:47.329998
	Time Delta: 0.002848
	Channel: 13
	Length: 28
	Link Quality: -27 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFE88000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 232
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.333798]	Beacon	00-80-6F-43-7F-68-33-FF-0F-00-00-00-22-8C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 38
	Protocol: ZigBee
	Timestamp: 11:50:47.333798
	Time Delta: 0.003800
	Channel: 13
	Length: 28
	Link Quality: -54 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x33687F436F8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 111
	Source PAN ID: 0x7F43
	Source Address: 0x3368
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 1··· ···· ···· = Device Depth: 0x1
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.730686]	Rejoin Request	61-88-AD-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-AF-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 39
	Protocol: ZigBee
	Timestamp: 11:50:47.730686
	Time Delta: 0.396888
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 173
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 175
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.733358]	Rejoin Request	61-88-AD-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-AF-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 40
	Protocol: ZigBee
	Timestamp: 11:50:47.733358
	Time Delta: 0.002672
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 173
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 175
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.736990]	Rejoin Request	61-88-AD-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-AF-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 41
	Protocol: ZigBee
	Timestamp: 11:50:47.736990
	Time Delta: 0.003632
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 173
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 175
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.740014]	Rejoin Request	61-88-AD-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-AF-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 42
	Protocol: ZigBee
	Timestamp: 11:50:47.740014
	Time Delta: 0.003024
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 173
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 175
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.745822]	Rejoin Request	61-88-AE-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-AF-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 43
	Protocol: ZigBee
	Timestamp: 11:50:47.745822
	Time Delta: 0.005808
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 174
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 175
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.748814]	Rejoin Request	61-88-AE-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-AF-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 44
	Protocol: ZigBee
	Timestamp: 11:50:47.748814
	Time Delta: 0.002992
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 174
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 175
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.752782]	Rejoin Request	61-88-AE-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-AF-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 45
	Protocol: ZigBee
	Timestamp: 11:50:47.752782
	Time Delta: 0.003968
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 174
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 175
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:47.757374]	Rejoin Request	61-88-AE-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-AF-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 46
	Protocol: ZigBee
	Timestamp: 11:50:47.757374
	Time Delta: 0.004592
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 174
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 175
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.166726]	Data Request	63-88-AF-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 47
	Protocol: ZigBee
	Timestamp: 11:50:48.166726
	Time Delta: 0.409352
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 175
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.170766]	Data Request	63-88-AF-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 48
	Protocol: ZigBee
	Timestamp: 11:50:48.170766
	Time Delta: 0.004040
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 175
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.172894]	Data Request	63-88-AF-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 49
	Protocol: ZigBee
	Timestamp: 11:50:48.172894
	Time Delta: 0.002128
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 175
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.175358]	Data Request	63-88-AF-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 50
	Protocol: ZigBee
	Timestamp: 11:50:48.175358
	Time Delta: 0.002464
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 175
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.182838]	Orphan Notification	43-C8-B0-FF-FF-FF-FF-F0-BC-8D-01-00-4B-12-00-06-FF-FF
Frame Information: (18 bytes)
	Packet Number: 51
	Protocol: ZigBee
	Timestamp: 11:50:48.182838
	Time Delta: 0.007480
	Channel: 13
	Length: 18
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (15 bytes)
	Frame Control: 0xC843
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		11·· ···· ···· ···· = Source Addr Mode: [0x3] 64-bit Extended Address
	Sequence Number: 176
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
	Source Address: 00:12:4B:00:01:8D:BC:F0
MAC Payload: 0x06
	Command Frame ID: [0x06] Orphan Notification
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.192118]	Coordinator Realignment	23-CC-95-FF-FF-F0-BC-8D-01-00-4B-12-00-43-7F-E1-2A-70-02-00-4B-12-00-08-43-7F-68-33-0D-35-64-FF-FF
Frame Information: (33 bytes)
	Packet Number: 52
	Protocol: ZigBee
	Timestamp: 11:50:48.192118
	Time Delta: 0.009280
	Channel: 13
	Length: 33
	Link Quality: -54 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (23 bytes)
	Frame Control: 0xCC23
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 11·· ···· ···· = Destination Addr Mode: [0x3] 64-bit Extended Address
		··00 ···· ···· ···· = Reserved: 0x0
		11·· ···· ···· ···· = Source Addr Mode: [0x3] 64-bit Extended Address
	Sequence Number: 149
	Destination PAN ID: 0xFFFF
	Destination Address: 00:12:4B:00:01:8D:BC:F0
	Source PAN ID: 0x7F43
	Source Address: 00:12:4B:00:02:70:2A:E1
MAC Payload: 0x64350D33687F4308
	Command Frame ID: [0x08] Coordinator Realignment
	Command Payload: 0x64350D33687F43
		Re-PAN ID: 0x7F43
		Re-Coordinator Short Address: 0x3368
		Re-Logical Channel: 0x0D
		Re-Short Address: 0x6435
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.193558]	Acknowledgement	02-00-95-FF-FF
Frame Information: (5 bytes)
	Packet Number: 53
	Protocol: ZigBee
	Timestamp: 11:50:48.193558
	Time Delta: 0.001440
	Channel: 13
	Length: 5
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0x950002
	Frame Control: 0x0002
		···· ···· ···· ·010 = Frame Type: [0x2] Acknowledgement
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 149
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.393910]	Beacon Request	03-08-B1-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 54
	Protocol: ZigBee
	Timestamp: 11:50:48.393910
	Time Delta: 0.200352
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFB10803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 177
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.396454]	Beacon	00-80-E9-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 55
	Protocol: ZigBee
	Timestamp: 11:50:48.396454
	Time Delta: 0.002544
	Channel: 13
	Length: 28
	Link Quality: -27 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFE98000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 233
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.398462]	Beacon	00-80-70-43-7F-68-33-FF-0F-00-00-00-22-8C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 56
	Protocol: ZigBee
	Timestamp: 11:50:48.398462
	Time Delta: 0.002008
	Channel: 13
	Length: 28
	Link Quality: -54 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x33687F43708000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 112
	Source PAN ID: 0x7F43
	Source Address: 0x3368
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 1··· ···· ···· = Device Depth: 0x1
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.400462]	Beacon	00-80-6B-43-7F-7B-64-FF-0F-00-00-00-22-9C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 57
	Protocol: ZigBee
	Timestamp: 11:50:48.400462
	Time Delta: 0.002000
	Channel: 13
	Length: 28
	Link Quality: -45 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x647B7F436B8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 107
	Source PAN ID: 0x7F43
	Source Address: 0x647B
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:48.405014]	Beacon	00-80-68-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 58
	Protocol: ZigBee
	Timestamp: 11:50:48.405014
	Time Delta: 0.004552
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F43688000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 104
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:49.116926]	Beacon Request	03-08-B6-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 59
	Protocol: ZigBee
	Timestamp: 11:50:49.116926
	Time Delta: 0.711912
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFB60803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 182
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:49.120590]	Beacon	00-80-EA-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 60
	Protocol: ZigBee
	Timestamp: 11:50:49.120590
	Time Delta: 0.003664
	Channel: 13
	Length: 28
	Link Quality: -27 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFEA8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 234
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:49.123830]	Beacon	00-80-71-43-7F-68-33-FF-0F-00-00-00-22-8C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 61
	Protocol: ZigBee
	Timestamp: 11:50:49.123830
	Time Delta: 0.003240
	Channel: 13
	Length: 28
	Link Quality: -58 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x33687F43718000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 113
	Source PAN ID: 0x7F43
	Source Address: 0x3368
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 1··· ···· ···· = Device Depth: 0x1
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:49.126134]	Beacon	00-80-69-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 62
	Protocol: ZigBee
	Timestamp: 11:50:49.126134
	Time Delta: 0.002304
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F43698000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 105
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:49.128758]	Beacon	00-80-6C-43-7F-7B-64-FF-0F-00-00-00-22-9C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 63
	Protocol: ZigBee
	Timestamp: 11:50:49.128758
	Time Delta: 0.002624
	Channel: 13
	Length: 28
	Link Quality: -43 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x647B7F436C8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 108
	Source PAN ID: 0x7F43
	Source Address: 0x647B
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:49.794494]	Beacon Request	03-08-BB-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 64
	Protocol: ZigBee
	Timestamp: 11:50:49.794494
	Time Delta: 0.665736
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFBB0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 187
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:49.797446]	Beacon	00-80-6A-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 65
	Protocol: ZigBee
	Timestamp: 11:50:49.797446
	Time Delta: 0.002952
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F436A8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 106
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:49.799214]	Beacon	00-80-EB-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 66
	Protocol: ZigBee
	Timestamp: 11:50:49.799214
	Time Delta: 0.001768
	Channel: 13
	Length: 28
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFEB8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 235
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:49.800894]	Beacon	00-80-44-43-7F-0A-F0-FF-0F-00-00-00-22-A4-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 67
	Protocol: ZigBee
	Timestamp: 11:50:49.800894
	Time Delta: 0.001680
	Channel: 13
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xF00A7F43448000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 68
	Source PAN ID: 0x7F43
	Source Address: 0xF00A
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0xA422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·010 0··· ···· ···· = Device Depth: 0x4
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:49.803254]	Beacon	00-80-6D-43-7F-7B-64-FF-0F-00-00-00-22-9C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 68
	Protocol: ZigBee
	Timestamp: 11:50:49.803254
	Time Delta: 0.002360
	Channel: 13
	Length: 28
	Link Quality: -43 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x647B7F436D8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 109
	Source PAN ID: 0x7F43
	Source Address: 0x647B
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.016790]	Link Status	41-88-27-EF-BA-FF-FF-00-00-09-00-FC-FF-00-00-01-E3-08-60-FF-FF
Frame Information: (21 bytes)
	Packet Number: 69
	Protocol: ZigBee
	Timestamp: 11:50:50.016790
	Time Delta: 0.213536
	Channel: 13
	Length: 21
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 39
	Destination PAN ID: 0xBAEF
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (10 bytes)
	NWK Header: 0xE3010000FFFC0009
		Frame Control: 0x0009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···0 ···· ···· ···· = Source IEEE Address Included: [0x0] No
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 227
	NWK Payload: 0x6008
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x60
			···0 0000 = Entry Count: 0x0
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.199422]	Rejoin Request	61-88-C0-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B0-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 70
	Protocol: ZigBee
	Timestamp: 11:50:50.199422
	Time Delta: 0.182632
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 192
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 176
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.203382]	Rejoin Request	61-88-C0-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B0-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 71
	Protocol: ZigBee
	Timestamp: 11:50:50.203382
	Time Delta: 0.003960
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 192
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 176
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.206686]	Rejoin Request	61-88-C0-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B0-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 72
	Protocol: ZigBee
	Timestamp: 11:50:50.206686
	Time Delta: 0.003304
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 192
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 176
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.211278]	Rejoin Request	61-88-C0-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B0-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 73
	Protocol: ZigBee
	Timestamp: 11:50:50.211278
	Time Delta: 0.004592
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 192
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 176
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.218702]	Rejoin Request	61-88-C1-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B0-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 74
	Protocol: ZigBee
	Timestamp: 11:50:50.218702
	Time Delta: 0.007424
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 193
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 176
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.223006]	Rejoin Request	61-88-C1-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B0-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 75
	Protocol: ZigBee
	Timestamp: 11:50:50.223006
	Time Delta: 0.004304
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 193
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 176
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.226014]	Rejoin Request	61-88-C1-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B0-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 76
	Protocol: ZigBee
	Timestamp: 11:50:50.226014
	Time Delta: 0.003008
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 193
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 176
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.229966]	Rejoin Request	61-88-C1-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B0-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 77
	Protocol: ZigBee
	Timestamp: 11:50:50.229966
	Time Delta: 0.003952
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 193
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 176
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.635366]	Data Request	63-88-C2-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 78
	Protocol: ZigBee
	Timestamp: 11:50:50.635366
	Time Delta: 0.405400
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 194
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.639118]	Data Request	63-88-C2-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 79
	Protocol: ZigBee
	Timestamp: 11:50:50.639118
	Time Delta: 0.003752
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 194
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.641894]	Data Request	63-88-C2-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 80
	Protocol: ZigBee
	Timestamp: 11:50:50.641894
	Time Delta: 0.002776
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 194
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.645934]	Data Request	63-88-C2-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 81
	Protocol: ZigBee
	Timestamp: 11:50:50.645934
	Time Delta: 0.004040
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 194
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.652878]	Orphan Notification	43-C8-C3-FF-FF-FF-FF-F0-BC-8D-01-00-4B-12-00-06-FF-FF
Frame Information: (18 bytes)
	Packet Number: 82
	Protocol: ZigBee
	Timestamp: 11:50:50.652878
	Time Delta: 0.006944
	Channel: 13
	Length: 18
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (15 bytes)
	Frame Control: 0xC843
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		11·· ···· ···· ···· = Source Addr Mode: [0x3] 64-bit Extended Address
	Sequence Number: 195
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
	Source Address: 00:12:4B:00:01:8D:BC:F0
MAC Payload: 0x06
	Command Frame ID: [0x06] Orphan Notification
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.660246]	Coordinator Realignment	23-CC-96-FF-FF-F0-BC-8D-01-00-4B-12-00-43-7F-E1-2A-70-02-00-4B-12-00-08-43-7F-68-33-0D-35-64-FF-FF
Frame Information: (33 bytes)
	Packet Number: 83
	Protocol: ZigBee
	Timestamp: 11:50:50.660246
	Time Delta: 0.007368
	Channel: 13
	Length: 33
	Link Quality: -60 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (23 bytes)
	Frame Control: 0xCC23
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 11·· ···· ···· = Destination Addr Mode: [0x3] 64-bit Extended Address
		··00 ···· ···· ···· = Reserved: 0x0
		11·· ···· ···· ···· = Source Addr Mode: [0x3] 64-bit Extended Address
	Sequence Number: 150
	Destination PAN ID: 0xFFFF
	Destination Address: 00:12:4B:00:01:8D:BC:F0
	Source PAN ID: 0x7F43
	Source Address: 00:12:4B:00:02:70:2A:E1
MAC Payload: 0x64350D33687F4308
	Command Frame ID: [0x08] Coordinator Realignment
	Command Payload: 0x64350D33687F43
		Re-PAN ID: 0x7F43
		Re-Coordinator Short Address: 0x3368
		Re-Logical Channel: 0x0D
		Re-Short Address: 0x6435
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.661686]	Acknowledgement	02-00-96-FF-FF
Frame Information: (5 bytes)
	Packet Number: 84
	Protocol: ZigBee
	Timestamp: 11:50:50.661686
	Time Delta: 0.001440
	Channel: 13
	Length: 5
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0x960002
	Frame Control: 0x0002
		···· ···· ···· ·010 = Frame Type: [0x2] Acknowledgement
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 150
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.774782]	Beacon Request	03-08-C4-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 85
	Protocol: ZigBee
	Timestamp: 11:50:50.774782
	Time Delta: 0.113096
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFC40803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 196
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.777974]	Beacon	00-80-EC-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 86
	Protocol: ZigBee
	Timestamp: 11:50:50.777974
	Time Delta: 0.003192
	Channel: 13
	Length: 28
	Link Quality: -27 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFEC8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 236
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.779950]	Beacon	00-80-45-43-7F-0A-F0-FF-0F-00-00-00-22-A4-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 87
	Protocol: ZigBee
	Timestamp: 11:50:50.779950
	Time Delta: 0.001976
	Channel: 13
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xF00A7F43458000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 69
	Source PAN ID: 0x7F43
	Source Address: 0xF00A
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0xA422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·010 0··· ···· ···· = Device Depth: 0x4
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.782542]	Beacon	00-80-73-43-7F-68-33-FF-0F-00-00-00-22-8C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 88
	Protocol: ZigBee
	Timestamp: 11:50:50.782542
	Time Delta: 0.002592
	Channel: 13
	Length: 28
	Link Quality: -58 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x33687F43738000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 115
	Source PAN ID: 0x7F43
	Source Address: 0x3368
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 1··· ···· ···· = Device Depth: 0x1
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:50.785846]	Beacon	00-80-6B-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 89
	Protocol: ZigBee
	Timestamp: 11:50:50.785846
	Time Delta: 0.003304
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F436B8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 107
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:51.475830]	Beacon Request	03-08-C9-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 90
	Protocol: ZigBee
	Timestamp: 11:50:51.475830
	Time Delta: 0.689984
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFC90803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 201
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:51.477878]	Beacon	00-80-ED-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 91
	Protocol: ZigBee
	Timestamp: 11:50:51.477878
	Time Delta: 0.002048
	Channel: 13
	Length: 28
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFED8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 237
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:51.479270]	Beacon	00-80-74-43-7F-68-33-FF-0F-00-00-00-22-8C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 92
	Protocol: ZigBee
	Timestamp: 11:50:51.479270
	Time Delta: 0.001392
	Channel: 13
	Length: 28
	Link Quality: -59 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x33687F43748000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 116
	Source PAN ID: 0x7F43
	Source Address: 0x3368
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 1··· ···· ···· = Device Depth: 0x1
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:51.481478]	Beacon	00-80-46-43-7F-0A-F0-FF-0F-00-00-00-22-A4-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 93
	Protocol: ZigBee
	Timestamp: 11:50:51.481478
	Time Delta: 0.002208
	Channel: 13
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xF00A7F43468000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 70
	Source PAN ID: 0x7F43
	Source Address: 0xF00A
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0xA422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·010 0··· ···· ···· = Device Depth: 0x4
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:51.486950]	Beacon	00-80-6F-43-7F-7B-64-FF-0F-00-00-00-22-9C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 94
	Protocol: ZigBee
	Timestamp: 11:50:51.486950
	Time Delta: 0.005472
	Channel: 13
	Length: 28
	Link Quality: -45 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x647B7F436F8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 111
	Source PAN ID: 0x7F43
	Source Address: 0x647B
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:51.492990]	Beacon	00-80-6C-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 95
	Protocol: ZigBee
	Timestamp: 11:50:51.492990
	Time Delta: 0.006040
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F436C8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 108
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:51.628078]	Link Status	41-88-97-43-7F-FF-FF-68-33-09-10-FC-FF-68-33-01-E5-E1-2A-70-02-00-4B-12-00-08-63-7B-64-11-9C-D9-11-0A-F0-11-FF-FF
Frame Information: (38 bytes)
	Packet Number: 96
	Protocol: ZigBee
	Timestamp: 11:50:51.628078
	Time Delta: 0.135088
	Channel: 13
	Length: 38
	Link Quality: -59 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 151
	Destination PAN ID: 0x7F43
	Destination Address: 0xFFFF
	Source Address: 0x3368
MAC Payload: (27 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x3368
		Radius: 0x01
		Sequence Number: 229
		Source IEEE Address: 00:12:4B:00:02:70:2A:E1
	NWK Payload: (11 bytes)
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x63
			···0 0011 = Entry Count: 0x3
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: (9 bytes)
			Entry 0: 0x11647B
				Neighbor Network Address: 0x647B
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11D99C
				Neighbor Network Address: 0xD99C
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 2: 0x11F00A
				Neighbor Network Address: 0xF00A
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.217294]	Beacon Request	03-08-CE-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 97
	Protocol: ZigBee
	Timestamp: 11:50:52.217294
	Time Delta: 0.589216
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFCE0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 206
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.219430]	Beacon	00-80-EE-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 98
	Protocol: ZigBee
	Timestamp: 11:50:52.219430
	Time Delta: 0.002136
	Channel: 13
	Length: 28
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFEE8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 238
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.221366]	Beacon	00-80-47-43-7F-0A-F0-FF-0F-00-00-00-22-A4-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 99
	Protocol: ZigBee
	Timestamp: 11:50:52.221366
	Time Delta: 0.001936
	Channel: 13
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xF00A7F43478000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 71
	Source PAN ID: 0x7F43
	Source Address: 0xF00A
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0xA422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·010 0··· ···· ···· = Device Depth: 0x4
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.224870]	Beacon	00-80-75-43-7F-68-33-FF-0F-00-00-00-22-8C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 100
	Protocol: ZigBee
	Timestamp: 11:50:52.224870
	Time Delta: 0.003504
	Channel: 13
	Length: 28
	Link Quality: -60 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x33687F43758000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 117
	Source PAN ID: 0x7F43
	Source Address: 0x3368
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 1··· ···· ···· = Device Depth: 0x1
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.630958]	Rejoin Request	61-88-D3-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B1-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 101
	Protocol: ZigBee
	Timestamp: 11:50:52.630958
	Time Delta: 0.406088
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 211
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 177
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.634910]	Rejoin Request	61-88-D3-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B1-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 102
	Protocol: ZigBee
	Timestamp: 11:50:52.634910
	Time Delta: 0.003952
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 211
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 177
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.638222]	Rejoin Request	61-88-D3-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B1-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 103
	Protocol: ZigBee
	Timestamp: 11:50:52.638222
	Time Delta: 0.003312
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 211
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 177
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.642846]	Rejoin Request	61-88-D3-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B1-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 104
	Protocol: ZigBee
	Timestamp: 11:50:52.642846
	Time Delta: 0.004624
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 211
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 177
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.650318]	Rejoin Request	61-88-D4-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B1-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 105
	Protocol: ZigBee
	Timestamp: 11:50:52.650318
	Time Delta: 0.007472
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 212
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 177
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.652998]	Rejoin Request	61-88-D4-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B1-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 106
	Protocol: ZigBee
	Timestamp: 11:50:52.652998
	Time Delta: 0.002680
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 212
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 177
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.656670]	Rejoin Request	61-88-D4-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B1-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 107
	Protocol: ZigBee
	Timestamp: 11:50:52.656670
	Time Delta: 0.003672
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 212
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 177
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:52.659358]	Rejoin Request	61-88-D4-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B1-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 108
	Protocol: ZigBee
	Timestamp: 11:50:52.659358
	Time Delta: 0.002688
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 212
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 177
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.066774]	Data Request	63-88-D5-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 109
	Protocol: ZigBee
	Timestamp: 11:50:53.066774
	Time Delta: 0.407416
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 213
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.070806]	Data Request	63-88-D5-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 110
	Protocol: ZigBee
	Timestamp: 11:50:53.070806
	Time Delta: 0.004032
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 213
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.073894]	Data Request	63-88-D5-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 111
	Protocol: ZigBee
	Timestamp: 11:50:53.073894
	Time Delta: 0.003088
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 213
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.077302]	Data Request	63-88-D5-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 112
	Protocol: ZigBee
	Timestamp: 11:50:53.077302
	Time Delta: 0.003408
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 213
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.085390]	Orphan Notification	43-C8-D6-FF-FF-FF-FF-F0-BC-8D-01-00-4B-12-00-06-FF-FF
Frame Information: (18 bytes)
	Packet Number: 113
	Protocol: ZigBee
	Timestamp: 11:50:53.085390
	Time Delta: 0.008088
	Channel: 13
	Length: 18
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (15 bytes)
	Frame Control: 0xC843
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		11·· ···· ···· ···· = Source Addr Mode: [0x3] 64-bit Extended Address
	Sequence Number: 214
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
	Source Address: 00:12:4B:00:01:8D:BC:F0
MAC Payload: 0x06
	Command Frame ID: [0x06] Orphan Notification
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.094254]	Acknowledgement	02-00-98-FF-FF
Frame Information: (5 bytes)
	Packet Number: 114
	Protocol: ZigBee
	Timestamp: 11:50:53.094254
	Time Delta: 0.008864
	Channel: 13
	Length: 5
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0x980002
	Frame Control: 0x0002
		···· ···· ···· ·010 = Frame Type: [0x2] Acknowledgement
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 152
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.242270]	Beacon Request	03-08-D7-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 115
	Protocol: ZigBee
	Timestamp: 11:50:53.242270
	Time Delta: 0.148016
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFD70803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 215
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.244726]	Beacon	00-80-EF-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 116
	Protocol: ZigBee
	Timestamp: 11:50:53.244726
	Time Delta: 0.002456
	Channel: 13
	Length: 28
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFEF8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 239
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.246270]	Beacon	00-80-48-43-7F-0A-F0-FF-0F-00-00-00-22-A4-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 117
	Protocol: ZigBee
	Timestamp: 11:50:53.246270
	Time Delta: 0.001544
	Channel: 13
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xF00A7F43488000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 72
	Source PAN ID: 0x7F43
	Source Address: 0xF00A
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0xA422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·010 0··· ···· ···· = Device Depth: 0x4
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.248374]	Beacon	00-80-6E-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 118
	Protocol: ZigBee
	Timestamp: 11:50:53.248374
	Time Delta: 0.002104
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F436E8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 110
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.250606]	Beacon	00-80-71-43-7F-7B-64-FF-0F-00-00-00-22-9C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 119
	Protocol: ZigBee
	Timestamp: 11:50:53.250606
	Time Delta: 0.002232
	Channel: 13
	Length: 28
	Link Quality: -44 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x647B7F43718000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 113
	Source PAN ID: 0x7F43
	Source Address: 0x647B
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.349246]	Link Status	41-88-2E-43-7F-FF-FF-0A-F0-09-10-FC-FF-0A-F0-01-F8-B9-2C-70-02-00-4B-12-00-08-63-68-33-11-7B-64-11-9C-D9-11-FF-FF
Frame Information: (38 bytes)
	Packet Number: 120
	Protocol: ZigBee
	Timestamp: 11:50:53.349246
	Time Delta: 0.098640
	Channel: 13
	Length: 38
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 46
	Destination PAN ID: 0x7F43
	Destination Address: 0xFFFF
	Source Address: 0xF00A
MAC Payload: (27 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xF00A
		Radius: 0x01
		Sequence Number: 248
		Source IEEE Address: 00:12:4B:00:02:70:2C:B9
	NWK Payload: (11 bytes)
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x63
			···0 0011 = Entry Count: 0x3
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: (9 bytes)
			Entry 0: 0x113368
				Neighbor Network Address: 0x3368
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11647B
				Neighbor Network Address: 0x647B
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 2: 0x11D99C
				Neighbor Network Address: 0xD99C
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.894702]	Beacon Request	03-08-DC-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 121
	Protocol: ZigBee
	Timestamp: 11:50:53.894702
	Time Delta: 0.545456
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFDC0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 220
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.897606]	Beacon	00-80-6F-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 122
	Protocol: ZigBee
	Timestamp: 11:50:53.897606
	Time Delta: 0.002904
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F436F8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 111
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.899398]	Beacon	00-80-49-43-7F-0A-F0-FF-0F-00-00-00-22-A4-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 123
	Protocol: ZigBee
	Timestamp: 11:50:53.899398
	Time Delta: 0.001792
	Channel: 13
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xF00A7F43498000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 73
	Source PAN ID: 0x7F43
	Source Address: 0xF00A
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0xA422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·010 0··· ···· ···· = Device Depth: 0x4
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:53.902934]	Beacon	00-80-F0-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 124
	Protocol: ZigBee
	Timestamp: 11:50:53.902934
	Time Delta: 0.003536
	Channel: 13
	Length: 28
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFF08000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 240
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.447942]	Beacon Request	03-08-E1-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 125
	Protocol: ZigBee
	Timestamp: 11:50:54.447942
	Time Delta: 0.545008
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFE10803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 225
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.453478]	Beacon	00-80-4A-43-7F-0A-F0-FF-0F-00-00-00-22-A4-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 126
	Protocol: ZigBee
	Timestamp: 11:50:54.453478
	Time Delta: 0.005536
	Channel: 13
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xF00A7F434A8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 74
	Source PAN ID: 0x7F43
	Source Address: 0xF00A
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0xA422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·010 0··· ···· ···· = Device Depth: 0x4
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.455558]	Beacon	00-80-70-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 127
	Protocol: ZigBee
	Timestamp: 11:50:54.455558
	Time Delta: 0.002080
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F43708000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 112
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.463942]	Beacon	00-80-78-43-7F-68-33-FF-0F-00-00-00-22-8C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 128
	Protocol: ZigBee
	Timestamp: 11:50:54.463942
	Time Delta: 0.008384
	Channel: 13
	Length: 28
	Link Quality: -63 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x33687F43788000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 120
	Source PAN ID: 0x7F43
	Source Address: 0x3368
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 1··· ···· ···· = Device Depth: 0x1
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.853286]	Rejoin Request	61-88-E6-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B2-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 129
	Protocol: ZigBee
	Timestamp: 11:50:54.853286
	Time Delta: 0.389344
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 230
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 178
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.855950]	Rejoin Request	61-88-E6-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B2-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 130
	Protocol: ZigBee
	Timestamp: 11:50:54.855950
	Time Delta: 0.002664
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 230
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 178
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.860238]	Rejoin Request	61-88-E6-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B2-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 131
	Protocol: ZigBee
	Timestamp: 11:50:54.860238
	Time Delta: 0.004288
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 230
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 178
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.862910]	Rejoin Request	61-88-E6-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B2-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 132
	Protocol: ZigBee
	Timestamp: 11:50:54.862910
	Time Delta: 0.002672
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 230
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 178
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.870230]	Rejoin Request	61-88-E7-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B2-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 133
	Protocol: ZigBee
	Timestamp: 11:50:54.870230
	Time Delta: 0.007320
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 231
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 178
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.873214]	Rejoin Request	61-88-E7-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B2-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 134
	Protocol: ZigBee
	Timestamp: 11:50:54.873214
	Time Delta: 0.002984
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 231
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 178
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.877806]	Rejoin Request	61-88-E7-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B2-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 135
	Protocol: ZigBee
	Timestamp: 11:50:54.877806
	Time Delta: 0.004592
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 231
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 178
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:54.882078]	Rejoin Request	61-88-E7-17-F8-00-00-4D-A4-09-10-00-00-4D-A4-01-B2-F0-BC-8D-01-00-4B-12-00-06-80-FF-FF
Frame Information: (29 bytes)
	Packet Number: 136
	Protocol: ZigBee
	Timestamp: 11:50:54.882078
	Time Delta: 0.004272
	Channel: 13
	Length: 29
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8861
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 231
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: (18 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0x0000
		Source Address: 0xA44D
		Radius: 0x01
		Sequence Number: 178
		Source IEEE Address: 00:12:4B:00:01:8D:BC:F0
	NWK Payload: 0x8006
		NWK Command ID: [0x06] Rejoin Request
		Capability Information: 0x80
			···· ···0 = Alternate PAN Coordinator Capability: 0x0
			···· ··0· = Device Type: [0x0] End Device
			···· ·0·· = Power Source: [0x0] Other Power Source
			···· 0··· = Receiver On When Idle: [0x0] No
			··00 ···· = Reserved: 0x0
			·0·· ···· = Security Capability: [0x0] Standard Security Mode
			1··· ···· = Allocate Address: [0x1] Yes
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.289854]	Data Request	63-88-E8-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 137
	Protocol: ZigBee
	Timestamp: 11:50:55.289854
	Time Delta: 0.407776
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 232
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.293262]	Data Request	63-88-E8-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 138
	Protocol: ZigBee
	Timestamp: 11:50:55.293262
	Time Delta: 0.003408
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 232
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.296046]	Data Request	63-88-E8-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 139
	Protocol: ZigBee
	Timestamp: 11:50:55.296046
	Time Delta: 0.002784
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 232
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.299478]	Data Request	63-88-E8-17-F8-00-00-4D-A4-04-FF-FF
Frame Information: (12 bytes)
	Packet Number: 140
	Protocol: ZigBee
	Timestamp: 11:50:55.299478
	Time Delta: 0.003432
	Channel: 13
	Length: 12
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8863
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 232
	Destination PAN ID: 0xF817
	Destination Address: 0x0000
	Source Address: 0xA44D
MAC Payload: 0x04
	Command Frame ID: [0x04] Data Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.308254]	Orphan Notification	43-C8-E9-FF-FF-FF-FF-F0-BC-8D-01-00-4B-12-00-06-FF-FF
Frame Information: (18 bytes)
	Packet Number: 141
	Protocol: ZigBee
	Timestamp: 11:50:55.308254
	Time Delta: 0.008776
	Channel: 13
	Length: 18
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (15 bytes)
	Frame Control: 0xC843
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		11·· ···· ···· ···· = Source Addr Mode: [0x3] 64-bit Extended Address
	Sequence Number: 233
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
	Source Address: 00:12:4B:00:01:8D:BC:F0
MAC Payload: 0x06
	Command Frame ID: [0x06] Orphan Notification
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.315742]	Coordinator Realignment	23-CC-99-FF-FF-F0-BC-8D-01-00-4B-12-00-43-7F-E1-2A-70-02-00-4B-12-00-08-43-7F-68-33-0D-35-64-FF-FF
Frame Information: (33 bytes)
	Packet Number: 142
	Protocol: ZigBee
	Timestamp: 11:50:55.315742
	Time Delta: 0.007488
	Channel: 13
	Length: 33
	Link Quality: -63 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: (23 bytes)
	Frame Control: 0xCC23
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··1· ···· = Acknowledgement Request: [0x1] Yes
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 11·· ···· ···· = Destination Addr Mode: [0x3] 64-bit Extended Address
		··00 ···· ···· ···· = Reserved: 0x0
		11·· ···· ···· ···· = Source Addr Mode: [0x3] 64-bit Extended Address
	Sequence Number: 153
	Destination PAN ID: 0xFFFF
	Destination Address: 00:12:4B:00:01:8D:BC:F0
	Source PAN ID: 0x7F43
	Source Address: 00:12:4B:00:02:70:2A:E1
MAC Payload: 0x64350D33687F4308
	Command Frame ID: [0x08] Coordinator Realignment
	Command Payload: 0x64350D33687F43
		Re-PAN ID: 0x7F43
		Re-Coordinator Short Address: 0x3368
		Re-Logical Channel: 0x0D
		Re-Short Address: 0x6435
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.317182]	Acknowledgement	02-00-99-FF-FF
Frame Information: (5 bytes)
	Packet Number: 143
	Protocol: ZigBee
	Timestamp: 11:50:55.317182
	Time Delta: 0.001440
	Channel: 13
	Length: 5
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0x990002
	Frame Control: 0x0002
		···· ···· ···· ·010 = Frame Type: [0x2] Acknowledgement
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 153
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.423470]	Beacon Request	03-08-EA-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 144
	Protocol: ZigBee
	Timestamp: 11:50:55.423470
	Time Delta: 0.106288
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFEA0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 234
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.425974]	Beacon	00-80-79-43-7F-68-33-FF-0F-00-00-00-22-8C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 145
	Protocol: ZigBee
	Timestamp: 11:50:55.425974
	Time Delta: 0.002504
	Channel: 13
	Length: 28
	Link Quality: -63 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x33687F43798000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 121
	Source PAN ID: 0x7F43
	Source Address: 0x3368
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 1··· ···· ···· = Device Depth: 0x1
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.427526]	Beacon	00-80-F2-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 146
	Protocol: ZigBee
	Timestamp: 11:50:55.427526
	Time Delta: 0.001552
	Channel: 13
	Length: 28
	Link Quality: -27 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFF28000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 242
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.431054]	Beacon	00-80-74-43-7F-7B-64-FF-0F-00-00-00-22-9C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 147
	Protocol: ZigBee
	Timestamp: 11:50:55.431054
	Time Delta: 0.003528
	Channel: 13
	Length: 28
	Link Quality: -44 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x647B7F43748000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 116
	Source PAN ID: 0x7F43
	Source Address: 0x647B
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.441206]	Beacon	00-80-71-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 148
	Protocol: ZigBee
	Timestamp: 11:50:55.441206
	Time Delta: 0.010152
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F43718000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 113
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:55.571438]	Link Status	41-88-D9-43-7F-FF-FF-9C-D9-09-10-FC-FF-9C-D9-01-F9-AB-2B-70-02-00-4B-12-00-08-63-68-33-11-7B-64-11-0A-F0-11-FF-FF
Frame Information: (38 bytes)
	Packet Number: 149
	Protocol: ZigBee
	Timestamp: 11:50:55.571438
	Time Delta: 0.130232
	Channel: 13
	Length: 38
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 217
	Destination PAN ID: 0x7F43
	Destination Address: 0xFFFF
	Source Address: 0xD99C
MAC Payload: (27 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xD99C
		Radius: 0x01
		Sequence Number: 249
		Source IEEE Address: 00:12:4B:00:02:70:2B:AB
	NWK Payload: (11 bytes)
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x63
			···0 0011 = Entry Count: 0x3
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: (9 bytes)
			Entry 0: 0x113368
				Neighbor Network Address: 0x3368
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11647B
				Neighbor Network Address: 0x647B
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 2: 0x11F00A
				Neighbor Network Address: 0xF00A
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:56.026558]	Beacon Request	03-08-EF-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 150
	Protocol: ZigBee
	Timestamp: 11:50:56.026558
	Time Delta: 0.455120
	Channel: 13
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFEF0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 239
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:56.028750]	Beacon	00-80-F3-EF-BA-00-00-FF-4F-00-00-00-22-84-66-2B-2F-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 151
	Protocol: ZigBee
	Timestamp: 11:50:56.028750
	Time Delta: 0.002192
	Channel: 13
	Length: 28
	Link Quality: -26 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000BAEFF38000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 243
	Source PAN ID: 0xBAEF
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:2F:2B:66
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:56.030382]	Beacon	00-80-72-43-7F-9C-D9-FF-0F-00-00-00-22-94-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 152
	Protocol: ZigBee
	Timestamp: 11:50:56.030382
	Time Delta: 0.001632
	Channel: 13
	Length: 28
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xD99C7F43728000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 114
	Source PAN ID: 0x7F43
	Source Address: 0xD99C
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:56.033038]	Beacon	00-80-4C-43-7F-0A-F0-FF-0F-00-00-00-22-A4-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 153
	Protocol: ZigBee
	Timestamp: 11:50:56.033038
	Time Delta: 0.002656
	Channel: 13
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xF00A7F434C8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 76
	Source PAN ID: 0x7F43
	Source Address: 0xF00A
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0xA422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·010 0··· ···· ···· = Device Depth: 0x4
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:50:56.034726]	Beacon	00-80-7A-43-7F-68-33-FF-0F-00-00-00-22-8C-84-C3-17-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 154
	Protocol: ZigBee
	Timestamp: 11:50:56.034726
	Time Delta: 0.001688
	Channel: 13
	Length: 28
	Link Quality: -63 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x33687F437A8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 122
	Source PAN ID: 0x7F43
	Source Address: 0x3368
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 1··· ···· ···· = Device Depth: 0x1
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:17:C3:84
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:00.531966]	Link Status	41-88-4B-43-7F-FF-FF-7B-64-09-10-FC-FF-7B-64-01-3E-F9-AA-C6-01-00-4B-12-00-08-63-68-33-11-9C-D9-11-0A-F0-11-FF-FF
Frame Information: (38 bytes)
	Packet Number: 155
	Protocol: ZigBee
	Timestamp: 11:51:00.531966
	Time Delta: 4.497240
	Channel: 13
	Length: 38
	Link Quality: -42 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 75
	Destination PAN ID: 0x7F43
	Destination Address: 0xFFFF
	Source Address: 0x647B
MAC Payload: (27 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x647B
		Radius: 0x01
		Sequence Number: 62
		Source IEEE Address: 00:12:4B:00:01:C6:AA:F9
	NWK Payload: (11 bytes)
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x63
			···0 0011 = Entry Count: 0x3
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: (9 bytes)
			Entry 0: 0x113368
				Neighbor Network Address: 0x3368
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11D99C
				Neighbor Network Address: 0xD99C
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 2: 0x11F00A
				Neighbor Network Address: 0xF00A
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:05.126774]	Link Status	41-88-28-EF-BA-FF-FF-00-00-09-00-FC-FF-00-00-01-E4-08-60-FF-FF
Frame Information: (21 bytes)
	Packet Number: 156
	Protocol: ZigBee
	Timestamp: 11:51:05.126774
	Time Delta: 4.594808
	Channel: 13
	Length: 21
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 40
	Destination PAN ID: 0xBAEF
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (10 bytes)
	NWK Header: 0xE4010000FFFC0009
		Frame Control: 0x0009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···0 ···· ···· ···· = Source IEEE Address Included: [0x0] No
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 228
	NWK Payload: 0x6008
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x60
			···0 0000 = Entry Count: 0x0
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:09.687500]	Beacon Request	03-08-F7-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 157
	Protocol: ZigBee
	Timestamp: 11:51:09.687500
	Time Delta: 4216.792877
	Channel: 21
	Length: 10
	Link Quality: -41 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFF70803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 247
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:09.689724]	Beacon	00-80-FE-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 158
	Protocol: ZigBee
	Timestamp: 11:51:09.689724
	Time Delta: 0.002224
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817FE8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 254
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:09.692244]	Beacon	00-80-01-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 159
	Protocol: ZigBee
	Timestamp: 11:51:09.692244
	Time Delta: 0.002520
	Channel: 21
	Length: 28
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817018000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 1
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:09.693844]	Beacon	00-80-6E-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 160
	Protocol: ZigBee
	Timestamp: 11:51:09.693844
	Time Delta: 0.001600
	Channel: 21
	Length: 28
	Link Quality: -47 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F8176E8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 110
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:10.366556]	Beacon Request	03-08-FC-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 161
	Protocol: ZigBee
	Timestamp: 11:51:10.366556
	Time Delta: 0.672712
	Channel: 21
	Length: 10
	Link Quality: -32 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFFFC0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 252
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:10.370004]	Beacon	00-80-6F-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 162
	Protocol: ZigBee
	Timestamp: 11:51:10.370004
	Time Delta: 0.003448
	Channel: 21
	Length: 28
	Link Quality: -49 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F8176F8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 111
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:10.371988]	Beacon	00-80-02-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 163
	Protocol: ZigBee
	Timestamp: 11:51:10.371988
	Time Delta: 0.001984
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817028000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 2
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:10.375660]	Beacon	00-80-FF-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 164
	Protocol: ZigBee
	Timestamp: 11:51:10.375660
	Time Delta: 0.003672
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817FF8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 255
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:11.431404]	Beacon Request	03-08-05-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 165
	Protocol: ZigBee
	Timestamp: 11:51:11.431404
	Time Delta: 1.055744
	Channel: 21
	Length: 10
	Link Quality: -28 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF050803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 5
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:11.433764]	Beacon	00-80-70-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 166
	Protocol: ZigBee
	Timestamp: 11:51:11.433764
	Time Delta: 0.002360
	Channel: 21
	Length: 28
	Link Quality: -47 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817708000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 112
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:11.435916]	Beacon	00-80-03-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 167
	Protocol: ZigBee
	Timestamp: 11:51:11.435916
	Time Delta: 0.002152
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817038000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 3
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:11.442540]	Beacon	00-80-00-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 168
	Protocol: ZigBee
	Timestamp: 11:51:11.442540
	Time Delta: 0.006624
	Channel: 21
	Length: 28
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817008000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 0
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:12.041524]	Beacon Request	03-08-0A-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 169
	Protocol: ZigBee
	Timestamp: 11:51:12.041524
	Time Delta: 0.598984
	Channel: 21
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF0A0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 10
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:12.044116]	Beacon	00-80-71-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 170
	Protocol: ZigBee
	Timestamp: 11:51:12.044116
	Time Delta: 0.002592
	Channel: 21
	Length: 28
	Link Quality: -48 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817718000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 113
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:12.700348]	Beacon Request	03-08-0F-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 171
	Protocol: ZigBee
	Timestamp: 11:51:12.700348
	Time Delta: 0.656232
	Channel: 21
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF0F0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 15
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:12.705212]	Beacon	00-80-05-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 172
	Protocol: ZigBee
	Timestamp: 11:51:12.705212
	Time Delta: 0.004864
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817058000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 5
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:13.785820]	Beacon Request	03-08-18-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 173
	Protocol: ZigBee
	Timestamp: 11:51:13.785820
	Time Delta: 1.080608
	Channel: 21
	Length: 10
	Link Quality: -27 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF180803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 24
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:13.793380]	Beacon	00-80-06-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 174
	Protocol: ZigBee
	Timestamp: 11:51:13.793380
	Time Delta: 0.007560
	Channel: 21
	Length: 28
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817068000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 6
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:13.799700]	Beacon	00-80-03-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 175
	Protocol: ZigBee
	Timestamp: 11:51:13.799700
	Time Delta: 0.006320
	Channel: 21
	Length: 28
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817038000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 3
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:14.402460]	Beacon Request	03-08-1D-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 176
	Protocol: ZigBee
	Timestamp: 11:51:14.402460
	Time Delta: 0.602760
	Channel: 21
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF1D0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 29
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:14.406076]	Beacon	00-80-74-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 177
	Protocol: ZigBee
	Timestamp: 11:51:14.406076
	Time Delta: 0.003616
	Channel: 21
	Length: 28
	Link Quality: -48 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817748000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 116
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:14.409492]	Beacon	00-80-04-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 178
	Protocol: ZigBee
	Timestamp: 11:51:14.409492
	Time Delta: 0.003416
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817048000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 4
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:14.411284]	Beacon	00-80-07-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 179
	Protocol: ZigBee
	Timestamp: 11:51:14.411284
	Time Delta: 0.001792
	Channel: 21
	Length: 28
	Link Quality: -37 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817078000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 7
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:15.161892]	Beacon Request	03-08-22-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 180
	Protocol: ZigBee
	Timestamp: 11:51:15.161892
	Time Delta: 0.750608
	Channel: 21
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF220803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 34
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:15.165428]	Beacon	00-80-08-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 181
	Protocol: ZigBee
	Timestamp: 11:51:15.165428
	Time Delta: 0.003536
	Channel: 21
	Length: 28
	Link Quality: -37 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817088000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 8
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:15.167076]	Beacon	00-80-75-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 182
	Protocol: ZigBee
	Timestamp: 11:51:15.167076
	Time Delta: 0.001648
	Channel: 21
	Length: 28
	Link Quality: -47 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817758000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 117
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:15.169812]	Beacon	00-80-05-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 183
	Protocol: ZigBee
	Timestamp: 11:51:15.169812
	Time Delta: 0.002736
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817058000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 5
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:16.155956]	Beacon Request	03-08-2B-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 184
	Protocol: ZigBee
	Timestamp: 11:51:16.155956
	Time Delta: 0.986144
	Channel: 21
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF2B0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 43
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:16.160620]	Beacon	00-80-06-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 185
	Protocol: ZigBee
	Timestamp: 11:51:16.160620
	Time Delta: 0.004664
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817068000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 6
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:16.162092]	Beacon	00-80-09-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 186
	Protocol: ZigBee
	Timestamp: 11:51:16.162092
	Time Delta: 0.001472
	Channel: 21
	Length: 28
	Link Quality: -37 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817098000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 9
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:16.738004]	Beacon Request	03-08-30-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 187
	Protocol: ZigBee
	Timestamp: 11:51:16.738004
	Time Delta: 0.575912
	Channel: 21
	Length: 10
	Link Quality: -26 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF300803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 48
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:16.742244]	Beacon	00-80-77-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 188
	Protocol: ZigBee
	Timestamp: 11:51:16.742244
	Time Delta: 0.004240
	Channel: 21
	Length: 28
	Link Quality: -47 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817778000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 119
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:17.412004]	Beacon Request	03-08-35-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 189
	Protocol: ZigBee
	Timestamp: 11:51:17.412004
	Time Delta: 0.669760
	Channel: 21
	Length: 10
	Link Quality: -25 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF350803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 53
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:17.416980]	Beacon	00-80-08-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 190
	Protocol: ZigBee
	Timestamp: 11:51:17.416980
	Time Delta: 0.004976
	Channel: 21
	Length: 28
	Link Quality: -37 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817088000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 8
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:17.440668]	Link Status	41-88-53-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-C6-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 191
	Protocol: ZigBee
	Timestamp: 11:51:17.440668
	Time Delta: 0.023688
	Channel: 21
	Length: 35
	Link Quality: -48 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 83
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 198
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:18.493652]	Beacon Request	03-08-3E-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 192
	Protocol: ZigBee
	Timestamp: 11:51:18.493652
	Time Delta: 1.052984
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF3E0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 62
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:18.499252]	Beacon	00-80-79-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 193
	Protocol: ZigBee
	Timestamp: 11:51:18.499252
	Time Delta: 0.005600
	Channel: 21
	Length: 28
	Link Quality: -42 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817798000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 121
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:19.112404]	Beacon Request	03-08-43-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 194
	Protocol: ZigBee
	Timestamp: 11:51:19.112404
	Time Delta: 0.613152
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF430803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 67
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:19.116012]	Beacon	00-80-7A-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 195
	Protocol: ZigBee
	Timestamp: 11:51:19.116012
	Time Delta: 0.003608
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F8177A8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 122
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:19.117420]	Beacon	00-80-0D-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 196
	Protocol: ZigBee
	Timestamp: 11:51:19.117420
	Time Delta: 0.001408
	Channel: 21
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F8170D8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 13
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:19.119212]	Beacon	00-80-0A-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 197
	Protocol: ZigBee
	Timestamp: 11:51:19.119212
	Time Delta: 0.001792
	Channel: 21
	Length: 28
	Link Quality: -42 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F8170A8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 10
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:19.654484]	Beacon Request	03-08-48-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 198
	Protocol: ZigBee
	Timestamp: 11:51:19.654484
	Time Delta: 0.535272
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF480803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 72
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:19.657076]	Beacon	00-80-0B-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 199
	Protocol: ZigBee
	Timestamp: 11:51:19.657076
	Time Delta: 0.002592
	Channel: 21
	Length: 28
	Link Quality: -42 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F8170B8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 11
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:19.660828]	Beacon	00-80-7B-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 200
	Protocol: ZigBee
	Timestamp: 11:51:19.660828
	Time Delta: 0.003752
	Channel: 21
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F8177B8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 123
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:19.663476]	Beacon	00-80-0E-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 201
	Protocol: ZigBee
	Timestamp: 11:51:19.663476
	Time Delta: 0.002648
	Channel: 21
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F8170E8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 14
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:20.648284]	Beacon Request	03-08-51-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 202
	Protocol: ZigBee
	Timestamp: 11:51:20.648284
	Time Delta: 0.984808
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF510803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 81
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:20.650964]	Beacon	00-80-7C-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 203
	Protocol: ZigBee
	Timestamp: 11:51:20.650964
	Time Delta: 0.002680
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F8177C8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 124
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:20.652484]	Beacon	00-80-0F-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 204
	Protocol: ZigBee
	Timestamp: 11:51:20.652484
	Time Delta: 0.001520
	Channel: 21
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F8170F8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 15
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:20.654228]	Beacon	00-80-0C-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 205
	Protocol: ZigBee
	Timestamp: 11:51:20.654228
	Time Delta: 0.001744
	Channel: 21
	Length: 28
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F8170C8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 12
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:20.907548]	Link Status	41-88-A3-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-F7-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 206
	Protocol: ZigBee
	Timestamp: 11:51:20.907548
	Time Delta: 0.253320
	Channel: 21
	Length: 35
	Link Quality: -44 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 163
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 247
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:21.368268]	Beacon Request	03-08-56-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 207
	Protocol: ZigBee
	Timestamp: 11:51:21.368268
	Time Delta: 0.460720
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF560803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 86
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:21.370956]	Beacon	00-80-0D-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 208
	Protocol: ZigBee
	Timestamp: 11:51:21.370956
	Time Delta: 0.002688
	Channel: 21
	Length: 28
	Link Quality: -42 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F8170D8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 13
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:21.372772]	Beacon	00-80-7D-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 209
	Protocol: ZigBee
	Timestamp: 11:51:21.372772
	Time Delta: 0.001816
	Channel: 21
	Length: 28
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F8177D8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 125
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:21.375540]	Beacon	00-80-10-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 210
	Protocol: ZigBee
	Timestamp: 11:51:21.375540
	Time Delta: 0.002768
	Channel: 21
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817108000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 16
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:21.379004]	Link Status	41-88-27-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-18-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 211
	Protocol: ZigBee
	Timestamp: 11:51:21.379004
	Time Delta: 0.003464
	Channel: 21
	Length: 35
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 39
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 24
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:22.008732]	Beacon Request	03-08-5B-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 212
	Protocol: ZigBee
	Timestamp: 11:51:22.008732
	Time Delta: 0.629728
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF5B0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 91
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:22.012052]	Beacon	00-80-7E-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 213
	Protocol: ZigBee
	Timestamp: 11:51:22.012052
	Time Delta: 0.003320
	Channel: 21
	Length: 28
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F8177E8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 126
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:22.021892]	Beacon	00-80-0E-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 214
	Protocol: ZigBee
	Timestamp: 11:51:22.021892
	Time Delta: 0.009840
	Channel: 21
	Length: 28
	Link Quality: -42 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F8170E8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 14
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:22.027172]	Beacon	00-80-11-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 215
	Protocol: ZigBee
	Timestamp: 11:51:22.027172
	Time Delta: 0.005280
	Channel: 21
	Length: 28
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817118000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 17
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:23.028964]	Beacon Request	03-08-64-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 216
	Protocol: ZigBee
	Timestamp: 11:51:23.028964
	Time Delta: 1.001792
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF640803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 100
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:23.038260]	Beacon	00-80-7F-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 217
	Protocol: ZigBee
	Timestamp: 11:51:23.038260
	Time Delta: 0.009296
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F8177F8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 127
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:23.705940]	Beacon Request	03-08-69-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 218
	Protocol: ZigBee
	Timestamp: 11:51:23.705940
	Time Delta: 0.667680
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF690803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 105
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:23.709404]	Beacon	00-80-80-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 219
	Protocol: ZigBee
	Timestamp: 11:51:23.709404
	Time Delta: 0.003464
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817808000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 128
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:23.714620]	Beacon	00-80-13-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 220
	Protocol: ZigBee
	Timestamp: 11:51:23.714620
	Time Delta: 0.005216
	Channel: 21
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817138000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 19
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:24.407716]	Beacon Request	03-08-6E-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 221
	Protocol: ZigBee
	Timestamp: 11:51:24.407716
	Time Delta: 0.693096
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF6E0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 110
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:24.410892]	Beacon	00-80-11-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 222
	Protocol: ZigBee
	Timestamp: 11:51:24.410892
	Time Delta: 0.003176
	Channel: 21
	Length: 28
	Link Quality: -44 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817118000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 17
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:24.416612]	Beacon	00-80-81-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 223
	Protocol: ZigBee
	Timestamp: 11:51:24.416612
	Time Delta: 0.005720
	Channel: 21
	Length: 28
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817818000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 129
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:24.418796]	Beacon	00-80-14-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 224
	Protocol: ZigBee
	Timestamp: 11:51:24.418796
	Time Delta: 0.002184
	Channel: 21
	Length: 28
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817148000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 20
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:25.448620]	Beacon Request	03-08-77-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 225
	Protocol: ZigBee
	Timestamp: 11:51:25.448620
	Time Delta: 1.029824
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF770803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 119
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:25.451644]	Beacon	00-80-82-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 226
	Protocol: ZigBee
	Timestamp: 11:51:25.451644
	Time Delta: 0.003024
	Channel: 21
	Length: 28
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817828000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 130
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:25.453564]	Beacon	00-80-15-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 227
	Protocol: ZigBee
	Timestamp: 11:51:25.453564
	Time Delta: 0.001920
	Channel: 21
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817158000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 21
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:26.088428]	Beacon Request	03-08-7C-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 228
	Protocol: ZigBee
	Timestamp: 11:51:26.088428
	Time Delta: 0.634864
	Channel: 21
	Length: 10
	Link Quality: -22 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF7C0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 124
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:26.092892]	Beacon	00-80-13-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 229
	Protocol: ZigBee
	Timestamp: 11:51:26.092892
	Time Delta: 0.004464
	Channel: 21
	Length: 28
	Link Quality: -43 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817138000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 19
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:26.813332]	Beacon Request	03-08-81-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 230
	Protocol: ZigBee
	Timestamp: 11:51:26.813332
	Time Delta: 0.720440
	Channel: 21
	Length: 10
	Link Quality: -22 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF810803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 129
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:27.847748]	Beacon Request	03-08-8A-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 231
	Protocol: ZigBee
	Timestamp: 11:51:27.847748
	Time Delta: 1.034416
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF8A0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 138
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:27.851300]	Beacon	00-80-85-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 232
	Protocol: ZigBee
	Timestamp: 11:51:27.851300
	Time Delta: 0.003552
	Channel: 21
	Length: 28
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817858000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 133
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:27.853140]	Beacon	00-80-15-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 233
	Protocol: ZigBee
	Timestamp: 11:51:27.853140
	Time Delta: 0.001840
	Channel: 21
	Length: 28
	Link Quality: -42 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817158000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 21
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:27.855732]	Beacon	00-80-18-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 234
	Protocol: ZigBee
	Timestamp: 11:51:27.855732
	Time Delta: 0.002592
	Channel: 21
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817188000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 24
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:28.506500]	Beacon Request	03-08-8F-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 235
	Protocol: ZigBee
	Timestamp: 11:51:28.506500
	Time Delta: 0.650768
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF8F0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 143
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:28.509436]	Beacon	00-80-86-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 236
	Protocol: ZigBee
	Timestamp: 11:51:28.509436
	Time Delta: 0.002936
	Channel: 21
	Length: 28
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817868000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 134
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:28.514236]	Beacon	00-80-16-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 237
	Protocol: ZigBee
	Timestamp: 11:51:28.514236
	Time Delta: 0.004800
	Channel: 21
	Length: 28
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817168000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 22
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:28.519740]	Beacon	00-80-19-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 238
	Protocol: ZigBee
	Timestamp: 11:51:28.519740
	Time Delta: 0.005504
	Channel: 21
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F817198000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 25
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:29.109420]	Beacon Request	03-08-94-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 239
	Protocol: ZigBee
	Timestamp: 11:51:29.109420
	Time Delta: 0.589680
	Channel: 21
	Length: 10
	Link Quality: -23 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF940803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 148
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:29.112404]	Beacon	00-80-17-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 240
	Protocol: ZigBee
	Timestamp: 11:51:29.112404
	Time Delta: 0.002984
	Channel: 21
	Length: 28
	Link Quality: -42 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817178000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 23
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:29.114124]	Beacon	00-80-87-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 241
	Protocol: ZigBee
	Timestamp: 11:51:29.114124
	Time Delta: 0.001720
	Channel: 21
	Length: 28
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817878000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 135
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:29.116092]	Beacon	00-80-1A-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 242
	Protocol: ZigBee
	Timestamp: 11:51:29.116092
	Time Delta: 0.001968
	Channel: 21
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F8171A8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 26
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:30.138180]	Beacon Request	03-08-9D-FF-FF-FF-FF-07-FF-FF
Frame Information: (10 bytes)
	Packet Number: 243
	Protocol: ZigBee
	Timestamp: 11:51:30.138180
	Time Delta: 1.022088
	Channel: 21
	Length: 10
	Link Quality: -22 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0xFFFFFFFF9D0803
	Frame Control: 0x0803
		···· ···· ···· ·011 = Frame Type: [0x3] MAC Command
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 157
	Destination PAN ID: 0xFFFF
	Destination Address: 0xFFFF
MAC Payload: 0x07
	Command Frame ID: [0x07] Beacon Request
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:30.143156]	Beacon	00-80-88-17-F8-47-C8-FF-0F-00-00-00-22-9C-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 244
	Protocol: ZigBee
	Timestamp: 11:51:30.143156
	Time Delta: 0.004976
	Channel: 21
	Length: 28
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0xC847F817888000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 136
	Source PAN ID: 0xF817
	Source Address: 0xC847
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9C22
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 1··· ···· ···· = Device Depth: 0x3
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:30.149188]	Beacon	00-80-18-17-F8-00-00-FF-4F-00-00-00-22-84-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 245
	Protocol: ZigBee
	Timestamp: 11:51:30.149188
	Time Delta: 0.006032
	Channel: 21
	Length: 28
	Link Quality: -42 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x0000F817188000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 24
	Source PAN ID: 0xF817
	Source Address: 0x0000
MAC Payload: (19 bytes)
	Super Frame Specification: 0x4FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·1·· ···· ···· ···· = PAN Coordinator: [0x1] Yes
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x8422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·000 0··· ···· ···· = Device Depth: 0x0
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:30.153700]	Beacon	00-80-1B-17-F8-E0-7A-FF-0F-00-00-00-22-94-94-AB-C6-01-00-4B-12-00-FF-FF-FF-00-FF-FF
Frame Information: (28 bytes)
	Packet Number: 246
	Protocol: ZigBee
	Timestamp: 11:51:30.153700
	Time Delta: 0.004512
	Channel: 21
	Length: 28
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: 0x7AE0F8171B8000
	Frame Control: 0x8000
		···· ···· ···· ·000 = Frame Type: [0x0] Beacon
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 27
	Source PAN ID: 0xF817
	Source Address: 0x7AE0
MAC Payload: (19 bytes)
	Super Frame Specification: 0x0FFF
		···· ···· ···· 1111 = Beacon Order: 0xF
		···· ···· 1111 ···· = Super Frame Order: 0xF
		···· 1111 ···· ···· = Final Capacity Slot: 0xF
		···0 ···· ···· ···· = Battery Life Extension: [0x0] No
		··0· ···· ···· ···· = Reserved: 0x0
		·0·· ···· ···· ···· = PAN Coordinator: [0x0] No
		0··· ···· ···· ···· = Association Permit: [0x0] No
	GTS Fields: 0x00
		GTS Specifications: 0x00
			···· ·000 = GTS Descriptor Count: 0x0
			·000 0··· = Reserved: 0x0
			0··· ···· = GTS Permit: [0x0] No
	Pending Addresses Fields: 0x00
		Pending Addresses Specification: 0x00
			···· ·000 = Pending Short Addresses Count: 0x0
			···· 0··· = Reserved: 0x0
			·000 ···· = Pending Extended Addresses Count: 0x0
			0··· ···· = Reserved: 0x0
	Beacon Payload: (15 bytes)
		Protocol ID: [0x00] ZigBee
		NWK Layer Information: 0x9422
			···· ···· ···· 0010 = Stack Profile: 0x2
			···· ···· 0010 ···· = NWK Protocol Version: 0x2
			···· ··00 ···· ···· = Reserved: 0x0
			···· ·1·· ···· ···· = Router Capacity: [0x1] Yes
			·001 0··· ···· ···· = Device Depth: 0x2
			1··· ···· ···· ···· = End Device Capacity: [0x1] Yes
		NWK Extended PAN ID: 00:12:4B:00:01:C6:AB:94
		Tx Offset: 0xFFFFFF
		NWK Update ID: 0x00
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:32.534716]	Link Status	41-88-54-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-C7-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 247
	Protocol: ZigBee
	Timestamp: 11:51:32.534716
	Time Delta: 2.381016
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 84
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 199
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:35.911804]	Link Status	41-88-A4-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-F8-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 248
	Protocol: ZigBee
	Timestamp: 11:51:35.911804
	Time Delta: 3.377088
	Channel: 21
	Length: 35
	Link Quality: -44 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 164
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 248
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:36.424908]	Link Status	41-88-28-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-19-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 249
	Protocol: ZigBee
	Timestamp: 11:51:36.424908
	Time Delta: 0.513104
	Channel: 21
	Length: 35
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 40
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 25
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:47.628884]	Link Status	41-88-55-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-C8-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 250
	Protocol: ZigBee
	Timestamp: 11:51:47.628884
	Time Delta: 11.203976
	Channel: 21
	Length: 35
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 85
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 200
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:50.914980]	Link Status	41-88-A5-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-F9-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 251
	Protocol: ZigBee
	Timestamp: 11:51:50.914980
	Time Delta: 3.286096
	Channel: 21
	Length: 35
	Link Quality: -43 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 165
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 249
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:51:51.479012]	Link Status	41-88-29-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-1A-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 252
	Protocol: ZigBee
	Timestamp: 11:51:51.479012
	Time Delta: 0.564032
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 41
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 26
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:52:02.718732]	Link Status	41-88-56-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-C9-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 253
	Protocol: ZigBee
	Timestamp: 11:52:02.718732
	Time Delta: 11.239720
	Channel: 21
	Length: 35
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 86
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 201
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:52:05.918500]	Link Status	41-88-A6-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-FA-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 254
	Protocol: ZigBee
	Timestamp: 11:52:05.918500
	Time Delta: 3.199768
	Channel: 21
	Length: 35
	Link Quality: -43 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 166
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 250
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:52:06.533820]	Link Status	41-88-2A-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-1B-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 255
	Protocol: ZigBee
	Timestamp: 11:52:06.533820
	Time Delta: 0.615320
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 42
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 27
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:52:17.811460]	Link Status	41-88-57-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-CA-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 256
	Protocol: ZigBee
	Timestamp: 11:52:17.811460
	Time Delta: 11.277640
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 87
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 202
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:52:20.921468]	Link Status	41-88-A7-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-FB-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 257
	Protocol: ZigBee
	Timestamp: 11:52:20.921468
	Time Delta: 3.110008
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 167
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 251
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:52:21.586828]	Link Status	41-88-2B-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-1C-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 258
	Protocol: ZigBee
	Timestamp: 11:52:21.586828
	Time Delta: 0.665360
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 43
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 28
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:52:32.903172]	Link Status	41-88-58-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-CB-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 259
	Protocol: ZigBee
	Timestamp: 11:52:32.903172
	Time Delta: 11.316344
	Channel: 21
	Length: 35
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 88
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 203
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:52:35.925396]	Link Status	41-88-A8-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-FC-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 260
	Protocol: ZigBee
	Timestamp: 11:52:35.925396
	Time Delta: 3.022224
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 168
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 252
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:52:36.639372]	Link Status	41-88-2C-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-1D-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 261
	Protocol: ZigBee
	Timestamp: 11:52:36.639372
	Time Delta: 0.713976
	Channel: 21
	Length: 35
	Link Quality: -37 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 44
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 29
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:52:47.996140]	Link Status	41-88-59-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-CC-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 262
	Protocol: ZigBee
	Timestamp: 11:52:47.996140
	Time Delta: 11.356768
	Channel: 21
	Length: 35
	Link Quality: -42 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 89
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 204
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:52:51.702988]	Link Status	41-88-2D-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-1E-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 263
	Protocol: ZigBee
	Timestamp: 11:52:51.702988
	Time Delta: 3.706848
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 45
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 30
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:03.088004]	Link Status	41-88-5A-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-CD-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 264
	Protocol: ZigBee
	Timestamp: 11:53:03.088004
	Time Delta: 11.385016
	Channel: 21
	Length: 35
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 90
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 205
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:03.275764]	Link Status	41-88-AA-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-FD-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 265
	Protocol: ZigBee
	Timestamp: 11:53:03.275764
	Time Delta: 0.187760
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 170
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 253
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:05.929956]	Link Status	41-88-AB-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-FE-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 266
	Protocol: ZigBee
	Timestamp: 11:53:05.929956
	Time Delta: 2.654192
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 171
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 254
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:06.747452]	Link Status	41-88-2E-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-1F-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 267
	Protocol: ZigBee
	Timestamp: 11:53:06.747452
	Time Delta: 0.817496
	Channel: 21
	Length: 35
	Link Quality: -37 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 46
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 31
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:18.180092]	Link Status	41-88-5B-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-CE-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 268
	Protocol: ZigBee
	Timestamp: 11:53:18.180092
	Time Delta: 11.432640
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 91
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 206
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:20.933700]	Link Status	41-88-AC-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-FF-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 269
	Protocol: ZigBee
	Timestamp: 11:53:20.933700
	Time Delta: 2.753608
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 172
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 255
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:21.799964]	Link Status	41-88-2F-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-20-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 270
	Protocol: ZigBee
	Timestamp: 11:53:21.799964
	Time Delta: 0.866264
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 47
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 32
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:33.272964]	Link Status	41-88-5C-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-CF-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 271
	Protocol: ZigBee
	Timestamp: 11:53:33.272964
	Time Delta: 11.473000
	Channel: 21
	Length: 35
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 92
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 207
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:35.936756]	Link Status	41-88-AD-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-00-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 272
	Protocol: ZigBee
	Timestamp: 11:53:35.936756
	Time Delta: 2.663792
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 173
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 0
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:36.853836]	Link Status	41-88-30-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-21-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 273
	Protocol: ZigBee
	Timestamp: 11:53:36.853836
	Time Delta: 0.917080
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 48
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 33
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:48.366428]	Link Status	41-88-5D-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-D0-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 274
	Protocol: ZigBee
	Timestamp: 11:53:48.366428
	Time Delta: 11.512592
	Channel: 21
	Length: 35
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 93
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 208
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:50.940308]	Link Status	41-88-AE-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-01-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 275
	Protocol: ZigBee
	Timestamp: 11:53:50.940308
	Time Delta: 2.573880
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 174
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 1
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:53:51.908572]	Link Status	41-88-31-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-22-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 276
	Protocol: ZigBee
	Timestamp: 11:53:51.908572
	Time Delta: 0.968264
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 49
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 34
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:03.459820]	Link Status	41-88-5E-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-D1-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 277
	Protocol: ZigBee
	Timestamp: 11:54:03.459820
	Time Delta: 11.551248
	Channel: 21
	Length: 35
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 94
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 209
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:05.943620]	Link Status	41-88-AF-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-02-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 278
	Protocol: ZigBee
	Timestamp: 11:54:05.943620
	Time Delta: 2.483800
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 175
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 2
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:06.961180]	Link Status	41-88-32-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-23-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 279
	Protocol: ZigBee
	Timestamp: 11:54:06.961180
	Time Delta: 1.017560
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 50
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 35
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:18.549732]	Link Status	41-88-5F-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-D2-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 280
	Protocol: ZigBee
	Timestamp: 11:54:18.549732
	Time Delta: 11.588552
	Channel: 21
	Length: 35
	Link Quality: -37 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 95
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 210
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:20.948012]	Link Status	41-88-B0-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-03-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 281
	Protocol: ZigBee
	Timestamp: 11:54:20.948012
	Time Delta: 2.398280
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 176
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 3
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:22.015868]	Link Status	41-88-33-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-24-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 282
	Protocol: ZigBee
	Timestamp: 11:54:22.015868
	Time Delta: 1.067856
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 51
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 36
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:33.642148]	Link Status	41-88-60-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-D3-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 283
	Protocol: ZigBee
	Timestamp: 11:54:33.642148
	Time Delta: 11.626280
	Channel: 21
	Length: 35
	Link Quality: -37 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 96
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 211
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:35.950628]	Link Status	41-88-B1-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-04-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 284
	Protocol: ZigBee
	Timestamp: 11:54:35.950628
	Time Delta: 2.308480
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 177
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 4
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:37.068852]	Link Status	41-88-34-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-25-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 285
	Protocol: ZigBee
	Timestamp: 11:54:37.068852
	Time Delta: 1.118224
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 52
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 37
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:37.468036]	Link Status	41-88-37-B2-95-FF-FF-00-00-09-10-FC-FF-00-00-01-5D-86-A9-C6-01-00-4B-12-00-08-61-5D-EF-11-FF-FF
Frame Information: (32 bytes)
	Packet Number: 286
	Protocol: ZigBee
	Timestamp: 11:54:37.468036
	Time Delta: 0.399184
	Channel: 21
	Length: 32
	Link Quality: -71 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 55
	Destination PAN ID: 0x95B2
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (21 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 93
		Source IEEE Address: 00:12:4B:00:01:C6:A9:86
	NWK Payload: 0x11EF5D6108
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x61
			···0 0001 = Entry Count: 0x1
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11EF5D
			Entry 0: 0x11EF5D
				Neighbor Network Address: 0xEF5D
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:48.733940]	Link Status	41-88-61-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-D4-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 287
	Protocol: ZigBee
	Timestamp: 11:54:48.733940
	Time Delta: 11.265904
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 97
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 212
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:50.954908]	Link Status	41-88-B2-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-05-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 288
	Protocol: ZigBee
	Timestamp: 11:54:50.954908
	Time Delta: 2.220968
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 178
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 5
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:52.122796]	Link Status	41-88-35-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-26-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 289
	Protocol: ZigBee
	Timestamp: 11:54:52.122796
	Time Delta: 1.167888
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 53
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 38
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:54:52.488244]	Link Status	41-88-38-B2-95-FF-FF-00-00-09-10-FC-FF-00-00-01-5E-86-A9-C6-01-00-4B-12-00-08-61-5D-EF-11-FF-FF
Frame Information: (32 bytes)
	Packet Number: 290
	Protocol: ZigBee
	Timestamp: 11:54:52.488244
	Time Delta: 0.365448
	Channel: 21
	Length: 32
	Link Quality: -71 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 56
	Destination PAN ID: 0x95B2
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (21 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 94
		Source IEEE Address: 00:12:4B:00:01:C6:A9:86
	NWK Payload: 0x11EF5D6108
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x61
			···0 0001 = Entry Count: 0x1
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11EF5D
			Entry 0: 0x11EF5D
				Neighbor Network Address: 0xEF5D
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:55:03.827788]	Link Status	41-88-62-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-D5-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 291
	Protocol: ZigBee
	Timestamp: 11:55:03.827788
	Time Delta: 11.339544
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 98
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 213
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:55:05.957100]	Link Status	41-88-B3-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-06-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 292
	Protocol: ZigBee
	Timestamp: 11:55:05.957100
	Time Delta: 2.129312
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 179
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 6
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:55:07.178252]	Link Status	41-88-36-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-27-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 293
	Protocol: ZigBee
	Timestamp: 11:55:07.178252
	Time Delta: 1.221152
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 54
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 39
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:55:18.921644]	Link Status	41-88-63-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-D6-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 294
	Protocol: ZigBee
	Timestamp: 11:55:18.921644
	Time Delta: 11.743392
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 99
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 214
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:55:20.961284]	Link Status	41-88-B4-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-07-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 295
	Protocol: ZigBee
	Timestamp: 11:55:20.961284
	Time Delta: 2.039640
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 180
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 7
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:55:34.011332]	Link Status	41-88-64-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-D7-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 296
	Protocol: ZigBee
	Timestamp: 11:55:34.011332
	Time Delta: 13.050048
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 100
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 215
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:55:35.963092]	Link Status	41-88-B5-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-08-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 297
	Protocol: ZigBee
	Timestamp: 11:55:35.963092
	Time Delta: 1.951760
	Channel: 21
	Length: 35
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 181
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 8
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:55:37.285140]	Link Status	41-88-38-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-29-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 298
	Protocol: ZigBee
	Timestamp: 11:55:37.285140
	Time Delta: 1.322048
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 56
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 41
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:55:49.104092]	Link Status	41-88-65-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-D8-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 299
	Protocol: ZigBee
	Timestamp: 11:55:49.104092
	Time Delta: 11.818952
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 101
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 216
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:55:50.964780]	Link Status	41-88-B6-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-09-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 300
	Protocol: ZigBee
	Timestamp: 11:55:50.964780
	Time Delta: 1.860688
	Channel: 21
	Length: 35
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 182
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 9
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:55:52.337932]	Link Status	41-88-39-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-2A-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 301
	Protocol: ZigBee
	Timestamp: 11:55:52.337932
	Time Delta: 1.373152
	Channel: 21
	Length: 35
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 57
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 42
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:04.203516]	Link Status	41-88-66-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-D9-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 302
	Protocol: ZigBee
	Timestamp: 11:56:04.203516
	Time Delta: 11.865584
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 102
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 217
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:05.969124]	Link Status	41-88-B7-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-0A-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 303
	Protocol: ZigBee
	Timestamp: 11:56:05.969124
	Time Delta: 1.765608
	Channel: 21
	Length: 35
	Link Quality: -32 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 183
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 10
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:07.392740]	Link Status	41-88-3A-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-2B-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 304
	Protocol: ZigBee
	Timestamp: 11:56:07.392740
	Time Delta: 1.423616
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 58
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 43
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:19.295916]	Link Status	41-88-67-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-DA-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 305
	Protocol: ZigBee
	Timestamp: 11:56:19.295916
	Time Delta: 11.903176
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 103
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 218
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:20.973012]	Link Status	41-88-B8-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-0B-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 306
	Protocol: ZigBee
	Timestamp: 11:56:20.973012
	Time Delta: 1.677096
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 184
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 11
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:22.446868]	Link Status	41-88-3B-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-2C-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 307
	Protocol: ZigBee
	Timestamp: 11:56:22.446868
	Time Delta: 1.473856
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 59
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 44
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:34.394268]	Link Status	41-88-68-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-DB-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 308
	Protocol: ZigBee
	Timestamp: 11:56:34.394268
	Time Delta: 11.947400
	Channel: 21
	Length: 35
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 104
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 219
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:35.977868]	Link Status	41-88-B9-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-0C-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 309
	Protocol: ZigBee
	Timestamp: 11:56:35.977868
	Time Delta: 1.583600
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 185
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 12
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:37.500644]	Link Status	41-88-3C-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-2D-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 310
	Protocol: ZigBee
	Timestamp: 11:56:37.500644
	Time Delta: 1.522776
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 60
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 45
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:49.475948]	Link Status	41-88-69-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-DC-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 311
	Protocol: ZigBee
	Timestamp: 11:56:49.475948
	Time Delta: 11.975304
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 105
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 220
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:50.981604]	Link Status	41-88-BA-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-0D-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 312
	Protocol: ZigBee
	Timestamp: 11:56:50.981604
	Time Delta: 1.505656
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 186
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 13
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:56:52.553876]	Link Status	41-88-3D-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-2E-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 313
	Protocol: ZigBee
	Timestamp: 11:56:52.553876
	Time Delta: 1.572272
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 61
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 46
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:04.568068]	Link Status	41-88-6A-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-DD-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 314
	Protocol: ZigBee
	Timestamp: 11:57:04.568068
	Time Delta: 12.014192
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 106
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 221
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:05.986156]	Link Status	41-88-BB-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-0E-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 315
	Protocol: ZigBee
	Timestamp: 11:57:05.986156
	Time Delta: 1.418088
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 187
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 14
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:07.606428]	Link Status	41-88-3E-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-2F-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 316
	Protocol: ZigBee
	Timestamp: 11:57:07.606428
	Time Delta: 1.620272
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 62
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 47
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:19.661636]	Link Status	41-88-6B-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-DE-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 317
	Protocol: ZigBee
	Timestamp: 11:57:19.661636
	Time Delta: 12.055208
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 107
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 222
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:20.987676]	Link Status	41-88-BC-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-0F-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 318
	Protocol: ZigBee
	Timestamp: 11:57:20.987676
	Time Delta: 1.326040
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 188
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 15
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:22.660092]	Link Status	41-88-3F-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-30-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 319
	Protocol: ZigBee
	Timestamp: 11:57:22.660092
	Time Delta: 1.672416
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 63
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 48
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:34.753884]	Link Status	41-88-6C-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-DF-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 320
	Protocol: ZigBee
	Timestamp: 11:57:34.753884
	Time Delta: 12.093792
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 108
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 223
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:35.991228]	Link Status	41-88-BD-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-10-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 321
	Protocol: ZigBee
	Timestamp: 11:57:35.991228
	Time Delta: 1.237344
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 189
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 16
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:37.712988]	Link Status	41-88-40-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-31-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 322
	Protocol: ZigBee
	Timestamp: 11:57:37.712988
	Time Delta: 1.721760
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 64
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 49
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:49.847484]	Link Status	41-88-6D-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-E0-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 323
	Protocol: ZigBee
	Timestamp: 11:57:49.847484
	Time Delta: 12.134496
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 109
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 224
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:50.996612]	Link Status	41-88-BE-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-11-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 324
	Protocol: ZigBee
	Timestamp: 11:57:50.996612
	Time Delta: 1.149128
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 190
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 17
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:57:52.764388]	Link Status	41-88-41-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-32-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 325
	Protocol: ZigBee
	Timestamp: 11:57:52.764388
	Time Delta: 1.767776
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 65
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 50
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:04.938124]	Link Status	41-88-6E-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-E1-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 326
	Protocol: ZigBee
	Timestamp: 11:58:04.938124
	Time Delta: 12.173736
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 110
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 225
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:05.999988]	Link Status	41-88-BF-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-12-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 327
	Protocol: ZigBee
	Timestamp: 11:58:05.999988
	Time Delta: 1.061864
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 191
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 18
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:07.819812]	Link Status	41-88-42-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-33-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 328
	Protocol: ZigBee
	Timestamp: 11:58:07.819812
	Time Delta: 1.819824
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 66
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 51
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:20.029228]	Link Status	41-88-6F-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-E2-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 329
	Protocol: ZigBee
	Timestamp: 11:58:20.029228
	Time Delta: 12.209416
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 111
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 226
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:21.004100]	Link Status	41-88-C0-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-13-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 330
	Protocol: ZigBee
	Timestamp: 11:58:21.004100
	Time Delta: 0.974872
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 192
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 19
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:22.872660]	Link Status	41-88-43-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-34-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 331
	Protocol: ZigBee
	Timestamp: 11:58:22.872660
	Time Delta: 1.868560
	Channel: 21
	Length: 35
	Link Quality: -36 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 67
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 52
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:35.121956]	Link Status	41-88-70-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-E3-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 332
	Protocol: ZigBee
	Timestamp: 11:58:35.121956
	Time Delta: 12.249296
	Channel: 21
	Length: 35
	Link Quality: -36 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 112
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 227
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:36.008028]	Link Status	41-88-C1-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-14-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 333
	Protocol: ZigBee
	Timestamp: 11:58:36.008028
	Time Delta: 0.886072
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 193
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 20
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:37.924908]	Link Status	41-88-44-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-35-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 334
	Protocol: ZigBee
	Timestamp: 11:58:37.924908
	Time Delta: 1.916880
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 68
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 53
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:50.215436]	Link Status	41-88-71-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-E4-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 335
	Protocol: ZigBee
	Timestamp: 11:58:50.215436
	Time Delta: 12.290528
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 113
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 228
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:51.010876]	Link Status	41-88-C2-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-15-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 336
	Protocol: ZigBee
	Timestamp: 11:58:51.010876
	Time Delta: 0.795440
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 194
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 21
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:58:52.978236]	Link Status	41-88-45-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-36-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 337
	Protocol: ZigBee
	Timestamp: 11:58:52.978236
	Time Delta: 1.967360
	Channel: 21
	Length: 35
	Link Quality: -34 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 69
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 54
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:05.308876]	Link Status	41-88-72-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-E5-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 338
	Protocol: ZigBee
	Timestamp: 11:59:05.308876
	Time Delta: 12.330640
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 114
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 229
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:06.016492]	Link Status	41-88-C3-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-16-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 339
	Protocol: ZigBee
	Timestamp: 11:59:06.016492
	Time Delta: 0.707616
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 195
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 22
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:08.036132]	Link Status	41-88-46-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-37-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 340
	Protocol: ZigBee
	Timestamp: 11:59:08.036132
	Time Delta: 2.019640
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 70
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 55
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:20.399604]	Link Status	41-88-73-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-E6-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 341
	Protocol: ZigBee
	Timestamp: 11:59:20.399604
	Time Delta: 12.363472
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 115
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 230
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:21.019012]	Link Status	41-88-C4-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-17-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 342
	Protocol: ZigBee
	Timestamp: 11:59:21.019012
	Time Delta: 0.619408
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 196
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 23
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:23.087780]	Link Status	41-88-47-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-38-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 343
	Protocol: ZigBee
	Timestamp: 11:59:23.087780
	Time Delta: 2.068768
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 71
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 56
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:35.493804]	Link Status	41-88-74-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-E7-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 344
	Protocol: ZigBee
	Timestamp: 11:59:35.493804
	Time Delta: 12.406024
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 116
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 231
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:36.023268]	Link Status	41-88-C5-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-18-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 345
	Protocol: ZigBee
	Timestamp: 11:59:36.023268
	Time Delta: 0.529464
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 197
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 24
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:38.141604]	Link Status	41-88-48-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-39-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 346
	Protocol: ZigBee
	Timestamp: 11:59:38.141604
	Time Delta: 2.118336
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 72
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 57
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:42.995148]	Acknowledgement	02-00-2F-FF-FF
Frame Information: (5 bytes)
	Packet Number: 347
	Protocol: ZigBee
	Timestamp: 11:59:42.995148
	Time Delta: 4.853544
	Channel: 21
	Length: 5
	Link Quality: -70 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0x2F0002
	Frame Control: 0x0002
		···· ···· ···· ·010 = Frame Type: [0x2] Acknowledgement
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 47
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:50.586828]	Link Status	41-88-75-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-E8-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 348
	Protocol: ZigBee
	Timestamp: 11:59:50.586828
	Time Delta: 7.591680
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 117
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 232
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:51.028636]	Link Status	41-88-C6-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-19-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 349
	Protocol: ZigBee
	Timestamp: 11:59:51.028636
	Time Delta: 0.441808
	Channel: 21
	Length: 35
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 198
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 25
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[11:59:53.194124]	Link Status	41-88-49-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-3A-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 350
	Protocol: ZigBee
	Timestamp: 11:59:53.194124
	Time Delta: 2.165488
	Channel: 21
	Length: 35
	Link Quality: -44 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 73
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 58
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:05.677868]	Link Status	41-88-76-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-E9-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 351
	Protocol: ZigBee
	Timestamp: 12:00:05.677868
	Time Delta: 12.483744
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 118
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 233
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:06.031300]	Link Status	41-88-C7-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-1A-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 352
	Protocol: ZigBee
	Timestamp: 12:00:06.031300
	Time Delta: 0.353432
	Channel: 21
	Length: 35
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 199
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 26
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:07.995180]	Link Status	41-88-4D-B2-95-FF-FF-00-00-09-10-FC-FF-00-00-01-73-86-A9-C6-01-00-4B-12-00-08-61-5D-EF-11-FF-FF
Frame Information: (32 bytes)
	Packet Number: 353
	Protocol: ZigBee
	Timestamp: 12:00:07.995180
	Time Delta: 1.963880
	Channel: 21
	Length: 32
	Link Quality: -71 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 77
	Destination PAN ID: 0x95B2
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (21 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 115
		Source IEEE Address: 00:12:4B:00:01:C6:A9:86
	NWK Payload: 0x11EF5D6108
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x61
			···0 0001 = Entry Count: 0x1
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11EF5D
			Entry 0: 0x11EF5D
				Neighbor Network Address: 0xEF5D
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:08.248380]	Link Status	41-88-4A-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-3B-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 354
	Protocol: ZigBee
	Timestamp: 12:00:08.248380
	Time Delta: 0.253200
	Channel: 21
	Length: 35
	Link Quality: -45 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 74
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 59
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:21.035372]	Link Status	41-88-C8-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-1B-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 355
	Protocol: ZigBee
	Timestamp: 12:00:21.035372
	Time Delta: 12.786992
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 200
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 27
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:23.300620]	Link Status	41-88-4B-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-3C-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 356
	Protocol: ZigBee
	Timestamp: 12:00:23.300620
	Time Delta: 2.265248
	Channel: 21
	Length: 35
	Link Quality: -47 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 75
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 60
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:35.864084]	Link Status	41-88-78-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-EB-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 357
	Protocol: ZigBee
	Timestamp: 12:00:35.864084
	Time Delta: 12.563464
	Channel: 21
	Length: 35
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 120
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 235
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:36.039292]	Link Status	41-88-C9-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-1C-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 358
	Protocol: ZigBee
	Timestamp: 12:00:36.039292
	Time Delta: 0.175208
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 201
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 28
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:38.353292]	Link Status	41-88-4C-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-3D-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 359
	Protocol: ZigBee
	Timestamp: 12:00:38.353292
	Time Delta: 2.314000
	Channel: 21
	Length: 35
	Link Quality: -46 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 76
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 61
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:50.956732]	Link Status	41-88-79-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-EC-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 360
	Protocol: ZigBee
	Timestamp: 12:00:50.956732
	Time Delta: 12.603440
	Channel: 21
	Length: 35
	Link Quality: -44 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 121
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 236
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:51.043716]	Link Status	41-88-CA-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-1D-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 361
	Protocol: ZigBee
	Timestamp: 12:00:51.043716
	Time Delta: 0.086984
	Channel: 21
	Length: 35
	Link Quality: -40 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 202
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 29
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:53.406484]	Link Status	41-88-4D-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-3E-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 362
	Protocol: ZigBee
	Timestamp: 12:00:53.406484
	Time Delta: 2.362768
	Channel: 21
	Length: 35
	Link Quality: -49 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 77
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 62
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:00:55.195268]	Acknowledgement	02-00-53-FF-FF
Frame Information: (5 bytes)
	Packet Number: 363
	Protocol: ZigBee
	Timestamp: 12:00:55.195268
	Time Delta: 1.788784
	Channel: 21
	Length: 5
	Link Quality: -71 dBm
	Source: USB5172
	Layer: MAC
	Status: Normal
MAC Header: 0x530002
	Frame Control: 0x0002
		···· ···· ···· ·010 = Frame Type: [0x2] Acknowledgement
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·0·· ···· = Intra-PAN: [0x0] No
		···· ··00 0··· ···· = Reserved: 0x0
		···· 00·· ···· ···· = Destination Addr Mode: [0x0] No Address
		··00 ···· ···· ···· = Reserved: 0x0
		00·· ···· ···· ···· = Source Addr Mode: [0x0] No Address
	Sequence Number: 83
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:01:06.045620]	Link Status	41-88-CB-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-1E-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 364
	Protocol: ZigBee
	Timestamp: 12:01:06.045620
	Time Delta: 10.850352
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 203
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 30
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:01:06.049708]	Link Status	41-88-7A-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-ED-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 365
	Protocol: ZigBee
	Timestamp: 12:01:06.049708
	Time Delta: 0.004088
	Channel: 21
	Length: 35
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 122
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 237
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:01:08.459132]	Link Status	41-88-4E-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-3F-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 366
	Protocol: ZigBee
	Timestamp: 12:01:08.459132
	Time Delta: 2.409424
	Channel: 21
	Length: 35
	Link Quality: -48 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 78
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 63
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:01:21.051348]	Link Status	41-88-CC-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-1F-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 367
	Protocol: ZigBee
	Timestamp: 12:01:21.051348
	Time Delta: 12.592216
	Channel: 21
	Length: 35
	Link Quality: -41 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 204
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 31
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:01:21.142084]	Link Status	41-88-7B-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-EE-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 368
	Protocol: ZigBee
	Timestamp: 12:01:21.142084
	Time Delta: 0.090736
	Channel: 21
	Length: 35
	Link Quality: -39 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 123
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 238
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:01:23.513884]	Link Status	41-88-4F-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-40-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 369
	Protocol: ZigBee
	Timestamp: 12:01:23.513884
	Time Delta: 2.371800
	Channel: 21
	Length: 35
	Link Quality: -35 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 79
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 64
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:01:36.053252]	Link Status	41-88-CD-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-20-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 370
	Protocol: ZigBee
	Timestamp: 12:01:36.053252
	Time Delta: 12.539368
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 205
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 32
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:01:36.234068]	Link Status	41-88-7C-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-EF-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 371
	Protocol: ZigBee
	Timestamp: 12:01:36.234068
	Time Delta: 0.180816
	Channel: 21
	Length: 35
	Link Quality: -38 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 124
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 239
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:01:38.567356]	Link Status	41-88-50-17-F8-FF-FF-E0-7A-09-10-FC-FF-E0-7A-01-41-D3-AB-C6-01-00-4B-12-00-08-62-00-00-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 372
	Protocol: ZigBee
	Timestamp: 12:01:38.567356
	Time Delta: 2.333288
	Channel: 21
	Length: 35
	Link Quality: -33 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 80
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x7AE0
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x7AE0
		Radius: 0x01
		Sequence Number: 65
		Source IEEE Address: 00:12:4B:00:01:C6:AB:D3
	NWK Payload: 0x11C8471100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:01:51.055348]	Link Status	41-88-CE-17-F8-FF-FF-00-00-09-10-FC-FF-00-00-01-21-94-AB-C6-01-00-4B-12-00-08-62-E0-7A-11-47-C8-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 373
	Protocol: ZigBee
	Timestamp: 12:01:51.055348
	Time Delta: 12.487992
	Channel: 21
	Length: 35
	Link Quality: -37 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 206
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0x0000
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0x0000
		Radius: 0x01
		Sequence Number: 33
		Source IEEE Address: 00:12:4B:00:01:C6:AB:94
	NWK Payload: 0x11C847117AE06208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x11C847117AE0
			Entry 0: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x11C847
				Neighbor Network Address: 0xC847
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

[12:01:51.327548]	Link Status	41-88-7D-17-F8-FF-FF-47-C8-09-10-FC-FF-47-C8-01-F0-4E-2C-70-02-00-4B-12-00-08-62-00-00-11-E0-7A-11-FF-FF
Frame Information: (35 bytes)
	Packet Number: 374
	Protocol: ZigBee
	Timestamp: 12:01:51.327548
	Time Delta: 0.272200
	Channel: 21
	Length: 35
	Link Quality: -36 dBm
	Source: USB5172
	Layer: NWK
	Status: Normal
MAC Header: (9 bytes)
	Frame Control: 0x8841
		···· ···· ···· ·001 = Frame Type: [0x1] Data
		···· ···· ···· 0··· = Security Enabled: [0x0] No
		···· ···· ···0 ···· = Frame Pending: [0x0] No
		···· ···· ··0· ···· = Acknowledgement Request: [0x0] No
		···· ···· ·1·· ···· = Intra-PAN: [0x1] Yes
		···· ··00 0··· ···· = Reserved: 0x0
		···· 10·· ···· ···· = Destination Addr Mode: [0x2] 16-bit Short Address
		··00 ···· ···· ···· = Reserved: 0x0
		10·· ···· ···· ···· = Source Addr Mode: [0x2] 16-bit Short Address
	Sequence Number: 125
	Destination PAN ID: 0xF817
	Destination Address: 0xFFFF
	Source Address: 0xC847
MAC Payload: (24 bytes)
	NWK Header: (16 bytes)
		Frame Control: 0x1009
			···· ···· ···· ··01 = Frame Type: [0x1] Command
			···· ···· ··00 10·· = Protocol Version: 0x2
			···· ···· 00·· ···· = Route Discovery: [0x0] Suppressed
			···· ···0 ···· ···· = Multicast Flag: [0x0] Unicast or Broadcast
			···· ··0· ···· ···· = Security Enabled: [0x0] No
			···· ·0·· ···· ···· = Source Route Included: [0x0] No
			···· 0··· ···· ···· = Destination IEEE Address Included: [0x0] No
			···1 ···· ···· ···· = Source IEEE Address Included: [0x1] Yes
			000· ···· ···· ···· = Reserved: 0x0
		Destination Address: 0xFFFC
		Source Address: 0xC847
		Radius: 0x01
		Sequence Number: 240
		Source IEEE Address: 00:12:4B:00:02:70:2C:4E
	NWK Payload: 0x117AE01100006208
		NWK Command ID: [0x08] Link Status
		Link Status Options: 0x62
			···0 0010 = Entry Count: 0x2
			··1· ···· = First Frame: 0x1
			·1·· ···· = Last Frame: 0x1
			0··· ···· = Reserved: 0x0
		Link Status List: 0x117AE0110000
			Entry 0: 0x110000
				Neighbor Network Address: 0x0000
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
			Entry 1: 0x117AE0
				Neighbor Network Address: 0x7AE0
				Link Status: 0x11
					···· ·001 = Incoming Cost: 0x1
					···· 0··· = Reserved: 0x0
					·001 ···· = Outgoing Cost: 0x1
					0··· ···· = Reserved: 0x0
MAC Footer: 0xFFFF
	Frame Check Sequence: 0xFFFF

