2/13/14 Stellaris InstaSpin via Paul's code on DRV3812 with new motor.  PWR supply @ 30V, max current 0.6a.  Everything is OK.

Increase PWM slightly and this happens with LED 6 fault light on.