[image: ]

image1.png
[ Pin Number
attributes: VDD +15

Will Detach: No AGND
Manifest Tolerant: Yos
Upload Capable:  Yes

Dounload Gapable: Yoo
Found 1 device. AGND
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