[Header]
bq EVSW Version = 0.9.65	
DeviceName = bq20z65R1 v1.05
Time = 10/4/2011 2:09:39 AM	


[Voltage(1st Level Safety)]
LT COV Threshold = 4200
LT COV Recovery = 3800
ST COV Threshold = 4400
ST COV Recovery = 4000
HT COV Threshold = 4300
HT COV Recovery = 3900
COV Time = 2
CUV Threshold = 2000
CUV Time = 2
CUV Recovery = 2500
[Current(1st Level Safety)]
OC (1st Tier) Chg = 6500
OC (1st Tier) Chg Time = 2
OC Chg Recovery = 200
OC (1st Tier) Dsg = 6500
OC (1st Tier) Dsg Time = 2
OC Dsg Recovery = 200
OC (2nd Tier) Chg = 6750
OC (2nd Tier) Chg Time = 2
OC (2nd Tier) Dsg = 6750
OC (2nd Tier) Dsg Time = 2
Current Recovery Time = 8
AFE OC Dsg = 03
AFE OC Dsg Time = 0F
AFE OC Dsg Recovery = 5
AFE SC Chg Cfg = 76
AFE SC Dsg Cfg = 76
AFE SC Recovery = 1
[Temperature(1st Level Safety)]
OT1 Chg Threshold = 70.0
OT1 Chg Time = 2
OT1 Chg Recovery = 65.0
OT2 Chg Threshold = 70.0
OT2 Chg Time = 2
OT2 Chg Recovery = 65.0
OT1 Dsg Threshold = 70.0
OT1 Dsg Time = 2
OT1 Dsg Recovery = 65.0
OT2 Dsg Threshold = 70.0
OT2 Dsg Time = 2
OT2 Dsg Recovery = 65.0
Hi Dsg Start Temp = 70.0
[Host Comm(1st Level Safety)]
Host Watchdog Timeout = 0

[Voltage(2nd Level Safety)]
LT SOV Threshold = 4400
ST SOV Threshold = 4600
HT SOV Threshold = 4500
SOV Time = 5
PF SOV Fuse Blow Delay = 5
SUV Threshold = 1000
SUV Time = 5
Rest CIM Current = 5
Rest CIM Fail Voltage = 1000
Rest CIM Time = 5
CIM Battery Rest Time = 1800
Rest CIM Check Voltage = 3000
Active CIM Fail Voltage = 1000
Active CIM Time = 5
Active CIM Check Voltage = 3000
PFIN Detect Time = 5
PF Min Fuse Blow Voltage = 9600
[Current(2nd Level Safety)]
SOC Chg = 7000
SOC Chg Time = 1
SOC Dsg = 7000
SOC Dsg Time = 1
[Temperature(2nd Level Safety)]
SOT1 Chg Threshold = 75.0
SOT1 Chg Time = 5
SOT2 Chg Threshold = 75.0
SOT2 Chg Time = 5
SOT1 Dsg Threshold = 75.0
SOT1 Dsg Time = 5
SOT2 Dsg Threshold = 75.0
SOT2 Dsg Time = 5
Open Thermistor = -33.3
Open Time = 0
[FET Verification(2nd Level Safety)]
FET Fail Limit = 20
FET Fail Time = 5
[AFE Verification(2nd Level Safety)]
AFE Check Time = 0
AFE Fail Limit = 0
AFE Fail Recovery Time = 20
AFE Init Retry Limit = 6
AFE Init Limit = 20
[Fuse Verification(2nd Level Safety)]
Fuse Fail Limit = 2
Fuse Fail Time = 0

[Charge Temp Cfg(Charge Control)]
JT1 = 0.0
JT2 = 10.0
JT2a = 27.5
JT3 = 45.0
JT4 = 70.0
Temp Hys = 1.0
[Pre-Charge Cfg(Charge Control)]
Pre-chg Voltage Threshold = 3000
Pre-chg Recovery Voltage = 3100
Pre-chg Current = 500
[Charge Cfg(Charge Control)]
LT Chg Voltage = 12000
LT Chg Current1 = 250
LT Chg Current2 = 250
LT Chg Current3 = 250
ST1 Chg Voltage = 16800
ST1 Chg Current1 = 6000
ST1 Chg Current2 = 6000
ST1 Chg Current3 = 6000
ST2 Chg Voltage = 16800
ST2 Chg Current1 = 6000
ST2 Chg Current2 = 6000
ST2 Chg Current3 = 6000
HT Chg Voltage = 16800
HT Chg Current1 = 2000
HT Chg Current2 = 2000
HT Chg Current3 = 2000
Cell Voltage Threshold1 = 4100
Cell Voltage Threshold2 = 4200
Cell Voltage Thresh Hys = 10
[Termination Cfg.(Charge Control)]
Maintenance Current = 0
Taper Current = 250
Taper Voltage = 75
Current Taper Window = 40
TCA Set % = -1
TCA Clear % = 95
FC Set % = -1
FC Clear % = 98
[Cell Balancing Cfg(Charge Control)]
Min Cell Deviation = 1350
[Charging Faults(Charge Control)]
Over Charging Voltage = 500
Over Charging Volt Time = 2
Over Charging Current = 500
Over Charging Curr Time = 2
Over Charging Curr Recov = 100
Depleted Voltage = 10000
Depleted Voltage Time = 2
Depleted Recovery = 10500
Over Charge Capacity = 1000
Over Charge Recovery = 2
CMTO = 28800
PCMTO = 3600
Charge Fault Cfg = 00

[Data(SBS Configuration)]
Rem Cap Alarm = 1000
Rem Energy Alarm = 2870
Rem Time Alarm = 10
Init Battery Mode = 0081
Design Voltage = 14400
Spec Info = 0031
Manuf Date = 01-Jun-2011
Ser. Num. = 0056
Cycle Count = 3
CC Threshold = 9000
CC % = 90
CF MaxError Limit = 100
Design Capacity = 10000
Design Energy = 143990
Manuf Name = EIC Labs
Device Name = BP150
Device Chemistry = LION
Deterioration Warn Limit = 50
Deterioration Fault Limit = 30
Cell Life Limit = 20
[Configuration(SBS Configuration)]
TDA Set % = 6
TDA Clear % = 8
FD Set % = 2
FD Clear % = 5
TDA Set Volt Threshold = 3750
TDA Set Volt Time = 5
TDA Clear Volt = 4125
FD Set Volt Threshold = 3750
FD Volt Time = 5
FD Clear Volt = 4125

[Manufacturer Data(System Data)]
Pack Lot Code = 0000
PCB Lot Code = 0000
Firmware Version = 0000
Hardware Revision = 0000
Cell Revision = 0000
[Manufacturer Info(System Data)]
Manuf. Info 0 = BP150
Manuf. Block 1 = 0123456789ABCDEF0123
Manuf. Block 2 = 0123456789ABCDEF0123
Manuf. Block 3 = 0123456789ABCDEF0123
Manuf. Block 4 = 0123456789ABCDEF0123
[Lifetime Data(System Data)]
Lifetime Max Temp = 39.0
Lifetime Min Temp = 19.4
Lifetime Max Cell Voltage = 4214
Lifetime Min Cell Voltage = 1600
Lifetime Max Pack Voltage = 16808
Lifetime Min Pack Voltage = 7918
Lifetime Max Chg Current = 2331
Lifetime Max Dsg Current = -4003
Lifetime Max Chg Power = 32020
Lifetime Max Dsg Power = -62740
Life Max AvgDsg Cur = -5000
Life Max AvgDsg Pow = -7200
Life Avg Temp = 25.5
Life OT Count = 0
Life OT Duration = 0
Life OV Count = 0
Life OV Duration = 0
[Lifetime Temp Samples(System Data)]
LT Temp Samples = 8834

[Registers(Configuration)]
Operation Cfg A = 0F30
Operation Cfg B = 6449
Operation Cfg C = 0170
Permanent Fail Cfg = 0000
Permanent Fail Cfg 2 = 0000
Non-Removable Cfg = 0000
[AFE(Configuration)]
AFE.State_CTL = 00

[LED Cfg(LED Support)]
LED Flash Period = 512
LED Blink Period = 1024
LED Delay = 100
LED Hold Time = 4
CHG Flash Alarm = 10
CHG Thresh 1 = 0
CHG Thresh 2 = 20
CHG Thresh 3 = 40
CHG Thresh 4 = 60
CHG Thresh 5 = 80
DSG Flash Alarm = 10
DSG Thresh 1 = 0
DSG Thresh 2 = 20
DSG Thresh 3 = 40
DSG Thresh 4 = 60
DSG Thresh 5 = 80
Sink Current = 3

[Power(Power)]
Flash Update OK Voltage = 7500
Shutdown Voltage = 7000
Shutdown Time = 10
Cell Shutdown Voltage = 1750
Cell Shutdown Time = 10
Charger Present = 3000
Sleep Current = 10
Bus Low Time = 5
Cal Inhibit Temp Low = 5.0
Cal Inhibit Temp High = 45.0
Sleep Voltage Time = 5
Sleep Current Time = 20
Wake Current Reg = 00
Sealed Ship Delay = 5

[IT Cfg(Gas Gauging)]
Load Select = 4
Load Mode = 1
Term Voltage = 8000
User Rate-mA = 0
User Rate-mW = 0
Reserve Cap-mAh = 0
Reserve Cap-mWh = 0
Ra Max Delta = 44
[Current Thresholds(Gas Gauging)]
Dsg Current Threshold = 100
Chg Current Threshold = 50
Quit Current = 10
Dsg Relax Time = 1
Chg Relax Time = 60
[State(Gas Gauging)]
Qmax Cell 0 = 10334
Qmax Cell 1 = 10399
Qmax Cell 2 = 10427
Qmax Cell 3 = 10410
Qmax Pack = 10334
Update Status = 0E
Cell 0 Chg dod at EoC = 1024
Cell 1 Chg dod at EoC = 1184
Cell 2 Chg dod at EoC = 768
Cell 3 Chg dod at EoC = 944
Avg I Last Run = -3026
Avg P Last Run = -4494
Delta Voltage = 7
Max Avg I Last Run = -3028
Max Avg P Last Run = -4901

[R_a0(Ra Table)]
Cell0 R_a flag = 0000
Cell0 R_a 0 = 31
Cell0 R_a 1 = 33
Cell0 R_a 2 = 42
Cell0 R_a 3 = 51
Cell0 R_a 4 = 41
Cell0 R_a 5 = 40
Cell0 R_a 6 = 46
Cell0 R_a 7 = 35
Cell0 R_a 8 = 39
Cell0 R_a 9 = 46
Cell0 R_a 10 = 41
Cell0 R_a 11 = 32
Cell0 R_a 12 = 11
Cell0 R_a 13 = 12
Cell0 R_a 14 = 127
[R_a1(Ra Table)]
Cell1 R_a flag = 0000
Cell1 R_a 0 = 23
Cell1 R_a 1 = 25
Cell1 R_a 2 = 34
Cell1 R_a 3 = 46
Cell1 R_a 4 = 35
Cell1 R_a 5 = 35
Cell1 R_a 6 = 42
Cell1 R_a 7 = 28
Cell1 R_a 8 = 31
Cell1 R_a 9 = 41
Cell1 R_a 10 = 37
Cell1 R_a 11 = 27
Cell1 R_a 12 = 2
Cell1 R_a 13 = 2
Cell1 R_a 14 = 29
[R_a2(Ra Table)]
Cell2 R_a flag = 0000
Cell2 R_a 0 = 25
Cell2 R_a 1 = 27
Cell2 R_a 2 = 37
Cell2 R_a 3 = 47
Cell2 R_a 4 = 35
Cell2 R_a 5 = 35
Cell2 R_a 6 = 43
Cell2 R_a 7 = 30
Cell2 R_a 8 = 34
Cell2 R_a 9 = 41
Cell2 R_a 10 = 37
Cell2 R_a 11 = 30
Cell2 R_a 12 = 6
Cell2 R_a 13 = 6
Cell2 R_a 14 = 73
[R_a3(Ra Table)]
Cell3 R_a flag = 0055
Cell3 R_a 0 = 34
Cell3 R_a 1 = 36
Cell3 R_a 2 = 47
Cell3 R_a 3 = 55
Cell3 R_a 4 = 45
Cell3 R_a 5 = 45
Cell3 R_a 6 = 51
Cell3 R_a 7 = 39
Cell3 R_a 8 = 43
Cell3 R_a 9 = 52
Cell3 R_a 10 = 46
Cell3 R_a 11 = 42
Cell3 R_a 12 = 26
Cell3 R_a 13 = 29
Cell3 R_a 14 = 286
[R_a0x(Ra Table)]
xCell0 R_a flag = 0055
xCell0 R_a 0 = 31
xCell0 R_a 1 = 33
xCell0 R_a 2 = 42
xCell0 R_a 3 = 51
xCell0 R_a 4 = 41
xCell0 R_a 5 = 40
xCell0 R_a 6 = 46
xCell0 R_a 7 = 35
xCell0 R_a 8 = 39
xCell0 R_a 9 = 46
xCell0 R_a 10 = 41
xCell0 R_a 11 = 35
xCell0 R_a 12 = 12
xCell0 R_a 13 = 13
xCell0 R_a 14 = 139
[R_a1x(Ra Table)]
xCell1 R_a flag = 0055
xCell1 R_a 0 = 23
xCell1 R_a 1 = 25
xCell1 R_a 2 = 34
xCell1 R_a 3 = 46
xCell1 R_a 4 = 35
xCell1 R_a 5 = 35
xCell1 R_a 6 = 42
xCell1 R_a 7 = 28
xCell1 R_a 8 = 31
xCell1 R_a 9 = 41
xCell1 R_a 10 = 37
xCell1 R_a 11 = 31
xCell1 R_a 12 = 2
xCell1 R_a 13 = 2
xCell1 R_a 14 = 33
[R_a2x(Ra Table)]
xCell2 R_a flag = 0055
xCell2 R_a 0 = 25
xCell2 R_a 1 = 27
xCell2 R_a 2 = 37
xCell2 R_a 3 = 47
xCell2 R_a 4 = 35
xCell2 R_a 5 = 35
xCell2 R_a 6 = 43
xCell2 R_a 7 = 30
xCell2 R_a 8 = 34
xCell2 R_a 9 = 41
xCell2 R_a 10 = 37
xCell2 R_a 11 = 34
xCell2 R_a 12 = 7
xCell2 R_a 13 = 7
xCell2 R_a 14 = 83
[R_a3x(Ra Table)]
xCell3 R_a flag = 0000
xCell3 R_a 0 = 34
xCell3 R_a 1 = 36
xCell3 R_a 2 = 47
xCell3 R_a 3 = 55
xCell3 R_a 4 = 45
xCell3 R_a 5 = 45
xCell3 R_a 6 = 51
xCell3 R_a 7 = 39
xCell3 R_a 8 = 43
xCell3 R_a 9 = 52
xCell3 R_a 10 = 46
xCell3 R_a 11 = 42
xCell3 R_a 12 = 15
xCell3 R_a 13 = 17
xCell3 R_a 14 = 165

[Device Status Data(PF Status)]
Saved PF Flags 1 = 0000
Saved PF Flags 2 = 0000
Fuse Flag = 00
PF Voltage = 15984
PF C4 Voltage = 3978
PF C3 Voltage = 4020
PF C2 Voltage = 3997
PF C1 Voltage = 3988
PF Current = -2942
PF Temperature = 312.3
PF Batt Stat = 18C0
PF RC-mAh = 9400
PF RC-10mWh = 140530
PF Chg Status = 1000
PF Safety Status 1 = 8020
PF Safety Status2 = 0000
Saved 1st PF Flags 1 = 0040
Saved 1st PF Flags 2 = 0000
[AFE Regs(PF Status)]
AFE Status = 00
AFE Output = 08
AFE State = 00
AFE Function = 00
AFE Cell Select = 00
AFE OLV = 03
AFE OLT = 0F
AFE SCC = 76
AFE SCD = 76

[Data(Calibration)]
CC Gain = 10
CC Delta = 10
Ref Voltage = 1227.05
AFE Pack Gain = 672.91
CC Offset = -0.284
Board Offset = 0
Int Temp Offset = 0.0
Ext1 Temp Offset = 0.0
Ext2 Temp Offset = 0.0
[Config(Calibration)]
CC Current = 3000
Voltage Signal = 12600
Temp Signal = 298.0
CC Offset Time = 250
ADC Offset Time = 32
CC Gain Time = 250
Voltage Time = 1888
Temperature Time = 32
Cal Mode Timeout = 300
[Temp Model(Calibration)]
Ext Coef 1 = -28285
Ext Coef 2 = 20848
Ext Coef 3 = -7537
Ext Coef 4 = 401.2
Ext Min AD = 0
Ext Max Temp = 401.2
Int Coef 1 = 0
Int Coef 2 = 0
Int Coef 3 = -11136
Int Coef 4 = 575.4
Int Min AD = 0
Int Max Temp = 575.4
[Current(Calibration)]
Filter = 239
Deadband = 3
CC Deadband = 10.0
